### Bug Summary

File: | plugins/epan/ethercat/packet-ams.c
Warning: | line 673, column 19 Value stored to 'offset' is never read

### Annotated Source Code

Press '?' to see keyboard shortcuts

Show analyzer invocation
clang -cc1 -cc1 -triple x86_64-pc-linux-gnu -analyze -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name packet-ams.c -analyzer-checker=core -analyzer-checker=apiModeling -analyzer-checker=unix -analyzer-checker=deadcode -analyzer-checker=security.insecureAPI.UncheckedReturn -analyzer-checker=security.insecureAPI.getpw -analyzer-checker=security.insecureAPI.gets -analyzer-checker=security.insecureAPI.mktemp -analyzer-checker=security.insecureAPI.mkstemp -analyzer-checker=security.insecureAPI.vfork -analyzer-checker=nullability.NullPassedToNonnull -analyzer-checker=nullability.NullReturnedFromNonnull -analyzer-output plist -w -setup-static-analyzer -mrelocation-model pic -pic-level 2 -fhalf-no-semantic-interposition -fno-delete-null-pointer-checks -mframe-pointer=all -relaxed-aliasing -fmath-errno -ffp-contract=on -fno-rounding-math -ffloat16-excess-precision=fast -fbfloat16-excess-precision=fast -mconstructor-aliases -funwind-tables=2 -target-cpu x86-64 -tune-cpu generic -debugger-tuning=gdb -fdebug-compilation-dir=/builds/wireshark/wireshark/build -fcoverage-compilation-dir=/builds/wireshark/wireshark/build -resource-dir /usr/lib/llvm-21/lib/clang/21 -isystem /usr/include/glib-2.0 -isystem /usr/lib/x86_64-linux-gnu/glib-2.0/include -D G_DISABLE_DEPRECATED -D G_DISABLE_SINGLE_INCLUDES -D PLUGIN_VERSION="0.1.0" -D WS_DEBUG -D WS_DEBUG_UTF_8 -D ethercat_EXPORTS -I /builds/wireshark/wireshark/build -I /builds/wireshark/wireshark -I /builds/wireshark/wireshark/include -I /builds/wireshark/wireshark/plugins/epan/ethercat -D _GLIBCXX_ASSERTIONS -internal-isystem /usr/lib/llvm-21/lib/clang/21/include -internal-isystem /usr/local/include -internal-isystem /usr/lib/gcc/x86_64-linux-gnu/14/../../../../x86_64-linux-gnu/include -internal-externc-isystem /usr/include/x86_64-linux-gnu -internal-externc-isystem /include -internal-externc-isystem /usr/include -fmacro-prefix-map=/builds/wireshark/wireshark/= -fmacro-prefix-map=/builds/wireshark/wireshark/build/= -fmacro-prefix-map=../= -Wno-format-truncation -Wno-format-nonliteral -Wno-pointer-sign -std=gnu11 -ferror-limit 19 -fvisibility=hidden -fwrapv -fwrapv-pointer -fstrict-flex-arrays=3 -stack-protector 2 -fstack-clash-protection -fcf-protection=full -fgnuc-version=4.2.1 -fskip-odr-check-in-gmf -fexceptions -fcolor-diagnostics -analyzer-output=html -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -o /builds/wireshark/wireshark/sbout/2025-10-13-100350-3623-1 -x c /builds/wireshark/wireshark/plugins/epan/ethercat/packet-ams.c

Keyboard shortcuts:

- Use 'j/k' keys for keyboard navigation
- Use 'Shift+S' to show/hide relevant lines
- Use '?' to toggle this window

Close
Show only relevant lines Show control flow arrows

1 | /* packet-ams.c
2 | * Routines for ethercat packet disassembly
3 | *
4 | * Copyright (c) 2007 by Beckhoff Automation GmbH
5 | *
6 | * Wireshark - Network traffic analyzer
7 | * By Gerald Combs <gerald@wireshark.org>
8 | * Copyright 1998 Gerald Combs
9 | *
10 | * SPDX-License-Identifier: GPL-2.0-or-later
11 | */
12 |
13 | /* Include files */
14 |
15 | #include "config.h"
16 |
17 | #include <epan/packet.h>
18 | #include <epan/conversation.h>
19 | #include <epan/tfs.h>
20 | #include <wsutil/array.h>
21 |
22 | #include "packet-ams.h"
23 |
24 | #include "epan/dissectors/packet-tcp.h"
25 |
26 | void proto_register_ams(void);
27 | void proto_reg_handoff_ams(void);
28 |
29 | #define AMS_TCP_PORT_RANGE"48898" "48898" /* Not IANA registered */
30 |
31 | /* Define the ams proto */
32 | int proto_ams;
33 |
34 | static dissector_handle_t amstcp_handle;
35 |
36 | /* Define the tree for ams */
37 | static int ett_ams;
38 | static int ett_ams_stateflags;
39 | static int ett_ams_adsreadrequest;
40 | static int ett_ams_adsreadresponse;
41 | static int ett_ams_adswriterequest;
42 | static int ett_ams_adswriteresponse;
43 | static int ett_ams_adsreadwriterequest;
44 | static int ett_ams_adsreadwriteresponse;
45 | static int ett_ams_adsreadstaterequest;
46 | static int ett_ams_adsreadstateresponse;
47 | static int ett_ams_adswritectrlrequest;
48 | static int ett_ams_adswritectrlresponse;
49 | static int ett_ams_adsreaddinforequest;
50 | static int ett_ams_adsreaddinforesponse;
51 | static int ett_ams_adsadddnrequest;
52 | static int ett_ams_adsadddnresponse;
53 | static int ett_ams_adsdeldnrequest;
54 | static int ett_ams_adsdeldnresponse;
55 | static int ett_ams_adsdnrequest;
56 |
57 | static int hf_ams_sendernetid;
58 | static int hf_ams_senderport;
59 | static int hf_ams_targetnetid;
60 | static int hf_ams_targetport;
61 | static int hf_ams_cmdid;
62 | static int hf_ams_stateflags;
63 | static int hf_ams_stateresponse;
64 | static int hf_ams_statenoreturn;
65 | static int hf_ams_stateadscmd;
66 | static int hf_ams_statesyscmd;
67 | static int hf_ams_statehighprio;
68 | static int hf_ams_statetimestampadded;
69 | static int hf_ams_stateudp;
70 | static int hf_ams_stateinitcmd;
71 | static int hf_ams_statebroadcast;
72 | static int hf_ams_cbdata;
73 | static int hf_ams_errorcode;
74 | static int hf_ams_invokeid;
75 | static int hf_ams_response_in;
76 | static int hf_ams_response_to;
77 | static int hf_ams_response_time;
78 | static int hf_ams_data;
79 |
80 | /*ads Commands */
81 | static int hf_ams_adsindexgroup;
82 | static int hf_ams_adsindexoffset;
83 | static int hf_ams_adscblength;
84 | static int hf_ams_adsreadrequest;
85 | static int hf_ams_adsreadresponse;
86 | static int hf_ams_adsinvokeid;
87 | static int hf_ams_adsresult;
88 | static int hf_ams_adsdata;
89 | static int hf_ams_adswriterequest;
90 | static int hf_ams_adswriteresponse;
91 | static int hf_ams_adsreadwriterequest;
92 | static int hf_ams_adsreadwriteresponse;
93 | static int hf_ams_adscbreadlength;
94 | static int hf_ams_adscbwritelength;
95 | static int hf_ams_adsstate;
96 | static int hf_ams_adsdevicestate;
97 | static int hf_ams_adsnotificationhandle;
98 | static int hf_ams_adsreadstaterequest;
99 | static int hf_ams_adsreadstateresponse;
100 | static int hf_ams_adswritectrlrequest;
101 | static int hf_ams_adswritectrlresponse;
102 | static int hf_ams_adsreaddinforequest;
103 | static int hf_ams_adsreaddinforesponse;
104 | static int hf_ams_adsadddnrequest;
105 | static int hf_ams_adsadddnresponse;
106 | static int hf_ams_adsdeldnrequest;
107 | static int hf_ams_adsdeldnresponse;
108 | static int hf_ams_adsdnrequest;
109 | /* static int hf_ams_adsdnresponse; */
110 | /* static int hf_ams_adsnoteattrib; */
111 | /* static int hf_ams_adsnoteblocks; */
112 | /* static int hf_ams_adsversion; */
113 | static int hf_ams_adsdevicename;
114 | static int hf_ams_adsversionversion;
115 | static int hf_ams_adsversionrevision;
116 | static int hf_ams_adsversionbuild;
117 | static int hf_ams_adsnoteblocksstamps;
118 | /* static int hf_ams_adsnoteblocksstamp; */
119 | /* static int hf_ams_adstimestamp; */
120 | /* static int hf_ams_adssamplecnt; */
121 | /* static int hf_ams_adsnoteblockssample; */
122 | static int hf_ams_adstransmode;
123 | static int hf_ams_adsmaxdelay;
124 | static int hf_ams_adscycletime;
125 | /* static int hf_ams_adscmpmax; */
126 | /* static int hf_ams_adscmpmin; */
127 |
128 | static dissector_handle_t ams_handle;
129 |
130 | /* Structure for tracking request/response transactions */
131 | typedef struct _ams_transaction_t {
132 | uint32_t req_frame;
133 | uint32_t rep_frame;
134 | nstime_t req_time;
135 | } ams_transaction_t;
136 |
137 | /* Structure for per-conversation data */
138 | typedef struct _ams_conv_info_t {
139 | wmem_map_t *transactions; /* Maps invokeId -> ams_transaction_t */
140 | } ams_conv_info_t;
141 |
142 | static const value_string TransMode[] =
143 | {
144 | { 0, "NO TRANS"},
145 | { 1, "CLIENT CYCLE"},
146 | { 2, "CLIENT ON CHANGE"},
147 | { 3, "SERVER CYCLE"},
148 | { 4, "SERVER ON CHANGE"},
149 | { 10, "CLIENT FIRST REQUEST"},
150 | { 0, NULL((void*)0) }
151 | };
152 |
153 | static const value_string ErrorCode[] =
154 | {
155 | { ERR_NOERROR0, "NO ERROR"},
156 | { ERR_INTERNAL1, "INTERNAL"},
157 | { ERR_NORTIME2, "NO RTIME"},
158 | { ERR_ALLOCLOCKEDMEM3, "ALLOC LOCKED MEM"},
159 | { ERR_INSERTMAILBOX4, "INSERT MAILBOX"},
160 | { ERR_WRONGRECEIVEHMSG5, "WRONGRECEIVEHMSG"},
161 | { ERR_TARGETPORTNOTFOUND6, "TARGET PORT NOT FOUND"},
162 | { ERR_TARGETMACHINENOTFOUND7, "TARGET MACHINE NOT FOUND"},
163 | { ERR_UNKNOWNCMDID8, "UNKNOWN CMDID"},
164 | { ERR_BADTASKID9, "BAD TASKID"},
165 | { ERR_NOIO10, "NOIO"},
166 | { ERR_UNKNOWNAMSCMD11, "UNKNOWN AMSCMD"},
167 | { ERR_WIN32ERROR12, "WIN32 ERROR"},
168 | { ERR_PORTNOTCONNECTED13, "PORT NOT CONNECTED"},
169 | { ERR_INVALIDAMSLENGTH14, "INVALID AMS LENGTH"},
170 | { ERR_INVALIDAMSNETID15, "INVALID AMS NETID"},
171 | { ERR_LOWINSTLEVEL16, "LOW INST LEVEL"},
172 | { ERR_NODEBUGINTAVAILABLE17, "NO DEBUG INT AVAILABLE"},
173 | { ERR_PORTDISABLED18, "PORT DISABLED"},
174 | { ERR_PORTALREADYCONNECTED19, "PORT ALREADY CONNECTED"},
175 | { ERR_AMSSYNC_W32ERROR20, "AMSSYNC_W32ERROR"},
176 | { ERR_AMSSYNC_TIMEOUT21, "AMSSYNC_TIMEOUT"},
177 | { ERR_AMSSYNC_AMSERROR22, "AMSSYNC_AMSERROR"},
178 | { ERR_AMSSYNC_NOINDEXINMAP23, "AMSSYNC_NOINDEXINMAP"},
179 | { ERR_INVALIDAMSPORT24, "INVALID AMSPORT"},
180 | { ERR_NOMEMORY25, "NO MEMORY"},
181 | { ERR_TCPSEND26, "TCP SEND"},
182 | { ERR_HOSTUNREACHABLE27, "HOST UNREACHABLE"},
183 | { ROUTERERR_NOLOCKEDMEMORY0 + 0x0500, "ROUTERERR_NOLOCKEDMEMORY"},
184 | { ROUTERERR_RESIZEMEMORY1 + 0x0500, "ROUTERERR_RESIZEMEMORY"},
185 | { ROUTERERR_MAILBOXFULL2 + 0x0500, "ROUTERERR_MAILBOXFULL"},
186 | { ROUTERERR_DEBUGBOXFULL3 + 0x0500, "ROUTERERR_DEBUGBOXFULL"},
187 | { ROUTERERR_UNKNOWNPORTTYPE4 + 0x0500, "ROUTERERR_UNKNOWNPORTTYPE"},
188 | { ROUTERERR_NOTINITIALIZED5 + 0x0500, "ROUTERERR_NOTINITIALIZED"},
189 | { ROUTERERR_PORTALREADYINUSE6 + 0x0500, "ROUTERERR_PORTALREADYINUSE"},
190 | { ROUTERERR_NOTREGISTERED7 + 0x0500, "ROUTERERR_NOTREGISTERED "},
191 | { ROUTERERR_NOMOREQUEUES8 + 0x0500, "ROUTERERR_NOMOREQUEUES"},
192 | { ROUTERERR_INVALIDPORT9 + 0x0500, "ROUTERERR_INVALIDPORT"},
193 | { ROUTERERR_NOTACTIVATED10 + 0x0500, "ROUTERERR_NOTACTIVATED"},
194 | { IOERR_INTERNAL(0 + 0x2000), "IOERR_INTERNAL"},
195 | { IOERR_BADCARDNO(1 + 0x2000), "IOERR_BADCARDNO"},
196 | { IOERR_INVALIDCARDADDR(2 + 0x2000), "IOERR_INVALIDCARDADDR"},
197 | { IOERR_CDLLISTFULL(3 + 0x2000), "IOERR_CDLLISTFULL"},
198 | { IOERR_BADCDLPARAM(4 + 0x2000), "IOERR_BADCDLPARAM"},
199 | { IOERR_OPENIOFAILED(5 + 0x2000), "IOERR_OPENIOFAILED"},
200 | { IOERR_RESETIOFAILED(6 + 0x2000), "IOERR_RESETIOFAILED"},
201 | { IOERR_UNKNOWNDEVICE(7 + 0x2000), "IOERR_UNKNOWNDEVICE"},
202 | { IOERR_UNKNOWNDEVICEID(8 + 0x2000), "IOERR_UNKNOWNDEVICEID"},
203 | { IOERR_UNKNOWNIMAGEID(9 + 0x2000), "IOERR_UNKNOWNIMAGEID"},
204 | { IOERR_GETIOSTATE(10 + 0x2000), "IOERR_GETIOSTATE"},
205 | { IOERR_BADIMAGEID(11 + 0x2000), "IOERR_BADIMAGEID"},
206 | { IOERR_NOMORECLIENTSPACE(12 + 0x2000), "IOERR_NOMORECLIENTSPACE"},
207 | { IOERR_CLIENTINFONOTFOUND(13 + 0x2000), "IOERR_CLIENTINFONOTFOUND"},
208 | { IOERR_CDLNOTINUSE(14 + 0x2000), "IOERR_CDLNOTINUSE"},
209 | { IOERR_TIMEOUTWITHDEVICE(15 + 0x2000), "IOERR_TIMEOUTWITHDEVICE"},
210 | { IOERR_C1220FUNC_1(16 + 0x2000), "IOERR_C1220FUNC_1"},
211 | { IOERR_C1220FUNC_9(17 + 0x2000), "IOERR_C1220FUNC_9"},
212 | { IOERR_C1220FUNC_C(18 + 0x2000), "IOERR_C1220FUNC_C"},
213 | { IOERR_C1220FUNC_10(19 + 0x2000), "IOERR_C1220FUNC_10"},
214 | { IOERR_C1220FUNC_1_MAXSEND(20 + 0x2000), "IOERR_C1220FUNC_1_MAXSEND"},
215 | { IOERR_C1220FUNC_1_ADDRSET(21 + 0x2000), "IOERR_C1220FUNC_1_ADDRSET"},
216 | { IOERR_C1220FUNC_1_BREAK(22 + 0x2000), "IOERR_C1220FUNC_1_BREAK"},
217 | { IOERR_C1220FUNC_1_BREAK0(23 + 0x2000), "IOERR_C1220FUNC_1_BREAK0"},
218 | { IOERR_C1220FUNC_1_BREAK1(24 + 0x2000), "IOERR_C1220FUNC_1_BREAK1"},
219 | { IOERR_C1220FUNC_1_BREAK2(25 + 0x2000), "IOERR_C1220FUNC_1_BREAK2"},
220 | { IOERR_C1220FUNC_1_BREAK3(26 + 0x2000), "IOERR_C1220FUNC_1_BREAK3"},
221 | { IOERR_C1220FUNC_1_BREAK4(27 + 0x2000), "IOERR_C1220FUNC_1_BREAK4"},
222 | { IOERR_C1220FUNC_1_BREAK5(28 + 0x2000), "IOERR_C1220FUNC_1_BREAK5"},
223 | { IOERR_C1220FUNC_1_BREAK6(29 + 0x2000), "IOERR_C1220FUNC_1_BREAK6"},
224 | { IOERR_C1220FUNC_1_BREAK7(30 + 0x2000), "IOERR_C1220FUNC_1_BREAK7"},
225 | { IOERR_C1220FUNC_1_BREAK8(31 + 0x2000), "IOERR_C1220FUNC_1_BREAK8"},
226 | { IOERR_C1220FUNC_1_BREAK9(32 + 0x2000), "IOERR_C1220FUNC_1_BREAK9"},
227 | { IOERR_C1220FUNC_1_BREAK10(33 + 0x2000), "IOERR_C1220FUNC_1_BREAK10"},
228 | { IOERR_C1220FUNC_1_BREAK11(34 + 0x2000), "IOERR_C1220FUNC_1_BREAK11"},
229 | { IOERR_C1220FUNC_1_BREAK12(35 + 0x2000), "IOERR_C1220FUNC_1_BREAK12"},
230 | { IOERR_C1220FUNC_1_BREAK13(36 + 0x2000), "IOERR_C1220FUNC_1_BREAK13"},
231 | { IOERR_C1220FUNC_1_BREAK14(37 + 0x2000), "IOERR_C1220FUNC_1_BREAK14"},
232 | { IOERR_C1220FUNC_1_BREAK15(38 + 0x2000), "IOERR_C1220FUNC_1_BREAK15"},
233 | { IOERR_C1220FUNC_1_BREAK16(39 + 0x2000), "IOERR_C1220FUNC_1_BREAK16"},
234 | { IOERR_SPC3DEVINITDP(40 + 0x2000), "IOERR_SPC3DEVINITDP"},
235 | { IOERR_SPC3UPDATEOUTPUT(41 + 0x2000), "IOERR_SPC3UPDATEOUTPUT"},
236 | { IOERR_CIF30READDIAG(42 + 0x2000), "IOERR_CIF30READDIAG"},
237 | { IOERR_CIF30COMMNOTSTARTED(43 + 0x2000), "IOERR_CIF30COMMNOTSTARTED"},
238 | { IOERR_CIF30SLAVEPARASIZE(44 + 0x2000), "IOERR_CIF30SLAVEPARASIZE"},
239 | { IOERR_CIF30NOPARAS(45 + 0x2000), "IOERR_CIF30NOPARAS"},
240 | { IOERR_CIF30SLAVEERROR(46 + 0x2000), "IOERR_CIF30SLAVEERROR"},
241 | { IOERR_CIF30WATCHDOGEXPIRED(47 + 0x2000), "IOERR_CIF30WATCHDOGEXPIRED"},
242 | { IOERR_UNKNOWNDEVICECMD(48 + 0x2000), "IOERR_UNKNOWNDEVICECMD"},
243 | { IOERR_CIF40MESSAGEHANDLING(49 + 0x2000), "IOERR_CIF40MESSAGEHANDLING"},
244 | { IOERR_CIF40PARAERROR(50 + 0x2000), "IOERR_CIF40PARAERROR"},
245 | { IOERR_CIF40WATCHDOGEXPIRED(51 + 0x2000), "IOERR_CIF40WATCHDOGEXPIRED"},
246 | { IOERR_CIF40FLAGERROR(52 + 0x2000), "IOERR_CIF40FLAGERROR"},
247 | { IOERR_CIF40COMMNOTSTARTED(53 + 0x2000), "IOERR_CIF40COMMNOTSTARTED"},
248 | { IOERR_CIF40READDIAG(54 + 0x2000), "IOERR_CIF40READDIAG"},
249 | { IOERR_CIF40SLAVEERROR(55 + 0x2000), "IOERR_CIF40SLAVEERROR"},
250 | { IOERR_CIF40GLOBALERROR(56 + 0x2000), "IOERR_CIF40GLOBALERROR"},
251 | { IOERR_CIF40CONFIGLIST(57 + 0x2000), "IOERR_CIF40CONFIGLIST"},
252 | { IOERR_CP5412A2SLAVEPARASIZE(58 + 0x2000), "IOERR_CP5412A2SLAVEPARASIZE"},
253 | { IOERR_CP5412A2NOPARAS(59 + 0x2000), "IOERR_CP5412A2NOPARAS"},
254 | { IOERR_CP5412A2SLAVEERROR(60 + 0x2000), "IOERR_CP5412A2SLAVEERROR"},
255 | { IOERR_CP5412A2FATAL(61 + 0x2000), "IOERR_CP5412A2FATAL"},
256 | { IOERR_CP5412A2MAILBOXUSED(62 + 0x2000), "IOERR_CP5412A2MAILBOXUSED"},
257 | { IOERR_BEGINCONFIGWHILETICKER(63 + 0x2000), "IOERR_BEGINCONFIGWHILETICKER"},
258 | { IOERR_UNEXPECTEDBOXCOUNT(64 + 0x2000), "IOERR_UNEXPECTEDBOXCOUNT"},
259 | { IOERR_C1200CHECKADDR(65 + 0x2000), "IOERR_C1200CHECKADDR"},
260 | { IOERR_C1200INTENSITYTEST(66 + 0x2000), "IOERR_C1200INTENSITYTEST"},
261 | { IOERR_NOIMAGE(67 + 0x2000), "IOERR_NOIMAGE"},
262 | { IOERR_INVALIDIMAGEOFFSSIZE(68 + 0x2000), "IOERR_INVALIDIMAGEOFFSSIZE"},
263 | { IOERR_FORCESCOUNTEXCEEDEDMAXIMUM(69 + 0x2000), "IOERR_FORCESCOUNTEXCEEDEDMAXIMUM"},
264 | { IOERR_SERCOSLIFECOUNTERERR(70 + 0x2000), "IOERR_SERCOSLIFECOUNTERERR"},
265 | { IOERR_C1220NOTFOUND(71 + 0x2000), "IOERR_C1220NOTFOUND"},
266 | { IOERR_AMSDEVICENOAMSINTF(72 + 0x2000), "IOERR_AMSDEVICENOAMSINTF"},
267 | { IOERR_AMSDEVICEAMSCMDIDNOTSUPP(73 + 0x2000), "IOERR_AMSDEVICEAMSCMDIDNOTSUPP"},
268 | { IOERR_AMSDEVICEAMSSERVICERUNNING(74 + 0x2000), "IOERR_AMSDEVICEAMSSERVICERUNNING"},
269 | { IOERR_PLCINTERFACE_BUSY(75 + 0x2000), "IOERR_PLCINTERFACE_BUSY"},
270 | { IOERR_PLCINTERFACE_FAULT(76 + 0x2000), "IOERR_PLCINTERFACE_FAULT"},
271 | { IOERR_PLCINTERFACE_TIMEOUT(77 + 0x2000), "IOERR_PLCINTERFACE_TIMEOUT"},
272 | { IOERR_PLCINTERFACE_RESETTIMEOUT(78 + 0x2000), "IOERR_PLCINTERFACE_RESETTIMEOUT"},
273 | { IOERR_PLCINTERFACE_NODATAEXCH(79 + 0x2000), "IOERR_PLCINTERFACE_NODATAEXCH"},
274 | { IOERR_PLCINTERFACE_RESET(80 + 0x2000), "IOERR_PLCINTERFACE_RESET"},
275 | { IOERR_CP5412A2INVALIDADDR(81 + 0x2000), "IOERR_CP5412A2INVALIDADDR"},
276 | { IOERR_CP5412A2INVALIDPORT(82 + 0x2000), "IOERR_CP5412A2INVALIDPORT"},
277 | { IOERR_AMSDEVICEBADBOXNO(83 + 0x2000), "IOERR_AMSDEVICEBADBOXNO"},
278 | { IOERR_AMSDEVICEBADTYPE(84 + 0x2000), "IOERR_AMSDEVICEBADTYPE"},
279 | { IOERR_AMSDEVICEILLEGALADDRESS(85 + 0x2000), "IOERR_AMSDEVICEILLEGALADDRESS"},
280 | { IOERR_CP5412A2INVALIDBOX(86 + 0x2000), "IOERR_CP5412A2INVALIDBOX"},
281 | { IOERR_AMSDEVICEFIFOOVERFLOW(87 + 0x2000), "IOERR_AMSDEVICEFIFOOVERFLOW"},
282 | { IOERR_AMSDEVICEAMSSEQUENCEERROR(88 + 0x2000), "IOERR_AMSDEVICEAMSSEQUENCEERROR"},
283 | { IOERR_CP5412A2DPV1SYNTAXERROR(89 + 0x2000), "IOERR_CP5412A2DPV1SYNTAXERROR"},
284 | { IOERR_CP5412A2DEVICENOTRUNNING(90 + 0x2000), "IOERR_CP5412A2DEVICENOTRUNNING"},
285 | { IOERR_AMSDEVICENOTRUNNING(91 + 0x2000), "IOERR_AMSDEVICENOTRUNNING"},
286 | { IOERR_AMSDEVICEBOXNOTDEFINED(92 + 0x2000), "IOERR_AMSDEVICEBOXNOTDEFINED"},
287 | { IOERR_CP5412A2BADSERVICEPARA(93 + 0x2000), "IOERR_CP5412A2BADSERVICEPARA"},
288 | { IOERR_CP5412A2FIFOOVERFLOW(94 + 0x2000), "IOERR_CP5412A2FIFOOVERFLOW"},
289 | { IOERR_COMPORTOPENFAILED(95 + 0x2000), "IOERR_COMPORTOPENFAILED"},
290 | { IOERR_CIF30BADMESSAGERESPONSE(96 + 0x2000), "IOERR_CIF30BADMESSAGERESPONSE"},
291 | { IOERR_CIF30DELETEDATABASE(97 + 0x2000), "IOERR_CIF30DELETEDATABASE"},
292 | { IOERR_CIF30STARTSEQFAILED(98 + 0x2000), "IOERR_CIF30STARTSEQFAILED"},
293 | { IOERR_CIF30DOWNLOADFAILED(99 + 0x2000), "IOERR_CIF30DOWNLOADFAILED"},
294 | { IOERR_CIF30ENDSEQFAILED(100 + 0x2000), "IOERR_CIF30ENDSEQFAILED"},
295 | { IOERR_CIF30BUSLOADFAILED(101 + 0x2000), "IOERR_CIF30BUSLOADFAILED"},
296 | { IOERR_PLCINTERFACE_RESETREQ(102 + 0x2000), "IOERR_PLCINTERFACE_RESETREQ"},
297 | { IOERR_CP5412A2INVALIDCYCLETICKS(103 + 0x2000), "IOERR_CP5412A2INVALIDCYCLETICKS"},
298 | { IOERR_CP5412A2DPBUSFAULT(104 + 0x2000), "IOERR_CP5412A2DPBUSFAULT"},
299 | { IOERR_INVALIDTERMCONFIG(105 + 0x2000), "IOERR_INVALIDTERMCONFIG"},
300 | { IOERR_SERCANSBREAK(106 + 0x2000), "IOERR_SERCANSBREAK"},
301 | { IOERR_SERCANSPHASE0(107 + 0x2000), "IOERR_SERCANSPHASE0"},
302 | { IOERR_SERCANSPHASE1(108 + 0x2000), "IOERR_SERCANSPHASE1"},
303 | { IOERR_SERCANSPHASE2(109 + 0x2000), "IOERR_SERCANSPHASE2"},
304 | { IOERR_SERCANSPHASE3(110 + 0x2000), "IOERR_SERCANSPHASE3"},
305 | { IOERR_SERCANSPHASE4(111 + 0x2000), "IOERR_SERCANSPHASE4"},
306 | { IOERR_SERCANSNCSERVICECHNFAILED(112 + 0x2000), "IOERR_SERCANSNCSERVICECHNFAILED"},
307 | { IOERR_RESOURCECONFICT(113 + 0x2000), "IOERR_RESOURCECONFICT"},
308 | { IOERR_C1220INITSTRINGCOMM(114 + 0x2000), "IOERR_C1220INITSTRINGCOMM"},
309 | { IOERR_C1220REGSTRINGSLAVE(115 + 0x2000), "IOERR_C1220REGSTRINGSLAVE"},
310 | { IOERR_C1220STRREGFAULT(116 + 0x2000), "IOERR_C1220STRREGFAULT"},
311 | { IOERR_IOSTATEBUSY(117 + 0x2000), "IOERR_IOSTATEBUSY"},
312 | { IOERR_IBSSCITWATCHDOGEXPIRED(118 + 0x2000), "IOERR_IBSSCITWATCHDOGEXPIRED"},
313 | { IOERR_IBSSCITSYNCMAILBOXERROR(119 + 0x2000), "IOERR_IBSSCITSYNCMAILBOXERROR"},
314 | { IOERR_IBSSCITCONFIRMDIAGERROR(120 + 0x2000), "IOERR_IBSSCITCONFIRMDIAGERROR"},
315 | { IOERR_IBSSCITCREATECFGERROR(121 + 0x2000), "IOERR_IBSSCITCREATECFGERROR"},
316 | { 0, NULL((void*)0) }
317 | };
318 |
319 | static const value_string AdsErrorMode[] =
320 | {
321 | { ADSERR_NOERR0x00, "NO ERROR", },
322 | { ADSERR_DEVICE_ERROR(0x700), "ERROR", },
323 | { ADSERR_DEVICE_SRVNOTSUPP(0x701), "SRV NOT SUPP", },
324 | { ADSERR_DEVICE_INVALIDGRP(0x702), "INVALID GRP", },
325 | { ADSERR_DEVICE_INVALIDOFFSET(0x703), "INVALID OFFSET", },
326 | { ADSERR_DEVICE_INVALIDACCESS(0x704), "INVALID ACCESS", },
327 | { ADSERR_DEVICE_INVALIDSIZE(0x705), "INVALID SIZE", },
328 | { ADSERR_DEVICE_INVALIDDATA(0x706), "INVALID DATA", },
329 | { ADSERR_DEVICE_NOTREADY(0x707), "NOT READY", },
330 | { ADSERR_DEVICE_BUSY(0x708), "BUSY", },
331 | { ADSERR_DEVICE_INVALIDCONTEXT(0x709), "INVALID CONTEXT", },
332 | { ADSERR_DEVICE_NOMEMORY(0x70A), "NO MEMORY", },
333 | { ADSERR_DEVICE_INVALIDPARM(0x70B), "INVALID PARM", },
334 | { ADSERR_DEVICE_NOTFOUND(0x70C), "NOT FOUND", },
335 | { ADSERR_DEVICE_SYNTAX(0x70D), "SYNTAX", },
336 | { ADSERR_DEVICE_INCOMPATIBLE(0x70E), "INCOMPATIBLE", },
337 | { ADSERR_DEVICE_EXISTS(0x70F), "EXISTS", },
338 | { ADSERR_DEVICE_SYMBOLNOTFOUND(0x710), "SYMBOL NOT FOUND", },
339 | { ADSERR_DEVICE_SYMBOLVERSIONINVALID(0x711), "SYMBOL VERSION INVALID", },
340 | { ADSERR_DEVICE_INVALIDSTATE(0x712), "INVALID STATE", },
341 | { ADSERR_DEVICE_TRANSMODENOTSUPP(0x713), "TRANS MODE NOT SUPP", },
342 | { ADSERR_DEVICE_NOTIFYHNDINVALID(0x714), "NOTIFY HND INVALID", },
343 | { ADSERR_DEVICE_CLIENTUNKNOWN(0x715), "CLIENT UNKNOWN", },
344 | { ADSERR_DEVICE_NOMOREHDLS(0x716), "NO MORE HDLS", },
345 | { ADSERR_DEVICE_INVALIDWATCHSIZE(0x717), "INVALID WATCHSIZE", },
346 | { ADSERR_DEVICE_NOTINIT(0x718), "NOT INIT", },
347 | { ADSERR_DEVICE_TIMEOUT(0x719), "TIMEOUT", },
348 | { ADSERR_DEVICE_NOINTERFACE(0x71A), "NO INTERFACE", },
349 | { ADSERR_DEVICE_INVALIDINTERFACE(0x71B), "INVALID INTERFACE", },
350 | { ADSERR_DEVICE_INVALIDCLSID(0x71C), "INVALID CLSID", },
351 | { ADSERR_DEVICE_INVALIDOBJID(0x71D), "INVALID OBJID", },
352 | { ADSERR_DEVICE_PENDING(0x71E), "PENDING", },
353 | { ADSERR_DEVICE_ABORTED(0x71F), "ABORTED", },
354 | { ADSERR_DEVICE_WARNING(0x720), "WARNING", },
355 | { ADSERR_DEVICE_INVALIDARRAYIDX(0x721), "INVALID ARRAY IDX", },
356 | { ADSERR_CLIENT_ERROR(0x740), "CLIENT ERROR", },
357 | { ADSERR_CLIENT_INVALIDPARM(0x741), "CLIENT INVALID PARM", },
358 | { ADSERR_CLIENT_LISTEMPTY(0x742), "CLIENT LIST EMPTY", },
359 | { ADSERR_CLIENT_VARUSED(0x743), "CLIENT VAR USED", },
360 | { ADSERR_CLIENT_DUPLINVOKEID(0x744), "CLIENT DUPL INVOKEID", },
361 | { ADSERR_CLIENT_SYNCTIMEOUT(0x745), "CLIENT SYNC TIMEOUT", },
362 | { ADSERR_CLIENT_W32ERROR(0x746), "CLIENT W32ERROR", },
363 | { ADSERR_CLIENT_TIMEOUTINVALID(0x747), "CLIENT TIMEOUT INVALID", },
364 | { ADSERR_CLIENT_PORTNOTOPEN(0x748), "CLIENT PORT NOT OPEN", },
365 | { ADSERR_CLIENT_NOAMSADDR(0x749), "CLIENT NO AMS ADDR", },
366 | { ADSERR_CLIENT_SYNCINTERNAL(0x750), "CLIENT SYNC INTERNAL", },
367 | { ADSERR_CLIENT_ADDHASH(0x751), "CLIENT ADD HASH", },
368 | { ADSERR_CLIENT_REMOVEHASH(0x752), "CLIENT REMOVE HASH", },
369 | { ADSERR_CLIENT_NOMORESYM(0x753), "CLIENT NO MORE SYM", },
370 | { ADSERR_CLIENT_SYNCRESINVALID(0x754), "CLIENT SYNC RES INVALID", },
371 | { ADSERR_CLIENT_SYNCPORTLOCKED(0x755), "CLIENT SYNC PORT LOCKED", },
372 | { 0, NULL((void*)0) }
373 | };
374 |
375 |
376 | /* AMS Command Id
377 | * https://infosys.beckhoff.com/english.php?content=../content/1033/tcadsamsspec/html/tcadsamsspec_adscmd_readstate.htm&id=10652
378 | */
379 | static const value_string AMS_CommandId_vals[] =
380 | {
381 | { ADSSRVID_INVALID0x00, "Invalid", },
382 | { ADSSRVID_READDEVICEINFO0x01, "ADS Read Device Info", },
383 | { ADSSRVID_READ0x02, "ADS Read", },
384 | { ADSSRVID_WRITE0x03, "ADS Write", },
385 | { ADSSRVID_READSTATE0x04, "ADS Read State", },
386 | { ADSSRVID_WRITECTRL0x05, "ADS Write Control", },
387 | { ADSSRVID_ADDDEVICENOTE0x06, "ADS Add Device Notification", },
388 | { ADSSRVID_DELDEVICENOTE0x07, "ADS Delete Device Notification", },
389 | { ADSSRVID_DEVICENOTE0x08, "ADS Device Notification", },
390 | { ADSSRVID_READWRITE0x09, "ADS Read Write", },
391 | { 0, NULL((void*)0) }
392 | };
393 |
394 |
395 | static const char* NetIdFormater(wmem_allocator_t* scope, tvbuff_t *tvb, unsigned offset)
396 | {
397 | return wmem_strdup_printf (scope, "%d.%d.%d.%d.%d.%d", tvb_get_uint8(tvb, offset),
398 | tvb_get_uint8(tvb, offset+1),
399 | tvb_get_uint8(tvb, offset+2),
400 | tvb_get_uint8(tvb, offset+3),
401 | tvb_get_uint8(tvb, offset+4),
402 | tvb_get_uint8(tvb, offset+5)
403 | );
404 | }
405 |
406 |
407 |
408 | /*ams*/
409 | static int dissect_ams_pdu(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, int offset)
410 | {
411 | proto_item *ti, *anItem;
412 | proto_tree *ams_tree, *ams_adstree;
413 | unsigned ams_length = tvb_reported_length(tvb);
414 | uint16_t stateflags;
415 | uint32_t cmdId, cbdata = 0;
416 | uint32_t invokeId;
417 | conversation_t *conversation;
418 | ams_conv_info_t *ams_info;
419 | ams_transaction_t *ams_trans = NULL((void*)0);
420 | static int* const state_flags[] = {
421 | &hf_ams_stateresponse,
422 | &hf_ams_statenoreturn,
423 | &hf_ams_stateadscmd,
424 | &hf_ams_statesyscmd,
425 | &hf_ams_statehighprio,
426 | &hf_ams_statetimestampadded,
427 | &hf_ams_stateudp,
428 | &hf_ams_stateinitcmd,
429 | &hf_ams_statebroadcast,
430 | NULL((void*)0)
431 | };
432 |
433 | col_set_str(pinfo->cinfo, COL_PROTOCOL, "AMS");
434 | col_clear(pinfo->cinfo, COL_INFO);
435 |
436 | if( ams_length < AmsHead_Len(int)sizeof(AmsHead) )
437 | return offset;
438 |
439 | ti = proto_tree_add_item(tree, proto_ams, tvb, 0, -1, ENC_NA0x00000000);
440 | ams_tree = proto_item_add_subtree(ti, ett_ams);
441 |
442 | proto_tree_add_string(ams_tree, hf_ams_targetnetid, tvb, offset, AmsNetId_Len(int)sizeof(AmsNetId), NetIdFormater(pinfo->pool, tvb, offset));
443 | offset += AmsNetId_Len(int)sizeof(AmsNetId);
444 |
445 | proto_tree_add_item(ams_tree, hf_ams_targetport, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
446 | offset += 2;
447 |
448 | proto_tree_add_string(ams_tree, hf_ams_sendernetid, tvb, offset, AmsNetId_Len(int)sizeof(AmsNetId), NetIdFormater(pinfo->pool, tvb, offset));
449 | offset += AmsNetId_Len(int)sizeof(AmsNetId);
450 |
451 | proto_tree_add_item(ams_tree, hf_ams_senderport, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
452 | offset += 2;
453 |
454 | proto_tree_add_item_ret_uint(ams_tree, hf_ams_cmdid, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000, &cmdId);
455 | offset += 2;
456 |
457 | proto_tree_add_bitmask(ams_tree, tvb, offset, hf_ams_stateflags, ett_ams_stateflags, state_flags, ENC_LITTLE_ENDIAN0x80000000);
458 | stateflags = tvb_get_letohs(tvb, offset);
459 | offset += 2;
460 |
461 | proto_tree_add_item_ret_uint(ams_tree, hf_ams_cbdata, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000, &cbdata);
462 | offset += 4;
463 |
464 | proto_tree_add_item(ams_tree, hf_ams_errorcode, tvb, offset, 4,ENC_LITTLE_ENDIAN0x80000000);
465 | offset += 4;
466 |
467 | proto_tree_add_item_ret_uint(ams_tree, hf_ams_invokeid, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000, &invokeId);
468 | offset += 4;
469 |
470 | /* Track request/response using conversation */
471 | conversation = find_or_create_conversation(pinfo);
472 | ams_info = (ams_conv_info_t *)conversation_get_proto_data(conversation, proto_ams);
473 | if (!ams_info) {
474 | /* No conversation data yet, create it */
475 | ams_info = wmem_new(wmem_file_scope(), ams_conv_info_t)((ams_conv_info_t*)wmem_alloc((wmem_file_scope()), sizeof(ams_conv_info_t )));
476 | ams_info->transactions = wmem_map_new(wmem_file_scope(), g_direct_hash, g_direct_equal);
477 | conversation_add_proto_data(conversation, proto_ams, ams_info);
478 | }
479 |
480 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
481 | /* First pass - track the transaction */
482 | if ((stateflags & AMSCMDSF_RESPONSE0x0001) == 0) {
483 | /* This is a request */
484 | ams_trans = wmem_new(wmem_file_scope(), ams_transaction_t)((ams_transaction_t*)wmem_alloc((wmem_file_scope()), sizeof(ams_transaction_t )));
485 | ams_trans->req_frame = pinfo->num;
486 | ams_trans->rep_frame = 0;
487 | ams_trans->req_time = pinfo->abs_ts;
488 | wmem_map_insert(ams_info->transactions, GUINT_TO_POINTER(invokeId)((gpointer) (gulong) (invokeId)), ams_trans);
489 | } else {
490 | /* This is a response */
491 | ams_trans = (ams_transaction_t *)wmem_map_lookup(ams_info->transactions, GUINT_TO_POINTER(invokeId)((gpointer) (gulong) (invokeId)));
492 | if (ams_trans && ams_trans->rep_frame == 0) {
493 | ams_trans->rep_frame = pinfo->num;
494 | }
495 | }
496 | } else {
497 | /* Subsequent pass - retrieve the transaction */
498 | ams_trans = (ams_transaction_t *)wmem_map_lookup(ams_info->transactions, GUINT_TO_POINTER(invokeId)((gpointer) (gulong) (invokeId)));
499 | }
500 |
501 | if (!ams_trans) {
502 | /* Create a "fake" transaction structure for this packet */
503 | ams_trans = wmem_new(pinfo->pool, ams_transaction_t)((ams_transaction_t*)wmem_alloc((pinfo->pool), sizeof(ams_transaction_t )));
504 | ams_trans->req_frame = 0;
505 | ams_trans->rep_frame = 0;
506 | ams_trans->req_time = pinfo->abs_ts;
507 | }
508 |
509 | if ( (stateflags & AMSCMDSF_ADSCMD0x0004) != 0 )
510 | {
511 | /* ADS */
512 | if ( (stateflags & AMSCMDSF_RESPONSE0x0001) == 0 )
513 | {
514 | col_append_fstr(pinfo->cinfo, COL_INFO, "%s Request", val_to_str_const(cmdId, AMS_CommandId_vals, "Unknown"));
515 |
516 | /* Add request state tracking info to the tree */
517 | if (ams_trans->rep_frame) {
518 | proto_item *it;
519 | it = proto_tree_add_uint(ams_tree, hf_ams_response_in, tvb, 0, 0, ams_trans->rep_frame);
520 | proto_item_set_generated(it);
521 | }
522 |
523 | /* Request */
524 | switch ( cmdId )
525 | {
526 | case ADSSRVID_READ0x02:
527 | {
528 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsreadrequest, tvb, offset, ams_length-offset, ENC_NA0x00000000);
529 | if( ams_length-offset >= TAdsReadReq_Len(int)sizeof(TAdsReadReq) )
530 | {
531 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsreadrequest);
532 | proto_tree_add_item(ams_adstree, hf_ams_adsindexgroup, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
533 | offset += 4;
534 |
535 | proto_tree_add_item(ams_adstree, hf_ams_adsindexoffset, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
536 | offset += 4;
537 |
538 | proto_tree_add_item(ams_adstree, hf_ams_adscblength, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
539 | }
540 | }
541 | break;
542 | case ADSSRVID_WRITE0x03:
543 | {
544 | anItem = proto_tree_add_item(ams_tree, hf_ams_adswriterequest, tvb, offset, ams_length-offset, ENC_NA0x00000000);
545 | if( ams_length-offset >= TAdsWriteReq_Len14 - 2 )
546 | {
547 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adswriterequest);
548 | proto_tree_add_item(ams_adstree, hf_ams_adsindexgroup, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
549 | offset += 4;
550 |
551 | proto_tree_add_item(ams_adstree, hf_ams_adsindexoffset, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
552 | offset += 4;
553 |
554 | proto_tree_add_item(ams_adstree, hf_ams_adscblength, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
555 | offset += 4;
556 |
557 | proto_tree_add_item(ams_adstree, hf_ams_adsdata, tvb, offset, ams_length-offset, ENC_NA0x00000000);
558 | }
559 | }
560 | break;
561 | case ADSSRVID_READWRITE0x09:
562 | {
563 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsreadwriterequest, tvb, offset, ams_length-offset, ENC_NA0x00000000);
564 | if( ams_length-offset >= TAdsReadWriteReq_Len18 - 2)
565 | {
566 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsreadwriterequest);
567 | proto_tree_add_item(ams_adstree, hf_ams_adsindexgroup, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
568 | offset += 4;
569 |
570 | proto_tree_add_item(ams_adstree, hf_ams_adsindexoffset, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
571 | offset += 4;
572 |
573 | proto_tree_add_item(ams_adstree, hf_ams_adscbreadlength, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
574 | offset += 4;
575 |
576 | proto_tree_add_item(ams_adstree, hf_ams_adscbwritelength, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
577 | offset += 4;
578 |
579 | proto_tree_add_item(ams_adstree, hf_ams_adsdata, tvb, offset, ams_length-offset, ENC_NA0x00000000);
580 | }
581 | }
582 | break;
583 | case ADSSRVID_READSTATE0x04:
584 | {
585 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsreadstaterequest, tvb, offset, ams_length-offset, ENC_NA0x00000000);
586 | if( ams_length-offset >= TAdsReadStateReq_Len(int)sizeof(TAdsReadStateReq) )
587 | {
588 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsreadstaterequest);
589 | proto_tree_add_item(ams_adstree, hf_ams_adsinvokeid, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
590 | }
591 | }
592 | break;
593 | case ADSSRVID_WRITECTRL0x05:
594 | {
595 | anItem = proto_tree_add_item(ams_tree, hf_ams_adswritectrlrequest, tvb, offset, ams_length-offset, ENC_NA0x00000000);
596 | if( ams_length-offset >= TAdsWriteControlReq_Len10 - 2 )
597 | {
598 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adswritectrlrequest);
599 | proto_tree_add_item(ams_adstree, hf_ams_adsstate, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
600 | offset += 2;
601 |
602 | proto_tree_add_item(ams_adstree, hf_ams_adsdevicestate, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
603 | offset += 2;
604 |
605 | proto_tree_add_item(ams_adstree, hf_ams_adscblength, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
606 | offset += 4;
607 |
608 | proto_tree_add_item(ams_adstree, hf_ams_adsdata, tvb, offset, ams_length-offset, ENC_NA0x00000000);
609 | }
610 | }
611 | break;
612 | case ADSSRVID_READDEVICEINFO0x01:
613 | {
614 | if (cbdata !=0 )
615 | {
616 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsreaddinforequest, tvb, offset, ams_length-offset, ENC_NA0x00000000);
617 | if( ams_length-offset >= TAdsReadDeviceInfoReq_Len(int)sizeof(TAdsReadDeviceInfoReq) )
618 | {
619 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsreaddinforequest);
620 | proto_tree_add_item(ams_adstree, hf_ams_adsresult, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
621 | }
622 | }
623 | }
624 | break;
625 | case ADSSRVID_ADDDEVICENOTE0x06:
626 | {
627 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsadddnrequest, tvb, offset, ams_length-offset, ENC_NA0x00000000);
628 | if( ams_length-offset >= TAdsAddDeviceNotificationReq_Len(int)sizeof(TAdsAddDeviceNotificationReq) )
629 | {
630 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsadddnrequest);
631 | proto_tree_add_item(ams_adstree, hf_ams_adsindexgroup, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
632 | offset += 4;
633 |
634 | proto_tree_add_item(ams_adstree, hf_ams_adsindexoffset, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
635 | offset += 4;
636 |
637 | proto_tree_add_item(ams_adstree, hf_ams_adscblength, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
638 | offset += 4;
639 |
640 | proto_tree_add_item(ams_adstree, hf_ams_adstransmode, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
641 | offset += 4;
642 |
643 | proto_tree_add_item(ams_adstree, hf_ams_adsmaxdelay, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
644 | offset += 4;
645 |
646 | proto_tree_add_item(ams_adstree, hf_ams_adscycletime, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
647 | offset += 4;
648 | }
649 | }
650 | break;
651 | case ADSSRVID_DELDEVICENOTE0x07:
652 | {
653 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsdeldnrequest, tvb, offset, ams_length-offset, ENC_NA0x00000000);
654 | if( ams_length-offset >= TAdsDelDeviceNotificationReq_Len(int)sizeof(TAdsDelDeviceNotificationReq) )
655 | {
656 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsdeldnrequest);
657 | proto_tree_add_item(ams_adstree, hf_ams_adsnotificationhandle, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
658 | }
659 | }
660 | break;
661 | case ADSSRVID_DEVICENOTE0x08:
662 | {
663 | uint32_t cbLength, nStamps;
664 |
665 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsdnrequest, tvb, offset, ams_length-offset, ENC_NA0x00000000);
666 | if( ams_length-offset >= TAdsDeviceNotificationReq_Len(int)sizeof(TAdsDeviceNotificationReq) )
667 | {
668 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsdnrequest);
669 | proto_tree_add_item_ret_uint(ams_adstree, hf_ams_adscblength, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000, &cbLength);
670 | offset += 4;
671 |
672 | proto_tree_add_item_ret_uint(ams_adstree, hf_ams_adsnoteblocksstamps, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000, &nStamps);
673 | offset += 4;
| Value stored to 'offset' is never read
674 |
675 | /*ToDo: dissect noteblocks*/
676 | }
677 | }
678 | break;
679 | }
680 | }
681 | else
682 | {
683 | col_append_fstr(pinfo->cinfo, COL_INFO, "%s Response", val_to_str_const(cmdId, AMS_CommandId_vals, "Unknown"));
684 |
685 | /* Add response state tracking info to the tree */
686 | if (ams_trans->req_frame) {
687 | proto_item *it;
688 | nstime_t ns;
689 |
690 | it = proto_tree_add_uint(ams_tree, hf_ams_response_to, tvb, 0, 0, ams_trans->req_frame);
691 | proto_item_set_generated(it);
692 |
693 | nstime_delta(&ns, &pinfo->abs_ts, &ams_trans->req_time);
694 | it = proto_tree_add_time(ams_tree, hf_ams_response_time, tvb, 0, 0, &ns);
695 | proto_item_set_generated(it);
696 | }
697 |
698 | /* Response */
699 | switch ( cmdId )
700 | {
701 | case ADSSRVID_READ0x02:
702 | {
703 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsreadresponse, tvb, offset, ams_length-offset, ENC_NA0x00000000);
704 | if( ams_length-offset >= TAdsReadRes_Len(int)sizeof(TAdsReadRes) - 2 )
705 | {
706 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsreadresponse);
707 | proto_tree_add_item(ams_adstree, hf_ams_adsresult, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
708 | offset += 4;
709 |
710 | proto_tree_add_item(ams_adstree, hf_ams_adscblength, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
711 | offset += 4;
712 |
713 | proto_tree_add_item(ams_adstree, hf_ams_adsdata, tvb, offset, ams_length-offset, ENC_NA0x00000000);
714 | }
715 | }
716 | break;
717 | case ADSSRVID_WRITE0x03:
718 | {
719 | anItem = proto_tree_add_item(ams_tree, hf_ams_adswriteresponse, tvb, offset, ams_length-offset, ENC_NA0x00000000);
720 | if( ams_length-offset >= TAdsWriteRes_Len(int)sizeof(TAdsWriteRes) )
721 | {
722 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adswriteresponse);
723 | proto_tree_add_item(ams_adstree, hf_ams_adsresult, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
724 | }
725 | }
726 | break;
727 | case ADSSRVID_READWRITE0x09:
728 | {
729 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsreadwriteresponse, tvb, offset, ams_length-offset, ENC_NA0x00000000);
730 | if( ams_length-offset >= TAdsReadWriteRes_Len(int)sizeof(TAdsReadWriteRes) - 2 )
731 | {
732 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsreadwriteresponse);
733 | proto_tree_add_item(ams_adstree, hf_ams_adsresult, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
734 | offset += 4;
735 |
736 | proto_tree_add_item(ams_adstree, hf_ams_adscblength, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
737 | offset += 4;
738 |
739 | proto_tree_add_item(ams_adstree, hf_ams_adsdata, tvb, offset, ams_length-offset, ENC_NA0x00000000);
740 | }
741 | }
742 | break;
743 | case ADSSRVID_READSTATE0x04:
744 | {
745 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsreadstateresponse, tvb, offset, ams_length-offset, ENC_NA0x00000000);
746 | if( ams_length-offset >= TAdsReadStateRes_Len(int)sizeof(TAdsReadStateRes) )
747 | {
748 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsreadstateresponse);
749 | proto_tree_add_item(ams_adstree, hf_ams_adsresult, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
750 | offset += 4;
751 |
752 | proto_tree_add_item(ams_adstree, hf_ams_adsstate, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
753 | offset += 2;
754 |
755 | proto_tree_add_item(ams_adstree, hf_ams_adsdevicestate, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
756 | }
757 | }
758 | break;
759 | case ADSSRVID_WRITECTRL0x05:
760 | {
761 | anItem = proto_tree_add_item(ams_tree, hf_ams_adswritectrlresponse, tvb, offset, ams_length-offset, ENC_NA0x00000000);
762 | if( ams_length-offset >= TAdsWriteControlRes_Len(int)sizeof(TAdsWriteControlRes) )
763 | {
764 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adswritectrlresponse);
765 | proto_tree_add_item(ams_adstree, hf_ams_adsresult, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
766 | }
767 | }
768 | break;
769 | case ADSSRVID_READDEVICEINFO0x01:
770 | {
771 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsreaddinforesponse, tvb, offset, ams_length-offset, ENC_NA0x00000000);
772 | if( ams_length-offset >= TAdsReadDeviceInfoRes_Len(int)sizeof(TAdsReadDeviceInfoRes) )
773 | {
774 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsreaddinforesponse);
775 | proto_tree_add_item(ams_adstree, hf_ams_adsresult, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
776 | offset += 4;
777 |
778 | proto_tree_add_item(ams_adstree, hf_ams_adsversionversion, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
779 | offset += 1;
780 | proto_tree_add_item(ams_adstree, hf_ams_adsversionrevision, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
781 | offset += 1;
782 | proto_tree_add_item(ams_adstree, hf_ams_adsversionbuild, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
783 | offset += 2;
784 |
785 | proto_tree_add_item(ams_adstree, hf_ams_adsdevicename, tvb, offset, ams_length-offset, ENC_ASCII0x00000000);
786 | }
787 | }
788 | break;
789 | case ADSSRVID_ADDDEVICENOTE0x06:
790 | {
791 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsadddnresponse, tvb, offset, ams_length-offset, ENC_NA0x00000000);
792 | if( ams_length-offset >= TAdsAddDeviceNotificationRes_Len(int)sizeof(TAdsAddDeviceNotificationRes) )
793 | {
794 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsadddnresponse);
795 | proto_tree_add_item(ams_adstree, hf_ams_adsresult, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
796 | offset += 4;
797 |
798 | proto_tree_add_item(ams_adstree, hf_ams_adsnotificationhandle, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
799 | }
800 | }
801 | break;
802 | case ADSSRVID_DELDEVICENOTE0x07:
803 | {
804 | anItem = proto_tree_add_item(ams_tree, hf_ams_adsdeldnresponse, tvb, offset, ams_length-offset, ENC_NA0x00000000);
805 | if( ams_length-offset >= TAdsDelDeviceNotificationRes_Len(int)sizeof(TAdsDelDeviceNotificationRes) )
806 | {
807 | ams_adstree = proto_item_add_subtree(anItem, ett_ams_adsdeldnresponse);
808 | proto_tree_add_item(ams_adstree, hf_ams_adsresult, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
809 | }
810 | }
811 | break;
812 | }
813 | }
814 | }
815 | else
816 | {
817 | if ( (stateflags & AMSCMDSF_RESPONSE0x0001) == 0 )
818 | col_append_str(pinfo->cinfo, COL_INFO, "AMS Request");
819 | else
820 | col_append_str(pinfo->cinfo, COL_INFO, "AMS Response");
821 | if (ams_length-offset > 0 )
822 | proto_tree_add_item(ams_tree, hf_ams_data, tvb, offset, ams_length-offset, ENC_NA0x00000000);
823 | }
824 |
825 | return ams_length;
826 | }
827 |
828 |
829 | /*ams*/
830 | static int dissect_ams(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, void *data _U___attribute__((unused)))
831 | {
832 | return dissect_ams_pdu(tvb, pinfo, tree, 0);
833 | }
834 |
835 | static unsigned get_amstcp_length(packet_info* pinfo _U___attribute__((unused)), tvbuff_t* tvb, int offset, void* data _U___attribute__((unused)))
836 | {
837 | // The 6-byte AMS/TCP header is 2 reserved bytes followed by 4 bytes
838 | // indicating the length of the AMS header and data that follows.
839 |
840 | return tvb_get_letohl(tvb, offset + 2) + TcpAdsParserHDR_Len6;
841 | }
842 |
843 | static int dissect_amstcp_reassembled(tvbuff_t* tvb, packet_info* pinfo, proto_tree* tree, void* data _U___attribute__((unused)))
844 | {
845 | return dissect_ams_pdu(tvb, pinfo, tree, TcpAdsParserHDR_Len6);
846 | }
847 |
848 | static int dissect_amstcp(tvbuff_t* tvb, packet_info* pinfo, proto_tree* tree, void* data _U___attribute__((unused)))
849 | {
850 | tcp_dissect_pdus(tvb, pinfo, tree, true1, TcpAdsParserHDR_Len6, get_amstcp_length, dissect_amstcp_reassembled, NULL((void*)0));
851 |
852 | return tvb_captured_length(tvb);
853 | }
854 |
855 | void proto_register_ams(void)
856 | {
857 | static const true_false_string flags_set_truth =
858 | {
859 | "Set",
860 | "Not set"
861 | };
862 |
863 | static hf_register_info hf[] =
864 | {
865 | { &hf_ams_sendernetid,
866 | { "AMS Sender Net Id", "ams.sendernetid",
867 | FT_STRING, BASE_NONE, NULL((void*)0), 0x0,
868 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
869 | },
870 | { &hf_ams_senderport,
871 | { "AMS Sender port", "ams.senderport",
872 | FT_UINT16, BASE_DEC, NULL((void*)0), 0x0,
873 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
874 | },
875 | { &hf_ams_targetnetid,
876 | { "AMS Target Net Id", "ams.targetnetid",
877 | FT_STRING, BASE_NONE, NULL((void*)0), 0x0,
878 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
879 | },
880 | { &hf_ams_targetport,
881 | { "AMS Target port", "ams.targetport",
882 | FT_UINT16, BASE_DEC, NULL((void*)0), 0x0,
883 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
884 | },
885 | { &hf_ams_cmdid,
886 | { "CmdId", "ams.cmdid",
887 | FT_UINT16, BASE_DEC, VALS(AMS_CommandId_vals)((0 ? (const struct _value_string*)0 : ((AMS_CommandId_vals)) )), 0x0,
888 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
889 | },
890 | { &hf_ams_stateflags,
891 | { "StateFlags", "ams.stateflags",
892 | FT_UINT16, BASE_HEX, NULL((void*)0), 0x0,
893 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
894 | },
895 | { &hf_ams_stateresponse,
896 | { "RESPONSE", "ams.state_response",
897 | FT_BOOLEAN, 16, TFS(&flags_set_truth)((0 ? (const struct true_false_string*)0 : ((&flags_set_truth )))), AMSCMDSF_RESPONSE0x0001,
898 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
899 | },
900 | { &hf_ams_statenoreturn,
901 | { "NO RETURN", "ams.state_noreturn",
902 | FT_BOOLEAN, 16, TFS(&flags_set_truth)((0 ? (const struct true_false_string*)0 : ((&flags_set_truth )))), AMSCMDSF_NORETURN0x0002,
903 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
904 | },
905 | { &hf_ams_stateadscmd,
906 | { "ADS COMMAND", "ams.state_adscmd",
907 | FT_BOOLEAN, 16, TFS(&flags_set_truth)((0 ? (const struct true_false_string*)0 : ((&flags_set_truth )))), AMSCMDSF_ADSCMD0x0004,
908 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
909 | },
910 | { &hf_ams_statesyscmd,
911 | { "SYSTEM COMMAND", "ams.state_syscmd",
912 | FT_BOOLEAN, 16, TFS(&flags_set_truth)((0 ? (const struct true_false_string*)0 : ((&flags_set_truth )))), AMSCMDSF_SYSCMD0x0008,
913 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
914 | },
915 | { &hf_ams_statehighprio,
916 | { "HIGH PRIORITY COMMAND", "ams.state_highprio",
917 | FT_BOOLEAN, 16, TFS(&flags_set_truth)((0 ? (const struct true_false_string*)0 : ((&flags_set_truth )))), AMSCMDSF_HIGHPRIO0x0010,
918 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
919 | },
920 | { &hf_ams_statetimestampadded,
921 | { "TIMESTAMP ADDED", "ams.state_timestampadded",
922 | FT_BOOLEAN, 16, TFS(&flags_set_truth)((0 ? (const struct true_false_string*)0 : ((&flags_set_truth )))), AMSCMDSF_TIMESTAMPADDED0x0020,
923 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
924 | },
925 | { &hf_ams_stateudp,
926 | { "UDP COMMAND", "ams.state_udp",
927 | FT_BOOLEAN, 16, TFS(&flags_set_truth)((0 ? (const struct true_false_string*)0 : ((&flags_set_truth )))), AMSCMDSF_UDP0x0040,
928 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
929 | },
930 | { &hf_ams_stateinitcmd,
931 | { "INIT COMMAND", "ams.state_initcmd",
932 | FT_BOOLEAN, 16, TFS(&flags_set_truth)((0 ? (const struct true_false_string*)0 : ((&flags_set_truth )))), AMSCMDSF_INITCMD0x0080,
933 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
934 | },
935 | { &hf_ams_statebroadcast,
936 | { "BROADCAST", "ams.state_broadcast",
937 | FT_BOOLEAN, 16, TFS(&flags_set_truth)((0 ? (const struct true_false_string*)0 : ((&flags_set_truth )))), AMSCMDSF_BROADCAST0x8000,
938 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
939 | },
940 | { &hf_ams_cbdata,
941 | { "cbData", "ams.cbdata",
942 | FT_UINT32, BASE_DEC, NULL((void*)0), 0x0,
943 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
944 | },
945 | { &hf_ams_errorcode,
946 | { "ErrorCode", "ams.errorcode",
947 | FT_UINT32, BASE_HEX, VALS(ErrorCode)((0 ? (const struct _value_string*)0 : ((ErrorCode)))), 0x0,
948 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
949 | },
950 | { &hf_ams_invokeid,
951 | { "InvokeId", "ams.invokeid",
952 | FT_UINT32, BASE_HEX, NULL((void*)0), 0x0,
953 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
954 | },
955 | { &hf_ams_response_in,
956 | { "Response In", "ams.response_in",
957 | FT_FRAMENUM, BASE_NONE, FRAMENUM_TYPE(FT_FRAMENUM_RESPONSE)((gpointer) (glong) (FT_FRAMENUM_RESPONSE)), 0x0,
958 | "The response to this AMS request is in this frame", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
959 | },
960 | { &hf_ams_response_to,
961 | { "Request In", "ams.response_to",
962 | FT_FRAMENUM, BASE_NONE, FRAMENUM_TYPE(FT_FRAMENUM_REQUEST)((gpointer) (glong) (FT_FRAMENUM_REQUEST)), 0x0,
963 | "This is a response to the AMS request in this frame", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
964 | },
965 | { &hf_ams_response_time,
966 | { "Response Time", "ams.response_time",
967 | FT_RELATIVE_TIME, BASE_NONE, NULL((void*)0), 0x0,
968 | "The time between the Request and the Response", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
969 | },
970 | { &hf_ams_adsdata,
971 | { "Data", "ams.ads_data",
972 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
973 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
974 | },
975 | { &hf_ams_data,
976 | { "Data", "ams.data",
977 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
978 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
979 | },
980 | { &hf_ams_adsindexgroup,
981 | { "IndexGroup", "ams.ads_indexgroup",
982 | FT_UINT32, BASE_HEX, NULL((void*)0), 0x0,
983 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
984 | },
985 | { &hf_ams_adsindexoffset,
986 | { "IndexOffset", "ams.ads_indexoffset",
987 | FT_UINT32, BASE_HEX, NULL((void*)0), 0x0,
988 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
989 | },
990 | { &hf_ams_adscblength,
991 | { "CbLength", "ams.ads_cblength",
992 | FT_UINT32, BASE_DEC, NULL((void*)0), 0x0,
993 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
994 | },
995 | { &hf_ams_adsreadrequest,
996 | { "ADS Read Request", "ams.ads_read_req",
997 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
998 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
999 | },
1000 | { &hf_ams_adsreadresponse,
1001 | { "ADS Read Response", "ams.ads_read_res",
1002 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1003 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1004 | },
1005 | { &hf_ams_adsinvokeid,
1006 | { "InvokeId", "ams.ads_invokeid",
1007 | FT_UINT32, BASE_HEX, NULL((void*)0), 0x0,
1008 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1009 | },
1010 | { &hf_ams_adsresult,
1011 | { "Result", "ams.adsresult",
1012 | FT_UINT32, BASE_HEX, VALS(AdsErrorMode)((0 ? (const struct _value_string*)0 : ((AdsErrorMode)))), 0x0,
1013 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1014 | },
1015 | { &hf_ams_adswriterequest,
1016 | { "ADS Write Request", "ams.ads_write_req",
1017 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1018 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1019 | },
1020 | { &hf_ams_adswriteresponse,
1021 | { "ADS Write Response", "ams.ads_write_res",
1022 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1023 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1024 | },
1025 | { &hf_ams_adsreadwriterequest,
1026 | { "ADS ReadWrite Request", "ams.ads_readwrite_req",
1027 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1028 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1029 | },
1030 | { &hf_ams_adsreadwriteresponse,
1031 | { "ADS ReadWrite Response", "ams.ads_readwrite_res",
1032 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1033 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1034 | },
1035 | { &hf_ams_adscbreadlength,
1036 | { "CBReadLength", "ams.ads_cbreadlength",
1037 | FT_UINT32, BASE_DEC, NULL((void*)0), 0x0,
1038 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1039 | },
1040 | { &hf_ams_adscbwritelength,
1041 | { "CBWriteLength", "ams.ads_cbwritelength",
1042 | FT_UINT32, BASE_DEC, NULL((void*)0), 0x0,
1043 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1044 | },
1045 | { &hf_ams_adsstate,
1046 | { "AdsState", "ams.ads_state",
1047 | FT_UINT16, BASE_HEX, NULL((void*)0), 0x0,
1048 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1049 | },
1050 | { &hf_ams_adsdevicestate,
1051 | { "DeviceState", "ams.ads_devicestate",
1052 | FT_UINT16, BASE_HEX, NULL((void*)0), 0x0,
1053 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1054 | },
1055 | { &hf_ams_adsnotificationhandle,
1056 | { "NotificationHandle", "ams.ads_notificationhandle",
1057 | FT_UINT32, BASE_HEX, NULL((void*)0), 0x0,
1058 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1059 | },
1060 | { &hf_ams_adsreadstaterequest,
1061 | { "ADS Read State Request", "ams.ads_readstate_req",
1062 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1063 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1064 | },
1065 | { &hf_ams_adsreadstateresponse,
1066 | { "ADS Read State Response", "ams.ads_readstate_res",
1067 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1068 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1069 | },
1070 | { &hf_ams_adswritectrlrequest,
1071 | { "ADS Write Ctrl Request", "ams.ads_writectrl_req",
1072 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1073 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1074 | },
1075 | { &hf_ams_adswritectrlresponse,
1076 | { "ADS Write Ctrl Response", "ams.ads_writectrl_res",
1077 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1078 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1079 | },
1080 | { &hf_ams_adsreaddinforequest,
1081 | { "ADS Read Device Info Request", "ams.ads_readdinfo_req",
1082 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1083 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1084 | },
1085 | { &hf_ams_adsreaddinforesponse,
1086 | { "ADS Read Device Info Response", "ams.ads_readdinfo_res",
1087 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1088 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1089 | },
1090 | { &hf_ams_adsadddnrequest,
1091 | { "ADS Add Device Notification Request", "ams.ads_adddn_req",
1092 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1093 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1094 | },
1095 | { &hf_ams_adsadddnresponse,
1096 | { "ADS Add Device Notification Response", "ams.ads_adddn_res",
1097 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1098 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1099 | },
1100 | { &hf_ams_adsdeldnrequest,
1101 | { "ADS Delete Device Notification Request", "ams.ads_deldn_req",
1102 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1103 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1104 | },
1105 | { &hf_ams_adsdeldnresponse,
1106 | { "ADS Delete Device Notification Response", "ams.ads_deldn_res",
1107 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1108 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1109 | },
1110 | { &hf_ams_adsdnrequest,
1111 | { "ADS Device Notification Request", "ams.ads_dn_req",
1112 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1113 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1114 | },
1115 | #if 0
1116 | { &hf_ams_adsdnresponse,
1117 | { "ADS Device Notification Response", "ams.ads_dn_res",
1118 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1119 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1120 | },
1121 | { &hf_ams_adsnoteattrib,
1122 | { "InvokeId", "ams.ads_noteattrib",
1123 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1124 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1125 | },
1126 | { &hf_ams_adsnoteblocks,
1127 | { "InvokeId", "ams.ads_noteblocks",
1128 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1129 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1130 | },
1131 | { &hf_ams_adsversion,
1132 | { "ADS Version", "ams.ads_version",
1133 | FT_UINT32, BASE_DEC, NULL((void*)0), 0x0,
1134 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1135 | },
1136 | #endif
1137 | { &hf_ams_adsdevicename,
1138 | { "Device Name","ams.ads_devicename",
1139 | FT_STRING, BASE_NONE, NULL((void*)0), 0x0,
1140 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1141 | },
1142 | { &hf_ams_adsversionversion,
1143 | { "ADS Major Version", "ams.ads_versionversion",
1144 | FT_UINT8, BASE_DEC, NULL((void*)0), 0x0,
1145 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1146 | },
1147 | { &hf_ams_adsversionrevision,
1148 | { "ADS Minor Version", "ams.ads_versionrevision",
1149 | FT_UINT8, BASE_DEC, NULL((void*)0), 0x0,
1150 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1151 | },
1152 | { &hf_ams_adsversionbuild,
1153 | { "ADS Version Build", "ams.ads_versionbuild",
1154 | FT_UINT16, BASE_DEC, NULL((void*)0), 0x0,
1155 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1156 | },
1157 | { &hf_ams_adsnoteblocksstamps,
1158 | { "Count of Stamps", "ams.ads_noteblocksstamps",
1159 | FT_UINT32, BASE_DEC, NULL((void*)0), 0x0,
1160 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1161 | },
1162 | #if 0
1163 | { &hf_ams_adsnoteblocksstamp,
1164 | { "Notification Stamp", "ams.ads_noteblocksstamp",
1165 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1166 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1167 | },
1168 | { &hf_ams_adstimestamp,
1169 | { "Time Stamp", "ams.ads_timestamp",
1170 | FT_UINT64, BASE_DEC, NULL((void*)0), 0x0,
1171 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1172 | },
1173 | { &hf_ams_adssamplecnt,
1174 | { "Count of Stamps", "ams.ads_samplecnt",
1175 | FT_UINT32, BASE_DEC, NULL((void*)0), 0x0,
1176 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1177 | },
1178 | { &hf_ams_adsnoteblockssample,
1179 | { "Notification Sample", "ams.ads_noteblockssample",
1180 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1181 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1182 | },
1183 | #endif
1184 | { &hf_ams_adstransmode,
1185 | { "Trans Mode", "ams.ads_transmode",
1186 | FT_UINT32, BASE_DEC, VALS(TransMode)((0 ? (const struct _value_string*)0 : ((TransMode)))), 0x0,
1187 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1188 | },
1189 | { &hf_ams_adsmaxdelay,
1190 | { "Max Delay", "ams.ads_maxdelay",
1191 | FT_UINT32, BASE_DEC, NULL((void*)0), 0x0,
1192 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1193 | },
1194 | { &hf_ams_adscycletime,
1195 | { "Cycle Time", "ams.ads_cycletime",
1196 | FT_UINT32, BASE_DEC, NULL((void*)0), 0x0,
1197 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1198 | },
1199 | #if 0
1200 | { &hf_ams_adscmpmax,
1201 | { "Cmp Mad", "ams.ads_cmpmax",
1202 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1203 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1204 | },
1205 | { &hf_ams_adscmpmin,
1206 | { "Cmp Min", "ams.ads_cmpmin",
1207 | FT_NONE, BASE_NONE, NULL((void*)0), 0x0,
1208 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
1209 | }
1210 | #endif
1211 | };
1212 |
1213 | static int *ett[] =
1214 | {
1215 | &ett_ams,
1216 | &ett_ams_stateflags,
1217 | &ett_ams_adsreadrequest,
1218 | &ett_ams_adsreadresponse,
1219 | &ett_ams_adswriterequest,
1220 | &ett_ams_adswriteresponse,
1221 | &ett_ams_adsreadwriterequest,
1222 | &ett_ams_adsreadwriteresponse,
1223 | &ett_ams_adsreadstaterequest,
1224 | &ett_ams_adsreadstateresponse,
1225 | &ett_ams_adswritectrlrequest,
1226 | &ett_ams_adswritectrlresponse,
1227 | &ett_ams_adsreaddinforequest,
1228 | &ett_ams_adsreaddinforesponse,
1229 | &ett_ams_adsadddnrequest,
1230 | &ett_ams_adsadddnresponse,
1231 | &ett_ams_adsdeldnrequest,
1232 | &ett_ams_adsdeldnresponse,
1233 | &ett_ams_adsdnrequest
1234 | };
1235 |
1236 | proto_ams = proto_register_protocol("AMS", "AMS", "ams");
1237 | proto_register_field_array(proto_ams, hf, array_length(hf)(sizeof (hf) / sizeof (hf)[0]));
1238 | proto_register_subtree_array(ett, array_length(ett)(sizeof (ett) / sizeof (ett)[0]));
1239 |
1240 | ams_handle = register_dissector("ams", dissect_ams, proto_ams);
1241 | amstcp_handle = register_dissector("ams.tcp", dissect_amstcp, proto_ams );
1242 | }
1243 |
1244 | /* The registration hand-off routing */
1245 |
1246 | void proto_reg_handoff_ams(void)
1247 | {
1248 | dissector_add_uint_range_with_preference("tcp.port", AMS_TCP_PORT_RANGE"48898", amstcp_handle);
1249 | dissector_add_uint("ecatf.type", 2, ams_handle);
1250 | }
1251 |
1252 | /*
1253 | * Editor modelines - https://www.wireshark.org/tools/modelines.html
1254 | *
1255 | * Local Variables:
1256 | * c-basic-offset: 3
1257 | * tab-width: 8
1258 | * indent-tabs-mode: nil
1259 | * End:
1260 | *
1261 | * ex: set shiftwidth=3 tabstop=8 expandtab:
1262 | * :indentSize=3:tabSize=8:noTabs=true:
1263 | */