### Bug Summary

File: | epan/dissectors/packet-oran.c
Warning: | line 3788, column 67 The left operand of '==' is a garbage value

### Annotated Source Code

Press '?' to see keyboard shortcuts

Show analyzer invocation
clang -cc1 -cc1 -triple x86_64-pc-linux-gnu -analyze -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name packet-oran.c -analyzer-checker=core -analyzer-checker=apiModeling -analyzer-checker=unix -analyzer-checker=deadcode -analyzer-checker=security.insecureAPI.UncheckedReturn -analyzer-checker=security.insecureAPI.getpw -analyzer-checker=security.insecureAPI.gets -analyzer-checker=security.insecureAPI.mktemp -analyzer-checker=security.insecureAPI.mkstemp -analyzer-checker=security.insecureAPI.vfork -analyzer-checker=nullability.NullPassedToNonnull -analyzer-checker=nullability.NullReturnedFromNonnull -analyzer-output plist -w -setup-static-analyzer -mrelocation-model pic -pic-level 2 -fhalf-no-semantic-interposition -fno-delete-null-pointer-checks -mframe-pointer=all -relaxed-aliasing -fmath-errno -ffp-contract=on -fno-rounding-math -ffloat16-excess-precision=fast -fbfloat16-excess-precision=fast -mconstructor-aliases -funwind-tables=2 -target-cpu x86-64 -tune-cpu generic -debugger-tuning=gdb -fdebug-compilation-dir=/builds/wireshark/wireshark/build -fcoverage-compilation-dir=/builds/wireshark/wireshark/build -resource-dir /usr/lib/llvm-21/lib/clang/21 -isystem /usr/include/glib-2.0 -isystem /usr/lib/x86_64-linux-gnu/glib-2.0/include -isystem /builds/wireshark/wireshark/epan/dissectors -isystem /builds/wireshark/wireshark/build/epan/dissectors -isystem /usr/include/mit-krb5 -isystem /usr/include/libxml2 -isystem /builds/wireshark/wireshark/epan -D G_DISABLE_DEPRECATED -D G_DISABLE_SINGLE_INCLUDES -D WS_BUILD_DLL -D WS_DEBUG -D WS_DEBUG_UTF_8 -I /builds/wireshark/wireshark/build -I /builds/wireshark/wireshark -I /builds/wireshark/wireshark/include -D _GLIBCXX_ASSERTIONS -internal-isystem /usr/lib/llvm-21/lib/clang/21/include -internal-isystem /usr/local/include -internal-isystem /usr/lib/gcc/x86_64-linux-gnu/14/../../../../x86_64-linux-gnu/include -internal-externc-isystem /usr/include/x86_64-linux-gnu -internal-externc-isystem /include -internal-externc-isystem /usr/include -fmacro-prefix-map=/builds/wireshark/wireshark/= -fmacro-prefix-map=/builds/wireshark/wireshark/build/= -fmacro-prefix-map=../= -Wno-format-truncation -Wno-format-nonliteral -Wno-pointer-sign -std=gnu11 -ferror-limit 19 -fvisibility=hidden -fwrapv -fwrapv-pointer -fstrict-flex-arrays=3 -stack-protector 2 -fstack-clash-protection -fcf-protection=full -fgnuc-version=4.2.1 -fskip-odr-check-in-gmf -fexceptions -fcolor-diagnostics -analyzer-output=html -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -o /builds/wireshark/wireshark/sbout/2025-10-14-100335-3623-1 -x c /builds/wireshark/wireshark/epan/dissectors/packet-oran.c

Keyboard shortcuts:

- Use 'j/k' keys for keyboard navigation
- Use 'Shift+S' to show/hide relevant lines
- Use '?' to toggle this window

Close
Show only relevant lines Show control flow arrows

1 | /* packet-oran.c
2 | * Routines for O-RAN fronthaul UC-plane dissection
3 | * Copyright 2020, Jan Schiefer, Keysight Technologies, Inc.
4 | * Copyright 2020- Martin Mathieson
5 | *
6 | * Wireshark - Network traffic analyzer
7 | * By Gerald Combs <gerald@wireshark.org>
8 | * Copyright 1998 Gerald Combs
9 | *
10 | * SPDX-License-Identifier: GPL-2.0-or-later
11 | */
12 |
13 | /*
14 | * Dissector for the O-RAN Fronthaul CUS protocol specification.
15 | * See https://specifications.o-ran.org/specifications, WG4, Fronthaul Interfaces Workgroup
16 | * The current implementation is based on the ORAN-WG4.CUS.0-v17.01 specification.
17 | * - haven't spotted any differences in v18.00
18 | * Note that other eCPRI message types are handled in packet-ecpri.c
19 | */
20 |
21 | #include <config.h>
22 |
23 | #include <math.h>
24 |
25 | #include <epan/packet.h>
26 | #include <epan/expert.h>
27 | #include <epan/prefs.h>
28 | #include <epan/tap.h>
29 |
30 | #include <epan/tfs.h>
31 |
32 | #include <wsutil/ws_roundup.h>
33 | #include <wsutil/ws_padding_to.h>
34 |
35 | #include "epan/dissectors/packet-oran.h"
36 |
37 | /* N.B. dissector preferences are taking the place of (some) M-plane parameters, so unfortunately it can be
38 | * fiddly to get the preferences into a good state to decode a given capture..
39 | * TODO:
40 | * - for U-Plane, track back to last C-Plane frame for that eAxC
41 | * - use udCompHdr values from C-Plane if not overridden by U-Plane?
42 | * N.B. this matching is tricky see 7.8.1 Coupling of C-Plane and U-Plane
43 | * - Radio transport layer (eCPRI) fragmentation / reassembly
44 | * - Detect/indicate signs of application layer fragmentation?
45 | * - Not handling M-plane setting for "little endian byte order" as applied to IQ samples and beam weights
46 | * - for section extensions, check more constraints (which other extension types appear with them, order)
47 | * - when some section extensions are present, some section header fields are effectively ignored - flag any remaining ("ignored, "shall")?
48 | * - re-order items (decl and hf definitions) to match spec order?
49 | */
50 |
51 | /* Prototypes */
52 | void proto_reg_handoff_oran(void);
53 | void proto_register_oran(void);
54 |
55 | /* Initialize the protocol and registered fields */
56 | static int proto_oran;
57 |
58 | static int oran_tap = -1;
59 |
60 | static int hf_oran_du_port_id;
61 | static int hf_oran_bandsector_id;
62 | static int hf_oran_cc_id;
63 | static int hf_oran_ru_port_id;
64 | static int hf_oran_sequence_id;
65 | static int hf_oran_e_bit;
66 | static int hf_oran_subsequence_id;
67 | static int hf_oran_previous_frame;
68 |
69 |
70 | static int hf_oran_data_direction;
71 | static int hf_oran_payload_version;
72 | static int hf_oran_filter_index;
73 | static int hf_oran_frame_id;
74 | static int hf_oran_subframe_id;
75 | static int hf_oran_slot_id;
76 | static int hf_oran_slot_within_frame;
77 | static int hf_oran_start_symbol_id;
78 | static int hf_oran_numberOfSections;
79 | static int hf_oran_sectionType;
80 |
81 | static int hf_oran_udCompHdr;
82 | static int hf_oran_udCompHdrIqWidth;
83 | static int hf_oran_udCompHdrIqWidth_pref;
84 | static int hf_oran_udCompHdrMeth;
85 | static int hf_oran_udCompHdrMeth_pref;
86 | static int hf_oran_udCompLen;
87 | static int hf_oran_numberOfUEs;
88 | static int hf_oran_timeOffset;
89 | static int hf_oran_frameStructure_fft;
90 | static int hf_oran_frameStructure_subcarrier_spacing;
91 | static int hf_oran_cpLength;
92 | static int hf_oran_timing_header;
93 | static int hf_oran_section_id;
94 | static int hf_oran_rb;
95 | static int hf_oran_symInc;
96 | static int hf_oran_startPrbc;
97 | static int hf_oran_reMask_re1;
98 | static int hf_oran_reMask_re2;
99 | static int hf_oran_reMask_re3;
100 | static int hf_oran_reMask_re4;
101 | static int hf_oran_reMask_re5;
102 | static int hf_oran_reMask_re6;
103 | static int hf_oran_reMask_re7;
104 | static int hf_oran_reMask_re8;
105 | static int hf_oran_reMask_re9;
106 | static int hf_oran_reMask_re10;
107 | static int hf_oran_reMask_re11;
108 | static int hf_oran_reMask_re12;
109 | static int hf_oran_reMask;
110 | static int hf_oran_numPrbc;
111 | static int hf_oran_numSymbol;
112 | static int hf_oran_ef;
113 | static int hf_oran_beamId;
114 |
115 | static int hf_oran_sinrCompHdrIqWidth_pref;
116 | static int hf_oran_sinrCompHdrMeth_pref;
117 |
118 | static int hf_oran_ciCompHdr;
119 | static int hf_oran_ciCompHdrIqWidth;
120 | static int hf_oran_ciCompHdrMeth;
121 | static int hf_oran_ciCompOpt;
122 |
123 | static int hf_oran_extension;
124 | static int hf_oran_exttype;
125 | static int hf_oran_extlen;
126 |
127 | static int hf_oran_bfw_bundle;
128 | static int hf_oran_bfw_bundle_id;
129 | static int hf_oran_bfw;
130 | static int hf_oran_bfw_i;
131 | static int hf_oran_bfw_q;
132 |
133 | static int hf_oran_ueId;
134 | static int hf_oran_freqOffset;
135 | static int hf_oran_regularizationFactor;
136 | static int hf_oran_laaMsgType;
137 | static int hf_oran_laaMsgLen;
138 | static int hf_oran_lbtHandle;
139 | static int hf_oran_lbtDeferFactor;
140 | static int hf_oran_lbtBackoffCounter;
141 | static int hf_oran_lbtOffset;
142 | static int hf_oran_MCOT;
143 | static int hf_oran_lbtMode;
144 | static int hf_oran_sfnSfEnd;
145 | static int hf_oran_lbtPdschRes;
146 | static int hf_oran_sfStatus;
147 | static int hf_oran_initialPartialSF;
148 | static int hf_oran_lbtDrsRes;
149 | static int hf_oran_lbtBufErr;
150 | static int hf_oran_lbtTrafficClass;
151 | static int hf_oran_lbtCWConfig_H;
152 | static int hf_oran_lbtCWConfig_T;
153 | static int hf_oran_lbtCWR_Rst;
154 |
155 | static int hf_oran_reserved;
156 | static int hf_oran_reserved_1bit;
157 | static int hf_oran_reserved_2bits;
158 | static int hf_oran_reserved_3bits;
159 | static int hf_oran_reserved_4bits;
160 | static int hf_oran_reserved_last_4bits;
161 | static int hf_oran_reserved_last_5bits;
162 | static int hf_oran_reserved_6bits;
163 | static int hf_oran_reserved_last_6bits;
164 | static int hf_oran_reserved_7bits;
165 | static int hf_oran_reserved_last_7bits;
166 | static int hf_oran_reserved_8bits;
167 | static int hf_oran_reserved_16bits;
168 | static int hf_oran_reserved_15bits;
169 | static int hf_oran_reserved_bit1;
170 | static int hf_oran_reserved_bit2;
171 | static int hf_oran_reserved_bit4;
172 | static int hf_oran_reserved_bit5;
173 | static int hf_oran_reserved_bits123;
174 | static int hf_oran_reserved_bits456;
175 |
176 | static int hf_oran_bundle_offset;
177 | static int hf_oran_cont_ind;
178 |
179 | static int hf_oran_bfwCompHdr;
180 | static int hf_oran_bfwCompHdr_iqWidth;
181 | static int hf_oran_bfwCompHdr_compMeth;
182 | static int hf_oran_symbolId;
183 | static int hf_oran_startPrbu;
184 | static int hf_oran_numPrbu;
185 |
186 | static int hf_oran_udCompParam;
187 | static int hf_oran_sReSMask;
188 | static int hf_oran_sReSMask_re12;
189 | static int hf_oran_sReSMask_re11;
190 | static int hf_oran_sReSMask_re10;
191 | static int hf_oran_sReSMask_re9;
192 | static int hf_oran_sReSMask_re8;
193 | static int hf_oran_sReSMask_re7;
194 | static int hf_oran_sReSMask_re6;
195 | static int hf_oran_sReSMask_re5;
196 | static int hf_oran_sReSMask_re4;
197 | static int hf_oran_sReSMask_re3;
198 | static int hf_oran_sReSMask_re2;
199 | static int hf_oran_sReSMask_re1;
200 |
201 | static int hf_oran_sReSMask1;
202 | static int hf_oran_sReSMask2;
203 | static int hf_oran_sReSMask1_2_re12;
204 | static int hf_oran_sReSMask1_2_re11;
205 | static int hf_oran_sReSMask1_2_re10;
206 | static int hf_oran_sReSMask1_2_re9;
207 |
208 | static int hf_oran_bfwCompParam;
209 |
210 | static int hf_oran_iSample;
211 | static int hf_oran_qSample;
212 |
213 | static int hf_oran_ciCompParam;
214 |
215 | static int hf_oran_blockScaler;
216 | static int hf_oran_compBitWidth;
217 | static int hf_oran_compShift;
218 |
219 | static int hf_oran_active_beamspace_coefficient_n1;
220 | static int hf_oran_active_beamspace_coefficient_n2;
221 | static int hf_oran_active_beamspace_coefficient_n3;
222 | static int hf_oran_active_beamspace_coefficient_n4;
223 | static int hf_oran_active_beamspace_coefficient_n5;
224 | static int hf_oran_active_beamspace_coefficient_n6;
225 | static int hf_oran_active_beamspace_coefficient_n7;
226 | static int hf_oran_active_beamspace_coefficient_n8;
227 | static int hf_oran_activeBeamspaceCoefficientMask;
228 | static int hf_oran_activeBeamspaceCoefficientMask_bits_set;
229 |
230 | static int hf_oran_se6_repetition;
231 |
232 | static int hf_oran_rbgSize;
233 | static int hf_oran_rbgMask;
234 | static int hf_oran_noncontig_priority;
235 |
236 | static int hf_oran_symbol_mask;
237 | static int hf_oran_symbol_mask_s13;
238 | static int hf_oran_symbol_mask_s12;
239 | static int hf_oran_symbol_mask_s11;
240 | static int hf_oran_symbol_mask_s10;
241 | static int hf_oran_symbol_mask_s9;
242 | static int hf_oran_symbol_mask_s8;
243 | static int hf_oran_symbol_mask_s7;
244 | static int hf_oran_symbol_mask_s6;
245 | static int hf_oran_symbol_mask_s5;
246 | static int hf_oran_symbol_mask_s4;
247 | static int hf_oran_symbol_mask_s3;
248 | static int hf_oran_symbol_mask_s2;
249 | static int hf_oran_symbol_mask_s1;
250 | static int hf_oran_symbol_mask_s0;
251 |
252 | static int hf_oran_exponent;
253 | static int hf_oran_iq_user_data;
254 |
255 | static int hf_oran_disable_bfws;
256 | static int hf_oran_rad;
257 | static int hf_oran_num_bund_prbs;
258 | static int hf_oran_beam_id;
259 | static int hf_oran_num_weights_per_bundle;
260 |
261 | static int hf_oran_ack_nack_req_id;
262 |
263 | static int hf_oran_frequency_range;
264 | static int hf_oran_off_start_prb;
265 | static int hf_oran_num_prb;
266 |
267 | static int hf_oran_samples_prb;
268 | static int hf_oran_ciSample;
269 | static int hf_oran_ciIsample;
270 | static int hf_oran_ciQsample;
271 |
272 | static int hf_oran_beamGroupType;
273 | static int hf_oran_numPortc;
274 |
275 | static int hf_oran_csf;
276 | static int hf_oran_modcompscaler;
277 |
278 | static int hf_oran_modcomp_param_set;
279 | static int hf_oran_mc_scale_re_mask;
280 | static int hf_oran_mc_scale_offset;
281 |
282 | static int hf_oran_eAxC_mask;
283 | static int hf_oran_technology;
284 | static int hf_oran_nullLayerInd;
285 |
286 | static int hf_oran_se19_repetition;
287 | static int hf_oran_portReMask;
288 | static int hf_oran_portSymbolMask;
289 |
290 | static int hf_oran_ext19_port;
291 |
292 | static int hf_oran_prb_allocation;
293 | static int hf_oran_nextSymbolId;
294 | static int hf_oran_nextStartPrbc;
295 |
296 | static int hf_oran_puncPattern;
297 | static int hf_oran_numPuncPatterns;
298 | static int hf_oran_symbolMask_ext20;
299 | static int hf_oran_startPuncPrb;
300 | static int hf_oran_numPuncPrb;
301 | static int hf_oran_puncReMask;
302 | static int hf_oran_multiSDScope;
303 | static int hf_oran_RbgIncl;
304 |
305 | static int hf_oran_ci_prb_group_size;
306 | static int hf_oran_prg_size_st5;
307 | static int hf_oran_prg_size_st6;
308 |
309 | static int hf_oran_num_ueid;
310 |
311 | static int hf_oran_antMask;
312 |
313 | static int hf_oran_transmissionWindowOffset;
314 | static int hf_oran_transmissionWindowSize;
315 | static int hf_oran_toT;
316 |
317 | static int hf_oran_bfaCompHdr;
318 | static int hf_oran_bfAzPtWidth;
319 | static int hf_oran_bfZePtWidth;
320 | static int hf_oran_bfAz3ddWidth;
321 | static int hf_oran_bfZe3ddWidth;
322 | static int hf_oran_bfAzPt;
323 | static int hf_oran_bfZePt;
324 | static int hf_oran_bfAz3dd;
325 | static int hf_oran_bfZe3dd;
326 | static int hf_oran_bfAzSl;
327 | static int hf_oran_bfZeSl;
328 |
329 | static int hf_oran_cmd_scope;
330 | static int hf_oran_number_of_st4_cmds;
331 |
332 | static int hf_oran_st4_cmd_header;
333 | static int hf_oran_st4_cmd_type;
334 | static int hf_oran_st4_cmd_len;
335 | static int hf_oran_st4_cmd_num_slots;
336 | static int hf_oran_st4_cmd_ack_nack_req_id;
337 |
338 | static int hf_oran_st4_cmd;
339 |
340 | static int hf_oran_sleepmode_trx;
341 | static int hf_oran_sleepmode_asm;
342 | static int hf_oran_log2maskbits;
343 | static int hf_oran_num_slots_ext;
344 | static int hf_oran_antMask_trx_control;
345 |
346 | static int hf_oran_ready;
347 | static int hf_oran_number_of_acks;
348 | static int hf_oran_number_of_nacks;
349 | static int hf_oran_ackid;
350 | static int hf_oran_nackid;
351 |
352 | static int hf_oran_acknack_request_frame;
353 | static int hf_oran_acknack_request_time;
354 | static int hf_oran_acknack_request_type;
355 | static int hf_oran_acknack_response_frame;
356 | static int hf_oran_acknack_response_time;
357 |
358 | static int hf_oran_disable_tdbfns;
359 | static int hf_oran_td_beam_group;
360 | static int hf_oran_disable_tdbfws;
361 | static int hf_oran_td_beam_num;
362 |
363 | static int hf_oran_dir_pattern;
364 | static int hf_oran_guard_pattern;
365 |
366 | static int hf_oran_ecpri_pcid;
367 | static int hf_oran_ecpri_rtcid;
368 | static int hf_oran_ecpri_seqid;
369 |
370 | static int hf_oran_num_sym_prb_pattern;
371 | static int hf_oran_prb_mode;
372 | static int hf_oran_sym_prb_pattern;
373 | static int hf_oran_sym_mask;
374 | static int hf_oran_num_mc_scale_offset;
375 | static int hf_oran_prb_pattern;
376 | static int hf_oran_prb_block_offset;
377 | static int hf_oran_prb_block_size;
378 |
379 | static int hf_oran_codebook_index;
380 | static int hf_oran_layerid;
381 | static int hf_oran_numlayers;
382 | static int hf_oran_txscheme;
383 | static int hf_oran_crs_remask;
384 | static int hf_oran_crs_shift;
385 | static int hf_oran_crs_symnum;
386 | static int hf_oran_beamid_ap1;
387 | static int hf_oran_beamid_ap2;
388 | static int hf_oran_beamid_ap3;
389 |
390 | static int hf_oran_port_list_index;
391 | static int hf_oran_alpn_per_sym;
392 | static int hf_oran_ant_dmrs_snr;
393 | static int hf_oran_user_group_size;
394 | static int hf_oran_user_group_id;
395 | static int hf_oran_entry_type;
396 | static int hf_oran_dmrs_port_number;
397 | static int hf_oran_ueid_reset;
398 |
399 | static int hf_oran_dmrs_symbol_mask;
400 | static int hf_oran_dmrs_symbol_mask_s13;
401 | static int hf_oran_dmrs_symbol_mask_s12;
402 | static int hf_oran_dmrs_symbol_mask_s11;
403 | static int hf_oran_dmrs_symbol_mask_s10;
404 | static int hf_oran_dmrs_symbol_mask_s9;
405 | static int hf_oran_dmrs_symbol_mask_s8;
406 | static int hf_oran_dmrs_symbol_mask_s7;
407 | static int hf_oran_dmrs_symbol_mask_s6;
408 | static int hf_oran_dmrs_symbol_mask_s5;
409 | static int hf_oran_dmrs_symbol_mask_s4;
410 | static int hf_oran_dmrs_symbol_mask_s3;
411 | static int hf_oran_dmrs_symbol_mask_s2;
412 | static int hf_oran_dmrs_symbol_mask_s1;
413 | static int hf_oran_dmrs_symbol_mask_s0;
414 |
415 | static int hf_oran_scrambling;
416 | static int hf_oran_nscid;
417 | static int hf_oran_dtype;
418 | static int hf_oran_cmd_without_data;
419 | static int hf_oran_lambda;
420 | static int hf_oran_first_prb;
421 | static int hf_oran_last_prb;
422 | static int hf_oran_low_papr_type;
423 | static int hf_oran_hopping_mode;
424 |
425 | static int hf_oran_tx_win_for_on_air_symbol_l;
426 | static int hf_oran_tx_win_for_on_air_symbol_r;
427 |
428 | static int hf_oran_num_fo_fb;
429 | static int hf_oran_freq_offset_fb;
430 |
431 | static int hf_oran_num_ue_sinr_rpt;
432 | static int hf_oran_num_sinr_per_prb;
433 | static int hf_oran_num_sinr_per_prb_right;
434 |
435 | static int hf_oran_sinr_value;
436 |
437 | static int hf_oran_measurement_report;
438 | static int hf_oran_mf;
439 | static int hf_oran_meas_data_size;
440 | static int hf_oran_meas_type_id;
441 | static int hf_oran_ipn_power;
442 | static int hf_oran_ue_tae;
443 | static int hf_oran_ue_layer_power;
444 | static int hf_oran_num_elements;
445 | static int hf_oran_ant_dmrs_snr_val;
446 | static int hf_oran_ue_freq_offset;
447 |
448 | static int hf_oran_measurement_command;
449 |
450 | static int hf_oran_beam_type;
451 | static int hf_oran_meas_cmd_size;
452 |
453 | static int hf_oran_symbol_reordering_layer;
454 | static int hf_oran_dmrs_entry;
455 |
456 | static int hf_oran_c_section_common;
457 | static int hf_oran_c_section;
458 | static int hf_oran_u_section;
459 |
460 | static int hf_oran_u_section_ul_symbol_time;
461 | static int hf_oran_u_section_ul_symbol_frames;
462 | static int hf_oran_u_section_ul_symbol_first_frame;
463 | static int hf_oran_u_section_ul_symbol_last_frame;
464 |
465 | /* Computed fields */
466 | static int hf_oran_c_eAxC_ID;
467 | static int hf_oran_refa;
468 |
469 | /* Convenient fields for filtering, mostly shown as hidden */
470 | static int hf_oran_cplane;
471 | static int hf_oran_uplane;
472 | static int hf_oran_bf; /* to match frames that configure beamforming in any way */
473 | static int hf_oran_zero_prb;
474 |
475 | static int hf_oran_ul_cplane_ud_comp_hdr_frame;
476 |
477 | /* Initialize the subtree pointers */
478 | static int ett_oran;
479 | static int ett_oran_ecpri_rtcid;
480 | static int ett_oran_ecpri_pcid;
481 | static int ett_oran_ecpri_seqid;
482 | static int ett_oran_section;
483 | static int ett_oran_section_type;
484 | static int ett_oran_u_timing;
485 | static int ett_oran_u_section;
486 | static int ett_oran_u_prb;
487 | static int ett_oran_iq;
488 | static int ett_oran_bfw_bundle;
489 | static int ett_oran_bfw;
490 | static int ett_oran_frequency_range;
491 | static int ett_oran_prb_cisamples;
492 | static int ett_oran_cisample;
493 | static int ett_oran_udcomphdr;
494 | static int ett_oran_udcompparam;
495 | static int ett_oran_cicomphdr;
496 | static int ett_oran_cicompparam;
497 | static int ett_oran_bfwcomphdr;
498 | static int ett_oran_bfwcompparam;
499 | static int ett_oran_ext19_port;
500 | static int ett_oran_prb_allocation;
501 | static int ett_oran_punc_pattern;
502 | static int ett_oran_bfacomphdr;
503 | static int ett_oran_modcomp_param_set;
504 | static int ett_oran_st4_cmd_header;
505 | static int ett_oran_st4_cmd;
506 | static int ett_oran_sym_prb_pattern;
507 | static int ett_oran_measurement_report;
508 | static int ett_oran_measurement_command;
509 | static int ett_oran_sresmask;
510 | static int ett_oran_c_section_common;
511 | static int ett_oran_c_section;
512 | static int ett_oran_remask;
513 | static int ett_oran_symbol_reordering_layer;
514 | static int ett_oran_dmrs_entry;
515 | static int ett_oran_dmrs_symbol_mask;
516 | static int ett_oran_symbol_mask;
517 | static int ett_active_beamspace_coefficient_mask;
518 |
519 |
520 | /* Don't want all extensions to open and close together. Use extType-1 entry */
521 | static int ett_oran_c_section_extension[HIGHEST_EXTTYPE28];
522 |
523 | /* Expert info */
524 | static expert_field ei_oran_unsupported_bfw_compression_method;
525 | static expert_field ei_oran_invalid_sample_bit_width;
526 | static expert_field ei_oran_reserved_numBundPrb;
527 | static expert_field ei_oran_extlen_wrong;
528 | static expert_field ei_oran_invalid_eaxc_bit_width;
529 | static expert_field ei_oran_extlen_zero;
530 | static expert_field ei_oran_rbg_size_reserved;
531 | static expert_field ei_oran_frame_length;
532 | static expert_field ei_oran_numprbc_ext21_zero;
533 | static expert_field ei_oran_ci_prb_group_size_reserved;
534 | static expert_field ei_oran_st8_nackid;
535 | static expert_field ei_oran_st4_no_cmds;
536 | static expert_field ei_oran_st4_zero_len_cmd;
537 | static expert_field ei_oran_st4_wrong_len_cmd;
538 | static expert_field ei_oran_st4_unknown_cmd;
539 | static expert_field ei_oran_mcot_out_of_range;
540 | static expert_field ei_oran_se10_unknown_beamgrouptype;
541 | static expert_field ei_oran_se10_not_allowed;
542 | static expert_field ei_oran_start_symbol_id_not_zero;
543 | static expert_field ei_oran_trx_control_cmd_scope;
544 | static expert_field ei_oran_unhandled_se;
545 | static expert_field ei_oran_bad_symbolmask;
546 | static expert_field ei_oran_numslots_not_zero;
547 | static expert_field ei_oran_version_unsupported;
548 | static expert_field ei_oran_laa_msg_type_unsupported;
549 | static expert_field ei_oran_se_on_unsupported_st;
550 | static expert_field ei_oran_cplane_unexpected_sequence_number_ul;
551 | static expert_field ei_oran_cplane_unexpected_sequence_number_dl;
552 | static expert_field ei_oran_uplane_unexpected_sequence_number_ul;
553 | static expert_field ei_oran_uplane_unexpected_sequence_number_dl;
554 | static expert_field ei_oran_acknack_no_request;
555 | static expert_field ei_oran_udpcomphdr_should_be_zero;
556 | static expert_field ei_oran_radio_fragmentation_c_plane;
557 | static expert_field ei_oran_radio_fragmentation_u_plane;
558 | static expert_field ei_oran_lastRbdid_out_of_range;
559 | static expert_field ei_oran_rbgMask_beyond_last_rbdid;
560 | static expert_field ei_oran_unexpected_measTypeId;
561 | static expert_field ei_oran_unsupported_compression_method;
562 | static expert_field ei_oran_ud_comp_len_wrong_size;
563 | static expert_field ei_oran_sresmask2_not_zero_with_rb;
564 | static expert_field ei_oran_st6_rb_shall_be_0;
565 | static expert_field ei_oran_st9_not_ul;
566 | static expert_field ei_oran_st10_numsymbol_not_14;
567 | static expert_field ei_oran_st10_startsymbolid_not_0;
568 | static expert_field ei_oran_st10_not_ul;
569 | static expert_field ei_oran_se24_nothing_to_inherit;
570 | static expert_field ei_oran_num_sinr_per_prb_unknown;
571 | static expert_field ei_oran_start_symbol_id_bits_ignored;
572 | static expert_field ei_oran_user_group_id_reserved_value;
573 | static expert_field ei_oran_port_list_index_zero;
574 | static expert_field ei_oran_ul_uplane_symbol_too_long;
575 |
576 |
577 | /* These are the message types handled by this dissector */
578 | #define ECPRI_MT_IQ_DATA0 0
579 | #define ECPRI_MT_RT_CTRL_DATA2 2
580 |
581 |
582 | /* Preference settings - try to set reasonable defaults */
583 | static unsigned pref_du_port_id_bits = 4;
584 | static unsigned pref_bandsector_id_bits = 4;
585 | static unsigned pref_cc_id_bits = 4;
586 | static unsigned pref_ru_port_id_bits = 4;
587 |
588 | /* TODO: ideally should be per-flow */
589 | static unsigned pref_sample_bit_width_uplink = 14;
590 | static unsigned pref_sample_bit_width_downlink = 14;
591 | static unsigned pref_sample_bit_width_sinr = 14;
592 |
593 | /* 8.3.3.15 Compression schemes */
594 | #define COMP_NONE0 0
595 | #define COMP_BLOCK_FP1 1
596 | #define COMP_BLOCK_SCALE2 2
597 | #define COMP_U_LAW3 3
598 | #define COMP_MODULATION4 4
599 | #define BFP_AND_SELECTIVE_RE5 5
600 | #define MOD_COMPR_AND_SELECTIVE_RE6 6
601 | #define BFP_AND_SELECTIVE_RE_WITH_MASKS7 7
602 | #define MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8 8
603 |
604 | /* TODO: these ideally should be per-flow too */
605 | static int pref_iqCompressionUplink = COMP_BLOCK_FP1;
606 | static int pref_iqCompressionDownlink = COMP_BLOCK_FP1;
607 |
608 | static int pref_iqCompressionSINR = COMP_BLOCK_FP1;
609 |
610 |
611 | /* Is udCompHeader present (both directions) */
612 | static int pref_includeUdCompHeaderUplink = 2; /* start heuristic */
613 | static int pref_includeUdCompHeaderDownlink = 2; /* start heuristic */
614 |
615 | static unsigned pref_data_plane_section_total_rbs = 273;
616 | static unsigned pref_num_bf_antennas = 32;
617 | static bool_Bool pref_showIQSampleValues = true1;
618 |
619 | /* Based upon m-plane param, so will be system-wide */
620 | static int pref_support_udcompLen = 2; /* start heuristic, can force other settings if necessary */
621 | static bool_Bool udcomplen_heuristic_result_set = false0;
622 | static bool_Bool udcomplen_heuristic_result = false0;
623 |
624 | /* st6-4byte-alignment-required */
625 | static bool_Bool st6_4byte_alignment = false0;
626 |
627 | /* Requested, allows I/Q to be stored as integers.. */
628 | static bool_Bool show_unscaled_values = false0;
629 |
630 | /* Initialized off. Timing is in microseconds. */
631 | static unsigned us_allowed_for_ul_in_symbol = 0;
632 |
633 | static const enum_val_t dl_compression_options[] = {
634 | { "COMP_NONE", "No Compression", COMP_NONE0 },
635 | { "COMP_BLOCK_FP", "Block Floating Point Compression", COMP_BLOCK_FP1 },
636 | { "COMP_BLOCK_SCALE", "Block Scaling Compression", COMP_BLOCK_SCALE2 },
637 | { "COMP_U_LAW", "u-Law Compression", COMP_U_LAW3 },
638 | { "COMP_MODULATION", "Modulation Compression", COMP_MODULATION4 },
639 | { "BFP_AND_SELECTIVE_RE", "Block Floating Point + selective RE sending", BFP_AND_SELECTIVE_RE5 },
640 | { "MOD_COMPR_AND_SELECTIVE_RE", "Modulation Compression + selective RE sending", MOD_COMPR_AND_SELECTIVE_RE6 },
641 | { "BFP_AND_SELECTIVE_RE_WITH_MASKS", "Block Floating Point + selective RE sending with masks in section header", BFP_AND_SELECTIVE_RE_WITH_MASKS7 },
642 | { "MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS", "Modulation Compression + selective RE sending with masks in section header", MOD_COMPR_AND_SELECTIVE_RE6 },
643 | { NULL((void*)0), NULL((void*)0), 0 }
644 | };
645 |
646 | static const enum_val_t ul_compression_options[] = {
647 | { "COMP_NONE", "No Compression", COMP_NONE0 },
648 | { "COMP_BLOCK_FP", "Block Floating Point Compression", COMP_BLOCK_FP1 },
649 | { "COMP_BLOCK_SCALE", "Block Scaling Compression", COMP_BLOCK_SCALE2 },
650 | { "COMP_U_LAW", "u-Law Compression", COMP_U_LAW3 },
651 | { "BFP_AND_SELECTIVE_RE", "Block Floating Point + selective RE sending", BFP_AND_SELECTIVE_RE5 },
652 | { "BFP_AND_SELECTIVE_RE_WITH_MASKS", "Block Floating Point + selective RE sending with masks in section header", BFP_AND_SELECTIVE_RE_WITH_MASKS7 },
653 | { NULL((void*)0), NULL((void*)0), 0 }
654 | };
655 |
656 | static const enum_val_t udcomplen_support_options[] = {
657 | { "NOT_SUPPORTED", "Not Supported", 0 },
658 | { "SUPPORTED", "Supported", 1 },
659 | { "HEURISTIC", "Attempt Heuristic", 2 },
660 | { NULL((void*)0), NULL((void*)0), 0 }
661 | };
662 |
663 | static const enum_val_t udcomphdr_present_options[] = {
664 | { "NOT_PRESENT", "Not Present", 0 },
665 | { "PRESENT", "Present", 1 },
666 | { "HEURISTIC", "Attempt Heuristic", 2 },
667 | { NULL((void*)0), NULL((void*)0), 0 }
668 | };
669 |
670 |
671 |
672 | static const value_string e_bit[] = {
673 | { 0, "More fragments follow" },
674 | { 1, "Last fragment" },
675 | { 0, NULL((void*)0)}
676 | };
677 |
678 | #define DIR_UPLINK0 0
679 | #define DIR_DOWNLINK1 1
680 |
681 |
682 | static const value_string data_direction_vals[] = {
683 | { DIR_UPLINK0, "Uplink" }, /* gNB Rx */
684 | { DIR_DOWNLINK1, "Downlink" }, /* gNB Tx */
685 | { 0, NULL((void*)0)}
686 | };
687 |
688 | static const value_string rb_vals[] = {
689 | { 0, "Every RB used" },
690 | { 1, "Every other RB used" },
691 | { 0, NULL((void*)0)}
692 | };
693 |
694 | static const value_string sym_inc_vals[] = {
695 | { 0, "Use the current symbol number" },
696 | { 1, "Increment the current symbol number" },
697 | { 0, NULL((void*)0)}
698 | };
699 |
700 | static const value_string lbtMode_vals[] = {
701 | { 0, "Full LBT (regular LBT, sending reservation signal until the beginning of the SF/slot)" },
702 | { 1, "Partial LBT (looking back 25 usec prior to transmission" },
703 | { 2, "Partial LBT (looking back 34 usec prior to transmission" },
704 | { 3, "Full LBT and stop (regular LBT, without sending reservation signal" },
705 | { 0, NULL((void*)0)}
706 | };
707 |
708 | static const range_string filter_indices[] = {
709 | {0, 0, "standard channel filter"},
710 | {1, 1, "UL filter for PRACH preamble formats 0, 1, 2; min. passband 839 x 1.25kHz = 1048.75 kHz"},
711 | {2, 2, "UL filter for PRACH preamble format 3, min. passband 839 x 5 kHz = 4195 kHz"},
712 | {3, 3, "UL filter for PRACH preamble formats A1, A2, A3, B1, B2, B3, B4, C0, C2; min. passband 139 x \u0394fRA"},
713 | {4, 4, "UL filter for NPRACH 0, 1; min. passband 48 x 3.75KHz = 180 KHz"},
714 | {5, 5, "UL filter for PRACH preamble formats"},
715 | {8, 8, "UL filter NPUSCH"},
716 | {9, 9, "Mixed numerology and other channels except PRACH and NB-IoT"},
717 | {9, 15, "Reserved"},
718 | {0, 0, NULL((void*)0)}
719 | };
720 |
721 | static const range_string section_types[] = {
722 | { SEC_C_UNUSED_RB, SEC_C_UNUSED_RB, "Unused Resource Blocks or symbols in Downlink or Uplink" },
723 | { SEC_C_NORMAL, SEC_C_NORMAL, "Most DL/UL radio channels" },
724 | { SEC_C_RSVD2, SEC_C_RSVD2, "Reserved for future use" },
725 | { SEC_C_PRACH, SEC_C_PRACH, "PRACH and mixed-numerology channels" },
726 | { SEC_C_SLOT_CONTROL, SEC_C_SLOT_CONTROL, "Slot Configuration Control" },
727 | { SEC_C_UE_SCHED, SEC_C_UE_SCHED, "UE scheduling information (UE-ID assignment to section)" },
728 | { SEC_C_CH_INFO, SEC_C_CH_INFO, "Channel information" },
729 | { SEC_C_LAA, SEC_C_LAA, "LAA (License Assisted Access)" },
730 | { SEC_C_ACK_NACK_FEEDBACK, SEC_C_ACK_NACK_FEEDBACK, "ACK/NACK Feedback" },
731 | { SEC_C_SINR_REPORTING, SEC_C_SINR_REPORTING, "SINR Reporting" },
732 | { SEC_C_RRM_MEAS_REPORTS, SEC_C_RRM_MEAS_REPORTS, "RRM Measurement Reports" },
733 | { SEC_C_REQUEST_RRM_MEAS, SEC_C_REQUEST_RRM_MEAS, "Request RRM Measurements" },
734 | { 12, 255, "Reserved for future use" },
735 | { 0, 0, NULL((void*)0)} };
736 |
737 | static const range_string section_types_short[] = {
738 | { SEC_C_UNUSED_RB, SEC_C_UNUSED_RB, "(Unused RBs) " },
739 | { SEC_C_NORMAL, SEC_C_NORMAL, "(Most channels) " },
740 | { SEC_C_RSVD2, SEC_C_RSVD2, "(reserved) " },
741 | { SEC_C_PRACH, SEC_C_PRACH, "(PRACH/mixed-\u03bc)" },
742 | { SEC_C_SLOT_CONTROL, SEC_C_SLOT_CONTROL, "(Slot info) " },
743 | { SEC_C_UE_SCHED, SEC_C_UE_SCHED, "(UE scheduling info)" },
744 | { SEC_C_CH_INFO, SEC_C_CH_INFO, "(Channel info) " },
745 | { SEC_C_LAA, SEC_C_LAA, "(LAA) " },
746 | { SEC_C_ACK_NACK_FEEDBACK, SEC_C_ACK_NACK_FEEDBACK, "(ACK/NACK) " },
747 | { SEC_C_SINR_REPORTING, SEC_C_SINR_REPORTING, "(SINR Reporting) " },
748 | { SEC_C_RRM_MEAS_REPORTS, SEC_C_RRM_MEAS_REPORTS, "(RRM Meas Reports) " },
749 | { SEC_C_REQUEST_RRM_MEAS, SEC_C_REQUEST_RRM_MEAS, "(Req RRM Meas) " },
750 | { 12, 255, "Reserved for future use" },
751 | { 0, 0, NULL((void*)0) }
752 | };
753 |
754 | static const range_string ud_comp_header_width[] = {
755 | {0, 0, "I and Q are each 16 bits wide"},
756 | {1, 15, "Bit width of I and Q"},
757 | {0, 0, NULL((void*)0)} };
758 |
759 | /* Table 8.3.3.13-3 */
760 | static const range_string ud_comp_header_meth[] = {
761 | {COMP_NONE0, COMP_NONE0, "No compression" },
762 | {COMP_BLOCK_FP1, COMP_BLOCK_FP1, "Block floating point compression" },
763 | {COMP_BLOCK_SCALE2, COMP_BLOCK_SCALE2, "Block scaling" },
764 | {COMP_U_LAW3, COMP_U_LAW3, "Mu - law" },
765 | {COMP_MODULATION4, COMP_MODULATION4, "Modulation compression" },
766 | {BFP_AND_SELECTIVE_RE5, BFP_AND_SELECTIVE_RE5, "BFP + selective RE sending" },
767 | {MOD_COMPR_AND_SELECTIVE_RE6, MOD_COMPR_AND_SELECTIVE_RE6, "mod-compr + selective RE sending" },
768 | {BFP_AND_SELECTIVE_RE_WITH_MASKS7, BFP_AND_SELECTIVE_RE_WITH_MASKS7, "BFP + selective RE sending with masks in section header" },
769 | {MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8, MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8, "mod-compr + selective RE sending with masks in section header"},
770 | {9, 15, "Reserved"},
771 | {0, 0, NULL((void*)0)}
772 | };
773 |
774 | /* Table 7.5.2.13-2 */
775 | static const range_string frame_structure_fft[] = {
776 | {0, 0, "Reserved (no FFT/iFFT processing)"},
777 | {1, 3, "Reserved"},
778 | {4, 4, "FFT size 16"},
779 | {5, 5, "FFT size 32"},
780 | {6, 6, "FFT size 64"},
781 | {7, 7, "FFT size 128"},
782 | {8, 8, "FFT size 256"},
783 | {9, 9, "FFT size 512"},
784 | {10, 10, "FFT size 1024"},
785 | {11, 11, "FFT size 2048"},
786 | {12, 12, "FFT size 4096"},
787 | {13, 13, "FFT size 1536"},
788 | {14, 14, "FFT size 3072"},
789 | {15, 15, "Reserved"},
790 | {0, 0, NULL((void*)0)}
791 | };
792 |
793 | /* Table 7.5.2.13-3 */
794 | static const range_string subcarrier_spacings[] = {
795 | { 0, 0, "SCS 15 kHz, 1 slot/subframe, slot length 1 ms" },
796 | { 1, 1, "SCS 30 kHz, 2 slots/subframe, slot length 500 \u03bcs" },
797 | { 2, 2, "SCS 60 kHz, 4 slots/subframe, slot length 250 \u03bcs" },
798 | { 3, 3, "SCS 120 kHz, 8 slots/subframe, slot length 125 \u03bcs" },
799 | { 4, 4, "SCS 240 kHz, 16 slots/subframe, slot length 62.5 \u03bcs" },
800 | { 5, 11, "Reserved" }, /* N.B., 5 was 480kHz in early spec versions */
801 | { 12, 12, "SCS 1.25 kHz, 1 slot/subframe, slot length 1 ms" },
802 | { 13, 13, "SCS 3.75 kHz(LTE - specific), 1 slot/subframe, slot length 1 ms" },
803 | { 14, 14, "SCS 5 kHz, 1 slot/subframe, slot length 1 ms" },
804 | { 15, 15, "SCS 7.5 kHz(LTE - specific), 1 slot/subframe, slot length 1 ms" },
805 | { 0, 0, NULL((void*)0) }
806 | };
807 |
808 | /* Table 7.5.3.14-1 laaMsgType definition */
809 | static const range_string laaMsgTypes[] = {
810 | {0, 0, "LBT_PDSCH_REQ - lls - O-DU to O-RU request to obtain a PDSCH channel"},
811 | {1, 1, "LBT_DRS_REQ - lls - O-DU to O-RU request to obtain the channel and send DRS"},
812 | {2, 2, "LBT_PDSCH_RSP - O-RU to O-DU response, channel acq success or failure"},
813 | {3, 3, "LBT_DRS_RSP - O-RU to O-DU response, DRS sending success or failure"},
814 | {4, 4, "LBT_Buffer_Error - O-RU to O-DU response, reporting buffer overflow"},
815 | {5, 5, "LBT_CWCONFIG_REQ - O-DU to O-RU request, congestion window configuration"},
816 | {6, 6, "LBT_CWCONFIG_RST - O-RU to O-DU request, congestion window config, response"},
817 | {7, 15, "reserved for future methods"},
818 | {0, 0, NULL((void*)0)}
819 | };
820 |
821 | static const range_string freq_offset_fb_values[] = {
822 | {0, 0, "no frequency offset"},
823 | {8000, 8000, "value not provided"},
824 | {1, 30000, "positive frequency offset, (0, +0.5] subcarrier"},
825 | {0x8ad0, 0xffff, "negative frequency offset, [-0.5, 0) subcarrier"},
826 | {0x0, 0xffff, "reserved"},
827 | {0, 0, NULL((void*)0)}
828 | };
829 |
830 | static const value_string num_sinr_per_prb_vals[] = {
831 | { 0, "1" },
832 | { 1, "2" },
833 | { 2, "3" },
834 | { 3, "4" },
835 | { 4, "6" },
836 | { 5, "12" },
837 | { 6, "reserved" },
838 | { 7, "reserved" },
839 | { 0, NULL((void*)0)}
840 | };
841 |
842 | static const value_string meas_type_id_vals[] = {
843 | { 1, "UE Timing Advance Error" },
844 | { 2, "UE Layer power" },
845 | { 3, "UE frequency offset" },
846 | { 4, "Interference plus Noise for allocated PRBs" },
847 | { 5, "Interference plus Noise for unallocated PRBs" },
848 | { 6, "DMRS SNR per antenna" },
849 | { 0, NULL((void*)0)}
850 | };
851 |
852 | static const value_string beam_type_vals[] = {
853 | { 0, "List of beamId values" },
854 | { 1, "Range of beamId values" },
855 | { 0, NULL((void*)0)}
856 | };
857 |
858 | /* 7.7.24.3 */
859 | static const value_string entry_type_vals[] = {
860 | { 0, "inherit config from preceding entry (2 or 3) ueIdReset=0" },
861 | { 1, "inherit config from preceding entry (2 or 3) ueIdReset=1" },
862 | { 2, "related parameters if have transform precoding disabled " },
863 | { 3, "related parameters if have transform precoding enabled " },
864 | { 0, NULL((void*)0)}
865 | };
866 |
867 |
868 | /* Table 7.6.1-1 */
869 | static const value_string exttype_vals[] = {
870 | {0, "Reserved"},
871 | {1, "Beamforming weights"},
872 | {2, "Beamforming attributes"},
873 | {3, "DL Precoding configuration parameters and indications"},
874 | {4, "Modulation compr. params"},
875 | {5, "Modulation compression additional scaling parameters"},
876 | {6, "Non-contiguous PRB allocation"},
877 | {7, "Multiple-eAxC designation"},
878 | {8, "Regularization factor"},
879 | {9, "Dynamic Spectrum Sharing parameters"},
880 | {10, "Multiple ports grouping"},
881 | {11, "Flexible BF weights"},
882 | {12, "Non-Contiguous PRB Allocation with Frequency Ranges"},
883 | {13, "PRB Allocation with Frequency Hopping"},
884 | {14, "Nulling-layer Info. for ueId-based beamforming"},
885 | {15, "Mixed-numerology Info. for ueId-based beamforming"},
886 | {16, "Section description for antenna mapping in UE channel information based UL beamforming"},
887 | {17, "Section description for indication of user port group"},
888 | {18, "Section description for Uplink Transmission Management"},
889 | {19, "Compact beamforming information for multiple port"},
890 | {20, "Puncturing extension"},
891 | {21, "Variable PRB group size for channel information"},
892 | {22, "ACK/NACK request"},
893 | {23, "Multiple symbol modulation compression parameters"},
894 | {24, "PUSCH DMRS configuration"},
895 | {25, "Symbol reordering for DMRS-BF"},
896 | {26, "Frequency offset feedback"},
897 | {27, "O-DU controlled dimensionality reduction"},
898 | {28, "O-DU controlled frequency resolution for SINR reporting"},
899 | {0, NULL((void*)0)}
900 | };
901 |
902 | /**************************************************************************************/
903 | /* Keep track for each Section Extension, which section types are allowed to carry it */
904 | typedef struct {
905 | bool_Bool ST0;
906 | bool_Bool ST1;
907 | bool_Bool ST3;
908 | bool_Bool ST5;
909 | bool_Bool ST6;
910 | bool_Bool ST10;
911 | bool_Bool ST11;
912 | } AllowedCTs_t;
913 |
914 |
915 | static AllowedCTs_t ext_cts[HIGHEST_EXTTYPE28] = {
916 | /* ST0 ST1 ST3 ST5 ST6 ST10 ST11 */
917 | { false0, true1, true1, false0, false0, false0, false0}, // SE 1 (1,3)
918 | { false0, true1, true1, false0, false0, false0, false0}, // SE 2 (1,3)
919 | { false0, true1, true1, false0, false0, false0, false0}, // SE 3 (1,3)
920 | { false0, true1, true1, true1, false0, false0, false0}, // SE 4 (1,3,5)
921 | { false0, true1, true1, true1, false0, false0, false0}, // SE 5 (1,3,5)
922 | { false0, true1, true1, true1, false0, true1, true1 }, // SE 6 (1,3,5,10,11)
923 | { true1, false0, false0, false0, false0, false0, false0}, // SE 7 (0)
924 | { false0, false0, false0, true1, false0, false0, false0}, // SE 8 (5)
925 | { true1, true1, true1, true1, true1, true1, true1 }, // SE 9 (all)
926 | { false0, true1, true1, true1, false0, false0, false0}, // SE 10 (1,3,5)
927 | { false0, true1, true1, false0, false0, false0, false0}, // SE 11 (1,3)
928 | { false0, true1, true1, true1, false0, true1, true1 }, // SE 12 (1,3,5,10,11)
929 | { false0, true1, true1, true1, false0, false0, false0}, // SE 13 (1,3,5)
930 | { false0, false0, false0, true1, false0, false0, false0}, // SE 14 (5)
931 | { false0, false0, false0, true1, true1, false0, false0}, // SE 15 (5,6)
932 | { false0, false0, false0, true1, false0, false0, false0}, // SE 16 (5)
933 | { false0, false0, false0, true1, false0, false0, false0}, // SE 17 (5)
934 | { false0, true1, true1, true1, false0, false0, false0}, // SE 18 (1,3,5)
935 | { false0, true1, true1, false0, false0, false0, false0}, // SE 19 (1,3)
936 | { true1, true1, true1, true1, true1, true1, true1 }, // SE 20 (0,1,3,5,10,11)
937 | { false0, false0, false0, true1, true1, false0, false0}, // SE 21 (5,6)
938 | { true1, true1, true1, true1, true1, true1, true1 }, // SE 22 (all)
939 | { false0, true1, true1, true1, false0, false0, false0}, // SE 23 (1,3,5)
940 | { false0, false0, false0, true1, false0, false0, false0}, // SE 24 (5)
941 | { false0, false0, false0, true1, false0, false0, false0}, // SE 25 (5)
942 | { false0, false0, false0, true1, false0, false0, false0}, // SE 26 (5)
943 | { false0, false0, false0, true1, false0, false0, false0}, // SE 27 (5)
944 | { false0, false0, false0, true1, false0, false0, false0}, // SE 28 (5)
945 | };
946 |
947 | static bool_Bool se_allowed_in_st(unsigned se, unsigned ct)
948 | {
949 | if (se==0 || se>HIGHEST_EXTTYPE28) {
950 | /* Don't know about new SE, so don't complain.. */
951 | return true1;
952 | }
953 |
954 | switch (ct) {
955 | case 1:
956 | return ext_cts[se-1].ST1;
957 | case 3:
958 | return ext_cts[se-1].ST3;
959 | case 5:
960 | return ext_cts[se-1].ST5;
961 | case 6:
962 | return ext_cts[se-1].ST6;
963 | case 10:
964 | return ext_cts[se-1].ST10;
965 | case 11:
966 | return ext_cts[se-1].ST11;
967 | default:
968 | /* New/unknown section type that includes 'ef'.. assume ok */
969 | return true1;
970 | }
971 | }
972 |
973 | /************************************************************************************/
974 |
975 | /* Table 7.7.1.2-2 */
976 | static const value_string bfw_comp_headers_iq_width[] = {
977 | {0, "I and Q are 16 bits wide"},
978 | {1, "I and Q are 1 bit wide"},
979 | {2, "I and Q are 2 bits wide"},
980 | {3, "I and Q are 3 bits wide"},
981 | {4, "I and Q are 4 bits wide"},
982 | {5, "I and Q are 5 bits wide"},
983 | {6, "I and Q are 6 bits wide"},
984 | {7, "I and Q are 7 bits wide"},
985 | {8, "I and Q are 8 bits wide"},
986 | {9, "I and Q are 9 bits wide"},
987 | {10, "I and Q are 10 bits wide"},
988 | {11, "I and Q are 11 bits wide"},
989 | {12, "I and Q are 12 bits wide"},
990 | {13, "I and Q are 13 bits wide"},
991 | {14, "I and Q are 14 bits wide"},
992 | {15, "I and Q are 15 bits wide"},
993 | {0, NULL((void*)0)}
994 | };
995 |
996 | /* Table 7.7.1.2-3 */
997 | static const value_string bfw_comp_headers_comp_meth[] = {
998 | {COMP_NONE0, "no compression"},
999 | {COMP_BLOCK_FP1, "block floating point"},
1000 | {COMP_BLOCK_SCALE2, "block scaling"},
1001 | {COMP_U_LAW3, "u-law"},
1002 | {4, "beamspace compression type I"},
1003 | {5, "beamspace compression type II"},
1004 | {0, NULL((void*)0)}
1005 | };
1006 |
1007 | /* 7.7.6.2 rbgSize (resource block group size) */
1008 | static const value_string rbg_size_vals[] = {
1009 | {0, "reserved"},
1010 | {1, "1"},
1011 | {2, "2"},
1012 | {3, "3"},
1013 | {4, "4"},
1014 | {5, "6"},
1015 | {6, "8"},
1016 | {7, "16"},
1017 | {0, NULL((void*)0)}
1018 | };
1019 |
1020 | /* 7.7.6.5 */
1021 | static const value_string priority_vals[] = {
1022 | {0, "0"},
1023 | {1, "+1"},
1024 | {2, "-2 (reserved, should not be used)"},
1025 | {3, "-1"},
1026 | {0, NULL((void*)0)}
1027 | };
1028 |
1029 | /* 7.7.10.2 beamGroupType */
1030 | static const value_string beam_group_type_vals[] = {
1031 | {0x0, "common beam"},
1032 | {0x1, "beam matrix indication"},
1033 | {0x2, "beam vector listing"},
1034 | {0x3, "beamId/ueId listing with associated port-list index"},
1035 | {0, NULL((void*)0)}
1036 | };
1037 |
1038 | /* 7.7.9.2 technology (interface name) */
1039 | static const value_string interface_name_vals[] = {
1040 | {0x0, "LTE"},
1041 | {0x1, "NR"},
1042 | {0, NULL((void*)0)}
1043 | };
1044 |
1045 | /* 7.7.18.4 toT (type of transmission) */
1046 | static const value_string type_of_transmission_vals[] = {
1047 | {0x0, "normal transmission mode, data can be distributed in any way the O-RU is implemented to transmit data"},
1048 | {0x1, "uniformly distributed over the transmission window"},
1049 | {0x2, "Reserved"},
1050 | {0x3, "Reserved"},
1051 | {0, NULL((void*)0)}
1052 | };
1053 |
1054 | /* 7.7.2.2 (width of bfa parameters) */
1055 | static const value_string bfa_bw_vals[] = {
1056 | {0, "no bits, the field is not applicable (e.g., O-RU does not support it) or the default value shall be used"},
1057 | {1, "2-bit bitwidth"},
1058 | {2, "3-bit bitwidth"},
1059 | {3, "4-bit bitwidth"},
1060 | {4, "5-bit bitwidth"},
1061 | {5, "6-bit bitwidth"},
1062 | {6, "7-bit bitwidth"},
1063 | {7, "8-bit bitwidth"},
1064 | {0, NULL((void*)0)}
1065 | };
1066 |
1067 | /* 7.7.2.7 & 7.7.2.8 */
1068 | static const value_string sidelobe_suppression_vals[] = {
1069 | {0, "10 dB"},
1070 | {1, "15 dB"},
1071 | {2, "20 dB"},
1072 | {3, "25 dB"},
1073 | {4, "30 dB"},
1074 | {5, "35 dB"},
1075 | {6, "40 dB"},
1076 | {7, ">= 45 dB"},
1077 | {0, NULL((void*)0)}
1078 | };
1079 |
1080 | static const value_string lbtTrafficClass_vals[] = {
1081 | {1, "Priority 1"},
1082 | {2, "Priority 2"},
1083 | {3, "Priority 3"},
1084 | {4, "Priority 4"},
1085 | {0, NULL((void*)0)}
1086 | };
1087 |
1088 | /* 7.5.3.22 */
1089 | static const value_string lbtPdschRes_vals[] = {
1090 | {0, "not sensing – indicates that the O-RU is transmitting data"},
1091 | {1, "currently sensing – indicates the O-RU has not yet acquired the channel"},
1092 | {2, "success – indicates that the channel was successfully acquired"},
1093 | {3, "Failure – indicates expiration of the LBT timer. The LBT process should be reset"},
1094 | {0, NULL((void*)0)}
1095 | };
1096 |
1097 | /* Table 7.5.2.15-3 */
1098 | static const value_string ci_comp_opt_vals[] = {
1099 | {0, "compression per UE, one ciCompParam exists before the I/Q value of each UE"},
1100 | {1, "compression per PRB, one ciCompParam exists before the I/Q value of each PRB"},
1101 | {0, NULL((void*)0)}
1102 | };
1103 |
1104 | /* 7.5.2.17 */
1105 | static const range_string cmd_scope_vals[] = {
1106 | {0, 0, "ARRAY-COMMAND"},
1107 | {1, 1, "CARRIER-COMMAND"},
1108 | {2, 2, "O-RU-COMMAND"},
1109 | {3, 15, "reserved"},
1110 | {0, 0, NULL((void*)0)}
1111 | };
1112 |
1113 | /* N.B., table in 7.5.3.38 is truncated.. */
1114 | static const range_string st4_cmd_type_vals[] = {
1115 | {0, 0, "reserved for future command types"},
1116 | {1, 1, "TIME_DOMAIN_BEAM_CONFIG"},
1117 | {2, 2, "TDD_CONFIG_PATTERN"},
1118 | {3, 3, "TRX_CONTROL"},
1119 | {4, 4, "ASM"},
1120 | {5, 255, "reserved for future command types"},
1121 | {0, 0, NULL((void*)0)}
1122 | };
1123 |
1124 | /* Table 7.5.3.51-1 */
1125 | static const value_string log2maskbits_vals[] = {
1126 | {0, "reserved"},
1127 | {1, "min antMask size is 16 bits.."},
1128 | {2, "min antMask size is 16 bits.."},
1129 | {3, "min antMask size is 16 bits.."},
1130 | {4, "16 bits"},
1131 | {5, "32 bits"},
1132 | {6, "64 bits"},
1133 | {7, "128 bits"},
1134 | {8, "256 bits"},
1135 | {9, "512 bits"},
1136 | {10, "1024 bits"},
1137 | {11, "2048 bits"},
1138 | {12, "4096 bits"},
1139 | {13, "8192 bits"},
1140 | {14, "16384 bits"},
1141 | {15, "reserved"},
1142 | {0, NULL((void*)0)}
1143 | };
1144 |
1145 | /* Table 16.1-1 Sleep modes */
1146 | static const value_string sleep_mode_trx_vals[] = {
1147 | { 0, "TRXC-mode0-wake-up-duration (symbol)"},
1148 | { 1, "TRXC-mode1-wake-up-duration (L)"},
1149 | { 2, "TRXC-mode2-wake-up-duration (M)"},
1150 | { 3, "TRXC-mode3-wake-up-duration (N)"},
1151 | { 0, NULL((void*)0)}
1152 | };
1153 |
1154 | static const value_string sleep_mode_asm_vals[] = {
1155 | { 0, "ASM-mode0-wake-up-duration (symbol)"},
1156 | { 1, "ASM-mode1-wake-up-duration (L)"},
1157 | { 2, "ASM-mode2-wake-up-duration (M)"},
1158 | { 3, "ASM-mode3-wake-up-duration (N)"},
1159 | { 0, NULL((void*)0)}
1160 | };
1161 |
1162 | /* 7.7.21.3.1 */
1163 | static const value_string prg_size_st5_vals[] = {
1164 | { 0, "reserved"},
1165 | { 1, "Precoding resource block group size as WIDEBAND"},
1166 | { 2, "Precoding resource block group size 2"},
1167 | { 3, "Precoding resource block group size 4"},
1168 | { 0, NULL((void*)0)}
1169 | };
1170 |
1171 | /* 7.7.21.3.2 */
1172 | static const value_string prg_size_st6_vals[] = {
1173 | { 0, "if ciPrbGroupSize is 2 or 4, then ciPrbGroupSize, else WIDEBAND"},
1174 | { 1, "Precoding resource block group size as WIDEBAND"},
1175 | { 2, "Precoding resource block group size 2"},
1176 | { 3, "Precoding resource block group size 4"},
1177 | { 0, NULL((void*)0)}
1178 | };
1179 |
1180 | /* 7.7.24.4 */
1181 | static const value_string alpn_per_sym_vals[] = {
1182 | { 0, "report one allocated IPN value per all allocated symbols with DMRS"},
1183 | { 1, "report one allocated IPN value per group of consecutive DMRS symbols"},
1184 | { 0, NULL((void*)0)}
1185 | };
1186 |
1187 | /* 7.7.24.5 */
1188 | static const value_string ant_dmrs_snr_vals[] = {
1189 | { 0, "O-RU shall not report the MEAS_ANT_DMRS_SNR"},
1190 | { 1, "O-RU shall report the MEAS_ANT_DMRS_SNR"},
1191 | { 0, NULL((void*)0)}
1192 | };
1193 |
1194 | /* 7.7.24.14 */
1195 | static const value_string dtype_vals[] = {
1196 | { 0, "assume DMRS configuration type 1"},
1197 | { 1, "assume DMRS configuration type 2"},
1198 | { 0, NULL((void*)0)}
1199 | };
1200 |
1201 | /* 7.7.24.17 */
1202 | static const value_string papr_type_vals[] = {
1203 | { 0, "sequence generator type 1 for short sequence lengths"},
1204 | { 1, "sequence generator type 1 for long sequence lengths"},
1205 | { 2, "sequence generator type 2 for short sequence lengths"},
1206 | { 3, "sequence generator type 2 for long sequence lengths"},
1207 | { 0, NULL((void*)0)}
1208 | };
1209 |
1210 | /* 7.7.24.18 */
1211 | static const value_string hopping_mode_vals[] = {
1212 | { 0, "neither group, nor sequence hopping is enabled"},
1213 | { 1, "group hopping is enabled and sequence hopping is disabled"},
1214 | { 2, "sequence hopping is enabled and group hopping is disabled"},
1215 | { 3, "reserved"},
1216 | { 0, NULL((void*)0)}
1217 | };
1218 |
1219 |
1220 | static const true_false_string tfs_sfStatus =
1221 | {
1222 | "subframe was transmitted",
1223 | "subframe was dropped"
1224 | };
1225 |
1226 | static const true_false_string tfs_lbtBufErr =
1227 | {
1228 | "buffer overflow – data received at O-RU is larger than the available buffer size",
1229 | "reserved"
1230 | };
1231 |
1232 | static const true_false_string tfs_partial_full_sf = {
1233 | "partial SF",
1234 | "full SF"
1235 | };
1236 |
1237 | static const true_false_string disable_tdbfns_tfs = {
1238 | "beam numbers excluded",
1239 | "beam numbers included"
1240 | };
1241 |
1242 | static const true_false_string continuity_indication_tfs = {
1243 | "continuity between current and next bundle",
1244 | "discontinuity between current and next bundle"
1245 | };
1246 |
1247 | static const true_false_string prb_mode_tfs = {
1248 | "PRB-BLOCK mode",
1249 | "PRB-MASK mode"
1250 | };
1251 |
1252 | static const true_false_string symbol_direction_tfs = {
1253 | "DL symbol",
1254 | "UL symbol"
1255 | };
1256 |
1257 | static const true_false_string symbol_guard_tfs = {
1258 | "guard symbol",
1259 | "non-guard symbol"
1260 | };
1261 |
1262 | static const true_false_string beam_numbers_included_tfs = {
1263 | "time-domain beam numbers excluded in this command",
1264 | "time-domain beam numbers included in this command"
1265 | };
1266 |
1267 | static const true_false_string measurement_flag_tfs = {
1268 | "at least one additional measurement report or command after the current one",
1269 | "no additional measurement report or command"
1270 | };
1271 |
1272 | static const true_false_string repetition_se6_tfs = {
1273 | "repeated highest priority data section in the C-Plane message",
1274 | "no repetition"
1275 | };
1276 |
1277 | static const true_false_string repetition_se19_tfs = {
1278 | "per port information not present in the extension",
1279 | "per port info present in the extension"
1280 | };
1281 |
1282 |
1283 |
1284 | /* Forward declaration */
1285 | static int dissect_udcompparam(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree, unsigned offset,
1286 | unsigned comp_meth,
1287 | uint32_t *exponent, uint16_t *sReSMask, bool_Bool for_sinr);
1288 |
1289 |
1290 | static const true_false_string ready_tfs = {
1291 | "message is a \"ready\" message",
1292 | "message is a ACK message"
1293 | };
1294 |
1295 | static const true_false_string multi_sd_scope_tfs = {
1296 | "Puncturing pattern applies to current and following sections",
1297 | "Puncturing pattern applies to current section"
1298 | };
1299 |
1300 | static const true_false_string tfs_ueid_reset = {
1301 | "cannot assume same UE as in preceding slot",
1302 | "can assume same UE as in preceding slot"
1303 | };
1304 |
1305 |
1306 | /* Config for (and later, worked-out allocations) bundles for ext11 (dynamic BFW) */
1307 | typedef struct {
1308 | /* Ext 6 config */
1309 | bool_Bool ext6_set;
1310 | uint8_t ext6_rbg_size; /* number of PRBs allocated by bitmask */
1311 |
1312 | uint8_t ext6_num_bits_set;
1313 | uint8_t ext6_bits_set[28]; /* Which bit position this entry has */
1314 | /* TODO: store an f value for each bit position? */
1315 |
1316 | /* Ext 12 config */
1317 | bool_Bool ext12_set;
1318 | unsigned ext12_num_pairs;
1319 | #define MAX_BFW_EXT12_PAIRS128 128
1320 | struct {
1321 | uint8_t off_start_prb;
1322 | uint8_t num_prb;
1323 | } ext12_pairs[MAX_BFW_EXT12_PAIRS128];
1324 |
1325 | /* Ext 13 config */
1326 | bool_Bool ext13_set;
1327 | unsigned ext13_num_start_prbs;
1328 | #define MAX_BFW_EXT13_ALLOCATIONS128 128
1329 | unsigned ext13_start_prbs[MAX_BFW_EXT13_ALLOCATIONS128];
1330 | /* TODO: store nextSymbolId here too? */
1331 |
1332 | /* Ext 21 config */
1333 | bool_Bool ext21_set;
1334 | uint8_t ext21_ci_prb_group_size;
1335 |
1336 | /* Results/settings (after calling ext11_work_out_bundles()) */
1337 | uint32_t num_bundles;
1338 | #define MAX_BFW_BUNDLES512 512
1339 | struct {
1340 | uint32_t start; /* first prb of bundle */
1341 | uint32_t end; /* last prb of bundle*/
1342 | bool_Bool is_orphan; /* true if not complete (i.e., end-start < numBundPrb) */
1343 | } bundles[MAX_BFW_BUNDLES512];
1344 | } ext11_settings_t;
1345 |
1346 |
1347 | /* Work out bundle allocation for ext 11. Take into account ext6/ext21, ext12 or ext13 in this section before ext 11. */
1348 | /* Won't be called with numBundPrb=0 */
1349 | static void ext11_work_out_bundles(unsigned startPrbc,
1350 | unsigned numPrbc,
1351 | unsigned numBundPrb, /* number of PRBs pre (full) bundle */
1352 | ext11_settings_t *settings)
1353 | {
1354 | /* Allocation configured by ext 6 */
1355 | if (settings->ext6_set) {
1356 | unsigned bundles_per_entry = (settings->ext6_rbg_size / numBundPrb);
1357 |
1358 | /* Need to cope with these not dividing exactly, or even having more PRbs in a bundle that
1359 | rbg size. i.e. each bundle gets the correct number of PRBs until
1360 | all rbg entries are consumed... */
1361 |
1362 | /* TODO: need to check 7.9.4.2. Different cases depending upon value of RAD */
1363 |
1364 | if (bundles_per_entry == 0) {
1365 | bundles_per_entry = 1;
1366 | }
1367 |
1368 | /* Maybe also be affected by ext 21 */
1369 | if (settings->ext21_set) {
1370 | /* N.B., have already checked that numPrbc is not 0 */
1371 |
1372 | /* ciPrbGroupSize overrides number of contiguous PRBs in group */
1373 | bundles_per_entry = (settings->ext6_rbg_size / settings->ext21_ci_prb_group_size);
1374 |
1375 | /* numPrbc is the number of PRB groups per antenna - handled in call to dissect_bfw_bundle() */
1376 | }
1377 |
1378 | unsigned bundles_set = 0;
1379 | for (unsigned n=0;
1380 | n < (settings->ext6_num_bits_set * settings->ext6_rbg_size) / numBundPrb;
1381 | n++) {
1382 |
1383 | /* Watch out for array bound */
1384 | if (n >= 28) {
1385 | break;
1386 | }
1387 |
1388 | /* For each bundle... */
1389 |
1390 | /* TODO: Work out where first PRB is */
1391 | /* May not be the start of an rbg block... */
1392 | uint32_t prb_start = (settings->ext6_bits_set[n] * settings->ext6_rbg_size);
1393 |
1394 | /* For each bundle within identified rbgSize block */
1395 | for (unsigned m=0; m < bundles_per_entry; m++) {
1396 | settings->bundles[bundles_set].start = startPrbc+prb_start+(m*numBundPrb);
1397 | /* Start already beyond end, so doesn't count. */
1398 | if (settings->bundles[bundles_set].start > (startPrbc+numPrbc-1)) {
1399 | break;
1400 | }
1401 | /* Bundle consists of numBundPrb bundles */
1402 | /* TODO: may involve PRBs from >1 rbg blocks.. */
1403 | settings->bundles[bundles_set].end = startPrbc+prb_start+((m+1)*numBundPrb)-1;
1404 | if (settings->bundles[bundles_set].end > (startPrbc+numPrbc-1)) {
1405 | /* Extends beyond end, so counts but is an orphan bundle */
1406 | settings->bundles[bundles_set].end = numPrbc;
1407 | settings->bundles[bundles_set].is_orphan = true1;
1408 | }
1409 |
1410 | /* Get out if have reached array bound */
1411 | if (++bundles_set == MAX_BFW_BUNDLES512) {
1412 | return;
1413 | }
1414 | }
1415 | }
1416 | settings->num_bundles = bundles_set;
1417 | }
1418 |
1419 | /* Allocation configured by ext 12 */
1420 | else if (settings->ext12_set) {
1421 | /* First, allocate normally from startPrbc, numPrbc */
1422 | settings->num_bundles = (numPrbc+numBundPrb-1) / numBundPrb;
1423 |
1424 | /* Don't overflow settings->bundles[] ! */
1425 | settings->num_bundles = MIN(MAX_BFW_BUNDLES, settings->num_bundles)(((512) < (settings->num_bundles)) ? (512) : (settings-> num_bundles));
1426 |
1427 | for (uint32_t n=0; n < settings->num_bundles; n++) {
1428 | settings->bundles[n].start = startPrbc + n*numBundPrb;
1429 | settings->bundles[n].end = settings->bundles[n].start + numBundPrb-1;
1430 | /* Does it go beyond the end? */
1431 | if (settings->bundles[n].end > startPrbc+numPrbc) {
1432 | settings->bundles[n].end = numPrbc+numPrbc;
1433 | settings->bundles[n].is_orphan = true1;
1434 | }
1435 | }
1436 | if (settings->num_bundles == MAX_BFW_BUNDLES512) {
1437 | return;
1438 | }
1439 |
1440 | unsigned prb_offset = startPrbc + numPrbc;
1441 |
1442 | /* Loop over pairs, adding bundles for each */
1443 | for (unsigned p=0; p < settings->ext12_num_pairs; p++) {
1444 | prb_offset += settings->ext12_pairs[p].off_start_prb;
1445 | unsigned pair_bundles = (settings->ext12_pairs[p].num_prb+numBundPrb-1) / numBundPrb;
1446 |
1447 | for (uint32_t n=0; n < pair_bundles; n++) {
1448 | unsigned idx = settings->num_bundles;
1449 |
1450 | settings->bundles[idx].start = prb_offset + n*numBundPrb;
1451 | settings->bundles[idx].end = settings->bundles[idx].start + numBundPrb-1;
1452 | /* Does it go beyond the end? */
1453 | if (settings->bundles[idx].end > prb_offset + settings->ext12_pairs[p].num_prb) {
1454 | settings->bundles[idx].end = prb_offset + settings->ext12_pairs[p].num_prb;
1455 | settings->bundles[idx].is_orphan = true1;
1456 | }
1457 | /* Range check / return */
1458 | settings->num_bundles++;
1459 | if (settings->num_bundles == MAX_BFW_BUNDLES512) {
1460 | return;
1461 | }
1462 | }
1463 |
1464 | prb_offset += settings->ext12_pairs[p].num_prb;
1465 | }
1466 | }
1467 |
1468 | /* Allocation configured by ext 13 */
1469 | else if (settings->ext13_set) {
1470 | unsigned alloc_size = (numPrbc+numBundPrb-1) / numBundPrb;
1471 | settings->num_bundles = alloc_size * settings->ext13_num_start_prbs;
1472 |
1473 | /* Don't overflow settings->bundles[] ! */
1474 | settings->num_bundles = MIN(MAX_BFW_BUNDLES, settings->num_bundles)(((512) < (settings->num_bundles)) ? (512) : (settings-> num_bundles));
1475 |
1476 | for (unsigned alloc=0; alloc < settings->ext13_num_start_prbs; alloc++) {
1477 | unsigned alloc_start = alloc * alloc_size;
1478 | for (uint32_t n=0; n < alloc_size; n++) {
1479 | if ((alloc_start+n) >= MAX_BFW_BUNDLES512) {
1480 | /* ERROR */
1481 | return;
1482 | }
1483 | settings->bundles[alloc_start+n].start = settings->ext13_start_prbs[alloc] + startPrbc + n*numBundPrb;
1484 | settings->bundles[alloc_start+n].end = settings->bundles[alloc_start+n].start + numBundPrb-1;
1485 | if (settings->bundles[alloc_start+n].end > settings->ext13_start_prbs[alloc] + numPrbc) {
1486 | settings->bundles[alloc_start+n].end = settings->ext13_start_prbs[alloc] + numPrbc;
1487 | settings->bundles[alloc_start+n].is_orphan = true1;
1488 | }
1489 | }
1490 | }
1491 | }
1492 |
1493 | /* Case where bundles are not controlled by other extensions - just divide up range into bundles we have */
1494 | else {
1495 | settings->num_bundles = (numPrbc+numBundPrb-1) / numBundPrb; /* rounded up */
1496 |
1497 | /* Don't overflow settings->bundles[] */
1498 | settings->num_bundles = MIN(MAX_BFW_BUNDLES, settings->num_bundles)(((512) < (settings->num_bundles)) ? (512) : (settings-> num_bundles));
1499 |
1500 | /* For each bundle.. */
1501 | for (uint32_t n=0; n < settings->num_bundles; n++) {
1502 | /* Allocate start and end */
1503 | settings->bundles[n].start = startPrbc + n*numBundPrb;
1504 | settings->bundles[n].end = settings->bundles[n].start + numBundPrb - 1;
1505 | /* If would go beyond end of PRBs, limit and identify as orphan */
1506 | if (settings->bundles[n].end > startPrbc+numPrbc) {
1507 | settings->bundles[n].end = startPrbc+numPrbc;
1508 | settings->bundles[n].is_orphan = true1;
1509 | }
1510 | }
1511 | }
1512 | }
1513 |
1514 |
1515 | /*******************************************************/
1516 | /* Overall state of a flow (eAxC/plane) */
1517 | typedef struct {
1518 | /* State for sequence analysis [each direction] */
1519 | bool_Bool last_frame_seen[2];
1520 | uint32_t last_frame[2];
1521 | uint8_t next_expected_sequence_number[2];
1522 |
1523 | /* Table recording ackNack requests (ackNackId -> ack_nack_request_t*)
1524 | Note that this assumes that the same ackNackId will not be reused within a state,
1525 | which may well not be valid */
1526 | wmem_tree_t *ack_nack_requests;
1527 |
1528 | /* Store udCompHdr seen in C-Plane for UL - can be looked up and used by U-PLane.
1529 | Note that this appears in the common section header parts of ST1, ST3, ST5,
1530 | so can still be over-written per sectionId in the U-Plane */
1531 | unsigned ul_ud_comp_hdr_frame;
1532 | bool_Bool ul_ud_comp_hdr_set;
1533 | unsigned ul_ud_comp_hdr_bit_width;
1534 | int ul_ud_comp_hdr_compression;
1535 |
1536 | bool_Bool udcomphdrDownlink_heuristic_result_set;
1537 | bool_Bool udcomphdrDownlink_heuristic_result;
1538 | bool_Bool udcomphdrUplink_heuristic_result_set;
1539 | bool_Bool udcomphdrUplink_heuristic_result;
1540 |
1541 | /* Modulation compression params */
1542 | /* TODO: incomplete (see SE4, SE5, SE23), and needs to be per section! */
1543 | //uint16_t mod_comp_re_mask;
1544 | //bool mod_compr_csf;
1545 | //double mod_compr_mod_comp_scaler;
1546 | } flow_state_t;
1547 |
1548 | typedef struct {
1549 | uint32_t request_frame_number;
1550 | nstime_t request_frame_time;
1551 | enum {
1552 | SE22,
1553 | ST4Cmd1,
1554 | ST4Cmd2,
1555 | ST4Cmd3,
1556 | ST4Cmd4
1557 | } requestType;
1558 |
1559 | uint32_t response_frame_number;
1560 | nstime_t response_frame_time;
1561 | } ack_nack_request_t;
1562 |
1563 | static const value_string acknack_type_vals[] = {
1564 | { SE22, "SE 22" },
1565 | { ST4Cmd1, "ST4 (TIME_DOMAIN_BEAM_CONFIG)" },
1566 | { ST4Cmd2, "ST4 (TDD_CONFIG_PATTERN)" },
1567 | { ST4Cmd3, "ST4 (TRX_CONTROL)" },
1568 | { ST4Cmd4, "ST4 (ASM)" },
1569 | { 0, NULL((void*)0)}
1570 | };
1571 |
1572 | #define ORAN_C_PLANE0 0
1573 | #define ORAN_U_PLANE1 1
1574 |
1575 | /* Using parts of src/dst MAC address, so don't confuse UL messages with DL messages configuring UL.. */
1576 | static uint32_t make_flow_key(packet_info *pinfo, uint16_t eaxc_id, uint8_t plane, bool_Bool opposite_dir)
1577 | {
1578 | uint16_t eth_bits = 0;
1579 | if (pinfo->dl_src.len == 6 && pinfo->dl_dst.len == 6) {
1580 | /* Only using (most of) 2 bytes from addresses for now, but reluctant to make key longer.. */
1581 | uint8_t *src_eth = (uint8_t*)pinfo->dl_src.data;
1582 | uint8_t *dst_eth = (uint8_t*)pinfo->dl_dst.data;
1583 | if (!opposite_dir) {
1584 | eth_bits = (src_eth[0]<<8) | dst_eth[5];
1585 | }
1586 | else {
1587 | eth_bits = (dst_eth[0]<<8) | src_eth[5];
1588 | }
1589 | }
1590 | return eaxc_id | (plane << 16) | (eth_bits << 17);
1591 | }
1592 |
1593 |
1594 | /* Table maintained on first pass from flow_key(uint32_t) -> flow_state_t* */
1595 | static wmem_tree_t *flow_states_table;
1596 |
1597 | /* Table consulted on subsequent passes: frame_num -> flow_result_t* */
1598 | static wmem_tree_t *flow_results_table;
1599 |
1600 | typedef struct {
1601 | /* Sequence analysis */
1602 | bool_Bool unexpected_seq_number;
1603 | uint8_t expected_sequence_number;
1604 | uint32_t previous_frame;
1605 | } flow_result_t;
1606 |
1607 |
1608 | /* Uplink timing */
1609 | /* For a given symbol, track first to last UL frame to find out first-last time */
1610 | /* frameId (8) + subframeId (4) + slotId (6) + symbolId (6) = 24 bits */
1611 | /* N.B. if a capture lasts > 2.5s, may see same timing come around again... */
1612 | static uint32_t get_timing_key(uint8_t frameId, uint8_t subframeId, uint8_t slotId, uint8_t symbolId)
1613 | {
1614 | return symbolId + (slotId<<8) + (subframeId<<14) + (frameId<<18);
1615 | }
1616 |
1617 | typedef struct {
1618 | uint32_t first_frame;
1619 | nstime_t first_frame_time;
1620 | uint32_t frames_seen_in_symbol;
1621 | uint32_t last_frame_in_symbol;
1622 | } ul_timing_for_slot;
1623 |
1624 | /* Set during first pass. timing_key -> ul_timing_for_slot* */
1625 | static wmem_tree_t *ul_symbol_timing;
1626 |
1627 |
1628 | static void show_link_to_acknack_response(proto_tree *tree, tvbuff_t *tvb, packet_info *pinfo,
1629 | ack_nack_request_t *response);
1630 |
1631 |
1632 |
1633 |
1634 | static void write_pdu_label_and_info(proto_item *ti1, proto_item *ti2,
1635 | packet_info *pinfo, const char *format, ...) G_GNUC_PRINTF(4, 5)__attribute__((__format__ (__printf__, 4, 5)));
1636 |
1637 | /* Write the given formatted text to:
1638 | - the info column (if pinfo != NULL)
1639 | - 1 or 2 other labels (optional)
1640 | */
1641 | static void write_pdu_label_and_info(proto_item *ti1, proto_item *ti2,
1642 | packet_info *pinfo, const char *format, ...)
1643 | {
1644 | #define MAX_INFO_BUFFER256 256
1645 | char info_buffer[MAX_INFO_BUFFER256];
1646 | va_list ap;
1647 |
1648 | if ((ti1 == NULL((void*)0)) && (ti2 == NULL((void*)0)) && (pinfo == NULL((void*)0))) {
1649 | return;
1650 | }
1651 |
1652 | va_start(ap, format)__builtin_va_start(ap, format);
1653 | vsnprintf(info_buffer, MAX_INFO_BUFFER256, format, ap);
1654 | va_end(ap)__builtin_va_end(ap);
1655 |
1656 | /* Add to indicated places */
1657 | if (pinfo != NULL((void*)0)) {
1658 | col_append_str(pinfo->cinfo, COL_INFO, info_buffer);
1659 | }
1660 | if (ti1 != NULL((void*)0)) {
1661 | proto_item_append_text(ti1, "%s", info_buffer);
1662 | }
1663 | if (ti2 != NULL((void*)0)) {
1664 | proto_item_append_text(ti2, "%s", info_buffer);
1665 | }
1666 | }
1667 |
1668 | /* Add section labels (type + PRB range) for C-Plane, U-Plane */
1669 | static void
1670 | write_section_info(proto_item *section_heading, packet_info *pinfo, proto_item *protocol_item,
1671 | uint32_t section_id, uint32_t start_prbx, uint32_t num_prbx, uint32_t rb)
1672 | {
1673 | switch (num_prbx) {
1674 | case 0:
1675 | /* None -> all */
1676 | write_pdu_label_and_info(section_heading, protocol_item, pinfo, ", Id: %4d (all PRBs)", section_id);
1677 | break;
1678 | case 1:
1679 | /* Single PRB */
1680 | write_pdu_label_and_info(section_heading, protocol_item, pinfo, ", Id: %4d (PRB: %7u)", section_id, start_prbx);
1681 | break;
1682 | default:
1683 | /* Range */
1684 | write_pdu_label_and_info(section_heading, protocol_item, pinfo, ", Id: %4d (PRB: %3u-%3u%s)", section_id, start_prbx,
1685 | start_prbx + (num_prbx-1)*(1+rb), rb ? " (every-other)" : "");
1686 | }
1687 | }
1688 |
1689 | static void
1690 | write_channel_section_info(proto_item *section_heading, packet_info *pinfo,
1691 | uint32_t section_id, uint32_t ueId, uint32_t start_prbx, uint32_t num_prbx,
1692 | uint32_t num_trx)
1693 | {
1694 | switch (num_prbx) {
1695 | case 0:
1696 | /* TODO: ?? */
1697 | break;
1698 | case 1:
1699 | /* Single PRB */
1700 | write_pdu_label_and_info(section_heading, NULL((void*)0), pinfo,
1701 | ", Id: %4d (UEId=%5u PRB %7u, %2u antennas)",
1702 | section_id, ueId, start_prbx, num_trx);
1703 | break;
1704 | default:
1705 | /* Range */
1706 | write_pdu_label_and_info(section_heading, NULL((void*)0), pinfo,
1707 | ", Id: %4d (UEId=%5u PRBs %3u-%3u, %2u antennas)",
1708 | section_id, ueId, start_prbx, start_prbx+num_prbx-1, num_trx);
1709 | }
1710 | }
1711 |
1712 |
1713 | /* 5.1.3.2.7 (real time control data / IQ data transfer message series identifier) */
1714 | static void
1715 | addPcOrRtcid(tvbuff_t *tvb, proto_tree *tree, int *offset, int hf, uint16_t *eAxC)
1716 | {
1717 | /* Subtree */
1718 | proto_item *oran_pcid_ti = proto_tree_add_item(tree, hf,
1719 | tvb, *offset, 2, ENC_NA0x00000000);
1720 | proto_tree *oran_pcid_tree = proto_item_add_subtree(oran_pcid_ti, ett_oran_ecpri_pcid);
1721 |
1722 | uint64_t duPortId, bandSectorId, ccId, ruPortId = 0;
1723 | int id_offset = *offset;
1724 |
1725 | /* All parts of eAxC should be above 0, and should total 16 bits (breakdown controlled by preferences) */
1726 | if (!((pref_du_port_id_bits > 0) && (pref_bandsector_id_bits > 0) && (pref_cc_id_bits > 0) && (pref_ru_port_id_bits > 0) &&
1727 | ((pref_du_port_id_bits + pref_bandsector_id_bits + pref_cc_id_bits + pref_ru_port_id_bits) == 16))) {
1728 | expert_add_info(NULL((void*)0), tree, &ei_oran_invalid_eaxc_bit_width);
1729 | *eAxC = 0;
1730 | *offset += 2;
1731 | return;
1732 | }
1733 |
1734 | unsigned bit_offset = *offset * 8;
1735 |
1736 | /* N.B. For sequence analysis / tapping, just interpret these 2 bytes as eAxC ID... */
1737 | *eAxC = tvb_get_uint16(tvb, *offset, ENC_BIG_ENDIAN0x00000000);
1738 |
1739 | /* DU Port ID */
1740 | proto_tree_add_bits_ret_val(oran_pcid_tree, hf_oran_du_port_id, tvb, bit_offset, pref_du_port_id_bits, &duPortId, ENC_BIG_ENDIAN0x00000000);
1741 | bit_offset += pref_du_port_id_bits;
1742 | /* BandSector ID */
1743 | proto_tree_add_bits_ret_val(oran_pcid_tree, hf_oran_bandsector_id, tvb, bit_offset, pref_bandsector_id_bits, &bandSectorId, ENC_BIG_ENDIAN0x00000000);
1744 | bit_offset += pref_bandsector_id_bits;
1745 | /* CC ID */
1746 | proto_tree_add_bits_ret_val(oran_pcid_tree, hf_oran_cc_id, tvb, bit_offset, pref_cc_id_bits, &ccId, ENC_BIG_ENDIAN0x00000000);
1747 | bit_offset += pref_cc_id_bits;
1748 | /* RU Port ID */
1749 | proto_tree_add_bits_ret_val(oran_pcid_tree, hf_oran_ru_port_id, tvb, bit_offset, pref_ru_port_id_bits, &ruPortId, ENC_BIG_ENDIAN0x00000000);
1750 | *offset += 2;
1751 |
1752 | proto_item_append_text(oran_pcid_ti, " (DU_Port_ID: %d, BandSector_ID: %d, CC_ID: %d, RU_Port_ID: %d)",
1753 | (int)duPortId, (int)bandSectorId, (int)ccId, (int)ruPortId);
1754 | char id[16];
1755 | snprintf(id, 16, "%x:%x:%x:%x", (int)duPortId, (int)bandSectorId, (int)ccId, (int)ruPortId);
1756 | proto_item *pi = proto_tree_add_string(oran_pcid_tree, hf_oran_c_eAxC_ID, tvb, id_offset, 2, id);
1757 | proto_item_set_generated(pi);
1758 | }
1759 |
1760 | /* 5.1.3.2.8 ecpriSeqid (message identifier) */
1761 | static int
1762 | addSeqid(tvbuff_t *tvb, proto_tree *oran_tree, int offset, int plane, uint8_t *seq_id, proto_item **seq_id_ti, packet_info *pinfo)
1763 | {
1764 | /* Subtree */
1765 | proto_item *seqIdItem = proto_tree_add_item(oran_tree, hf_oran_ecpri_seqid, tvb, offset, 2, ENC_NA0x00000000);
1766 | proto_tree *oran_seqid_tree = proto_item_add_subtree(seqIdItem, ett_oran_ecpri_seqid);
1767 | uint32_t seqId, subSeqId, e = 0;
1768 |
1769 | /* Sequence ID (8 bits) */
1770 | *seq_id_ti = proto_tree_add_item_ret_uint(oran_seqid_tree, hf_oran_sequence_id, tvb, offset, 1, ENC_NA0x00000000, &seqId);
1771 | *seq_id = seqId;
1772 | offset += 1;
1773 |
1774 | /* Show link back to previous sequence ID, if set */
1775 | flow_result_t *result = wmem_tree_lookup32(flow_results_table, pinfo->num);
1776 | if (result) {
1777 | proto_item *prev_ti = proto_tree_add_uint(oran_seqid_tree, hf_oran_previous_frame, tvb, 0, 0, result->previous_frame);
1778 | proto_item_set_generated(prev_ti);
1779 | }
1780 |
1781 | /* E bit */
1782 | proto_tree_add_item_ret_uint(oran_seqid_tree, hf_oran_e_bit, tvb, offset, 1, ENC_NA0x00000000, &e);
1783 | /* Subsequence ID (7 bits) */
1784 | proto_tree_add_item_ret_uint(oran_seqid_tree, hf_oran_subsequence_id, tvb, offset, 1, ENC_NA0x00000000, &subSeqId);
1785 | offset += 1;
1786 |
1787 | /* radio-transport fragmentation not allowed for C-Plane messages */
1788 | if (plane == ORAN_C_PLANE0) {
1789 | if (e !=1 || subSeqId != 0) {
1790 | expert_add_info(NULL((void*)0), seqIdItem, &ei_oran_radio_fragmentation_c_plane);
1791 | }
1792 | }
1793 | else {
1794 | if (e !=1 || subSeqId != 0) {
1795 | /* TODO: Re-assembly of any radio-fragmentation on U-Plane */
1796 | expert_add_info(NULL((void*)0), seqIdItem, &ei_oran_radio_fragmentation_u_plane);
1797 | }
1798 | }
1799 |
1800 | /* Summary */
1801 | proto_item_append_text(seqIdItem, " (SeqId: %3d, E: %d, SubSeqId: %d)", seqId, e, subSeqId);
1802 | return offset;
1803 | }
1804 |
1805 | static int dissect_symbolmask(tvbuff_t *tvb, proto_tree *tree, int offset, uint32_t *symbol_mask, proto_item **ti)
1806 | {
1807 | uint64_t temp_val;
1808 |
1809 | static int * const symbol_mask_flags[] = {
1810 | &hf_oran_symbol_mask_s13,
1811 | &hf_oran_symbol_mask_s12,
1812 | &hf_oran_symbol_mask_s11,
1813 | &hf_oran_symbol_mask_s10,
1814 | &hf_oran_symbol_mask_s9,
1815 | &hf_oran_symbol_mask_s8,
1816 | &hf_oran_symbol_mask_s7,
1817 | &hf_oran_symbol_mask_s6,
1818 | &hf_oran_symbol_mask_s5,
1819 | &hf_oran_symbol_mask_s4,
1820 | &hf_oran_symbol_mask_s3,
1821 | &hf_oran_symbol_mask_s2,
1822 | &hf_oran_symbol_mask_s1,
1823 | &hf_oran_symbol_mask_s0,
1824 | NULL((void*)0)
1825 | };
1826 |
1827 | proto_item *temp_ti = proto_tree_add_bitmask_ret_uint64(tree, tvb, offset,
1828 | hf_oran_symbol_mask,
1829 | ett_oran_symbol_mask, symbol_mask_flags,
1830 | ENC_BIG_ENDIAN0x00000000, &temp_val);
1831 | /* Set out parameters */
1832 | if (symbol_mask) {
1833 | *symbol_mask = (uint32_t)temp_val;
1834 | }
1835 | if (ti) {
1836 | *ti = temp_ti;
1837 | }
1838 | return offset+2;
1839 | }
1840 |
1841 | /* 7.7.1.2 bfwCompHdr (beamforming weight compression header) */
1842 | static int dissect_bfwCompHdr(tvbuff_t *tvb, proto_tree *tree, int offset,
1843 | uint32_t *iq_width, uint32_t *comp_meth, proto_item **comp_meth_ti)
1844 | {
1845 | /* Subtree */
1846 | proto_item *bfwcomphdr_ti = proto_tree_add_string_format(tree, hf_oran_bfwCompHdr,
1847 | tvb, offset, 1, "",
1848 | "bfwCompHdr");
1849 | proto_tree *bfwcomphdr_tree = proto_item_add_subtree(bfwcomphdr_ti, ett_oran_bfwcomphdr);
1850 |
1851 | /* Width and method */
1852 | proto_tree_add_item_ret_uint(bfwcomphdr_tree, hf_oran_bfwCompHdr_iqWidth,
1853 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, iq_width);
1854 | /* Special case: 0 -> 16 */
1855 | *iq_width = (*iq_width==0) ? 16 : *iq_width;
1856 | *comp_meth_ti = proto_tree_add_item_ret_uint(bfwcomphdr_tree, hf_oran_bfwCompHdr_compMeth,
1857 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, comp_meth);
1858 | offset++;
1859 |
1860 | /* Summary */
1861 | proto_item_append_text(bfwcomphdr_ti, " (IqWidth=%u, compMeth=%s)",
1862 | *iq_width,
1863 | val_to_str_const(*comp_meth, bfw_comp_headers_comp_meth, "reserved"));
1864 |
1865 | return offset;
1866 | }
1867 |
1868 | /* Return offset */
1869 | /* Returning number of entries set - would be good to also return an array of set TRX# so could show which array element
1870 | each BFW is actually for.. */
1871 | static int dissect_active_beamspace_coefficient_mask(tvbuff_t *tvb, proto_tree *tree, int offset, unsigned *num_trx_entries, uint16_t **trx_entries)
1872 | {
1873 | /* activeBeamspaceCoefficientMask - ceil(K/8) octets */
1874 | /* K is the number of elements in uncompressed beamforming weight vector.
1875 | * Calculated from parameters describing tx-array or tx-array */
1876 | unsigned k_octets = (pref_data_plane_section_total_rbs + 7) / 8;
1877 |
1878 | static uint16_t trx_enabled[1024];
1879 |
1880 | /* TODO: could use a bigger bitmask array, but for now just uses this bytes-worth for each byte */
1881 | static int * const mask_bits[] = {
1882 | &hf_oran_active_beamspace_coefficient_n1,
1883 | &hf_oran_active_beamspace_coefficient_n2,
1884 | &hf_oran_active_beamspace_coefficient_n3,
1885 | &hf_oran_active_beamspace_coefficient_n4,
1886 | &hf_oran_active_beamspace_coefficient_n5,
1887 | &hf_oran_active_beamspace_coefficient_n6,
1888 | &hf_oran_active_beamspace_coefficient_n7,
1889 | &hf_oran_active_beamspace_coefficient_n8,
1890 | NULL((void*)0)
1891 | };
1892 |
1893 | *num_trx_entries = 0;
1894 | guint64 val;
1895 | for (unsigned n=0; n < k_octets; n++) {
1896 | proto_tree_add_bitmask_ret_uint64(tree, tvb, offset,
1897 | hf_oran_activeBeamspaceCoefficientMask,
1898 | ett_active_beamspace_coefficient_mask, mask_bits,
1899 | ENC_BIG_ENDIAN0x00000000, &val);
1900 | offset++;
1901 | /* Add up the set bits for this byte (but be careful not to count beyond last real K bit..) */
1902 | for (unsigned b=0; b < 8; b++) {
1903 | if ((1 << b) & (unsigned)val) {
1904 | if (((n*8)+b) < pref_data_plane_section_total_rbs) {
1905 | if (*num_trx_entries < 1024-1) { /* Don't write beyond array (which should be plenty big) */
1906 | trx_enabled[(*num_trx_entries)++] = (n*8) + b + 1;
1907 | }
1908 | }
1909 | }
1910 | }
1911 | }
1912 | /* Set pointer to static array */
1913 | *trx_entries = trx_enabled;
1914 |
1915 | /* Show how many bits set */
1916 | proto_item *ti = proto_tree_add_uint(tree, hf_oran_activeBeamspaceCoefficientMask_bits_set, tvb,
1917 | offset-k_octets, k_octets, *num_trx_entries);
1918 | proto_item_set_generated(ti);
1919 |
1920 | return offset;
1921 | }
1922 |
1923 | /* 7.7.1.3 bfwCompParam (beamforming weight compression parameter).
1924 | * Depends upon passed-in bfwCompMeth (field may be empty) */
1925 | static int dissect_bfwCompParam(tvbuff_t *tvb, proto_tree *tree, packet_info *pinfo, int offset,
1926 | proto_item *meth_ti, uint32_t *bfw_comp_method,
1927 | uint32_t *exponent, bool_Bool *supported, unsigned *num_trx_entries, uint16_t **trx_entries)
1928 | {
1929 | if (*bfw_comp_method == COMP_NONE0) {
33 | ← | Assuming the condition is true | →
34 | ← | Taking true branch | →
1930 | /* Absent! */
1931 | *supported = true1;
1932 | return offset;
35 | ← | Returning without writing to '*num_trx_entries' | →
1933 | }
1934 |
1935 | /* Subtree */
1936 | proto_item *bfwcompparam_ti = proto_tree_add_string_format(tree, hf_oran_bfwCompParam,
1937 | tvb, offset, 1, "",
1938 | "bfwCompParam");
1939 | proto_tree *bfwcompparam_tree = proto_item_add_subtree(bfwcompparam_ti, ett_oran_bfwcompparam);
1940 |
1941 | proto_item_append_text(bfwcompparam_ti,
1942 | " (meth=%s)", val_to_str_const(*bfw_comp_method, bfw_comp_headers_comp_meth, "reserved"));
1943 |
1944 | *num_trx_entries = 0;
1945 | *supported = false0;
1946 | switch (*bfw_comp_method) {
1947 | case COMP_BLOCK_FP1: /* block floating point */
1948 | /* 4 reserved bits + exponent */
1949 | proto_tree_add_item_ret_uint(bfwcompparam_tree, hf_oran_exponent,
1950 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, exponent);
1951 | proto_item_append_text(bfwcompparam_ti, " exponent=%u", *exponent);
1952 | *supported = true1;
1953 | offset++;
1954 | break;
1955 | case COMP_BLOCK_SCALE2: /* block scaling */
1956 | /* Separate into integer and fractional bits? */
1957 | proto_tree_add_item(bfwcompparam_tree, hf_oran_blockScaler,
1958 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
1959 | offset++;
1960 | break;
1961 | case COMP_U_LAW3: /* u-law */
1962 | /* compBitWidth, compShift */
1963 | proto_tree_add_item(bfwcompparam_tree, hf_oran_compBitWidth,
1964 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
1965 | proto_tree_add_item(bfwcompparam_tree, hf_oran_compShift,
1966 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
1967 | offset++;
1968 | break;
1969 | case 4: /* beamspace I (BLOCK SCALING) */
1970 | /* activeBeamspaceCoefficientMask */
1971 | offset = dissect_active_beamspace_coefficient_mask(tvb, bfwcompparam_tree, offset, num_trx_entries, trx_entries);
1972 | *bfw_comp_method = COMP_BLOCK_SCALE2;
1973 | *supported = false0; /* TODO: true once BLOCK SCALE is supported */
1974 | break;
1975 | case 5: /* beamspace II (BLOCK FLOATING POINT) */
1976 | /* activeBeamspaceCoefficientMask */
1977 | offset = dissect_active_beamspace_coefficient_mask(tvb, bfwcompparam_tree, offset, num_trx_entries, trx_entries);
1978 | /* reserved (4 bits) + exponent (4 bits) */
1979 | proto_tree_add_item(bfwcompparam_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_NA0x00000000);
1980 | proto_tree_add_item_ret_uint(bfwcompparam_tree, hf_oran_exponent, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, exponent);
1981 | offset += 1;
1982 | *bfw_comp_method = COMP_BLOCK_FP1;
1983 | *supported = true1;
1984 | break;
1985 |
1986 | default:
1987 | /* Not handled */
1988 | break;
1989 | }
1990 |
1991 | /* Can't go on if compression scheme not supported */
1992 | if (!(*supported) && meth_ti) {
1993 | expert_add_info_format(pinfo, meth_ti, &ei_oran_unsupported_bfw_compression_method,
1994 | "BFW Compression method %u (%s) not decompressed by dissector",
1995 | *bfw_comp_method,
1996 | val_to_str_const(*bfw_comp_method, bfw_comp_headers_comp_meth, "reserved"));
1997 | }
1998 | return offset;
1999 | }
2000 |
2001 |
2002 | /* Special case for uncompressed/16-bit value */
2003 | static float uncompressed_to_float(uint32_t h)
2004 | {
2005 | int16_t i16 = h & 0x0000ffff;
2006 | if (show_unscaled_values) {
2007 | return (float)i16;
2008 | }
2009 | return ((float)i16) / 0x7fff;
2010 | }
2011 |
2012 | /* Decompress I/Q value, taking into account method, width, exponent, other input-specific methods */
2013 | /* TODO: pass in info needed for Modulation methods (reMask, csf, mcScaler values) gleaned from SE 4,5,23 */
2014 | static float decompress_value(uint32_t bits, uint32_t comp_method, uint8_t iq_width, uint32_t exponent)
2015 | {
2016 | switch (comp_method) {
2017 | case COMP_NONE0: /* no compression */
2018 | return uncompressed_to_float(bits);
2019 |
2020 | case COMP_BLOCK_FP1: /* block floating point */
2021 | case BFP_AND_SELECTIVE_RE5:
2022 | {
2023 | /* A.1.3 Block Floating Point Decompression Algorithm */
2024 | int32_t cPRB = bits;
2025 | uint32_t scaler = 1 << exponent; /* i.e. 2^exponent */
2026 |
2027 | /* Check last bit, in case we need to flip to -ve */
2028 | if (cPRB >= (1<<(iq_width-1))) {
2029 | cPRB -= (1<<iq_width);
2030 | }
2031 |
2032 | /* Unscale (8.1.3.1) */
2033 | cPRB *= scaler;
2034 | if (show_unscaled_values) {
2035 | return (float)cPRB;
2036 | }
2037 |
2038 | uint32_t mantissa_scale_factor = 1 << (iq_width-1); /* 2^(mantissabits-1) */
2039 | uint32_t exp_scale_factor = 1 << 15; /* 2^(2^exponentbits - 1 ) The exponent bit width is fixed to 4, so the maximum exponent is 15 */
2040 |
2041 | float ret = cPRB / ((float)(mantissa_scale_factor*exp_scale_factor));
2042 | return ret;
2043 | }
2044 |
2045 | case COMP_BLOCK_SCALE2:
2046 | case COMP_U_LAW3:
2047 | /* Not supported! But will be reported as expert info outside of this function! */
2048 | return 0.0;
2049 |
2050 | case COMP_MODULATION4:
2051 | case MOD_COMPR_AND_SELECTIVE_RE6:
2052 | /* TODO: ! */
2053 | return 0.0;
2054 |
2055 |
2056 | default:
2057 | /* Not supported! But will be reported as expert info outside of this function! */
2058 | return 0.0;
2059 | }
2060 | }
2061 |
2062 | /* Out-of-range value used for special case */
2063 | #define ORPHAN_BUNDLE_NUMBER999 999
2064 |
2065 | /* Bundle of PRBs/TRX I/Q samples (ext 11) */
2066 | static uint32_t dissect_bfw_bundle(tvbuff_t *tvb, proto_tree *tree, packet_info *pinfo, unsigned offset,
2067 | proto_item *comp_meth_ti, uint32_t bfwcomphdr_comp_meth,
2068 | uint32_t num_weights_per_bundle,
2069 | uint8_t iq_width,
2070 | unsigned bundle_number,
2071 | unsigned first_prb, unsigned last_prb, bool_Bool is_orphan)
2072 | {
2073 | /* Set bundle name */
2074 | char bundle_name[32];
2075 | if (!is_orphan) {
2076 | snprintf(bundle_name, 32, "Bundle %3u", bundle_number);
2077 | }
2078 | else {
2079 | g_strlcpy(bundle_name, "Orphaned ", 32);
2080 | }
2081 |
2082 | /* Create Bundle root */
2083 | proto_item *bundle_ti;
2084 | if (first_prb != last_prb) {
2085 | bundle_ti = proto_tree_add_string_format(tree, hf_oran_bfw_bundle,
2086 | tvb, offset, 0, "",
2087 | "%s: (PRBs %3u-%3u)",
2088 | bundle_name,
2089 | first_prb, last_prb);
2090 | }
2091 | else {
2092 | bundle_ti = proto_tree_add_string_format(tree, hf_oran_bfw_bundle,
2093 | tvb, offset, 0, "",
2094 | "%s: (PRB %3u)",
2095 | bundle_name,
2096 | first_prb);
2097 | }
2098 | proto_tree *bundle_tree = proto_item_add_subtree(bundle_ti, ett_oran_bfw_bundle);
2099 |
2100 | /* Generated bundle id */
2101 | proto_item *bundleid_ti = proto_tree_add_uint(bundle_tree, hf_oran_bfw_bundle_id, tvb, 0, 0,
2102 | bundle_number);
2103 | proto_item_set_generated(bundleid_ti);
2104 | proto_item_set_hidden(bundleid_ti);
2105 |
2106 | /* bfwCompParam */
2107 | bool_Bool compression_method_supported = false0;
2108 | unsigned exponent = 0;
2109 | unsigned num_trx_entries = 0;
2110 | uint16_t *trx_entries;
2111 | offset = dissect_bfwCompParam(tvb, bundle_tree, pinfo, offset, comp_meth_ti,
2112 | &bfwcomphdr_comp_meth, &exponent, &compression_method_supported,
2113 | &num_trx_entries, &trx_entries);
2114 |
2115 | /* Can't show details of unsupported compression method */
2116 | if (!compression_method_supported) {
2117 | /* Don't know how to show, so give up */
2118 | return offset;
2119 | }
2120 |
2121 | /* Create Bundle subtree */
2122 | int bit_offset = offset*8;
2123 | int bfw_offset;
2124 | int prb_offset = offset;
2125 |
2126 | /* contInd */
2127 | proto_tree_add_item(bundle_tree, hf_oran_cont_ind,
2128 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2129 | /* beamId */
2130 | uint32_t beam_id;
2131 | proto_tree_add_item_ret_uint(bundle_tree, hf_oran_beam_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &beam_id);
2132 | proto_item_append_text(bundle_ti, " (beamId:%u) ", beam_id);
2133 | bit_offset += 16;
2134 |
2135 | /* Number of weights per bundle (from preference) */
2136 | proto_item *wpb_ti = proto_tree_add_uint(bundle_tree, hf_oran_num_weights_per_bundle, tvb, 0, 0,
2137 | num_weights_per_bundle);
2138 | proto_item_set_generated(wpb_ti);
2139 |
2140 | /* Add the weights for this bundle. Overwrite with what was seen in bfwCompParam if beamspace */
2141 | if (num_trx_entries != 0) {
2142 | num_weights_per_bundle = num_trx_entries;
2143 | }
2144 |
2145 | for (unsigned w=0; w < num_weights_per_bundle; w++) {
2146 |
2147 | uint16_t trx_index = (num_trx_entries) ? trx_entries[w] : w+1;
2148 |
2149 | /* Create subtree */
2150 | bfw_offset = bit_offset / 8;
2151 | uint8_t bfw_extent = ((bit_offset + (iq_width*2)) / 8) - bfw_offset;
2152 | proto_item *bfw_ti = proto_tree_add_string_format(bundle_tree, hf_oran_bfw,
2153 | tvb, bfw_offset, bfw_extent,
2154 | "", "TRX %3u: (", trx_index);
2155 | proto_tree *bfw_tree = proto_item_add_subtree(bfw_ti, ett_oran_bfw);
2156 |
2157 | /* I */
2158 | /* Get bits, and convert to float. */
2159 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, iq_width, ENC_BIG_ENDIAN0x00000000);
2160 | float value = decompress_value(bits, bfwcomphdr_comp_meth, iq_width, exponent);
2161 | /* Add to tree. */
2162 | proto_tree_add_float_format_value(bfw_tree, hf_oran_bfw_i, tvb, bit_offset/8, (iq_width+7)/8, value, "#%u=%f", w, value);
2163 | bit_offset += iq_width;
2164 | proto_item_append_text(bfw_ti, "I%u=%f ", w, value);
2165 |
2166 | /* Q */
2167 | /* Get bits, and convert to float. */
2168 | bits = tvb_get_bits32(tvb, bit_offset, iq_width, ENC_BIG_ENDIAN0x00000000);
2169 | value = decompress_value(bits, bfwcomphdr_comp_meth, iq_width, exponent);
2170 | /* Add to tree. */
2171 | proto_tree_add_float_format_value(bfw_tree, hf_oran_bfw_q, tvb, bit_offset/8, (iq_width+7)/8, value, "#%u=%f", w, value);
2172 | bit_offset += iq_width;
2173 | proto_item_append_text(bfw_ti, "Q%u=%f)", w, value);
2174 | }
2175 |
2176 | /* Set extent of bundle */
2177 | proto_item_set_len(bundle_ti, (bit_offset+7)/8 - prb_offset);
2178 |
2179 | return (bit_offset+7)/8;
2180 | }
2181 |
2182 | /* Return new bit offset. in/out will always be byte-aligned.. */
2183 | static int dissect_ciCompParam(tvbuff_t *tvb, proto_tree *tree, packet_info *pinfo _U___attribute__((unused)), unsigned bit_offset,
2184 | unsigned comp_meth, uint8_t *exponent)
2185 | {
2186 | if (comp_meth == COMP_NONE0) {
2187 | /* Nothing in frame so don't even create subtree */
2188 | return bit_offset;
2189 | }
2190 |
2191 | /* Subtree */
2192 | proto_item *cicompparam_ti = proto_tree_add_string_format(tree, hf_oran_ciCompParam,
2193 | tvb, bit_offset/8, 1, "",
2194 | "ciCompParam");
2195 | proto_tree *cicompparam_tree = proto_item_add_subtree(cicompparam_ti, ett_oran_cicompparam);
2196 | uint32_t ci_exponent;
2197 |
2198 | /* Contents differ by compression method */
2199 | switch (comp_meth) {
2200 | case COMP_BLOCK_FP1:
2201 | proto_tree_add_item(cicompparam_tree, hf_oran_reserved_4bits, tvb, bit_offset/8, 1, ENC_NA0x00000000);
2202 | proto_tree_add_item_ret_uint(cicompparam_tree, hf_oran_exponent,
2203 | tvb, bit_offset/8, 1, ENC_BIG_ENDIAN0x00000000, &ci_exponent);
2204 | *exponent = ci_exponent;
2205 | proto_item_append_text(cicompparam_ti, " (Exponent=%u)", ci_exponent);
2206 | bit_offset += 8; /* one byte */
2207 | break;
2208 | case COMP_BLOCK_SCALE2:
2209 | /* Separate into integer (1) and fractional (7) bits? */
2210 | proto_tree_add_item(cicompparam_tree, hf_oran_blockScaler,
2211 | tvb, bit_offset/8, 1, ENC_BIG_ENDIAN0x00000000);
2212 | bit_offset += 8;
2213 | break;
2214 | case COMP_U_LAW3:
2215 | /* compBitWidth, compShift (4 bits each) */
2216 | proto_tree_add_item(cicompparam_tree, hf_oran_compBitWidth,
2217 | tvb, bit_offset/8, 1, ENC_BIG_ENDIAN0x00000000);
2218 | proto_tree_add_item(cicompparam_tree, hf_oran_compShift,
2219 | tvb, bit_offset/8, 1, ENC_BIG_ENDIAN0x00000000);
2220 | bit_offset += 8;
2221 | break;
2222 |
2223 | default:
2224 | /* reserved, ? bytes of zeros.. */
2225 | break;
2226 | }
2227 |
2228 | return bit_offset;
2229 | }
2230 |
2231 | /* frameStructure (7.5.2.13) */
2232 | static unsigned dissect_frame_structure(proto_item *tree, tvbuff_t *tvb, unsigned offset,
2233 | uint32_t subframeId, uint32_t slotId)
2234 | {
2235 | uint32_t scs;
2236 | /* FFT Size (4 bits) */
2237 | proto_tree_add_item(tree, hf_oran_frameStructure_fft, tvb, offset, 1, ENC_NA0x00000000);
2238 | /* Subcarrier spacing (SCS) */
2239 | proto_tree_add_item_ret_uint(tree, hf_oran_frameStructure_subcarrier_spacing, tvb, offset, 1, ENC_NA0x00000000, &scs);
2240 |
2241 | /* Show slot within frame as a generated field. See table 7.5.13-3 */
2242 | uint32_t slots_per_subframe = 1;
2243 | if (scs <= 4) {
2244 | slots_per_subframe = 1 << scs;
2245 | }
2246 | if (scs <= 4 || scs >= 12) {
2247 | proto_item *ti = proto_tree_add_uint(tree, hf_oran_slot_within_frame, tvb, 0, 0,
2248 | (slots_per_subframe*subframeId) + slotId);
2249 | proto_item_set_generated(ti);
2250 | }
2251 | return offset + 1;
2252 | }
2253 |
2254 | static unsigned dissect_csf(proto_item *tree, tvbuff_t *tvb, unsigned bit_offset,
2255 | unsigned iq_width, bool_Bool *p_csf)
2256 | {
2257 | proto_item *csf_ti;
2258 | uint64_t csf;
2259 | csf_ti = proto_tree_add_bits_ret_val(tree, hf_oran_csf, tvb, bit_offset, 1, &csf, ENC_BIG_ENDIAN0x00000000);
2260 | if (csf) {
2261 | /* Table 7.7.4.2-1 Constellation shift definition (index is udIqWidth) */
2262 | const char* shift_value[] = { "n/a", "1/2", "1/4", "1/8", "1/16", "1/32" };
2263 | if (iq_width >=1 && iq_width <= 5) {
2264 | proto_item_append_text(csf_ti, " (Shift Value is %s)", shift_value[iq_width]);
2265 | }
2266 | }
2267 |
2268 | /* Set out parameter */
2269 | if (p_csf != NULL((void*)0)) {
2270 | *p_csf = (csf!=0);
2271 | }
2272 | return bit_offset+1;
2273 | }
2274 |
2275 |
2276 | /* Section 7.
2277 | * N.B. these are the green parts of the tables showing Section Types, differing by section Type */
2278 | static int dissect_oran_c_section(tvbuff_t *tvb, proto_tree *tree, packet_info *pinfo,
2279 | flow_state_t* state,
2280 | uint32_t sectionType, oran_tap_info *tap_info, proto_item *protocol_item,
2281 | uint32_t subframeId, uint32_t slotId,
2282 | uint8_t ci_iq_width, uint8_t ci_comp_meth, unsigned ci_comp_opt,
2283 | unsigned num_sinr_per_prb)
2284 | {
2285 | unsigned offset = 0;
2286 | proto_tree *c_section_tree = NULL((void*)0);
2287 | proto_item *sectionHeading = NULL((void*)0);
2288 |
2289 | /* Section subtree */
2290 | sectionHeading = proto_tree_add_string_format(tree, hf_oran_c_section,
2291 | tvb, offset, 0, "", "Section");
2292 | c_section_tree = proto_item_add_subtree(sectionHeading, ett_oran_c_section);
2293 |
2294 | uint32_t sectionId = 0;
2295 |
2296 | uint32_t startPrbc=0, startPrbu=0;
2297 | uint32_t numPrbc=0, numPrbu=0;
2298 | uint32_t ueId = 0;
2299 | proto_item *ueId_ti = NULL((void*)0);
2300 | uint32_t beamId = 0;
2301 | proto_item *beamId_ti = NULL((void*)0);
2302 | bool_Bool beamId_ignored = false0;
2303 |
2304 | proto_item *numsymbol_ti = NULL((void*)0);
2305 | bool_Bool numsymbol_ignored = false0;
2306 |
2307 | proto_item *numprbc_ti = NULL((void*)0);
2308 |
2309 | /* Config affecting ext11 bundles (initially unset) */
2310 | ext11_settings_t ext11_settings;
2311 | memset(&ext11_settings, 0, sizeof(ext11_settings));
2312 |
2313 | /* Section Type 10 needs to keep track of PRB range that should be reported
2314 | for msgTypeId=5 (Interference plus Noise for unallocated PRBs) */
2315 | /* All PRBs start as false */
2316 | #define MAX_PRBS273 273
2317 | bool_Bool prbs_for_st10_type5[MAX_PRBS273];
2318 | memset(&prbs_for_st10_type5, 0, sizeof(prbs_for_st10_type5));
2319 |
2320 |
2321 | #define MAX_UEIDS16 16
2322 | uint32_t ueids[MAX_UEIDS16];
2323 | uint32_t number_of_ueids = 0;
2324 |
2325 | bool_Bool extension_flag = false0;
2326 |
2327 | /* These sections (ST0, ST1, ST2, ST3, ST5, ST9, ST10, ST11) are similar, so handle as common with per-type differences */
2328 | if (((sectionType <= SEC_C_UE_SCHED) || (sectionType >= SEC_C_SINR_REPORTING)) &&
1 | Assuming 'sectionType' is > SEC_C_UE_SCHED | →
2 | ← | Assuming 'sectionType' is < SEC_C_SINR_REPORTING | →
2329 | (sectionType != SEC_C_SLOT_CONTROL)) {
2330 |
2331 | /* sectionID */
2332 | proto_item *ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_section_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &sectionId);
2333 | if (sectionId == 4095) {
2334 | proto_item_append_text(ti, " (not default coupling C/U planes using sectionId)");
2335 | }
2336 | offset++;
2337 |
2338 | if (tap_info->num_section_ids < MAX_SECTION_IDs32) {
2339 | tap_info->section_ids[tap_info->num_section_ids++] = sectionId;
2340 | }
2341 |
2342 | /* rb */
2343 | uint32_t rb;
2344 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_rb, tvb, offset, 1, ENC_NA0x00000000, &rb);
2345 | /* symInc (1 bit) */
2346 | if (sectionType != SEC_C_RRM_MEAS_REPORTS && /* Section Type 10 */
2347 | sectionType != SEC_C_REQUEST_RRM_MEAS) { /* Section Type 11 */
2348 | unsigned int sym_inc;
2349 | proto_item *sym_inc_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_symInc, tvb, offset, 1, ENC_NA0x00000000, &sym_inc);
2350 | if (sym_inc !=0 && (sectionType == SEC_C_SINR_REPORTING)) { /* Section Type 9 */
2351 | /* "0 shall be used" */
2352 | proto_item_append_text(sym_inc_ti, " (should be 0)");
2353 | }
2354 | }
2355 | else {
2356 | /* reserved (1 bit) */
2357 | proto_tree_add_item(c_section_tree, hf_oran_reserved_bit5, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2358 | }
2359 |
2360 | /* startPrbx and numPrbx */
2361 | if (sectionType == SEC_C_SINR_REPORTING) {
2362 | /* startPrbu (10 bits) */
2363 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_startPrbu, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPrbu);
2364 | offset += 2;
2365 | /* numPrbu */
2366 | numprbc_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_numPrbu, tvb, offset, 1, ENC_NA0x00000000, &numPrbu);
2367 | if (numPrbu == 0) {
2368 | proto_item_append_text(numprbc_ti, " (all PRBs - configured as %u)", pref_data_plane_section_total_rbs);
2369 | numPrbu = pref_data_plane_section_total_rbs;
2370 | }
2371 | offset += 1;
2372 | }
2373 | else {
2374 | /* startPrbc (10 bits) */
2375 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_startPrbc, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPrbc);
2376 | offset += 2;
2377 | /* numPrbc */
2378 | numprbc_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_numPrbc, tvb, offset, 1, ENC_NA0x00000000, &numPrbc);
2379 | if (numPrbc == 0) {
2380 | proto_item_append_text(numprbc_ti, " (all PRBs - configured as %u)", pref_data_plane_section_total_rbs);
2381 | /* TODO: should probably set to pref_data_plane_section_total_rbs, and define MAX_PRBS to > 273 ? */
2382 | numPrbc = MAX_PRBS273;
2383 | }
2384 | offset += 1;
2385 | }
2386 |
2387 | /* Start with range from section. May get changed by SE6, SE12, SE20 */
2388 | for (unsigned n=startPrbc; n < startPrbc+numPrbc; n++) {
2389 | if (n < MAX_PRBS273) {
2390 | prbs_for_st10_type5[n] = true1;
2391 | }
2392 | }
2393 |
2394 | if (sectionType != SEC_C_SINR_REPORTING) { /* Section Type 9 */
2395 | static int * const remask_flags[] = {
2396 | &hf_oran_reMask_re1,
2397 | &hf_oran_reMask_re2,
2398 | &hf_oran_reMask_re3,
2399 | &hf_oran_reMask_re4,
2400 | &hf_oran_reMask_re5,
2401 | &hf_oran_reMask_re6,
2402 | &hf_oran_reMask_re7,
2403 | &hf_oran_reMask_re8,
2404 | &hf_oran_reMask_re9,
2405 | &hf_oran_reMask_re10,
2406 | &hf_oran_reMask_re11,
2407 | &hf_oran_reMask_re12,
2408 | NULL((void*)0)
2409 | };
2410 |
2411 | /* reMask */
2412 | uint64_t remask;
2413 | proto_tree_add_bitmask_ret_uint64(c_section_tree, tvb, offset,
2414 | hf_oran_reMask, ett_oran_remask, remask_flags, ENC_BIG_ENDIAN0x00000000, &remask);
2415 | offset++;
2416 | /* numSymbol */
2417 | /* TODO: should warn if startSymbol + numSymbol would be > 14? */
2418 | uint32_t numSymbol;
2419 | numsymbol_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_numSymbol, tvb, offset, 1, ENC_NA0x00000000, &numSymbol);
2420 | if ((sectionType == SEC_C_RRM_MEAS_REPORTS) && (numSymbol != 14)) { /* Section type 10 */
2421 | proto_item_append_text(numsymbol_ti, " (for ST10, should be 14!)");
2422 | expert_add_info_format(pinfo, numsymbol_ti, &ei_oran_st10_numsymbol_not_14,
2423 | "numSymbol should be 14 for ST10 - found %u", numSymbol);
2424 | }
2425 | offset++;
2426 |
2427 | /* [ef] (extension flag) */
2428 | switch (sectionType) {
2429 | case SEC_C_UNUSED_RB: /* Section Type 0 */
2430 | case SEC_C_NORMAL: /* Section Type 1 */
2431 | case SEC_C_PRACH: /* Section Type 3 */
2432 | case SEC_C_UE_SCHED: /* Section Type 5 */
2433 | case SEC_C_RRM_MEAS_REPORTS: /* Section Type 10 */
2434 | case SEC_C_REQUEST_RRM_MEAS: /* Section Type 11 */
2435 | proto_tree_add_item_ret_boolean(c_section_tree, hf_oran_ef, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &extension_flag);
2436 | break;
2437 | default:
2438 | /* Other section types don't support extensions */
2439 | break;
2440 | }
2441 |
2442 | write_section_info(sectionHeading, pinfo, protocol_item, sectionId, startPrbc, numPrbc, rb);
2443 | proto_item_append_text(sectionHeading, ", Symbols: %2u", numSymbol);
2444 |
2445 | if (numPrbc == 0) {
2446 | /* Special case for all PRBs */
2447 | numPrbc = pref_data_plane_section_total_rbs;
2448 | startPrbc = 0; /* may already be 0... */
2449 | }
2450 | }
2451 | else {
2452 | /* Section Type 9 */
2453 | write_section_info(sectionHeading, pinfo, protocol_item, sectionId, startPrbu, numPrbu, rb);
2454 | proto_item_append_text(sectionHeading, ", numSinrPerPrb: %2u", num_sinr_per_prb);
2455 | }
2456 |
2457 | /* Section type specific fields (after 'numSymbol') */
2458 | switch (sectionType) {
2459 | case SEC_C_UNUSED_RB: /* Section Type 0 - Table 7.4.2-1 */
2460 | /* reserved (15 bits) */
2461 | proto_tree_add_item(c_section_tree, hf_oran_reserved_15bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
2462 | offset += 2;
2463 | break;
2464 |
2465 | case SEC_C_NORMAL: /* Section Type 1 - Table 7.4.3-1 */
2466 | /* beamId */
2467 | beamId_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &beamId);
2468 | offset += 2;
2469 |
2470 | proto_item_append_text(sectionHeading, ", BeamId: %d", beamId);
2471 | break;
2472 |
2473 | case SEC_C_PRACH: /* Section Type 3 - Table 7.4.5-1 */
2474 | {
2475 | /* beamId */
2476 | beamId_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &beamId);
2477 | offset += 2;
2478 |
2479 | /* freqOffset */
2480 | int32_t freqOffset; /* Yes, this is signed, so the implicit cast is intentional. */
2481 | proto_item *freq_offset_item = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_freqOffset, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000, &freqOffset);
2482 | freqOffset |= 0xff000000; /* Must sign-extend */
2483 | proto_item_set_text(freq_offset_item, "Frequency offset: %d \u0394f", freqOffset);
2484 | offset += 3;
2485 |
2486 | /* reserved */
2487 | proto_tree_add_item(c_section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000);
2488 | offset += 1;
2489 |
2490 | proto_item_append_text(sectionHeading, ", BeamId: %d, FreqOffset: %d \u0394f", beamId, freqOffset);
2491 | break;
2492 | }
2493 |
2494 | case SEC_C_UE_SCHED: /* Section Type 5 - Table 7.4.7-1 */
2495 | case SEC_C_RRM_MEAS_REPORTS: /* Section Type 10 - Table 7.4.12-1 */
2496 | /* ueId */
2497 | ueId_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_ueId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ueId);
2498 | offset += 2;
2499 | if (ueId == 0x7fff) {
2500 | proto_item_append_text(ueId_ti, " (PRBs not scheduled for eAxC ID in transport header)");
2501 | }
2502 | else {
2503 | ueids[number_of_ueids++] = ueId;
2504 | }
2505 |
2506 | proto_item_append_text(sectionHeading, ", UEId: %d", ueId);
2507 | break;
2508 |
2509 | case SEC_C_SINR_REPORTING: /* Section Type 9 - SINR Reporting */
2510 | {
2511 | /* Hidden filter for bf (DMFS-BF) */
2512 | proto_item *bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
2513 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
2514 |
2515 | unsigned bit_offset = offset*8;
2516 |
2517 | /* sinr iqWidth */
2518 | proto_item *iq_width_item = proto_tree_add_uint(c_section_tree, hf_oran_sinrCompHdrIqWidth_pref, tvb, 0, 0, pref_sample_bit_width_sinr);
2519 | proto_item_append_text(iq_width_item, " (from preferences)");
2520 | proto_item_set_generated(iq_width_item);
2521 |
2522 | /* sinr compMethod */
2523 | proto_item *sinr_comp_meth_item = proto_tree_add_uint(c_section_tree, hf_oran_sinrCompHdrMeth_pref, tvb, 0, 0, pref_iqCompressionSINR);
2524 | proto_item_append_text(sinr_comp_meth_item, " (from preferences)");
2525 | proto_item_set_generated(sinr_comp_meth_item);
2526 |
2527 | /* Add SINR entries for each PRB */
2528 | for (unsigned prb=0; prb < numPrbu; prb++) {
2529 | /* TODO: create a subtree for each PRB entry with good summary? */
2530 |
2531 | /* Each prb starts byte-aligned */
2532 | bit_offset = ((bit_offset+7)/8) * 8;
2533 |
2534 | /* N.B., using width/method from UL U-plane preferences, not certain that this is correct.. */
2535 |
2536 | /* sinrCompParam (udCompParam format, may be empty) */
2537 | uint32_t exponent = 0; /* N.B. init to silence warnings, but will always be set if read in COMP_BLOCK_FP case */
2538 | uint16_t sReSMask;
2539 | bit_offset = dissect_udcompparam(tvb, pinfo, c_section_tree, bit_offset/8,
2540 | pref_iqCompressionSINR, &exponent, &sReSMask,
2541 | true1) * 8; /* last param is for_sinr */
2542 |
2543 | /* sinrValues for this PRB. */
2544 | /* TODO: not sure how numSinrPerPrb interacts with rb==1... */
2545 | for (unsigned n=0; n < num_sinr_per_prb; n++) {
2546 | unsigned sinr_bits = tvb_get_bits32(tvb, bit_offset, pref_sample_bit_width_sinr, ENC_BIG_ENDIAN0x00000000);
2547 |
2548 | /* Using SINR compression settings from preferences */
2549 | float value = decompress_value(sinr_bits,
2550 | pref_iqCompressionSINR, pref_sample_bit_width_sinr,
2551 | exponent);
2552 | unsigned sample_len_in_bytes = ((bit_offset%8)+pref_sample_bit_width_sinr+7)/8;
2553 | proto_item *val_ti = proto_tree_add_float(c_section_tree, hf_oran_sinr_value, tvb,
2554 | bit_offset/8, sample_len_in_bytes, value);
2555 |
2556 | /* Show here which subcarriers share which values (they all divide 12..) */
2557 | if (num_sinr_per_prb == 12) {
2558 | proto_item_append_text(val_ti, " (PRB=%u, subcarrier %u)",
2559 | startPrbu+(prb*(rb+1)),
2560 | n*(12/num_sinr_per_prb));
2561 | }
2562 | else {
2563 | proto_item_append_text(val_ti, " (PRB=%u, subcarriers %u-%u)",
2564 | startPrbu+(prb*(rb+1)),
2565 | n*(12/num_sinr_per_prb), (n+1)*(12/num_sinr_per_prb)-1);
2566 | }
2567 | bit_offset += pref_sample_bit_width_sinr;
2568 | }
2569 |
2570 | /* 1-byte alignment per PRB (7.2.11) */
2571 | offset = (bit_offset+7)/8;
2572 | bit_offset = offset*8;
2573 | }
2574 | break;
2575 | }
2576 | case SEC_C_REQUEST_RRM_MEAS: /* Section Type 11 - Request RRM Measurements */
2577 | /* Reserved (15 bits) */
2578 | proto_tree_add_item(c_section_tree, hf_oran_reserved_15bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
2579 | offset += 2;
2580 | break;
2581 |
2582 | default:
2583 | break;
2584 | }
2585 | }
2586 | else if (sectionType == SEC_C_CH_INFO) { /* Section Type 6 */
3 | ← | Assuming 'sectionType' is equal to SEC_C_CH_INFO | →
4 | ← | Taking true branch | →
2587 | /* ef */
2588 | proto_tree_add_item_ret_boolean(c_section_tree, hf_oran_ef, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &extension_flag);
2589 | /* ueId */
2590 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_ueId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ueId);
2591 | offset += 2;
2592 | /* regularizationFactor */
2593 | proto_tree_add_item(c_section_tree, hf_oran_regularizationFactor, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
2594 | offset += 2;
2595 | /* reserved (4 bits) */
2596 | proto_tree_add_item(c_section_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_NA0x00000000);
2597 | /* rb ("Value=0 shall be set") */
2598 | uint32_t rb;
2599 | proto_item *rb_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_rb, tvb, offset, 1, ENC_NA0x00000000, &rb);
2600 | if (rb != 0) {
5 | ← | Assuming 'rb' is equal to 0 | →
6 | ← | Taking false branch | →
2601 | proto_item_append_text(rb_ti, " (should be set to 0)");
2602 | expert_add_info(pinfo, rb_ti, &ei_oran_st6_rb_shall_be_0);
2603 | }
2604 | /* symInc */
2605 | proto_tree_add_item(c_section_tree, hf_oran_symInc, tvb, offset, 1, ENC_NA0x00000000);
2606 | /* startPrbc */
2607 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_startPrbc, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPrbc);
2608 | offset += 2;
2609 | /* numPrbc */
2610 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_numPrbc, tvb, offset, 1, ENC_NA0x00000000, &numPrbc);
2611 | offset += 1;
2612 |
2613 | /* Hidden filter for bf */
2614 | proto_item *bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
2615 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
2616 |
2617 | /* ciIsample,ciQsample pairs */
2618 | unsigned m;
2619 | unsigned prb;
2620 | uint32_t bit_offset = offset*8;
2621 |
2622 | /* Antenna count from preference */
2623 | unsigned num_trx = pref_num_bf_antennas;
2624 |
2625 | write_channel_section_info(sectionHeading, pinfo,
2626 | sectionId, ueId, startPrbc, numPrbc, num_trx);
2627 |
2628 | bool_Bool first_prb = true1;
2629 | uint8_t exponent = 0;
2630 | for (prb=startPrbc; prb < startPrbc+numPrbc; prb++) {
7 | ← | Assuming the condition is false | →
8 | ← | Loop condition is false. Execution continues on line 2681 | →
2631 |
2632 | /* PRB subtree */
2633 | unsigned prb_start_offset = bit_offset;
2634 | proto_item *prb_ti = proto_tree_add_string_format(c_section_tree, hf_oran_samples_prb,
2635 | tvb, bit_offset/8, 0,
2636 | "", "PRB=%u", prb);
2637 | proto_tree *prb_tree = proto_item_add_subtree(prb_ti, ett_oran_prb_cisamples);
2638 |
2639 | /* There may be a ciCompParam here.. */
2640 | if (first_prb || ci_comp_opt==1) {
2641 | bit_offset = dissect_ciCompParam(tvb, prb_tree, pinfo, bit_offset, ci_comp_meth, &exponent);
2642 | }
2643 | first_prb = false0;
2644 |
2645 | /* Antennas */
2646 | for (m=0; m < num_trx; m++) {
2647 |
2648 | unsigned sample_offset = bit_offset / 8;
2649 | uint8_t sample_extent = ((bit_offset + (ci_iq_width*2)) / 8) - sample_offset;
2650 |
2651 | /* Create subtree for antenna */
2652 | proto_item *sample_ti = proto_tree_add_string_format(prb_tree, hf_oran_ciSample,
2653 | tvb, sample_offset, sample_extent,
2654 | "", "TRX=%2u: ", m);
2655 | proto_tree *sample_tree = proto_item_add_subtree(sample_ti, ett_oran_cisample);
2656 |
2657 | /* I */
2658 | /* Get bits, and convert to float. */
2659 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, ci_iq_width, ENC_BIG_ENDIAN0x00000000);
2660 | float value = decompress_value(bits, ci_comp_meth, ci_iq_width, exponent);
2661 |
2662 | /* Add to tree. */
2663 | proto_tree_add_float_format_value(sample_tree, hf_oran_ciIsample, tvb, bit_offset/8, (ci_iq_width+7)/8, value, "#%u=%f", m, value);
2664 | bit_offset += ci_iq_width;
2665 | proto_item_append_text(sample_ti, "I%u=%f ", m, value);
2666 |
2667 | /* Q */
2668 | /* Get bits, and convert to float. */
2669 | bits = tvb_get_bits32(tvb, bit_offset, ci_iq_width, ENC_BIG_ENDIAN0x00000000);
2670 | value = decompress_value(bits, ci_comp_meth, ci_iq_width, exponent);
2671 |
2672 | /* Add to tree. */
2673 | proto_tree_add_float_format_value(sample_tree, hf_oran_ciQsample, tvb, bit_offset/8, (ci_iq_width+7)/8, value, "#%u=%f", m, value);
2674 | bit_offset += ci_iq_width;
2675 | proto_item_append_text(sample_ti, "Q%u=%f ", m, value);
2676 | }
2677 | proto_item_set_len(prb_ti, (bit_offset-prb_start_offset+7)/8);
2678 | }
2679 |
2680 | /* Pad out by 1 or 4 bytes, according to preference */
2681 | if (!st6_4byte_alignment) {
9 | ← | Assuming 'st6_4byte_alignment' is true | →
10 | ← | Taking false branch | →
2682 | offset = (bit_offset + 7) / 8;
2683 | }
2684 | else {
2685 | int mode = bit_offset % 32;
2686 | if (mode
10.1 | 'mode' is not equal to 0
!= 0) {
11 | ← | Taking true branch | →
2687 | offset = (bit_offset + (32-mode))/8;
2688 | }
2689 | else {
2690 | offset = bit_offset/8;
2691 | }
2692 | }
2693 | proto_item_set_end(c_section_tree, tvb, offset);
2694 | }
2695 |
2696 | bool_Bool seen_se10 = false0;
2697 | uint32_t numPortc = 0;
2698 | proto_item *bf_ti = NULL((void*)0);
2699 |
2700 | /* Section extension commands */
2701 | while (extension_flag) {
12 | ← | Loop condition is true. Entering loop body | →
2702 | int extension_start_offset = offset;
2703 |
2704 | /* Prefetch extType so can use specific extension type ett */
2705 | uint32_t exttype = tvb_get_uint8(tvb, offset) & 0x7f;
2706 | uint32_t exttype_ett_index = exttype;
2707 | if (exttype == 0 || exttype > HIGHEST_EXTTYPE28) {
13 | ← | Assuming 'exttype' is not equal to 0 | →
14 | ← | Assuming 'exttype' is <= HIGHEST_EXTTYPE | →
15 | ← | Taking false branch | →
2708 | /* Just use first one if out of range */
2709 | exttype_ett_index = 1;
2710 | }
2711 |
2712 | /* Create subtree for each extension (with summary) */
2713 | proto_item *extension_ti = proto_tree_add_string_format(c_section_tree, hf_oran_extension,
2714 | tvb, offset, 0, "", "Extension");
2715 | proto_tree *extension_tree = proto_item_add_subtree(extension_ti, ett_oran_c_section_extension[exttype_ett_index-1]);
2716 |
2717 | /* ef (i.e. another extension after this one?) */
2718 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_ef, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &extension_flag);
2719 |
2720 | /* extType */
2721 | proto_item *exttype_ti;
2722 | exttype_ti = proto_tree_add_item(extension_tree, hf_oran_exttype, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2723 | offset++;
2724 | proto_item_append_text(sectionHeading, " (ext-%u)", exttype);
2725 |
2726 | proto_item_append_text(extension_ti, " (ext-%u: %s)", exttype, val_to_str_const(exttype, exttype_vals, "Reserved"));
2727 |
2728 | /* Don't tap if out of range. */
2729 | if (exttype
15.1 | 'exttype' is > 0
> 0 && exttype
15.2 | 'exttype' is <= HIGHEST_EXTTYPE
<= HIGHEST_EXTTYPE28) {
16 | ← | Taking true branch | →
2730 | tap_info->extensions[exttype] = true1;
2731 | }
2732 |
2733 | /* Is this SE allowed for this section type? */
2734 | if (!se_allowed_in_st(exttype, sectionType)) {
17 | ← | Assuming the condition is false | →
2735 | expert_add_info_format(pinfo, extension_tree, &ei_oran_se_on_unsupported_st,
2736 | "SE %u (%s) should not appear in ST %u (%s)!",
2737 | exttype, val_to_str_const(exttype, exttype_vals, "Reserved"),
2738 | sectionType, rval_to_str_const(sectionType, section_types, "Unknown"));
2739 | }
2740 |
2741 |
2742 | /* extLen (number of 32-bit words) */
2743 | uint32_t extlen_len = ((exttype==11)||(exttype==19)||(exttype==20)) ? 2 : 1; /* Extensions 11/19/20 are special */
18 | ← | Assuming 'exttype' is not equal to 11 | →
19 | ← | Assuming 'exttype' is equal to 19 | →
2744 | uint32_t extlen;
2745 | proto_item *extlen_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_extlen, tvb,
2746 | offset, extlen_len, ENC_BIG_ENDIAN0x00000000, &extlen);
2747 | proto_item_append_text(extlen_ti, " (%u bytes)", extlen*4);
2748 | offset += extlen_len;
2749 | if (extlen == 0) {
20 | ← | Assuming 'extlen' is not equal to 0 | →
21 | ← | Taking false branch | →
2750 | expert_add_info_format(pinfo, extlen_ti, &ei_oran_extlen_zero,
2751 | "extlen value of 0 is reserved");
2752 | /* Break out to avoid infinitely looping! */
2753 | break;
2754 | }
2755 |
2756 | bool_Bool ext_unhandled = false0;
2757 |
2758 | switch (exttype) {
22 | ← | Control jumps to 'case 19:' at line 3694 | →
2759 |
2760 | case 1: /* SE 1: Beamforming Weights */
2761 | {
2762 | uint32_t bfwcomphdr_iq_width, bfwcomphdr_comp_meth;
2763 | proto_item *comp_meth_ti = NULL((void*)0);
2764 |
2765 | /* Hidden filter for bf */
2766 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
2767 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
2768 |
2769 | /* bfwCompHdr (2 subheaders - bfwIqWidth and bfwCompMeth)*/
2770 | offset = dissect_bfwCompHdr(tvb, extension_tree, offset,
2771 | &bfwcomphdr_iq_width, &bfwcomphdr_comp_meth, &comp_meth_ti);
2772 |
2773 | /* bfwCompParam */
2774 | uint32_t exponent = 0;
2775 | bool_Bool compression_method_supported = false0;
2776 | unsigned num_trx = 0;
2777 | uint16_t *trx; /* ptr to array */
2778 | offset = dissect_bfwCompParam(tvb, extension_tree, pinfo, offset, comp_meth_ti,
2779 | &bfwcomphdr_comp_meth, &exponent, &compression_method_supported,
2780 | &num_trx, &trx);
2781 |
2782 | /* Can't show details of unsupported compression method */
2783 | if (!compression_method_supported) {
2784 | break;
2785 | }
2786 |
2787 | /* We know:
2788 | - iq_width (above)
2789 | - numBfWeights (taken from preference)
2790 | - remaining bytes in extension
2791 | We can therefore derive TRX (number of antennas).
2792 | */
2793 |
2794 | bool_Bool using_array = false0;
2795 |
2796 | /* I & Q samples
2797 | May know how many entries from activeBeamspaceCoefficientMask. */
2798 | if (num_trx == 0) {
2799 | /* Don't know how many there will be, so just fill available bytes... */
2800 | unsigned weights_bytes = (extlen*4)-3;
2801 | unsigned num_weights_pairs = (weights_bytes*8) / (bfwcomphdr_iq_width*2);
2802 | num_trx = num_weights_pairs;
2803 | }
2804 | else {
2805 | using_array = true1;
2806 | num_trx = pref_num_bf_antennas;
2807 | }
2808 |
2809 | int bit_offset = offset*8;
2810 |
2811 | for (unsigned n=0; n < num_trx; n++) {
2812 | /* Create antenna subtree */
2813 | int bfw_offset = bit_offset / 8;
2814 |
2815 | uint16_t trx_index = (using_array) ? trx[n] : n+1;
2816 |
2817 | proto_item *bfw_ti = proto_tree_add_string_format(extension_tree, hf_oran_bfw,
2818 | tvb, bfw_offset, 0, "", "TRX %3u: (", trx_index);
2819 | proto_tree *bfw_tree = proto_item_add_subtree(bfw_ti, ett_oran_bfw);
2820 |
2821 | /* I value */
2822 | /* Get bits, and convert to float. */
2823 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
2824 | float value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent);
2825 | /* Add to tree. */
2826 | proto_tree_add_float(bfw_tree, hf_oran_bfw_i, tvb, bit_offset/8,
2827 | (bfwcomphdr_iq_width+7)/8, value);
2828 | bit_offset += bfwcomphdr_iq_width;
2829 | proto_item_append_text(bfw_ti, "I=%f ", value);
2830 |
2831 | /* Leave a gap between I and Q values */
2832 | proto_item_append_text(bfw_ti, " ");
2833 |
2834 | /* Q value */
2835 | /* Get bits, and convert to float. */
2836 | bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
2837 | value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent);
2838 | /* Add to tree. */
2839 | proto_tree_add_float(bfw_tree, hf_oran_bfw_q, tvb, bit_offset/8,
2840 | (bfwcomphdr_iq_width+7)/8, value);
2841 | bit_offset += bfwcomphdr_iq_width;
2842 | proto_item_append_text(bfw_ti, "Q=%f", value);
2843 |
2844 | proto_item_append_text(bfw_ti, ")");
2845 | proto_item_set_len(bfw_ti, (bit_offset+7)/8 - bfw_offset);
2846 | }
2847 | /* Need to round to next byte */
2848 | offset = (bit_offset+7)/8;
2849 |
2850 | break;
2851 | }
2852 |
2853 | case 2: /* SE 2: Beamforming attributes */
2854 | {
2855 | /* Hidden filter for bf */
2856 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
2857 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
2858 |
2859 | /* bfaCompHdr (get widths of fields to follow) */
2860 | uint32_t bfAzPtWidth, bfZePtWidth, bfAz3ddWidth, bfZe3ddWidth;
2861 | /* subtree */
2862 | proto_item *bfa_ti = proto_tree_add_string_format(extension_tree, hf_oran_bfaCompHdr,
2863 | tvb, offset, 2, "", "bfaCompHdr");
2864 | proto_tree *bfa_tree = proto_item_add_subtree(bfa_ti, ett_oran_bfacomphdr);
2865 |
2866 | /* reserved (2 bits) */
2867 | proto_tree_add_item(bfa_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2868 | /* bfAzPtWidth (3 bits) */
2869 | proto_tree_add_item_ret_uint(bfa_tree, hf_oran_bfAzPtWidth, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &bfAzPtWidth);
2870 | /* bfZePtWidth (3 bits) */
2871 | proto_tree_add_item_ret_uint(bfa_tree, hf_oran_bfZePtWidth, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &bfZePtWidth);
2872 | offset += 1;
2873 |
2874 | /* reserved (2 bits) */
2875 | proto_tree_add_item(bfa_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2876 | /* bfAz3ddWidth (3 bits) */
2877 | proto_tree_add_item_ret_uint(bfa_tree, hf_oran_bfAz3ddWidth, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &bfAz3ddWidth);
2878 | /* bfZe3ddWidth (3 bits) */
2879 | proto_tree_add_item_ret_uint(bfa_tree, hf_oran_bfZe3ddWidth, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &bfZe3ddWidth);
2880 | offset += 1;
2881 |
2882 | unsigned bit_offset = offset*8;
2883 |
2884 | /* bfAzPt */
2885 | if (bfAzPtWidth > 0) {
2886 | proto_tree_add_bits_item(extension_tree, hf_oran_bfAzPt, tvb, bit_offset, bfAzPtWidth+1, ENC_BIG_ENDIAN0x00000000);
2887 | bit_offset += (bfAzPtWidth+1);
2888 | }
2889 | /* bfZePt */
2890 | if (bfZePtWidth > 0) {
2891 | proto_tree_add_bits_item(extension_tree, hf_oran_bfZePt, tvb, bit_offset, bfZePtWidth+1, ENC_BIG_ENDIAN0x00000000);
2892 | bit_offset += (bfZePtWidth+1);
2893 | }
2894 | /* bfAz3dd */
2895 | if (bfAz3ddWidth > 0) {
2896 | proto_tree_add_bits_item(extension_tree, hf_oran_bfAz3dd, tvb, bit_offset, bfAz3ddWidth+1, ENC_BIG_ENDIAN0x00000000);
2897 | bit_offset += (bfAz3ddWidth+1);
2898 | }
2899 | /* bfZe3dd */
2900 | if (bfZe3ddWidth > 0) {
2901 | proto_tree_add_bits_item(extension_tree, hf_oran_bfZe3dd, tvb, bit_offset, bfZe3ddWidth+1, ENC_BIG_ENDIAN0x00000000);
2902 | bit_offset += (bfZe3ddWidth+1);
2903 | }
2904 |
2905 | /* Pad to next byte (unless last 2 fields already fit in this one) */
2906 | if ((bit_offset % 8) > 2) {
2907 | offset = (bit_offset+7) / 8;
2908 | }
2909 | else {
2910 | offset = bit_offset / 8;
2911 | }
2912 |
2913 | /* bfAzSl (3 bits) */
2914 | proto_tree_add_item(extension_tree, hf_oran_bfAzSl, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2915 | /* bfZeSl (3 bits) */
2916 | proto_tree_add_item(extension_tree, hf_oran_bfZeSl, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2917 | offset += 1;
2918 | break;
2919 | }
2920 |
2921 | case 3: /* SE 3: DL precoding parameters */
2922 | {
2923 | /* codebookindex (8 bits) */
2924 | /* "This parameter is not used and shall be set to zero." */
2925 | proto_tree_add_item(extension_tree, hf_oran_codebook_index, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2926 | offset += 1;
2927 | /* layerid */
2928 | uint32_t layerid;
2929 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_layerid, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &layerid);
2930 | /* numLayers */
2931 | proto_tree_add_item(extension_tree, hf_oran_numlayers, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2932 | offset += 1;
2933 |
2934 | /* Stop here for non-first data layer */
2935 | if (layerid != 0 && layerid != 0xf) {
2936 | break;
2937 | }
2938 |
2939 | /* First data layer case */
2940 | /* txScheme */
2941 | proto_tree_add_item(extension_tree, hf_oran_txscheme, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2942 | /* crsReMask */
2943 | proto_tree_add_item(extension_tree, hf_oran_crs_remask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
2944 | offset += 2;
2945 |
2946 | /* crsShift (1 bit) */
2947 | proto_tree_add_item(extension_tree, hf_oran_crs_shift, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2948 | /* reserved (3 bits) */
2949 | proto_tree_add_item(extension_tree, hf_oran_reserved_bits123, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2950 | /* crsSymNum (4 bits) */
2951 | proto_tree_add_item(extension_tree, hf_oran_crs_symnum, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2952 | offset += 1;
2953 | /* reserved */
2954 | proto_tree_add_item(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2955 | offset += 1;
2956 |
2957 | /* reserved (1 bit) */
2958 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2959 | /* beamIdAP1 (15 bits) */
2960 | proto_tree_add_item(extension_tree, hf_oran_beamid_ap1, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
2961 | offset += 2;
2962 | /* reserved (1 bit) */
2963 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2964 | /* beamIdAP2 (15 bits) */
2965 | proto_tree_add_item(extension_tree, hf_oran_beamid_ap2, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
2966 | offset += 2;
2967 | /* reserved (1 bit) */
2968 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2969 | /* beamIdAP3 (15 bits) */
2970 | proto_tree_add_item(extension_tree, hf_oran_beamid_ap3, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
2971 | offset += 2;
2972 | break;
2973 | }
2974 |
2975 | case 4: /* SE 4: Modulation compression params (5.4.7.4) */
2976 | {
2977 | /* csf */
2978 | dissect_csf(extension_tree, tvb, offset*8, ci_iq_width, NULL((void*)0));
2979 |
2980 | /* modCompScaler */
2981 | uint32_t modCompScaler;
2982 | proto_item *ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_modcompscaler,
2983 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &modCompScaler);
2984 | offset += 2;
2985 |
2986 | /* Work out and show floating point value too. exponent and mantissa are both unsigned */
2987 | uint16_t exponent = (modCompScaler >> 11) & 0x000f; /* m.s. 4 bits */
2988 | uint16_t mantissa = modCompScaler & 0x07ff; /* l.s. 11 bits */
2989 | double value = ((double)mantissa/(1<<11)) * (1.0 / (1 << exponent));
2990 | proto_item_append_text(ti, " (%f)", value);
2991 |
2992 | /* TODO: need to store these in per-section data in state that gets looked up by U-Plane */
2993 | break;
2994 | }
2995 |
2996 | case 5: /* SE 5: Modulation Compression Additional Parameters (7.7.5) */
2997 | {
2998 | /* Applies only to section types 1,3 and 5 */
2999 | /* N.B. there may be multiple instances of this SE in the same frame */
3000 |
3001 | /* There may be one or 2 entries, depending upon extlen */
3002 | int sets = 1, reserved_bits = 0;
3003 | switch (extlen) {
3004 | case 2:
3005 | sets = 1;
3006 | reserved_bits = 20;
3007 | break;
3008 | case 3:
3009 | sets = 2;
3010 | reserved_bits = 24;
3011 | break;
3012 | case 4:
3013 | /* sets can be 3 or 4, depending upon whether last 28 bits are 0.. */
3014 | if ((tvb_get_ntohl(tvb, offset+10) & 0x0fffffff) == 0) {
3015 | sets = 3;
3016 | reserved_bits = 28;
3017 | }
3018 | else {
3019 | sets = 4;
3020 | reserved_bits = 0;
3021 | }
3022 | break;
3023 |
3024 | default:
3025 | /* Malformed error!!! */
3026 | expert_add_info_format(pinfo, extlen_ti, &ei_oran_extlen_wrong,
3027 | "For section 5, extlen must be 2, 3 or 4, but %u was dissected",
3028 | extlen);
3029 | break;
3030 | }
3031 |
3032 | unsigned bit_offset = offset*8;
3033 |
3034 | for (int n=0; n < sets; n++) {
3035 | /* Subtree for each set */
3036 | unsigned set_start_offset = bit_offset/8;
3037 | proto_item *set_ti = proto_tree_add_string(extension_tree, hf_oran_modcomp_param_set,
3038 | tvb, set_start_offset, 0, "");
3039 | proto_tree *set_tree = proto_item_add_subtree(set_ti, ett_oran_modcomp_param_set);
3040 |
3041 | uint64_t mcScaleReMask, mcScaleOffset;
3042 | bool_Bool csf;
3043 |
3044 | /* mcScaleReMask (12 bits) */
3045 | proto_tree_add_bits_ret_val(set_tree, hf_oran_mc_scale_re_mask, tvb, bit_offset, 12, &mcScaleReMask, ENC_BIG_ENDIAN0x00000000);
3046 | bit_offset += 12;
3047 | /* csf (1 bit) */
3048 | bit_offset = dissect_csf(set_tree, tvb, bit_offset, ci_iq_width, &csf);
3049 | /* mcScaleOffset (15 bits) */
3050 | proto_item *ti = proto_tree_add_bits_ret_val(set_tree, hf_oran_mc_scale_offset, tvb, bit_offset, 15, &mcScaleOffset, ENC_BIG_ENDIAN0x00000000);
3051 | uint16_t exponent = (mcScaleOffset >> 11) & 0x000f; /* m.s. 4 bits */
3052 | uint16_t mantissa = mcScaleOffset & 0x07ff; /* l.s. 11 bits */
3053 | double mcScaleOffset_value = ((double)mantissa/(1<<11)) * (1.0 / (1 << exponent));
3054 | proto_item_append_text(ti, " (%f)", mcScaleOffset_value);
3055 | bit_offset += 15;
3056 |
3057 | /* Summary */
3058 | proto_item_set_len(set_ti, (bit_offset+7)/8 - set_start_offset);
3059 | proto_item_append_text(set_ti, " (mcScaleReMask=0x%03x csf=%5s mcScaleOffset=%f)",
3060 | (unsigned)mcScaleReMask, tfs_get_true_false(csf)tfs_get_string(csf, ((void*)0)), mcScaleOffset_value);
3061 | }
3062 |
3063 | proto_item_append_text(extension_ti, " (%u sets)", sets);
3064 |
3065 | /* Reserved (variable-length) */
3066 | if (reserved_bits) {
3067 | proto_tree_add_bits_item(extension_tree, hf_oran_reserved, tvb, bit_offset, reserved_bits, ENC_BIG_ENDIAN0x00000000);
3068 | bit_offset += reserved_bits;
3069 | }
3070 |
3071 | offset = bit_offset/8;
3072 | break;
3073 | }
3074 |
3075 | case 6: /* SE 6: Non-contiguous PRB allocation in time and frequency domain */
3076 | {
3077 | /* numSymbol not used in this case */
3078 | if (numsymbol_ti && !numsymbol_ignored) {
3079 | proto_item_append_text(numsymbol_ti, " (ignored)");
3080 | numsymbol_ignored = true1;
3081 | }
3082 |
3083 | /* Will update ext6 recorded info */
3084 | ext11_settings.ext6_set = true1;
3085 |
3086 | /* repetition */
3087 | proto_tree_add_bits_item(extension_tree, hf_oran_se6_repetition, tvb, offset*8, 1, ENC_BIG_ENDIAN0x00000000);
3088 | /* rbgSize (PRBs per bit set in rbgMask) */
3089 | uint32_t rbgSize;
3090 | proto_item *rbg_size_ti;
3091 | rbg_size_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_rbgSize, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &rbgSize);
3092 | if (rbgSize == 0) {
3093 | /* N.B. this is only true if "se6-rb-bit-supported" is set... */
3094 | expert_add_info_format(pinfo, rbg_size_ti, &ei_oran_rbg_size_reserved,
3095 | "rbgSize value of 0 is reserved");
3096 | }
3097 | /* rbgMask (28 bits) */
3098 | uint32_t rbgMask;
3099 | proto_item *rbgmask_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_rbgMask, tvb, offset, 4, ENC_BIG_ENDIAN0x00000000, &rbgMask);
3100 | if (rbgSize == 0) {
3101 | proto_item_append_text(rbgmask_ti, " (value ignored since rbgSize is 0)");
3102 | }
3103 |
3104 | /* TODO: if receiver detects non-zero bits outside the valid range, those shall be ignored. */
3105 | offset += 4;
3106 | /* priority */
3107 | proto_tree_add_item(extension_tree, hf_oran_noncontig_priority, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3108 | /* symbolMask */
3109 | offset = dissect_symbolmask(tvb, extension_tree, offset, NULL((void*)0), NULL((void*)0));
3110 |
3111 | /* Look up rbg_size enum -> value */
3112 | switch (rbgSize) {
3113 | case 0:
3114 | /* N.B. reserved, but covered above with expert info (would remain 0) */
3115 | break;
3116 | case 1:
3117 | ext11_settings.ext6_rbg_size = 1; break;
3118 | case 2:
3119 | ext11_settings.ext6_rbg_size = 2; break;
3120 | case 3:
3121 | ext11_settings.ext6_rbg_size = 3; break;
3122 | case 4:
3123 | ext11_settings.ext6_rbg_size = 4; break;
3124 | case 5:
3125 | ext11_settings.ext6_rbg_size = 6; break;
3126 | case 6:
3127 | ext11_settings.ext6_rbg_size = 8; break;
3128 | case 7:
3129 | ext11_settings.ext6_rbg_size = 16; break;
3130 | /* N.B., encoded in 3 bits, so no other values are possible */
3131 | }
3132 |
3133 | /* Set to looked-up value */
3134 | rbgSize = ext11_settings.ext6_rbg_size;
3135 |
3136 | uint32_t lastRbgid = 0;
3137 | if (rbgSize != 0) {
3138 | /* The O-DU shall not use combinations of startPrbc, numPrbc and rbgSize leading to a value of lastRbgid larger than 27 */
3139 | /* i.e., leftmost bit used should not need to go off left end of rbgMask! */
3140 | lastRbgid = (uint32_t)ceil((numPrbc + (startPrbc % rbgSize)) / (float)rbgSize) - 1;
3141 | if (lastRbgid > 27) {
3142 | expert_add_info_format(pinfo, rbg_size_ti, &ei_oran_lastRbdid_out_of_range,
3143 | "SE6: rbgSize (%u) not compatible with startPrbc(%u) and numPrbc(%u)",
3144 | rbgSize, startPrbc, numPrbc);
3145 | break;
3146 | }
3147 | }
3148 |
3149 | /* Record (and count) which bits are set in rbgMask */
3150 | bool_Bool first_seen = false0;
3151 | unsigned first_seen_pos=0, last_seen_pos=0;
3152 | for (unsigned n=0; n < 28 && ext11_settings.ext6_num_bits_set < 28; n++) {
3153 | if ((rbgMask >> n) & 0x01) {
3154 | ext11_settings.ext6_bits_set[ext11_settings.ext6_num_bits_set++] = n;
3155 | if (!first_seen) {
3156 | first_seen = true1;
3157 | first_seen_pos = n;
3158 | }
3159 | last_seen_pos = n;
3160 | }
3161 | }
3162 |
3163 | /* Show how many bits were set in rbgMask */
3164 | proto_item_append_text(rbgmask_ti, " (%u bits set)", ext11_settings.ext6_num_bits_set);
3165 | /* Also, that is the range of bits */
3166 | if (first_seen) {
3167 | proto_item_append_text(rbgmask_ti, " (%u bits spread)", last_seen_pos-first_seen_pos+1);
3168 | }
3169 |
3170 | /* Complain if last set bit is beyond lastRbgid */
3171 | if (first_seen) {
3172 | if (last_seen_pos > lastRbgid) {
3173 | expert_add_info_format(pinfo, rbgmask_ti, &ei_oran_rbgMask_beyond_last_rbdid,
3174 | "SE6: rbgMask (0x%07x) has bit %u set, but lastRbgId is %u",
3175 | rbgMask, last_seen_pos, lastRbgid);
3176 | }
3177 | }
3178 |
3179 | /* Also update prbs_for_st10_type5[] */
3180 | if (sectionType == 10 && rbgSize != 0) {
3181 | /* Unset all entries */
3182 | memset(&prbs_for_st10_type5, 0, sizeof(prbs_for_st10_type5));
3183 |
3184 | /* Work out which PRB first bit corresponds to */
3185 | unsigned firstPrbStart = (startPrbc/rbgSize) * rbgSize;
3186 |
3187 | /* Add PRBs corresponding to each bit set */
3188 | for (unsigned n=0; n < 28 ; n++) {
3189 | if ((rbgMask >> n) & 0x01) {
3190 | /* Lazy way to clip any values that lie outside of range for section */
3191 | for (unsigned p=0; p < rbgSize; p++) {
3192 | unsigned start = firstPrbStart + (n*rbgSize);
3193 | if ((start+p < MAX_PRBS273) && (start+p >= startPrbc) && (start+p <= startPrbc+numPrbc-1)) {
3194 | prbs_for_st10_type5[start+p] = true1;
3195 | }
3196 | }
3197 | }
3198 | }
3199 | }
3200 |
3201 | break;
3202 | }
3203 |
3204 | case 7: /* SE 7: eAxC mask */
3205 | /* Allow ST0 to address multiple eAxC_ID values for transmission blanking */
3206 | proto_tree_add_item(extension_tree, hf_oran_eAxC_mask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3207 | offset += 2;
3208 | break;
3209 |
3210 | case 8: /* SE 8: Regularization factor */
3211 | proto_tree_add_item(extension_tree, hf_oran_regularizationFactor, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3212 | offset += 2;
3213 | break;
3214 |
3215 | case 9: /* SE 9: Dynamic Spectrum Sharing parameters */
3216 | proto_tree_add_item(extension_tree, hf_oran_technology, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3217 | offset += 1;
3218 | proto_tree_add_item(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3219 | offset += 1;
3220 | break;
3221 |
3222 | case 10: /* SE 10: Group configuration of multiple ports */
3223 | {
3224 | seen_se10 = true1;
3225 |
3226 | /* beamGroupType */
3227 | uint32_t beam_group_type = 0;
3228 | proto_item *bgt_ti;
3229 | bgt_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_beamGroupType,
3230 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &beam_group_type);
3231 | proto_item_append_text(extension_ti, " (%s)", val_to_str_const(beam_group_type, beam_group_type_vals, "Unknown"));
3232 |
3233 | /* numPortc */
3234 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_numPortc,
3235 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numPortc);
3236 | offset++;
3237 |
3238 | /* Will append all beamId values to extension_ti, regardless of beamGroupType */
3239 | unsigned n;
3240 |
3241 | switch (beam_group_type) {
3242 | case 0x0: /* common beam */
3243 | case 0x1: /* beam matrix indication */
3244 | /* Reserved byte */
3245 | proto_tree_add_item(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000);
3246 | offset++;
3247 |
3248 | /* Explain how entries are allocated */
3249 | if (beam_group_type == 0x0) {
3250 | proto_item_append_text(extension_ti, " (all %u ueid/Beam entries are %u)", numPortc, ueId);
3251 | }
3252 | else {
3253 | /* 'numPortc' consecutive BeamIds from section header */
3254 | proto_item_append_text(extension_ti, " (ueId/beam entries are %u -> %u)", ueId, ueId+numPortc);
3255 | }
3256 |
3257 | if (sectionType == 5) {
3258 | /* These types are not allowed */
3259 | expert_add_info_format(pinfo, bgt_ti, &ei_oran_se10_not_allowed,
3260 | "SE10: beamGroupType %u is not allowed for section type 5", beam_group_type);
3261 | }
3262 | break;
3263 |
3264 | case 0x2: /* beam vector listing */
3265 | {
3266 | proto_item_append_text(extension_ti, " [ ");
3267 |
3268 | /* Beam listing vector case */
3269 | /* Work out how many port beam entries there is room for */
3270 | /* Using numPortC as visible in issue 18116 */
3271 | for (n=0; n < numPortc; n++) {
3272 | /* 1 reserved bit */
3273 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3274 |
3275 | /* port beam ID (or UEID) (15 bits) */
3276 | uint32_t id;
3277 | proto_item *beamid_or_ueid_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_beamId,
3278 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &id);
3279 | proto_item_append_text(beamid_or_ueid_ti, " port #%u beam ID (or UEId) %u", n, id);
3280 | offset += 2;
3281 |
3282 | if (id != 0x7fff) {
3283 | if (number_of_ueids < MAX_UEIDS16) {
3284 | ueids[number_of_ueids++] = id;
3285 | }
3286 | }
3287 |
3288 | proto_item_append_text(extension_ti, "%u ", id);
3289 | }
3290 |
3291 | proto_item_append_text(extension_ti, "]");
3292 | break;
3293 | }
3294 | case 0x3: /* beamId/ueId listing with associated port-list index */
3295 | {
3296 | proto_item_append_text(extension_ti, " [ ");
3297 |
3298 | if (numPortc > 0) {
3299 | /* first portListIndex is outside loop */
3300 | uint32_t port_list_index;
3301 | proto_item *pli_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_port_list_index, tvb,
3302 | offset, 1, ENC_BIG_ENDIAN0x00000000, &port_list_index);
3303 | if (port_list_index == 0) {
3304 | /* Value 0 is reserved */
3305 | expert_add_info(pinfo, pli_ti, &ei_oran_port_list_index_zero);
3306 | }
3307 | offset += 1;
3308 |
3309 | for (n=0; n < numPortc-1; n++) {
3310 | /* 1 reserved bit */
3311 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3312 |
3313 | /* port beam ID (or UEID) */
3314 | uint32_t id;
3315 | proto_item *beamid_or_ueid_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_beamId,
3316 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &id);
3317 | proto_item_append_text(beamid_or_ueid_ti, " port #%u beam ID (or UEId) %u", n, id);
3318 | offset += 2;
3319 |
3320 | if (id != 0x7fff) {
3321 | if (number_of_ueids < MAX_UEIDS16) {
3322 | ueids[number_of_ueids++] = id;
3323 | }
3324 | }
3325 |
3326 | /* subsequent portListIndex */
3327 | pli_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_port_list_index, tvb,
3328 | offset, 1, ENC_BIG_ENDIAN0x00000000, &port_list_index);
3329 | if (port_list_index == 0) {
3330 | /* Value 0 is reserved */
3331 | expert_add_info(pinfo, pli_ti, &ei_oran_port_list_index_zero);
3332 | }
3333 | offset += 1;
3334 |
3335 | proto_item_append_text(extension_ti, "%u:%u ", port_list_index, id);
3336 | }
3337 | }
3338 |
3339 | proto_item_append_text(extension_ti, "]");
3340 | break;
3341 | }
3342 |
3343 |
3344 | default:
3345 | /* Warning for unsupported/reserved value */
3346 | expert_add_info(NULL((void*)0), bgt_ti, &ei_oran_se10_unknown_beamgrouptype);
3347 | break;
3348 | }
3349 | break;
3350 | }
3351 |
3352 | case 11: /* SE 11: Flexible Weights Extension Type */
3353 | {
3354 | /* Hidden filter for bf */
3355 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
3356 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
3357 |
3358 | /* beamId in section header should be ignored. Guard against appending multiple times.. */
3359 | if (beamId_ti && !beamId_ignored) {
3360 | proto_item_append_text(beamId_ti, " (ignored)");
3361 | beamId_ignored = true1;
3362 | }
3363 |
3364 | bool_Bool disableBFWs;
3365 | uint32_t numBundPrb;
3366 | bool_Bool rad;
3367 |
3368 | /* disableBFWs */
3369 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_disable_bfws,
3370 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &disableBFWs);
3371 | if (disableBFWs) {
3372 | proto_item_append_text(extension_ti, " (disableBFWs)");
3373 | }
3374 |
3375 | /* RAD */
3376 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_rad,
3377 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &rad);
3378 | /* bundleOffset (6 bits) */
3379 | proto_tree_add_item(extension_tree, hf_oran_bundle_offset, tvb,
3380 | offset, 1, ENC_BIG_ENDIAN0x00000000);
3381 | offset++;
3382 |
3383 | /* numBundPrb (number of prbs in each bundle) */
3384 | proto_item *num_bund_prb_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_bund_prbs,
3385 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numBundPrb);
3386 | offset++;
3387 | /* value zero is reserved.. */
3388 | if (numBundPrb == 0) {
3389 | expert_add_info_format(pinfo, num_bund_prb_ti, &ei_oran_reserved_numBundPrb,
3390 | "Reserved value 0 for numBundPrb seen - not valid");
3391 | }
3392 |
3393 | uint32_t num_bundles;
3394 | bool_Bool orphaned_prbs = false0;
3395 |
3396 | if (!disableBFWs) {
3397 | /********************************************/
3398 | /* Table 7.7.1.1-1 */
3399 | /********************************************/
3400 |
3401 | uint32_t bfwcomphdr_iq_width, bfwcomphdr_comp_meth;
3402 | proto_item *comp_meth_ti = NULL((void*)0);
3403 |
3404 | /* bfwCompHdr (2 subheaders - bfwIqWidth and bfwCompMeth)*/
3405 | offset = dissect_bfwCompHdr(tvb, extension_tree, offset,
3406 | &bfwcomphdr_iq_width, &bfwcomphdr_comp_meth, &comp_meth_ti);
3407 |
3408 | /* Work out number of bundles, but take care not to divide by zero. */
3409 | if (numBundPrb == 0) {
3410 | break;
3411 | }
3412 |
3413 | /* Work out bundles! */
3414 | ext11_work_out_bundles(startPrbc, numPrbc, numBundPrb, &ext11_settings);
3415 | num_bundles = ext11_settings.num_bundles;
3416 |
3417 | /* Add (complete) bundles */
3418 | for (unsigned b=0; b < num_bundles; b++) {
3419 |
3420 | offset = dissect_bfw_bundle(tvb, extension_tree, pinfo, offset,
3421 | comp_meth_ti, bfwcomphdr_comp_meth,
3422 | (ext11_settings.ext21_set) ?
3423 | numPrbc :
3424 | pref_num_bf_antennas,
3425 | bfwcomphdr_iq_width,
3426 | b, /* bundle number */
3427 | ext11_settings.bundles[b].start,
3428 | ext11_settings.bundles[b].end,
3429 | ext11_settings.bundles[b].is_orphan);
3430 | if (!offset) {
3431 | break;
3432 | }
3433 | }
3434 | if (num_bundles > 0) {
3435 | /* Set flag from last bundle entry */
3436 | orphaned_prbs = ext11_settings.bundles[num_bundles-1].is_orphan;
3437 | }
3438 | }
3439 | else {
3440 | /********************************************/
3441 | /* Table 7.7.1.1-2 */
3442 | /* No weights in this case */
3443 | /********************************************/
3444 |
3445 | /* Work out number of bundles, but take care not to divide by zero. */
3446 | if (numBundPrb == 0) {
3447 | break;
3448 | }
3449 |
3450 | ext11_work_out_bundles(startPrbc, numPrbc, numBundPrb, &ext11_settings);
3451 | num_bundles = ext11_settings.num_bundles;
3452 |
3453 | for (unsigned n=0; n < num_bundles; n++) {
3454 | /* contInd */
3455 | proto_tree_add_item(extension_tree, hf_oran_cont_ind,
3456 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3457 | /* beamId */
3458 | proto_item *ti = proto_tree_add_item(extension_tree, hf_oran_beam_id,
3459 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3460 | if (!ext11_settings.bundles[n].is_orphan) {
3461 | proto_item_append_text(ti, " (PRBs %3u-%3u) (Bundle %2u)",
3462 | ext11_settings.bundles[n].start,
3463 | ext11_settings.bundles[n].end,
3464 | n);
3465 | }
3466 | else {
3467 | orphaned_prbs = true1;
3468 | proto_item_append_text(ti, " (PRBs %3u-%3u) (Orphaned PRBs)",
3469 | ext11_settings.bundles[n].start,
3470 | ext11_settings.bundles[n].end);
3471 | }
3472 | offset += 2;
3473 | }
3474 | }
3475 |
3476 | /* Add summary to extension root */
3477 | if (orphaned_prbs) {
3478 | proto_item_append_text(extension_ti, " (%u full bundles + orphaned)", num_bundles-1);
3479 | }
3480 | else {
3481 | proto_item_append_text(extension_ti, " (%u bundles)", num_bundles);
3482 | }
3483 | }
3484 |
3485 | break;
3486 |
3487 | case 12: /* SE 12: Non-Contiguous PRB Allocation with Frequency Ranges */
3488 | {
3489 | /* numSymbol not used in this case */
3490 | if (numsymbol_ti && !numsymbol_ignored) {
3491 | proto_item_append_text(numsymbol_ti, " (ignored)");
3492 | numsymbol_ignored = true1;
3493 | }
3494 |
3495 | ext11_settings.ext12_set = true1;
3496 |
3497 | /* priority */
3498 | proto_tree_add_item(extension_tree, hf_oran_noncontig_priority, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3499 |
3500 | /* symbolMask */
3501 | offset = dissect_symbolmask(tvb, extension_tree, offset, NULL((void*)0), NULL((void*)0));
3502 |
3503 | /* There are now 'R' pairs of (offStartPrb, numPrb) values. Fill extlen bytes with values. If last one is not set,
3504 | should be populated with 0s. */
3505 | uint32_t extlen_remaining_bytes = (extlen*4) - 4;
3506 | uint8_t prb_index;
3507 |
3508 | /* This is for ST10/ST11. First pair starts after frames signalled there */
3509 | uint16_t st10_st11_offset = startPrbc + numPrbc;
3510 |
3511 | for (prb_index = 1; extlen_remaining_bytes > 0; prb_index++)
3512 | {
3513 | /* Create a subtree for each pair */
3514 | proto_item *pair_ti = proto_tree_add_string(extension_tree, hf_oran_frequency_range,
3515 | tvb, offset, 2, "");
3516 | proto_tree *pair_tree = proto_item_add_subtree(pair_ti, ett_oran_frequency_range);
3517 |
3518 | /* offStartPrb */
3519 | uint32_t off_start_prb;
3520 | proto_tree_add_item_ret_uint(pair_tree, hf_oran_off_start_prb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &off_start_prb);
3521 | offset++;
3522 |
3523 | /* numPrb */
3524 | uint32_t num_prb;
3525 | proto_tree_add_item_ret_uint(pair_tree, hf_oran_num_prb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_prb);
3526 | offset++;
3527 |
3528 | extlen_remaining_bytes -= 2;
3529 |
3530 | /* Last pair may be 0,0 if not used. Check for this */
3531 | if ((extlen_remaining_bytes == 0) && (off_start_prb == 0) && (num_prb == 0)) {
3532 | proto_item_append_text(pair_ti, " (not used)");
3533 | }
3534 | /* Add summary to pair root item, and configure details in ext11_settings */
3535 | else {
3536 | proto_item_append_text(pair_ti, "(%u) [%u : %u]",
3537 | prb_index, off_start_prb, num_prb);
3538 | proto_item_append_text(extension_ti, "[%u : %u]",
3539 | off_start_prb, num_prb);
3540 | if (ext11_settings.ext12_num_pairs < MAX_BFW_EXT12_PAIRS128) {
3541 | ext11_settings.ext12_pairs[ext11_settings.ext12_num_pairs].off_start_prb = off_start_prb;
3542 | ext11_settings.ext12_pairs[ext11_settings.ext12_num_pairs++].num_prb = num_prb;
3543 | }
3544 |
3545 | /* Also update PRBs to be covered for ST10 type 5 */
3546 | /* Original range from section is added to.. */
3547 | /* TODO: I don't think this is quite right.. */
3548 | for (unsigned prb=st10_st11_offset+off_start_prb; prb < st10_st11_offset+off_start_prb+num_prb; prb++) {
3549 | if (prb < MAX_PRBS273) {
3550 | prbs_for_st10_type5[prb] = true1;
3551 | }
3552 | }
3553 |
3554 | /* Any next pair will begin after this one */
3555 | st10_st11_offset += (off_start_prb + num_prb);
3556 | }
3557 | }
3558 | break;
3559 | }
3560 |
3561 | case 13: /* SE 13: PRB Allocation with Frequency Hopping */
3562 | {
3563 | /* Will update settings for ext11 */
3564 | ext11_settings.ext13_set = true1;
3565 |
3566 | uint32_t extlen_remaining_bytes = (extlen*4) - 2;
3567 | uint8_t allocation_index;
3568 |
3569 | unsigned prev_next_symbol_id = 0, prev_next_start_prbc = 0;
3570 |
3571 | for (allocation_index = 1; extlen_remaining_bytes > 0; allocation_index++)
3572 | {
3573 | /* Subtree for allocation */
3574 | proto_item *allocation_ti = proto_tree_add_string(extension_tree, hf_oran_prb_allocation,
3575 | tvb, offset, 2, "");
3576 | proto_tree *allocation_tree = proto_item_add_subtree(allocation_ti, ett_oran_prb_allocation);
3577 |
3578 | /* Reserved (2 bits) */
3579 | proto_tree_add_item(allocation_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3580 |
3581 | /* nextSymbolId (4 bits) */
3582 | uint32_t next_symbol_id;
3583 | proto_tree_add_item_ret_uint(allocation_tree, hf_oran_nextSymbolId, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &next_symbol_id);
3584 |
3585 | /* nextStartPrbc (10 bits) */
3586 | uint32_t next_start_prbc;
3587 | proto_tree_add_item_ret_uint(allocation_tree, hf_oran_nextStartPrbc, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &next_start_prbc);
3588 | offset += 2;
3589 |
3590 | /* Add summary to allocation root item */
3591 | proto_item_append_text(allocation_ti, "(%u) nextSymbolId=%3u, nextStartPrbc=%u",
3592 | allocation_index, next_symbol_id, next_start_prbc);
3593 |
3594 | /* Checking for duplicates (expected if e.g. had only 2 entries but extlen bytes still to fill */
3595 | if ((allocation_index > 1) && (next_symbol_id == prev_next_symbol_id) && (next_start_prbc == prev_next_start_prbc)) {
3596 | proto_item_append_text(allocation_ti, " (repeated - to fill up extlen)");
3597 | }
3598 | else {
3599 | /* Add entry for configuring ext11. don't store out of range */
3600 | if (ext11_settings.ext13_num_start_prbs < MAX_BFW_EXT13_ALLOCATIONS128) {
3601 | ext11_settings.ext13_start_prbs[ext11_settings.ext13_num_start_prbs++] = next_start_prbc;
3602 | }
3603 | }
3604 | prev_next_symbol_id = next_symbol_id;
3605 | prev_next_start_prbc = next_start_prbc;
3606 |
3607 | extlen_remaining_bytes -= 2;
3608 | }
3609 | break;
3610 | }
3611 |
3612 | case 14: /* SE 14: Nulling-layer Info. for ueId-based beamforming */
3613 | /* Hidden filter for bf (DMRS BF) */
3614 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
3615 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
3616 |
3617 | if (!seen_se10) {
3618 | proto_tree_add_item(extension_tree, hf_oran_nullLayerInd, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3619 | offset += 1;
3620 | proto_tree_add_item(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3621 | offset += 1;
3622 | }
3623 | else {
3624 | /* Loop over numPortc++1 (from SE 10) nullLayerInd fields */
3625 | for (unsigned port=0; port < numPortc+1; port++) {
3626 | proto_tree_add_item(extension_tree, hf_oran_nullLayerInd, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3627 | offset += 1;
3628 | }
3629 | }
3630 | break;
3631 |
3632 | case 15: /* SE 15: Mixed-numerology Info. for ueId-based beamforming */
3633 | {
3634 | /* frameStructure */
3635 | offset = dissect_frame_structure(extension_tree, tvb, offset,
3636 | subframeId, slotId);
3637 | /* freqOffset */
3638 | proto_tree_add_item(extension_tree, hf_oran_freqOffset, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000);
3639 | offset += 3;
3640 | /* cpLength */
3641 | proto_item *cplength_ti = proto_tree_add_item(extension_tree, hf_oran_cpLength, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3642 | if (sectionType != 0 && sectionType != 3) {
3643 | proto_item_append_text(cplength_ti, " (ignored - used only with ST0 and ST3)");
3644 | }
3645 | offset += 2;
3646 | break;
3647 | }
3648 |
3649 | case 16: /* SE 16: Antenna mapping in UE channel information based UL beamforming */
3650 | {
3651 | /* Just filling available bytes with antMask entries.
3652 | N.B., if SE 10 also used, could associate each antMask with (beamId or UEId) RX eAxC */
3653 | uint32_t extlen_remaining_bytes = (extlen*4) - 2;
3654 | unsigned num_ant_masks = extlen_remaining_bytes / 8;
3655 | for (unsigned n=0; n < num_ant_masks; n++) {
3656 | proto_item *ti = proto_tree_add_item(extension_tree, hf_oran_antMask, tvb, offset, 8, ENC_BIG_ENDIAN0x00000000);
3657 | proto_item_append_text(ti, " (RX eAxC #%u)", n+1);
3658 | offset += 8;
3659 | }
3660 | break;
3661 | }
3662 |
3663 | case 17: /* SE 17: Indication of user port group */
3664 | {
3665 | uint32_t extlen_remaining_bytes = (extlen*4) - 2;
3666 | uint32_t end_bit = (offset+extlen_remaining_bytes) * 8;
3667 | uint32_t ueid_index = 1;
3668 | /* TODO: just filling up all available bytes - some may actually be padding.. */
3669 | /* "the preceding Section Type and extension messages implicitly provide the number of scheduled users" */
3670 | for (uint32_t bit_offset=offset*8; bit_offset < end_bit; bit_offset+=4, ueid_index++) {
3671 | proto_item *ti = proto_tree_add_bits_item(extension_tree, hf_oran_num_ueid, tvb, bit_offset, 4, ENC_BIG_ENDIAN0x00000000);
3672 | proto_item_append_text(ti, " (user #%u)", ueid_index);
3673 | }
3674 | break;
3675 | }
3676 |
3677 | case 18: /* SE 18: Uplink transmission management */
3678 | /* transmissionWindowOffset */
3679 | proto_tree_add_item(extension_tree, hf_oran_transmissionWindowOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3680 | offset += 2;
3681 | /* reserved (2 bits) */
3682 | proto_tree_add_item(extension_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3683 | /* transmissionWindowSize (14 bits) */
3684 | proto_tree_add_item(extension_tree, hf_oran_transmissionWindowSize, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3685 | offset += 2;
3686 |
3687 | /* reserved (6 bits) */
3688 | proto_tree_add_item(extension_tree, hf_oran_reserved_6bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3689 | /* toT (2 bits) */
3690 | proto_tree_add_item(extension_tree, hf_oran_toT, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3691 | offset += 1;
3692 | break;
3693 |
3694 | case 19: /* SE 19: Compact beamforming information for multiple port */
3695 | {
3696 | /* beamId in section header should be ignored. Guard against appending multiple times.. */
3697 | if (beamId_ti
22.1 | 'beamId_ti' is null
&& !beamId_ignored) {
3698 | proto_item_append_text(beamId_ti, " (ignored)");
3699 | beamId_ignored = true1;
3700 | }
3701 |
3702 | /* numSymbol not used in this case */
3703 | if (numsymbol_ti
22.2 | 'numsymbol_ti' is null
&& !numsymbol_ignored) {
3704 | proto_item_append_text(numsymbol_ti, " (ignored)");
3705 | numsymbol_ignored = true1;
3706 | }
3707 |
3708 | /* disableBFWs */
3709 | bool_Bool disableBFWs;
3710 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_disable_bfws,
3711 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &disableBFWs);
3712 | if (disableBFWs) {
23 | ← | Assuming 'disableBFWs' is false | →
24 | ← | Taking false branch | →
3713 | proto_item_append_text(extension_ti, " (disableBFWs)");
3714 | }
3715 | /* repetition (1 bit) */
3716 | uint64_t repetition;
3717 | proto_tree_add_bits_ret_val(extension_tree, hf_oran_se19_repetition, tvb, (offset*8)+1, 1, &repetition, ENC_BIG_ENDIAN0x00000000);
3718 | /* numPortc (6 bits) */
3719 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_numPortc,
3720 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numPortc);
3721 | offset++;
3722 |
3723 | /* priority (2 bits) */
3724 | proto_tree_add_item(extension_tree, hf_oran_noncontig_priority, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3725 | /* symbolMask (14 bits) */
3726 | offset = dissect_symbolmask(tvb, extension_tree, offset, NULL((void*)0), NULL((void*)0));
3727 |
3728 | uint32_t bfwcomphdr_iq_width, bfwcomphdr_comp_meth;
3729 | proto_item *comp_meth_ti = NULL((void*)0);
3730 |
3731 | if (!repetition) {
25 | ← | Assuming 'repetition' is 0 | →
26 | ← | Taking true branch | →
3732 |
3733 | if (!disableBFWs
26.1 | 'disableBFWs' is false
) {
27 | ← | Taking true branch | →
3734 | /* bfwCompHdr */
3735 | offset = dissect_bfwCompHdr(tvb, extension_tree, offset,
3736 | &bfwcomphdr_iq_width, &bfwcomphdr_comp_meth, &comp_meth_ti);
3737 | }
3738 |
3739 | /* Add entries for each port */
3740 | for (unsigned port=0; port < numPortc; port++) {
28 | ← | Assuming 'port' is < 'numPortc' | →
29 | ← | Loop condition is true. Entering loop body | →
3741 |
3742 | /* Create subtree for port entry*/
3743 | int port_start_offset = offset;
3744 | proto_item *port_ti = proto_tree_add_string_format(extension_tree, hf_oran_ext19_port,
3745 | tvb, offset, 0,
3746 | "", "Port %u: ", port);
3747 | proto_tree *port_tree = proto_item_add_subtree(port_ti, ett_oran_ext19_port);
3748 |
3749 | /* Reserved (4 bits) */
3750 | proto_tree_add_item(port_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3751 | /* portReMask (12 bits) */
3752 | proto_tree_add_item(port_tree, hf_oran_portReMask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3753 | offset += 2;
3754 |
3755 | /* Reserved (2 bits) */
3756 | proto_tree_add_item(port_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3757 | /* portSymbolMask (14 bits) */
3758 | proto_tree_add_item(port_tree, hf_oran_portSymbolMask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3759 | offset += 2;
3760 |
3761 | /* Reserved (1 bit) */
3762 | proto_tree_add_item(port_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3763 | /* beamID (15 bits) */
3764 | proto_tree_add_item_ret_uint(port_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &beamId);
3765 | proto_item_append_text(port_ti, " (beamId=%u)", beamId);
3766 | offset += 2;
3767 |
3768 | /* No weights present */
3769 | if (!disableBFWs
29.1 | 'disableBFWs' is false
) {
30 | ← | Taking true branch | →
3770 | /*******************************************************************/
3771 | /* Table 7.7.19.1-1 (there is no part -2 for disableBFWs case...), */
3772 | /* but for SE 11, bfwCompParam was only present for !disableBFWs */
3773 | /*******************************************************************/
3774 |
3775 | /* bfwCompParam */
3776 | bool_Bool compression_method_supported = false0;
3777 | uint32_t exponent = 0;
3778 | unsigned num_trx_entries;
31 | ← | 'num_trx_entries' declared without an initial value | →
3779 | uint16_t *trx;
3780 | offset = dissect_bfwCompParam(tvb, port_tree, pinfo, offset, comp_meth_ti,
32 | ← | Calling 'dissect_bfwCompParam' | →
36 | ← | Returning from 'dissect_bfwCompParam' | →
3781 | &bfwcomphdr_comp_meth, &exponent, &compression_method_supported,
3782 | &num_trx_entries, &trx);
3783 |
3784 | int bit_offset = offset*8;
3785 | int bfw_offset;
3786 |
3787 | /* Add weights for each TRX */
3788 | unsigned trx_to_add = (num_trx_entries==0) ? pref_num_bf_antennas : num_trx_entries;
37 | ← | The left operand of '==' is a garbage value
3789 | for (unsigned b=0; b < trx_to_add; b++) {
3790 |
3791 | uint16_t trx_index = (num_trx_entries) ? trx[b] : b+1;
3792 |
3793 | /* Create BFW subtree */
3794 | bfw_offset = bit_offset / 8;
3795 | uint8_t bfw_extent = ((bit_offset + (bfwcomphdr_iq_width*2)) / 8) - bfw_offset;
3796 | proto_item *bfw_ti = proto_tree_add_string_format(port_tree, hf_oran_bfw,
3797 | tvb, bfw_offset, bfw_extent,
3798 | "", "TRX %u: (", trx_index);
3799 | proto_tree *bfw_tree = proto_item_add_subtree(bfw_ti, ett_oran_bfw);
3800 |
3801 | /* I */
3802 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
3803 | float value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent);
3804 | /* Add to tree. */
3805 | proto_tree_add_float_format_value(bfw_tree, hf_oran_bfw_i, tvb, bit_offset/8,
3806 | (bfwcomphdr_iq_width+7)/8, value, "#%u=%f", b, value);
3807 | bit_offset += bfwcomphdr_iq_width;
3808 | proto_item_append_text(bfw_ti, "I%u=%f ", b, value);
3809 |
3810 | /* Q */
3811 | bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
3812 | value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent);
3813 | /* Add to tree. */
3814 | proto_tree_add_float_format_value(bfw_tree, hf_oran_bfw_q, tvb, bit_offset/8,
3815 | (bfwcomphdr_iq_width+7)/8, value, "#%u=%f", b, value);
3816 | bit_offset += bfwcomphdr_iq_width;
3817 | proto_item_append_text(bfw_ti, "Q%u=%f)", b, value);
3818 | }
3819 |
3820 | offset = (bit_offset+7)/8;
3821 | }
3822 | else {
3823 | /* No weights... */
3824 | }
3825 |
3826 | /* Set length of this port entry */
3827 | proto_item_set_len(port_ti, offset-port_start_offset);
3828 | }
3829 | }
3830 | break;
3831 | }
3832 |
3833 | case 20: /* SE 20: Puncturing extension */
3834 | {
3835 | /* numPuncPatterns */
3836 | uint32_t numPuncPatterns;
3837 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_numPuncPatterns, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numPuncPatterns);
3838 | offset += 1;
3839 |
3840 | /* Add each puncturing pattern */
3841 | for (uint32_t n=0; n < numPuncPatterns; n++) {
3842 | unsigned pattern_start_offset = offset;
3843 |
3844 | /* Subtree for this puncturing pattern */
3845 | proto_item *pattern_ti = proto_tree_add_string_format(extension_tree, hf_oran_puncPattern,
3846 | tvb, offset, 0,
3847 | "", "Puncturing Pattern: %u/%u", n+1, numPuncPatterns);
3848 | proto_tree *pattern_tree = proto_item_add_subtree(pattern_ti, ett_oran_punc_pattern);
3849 |
3850 | /* SymbolMask (14 bits) */
3851 | proto_tree_add_item(pattern_tree, hf_oran_symbolMask_ext20, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3852 | offset += 1;
3853 |
3854 | uint32_t startPuncPrb, numPuncPrb;
3855 |
3856 | /* startPuncPrb (10 bits) */
3857 | proto_tree_add_item_ret_uint(pattern_tree, hf_oran_startPuncPrb, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPuncPrb);
3858 | offset += 2;
3859 | /* numPuncPrb (8 bits) */
3860 | proto_tree_add_item_ret_uint(pattern_tree, hf_oran_numPuncPrb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numPuncPrb);
3861 | offset += 1;
3862 |
3863 | proto_item_append_text(pattern_ti, " [%u->%u]", startPuncPrb, startPuncPrb+numPuncPrb-1);
3864 |
3865 | /* Make a hole in range of PRBs to report */
3866 | for (unsigned p=startPuncPrb; p < startPuncPrb+numPuncPrb; p++) {
3867 | if (p < MAX_PRBS273) {
3868 | prbs_for_st10_type5[p] = false0;
3869 | }
3870 | }
3871 |
3872 | /* puncReMask (12 bits) */
3873 | proto_tree_add_item(pattern_tree, hf_oran_puncReMask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3874 | offset += 1;
3875 | /* rb (1 bit) */
3876 | proto_item *rb_ti = proto_tree_add_item(pattern_tree, hf_oran_rb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3877 | /* reserved (1 bit) */
3878 | proto_tree_add_item(pattern_tree, hf_oran_reserved_bit5, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3879 | /* multiSDScope (1 bit) */
3880 | proto_tree_add_item(pattern_tree, hf_oran_multiSDScope, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3881 | /* rbgIncl (1 bit) */
3882 | bool_Bool rbgIncl;
3883 | proto_tree_add_item_ret_boolean(pattern_tree, hf_oran_RbgIncl, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &rbgIncl);
3884 | offset += 1;
3885 |
3886 | if (rbgIncl) {
3887 | /* reserved (1 bit) */
3888 | proto_tree_add_item(pattern_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3889 | /* rbgSize(3 bits) */
3890 | proto_tree_add_item(pattern_tree, hf_oran_rbgSize, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3891 | /* rbgMask (28 bits) */
3892 | proto_tree_add_item(pattern_tree, hf_oran_rbgMask, tvb, offset, 4, ENC_BIG_ENDIAN0x00000000);
3893 | offset += 4;
3894 |
3895 | proto_item_append_text(rb_ti, " (ignored)");
3896 | }
3897 |
3898 | proto_item_set_len(pattern_ti, offset-pattern_start_offset);
3899 | }
3900 |
3901 | break;
3902 | }
3903 | case 21: /* SE 21: Variable PRB group size for channel information */
3904 | {
3905 | /* ciPrbGroupSize */
3906 | uint32_t ci_prb_group_size;
3907 | proto_item *prb_group_size_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_ci_prb_group_size, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &ci_prb_group_size);
3908 | offset += 1;
3909 |
3910 | switch (ci_prb_group_size) {
3911 | case 0:
3912 | case 1:
3913 | case 255:
3914 | /* Reserved value */
3915 | expert_add_info_format(pinfo, prb_group_size_ti, &ei_oran_ci_prb_group_size_reserved,
3916 | "SE 11 ciPrbGroupSize is reserved value %u - must be 2-254",
3917 | ci_prb_group_size);
3918 | break;
3919 | default:
3920 | /* This value affects how SE 11 is interpreted */
3921 | ext11_settings.ext21_set = true1;
3922 | ext11_settings.ext21_ci_prb_group_size = ci_prb_group_size;
3923 |
3924 | if (numPrbc == 0) {
3925 | expert_add_info(pinfo, numprbc_ti, &ei_oran_numprbc_ext21_zero);
3926 | }
3927 | break;
3928 | }
3929 |
3930 | /* reserved (6 bits) */
3931 | proto_tree_add_item(extension_tree, hf_oran_reserved_6bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3932 |
3933 | /* prgSize (2 bits). Interpretation depends upon section type (5 or 6), but also mplane parameters? */
3934 | if (sectionType == SEC_C_UE_SCHED) { /* Section Type 5 */
3935 | proto_tree_add_item(extension_tree, hf_oran_prg_size_st5, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3936 | }
3937 | else if (sectionType == SEC_C_CH_INFO) { /* Section Type 6 */
3938 | proto_tree_add_item(extension_tree, hf_oran_prg_size_st6, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3939 | }
3940 | offset += 1;
3941 | break;
3942 | }
3943 |
3944 | case 22: /* SE 22: ACK/NACK request */
3945 | {
3946 | uint32_t ack_nack_req_id;
3947 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_ack_nack_req_id, tvb, offset, 2,
3948 | ENC_BIG_ENDIAN0x00000000, &ack_nack_req_id);
3949 | offset += 2;
3950 |
3951 | if (state) {
3952 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
3953 | /* Add this request into conversation state on first pass */
3954 | ack_nack_request_t *request_details = wmem_new0(wmem_file_scope(), ack_nack_request_t)((ack_nack_request_t*)wmem_alloc0((wmem_file_scope()), sizeof (ack_nack_request_t)));
3955 | request_details->request_frame_number = pinfo->num;
3956 | request_details->request_frame_time = pinfo->abs_ts;
3957 | request_details->requestType = SE22;
3958 | /* Insert into flow's tree */
3959 | wmem_tree_insert32(state->ack_nack_requests, ack_nack_req_id, request_details);
3960 | }
3961 | else {
3962 | /* Try to link forward to ST8 response */
3963 | ack_nack_request_t *response = wmem_tree_lookup32(state->ack_nack_requests,
3964 | ack_nack_req_id);
3965 | if (response) {
3966 | show_link_to_acknack_response(extension_tree, tvb, pinfo, response);
3967 | }
3968 | }
3969 | }
3970 | break;
3971 | }
3972 |
3973 | case 23: /* SE 23: Arbitrary symbol pattern modulation compression parameters */
3974 | {
3975 | /* Green common header */
3976 |
3977 | /* numSymPrbPattern (4 bits) */
3978 | uint32_t num_sym_prb_pattern;
3979 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_sym_prb_pattern, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_sym_prb_pattern);
3980 | /* reserved (3 bits) */
3981 | proto_tree_add_item(extension_tree, hf_oran_reserved_bits456, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3982 | /* prbMode (1 bit) */
3983 | bool_Bool prb_mode;
3984 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_prb_mode, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &prb_mode);
3985 | offset += 1;
3986 |
3987 | /* reserved (8 bits) */
3988 | proto_tree_add_item(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3989 | offset += 1;
3990 |
3991 | /* Dissect each SymPrbPattern */
3992 | for (uint32_t n=0; n < num_sym_prb_pattern; n++) {
3993 |
3994 | /* Subtree */
3995 | proto_item *pattern_ti = proto_tree_add_string_format(extension_tree, hf_oran_sym_prb_pattern,
3996 | tvb, offset, 1, "",
3997 | prb_mode ? "PRB-BLOCK" : "PRB-MASK");
3998 | proto_tree *pattern_tree = proto_item_add_subtree(pattern_ti, ett_oran_sym_prb_pattern);
3999 |
4000 |
4001 | /* Orange part */
4002 |
4003 | /* Reserved (2 bits) */
4004 | proto_tree_add_item(pattern_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4005 | /* symMask (14 bits) */
4006 | proto_tree_add_item(pattern_tree, hf_oran_sym_mask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4007 | offset += 2;
4008 | /* numMcScaleOffset (4 bits) */
4009 | proto_tree_add_item(pattern_tree, hf_oran_num_mc_scale_offset, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4010 |
4011 | if (!prb_mode) { /* PRB-MASK */
4012 | /* prbPattern (4 bits) */
4013 | proto_tree_add_item(pattern_tree, hf_oran_prb_pattern, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4014 | offset += 1;
4015 | /* reserved (8 bits) */
4016 | proto_tree_add_item(pattern_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4017 | offset += 1;
4018 | }
4019 | else { /* PRB-BLOCK */
4020 | /* prbBlkOffset (8 bits) */
4021 | proto_tree_add_item(pattern_tree, hf_oran_prb_block_offset, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4022 | offset += 1;
4023 | /* prbBlkSize (4 bits) */
4024 | proto_tree_add_item(pattern_tree, hf_oran_prb_block_size, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4025 | offset += 1;
4026 | }
4027 |
4028 | /* Yellowish part */
4029 | if (prb_mode) { /* PRB-BLOCK */
4030 | /* prbBlkSize (4 bits) */
4031 | proto_tree_add_item(pattern_tree, hf_oran_prb_block_size, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4032 | }
4033 | else {
4034 | /* reserved (4 bits) */
4035 | proto_tree_add_item(pattern_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4036 | }
4037 |
4038 | /* mcScaleReMask (12 bits) */
4039 | uint64_t mcScaleReMask, mcScaleOffset;
4040 | proto_tree_add_bits_ret_val(pattern_tree, hf_oran_mc_scale_re_mask, tvb, offset*8 + 4, 12, &mcScaleReMask, ENC_BIG_ENDIAN0x00000000);
4041 | offset += 2;
4042 | /* csf */
4043 | dissect_csf(pattern_tree, tvb, offset*8, ci_iq_width, NULL((void*)0));
4044 | /* mcScaleOffset (15 bits) */
4045 | proto_tree_add_bits_ret_val(pattern_tree, hf_oran_mc_scale_offset, tvb, offset*8 + 1, 15, &mcScaleOffset, ENC_BIG_ENDIAN0x00000000);
4046 | offset += 2;
4047 |
4048 | proto_item_set_end(pattern_ti, tvb, offset);
4049 | }
4050 | break;
4051 | }
4052 |
4053 | case 24: /* SE 24: PUSCH DMRS configuration */
4054 | {
4055 | /* Hidden filter for bf (DMRS BF) */
4056 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
4057 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
4058 |
4059 | /* alpnPerSym (1 bit) */
4060 | proto_tree_add_item(extension_tree, hf_oran_alpn_per_sym, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4061 | /* antDmrsSnr (1 bit) */
4062 | proto_tree_add_item(extension_tree, hf_oran_ant_dmrs_snr, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4063 | /* reserved (1 bit) */
4064 | proto_tree_add_item(extension_tree, hf_oran_reserved_bit2, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4065 | /* userGroupSize (5 bits) */
4066 | uint32_t user_group_size;
4067 | proto_item *ugs_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_user_group_size, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &user_group_size);
4068 | if (user_group_size == 0) {
4069 | proto_item_append_text(ugs_ti, " (not used)");
4070 | }
4071 | else if (user_group_size > 12) {
4072 | proto_item_append_text(ugs_ti, " (reserved)");
4073 | }
4074 | offset += 1;
4075 | /* userGroupId (8 bits)*/
4076 | uint32_t user_group_id;
4077 | proto_item *ugi_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_user_group_id, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &user_group_id);
4078 | if (user_group_id == 0) {
4079 | /* TODO: Value 0 can happen in several cases, described in 7.7.24.7.. */
4080 | }
4081 | if (user_group_id == 255) {
4082 | /* Value 255 is reserved */
4083 | expert_add_info(pinfo, ugi_ti, &ei_oran_user_group_id_reserved_value);
4084 | }
4085 | offset += 1;
4086 |
4087 | bool_Bool seen_value_to_inherit = false0;
4088 | bool_Bool inherited_config_has_transform_precoding = false0;
4089 | int dmrs_configs_seen = 0;
4090 |
4091 | /* Dissect each entry until reach number of configured ueIds (or run out of extlen bytes..) */
4092 | uint32_t ueid_index = 0;
4093 | while ((offset < (extension_start_offset + extlen*4)) && (ueid_index < number_of_ueids)) {
4094 | dmrs_configs_seen++;
4095 |
4096 | /* Subtree */
4097 | proto_item *entry_ti = proto_tree_add_string_format(extension_tree, hf_oran_dmrs_entry,
4098 | tvb, offset, 0, "",
4099 | "Entry");
4100 | proto_tree *entry_tree = proto_item_add_subtree(entry_ti, ett_oran_dmrs_entry);
4101 |
4102 | /* entryType (3 bits) */
4103 | uint32_t entry_type;
4104 | proto_item *entry_type_ti;
4105 | entry_type_ti = proto_tree_add_item_ret_uint(entry_tree, hf_oran_entry_type, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &entry_type);
4106 | if (entry_type > 3) {
4107 | proto_item_append_text(entry_type_ti, " (reserved)");
4108 | }
4109 |
4110 | /* dmrsPortNumber (5 bits). Values 0-11 allowed */
4111 | unsigned int dmrs_port_number;
4112 | proto_item *dpn_ti = proto_tree_add_item_ret_uint(entry_tree, hf_oran_dmrs_port_number, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &dmrs_port_number);
4113 | if (dmrs_port_number > 11) {
4114 | proto_item_append_text(dpn_ti, " (12-31 are reserved)");
4115 | }
4116 | offset += 1;
4117 |
4118 | /* What follows depends upon entryType */
4119 | switch (entry_type) {
4120 | case 0: /* dmrsPortNumber config same as previous, ueId ueIdReset=0 */
4121 | case 1: /* dmrsPortNumber config same as previous, ueId ueIdReset=1 */
4122 | /* No further fields for these */
4123 | /* Error here if no previous values to inherit!! */
4124 | if (!seen_value_to_inherit) {
4125 | expert_add_info_format(pinfo, entry_type_ti, &ei_oran_se24_nothing_to_inherit,
4126 | "SE24: have seen entry type %u, but no previous config (type 2 or 3) to inherit config from", entry_type);
4127 |
4128 | }
4129 | /* TODO: would be useful to repeat inherited config here? */
4130 | break;
4131 |
4132 | case 2: /* transform precoding disabled */
4133 | case 3: /* transform precoding enabled */
4134 | {
4135 | /* Type 2/3 are very similar.. */
4136 |
4137 | /* ueIdReset (1 bit) */
4138 | proto_tree_add_item(entry_tree, hf_oran_ueid_reset, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4139 | /* reserved (1 bit) */
4140 | proto_tree_add_item(entry_tree, hf_oran_reserved_bit1, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4141 |
4142 | /* dmrsSymbolMask (14 bits) */
4143 | static int * const dmrs_symbol_mask_flags[] = {
4144 | &hf_oran_dmrs_symbol_mask_s13,
4145 | &hf_oran_dmrs_symbol_mask_s12,
4146 | &hf_oran_dmrs_symbol_mask_s11,
4147 | &hf_oran_dmrs_symbol_mask_s10,
4148 | &hf_oran_dmrs_symbol_mask_s9,
4149 | &hf_oran_dmrs_symbol_mask_s8,
4150 | &hf_oran_dmrs_symbol_mask_s7,
4151 | &hf_oran_dmrs_symbol_mask_s6,
4152 | &hf_oran_dmrs_symbol_mask_s5,
4153 | &hf_oran_dmrs_symbol_mask_s4,
4154 | &hf_oran_dmrs_symbol_mask_s3,
4155 | &hf_oran_dmrs_symbol_mask_s2,
4156 | &hf_oran_dmrs_symbol_mask_s1,
4157 | &hf_oran_dmrs_symbol_mask_s0,
4158 | NULL((void*)0)
4159 | };
4160 | proto_tree_add_bitmask(entry_tree, tvb, offset,
4161 | hf_oran_dmrs_symbol_mask, ett_oran_dmrs_symbol_mask, dmrs_symbol_mask_flags, ENC_BIG_ENDIAN0x00000000);
4162 | offset += 2;
4163 |
4164 | /* scrambling */
4165 | proto_tree_add_item(entry_tree, hf_oran_scrambling, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4166 | offset += 2;
4167 |
4168 | /* nscid (1 bit) */
4169 | proto_tree_add_item(entry_tree, hf_oran_nscid, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4170 |
4171 | /* These 5 bits differ depending upon entry type */
4172 | if (entry_type == 2) { /* type 2 */
4173 | /* dType (1 bit) */
4174 | proto_tree_add_item(entry_tree, hf_oran_dtype, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4175 | /* cdmWithoutData (2 bits) */
4176 | proto_tree_add_item(entry_tree, hf_oran_cmd_without_data, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4177 | /* lambda (2 bits) */
4178 | proto_tree_add_item(entry_tree, hf_oran_lambda, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4179 | }
4180 | else { /* type 3 */
4181 | /* reserved (1 bit) */
4182 | proto_tree_add_item(entry_tree, hf_oran_reserved_bit1, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4183 | /* lowPaprType (2 bits) */
4184 | proto_tree_add_item(entry_tree, hf_oran_low_papr_type, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4185 | /* hoppingMode (2 bits) */
4186 | proto_tree_add_item(entry_tree, hf_oran_hopping_mode, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4187 | }
4188 |
4189 | /* firstPrb (9 bits) */
4190 | proto_tree_add_item(entry_tree, hf_oran_first_prb, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4191 | offset += 1;
4192 | /* lastPrb (9 bits) */
4193 | proto_tree_add_item(entry_tree, hf_oran_last_prb, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4194 | offset += 2;
4195 | /* Reserved (16 bits) */
4196 | proto_tree_add_item(entry_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4197 | offset += 2;
4198 |
4199 | /* Could now see entry types 0 or 1 - they have these values to inherit */
4200 | seen_value_to_inherit = true1;
4201 | inherited_config_has_transform_precoding = (entry_type == 3);
4202 | break;
4203 | }
4204 |
4205 | default:
4206 | /* reserved - expert info */
4207 | break;
4208 | }
4209 |
4210 | proto_item_append_text(entry_ti, " [UEId=%u] (dmrsPortNumber=%2u) (type %u - %s) ",
4211 | ueids[ueid_index++], dmrs_port_number, entry_type, val_to_str_const(entry_type, entry_type_vals, "Unknown"));
4212 | proto_item_set_end(entry_ti, tvb, offset);
4213 |
4214 | if (entry_type <= 1) {
4215 | proto_item_append_text(entry_ti, " [transform-precoding %s]",
4216 | inherited_config_has_transform_precoding ? "enabled" : "disabled");
4217 | }
4218 | }
4219 |
4220 | proto_item_append_text(extension_ti, " (%d DMRS configs seen)", dmrs_configs_seen);
4221 | break;
4222 | }
4223 |
4224 | case 25: /* SE 25: Symbol reordering for DMRS-BF */
4225 | /* Just dissect each available block of 7 bytes as the 14 symbols for a layer,
4226 | where each layer could be one or apply to all layers. */
4227 | {
4228 | /* TODO: should only appear in one section of a message - check? */
4229 | unsigned layer = 0;
4230 | proto_item *layer_ti;
4231 | while (offset+7 <= (extension_start_offset + extlen*4)) {
4232 | /* Layer subtree */
4233 | layer_ti = proto_tree_add_string_format(extension_tree, hf_oran_symbol_reordering_layer,
4234 | tvb, offset, 7, "",
4235 | "Layer");
4236 | proto_tree *layer_tree = proto_item_add_subtree(layer_ti, ett_oran_symbol_reordering_layer);
4237 |
4238 | /* All 14 symbols for a layer (or all layers) */
4239 | for (unsigned s=0; s < 14; s++) {
4240 | proto_item *sym_ti;
4241 | /* txWinForOnAirSymbol */
4242 | unsigned int tx_win_for_on_air_symbol;
4243 | sym_ti = proto_tree_add_item_ret_uint(layer_tree,
4244 | (s % 2) ? hf_oran_tx_win_for_on_air_symbol_r : hf_oran_tx_win_for_on_air_symbol_l,
4245 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &tx_win_for_on_air_symbol);
4246 | if (tx_win_for_on_air_symbol == 0x0F) {
4247 | /* Ordering not affected */
4248 | proto_item_append_text(sym_ti, " (sym %u - no info)", s);
4249 | }
4250 | else {
4251 | proto_item_append_text(sym_ti, " (sym %u)", s);
4252 | }
4253 | if (s % 2) {
4254 | offset += 1;
4255 | }
4256 | }
4257 |
4258 | proto_item_append_text(layer_ti, " (layer %u)", ++layer);
4259 | proto_item_append_text(extension_ti, " (layer %u)", layer);
4260 | }
4261 | /* Set layer subtree label */
4262 | if (layer == 1) {
4263 | proto_item_append_text(layer_ti, " (all)");
4264 | proto_item_append_text(extension_ti, " (all)");
4265 | }
4266 | if (layer == 0) {
4267 | /* TODO: are no layers valid? What does it mean? */
4268 | proto_item_append_text(extension_ti, " (none)");
4269 | }
4270 | break;
4271 | }
4272 |
4273 | case 26: /* SE 26: Frequency offset feedback */
4274 | /* Reserved (8 bits). N.B., added after draft? */
4275 | proto_tree_add_item(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4276 | offset += 1;
4277 | /* Reserved (1 bit) */
4278 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4279 | /* numFoFb (7 bits) */
4280 | unsigned num_fo_fb;
4281 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_fo_fb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_fo_fb);
4282 | offset += 1;
4283 |
4284 | /* Add each freqOffsetFb value */
4285 | for (unsigned n=0; n < num_fo_fb; n++) {
4286 | unsigned freq_offset_fb;
4287 | /* freqOffsetFb (16 bits) */
4288 | proto_item *offset_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_freq_offset_fb,
4289 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &freq_offset_fb);
4290 | /* Show if maps onto a -ve number */
4291 | if ((freq_offset_fb >= 0x8ad0) && (freq_offset_fb <= 0xffff)) {
4292 | proto_item_append_text(offset_ti, "(value %d)", -1 - (0xffff-freq_offset_fb));
4293 | }
4294 | proto_item_append_text(offset_ti, " [#%u]", n+1);
4295 | offset += 2;
4296 | }
4297 | break;
4298 |
4299 | case 27: /* SE 27: O-DU controlled dimensionality reduction */
4300 | {
4301 | /* Hidden filter for bf (DMRS BF) */
4302 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
4303 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
4304 |
4305 | /* beamType (2 bits) */
4306 | unsigned beam_type;
4307 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_beam_type, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &beam_type);
4308 | /* reserved (6 bits) */
4309 | proto_tree_add_item(extension_tree, hf_oran_reserved_last_6bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4310 | offset += 1;
4311 |
4312 | /* numElements */
4313 | unsigned num_elements;
4314 | proto_item *num_elements_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_elements, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_elements);
4315 | if (num_elements == 0) {
4316 | num_elements = 256;
4317 | proto_item_append_text(num_elements_ti, " (256");
4318 | }
4319 |
4320 | offset += 1;
4321 |
4322 | /* beamId value(s) */
4323 | switch (beam_type) {
4324 | case 0:
4325 | for (unsigned n=0; n < num_elements; n++) {
4326 | /* reserved (1 bit) + beamId */
4327 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4328 | proto_tree_add_item(c_section_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4329 | offset += 2;
4330 | }
4331 | break;
4332 | case 1:
4333 | /* reserved (1 bit) + beamId */
4334 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4335 | proto_tree_add_item(c_section_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4336 | offset += 2;
4337 | break;
4338 | default:
4339 | /* Unknown type... */
4340 | break;
4341 | }
4342 | break;
4343 | }
4344 |
4345 | case 28: /* SE 28: O-DU controlled frequency resolution for SINR reporting */
4346 | {
4347 | /* reserved (3 bits) */
4348 | proto_tree_add_item(extension_tree, hf_oran_reserved_3bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4349 | /* numUeSinrRpt */
4350 | uint32_t num_ue_sinr_rpt;
4351 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_ue_sinr_rpt, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_ue_sinr_rpt);
4352 | offset += 1;
4353 |
4354 | for (uint32_t n=0; n < num_ue_sinr_rpt; n++) {
4355 | /* reserved (1 bit) */
4356 | proto_tree_add_item(extension_tree, (n % 2) ? hf_oran_reserved_bit4 : hf_oran_reserved_1bit,
4357 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4358 |
4359 | /* numSinrPerPrb (3 bits). Taken from alternate nibbles within byte. */
4360 | proto_tree_add_item(extension_tree, (n % 2) ? hf_oran_num_sinr_per_prb_right : hf_oran_num_sinr_per_prb,
4361 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4362 | if (n % 2) {
4363 | offset += 1;
4364 | }
4365 | }
4366 |
4367 | /* May need to skip beyond half-used byte */
4368 | if (num_ue_sinr_rpt % 2) {
4369 | offset += 1;
4370 | }
4371 | break;
4372 | }
4373 |
4374 |
4375 | default:
4376 | /* Other/unexpected extension types */
4377 | expert_add_info_format(pinfo, exttype_ti, &ei_oran_unhandled_se,
4378 | "SE %u (%s) not supported by dissector",
4379 | exttype, val_to_str_const(exttype, exttype_vals, "Reserved"));
4380 | ext_unhandled = true1;
4381 | break;
4382 | }
4383 |
4384 | /* Check offset compared with extlen. There should be 0-3 bytes of padding */
4385 | int num_padding_bytes = (extension_start_offset + (extlen*4) - offset);
4386 | if (!ext_unhandled && ((num_padding_bytes<0) || (num_padding_bytes>3))) {
4387 | expert_add_info_format(pinfo, extlen_ti, &ei_oran_extlen_wrong,
4388 | "extlen signalled %u bytes (+ 0-3 bytes padding), but %u were dissected",
4389 | extlen*4, offset-extension_start_offset);
4390 | }
4391 |
4392 | /* Move offset to beyond signalled length of extension */
4393 | offset = extension_start_offset + (extlen*4);
4394 |
4395 | /* Set length of extension header. */
4396 | proto_item_set_len(extension_ti, extlen*4);
4397 | }
4398 | /* End of section extension handling */
4399 |
4400 |
4401 |
4402 | /* RRM measurement reports have measurement reports *after* extensions */
4403 | if (sectionType == SEC_C_RRM_MEAS_REPORTS) /* Section Type 10 */
4404 | {
4405 | /* Hidden filter for bf (DMFS-BF). No BF weights though.. */
4406 | bf_ti = proto_tree_add_item(c_section_tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
4407 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
4408 |
4409 | bool_Bool mf;
4410 | do {
4411 | /* Measurement report subtree */
4412 | proto_item *mr_ti = proto_tree_add_string_format(c_section_tree, hf_oran_measurement_report,
4413 | tvb, offset, 1, "", "Measurement Report");
4414 | proto_tree *mr_tree = proto_item_add_subtree(mr_ti, ett_oran_measurement_report);
4415 | unsigned report_start_offset = offset;
4416 |
4417 | /* more fragments (after this one) (1 bit) */
4418 | proto_tree_add_item_ret_boolean(mr_tree, hf_oran_mf, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &mf);
4419 |
4420 | /* measTypeId (7 bits) */
4421 | uint32_t meas_type_id;
4422 | proto_item *meas_type_id_ti;
4423 | meas_type_id_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_meas_type_id, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &meas_type_id);
4424 | offset += 1;
4425 |
4426 | /* Common to all measurement types */
4427 | unsigned num_elements = 0;
4428 | if (meas_type_id == 6) {
4429 | /* numElements */
4430 | proto_tree_add_item_ret_uint(mr_tree, hf_oran_num_elements, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_elements);
4431 | }
4432 | else {
4433 | /* All other meas ids have a reserved byte */
4434 | proto_tree_add_item(mr_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4435 | }
4436 | offset += 1;
4437 |
4438 | /* measDataSize (16 bits). N.B. begins at mf field, i.e. 2 bytes before this one */
4439 | unsigned meas_data_size;
4440 | proto_item *meas_data_size_ti;
4441 | meas_data_size_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_meas_data_size, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &meas_data_size);
4442 | meas_data_size *= 4;
4443 | proto_item_append_text(meas_data_size_ti, " (%u bytes)", meas_data_size);
4444 | offset += 2;
4445 |
4446 | /* Summary for measurement report root */
4447 | proto_item_append_text(mr_ti, " (measTypeId=%u - %s)",
4448 | meas_type_id, val_to_str_const(meas_type_id, meas_type_id_vals, "unknown"));
4449 | /* And section header */
4450 | proto_item_append_text(tree, " (%s)", val_to_str_const(meas_type_id, meas_type_id_vals, "unknown"));
4451 | /* And Info column */
4452 | col_append_fstr(pinfo->cinfo, COL_INFO, " (%s)", val_to_str_const(meas_type_id, meas_type_id_vals, "unknown"));
4453 |
4454 | /* Handle specific message type fields */
4455 | switch (meas_type_id) {
4456 | case 1:
4457 | {
4458 | /* ueTae */
4459 | unsigned ue_tae;
4460 | proto_item *ue_tae_ti;
4461 | ue_tae_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_tae, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ue_tae);
4462 | /* Show if maps onto a -ve number */
4463 | if ((ue_tae >= 0x8ad0) && (ue_tae <= 0xffff)) {
4464 | proto_item_append_text(ue_tae_ti, "(value %d)", -1 - (0xffff-ue_tae));
4465 | }
4466 | offset += 2;
4467 |
4468 | /* Reserved (16 bits) */
4469 | proto_tree_add_item(mr_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4470 | offset += 2;
4471 | break;
4472 | }
4473 | case 2:
4474 | /* ueLayerPower entries (how many? for now just use up meas_data_size..) */
4475 | /* TODO: add number of distinct dmrsPortNumber entries seen in SE24 and save in state? */
4476 | /* Or would it make sense to use the preference 'pref_num_bf_antennas' ? */
4477 | for (unsigned n=0; n < (meas_data_size-4)/2; n++) {
4478 | unsigned ue_layer_power;
4479 | proto_item *ue_layer_power_ti;
4480 | ue_layer_power_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_layer_power, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ue_layer_power);
4481 | /* Show if maps onto a -ve number */
4482 | if ((ue_layer_power >= 0x8ad0) && (ue_layer_power <= 0xffff)) {
4483 | proto_item_append_text(ue_layer_power_ti, "(value %d)", -1 - (0xffff-ue_layer_power));
4484 | }
4485 | offset += 2;
4486 | }
4487 | /* padding out to 4 bytes */
4488 | break;
4489 | case 3:
4490 | {
4491 | /* ueFreqOffset */
4492 | unsigned ue_freq_offset;
4493 | proto_item *ue_freq_offset_ti;
4494 | ue_freq_offset_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_freq_offset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ue_freq_offset);
4495 | /* Show if maps onto a -ve number */
4496 | if ((ue_freq_offset >= 0x8ad0) && (ue_freq_offset <= 0xffff)) {
4497 | proto_item_append_text(ue_freq_offset_ti, "(value %d)", -1 - (0xffff-ue_freq_offset));
4498 | }
4499 | offset += 2;
4500 |
4501 | /* Reserved (16 bits) */
4502 | proto_tree_add_item(mr_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4503 | offset += 2;
4504 | break;
4505 | }
4506 | case 4:
4507 | case 5:
4508 | /* reserved (2 bits) */
4509 | proto_tree_add_item(mr_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4510 | /* symbolMask (14 bits) */
4511 | offset = dissect_symbolmask(tvb, mr_tree, offset, NULL((void*)0), NULL((void*)0));
4512 |
4513 | /* 2 bytes for each PRB ipnPower */
4514 | for (unsigned prb=0; prb<MAX_PRBS273; prb++) {
4515 | /* Skip if should not be reported */
4516 | if (!prbs_for_st10_type5[prb]) {
4517 | continue;
4518 | }
4519 | unsigned ipn_power;
4520 | proto_item *ipn_power_ti;
4521 | /* ipnPower (2 bytes) */
4522 | ipn_power_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ipn_power, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ipn_power);
4523 | proto_item_append_text(ipn_power_ti, " (PRB %3d)", prb);
4524 | /* Show if maps onto a -ve number */
4525 | if ((ipn_power >= 0x8ad0) && (ipn_power <= 0xffff)) {
4526 | proto_item_append_text(ipn_power_ti, " (value %d)", -1 - (0xffff-ipn_power));
4527 | }
4528 | offset += 2;
4529 | }
4530 | /* padding out to 4 bytes */
4531 | break;
4532 | case 6:
4533 | /* antDmrsSnrVal entries */
4534 | for (unsigned n=0; n < num_elements; n++) {
4535 | unsigned snr_value;
4536 | proto_item *snr_value_ti;
4537 | /* antDmrsSnrVal (2 bytes) */
4538 | snr_value_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ant_dmrs_snr_val, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &snr_value);
4539 | proto_item_append_text(snr_value_ti, " (elem %2u)", n+1);
4540 | /* Show if maps onto a -ve number */
4541 | if ((snr_value >= 0x8ad0) && (snr_value <= 0xffff)) {
4542 | proto_item_append_text(snr_value_ti, " (value %d)", -1 - (0xffff-snr_value));
4543 | }
4544 | offset += 2;
4545 | }
4546 | break;
4547 |
4548 | default:
4549 | /* Anything else is not expected */
4550 | expert_add_info_format(pinfo, meas_type_id_ti, &ei_oran_unexpected_measTypeId,
4551 | "measTypeId %u (%s) not supported - only 1-6 are expected",
4552 | meas_type_id,
4553 | val_to_str_const(meas_type_id, meas_type_id_vals, "reserved"));
4554 | break;
4555 |
4556 | }
4557 |
4558 | /* Pad out to next 4 bytes */
4559 | offset += WS_PADDING_TO_4(offset-report_start_offset)((4U - ((offset-report_start_offset) % 4U)) % 4U);
4560 |
4561 | /* TODO: verify dissected size of report vs meas_data_size? */
4562 |
4563 | /* End of measurement report tree */
4564 | proto_item_set_end(mr_ti, tvb, offset);
4565 | } while (mf);
4566 | }
4567 |
4568 | /* Request for RRM Measurements has measurement commands after extensions */
4569 | else if (sectionType == SEC_C_REQUEST_RRM_MEAS) /* Section Type 11 */
4570 | {
4571 | bool_Bool mf = true1;
4572 | do {
4573 | /* Measurement command subtree */
4574 | proto_item *mc_ti = proto_tree_add_string_format(c_section_tree, hf_oran_measurement_command,
4575 | tvb, offset, 8, "", "Measurement Command");
4576 | proto_tree *mc_tree = proto_item_add_subtree(mc_ti, ett_oran_measurement_command);
4577 |
4578 | /* mf (1 bit). 1st measurement command is always preset */
4579 | proto_tree_add_item_ret_boolean(mc_tree, hf_oran_mf, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &mf);
4580 |
4581 | /* measTypeId (7 bits) */
4582 | uint32_t meas_type_id;
4583 | proto_item *meas_type_id_ti;
4584 | meas_type_id_ti = proto_tree_add_item_ret_uint(mc_tree, hf_oran_meas_type_id, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &meas_type_id);
4585 | offset += 1;
4586 |
4587 | proto_item *meas_command_ti;
4588 | uint32_t meas_command_size;
4589 |
4590 | switch (meas_type_id) {
4591 | case 5: /* command for IpN for unallocated PRBs */
4592 | /* reserved (1 byte) */
4593 | proto_tree_add_item(mc_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4594 | offset += 1;
4595 | /* measCmdSize. Presumably number of words so in future could skip unrecognised command types.. */
4596 | meas_command_ti = proto_tree_add_item_ret_uint(mc_tree, hf_oran_meas_cmd_size, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &meas_command_size);
4597 | proto_item_append_text(meas_command_ti, " (%u bytes)", meas_command_size*4);
4598 | offset += 2;
4599 | /* reserved (2 bits) */
4600 | proto_tree_add_item(mc_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4601 | /* symbolMask (14 bits) */
4602 | offset = dissect_symbolmask(tvb, mc_tree, offset, NULL((void*)0), NULL((void*)0));
4603 | /* reserved (16 bits) */
4604 | proto_tree_add_item(mc_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4605 | offset += 2;
4606 | break;
4607 |
4608 | default:
4609 | /* Anything else is not expected */
4610 | expert_add_info_format(pinfo, meas_type_id_ti, &ei_oran_unexpected_measTypeId,
4611 | "measTypeId %u (%s) not supported - only 5 is expected",
4612 | meas_type_id,
4613 | val_to_str_const(meas_type_id, meas_type_id_vals, "reserved"));
4614 | break;
4615 | }
4616 | proto_item_append_text(mc_ti, " (%s)", val_to_str_const(meas_type_id, meas_type_id_vals, "unknown"));
4617 |
4618 | } while (mf);
4619 | }
4620 |
4621 | /* Set extent of overall section */
4622 | proto_item_set_len(sectionHeading, offset);
4623 |
4624 | return offset;
4625 | }
4626 |
4627 | /* Dissect udCompHdr (user data compression header, 7.5.2.10) */
4628 | /* bit_width and comp_meth are out params */
4629 | static int dissect_udcomphdr(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, unsigned offset,
4630 | bool_Bool ignore,
4631 | unsigned *bit_width, unsigned *comp_meth, proto_item **comp_meth_ti)
4632 | {
4633 | /* Subtree */
4634 | proto_item *udcomphdr_ti = proto_tree_add_string_format(tree, hf_oran_udCompHdr,
4635 | tvb, offset, 1, "",
4636 | "udCompHdr");
4637 | proto_tree *udcomphdr_tree = proto_item_add_subtree(udcomphdr_ti, ett_oran_udcomphdr);
4638 |
4639 | /* udIqWidth */
4640 | uint32_t hdr_iq_width;
4641 | proto_item *iq_width_item = proto_tree_add_item_ret_uint(udcomphdr_tree, hf_oran_udCompHdrIqWidth , tvb, offset, 1, ENC_NA0x00000000, &hdr_iq_width);
4642 | *bit_width = (hdr_iq_width) ? hdr_iq_width : 16;
4643 | proto_item_append_text(iq_width_item, " (%u bits)", *bit_width);
4644 |
4645 | /* udCompMeth */
4646 | uint32_t ud_comp_meth;
4647 | *comp_meth_ti = proto_tree_add_item_ret_uint(udcomphdr_tree, hf_oran_udCompHdrMeth, tvb, offset, 1, ENC_NA0x00000000, &ud_comp_meth);
4648 | if (comp_meth) {
4649 | *comp_meth = ud_comp_meth;
4650 | }
4651 |
4652 | /* Summary */
4653 | if (!ignore) {
4654 | proto_item_append_text(udcomphdr_ti, " (IqWidth=%u, udCompMeth=%s)",
4655 | *bit_width, rval_to_str_const(ud_comp_meth, ud_comp_header_meth, "Unknown"));
4656 | }
4657 | else {
4658 | proto_item_append_text(udcomphdr_ti, " (ignored)");
4659 | if (hdr_iq_width || ud_comp_meth) {
4660 | expert_add_info_format(pinfo, udcomphdr_ti, &ei_oran_udpcomphdr_should_be_zero,
4661 | "udCompHdr in C-Plane for DL should be 0 - found 0x%02x",
4662 | tvb_get_uint8(tvb, offset));
4663 | }
4664 |
4665 | }
4666 | return offset+1;
4667 | }
4668 |
4669 | /* Dissect udCompParam (user data compression parameter, 8.3.3.15) */
4670 | /* bit_width and comp_meth are out params */
4671 | static int dissect_udcompparam(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree, unsigned offset,
4672 | unsigned comp_meth,
4673 | uint32_t *exponent, uint16_t *sReSMask,
4674 | bool_Bool for_sinr)
4675 | {
4676 | if (for_sinr && (comp_meth != COMP_BLOCK_FP1)) {
4677 | /* sinrCompParam only present when bfp is used */
4678 | return offset;
4679 | }
4680 |
4681 | if (comp_meth == COMP_NONE0 ||
4682 | comp_meth == COMP_MODULATION4 ||
4683 | comp_meth == MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8) {
4684 |
4685 | /* Not even creating a subtree for udCompMeth 0, 4, 8 */
4686 | return offset;
4687 | }
4688 |
4689 | /* Subtree */
4690 | unsigned start_offset = offset;
4691 | proto_item *udcompparam_ti = proto_tree_add_string_format(tree, hf_oran_udCompParam,
4692 | tvb, offset, 1, "",
4693 | (for_sinr) ? "sinrCompParam" : "udCompParam");
4694 | proto_tree *udcompparam_tree = proto_item_add_subtree(udcompparam_ti, ett_oran_udcompparam);
4695 |
4696 | /* Show comp_meth as a generated field */
4697 | proto_item *meth_ti = proto_tree_add_uint(udcompparam_tree, hf_oran_udCompHdrMeth_pref, tvb, 0, 0, comp_meth);
4698 | proto_item_set_generated(meth_ti);
4699 |
4700 | uint32_t param_exponent;
4701 | uint64_t param_sresmask;
4702 |
4703 | static int * const sres_mask_flags[] = {
4704 | &hf_oran_sReSMask_re12,
4705 | &hf_oran_sReSMask_re11,
4706 | &hf_oran_sReSMask_re10,
4707 | &hf_oran_sReSMask_re9,
4708 | &hf_oran_sReSMask_re8,
4709 | &hf_oran_sReSMask_re7,
4710 | &hf_oran_sReSMask_re6,
4711 | &hf_oran_sReSMask_re5,
4712 | &hf_oran_sReSMask_re4,
4713 | &hf_oran_sReSMask_re3,
4714 | &hf_oran_sReSMask_re2,
4715 | &hf_oran_sReSMask_re1,
4716 | NULL((void*)0)
4717 | };
4718 |
4719 | switch (comp_meth) {
4720 | case COMP_BLOCK_FP1: /* 1 */
4721 | case BFP_AND_SELECTIVE_RE_WITH_MASKS7: /* 7 */
4722 | /* reserved (4 bits) */
4723 | proto_tree_add_item(udcompparam_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_NA0x00000000);
4724 | /* exponent (4 bits) */
4725 | proto_tree_add_item_ret_uint(udcompparam_tree, hf_oran_exponent,
4726 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &param_exponent);
4727 | *exponent = param_exponent;
4728 | proto_item_append_text(udcompparam_ti, " (Exponent=%u)", param_exponent);
4729 | offset += 1;
4730 | break;
4731 |
4732 | case COMP_BLOCK_SCALE2: /* 2 */
4733 | /* Separate into integer and fractional bits? */
4734 | proto_tree_add_item(udcompparam_tree, hf_oran_blockScaler,
4735 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4736 | offset++;
4737 | break;
4738 |
4739 | case COMP_U_LAW3: /* 3 */
4740 | /* compBitWidth, compShift */
4741 | proto_tree_add_item(udcompparam_tree, hf_oran_compBitWidth,
4742 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4743 | proto_tree_add_item(udcompparam_tree, hf_oran_compShift,
4744 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4745 | offset += 1;
4746 | break;
4747 |
4748 | case BFP_AND_SELECTIVE_RE5: /* 5 */
4749 | {
4750 | /* sReSMask (exponent in middle!) */
4751 | proto_item *sresmask_ti;
4752 | sresmask_ti = proto_tree_add_bitmask_ret_uint64(udcompparam_tree, tvb, offset,
4753 | hf_oran_sReSMask,
4754 | ett_oran_sresmask,
4755 | sres_mask_flags,
4756 | ENC_NA0x00000000,
4757 | &param_sresmask);
4758 |
4759 | /* Get rid of exponent-shaped gap */
4760 | param_sresmask = ((param_sresmask >> 4) & 0x0f00) | (param_sresmask & 0xff);
4761 | unsigned res = 0;
4762 | for (unsigned n=0; n < 12; n++) {
4763 | if ((param_sresmask >> n) & 0x1) {
4764 | res++;
4765 | }
4766 | }
4767 | proto_item_append_text(sresmask_ti, " (%2u REs)", res);
4768 |
4769 | /* exponent */
4770 | proto_tree_add_item_ret_uint(udcompparam_tree, hf_oran_exponent,
4771 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &param_exponent);
4772 | *sReSMask = (uint16_t)param_sresmask;
4773 | *exponent = param_exponent;
4774 |
4775 | proto_item_append_text(udcompparam_ti, " (exponent=%u, %u REs)", *exponent, res);
4776 | offset += 2;
4777 | break;
4778 | }
4779 |
4780 | case MOD_COMPR_AND_SELECTIVE_RE6: /* 6 */
4781 | {
4782 | /* sReSMask (exponent in middle!) */
4783 | proto_item *sresmask_ti;
4784 |
4785 | sresmask_ti = proto_tree_add_bitmask_ret_uint64(udcompparam_tree, tvb, offset,
4786 | hf_oran_sReSMask,
4787 | ett_oran_sresmask,
4788 | sres_mask_flags,
4789 | ENC_NA0x00000000,
4790 | &param_sresmask);
4791 |
4792 | /* Get rid of reserved-shaped gap */
4793 | param_sresmask = ((param_sresmask >> 4) & 0x0f00) | (param_sresmask & 0xff);
4794 | unsigned res = 0;
4795 | for (unsigned n=0; n < 12; n++) {
4796 | if ((param_sresmask >> n) & 0x1) {
4797 | res++;
4798 | }
4799 | }
4800 | proto_item_append_text(sresmask_ti, " (%u REs)", res);
4801 |
4802 | /* reserved (4 bits) */
4803 | proto_tree_add_item(udcompparam_tree, hf_oran_reserved_last_4bits,
4804 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4805 | *sReSMask = (uint16_t)param_sresmask;
4806 |
4807 | proto_item_append_text(udcompparam_ti, " (%u REs)", res);
4808 | offset += 2;
4809 | break;
4810 | }
4811 |
4812 | default:
4813 | /* reserved (set to all zeros), but how many bytes?? */
4814 | break;
4815 | }
4816 |
4817 | proto_item_set_len(udcompparam_ti, offset-start_offset);
4818 | return offset;
4819 | }
4820 |
4821 |
4822 | /* Dissect ciCompHdr (channel information compression header, 7.5.2.15) */
4823 | /* bit_width and comp_meth are out params */
4824 | static int dissect_cicomphdr(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree, unsigned offset,
4825 | unsigned *bit_width, unsigned *comp_meth, uint8_t *comp_opt)
4826 | {
4827 | /* Subtree */
4828 | proto_item *cicomphdr_ti = proto_tree_add_string_format(tree, hf_oran_ciCompHdr,
4829 | tvb, offset, 1, "",
4830 | "ciCompHdr");
4831 | proto_tree *cicomphdr_tree = proto_item_add_subtree(cicomphdr_ti, ett_oran_cicomphdr);
4832 |
4833 | /* ciIqWidth */
4834 | uint32_t hdr_iq_width;
4835 | proto_item *iq_width_item = proto_tree_add_item_ret_uint(cicomphdr_tree, hf_oran_ciCompHdrIqWidth , tvb, offset, 1, ENC_NA0x00000000, &hdr_iq_width);
4836 | hdr_iq_width = (hdr_iq_width) ? hdr_iq_width : 16;
4837 | if (bit_width) {
4838 | *bit_width = hdr_iq_width;
4839 | }
4840 | proto_item_append_text(iq_width_item, " (%u bits)", hdr_iq_width);
4841 |
4842 | /* ciCompMeth */
4843 | uint32_t ci_comp_meth;
4844 | proto_tree_add_item_ret_uint(cicomphdr_tree, hf_oran_ciCompHdrMeth, tvb, offset, 1, ENC_NA0x00000000, &ci_comp_meth);
4845 | if (comp_meth) {
4846 | *comp_meth = ci_comp_meth;
4847 | }
4848 |
4849 | /* ciCompOpt */
4850 | uint32_t opt;
4851 | proto_tree_add_item_ret_uint(cicomphdr_tree, hf_oran_ciCompOpt, tvb, offset, 1, ENC_NA0x00000000, &opt);
4852 | *comp_opt = opt;
4853 | offset += 1;
4854 |
4855 | /* Summary */
4856 | proto_item_append_text(cicomphdr_ti, " (IqWidth=%u, ciCompMeth=%s, ciCompOpt=%s)",
4857 | hdr_iq_width,
4858 | rval_to_str_const(ci_comp_meth, ud_comp_header_meth, "Unknown"),
4859 | (*comp_opt) ? "compression per PRB" : "compression per UE");
4860 | return offset;
4861 | }
4862 |
4863 | static void dissect_payload_version(proto_tree *tree, tvbuff_t *tvb, packet_info *pinfo, unsigned offset)
4864 | {
4865 | unsigned version;
4866 | proto_item *ti = proto_tree_add_item_ret_uint(tree, hf_oran_payload_version, tvb, offset, 1, ENC_NA0x00000000, &version);
4867 | if (version != 1) {
4868 | expert_add_info_format(pinfo, ti, &ei_oran_version_unsupported,
4869 | "PayloadVersion %u not supported by dissector (only 1 is known)",
4870 | version);
4871 | /* TODO: should throw an exception? */
4872 | }
4873 | }
4874 |
4875 | static void show_link_to_acknack_request(proto_tree *tree, tvbuff_t *tvb, packet_info *pinfo,
4876 | ack_nack_request_t *request)
4877 | {
4878 | /* Request frame */
4879 | proto_item *ti = proto_tree_add_uint(tree, hf_oran_acknack_request_frame,
4880 | tvb, 0, 0, request->request_frame_number);
4881 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
4882 |
4883 | /* Work out gap between frames (in ms) */
4884 | int seconds_between_packets = (int)
4885 | (pinfo->abs_ts.secs - request->request_frame_time.secs);
4886 | int nseconds_between_packets =
4887 | pinfo->abs_ts.nsecs - request->request_frame_time.nsecs;
4888 |
4889 | int total_gap = (seconds_between_packets*1000) +
4890 | ((nseconds_between_packets+500000) / 1000000);
4891 |
4892 | ti = proto_tree_add_uint(tree, hf_oran_acknack_request_time,
4893 | tvb, 0, 0, total_gap);
4894 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
4895 |
4896 | /* Type of request */
4897 | ti = proto_tree_add_uint(tree, hf_oran_acknack_request_type,
4898 | tvb, 0, 0, request->requestType);
4899 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
4900 | }
4901 |
4902 | static void show_link_to_acknack_response(proto_tree *tree, tvbuff_t *tvb, packet_info *pinfo,
4903 | ack_nack_request_t *response)
4904 | {
4905 | if (response->response_frame_number == 0) {
4906 | /* Requests may not get a response, and can't always tell when to expect one */
4907 | return;
4908 | }
4909 |
4910 | /* Response frame */
4911 | proto_item *ti = proto_tree_add_uint(tree, hf_oran_acknack_response_frame,
4912 | tvb, 0, 0, response->response_frame_number);
4913 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
4914 |
4915 | /* Work out gap between frames (in ms) */
4916 | int seconds_between_packets = (int)
4917 | (response->response_frame_time.secs - pinfo->abs_ts.secs);
4918 | int nseconds_between_packets =
4919 | response->response_frame_time.nsecs - pinfo->abs_ts.nsecs;
4920 |
4921 | int total_gap = (seconds_between_packets*1000) +
4922 | ((nseconds_between_packets+500000) / 1000000);
4923 |
4924 | ti = proto_tree_add_uint(tree, hf_oran_acknack_response_time,
4925 | tvb, 0, 0, total_gap);
4926 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
4927 | }
4928 |
4929 |
4930 |
4931 | /* Control plane dissector (section 7). */
4932 | static int dissect_oran_c(tvbuff_t *tvb, packet_info *pinfo,
4933 | proto_tree *tree, oran_tap_info *tap_info, void *data _U___attribute__((unused)))
4934 | {
4935 | /* Hidden filter for plane */
4936 | proto_item *plane_ti = proto_tree_add_item(tree, hf_oran_cplane, tvb, 0, 0, ENC_NA0x00000000);
4937 | PROTO_ITEM_SET_HIDDEN(plane_ti)proto_item_set_hidden((plane_ti));
4938 |
4939 | /* Set up structures needed to add the protocol subtree and manage it */
4940 | unsigned offset = 0;
4941 |
4942 | col_set_str(pinfo->cinfo, COL_PROTOCOL, "O-RAN-FH-C");
4943 | col_set_str(pinfo->cinfo, COL_INFO, "C-Plane");
4944 |
4945 | tap_info->userplane = false0;
4946 |
4947 | /* Create display subtree for the protocol */
4948 | proto_item *protocol_item = proto_tree_add_item(tree, proto_oran, tvb, 0, -1, ENC_NA0x00000000);
4949 | proto_item_append_text(protocol_item, "-C");
4950 | proto_tree *oran_tree = proto_item_add_subtree(protocol_item, ett_oran);
4951 |
4952 | /* ecpriRtcid (eAxC ID) */
4953 | uint16_t eAxC;
4954 | addPcOrRtcid(tvb, oran_tree, &offset, hf_oran_ecpri_rtcid, &eAxC);
4955 | tap_info->eaxc = eAxC;
4956 |
4957 | /* Look up any existing conversation state for eAxC+plane */
4958 | uint32_t key = make_flow_key(pinfo, eAxC, ORAN_C_PLANE0, false0);
4959 | flow_state_t* state = (flow_state_t*)wmem_tree_lookup32(flow_states_table, key);
4960 |
4961 | /* Message identifier */
4962 | uint8_t seq_id;
4963 | proto_item *seq_id_ti;
4964 | offset = addSeqid(tvb, oran_tree, offset, ORAN_C_PLANE0, &seq_id, &seq_id_ti, pinfo);
4965 |
4966 | /* Section common subtree */
4967 | int section_tree_offset = offset;
4968 | proto_item *sectionHeading = proto_tree_add_string_format(oran_tree, hf_oran_c_section_common,
4969 | tvb, offset, 0, "", "C-Plane Section Type ");
4970 | proto_tree *section_tree = proto_item_add_subtree(sectionHeading, ett_oran_c_section_common);
4971 |
4972 | /* Peek ahead at the section type */
4973 | uint32_t sectionType = 0;
4974 | sectionType = tvb_get_uint8(tvb, offset+5);
4975 |
4976 | uint32_t scs = 0;
4977 | proto_item *scs_ti = NULL((void*)0);
4978 |
4979 | /* dataDirection */
4980 | uint32_t direction = 0;
4981 | proto_item *datadir_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_data_direction, tvb, offset, 1, ENC_NA0x00000000, &direction);
4982 | tap_info->uplink = (direction==0);
4983 |
4984 | /* Update/report status of conversation */
4985 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
4986 |
4987 | if (state == NULL((void*)0)) {
4988 | /* Allocate new state */
4989 | state = wmem_new0(wmem_file_scope(), flow_state_t)((flow_state_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_state_t )));
4990 | state->ack_nack_requests = wmem_tree_new(wmem_epan_scope());
4991 | wmem_tree_insert32(flow_states_table, key, state);
4992 | }
4993 |
4994 | /* Check sequence analysis status */
4995 | if (state->last_frame_seen[direction] && (seq_id != state->next_expected_sequence_number[direction])) {
4996 | /* Store this result */
4997 | flow_result_t *result = wmem_new0(wmem_file_scope(), flow_result_t)((flow_result_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_result_t )));
4998 | result->unexpected_seq_number = true1;
4999 | result->expected_sequence_number = state->next_expected_sequence_number[direction];
5000 | result->previous_frame = state->last_frame[direction];
5001 | wmem_tree_insert32(flow_results_table, pinfo->num, result);
5002 | }
5003 | /* Update conversation info */
5004 | state->last_frame[direction] = pinfo->num;
5005 | state->last_frame_seen[direction] = true1;
5006 | state->next_expected_sequence_number[direction] = (seq_id+1) % 256;
5007 | }
5008 |
5009 | /* Show any issues associated with this frame number */
5010 | flow_result_t *result = wmem_tree_lookup32(flow_results_table, pinfo->num);
5011 | if (result!=NULL((void*)0) && result->unexpected_seq_number) {
5012 | expert_add_info_format(pinfo, seq_id_ti,
5013 | (direction == DIR_UPLINK0) ?
5014 | &ei_oran_cplane_unexpected_sequence_number_ul :
5015 | &ei_oran_cplane_unexpected_sequence_number_dl,
5016 | "Sequence number %u expected, but got %u",
5017 | result->expected_sequence_number, seq_id);
5018 |
5019 | /* Update tap info */
5020 | uint32_t missing_sns = (256 + seq_id - result->expected_sequence_number) % 256;
5021 | /* Don't get confused by being slightly out of order.. */
5022 | if (missing_sns < 128) {
5023 | tap_info->missing_sns = missing_sns;
5024 | }
5025 | else {
5026 | tap_info->missing_sns = 0;
5027 | }
5028 |
5029 | /* TODO: could add previous/next frames (in seqId tree?) ? */
5030 | }
5031 |
5032 | /* payloadVersion */
5033 | dissect_payload_version(section_tree, tvb, pinfo, offset);
5034 |
5035 | /* filterIndex */
5036 | if (sectionType == SEC_C_SLOT_CONTROL || sectionType == SEC_C_ACK_NACK_FEEDBACK) {
5037 | /* scs (for ST4 and ST8) */
5038 | scs_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_frameStructure_subcarrier_spacing, tvb, offset, 1, ENC_NA0x00000000, &scs);
5039 | }
5040 | else if (sectionType == SEC_C_RRM_MEAS_REPORTS || sectionType == SEC_C_REQUEST_RRM_MEAS) {
5041 | /* reserved (4 bits) */
5042 | proto_tree_add_item(section_tree, hf_oran_reserved_last_4bits, tvb, offset, 1, ENC_NA0x00000000);
5043 | }
5044 | else if (sectionType != SEC_C_LAA) {
5045 | /* filterIndex (most common case) */
5046 | proto_tree_add_item(section_tree, hf_oran_filter_index, tvb, offset, 1, ENC_NA0x00000000);
5047 | }
5048 | offset += 1;
5049 |
5050 | unsigned ref_a_offset = offset;
5051 | /* frameId */
5052 | uint32_t frameId = 0;
5053 | proto_tree_add_item_ret_uint(section_tree, hf_oran_frame_id, tvb, offset, 1, ENC_NA0x00000000, &frameId);
5054 | tap_info->frame = frameId;
5055 | offset += 1;
5056 |
5057 | /* subframeId */
5058 | uint32_t subframeId = 0;
5059 | proto_tree_add_item_ret_uint(section_tree, hf_oran_subframe_id, tvb, offset, 1, ENC_NA0x00000000, &subframeId);
5060 | /* slotId */
5061 | uint32_t slotId = 0;
5062 | proto_tree_add_item_ret_uint(section_tree, hf_oran_slot_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &slotId);
5063 | tap_info->slot = slotId;
5064 | offset++;
5065 |
5066 | /* startSymbolId */
5067 | uint32_t startSymbolId = 0;
5068 | proto_item *ssid_ti = NULL((void*)0);
5069 | if ((sectionType == SEC_C_ACK_NACK_FEEDBACK) || /* Section Type 8 */
5070 | (sectionType == SEC_C_SINR_REPORTING)) { /* Section Type 9 */
5071 | /* symbolId */
5072 | proto_tree_add_item_ret_uint(section_tree, hf_oran_symbolId, tvb, offset, 1, ENC_NA0x00000000, &startSymbolId);
5073 | }
5074 | else if (sectionType != SEC_C_LAA) {
5075 | /* startSymbolId is in most section types */
5076 | ssid_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_start_symbol_id, tvb, offset, 1, ENC_NA0x00000000, &startSymbolId);
5077 | if (startSymbolId && (sectionType == SEC_C_RRM_MEAS_REPORTS)) { /* Section Type 10 */
5078 | proto_item_append_text(ssid_ti, " (should be 0 for ST10!)");
5079 | expert_add_info_format(pinfo, ssid_ti, &ei_oran_st10_startsymbolid_not_0,
5080 | "startSymbolId should be 0 for ST10 - found %u", startSymbolId);
5081 | }
5082 | }
5083 | else {
5084 | /* reserved (6 bits) */
5085 | proto_tree_add_item(section_tree, hf_oran_reserved_last_6bits, tvb, offset, 1, ENC_NA0x00000000);
5086 | }
5087 | offset++;
5088 |
5089 | char id[16];
5090 | snprintf(id, 16, "%d-%d-%d-%d", frameId, subframeId, slotId, startSymbolId);
5091 | proto_item *pi = proto_tree_add_string(section_tree, hf_oran_refa, tvb, ref_a_offset, 3, id);
5092 | proto_item_set_generated(pi);
5093 |
5094 | uint32_t cmd_scope = 0;
5095 | bool_Bool st8_ready = false0;
5096 |
5097 | /* numberOfSections (or whatever section has instead) */
5098 | uint32_t nSections = 0;
5099 | if (sectionType == SEC_C_SLOT_CONTROL) { /* Section Type 4 */
5100 | /* Slot Control has these fields instead */
5101 | /* reserved (4 bits) */
5102 | proto_tree_add_item(section_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_NA0x00000000);
5103 | /* cmdScope (4 bits) */
5104 | proto_tree_add_item_ret_uint(section_tree, hf_oran_cmd_scope, tvb, offset, 1, ENC_NA0x00000000, &cmd_scope);
5105 | }
5106 | else if (sectionType == SEC_C_ACK_NACK_FEEDBACK) { /* Section Type 8 */
5107 | /* reserved (7 bits) */
5108 | proto_tree_add_item(section_tree, hf_oran_reserved_7bits, tvb, offset, 1, ENC_NA0x00000000);
5109 | /* ready (1 bit) */
5110 | /* TODO: when set, ready in slotId+1.. */
5111 | proto_tree_add_item_ret_boolean(section_tree, hf_oran_ready, tvb, offset, 1, ENC_NA0x00000000, &st8_ready);
5112 | if (!st8_ready) {
5113 | /* SCS value is ignored, and may be set to any value by O-RU */
5114 | proto_item_append_text(scs_ti, " (ignored)");
5115 | }
5116 | }
5117 | else if (sectionType != SEC_C_LAA) {
5118 | /* numberOfSections */
5119 | proto_tree_add_item_ret_uint(section_tree, hf_oran_numberOfSections, tvb, offset, 1, ENC_NA0x00000000, &nSections);
5120 | }
5121 | else {
5122 | proto_tree_add_item(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000);
5123 | }
5124 | offset++;
5125 |
5126 | /* sectionType */
5127 | proto_tree_add_item_ret_uint(section_tree, hf_oran_sectionType, tvb, offset, 1, ENC_NA0x00000000, &sectionType);
5128 | offset += 1;
5129 |
5130 | /* Check that dataDirection is consistent with section type */
5131 | if (sectionType == SEC_C_SINR_REPORTING && direction != 0) { /* Section Type 9 */
5132 | expert_add_info(pinfo, datadir_ti, &ei_oran_st9_not_ul);
5133 | }
5134 | if (sectionType == SEC_C_RRM_MEAS_REPORTS && direction != 0) { /* Section Type 10 */
5135 | expert_add_info(pinfo, datadir_ti, &ei_oran_st10_not_ul);
5136 | }
5137 |
5138 | /* Note this section type in stats */
5139 | if (sectionType < SEC_C_MAX_INDEX) {
5140 | tap_info->section_types[sectionType] = true1;
5141 | }
5142 |
5143 | /* Section-type-specific fields following common header (white entries in Section Type diagrams) */
5144 | unsigned bit_width = 0;
5145 | int comp_meth = 0;
5146 | proto_item *comp_meth_ti;
5147 | unsigned ci_comp_method = 0;
5148 | uint8_t ci_comp_opt = 0;
5149 |
5150 | uint32_t num_ues = 0;
5151 | uint32_t number_of_acks = 0, number_of_nacks = 0;
5152 |
5153 | uint32_t num_sinr_per_prb = 0;
5154 |
5155 | switch (sectionType) {
5156 | case SEC_C_UNUSED_RB: /* Section Type 0 */
5157 | /* timeOffset */
5158 | proto_tree_add_item(section_tree, hf_oran_timeOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5159 | offset += 2;
5160 | /* frameStructure */
5161 | offset = dissect_frame_structure(section_tree, tvb, offset,
5162 | subframeId, slotId);
5163 |
5164 | /* cpLength */
5165 | proto_tree_add_item(section_tree, hf_oran_cpLength, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5166 | offset += 2;
5167 | /* reserved */
5168 | proto_tree_add_item(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000);
5169 | offset += 1;
5170 | break;
5171 |
5172 | case SEC_C_NORMAL: /* Section Type 1 */
5173 | case SEC_C_UE_SCHED: /* Section Type 5 */
5174 | /* udCompHdr */
5175 | offset = dissect_udcomphdr(tvb, pinfo, section_tree, offset,
5176 | (direction==1), /* ignore for DL */
5177 | &bit_width, &comp_meth, &comp_meth_ti);
5178 | /* reserved */
5179 | proto_tree_add_item(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000);
5180 | offset += 1;
5181 | break;
5182 |
5183 | case SEC_C_SLOT_CONTROL: /* Section Type 4 */
5184 | break;
5185 |
5186 | case SEC_C_PRACH: /* Section Type 3 */
5187 | /* timeOffset */
5188 | proto_tree_add_item(section_tree, hf_oran_timeOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5189 | offset += 2;
5190 | /* frameStructure */
5191 | offset = dissect_frame_structure(section_tree, tvb, offset,
5192 | subframeId, slotId);
5193 | /* cpLength */
5194 | proto_tree_add_item(section_tree, hf_oran_cpLength, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5195 | offset += 2;
5196 | /* udCompHdr */
5197 | offset = dissect_udcomphdr(tvb, pinfo, section_tree, offset,
5198 | (direction==1), /* ignore for DL */
5199 | &bit_width, &comp_meth, &comp_meth_ti);
5200 | break;
5201 |
5202 | case SEC_C_CH_INFO: /* Section Type 6 */
5203 | /* numberOfUEs */
5204 | proto_tree_add_item_ret_uint(section_tree, hf_oran_numberOfUEs, tvb, offset, 1, ENC_NA0x00000000, &num_ues);
5205 | offset += 1;
5206 | /* ciCompHdr (was reserved) */
5207 | offset = dissect_cicomphdr(tvb, pinfo, section_tree, offset, &bit_width, &ci_comp_method, &ci_comp_opt);
5208 |
5209 | /* Number of sections may not be filled in (at all, or correctly), so set to the number of UEs.
5210 | The data entries are per-UE... they don't have a sectionID, but they could have section extensions... */
5211 | if (nSections == 0 || num_ues > nSections) {
5212 | nSections = num_ues;
5213 | }
5214 | break;
5215 |
5216 | case SEC_C_RSVD2:
5217 | break;
5218 |
5219 | case SEC_C_LAA: /* Section Type 7 */
5220 | proto_tree_add_item(section_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5221 | offset += 2;
5222 | break;
5223 |
5224 | case SEC_C_ACK_NACK_FEEDBACK: /* Section Type 8 */
5225 | /* numberOfAcks (1 byte) */
5226 | proto_tree_add_item_ret_uint(section_tree, hf_oran_number_of_acks, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &number_of_acks);
5227 | offset += 1;
5228 | /* numberOfNacks (1 byte) */
5229 | proto_tree_add_item_ret_uint(section_tree, hf_oran_number_of_nacks, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &number_of_nacks);
5230 | offset += 1;
5231 |
5232 | /* Show ACKs and NACKs. For both, try to link back to request. */
5233 | for (unsigned int n=1; n <= number_of_acks; n++) {
5234 | uint32_t ackid;
5235 | proto_item *ack_ti;
5236 | ack_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_ackid, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ackid);
5237 | offset += 2;
5238 |
5239 | /* Look up request table in state (which really should be set by now, but test anyway). */
5240 | if (state && state->ack_nack_requests) {
5241 | ack_nack_request_t *request = wmem_tree_lookup32(state->ack_nack_requests, ackid);
5242 | if (request != NULL((void*)0)) {
5243 | /* On first pass, update with this response */
5244 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
5245 | request->response_frame_number = pinfo->num;
5246 | request->response_frame_time = pinfo->abs_ts;
5247 | }
5248 |
5249 | /* Show request details */
5250 | show_link_to_acknack_request(section_tree, tvb, pinfo, request);
5251 | }
5252 | else {
5253 | /* Request not found */
5254 | expert_add_info_format(pinfo, ack_ti, &ei_oran_acknack_no_request,
5255 | "Response for ackId=%u received, but no request found",
5256 | ackid);
5257 | }
5258 | }
5259 | }
5260 | for (unsigned int m=1; m <= number_of_nacks; m++) {
5261 | uint32_t nackid;
5262 | proto_item *nack_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_nackid, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &nackid);
5263 | offset += 2;
5264 |
5265 | expert_add_info_format(pinfo, nack_ti, &ei_oran_st8_nackid,
5266 | "Received Nack for ackNackId=%u",
5267 | nackid);
5268 |
5269 | /* Look up request table in state. */
5270 | if (state && state->ack_nack_requests) {
5271 | ack_nack_request_t *request = wmem_tree_lookup32(state->ack_nack_requests, nackid);
5272 | if (request) {
5273 | /* On first pass, update with this response */
5274 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
5275 | request->response_frame_number = pinfo->num;
5276 | request->response_frame_time = pinfo->abs_ts;
5277 | }
5278 |
5279 | /* Show request details */
5280 | show_link_to_acknack_request(section_tree, tvb, pinfo, request);
5281 | }
5282 | else {
5283 | /* Request not found */
5284 | expert_add_info_format(pinfo, nack_ti, &ei_oran_acknack_no_request,
5285 | "Response for nackId=%u received, but no request found",
5286 | nackid);
5287 | }
5288 | }
5289 | }
5290 | break;
5291 |
5292 | case SEC_C_SINR_REPORTING: /* Section Type 9 */
5293 | {
5294 | /* numSinrPerPrb (3 bits) */
5295 | proto_item *nspp_ti;
5296 | nspp_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_num_sinr_per_prb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_sinr_per_prb);
5297 | switch (num_sinr_per_prb) {
5298 | case 0:
5299 | num_sinr_per_prb = 1; break;
5300 | case 1:
5301 | num_sinr_per_prb = 2; break;
5302 | case 2:
5303 | num_sinr_per_prb = 3; break;
5304 | case 3:
5305 | num_sinr_per_prb = 4; break;
5306 | case 4:
5307 | num_sinr_per_prb = 6; break;
5308 | case 5:
5309 | num_sinr_per_prb = 12; break;
5310 |
5311 | default:
5312 | proto_item_append_text(nspp_ti, " (invalid)");
5313 | num_sinr_per_prb = 1;
5314 | expert_add_info_format(pinfo, nspp_ti, &ei_oran_num_sinr_per_prb_unknown,
5315 | "Invalid numSinrPerPrb value (%u)",
5316 | num_sinr_per_prb);
5317 | }
5318 |
5319 | /* reserved (13 bits) */
5320 | proto_tree_add_item(section_tree, hf_oran_reserved_last_5bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5321 | offset += 1;
5322 | proto_tree_add_item(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5323 | offset += 1;
5324 | break;
5325 | }
5326 |
5327 | case SEC_C_RRM_MEAS_REPORTS: /* Section Type 10 */
5328 | case SEC_C_REQUEST_RRM_MEAS: /* Section Type 11 */
5329 | /* reserved (16 bits) */
5330 | proto_tree_add_item(section_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5331 | offset += 2;
5332 | break;
5333 | };
5334 |
5335 | /* Update udCompHdr details in state for UL U-Plane */
5336 | if (state && direction==0) {
5337 | switch (sectionType) {
5338 | case SEC_C_NORMAL: /* Section Type 1 */
5339 | case SEC_C_PRACH: /* Section Type 3 */
5340 | case SEC_C_UE_SCHED: /* Section Type 5 */
5341 | state->ul_ud_comp_hdr_set = true1;
5342 | state->ul_ud_comp_hdr_bit_width = bit_width;
5343 | state->ul_ud_comp_hdr_compression = comp_meth;
5344 | state->ul_ud_comp_hdr_frame = pinfo->num;
5345 | break;
5346 | default:
5347 | break;
5348 | }
5349 | }
5350 |
5351 |
5352 | proto_item_append_text(sectionHeading, "%d, %s, frameId: %d, subframeId: %d, slotId: %d, startSymbolId: %d",
5353 | sectionType, val_to_str_const(direction, data_direction_vals, "Unknown"),
5354 | frameId, subframeId, slotId, startSymbolId);
5355 | if (nSections) {
5356 | proto_item_append_text(sectionHeading, ", numberOfSections=%u", nSections);
5357 | }
5358 |
5359 | write_pdu_label_and_info(protocol_item, NULL((void*)0), pinfo, ", Type: %2d %s", sectionType,
5360 | rval_to_str_const(sectionType, section_types_short, "Unknown"));
5361 |
5362 | /* Set actual length of C-Plane section header */
5363 | proto_item_set_len(section_tree, offset - section_tree_offset);
5364 |
5365 | if (sectionType == SEC_C_ACK_NACK_FEEDBACK) {
5366 | write_pdu_label_and_info(oran_tree, section_tree, pinfo,
5367 | (st8_ready) ? " (Ready)" : " (ACK)");
5368 | }
5369 |
5370 |
5371 | /* Section type 4 doesn't have normal sections, so deal with here before normal sections */
5372 | if (sectionType == SEC_C_SLOT_CONTROL) {
5373 | /* numberOfST4Cmds */
5374 | uint32_t no_st4_cmds, st4_cmd_len, num_slots, ack_nack_req_id, st4_cmd_type;
5375 | proto_item *no_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_number_of_st4_cmds,
5376 | tvb, offset, 1, ENC_NA0x00000000, &no_st4_cmds);
5377 | if (no_st4_cmds == 0) {
5378 | expert_add_info_format(pinfo, no_ti, &ei_oran_st4_no_cmds,
5379 | "Not valid for ST4 to carry no commands");
5380 | }
5381 | offset += 1;
5382 |
5383 | /* reserved (1 byte) */
5384 | proto_tree_add_item(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5385 | offset += 1;
5386 |
5387 | /* Loop over commands. Each has 8-byte common header, followed by cmd-specific payload */
5388 | proto_item *len_ti;
5389 | for (uint32_t n=0; n < no_st4_cmds; n++) {
5390 | /* Table 7.4.6-2: Section Type 4 Command common header format */
5391 | proto_item *hdr_ti = proto_tree_add_string_format(section_tree, hf_oran_st4_cmd_header,
5392 | tvb, offset, 8, "",
5393 | "Type 4 Command common header");
5394 | proto_tree *hdr_tree = proto_item_add_subtree(hdr_ti, ett_oran_st4_cmd_header);
5395 |
5396 | /* st4CmdType */
5397 | proto_tree_add_item_ret_uint(hdr_tree, hf_oran_st4_cmd_type, tvb, offset, 1, ENC_NA0x00000000, &st4_cmd_type);
5398 | offset += 1;
5399 |
5400 | /* st4CmdLen */
5401 | len_ti = proto_tree_add_item_ret_uint(hdr_tree, hf_oran_st4_cmd_len, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &st4_cmd_len);
5402 | if (st4_cmd_len == 0) {
5403 | /* Meaning of 0 not yet defined (v15.00) */
5404 | proto_item_append_text(len_ti, " (reserved)");
5405 | expert_add_info(pinfo, len_ti, &ei_oran_st4_zero_len_cmd);
5406 | }
5407 | else {
5408 | proto_item_append_text(len_ti, " (%u bytes)", st4_cmd_len*4);
5409 | }
5410 | offset += 2;
5411 |
5412 | /* numSlots */
5413 | proto_item *slots_ti = proto_tree_add_item_ret_uint(hdr_tree, hf_oran_st4_cmd_num_slots, tvb, offset, 1, ENC_NA0x00000000, &num_slots);
5414 | if (num_slots == 0) {
5415 | proto_item_append_text(slots_ti, " (until changed)");
5416 | }
5417 | offset += 1;
5418 |
5419 | /* ackNackReqId */
5420 | proto_item *ack_nack_req_id_ti;
5421 | ack_nack_req_id_ti = proto_tree_add_item_ret_uint(hdr_tree, hf_oran_st4_cmd_ack_nack_req_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ack_nack_req_id);
5422 | offset += 2;
5423 | if (ack_nack_req_id == 0) {
5424 | proto_item_append_text(ack_nack_req_id_ti, " (no Section type 8 response expected)");
5425 | }
5426 |
5427 | /* reserved (16 bits) */
5428 | proto_tree_add_item(hdr_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5429 | offset += 2;
5430 |
5431 | /* Set common header summary */
5432 | proto_item_append_text(hdr_ti, " (cmd=%s, len=%u, slots=%u, ackNackReqId=%u)",
5433 | rval_to_str_const(st4_cmd_type, st4_cmd_type_vals, "Unknown"),
5434 | st4_cmd_len, num_slots, ack_nack_req_id);
5435 |
5436 | col_append_fstr(pinfo->cinfo, COL_INFO, " (%s)",
5437 | rval_to_str_const(st4_cmd_type, st4_cmd_type_vals, "Unknown"));
5438 |
5439 |
5440 | /* Subtree for this command body */
5441 | proto_item *command_ti = proto_tree_add_string_format(section_tree, hf_oran_st4_cmd,
5442 | tvb, offset, 0, "",
5443 | "Type 4 Command (%s)", rval_to_str_const(st4_cmd_type, st4_cmd_type_vals, "Unknown"));
5444 | proto_tree *command_tree = proto_item_add_subtree(command_ti, ett_oran_st4_cmd);
5445 |
5446 | unsigned command_start_offset = offset;
5447 |
5448 | /* Check fields compatible with chosen command. */
5449 | if (st4_cmd_type==1) {
5450 | if (num_slots != 0) {
5451 | /* "the value of numSlots should be set to zero for this command type" */
5452 | expert_add_info_format(pinfo, slots_ti, &ei_oran_numslots_not_zero,
5453 | "numSlots should be zero for ST4 command 1 - found %u",
5454 | num_slots);
5455 | }
5456 | }
5457 |
5458 | if (st4_cmd_type==3 || st4_cmd_type==4) {
5459 | if (startSymbolId != 0) {
5460 | /* "expected reception window for the commands is the symbol zero reception window" */
5461 | expert_add_info_format(pinfo, ssid_ti, &ei_oran_start_symbol_id_not_zero,
5462 | "startSymbolId should be zero for ST4 commands 3&4 - found %u",
5463 | startSymbolId);
5464 | }
5465 | }
5466 |
5467 | /* Add format for this command */
5468 | switch (st4_cmd_type) {
5469 | case 1: /* TIME_DOMAIN_BEAM_CONFIG */
5470 | {
5471 | bool_Bool disable_tdbfns;
5472 | uint32_t bfwcomphdr_iq_width, bfwcomphdr_comp_meth;
5473 |
5474 | /* Hidden filter for bf */
5475 | proto_item *bf_ti = proto_tree_add_item(command_tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
5476 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
5477 |
5478 | /* reserved (2 bits) */
5479 | proto_tree_add_item(command_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5480 | /* symbolMask (14 bits) */
5481 | uint32_t symbol_mask;
5482 | proto_item *symbol_mask_ti;
5483 | offset = dissect_symbolmask(tvb, command_tree, offset, &symbol_mask, &symbol_mask_ti);
5484 | /* Symbol bits before 'startSymbolId' in Section Type 4 common header should be set to 0 by O-DU and shall be ignored by O-RU */
5485 | /* lsb is symbol 0 */
5486 | for (unsigned s=0; s < 14; s++) {
5487 | if ((startSymbolId & (1 << s)) && (startSymbolId > s)) {
5488 | proto_item_append_text(symbol_mask_ti, " (startSymbolId is %u, so some lower symbol bits ignored!)", startSymbolId);
5489 | expert_add_info(pinfo, symbol_mask_ti, &ei_oran_start_symbol_id_bits_ignored);
5490 | break;
5491 | }
5492 | }
5493 |
5494 | /* disableTDBFNs (1 bit) */
5495 | proto_tree_add_item_ret_boolean(command_tree, hf_oran_disable_tdbfns, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &disable_tdbfns);
5496 |
5497 | /* tdBeamNum (15 bits) */
5498 | proto_tree_add_item(command_tree, hf_oran_td_beam_num, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5499 | offset += 2;
5500 |
5501 | /* bfwCompHdr (2 subheaders - bfwIqWidth and bfwCompMeth)*/
5502 | offset = dissect_bfwCompHdr(tvb, command_tree, offset,
5503 | &bfwcomphdr_iq_width, &bfwcomphdr_comp_meth, &comp_meth_ti);
5504 | /* reserved (3 bytes) */
5505 | proto_tree_add_bits_item(command_tree, hf_oran_reserved, tvb, offset*8, 24, ENC_BIG_ENDIAN0x00000000);
5506 | offset += 3;
5507 |
5508 | if (disable_tdbfns) {
5509 | /* No beamnum information to show so get out. */
5510 | break;
5511 | }
5512 |
5513 | /* Read beam entries until reach end of command length */
5514 | while ((offset - command_start_offset) < (st4_cmd_len * 4)) {
5515 |
5516 | /* disableTDBFWs (1 bit) */
5517 | bool_Bool disable_tdbfws;
5518 | proto_tree_add_item_ret_boolean(command_tree, hf_oran_disable_tdbfws, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &disable_tdbfws);
5519 |
5520 | /* tdBeamNum (15 bits) */
5521 | proto_tree_add_item(command_tree, hf_oran_td_beam_num, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5522 | offset += 2;
5523 |
5524 | /* Showing BFWs? */
5525 | if (!disable_tdbfws) {
5526 |
5527 | /* bfwCompParam */
5528 | unsigned exponent = 0;
5529 | bool_Bool supported = false0;
5530 | unsigned num_trx_entries;
5531 | uint16_t *trx_entries;
5532 | offset = dissect_bfwCompParam(tvb, command_tree, pinfo, offset, comp_meth_ti,
5533 | &bfwcomphdr_comp_meth, &exponent, &supported,
5534 | &num_trx_entries, &trx_entries);
5535 |
5536 | /* Antenna count from preference */
5537 | unsigned num_trx = pref_num_bf_antennas;
5538 | int bit_offset = offset*8;
5539 |
5540 | for (unsigned trx=0; trx < num_trx; trx++) {
5541 | /* Create antenna subtree */
5542 | int bfw_offset = bit_offset / 8;
5543 | proto_item *bfw_ti = proto_tree_add_string_format(command_tree, hf_oran_bfw,
5544 | tvb, bfw_offset, 0, "", "TRX %3u: (", trx);
5545 | proto_tree *bfw_tree = proto_item_add_subtree(bfw_ti, ett_oran_bfw);
5546 |
5547 | /* I value */
5548 | /* Get bits, and convert to float. */
5549 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
5550 | float value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent);
5551 | /* Add to tree. */
5552 | proto_tree_add_float(bfw_tree, hf_oran_bfw_i, tvb, bit_offset/8,
5553 | (bfwcomphdr_iq_width+7)/8, value);
5554 | bit_offset += bfwcomphdr_iq_width;
5555 | proto_item_append_text(bfw_ti, "I=%f ", value);
5556 |
5557 | /* Leave a gap between I and Q values */
5558 | proto_item_append_text(bfw_ti, " ");
5559 |
5560 | /* Q value */
5561 | /* Get bits, and convert to float. */
5562 | bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
5563 | value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent);
5564 | /* Add to tree. */
5565 | proto_tree_add_float(bfw_tree, hf_oran_bfw_q, tvb, bit_offset/8,
5566 | (bfwcomphdr_iq_width+7)/8, value);
5567 | bit_offset += bfwcomphdr_iq_width;
5568 | proto_item_append_text(bfw_ti, "Q=%f", value);
5569 |
5570 | proto_item_append_text(bfw_ti, ")");
5571 | proto_item_set_len(bfw_ti, (bit_offset+7)/8 - bfw_offset);
5572 | }
5573 | /* Need to round to next byte */
5574 | offset = (bit_offset+7)/8;
5575 | }
5576 | }
5577 | break;
5578 | }
5579 | case 2: /* TDD_CONFIG_PATTERN */
5580 | /* reserved (2 bits) */
5581 | proto_tree_add_item(command_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5582 | /* dirPattern (14 bits) */
5583 | proto_tree_add_item(command_tree, hf_oran_dir_pattern, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5584 | offset += 2;
5585 |
5586 | /* reserved (2 bits) */
5587 | proto_tree_add_item(command_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5588 | /* guardPattern (14 bits) */
5589 | proto_tree_add_item(command_tree, hf_oran_guard_pattern, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5590 | offset += 2;
5591 | break;
5592 |
5593 | case 3: /* TRX_CONTROL */
5594 | {
5595 | /* Only allowed cmdScope is ARRAY-COMMAND */
5596 | if (cmd_scope != 0) {
5597 | expert_add_info(pinfo, command_tree, &ei_oran_trx_control_cmd_scope);
5598 | }
5599 |
5600 | /* reserved (2 bits) */
5601 | proto_tree_add_item(command_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5602 | /* log2MaskBits (4 bits) */
5603 | unsigned log2maskbits;
5604 | proto_tree_add_item_ret_uint(command_tree, hf_oran_log2maskbits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &log2maskbits);
5605 | /* sleepMode */
5606 | uint32_t sleep_mode;
5607 | proto_tree_add_item_ret_uint(command_tree, hf_oran_sleepmode_trx, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &sleep_mode);
5608 | offset += 1;
5609 |
5610 | /* reserved (4 bits) */
5611 | proto_tree_add_item(command_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5612 | /* numSlotsExt (20 bits) */
5613 | uint32_t num_slots_ext;
5614 | proto_item *num_slots_ext_ti = proto_tree_add_item_ret_uint(command_tree, hf_oran_num_slots_ext, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000, &num_slots_ext);
5615 | if (num_slots==0 && num_slots_ext==0) {
5616 | proto_item_append_text(num_slots_ext_ti, " (undefined sleep period)");
5617 | }
5618 | else {
5619 | /* Time should be rounded up according to SCS */
5620 | float total = (float)(num_slots + num_slots_ext);
5621 | /* From table 7.5.2.13-3 */
5622 | float slot_length_by_scs[16] = { 1000, 500, 250, 125, 62.5, 31.25,
5623 | 0, 0, 0, 0, 0, 0, /* reserved */
5624 | 1000, 1000, 1000, 1000 };
5625 | float slot_length = slot_length_by_scs[scs];
5626 | /* Only using valid SCS. TODO: is this test ok? */
5627 | if (slot_length != 0) {
5628 | /* Round up to next slot */
5629 | total = ((int)(total / slot_length) + 1) * slot_length;
5630 | proto_item_append_text(num_slots_ext_ti, " (defined sleep period of %f us)", total);
5631 | }
5632 | }
5633 | offset += 3;
5634 |
5635 | /* reserved (2 bits) */
5636 | proto_tree_add_item(command_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5637 |
5638 | /* symbolMask (14 bits) */
5639 | uint32_t symbol_mask;
5640 | proto_item *sm_ti;
5641 | offset = dissect_symbolmask(tvb, command_tree, offset, &symbol_mask, &sm_ti);
5642 | if (symbol_mask == 0x0) {
5643 | proto_item_append_text(sm_ti, " (wake)");
5644 | col_append_str(pinfo->cinfo, COL_INFO, " (wake)");
5645 | }
5646 | else if (symbol_mask == 0x3fff) {
5647 | proto_item_append_text(sm_ti, " (sleep)");
5648 | col_append_str(pinfo->cinfo, COL_INFO, " (sleep)");
5649 | }
5650 | else {
5651 | expert_add_info_format(pinfo, sm_ti, &ei_oran_bad_symbolmask,
5652 | "For non-zero sleepMode (%u), symbolMask should be 0x0 or 0x3fff - found 0x%05x",
5653 | sleep_mode, symbol_mask);
5654 | }
5655 | offset += 2;
5656 |
5657 | /* antMask (16-2048 bits). Size is lookup from log2MaskBits enum.. */
5658 | unsigned antmask_length = 2;
5659 | if (log2maskbits >= 4) {
5660 | antmask_length = (1 << log2maskbits) / 8;
5661 | }
5662 | proto_item *ant_mask_ti = proto_tree_add_item(command_tree, hf_oran_antMask_trx_control, tvb, offset, antmask_length, ENC_NA0x00000000);
5663 | /* show count */
5664 | unsigned antenna_count = 0;
5665 | for (unsigned b=0; b < antmask_length; b++) {
5666 | uint8_t byte = tvb_get_uint8(tvb, offset+b);
5667 | for (unsigned bit=0; bit < 8; bit++) {
5668 | if ((1 << bit) & byte) {
5669 | antenna_count++;
5670 | }
5671 | }
5672 | }
5673 | proto_item_append_text(ant_mask_ti, " (%u antennas)", antenna_count);
5674 | offset += antmask_length;
5675 |
5676 | /* Pad to next 4-byte boundary */
5677 | offset = WS_ROUNDUP_4(offset)(((offset) + ((unsigned)(4U-1U))) & (~((unsigned)(4U-1U)) ));
5678 | break;
5679 | }
5680 |
5681 | case 4: /* ASM (advanced sleep mode) */
5682 | /* reserved (2+4=6 bits) */
5683 | proto_tree_add_item(command_tree, hf_oran_reserved_6bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5684 | /* sleepMode (2 bits) */
5685 | uint32_t sleep_mode;
5686 | proto_tree_add_item_ret_uint(command_tree, hf_oran_sleepmode_asm, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &sleep_mode);
5687 | offset += 1;
5688 |
5689 | /* reserved (4 bits) */
5690 | proto_tree_add_item(command_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5691 | /* numSlotsExt (20 bits) */
5692 | proto_tree_add_item(command_tree, hf_oran_num_slots_ext, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000);
5693 | offset += 3;
5694 |
5695 | /* reserved (2 bits) */
5696 | proto_tree_add_item(command_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5697 | /* symbolMask (14 bits) */
5698 | uint32_t symbol_mask;
5699 | proto_item *sm_ti;
5700 | offset = dissect_symbolmask(tvb, command_tree, offset, &symbol_mask, &sm_ti);
5701 | if (symbol_mask == 0x0) {
5702 | proto_item_append_text(sm_ti, " (wake)");
5703 | col_append_str(pinfo->cinfo, COL_INFO, " (wake)");
5704 | }
5705 | else if (symbol_mask == 0x3fff) {
5706 | proto_item_append_text(sm_ti, " (sleep)");
5707 | col_append_str(pinfo->cinfo, COL_INFO, " (sleep)");
5708 | }
5709 | else {
5710 | expert_add_info_format(pinfo, sm_ti, &ei_oran_bad_symbolmask,
5711 | "For non-zero sleepMode (%u), symbolMask should be 0x0 or 0x3fff - found 0x%05x",
5712 | sleep_mode, symbol_mask);
5713 | }
5714 | offset += 2;
5715 |
5716 | /* reserved (2 bytes) */
5717 | proto_tree_add_item(command_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5718 | offset += 2;
5719 | break;
5720 |
5721 | default:
5722 | /* Error! */
5723 | expert_add_info_format(pinfo, len_ti, &ei_oran_st4_unknown_cmd,
5724 | "Dissected ST4 command (%u) not recognised",
5725 | st4_cmd_type);
5726 | break;
5727 | }
5728 |
5729 | /* Check apparent size of padding (0-3 bytes ok) */
5730 | long padding_remaining = command_start_offset + (st4_cmd_len * 4) - offset;
5731 | if (padding_remaining < 0 || padding_remaining > 3) {
5732 | expert_add_info_format(pinfo, len_ti, &ei_oran_st4_wrong_len_cmd,
5733 | "Dissected ST4 command does not match signalled st4CmdLen - set to %u (%u bytes) but dissected %u bytes",
5734 | st4_cmd_len, st4_cmd_len*4, offset-command_start_offset);
5735 | }
5736 |
5737 | /* Advance by signalled length (needs to be aligned on 4-byte boundary) */
5738 | offset = command_start_offset + (st4_cmd_len * 4);
5739 |
5740 | /* Set end of command tree */
5741 | proto_item_set_end(command_ti, tvb, offset);
5742 |
5743 | if (ack_nack_req_id != 0 && state && state->ack_nack_requests) {
5744 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
5745 | /* Add this request into conversation state on first pass */
5746 | ack_nack_request_t *request_details = wmem_new0(wmem_file_scope(), ack_nack_request_t)((ack_nack_request_t*)wmem_alloc0((wmem_file_scope()), sizeof (ack_nack_request_t)));
5747 | request_details->request_frame_number = pinfo->num;
5748 | request_details->request_frame_time = pinfo->abs_ts;
5749 | request_details->requestType = ST4Cmd1+st4_cmd_type-1;
5750 |
5751 | wmem_tree_insert32(state->ack_nack_requests,
5752 | ack_nack_req_id,
5753 | request_details);
5754 | }
5755 | else {
5756 | /* On later passes, try to link forward to ST8 response */
5757 | ack_nack_request_t *response = wmem_tree_lookup32(state->ack_nack_requests,
5758 | ack_nack_req_id);
5759 | if (response) {
5760 | show_link_to_acknack_response(section_tree, tvb, pinfo, response);
5761 | }
5762 | }
5763 | }
5764 | }
5765 | }
5766 | /* LAA doesn't have sections either.. */
5767 | else if (sectionType == SEC_C_LAA) { /* Section Type 7 */
5768 | /* 7.2.5 Table 6.4-6 */
5769 | unsigned mcot;
5770 | proto_item *mcot_ti;
5771 |
5772 | /* laaMsgType */
5773 | uint32_t laa_msg_type;
5774 | proto_item *laa_msg_type_ti;
5775 | laa_msg_type_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_laaMsgType, tvb, offset, 1, ENC_NA0x00000000, &laa_msg_type);
5776 | /* laaMsgLen */
5777 | uint32_t laa_msg_len;
5778 | proto_item *len_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_laaMsgLen, tvb, offset, 1, ENC_NA0x00000000, &laa_msg_len);
5779 | proto_item_append_text(len_ti, " (%u bytes)", 4*laa_msg_len);
5780 | if (laa_msg_len == 0) {
5781 | proto_item_append_text(len_ti, " (reserved)");
5782 | }
5783 | offset += 1;
5784 |
5785 | int payload_offset = offset;
5786 |
5787 | /* Payload */
5788 | switch (laa_msg_type) {
5789 | case 0:
5790 | /* LBT_PDSCH_REQ */
5791 | /* lbtHandle (16 bits) */
5792 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5793 | offset += 2;
5794 | /* lbtOffset (10 bits) */
5795 | proto_tree_add_item(section_tree, hf_oran_lbtOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5796 | offset += 1;
5797 | /* lbtMode (2 bits) */
5798 | proto_tree_add_bits_item(section_tree, hf_oran_lbtMode, tvb, offset*8+2, 2, ENC_BIG_ENDIAN0x00000000);
5799 | /* reserved (1 bit) */
5800 | proto_tree_add_item(section_tree, hf_oran_reserved_bit4, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5801 | /* lbtDeferFactor (3 bits) */
5802 | proto_tree_add_item(section_tree, hf_oran_lbtDeferFactor, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5803 | offset += 1;
5804 | /* lbtBackoffCounter (10 bits) */
5805 | proto_tree_add_item(section_tree, hf_oran_lbtBackoffCounter, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5806 | offset += 1;
5807 | /* MCOT (4 bits) */
5808 | mcot_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_MCOT, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &mcot);
5809 | if (mcot<1 || mcot>10) {
5810 | proto_item_append_text(mcot_ti, " (should be in range 1-10!)");
5811 | expert_add_info_format(pinfo, mcot_ti, &ei_oran_mcot_out_of_range,
5812 | "MCOT seen with value %u (must be 1-10)", mcot);
5813 |
5814 | }
5815 | /* reserved (10 bits) */
5816 | proto_tree_add_bits_item(section_tree, hf_oran_reserved, tvb, (offset*8)+6, 10, ENC_BIG_ENDIAN0x00000000);
5817 | break;
5818 | case 1:
5819 | /* LBT_DRS_REQ */
5820 | /* lbtHandle (16 bits) */
5821 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5822 | offset += 2;
5823 | /* lbtOffset (10 bits) */
5824 | proto_tree_add_item(section_tree, hf_oran_lbtOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5825 | offset += 1;
5826 | /* lbtMode (2 bits) */
5827 | proto_tree_add_bits_item(section_tree, hf_oran_lbtMode, tvb, offset*8+2, 2, ENC_BIG_ENDIAN0x00000000);
5828 | /* reserved (28 bits) */
5829 | proto_tree_add_bits_item(section_tree, hf_oran_reserved, tvb, (offset*8)+4, 28, ENC_BIG_ENDIAN0x00000000);
5830 | break;
5831 | case 2:
5832 | /* LBT_PDSCH_RSP */
5833 | /* lbtHandle (16 bits) */
5834 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5835 | offset += 2;
5836 | /* lbtPdschRes (2 bits) */
5837 | proto_tree_add_item(section_tree, hf_oran_lbtPdschRes, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5838 | /* inParSF (1 bit) */
5839 | proto_tree_add_item(section_tree, hf_oran_initialPartialSF, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5840 | /* sfStatus (1 bit) */
5841 | proto_tree_add_item(section_tree, hf_oran_sfStatus, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5842 | /* sfnSf (12 bits) */
5843 | proto_tree_add_item(section_tree, hf_oran_sfnSfEnd, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5844 | offset += 2;
5845 | /* reserved (24 bits) */
5846 | proto_tree_add_bits_item(section_tree, hf_oran_reserved, tvb, (offset*8), 24, ENC_BIG_ENDIAN0x00000000);
5847 | break;
5848 | case 3:
5849 | /* LBT_DRS_RSP */
5850 | /* lbtHandle (16 bits) */
5851 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5852 | offset += 2;
5853 | /* lbtDrsRes (1 bit) */
5854 | proto_tree_add_item(section_tree, hf_oran_lbtDrsRes, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5855 | /* reserved (7 bits) */
5856 | proto_tree_add_item(section_tree, hf_oran_reserved_last_7bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5857 | break;
5858 | case 4:
5859 | /* LBT_Buffer_Error */
5860 | /* lbtHandle (16 bits) */
5861 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5862 | offset += 2;
5863 | /* lbtBufErr (1 bit) */
5864 | proto_tree_add_item(section_tree, hf_oran_lbtBufErr, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5865 | /* reserved (7 bits) */
5866 | proto_tree_add_item(section_tree, hf_oran_reserved_last_7bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5867 | break;
5868 | case 5:
5869 | /* LBT_CWCONFIG_REQ */
5870 | /* lbtHandle (16 bits) */
5871 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5872 | offset += 2;
5873 | /* lbtCWConfig_H (8 bits) */
5874 | proto_tree_add_item(section_tree, hf_oran_lbtCWConfig_H, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5875 | offset += 1;
5876 | /* lbtCWConfig_T (8 bits) */
5877 | proto_tree_add_item(section_tree, hf_oran_lbtCWConfig_T, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5878 | offset += 1;
5879 | /* lbtMode (2 bits) */
5880 | proto_tree_add_bits_item(section_tree, hf_oran_lbtMode, tvb, offset*8, 2, ENC_BIG_ENDIAN0x00000000);
5881 | /* lbtTrafficClass (3 bits) */
5882 | proto_tree_add_item(section_tree, hf_oran_lbtTrafficClass, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5883 | /* reserved (19 bits) */
5884 | proto_tree_add_bits_item(section_tree, hf_oran_reserved, tvb, (offset*8)+5, 19, ENC_BIG_ENDIAN0x00000000);
5885 | break;
5886 | case 6:
5887 | /* LBT_CWCONFIG_RSP */
5888 | /* lbtHandle (16 bits) */
5889 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5890 | offset += 2;
5891 | /* lbtCWR_Rst (1 bit) */
5892 | proto_tree_add_item(section_tree, hf_oran_lbtCWR_Rst, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5893 | /* reserved (7 bits) */
5894 | proto_tree_add_item(section_tree, hf_oran_reserved_last_7bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5895 | break;
5896 |
5897 | default:
5898 | /* Unhandled! */
5899 | expert_add_info_format(pinfo, laa_msg_type_ti, &ei_oran_laa_msg_type_unsupported,
5900 | "laaMsgType %u not supported by dissector",
5901 | laa_msg_type);
5902 |
5903 | break;
5904 | }
5905 | /* For now just skip indicated length of bytes */
5906 | offset = payload_offset + 4*(laa_msg_len+1);
5907 | }
5908 |
5909 |
5910 | /* Dissect each C section */
5911 | for (uint32_t i = 0; i < nSections; ++i) {
5912 | tvbuff_t *section_tvb = tvb_new_subset_length_caplen(tvb, offset, -1, -1);
5913 | offset += dissect_oran_c_section(section_tvb, oran_tree, pinfo, state, sectionType, tap_info,
5914 | protocol_item,
5915 | subframeId, slotId,
5916 | bit_width, ci_comp_method, ci_comp_opt,
5917 | num_sinr_per_prb);
5918 | }
5919 |
5920 | /* Expert error if we are short of tvb by > 3 bytes */
5921 | if (tvb_reported_length_remaining(tvb, offset) > 3) {
5922 | expert_add_info_format(pinfo, protocol_item, &ei_oran_frame_length,
5923 | "%u bytes remain at end of frame - should be 0-3",
5924 | tvb_reported_length_remaining(tvb, offset));
5925 | }
5926 |
5927 | return tvb_captured_length(tvb);
5928 | }
5929 |
5930 | static int dissect_oran_u_re(tvbuff_t *tvb, proto_tree *tree,
5931 | unsigned sample_number, int samples_offset,
5932 | oran_tap_info *tap_info,
5933 | unsigned sample_bit_width,
5934 | int comp_meth,
5935 | uint32_t exponent)
5936 | {
5937 | /* I */
5938 | unsigned i_bits = tvb_get_bits32(tvb, samples_offset, sample_bit_width, ENC_BIG_ENDIAN0x00000000);
5939 | float i_value = decompress_value(i_bits, comp_meth, sample_bit_width, exponent);
5940 | unsigned sample_len_in_bytes = ((samples_offset%8)+sample_bit_width+7)/8;
5941 | proto_item *i_ti = proto_tree_add_float(tree, hf_oran_iSample, tvb, samples_offset/8, sample_len_in_bytes, i_value);
5942 | proto_item_set_text(i_ti, "iSample: % 0.7f 0x%04x (RE-%2u in the PRB)", i_value, i_bits, sample_number);
5943 | samples_offset += sample_bit_width;
5944 | /* Q */
5945 | unsigned q_bits = tvb_get_bits32(tvb, samples_offset, sample_bit_width, ENC_BIG_ENDIAN0x00000000);
5946 | float q_value = decompress_value(q_bits, comp_meth, sample_bit_width, exponent);
5947 | sample_len_in_bytes = ((samples_offset%8)+sample_bit_width+7)/8;
5948 | proto_item *q_ti = proto_tree_add_float(tree, hf_oran_qSample, tvb, samples_offset/8, sample_len_in_bytes, q_value);
5949 | proto_item_set_text(q_ti, "qSample: % 0.7f 0x%04x (RE-%2u in the PRB)", q_value, q_bits, sample_number);
5950 | samples_offset += sample_bit_width;
5951 |
5952 | /* Update RE stats */
5953 | tap_info->num_res++;
5954 | /* if (i_value == 0.0 && q_value == 0.0) { */
5955 | /* TODO: is just checking bits from frame good enough - assuming this always corresponds to a zero value? */
5956 | if (i_bits == 0 && q_bits == 0) {
5957 | tap_info->num_res_zero++;
5958 | }
5959 | else {
5960 | tap_info->non_zero_re_in_current_prb = true1;
5961 | }
5962 | return samples_offset;
5963 | }
5964 |
5965 |
5966 | static bool_Bool udcomplen_appears_present(bool_Bool udcomphdr_present, tvbuff_t *tvb, int offset)
5967 | {
5968 | if (!udcomplen_heuristic_result_set) {
5969 | /* All sections will start the same way */
5970 | unsigned int section_bytes_before_field = (udcomphdr_present) ? 6 : 4;
5971 |
5972 | /* Move offset back to the start of the section */
5973 | offset -= section_bytes_before_field;
5974 |
5975 | do {
5976 | /* This field appears several bytes into the U-plane section */
5977 | uint32_t length_remaining = tvb_reported_length_remaining(tvb, offset);
5978 | /* Are there enough bytes to still read the length field? */
5979 | if (section_bytes_before_field+2 > length_remaining) {
5980 | udcomplen_heuristic_result = false0;
5981 | udcomplen_heuristic_result_set = true1;
5982 | break;
5983 | }
5984 |
5985 | /* Read the length field */
5986 | uint16_t udcomplen = tvb_get_ntohs(tvb, offset+section_bytes_before_field);
5987 |
5988 | /* Is this less than a valid section? Realistic minimal section will be bigger than this..
5989 | * Could take into account numPrbU, etc */
5990 | if (udcomplen < section_bytes_before_field+2) {
5991 | udcomplen_heuristic_result = false0;
5992 | udcomplen_heuristic_result_set = true1;
5993 | break;
5994 | }
5995 |
5996 | /* Does this section fit into the frame? */
5997 | if (udcomplen > length_remaining) {
5998 | udcomplen_heuristic_result = false0;
5999 | udcomplen_heuristic_result_set = true1;
6000 | break;
6001 | }
6002 |
6003 | /* Move past this section */
6004 | offset += udcomplen;
6005 |
6006 | /* Are we at the end of the frame? */
6007 | /* TODO: if frame is less than 60 bytes, there may be > 4 bytes, likely zeros.. */
6008 | if (tvb_reported_length_remaining(tvb, offset) < 4) {
6009 | udcomplen_heuristic_result = true1;
6010 | udcomplen_heuristic_result_set = true1;
6011 | }
6012 | } while (!udcomplen_heuristic_result_set);
6013 | }
6014 | return udcomplen_heuristic_result;
6015 | }
6016 |
6017 | static bool_Bool at_udcomphdr(tvbuff_t *tvb, int offset)
6018 | {
6019 | if (tvb_captured_length_remaining(tvb, offset) < 2) {
6020 | return false0;
6021 | }
6022 | uint8_t first_byte = tvb_get_uint8(tvb, offset);
6023 | uint8_t reserved_byte = tvb_get_uint8(tvb, offset+1);
6024 |
6025 | /* - iq width could be anything, though unlikely to be signalled as (say) < 1-3? */
6026 | /* - meth should be 0-8 */
6027 | /* - reserved byte should be 0 */
6028 | return (((first_byte & 0x0f) <= MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8) && (reserved_byte == 0));
6029 | }
6030 |
6031 | static bool_Bool udcomphdr_appears_present(flow_state_t *flow, uint32_t direction, tvbuff_t *tvb, int offset)
6032 | {
6033 | /* Should really not happen, but guard against this anyway. */
6034 | if (flow == NULL((void*)0)) {
6035 | /* No state to update. */
6036 | return false0;
6037 | }
6038 |
6039 | if (direction == DIR_UPLINK0) {
6040 | if (flow->udcomphdrUplink_heuristic_result_set) {
6041 | /* Return cached value */
6042 | return flow->udcomphdrUplink_heuristic_result;
6043 | }
6044 | else {
6045 | /* Work it out, and save answer for next time */
6046 | flow->udcomphdrUplink_heuristic_result_set = true1;
6047 | flow->udcomphdrUplink_heuristic_result = at_udcomphdr(tvb, offset);
6048 | return flow->udcomphdrUplink_heuristic_result;
6049 | }
6050 | }
6051 | else {
6052 | /* Downlink */
6053 | if (flow->udcomphdrDownlink_heuristic_result_set) {
6054 | /* Return cached value */
6055 | return flow->udcomphdrDownlink_heuristic_result;
6056 | }
6057 | else {
6058 | /* Work it out, and save answer for next time */
6059 | flow->udcomphdrDownlink_heuristic_result_set = true1;
6060 | flow->udcomphdrDownlink_heuristic_result = at_udcomphdr(tvb, offset);
6061 | return flow->udcomphdrDownlink_heuristic_result;
6062 | }
6063 | }
6064 | }
6065 |
6066 | /* User plane dissector (section 8) */
6067 | static int
6068 | dissect_oran_u(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree,
6069 | oran_tap_info *tap_info, void *data _U___attribute__((unused)))
6070 | {
6071 | /* Hidden filter for plane */
6072 | proto_item *plane_ti = proto_tree_add_item(tree, hf_oran_uplane, tvb, 0, 0, ENC_NA0x00000000);
6073 | PROTO_ITEM_SET_HIDDEN(plane_ti)proto_item_set_hidden((plane_ti));
6074 |
6075 | /* Set up structures needed to add the protocol subtree and manage it */
6076 | int offset = 0;
6077 |
6078 | col_set_str(pinfo->cinfo, COL_PROTOCOL, "O-RAN-FH-U");
6079 | col_set_str(pinfo->cinfo, COL_INFO, "U-Plane");
6080 |
6081 | tap_info->userplane = true1;
6082 |
6083 | /* Create display subtree for the protocol */
6084 | proto_item *protocol_item = proto_tree_add_item(tree, proto_oran, tvb, 0, -1, ENC_NA0x00000000);
6085 | proto_item_append_text(protocol_item, "-U");
6086 | proto_tree *oran_tree = proto_item_add_subtree(protocol_item, ett_oran);
6087 |
6088 | /* Transport header */
6089 | /* Real-time control data / IQ data transfer message series identifier */
6090 | uint16_t eAxC;
6091 | addPcOrRtcid(tvb, oran_tree, &offset, hf_oran_ecpri_pcid, &eAxC);
6092 | tap_info->eaxc = eAxC;
6093 |
6094 | /* Update/report status of conversation */
6095 | uint32_t key = make_flow_key(pinfo, eAxC, ORAN_U_PLANE1, false0);
6096 | flow_state_t* state = (flow_state_t*)wmem_tree_lookup32(flow_states_table, key);
6097 |
6098 | /* Message identifier */
6099 | uint8_t seq_id;
6100 | proto_item *seq_id_ti;
6101 | offset = addSeqid(tvb, oran_tree, offset, ORAN_U_PLANE1, &seq_id, &seq_id_ti, pinfo);
6102 |
6103 | /* Common header for time reference */
6104 | proto_item *timingHeader = proto_tree_add_string_format(oran_tree, hf_oran_timing_header,
6105 | tvb, offset, 4, "", "Timing Header (");
6106 | proto_tree *timing_header_tree = proto_item_add_subtree(timingHeader, ett_oran_u_timing);
6107 |
6108 | /* dataDirection */
6109 | uint32_t direction;
6110 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_data_direction, tvb, offset, 1, ENC_NA0x00000000, &direction);
6111 | tap_info->uplink = (direction==0);
6112 | /* payloadVersion */
6113 | dissect_payload_version(timing_header_tree, tvb, pinfo, offset);
6114 | /* filterIndex */
6115 | proto_tree_add_item(timing_header_tree, hf_oran_filter_index, tvb, offset, 1, ENC_NA0x00000000);
6116 | offset += 1;
6117 |
6118 | int ref_a_offset = offset;
6119 |
6120 | /* frameId */
6121 | uint32_t frameId = 0;
6122 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_frame_id, tvb, offset, 1, ENC_NA0x00000000, &frameId);
6123 | tap_info->frame = frameId;
6124 | offset += 1;
6125 |
6126 | /* subframeId */
6127 | uint32_t subframeId = 0;
6128 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_subframe_id, tvb, offset, 1, ENC_NA0x00000000, &subframeId);
6129 | /* slotId */
6130 | uint32_t slotId = 0;
6131 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_slot_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &slotId);
6132 | tap_info->slot = slotId;
6133 | offset++;
6134 | /* symbolId */
6135 | uint32_t symbolId = 0;
6136 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_symbolId, tvb, offset, 1, ENC_NA0x00000000, &symbolId);
6137 | offset++;
6138 |
6139 | char id[16];
6140 | snprintf(id, 16, "%d-%d-%d-%d", frameId, subframeId, slotId, symbolId);
6141 | proto_item *pi = proto_tree_add_string(timing_header_tree, hf_oran_refa, tvb, ref_a_offset, 3, id);
6142 | proto_item_set_generated(pi);
6143 |
6144 | proto_item_append_text(timingHeader, "%s, frameId: %d, subframeId: %d, slotId: %d, symbolId: %d)",
6145 | val_to_str_const(direction, data_direction_vals, "Unknown"), frameId, subframeId, slotId, symbolId);
6146 |
6147 | unsigned sample_bit_width;
6148 | int compression;
6149 | int includeUdCompHeader;
6150 |
6151 | /* Also look up C-PLANE state (sent in opposite direction) so may check current compression settings */
6152 | uint32_t cplane_key = make_flow_key(pinfo, eAxC, ORAN_C_PLANE0, true1);
6153 | flow_state_t* cplane_state = (flow_state_t*)wmem_tree_lookup32(flow_states_table, cplane_key);
6154 |
6155 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
6156 | /* Create conversation if doesn't exist yet */
6157 | if (!state) {
6158 | /* Allocate new state */
6159 | state = wmem_new0(wmem_file_scope(), flow_state_t)((flow_state_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_state_t )));
6160 | state->ack_nack_requests = wmem_tree_new(wmem_epan_scope());
6161 | wmem_tree_insert32(flow_states_table, key, state);
6162 | }
6163 |
6164 | /* Check sequence analysis status */
6165 | if (state->last_frame_seen[direction] && (seq_id != state->next_expected_sequence_number[direction])) {
6166 | /* Store this result */
6167 | flow_result_t *result = wmem_new0(wmem_file_scope(), flow_result_t)((flow_result_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_result_t )));
6168 | result->unexpected_seq_number = true1;
6169 | result->expected_sequence_number = state->next_expected_sequence_number[direction];
6170 | result->previous_frame = state->last_frame[direction];
6171 | wmem_tree_insert32(flow_results_table, pinfo->num, result);
6172 | }
6173 | /* Update sequence analysis state */
6174 | state->last_frame[direction] = pinfo->num;
6175 | state->last_frame_seen[direction] = true1;
6176 | state->next_expected_sequence_number[direction] = (seq_id+1) % 256;
6177 | }
6178 |
6179 | /* Show any issues associated with this frame number */
6180 | flow_result_t *result = wmem_tree_lookup32(flow_results_table, pinfo->num);
6181 | if (result) {
6182 | if (result->unexpected_seq_number) {
6183 | expert_add_info_format(pinfo, seq_id_ti,
6184 | (direction == DIR_UPLINK0) ?
6185 | &ei_oran_uplane_unexpected_sequence_number_ul :
6186 | &ei_oran_uplane_unexpected_sequence_number_dl,
6187 | "Sequence number %u expected, but got %u",
6188 | result->expected_sequence_number, seq_id);
6189 | tap_info->missing_sns = (256 + seq_id - result->expected_sequence_number) % 256;
6190 | /* TODO: could add previous/next frame (in seqId tree?) ? */
6191 | }
6192 | }
6193 |
6194 | /* Checking UL timing within current slot. Disabled if limit set to 0. */
6195 | /* N.B., timing is relative to first seen frame,
6196 | not some notion of the beginning of the slot from sync, offset by some timing.. */
6197 | if (direction == DIR_UPLINK0 && us_allowed_for_ul_in_symbol > 0) {
6198 | uint32_t timing_key = get_timing_key(frameId, subframeId, slotId, symbolId);
6199 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
6200 | /* Set state on first pass */
6201 | ul_timing_for_slot* timing = (ul_timing_for_slot*)wmem_tree_lookup32(ul_symbol_timing, timing_key);
6202 | if (!timing) {
6203 | /* Allocate new state */
6204 | timing = wmem_new0(wmem_file_scope(), ul_timing_for_slot)((ul_timing_for_slot*)wmem_alloc0((wmem_file_scope()), sizeof (ul_timing_for_slot)));
6205 | timing->first_frame = pinfo->num;
6206 | timing->first_frame_time = pinfo->abs_ts;
6207 | timing->frames_seen_in_symbol = 1;
6208 | timing->last_frame_in_symbol = pinfo->num;
6209 | wmem_tree_insert32(ul_symbol_timing, timing_key, timing);
6210 | }
6211 | else {
6212 | /* Update existing state */
6213 | timing->frames_seen_in_symbol++;
6214 | timing->last_frame_in_symbol = pinfo->num;
6215 | }
6216 | }
6217 | else {
6218 | /* Subsequent passes - look up result */
6219 | ul_timing_for_slot* timing = (ul_timing_for_slot*)wmem_tree_lookup32(ul_symbol_timing, timing_key);
6220 | if (timing) { /* Really shouldn't fail! */
6221 | if (timing->frames_seen_in_symbol > 1) {
6222 | /* Work out gap between frames (in microseconds) back to frame carrying first seen symbol */
6223 | int seconds_between_packets = (int)
6224 | (pinfo->abs_ts.secs - timing->first_frame_time.secs);
6225 | int nseconds_between_packets =
6226 | pinfo->abs_ts.nsecs - timing->first_frame_time.nsecs;
6227 |
6228 |
6229 | /* Round to nearest microsecond. */
6230 | uint32_t total_gap = (seconds_between_packets*1000000) +
6231 | ((nseconds_between_packets+500) / 1000);
6232 |
6233 | /* Show how long it has been */
6234 | proto_item *ti = NULL((void*)0);
6235 | if (pinfo->num != timing->first_frame) {
6236 | ti = proto_tree_add_uint(timingHeader, hf_oran_u_section_ul_symbol_time, tvb, 0, 0, total_gap);
6237 | proto_item_set_generated(ti);
6238 | }
6239 |
6240 | if (total_gap > us_allowed_for_ul_in_symbol) {
6241 | expert_add_info_format(pinfo, ti, &ei_oran_ul_uplane_symbol_too_long,
6242 | "UL U-Plane Tx took longer (%u us) than limit set in preferences (%u us)",
6243 | total_gap, us_allowed_for_ul_in_symbol);
6244 | }
6245 |
6246 | /* Show how many frames were received */
6247 | ti = proto_tree_add_uint(timingHeader, hf_oran_u_section_ul_symbol_frames, tvb, 0, 0, timing->frames_seen_in_symbol);
6248 | proto_item_set_generated(ti);
6249 |
6250 | /* Link to first frame for this symbol */
6251 | if (pinfo->num != timing->first_frame) {
6252 | ti = proto_tree_add_uint(timingHeader, hf_oran_u_section_ul_symbol_first_frame, tvb, 0, 0, timing->first_frame);
6253 | proto_item_set_generated(ti);
6254 | }
6255 |
6256 | /* And also last frame */
6257 | if (pinfo->num != timing->last_frame_in_symbol) {
6258 | ti = proto_tree_add_uint(timingHeader, hf_oran_u_section_ul_symbol_last_frame, tvb, 0, 0, timing->last_frame_in_symbol);
6259 | proto_item_set_generated(ti);
6260 | }
6261 |
6262 | tap_info->ul_delay_in_us = total_gap;
6263 | }
6264 | }
6265 | }
6266 | }
6267 |
6268 |
6269 | /* Look up preferences for samples */
6270 | if (direction == DIR_UPLINK0) {
6271 | sample_bit_width = pref_sample_bit_width_uplink;
6272 | compression = pref_iqCompressionUplink;
6273 | includeUdCompHeader = pref_includeUdCompHeaderUplink;
6274 | } else {
6275 | sample_bit_width = pref_sample_bit_width_downlink;
6276 | compression = pref_iqCompressionDownlink;
6277 | includeUdCompHeader = pref_includeUdCompHeaderDownlink;
6278 | }
6279 |
6280 | /* If uplink, load any udCompHdr settings written by C-Plane */
6281 | bool_Bool ud_cmp_hdr_cplane = false0;
6282 | if (cplane_state && direction == 0) {
6283 | /* Initialise settings from udpCompHdr from C-Plane */
6284 | if (cplane_state->ul_ud_comp_hdr_set) {
6285 | sample_bit_width = cplane_state->ul_ud_comp_hdr_bit_width;
6286 | compression = cplane_state->ul_ud_comp_hdr_compression;
6287 | ud_cmp_hdr_cplane = true1;
6288 | }
6289 | }
6290 |
6291 | /* Need a valid value (e.g. 9, 14). 0 definitely won't work, as won't progress around loop! */
6292 | /* N.B. may yet be overwritten by udCompHdr settings in sections below! */
6293 | if (sample_bit_width == 0) {
6294 | expert_add_info_format(pinfo, protocol_item, &ei_oran_invalid_sample_bit_width,
6295 | "%cL Sample bit width from %s (%u) not valid, so can't decode sections",
6296 | (direction == DIR_UPLINK0) ? 'U' : 'D',
6297 | !ud_cmp_hdr_cplane ? "preference" : "C-Plane",
6298 | sample_bit_width);
6299 | return offset;
6300 | }
6301 |
6302 | unsigned bytesLeft;
6303 | unsigned number_of_sections = 0;
6304 | unsigned nBytesPerPrb =0;
6305 |
6306 | /* Add each section (not from count, just keep parsing until payload used) */
6307 | do {
6308 | /* Section subtree */
6309 | unsigned section_start_offset = offset;
6310 | proto_item *sectionHeading = proto_tree_add_string_format(oran_tree, hf_oran_u_section,
6311 | tvb, offset, 0, "", "Section");
6312 | proto_tree *section_tree = proto_item_add_subtree(sectionHeading, ett_oran_u_section);
6313 |
6314 | /* Section Header fields (darker green part) */
6315 |
6316 | /* sectionId */
6317 | uint32_t sectionId = 0;
6318 | proto_item *ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_section_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &sectionId);
6319 | if (sectionId == 4095) {
6320 | proto_item_append_text(ti, " (not default coupling C/U planes using sectionId)");
6321 | }
6322 | offset++;
6323 |
6324 | if (tap_info->num_section_ids < MAX_SECTION_IDs32) {
6325 | tap_info->section_ids[tap_info->num_section_ids++] = sectionId;
6326 | }
6327 |
6328 | /* rb */
6329 | uint32_t rb;
6330 | proto_tree_add_item_ret_uint(section_tree, hf_oran_rb, tvb, offset, 1, ENC_NA0x00000000, &rb);
6331 | /* symInc */
6332 | proto_tree_add_item(section_tree, hf_oran_symInc, tvb, offset, 1, ENC_NA0x00000000);
6333 | /* startPrbu */
6334 | uint32_t startPrbu = 0;
6335 | proto_tree_add_item_ret_uint(section_tree, hf_oran_startPrbu, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPrbu);
6336 | offset += 2;
6337 |
6338 | /* numPrbu */
6339 | uint32_t numPrbu = 0;
6340 | proto_tree_add_item_ret_uint(section_tree, hf_oran_numPrbu, tvb, offset, 1, ENC_NA0x00000000, &numPrbu);
6341 | offset += 1;
6342 |
6343 | proto_item *ud_comp_meth_item, *ud_comp_len_ti=NULL((void*)0);
6344 | uint32_t ud_comp_len;
6345 |
6346 | /* udCompHdr (if preferences indicate will be present) */
6347 | bool_Bool included = (includeUdCompHeader==1) || /* 1 means present.. */
6348 | (includeUdCompHeader==2 && udcomphdr_appears_present(state, direction, tvb, offset));
6349 | if (included) {
6350 | /* 7.5.2.10 */
6351 | /* Extract these values to inform how wide IQ samples in each PRB will be. */
6352 | offset = dissect_udcomphdr(tvb, pinfo, section_tree, offset, false0, &sample_bit_width,
6353 | &compression, &ud_comp_meth_item);
6354 |
6355 | /* Not part of udCompHdr */
6356 | proto_tree_add_item(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000);
6357 | offset += 1;
6358 | }
6359 | else {
6360 | /* No fields to dissect - just showing comp values from prefs */
6361 | /* iqWidth */
6362 | proto_item *iq_width_item = proto_tree_add_uint(section_tree, hf_oran_udCompHdrIqWidth_pref, tvb, 0, 0, sample_bit_width);
6363 | proto_item_append_text(iq_width_item, (ud_cmp_hdr_cplane) ? " (from c-plane)" : " (from preferences)");
6364 | proto_item_set_generated(iq_width_item);
6365 |
6366 | /* udCompMethod */
6367 | ud_comp_meth_item = proto_tree_add_uint(section_tree, hf_oran_udCompHdrMeth_pref, tvb, 0, 0, compression);
6368 | proto_item_append_text(ud_comp_meth_item, (ud_cmp_hdr_cplane) ? " (from c-plane)" : " (from preferences)");
6369 | proto_item_set_generated(ud_comp_meth_item);
6370 |
6371 | /* Point back to C-Plane, if used */
6372 | /* TODO: doesn't work with multiple port mappings using SE10.. */
6373 | if (ud_cmp_hdr_cplane) {
6374 | proto_item *cplane_ti = proto_tree_add_uint(section_tree, hf_oran_ul_cplane_ud_comp_hdr_frame, tvb, offset, 0, cplane_state->ul_ud_comp_hdr_frame);
6375 | proto_item_set_generated(cplane_ti);
6376 | }
6377 | }
6378 |
6379 | /* Not supported! TODO: other places where comp method is looked up (e.g., bfw?) */
6380 | switch (compression) {
6381 | case COMP_NONE0:
6382 | case COMP_BLOCK_FP1:
6383 | case BFP_AND_SELECTIVE_RE5:
6384 | break;
6385 | default:
6386 | expert_add_info_format(pinfo, ud_comp_meth_item, &ei_oran_unsupported_compression_method,
6387 | "Compression method %u (%s) not supported by dissector",
6388 | compression,
6389 | rval_to_str_const(compression, ud_comp_header_meth, "reserved"));
6390 | }
6391 |
6392 | /* udCompLen (when supported, methods 5,6,7,8) */
6393 | if (compression >= BFP_AND_SELECTIVE_RE5) {
6394 | bool_Bool supported = (pref_support_udcompLen==1) || /* supported */
6395 | (pref_support_udcompLen==2 && udcomplen_appears_present(includeUdCompHeader, tvb, offset));
6396 |
6397 | if (supported) {
6398 | ud_comp_len_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_udCompLen, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ud_comp_len);
6399 | if (ud_comp_len <= 1) {
6400 | proto_item_append_text(ud_comp_len_ti, " (reserved)");
6401 | }
6402 | /* TODO: report if less than a viable section in frame? */
6403 | /* Check that there is this much length left in the frame */
6404 | if ((int)ud_comp_len > tvb_reported_length_remaining(tvb, section_start_offset)) {
6405 | expert_add_info_format(pinfo, ud_comp_len_ti, &ei_oran_ud_comp_len_wrong_size,
6406 | "udCompLen indicates %u bytes in section, but only %u are left in frame",
6407 | ud_comp_len, tvb_reported_length_remaining(tvb, section_start_offset));
6408 | }
6409 | /* Actual length of section will be checked below, at the end of the section */
6410 | offset += 2;
6411 | }
6412 | }
6413 |
6414 | /* sReSMask1 + sReSMask2 (depends upon compression method) */
6415 | uint64_t sresmask1=0, sresmask2=0;
6416 | if (compression == BFP_AND_SELECTIVE_RE_WITH_MASKS7 ||
6417 | compression == MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8)
6418 | {
6419 | static int * const sres_mask1_2_flags[] = {
6420 | &hf_oran_sReSMask1_2_re12,
6421 | &hf_oran_sReSMask1_2_re11,
6422 | &hf_oran_sReSMask1_2_re10,
6423 | &hf_oran_sReSMask1_2_re9,
6424 | &hf_oran_sReSMask_re8,
6425 | &hf_oran_sReSMask_re7,
6426 | &hf_oran_sReSMask_re6,
6427 | &hf_oran_sReSMask_re5,
6428 | &hf_oran_sReSMask_re4,
6429 | &hf_oran_sReSMask_re3,
6430 | &hf_oran_sReSMask_re2,
6431 | &hf_oran_sReSMask_re1,
6432 | NULL((void*)0)
6433 | };
6434 |
6435 | /* reserved (4 bits) */
6436 | proto_tree_add_item(section_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_NA0x00000000);
6437 | /* sReSMask1 (12 bits) */
6438 | proto_item *sresmask_ti;
6439 | sresmask_ti = proto_tree_add_bitmask_ret_uint64(section_tree, tvb, offset,
6440 | hf_oran_sReSMask1,
6441 | ett_oran_sresmask,
6442 | sres_mask1_2_flags,
6443 | ENC_NA0x00000000,
6444 | &sresmask1);
6445 | offset += 2;
6446 | /* Count REs present */
6447 | unsigned res = 0;
6448 | for (unsigned n=0; n < 12; n++) {
6449 | if ((sresmask1 >> n) & 0x1) {
6450 | res++;
6451 | }
6452 | }
6453 | proto_item_append_text(sresmask_ti, " (%u REs)", res);
6454 |
6455 |
6456 | /* reserved (4 bits) */
6457 | proto_tree_add_item(section_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_NA0x00000000);
6458 | /* sReSMask2 (12 bits) */
6459 | sresmask_ti = proto_tree_add_bitmask_ret_uint64(section_tree, tvb, offset,
6460 | hf_oran_sReSMask2,
6461 | ett_oran_sresmask,
6462 | sres_mask1_2_flags,
6463 | ENC_NA0x00000000,
6464 | &sresmask2);
6465 | offset += 2;
6466 |
6467 | if (rb == 1) {
6468 | proto_item_append_text(sresmask_ti, " (ignored)");
6469 | if (sresmask2 != 0) {
6470 | expert_add_info(pinfo, ud_comp_len_ti, &ei_oran_sresmask2_not_zero_with_rb);
6471 | }
6472 | }
6473 | else {
6474 | /* Count REs present */
6475 | res = 0;
6476 | for (unsigned n=0; n < 12; n++) {
6477 | if ((sresmask2 >> n) & 0x1) {
6478 | res++;
6479 | }
6480 | }
6481 | proto_item_append_text(sresmask_ti, " (%u REs)", res);
6482 | }
6483 | }
6484 |
6485 | write_section_info(sectionHeading, pinfo, protocol_item, sectionId, startPrbu, numPrbu, rb);
6486 |
6487 | /* TODO: should this use the same pref as c-plane? */
6488 | if (numPrbu == 0) {
6489 | /* Special case for all PRBs (NR: the total number of PRBs may be > 255) */
6490 | numPrbu = pref_data_plane_section_total_rbs;
6491 | startPrbu = 0; /* may already be 0... */
6492 | }
6493 |
6494 | /* Add each PRB */
6495 | for (unsigned i = 0; i < numPrbu; i++) {
6496 | /* Create subtree */
6497 | proto_item *prbHeading = proto_tree_add_string_format(section_tree, hf_oran_samples_prb,
6498 | tvb, offset, 0,
6499 | "", "PRB");
6500 | proto_tree *rb_tree = proto_item_add_subtree(prbHeading, ett_oran_u_prb);
6501 | uint32_t exponent = 0;
6502 | uint16_t sresmask = 0;
6503 |
6504 | /* udCompParam (depends upon compression method) */
6505 | int before = offset;
6506 | offset = dissect_udcompparam(tvb, pinfo, rb_tree, offset, compression, &exponent, &sresmask, false0);
6507 | int udcompparam_len = offset-before;
6508 |
6509 | /* Show PRB number in root */
6510 | proto_item_append_text(prbHeading, " %3u", startPrbu + i*(1+rb));
6511 |
6512 | /* Work out how many REs / PRB */
6513 | unsigned res_per_prb = 12;
6514 | uint16_t sresmask_to_use = 0x0fff;
6515 |
6516 | if (compression >= BFP_AND_SELECTIVE_RE5) {
6517 | /* Work out which mask should be used */
6518 | if (compression==BFP_AND_SELECTIVE_RE5 || compression==MOD_COMPR_AND_SELECTIVE_RE6) {
6519 | /* Selective RE cases, use value from compModParam */
6520 | sresmask_to_use = (uint16_t)sresmask;
6521 | }
6522 | else {
6523 | /* With masks (in section). Choose between sresmask1 and sresmask2 */
6524 | if (rb==1 || (i%1)==0) {
6525 | /* Even values */
6526 | sresmask_to_use = (uint16_t)sresmask1;
6527 | }
6528 | else {
6529 | /* Odd values */
6530 | sresmask_to_use = (uint16_t)sresmask2;
6531 | }
6532 | }
6533 |
6534 | /* Count REs present using sresmask */
6535 | res_per_prb = 0;
6536 | /* Use sresmask to pick out which REs are present */
6537 | for (unsigned n=0; n<12; n++) {
6538 | if (sresmask_to_use & (1<<n)) {
6539 | res_per_prb++;
6540 | }
6541 | }
6542 | }
6543 |
6544 | /* N.B. bytes for samples need to be padded out to next byte
6545 | (certainly where there aren't 12 REs in PRB..) */
6546 | unsigned nBytesForSamples = (sample_bit_width * res_per_prb * 2 + 7) / 8;
6547 | nBytesPerPrb = nBytesForSamples + udcompparam_len;
6548 |
6549 | proto_tree_add_item(rb_tree, hf_oran_iq_user_data, tvb, offset, nBytesForSamples, ENC_NA0x00000000);
6550 |
6551 | tap_info->non_zero_re_in_current_prb = false0;
6552 |
6553 | /* Optionally trying to show I/Q RE values */
6554 | if (pref_showIQSampleValues) {
6555 | /* Individual values */
6556 | unsigned samples_offset = offset*8;
6557 | unsigned samples = 0;
6558 |
6559 | if (compression >= BFP_AND_SELECTIVE_RE5) {
6560 | /* Use sresmask to pick out which REs are present */
6561 | for (unsigned n=1; n<=12; n++) {
6562 | if (sresmask_to_use & (1<<(n-1))) {
6563 | samples_offset = dissect_oran_u_re(tvb, rb_tree,
6564 | n, samples_offset, tap_info, sample_bit_width, compression, exponent);
6565 | samples++;
6566 | }
6567 | }
6568 | }
6569 | else {
6570 | /* All 12 REs are present */
6571 | for (unsigned n=1; n<=12; n++) {
6572 | samples_offset = dissect_oran_u_re(tvb, rb_tree,
6573 | n, samples_offset, tap_info, sample_bit_width, compression, exponent);
6574 | samples++;
6575 | }
6576 | }
6577 | proto_item_append_text(prbHeading, " (%u REs)", samples);
6578 |
6579 | /* Was this PRB all zeros? */
6580 | if (!tap_info->non_zero_re_in_current_prb) {
6581 | tap_info->num_prbs_zero++;
6582 | /* Add a filter to make zero-valued PRBs more findable */
6583 | proto_tree_add_item(rb_tree, hf_oran_zero_prb, tvb,
6584 | samples_offset/8, nBytesForSamples, ENC_NA0x00000000);
6585 | proto_item_append_text(prbHeading, " (all zeros)");
6586 | }
6587 | }
6588 |
6589 | tap_info->num_prbs++;
6590 |
6591 |
6592 | /* Advance past samples */
6593 | offset += nBytesForSamples;
6594 |
6595 | /* Set end of prb subtree */
6596 | proto_item_set_end(prbHeading, tvb, offset);
6597 | }
6598 |
6599 | /* Set extent of section */
6600 | proto_item_set_len(sectionHeading, offset-section_start_offset);
6601 | if (ud_comp_len_ti != NULL((void*)0) && ((offset-section_start_offset != ud_comp_len))) {
6602 | expert_add_info_format(pinfo, ud_comp_len_ti, &ei_oran_ud_comp_len_wrong_size,
6603 | "udCompLen indicates %u bytes in section, but dissected %u instead",
6604 | ud_comp_len, offset-section_start_offset);
6605 | }
6606 |
6607 | bytesLeft = tvb_captured_length(tvb) - offset;
6608 | number_of_sections++;
6609 | } while (bytesLeft >= (4 + nBytesPerPrb)); /* FIXME: bad heuristic */
6610 |
6611 | /* Show number of sections found */
6612 | proto_item *ti = proto_tree_add_uint(oran_tree, hf_oran_numberOfSections, tvb, 0, 0, number_of_sections);
6613 | proto_item_set_generated(ti);
6614 |
6615 | /* Expert error if we are short of tvb by > 3 bytes */
6616 | if (tvb_reported_length_remaining(tvb, offset) > 3) {
6617 | expert_add_info_format(pinfo, protocol_item, &ei_oran_frame_length,
6618 | "%u bytes remain at end of frame - should be 0-3",
6619 | tvb_reported_length_remaining(tvb, offset));
6620 | }
6621 |
6622 | return tvb_captured_length(tvb);
6623 | }
6624 |
6625 |
6626 | /**********************************************************************/
6627 | /* Main dissection function. */
6628 | /* N.B. ecpri message type passed in as 'data' arg by eCPRI dissector */
6629 | static int
6630 | dissect_oran(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, void *data)
6631 | {
6632 | uint32_t ecpri_message_type = *(uint32_t *)data;
6633 | int offset = 0;
6634 |
6635 | /* Allocate and zero tap struct */
6636 | oran_tap_info *tap_info = wmem_new0(wmem_file_scope(), oran_tap_info)((oran_tap_info*)wmem_alloc0((wmem_file_scope()), sizeof(oran_tap_info )));
6637 | tap_info->pdu_size = pinfo->fd->pkt_len;
6638 |
6639 | switch (ecpri_message_type) {
6640 | case ECPRI_MT_IQ_DATA0:
6641 | offset = dissect_oran_u(tvb, pinfo, tree, tap_info, data);
6642 | break;
6643 | case ECPRI_MT_RT_CTRL_DATA2:
6644 | offset = dissect_oran_c(tvb, pinfo, tree, tap_info, data);
6645 | break;
6646 | default:
6647 | /* Not dissecting other types - assume these are handled by eCPRI dissector */
6648 | return 0;
6649 | }
6650 |
6651 | tap_queue_packet(oran_tap, pinfo, tap_info);
6652 |
6653 | return offset;
6654 | }
6655 |
6656 | static void oran_init_protocol(void)
6657 | {
6658 | udcomplen_heuristic_result_set = false0;
6659 | udcomplen_heuristic_result = false0;
6660 | }
6661 |
6662 |
6663 | /* Register the protocol with Wireshark. */
6664 | void
6665 | proto_register_oran(void)
6666 | {
6667 | static hf_register_info hf[] = {
6668 |
6669 | /* Section 5.1.3.2.7 */
6670 | { &hf_oran_du_port_id,
6671 | { "DU Port ID", "oran_fh_cus.du_port_id",
6672 | FT_UINT16, BASE_DEC,
6673 | NULL((void*)0), 0x0,
6674 | "Processing unit at O-RU - width set in dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6675 | },
6676 |
6677 | /* Section 5.1.3.2.7 */
6678 | { &hf_oran_bandsector_id,
6679 | { "BandSector ID", "oran_fh_cus.bandsector_id",
6680 | FT_UINT16, BASE_DEC,
6681 | NULL((void*)0), 0x0,
6682 | "Aggregated cell identified - width set in dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6683 | },
6684 |
6685 | /* Section 5.1.3.2.7 */
6686 | { &hf_oran_cc_id,
6687 | { "CC ID", "oran_fh_cus.cc_id",
6688 | FT_UINT16, BASE_DEC,
6689 | NULL((void*)0), 0x0,
6690 | "Component Carrier - width set in dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6691 | },
6692 |
6693 | /* Section 5.1.3.2.7 */
6694 | { &hf_oran_ru_port_id,
6695 | { "RU Port ID", "oran_fh_cus.ru_port_id",
6696 | FT_UINT16, BASE_DEC,
6697 | NULL((void*)0), 0x0,
6698 | "Logical flow - width set in dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6699 | },
6700 |
6701 | /* Section 5.1.3.2.8 */
6702 | { &hf_oran_sequence_id,
6703 | { "Sequence ID", "oran_fh_cus.sequence_id",
6704 | FT_UINT8, BASE_DEC,
6705 | NULL((void*)0), 0x0,
6706 | "The Sequence ID wraps around individually per eAxC", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6707 | },
6708 |
6709 | /* Section 5.1.3.2.8 */
6710 | { &hf_oran_e_bit,
6711 | { "E Bit", "oran_fh_cus.e_bit",
6712 | FT_UINT8, BASE_DEC,
6713 | VALS(e_bit)((0 ? (const struct _value_string*)0 : ((e_bit)))), 0x80,
6714 | "Indicate the last message of a subsequence (U-Plane only)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6715 | },
6716 |
6717 | /* Section 5.1.3.2.8 */
6718 | { &hf_oran_subsequence_id,
6719 | { "Subsequence ID", "oran_fh_cus.subsequence_id",
6720 | FT_UINT8, BASE_DEC,
6721 | NULL((void*)0), 0x7f,
6722 | "The subsequence ID (for eCPRI layer fragmentation)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6723 | },
6724 |
6725 | { &hf_oran_previous_frame,
6726 | { "Previous frame in stream", "oran_fh_cus.previous-frame",
6727 | FT_FRAMENUM, BASE_NONE,
6728 | FRAMENUM_TYPE(FT_FRAMENUM_NONE)((gpointer) (glong) (FT_FRAMENUM_NONE)), 0x0,
6729 | "Previous frame in sequence", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6730 | },
6731 |
6732 | /* Section 7.5.2.1 */
6733 | { &hf_oran_data_direction,
6734 | { "Data Direction", "oran_fh_cus.data_direction",
6735 | FT_UINT8, BASE_DEC,
6736 | VALS(data_direction_vals)((0 ? (const struct _value_string*)0 : ((data_direction_vals) ))), 0x80,
6737 | "gNB data direction", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6738 | },
6739 |
6740 | /* Section 7.5.2.2 */
6741 | { &hf_oran_payload_version,
6742 | { "Payload Version", "oran_fh_cus.payloadVersion",
6743 | FT_UINT8, BASE_DEC,
6744 | NULL((void*)0), 0x70,
6745 | "Payload protocol version the following IEs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6746 | },
6747 |
6748 | /* Section 7.5.2.3 */
6749 | { &hf_oran_filter_index,
6750 | { "Filter Index", "oran_fh_cus.filterIndex",
6751 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
6752 | RVALS(filter_indices)((0 ? (const struct _range_string*)0 : ((filter_indices)))), 0x0f,
6753 | "used between IQ data and air interface, both in DL and UL", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6754 | },
6755 |
6756 | /* Section 7.5.2.4 */
6757 | { &hf_oran_frame_id,
6758 | { "Frame ID", "oran_fh_cus.frameId",
6759 | FT_UINT8, BASE_DEC,
6760 | NULL((void*)0), 0x0,
6761 | "A counter for 10 ms frames (wrapping period 2.56 seconds)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6762 | },
6763 |
6764 | /* Section 7.5.2.5 */
6765 | { &hf_oran_subframe_id,
6766 | { "Subframe ID", "oran_fh_cus.subframe_id",
6767 | FT_UINT8, BASE_DEC,
6768 | NULL((void*)0), 0xf0,
6769 | "A counter for 1 ms sub-frames within 10ms frame", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6770 | },
6771 |
6772 | /* Section 7.5.2.6 */
6773 | { &hf_oran_slot_id,
6774 | { "Slot ID", "oran_fh_cus.slotId",
6775 | FT_UINT16, BASE_DEC,
6776 | NULL((void*)0), 0x0fc0,
6777 | "Slot number within a 1ms sub-frame", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6778 | },
6779 |
6780 | /* Generated for convenience */
6781 | { &hf_oran_slot_within_frame,
6782 | { "Slot within frame", "oran_fh_cus.slot-within-frame",
6783 | FT_UINT16, BASE_DEC,
6784 | NULL((void*)0), 0x0,
6785 | "Slot within frame, to match DCT logs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6786 | },
6787 |
6788 | /* Section 7.5.2.7 */
6789 | { &hf_oran_start_symbol_id,
6790 | { "Start Symbol ID", "oran_fh_cus.startSymbolId",
6791 | FT_UINT8, BASE_DEC,
6792 | NULL((void*)0), 0x3f,
6793 | "The first symbol number within slot affected", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6794 | },
6795 |
6796 | /* Section 7.5.2.8 */
6797 | { &hf_oran_numberOfSections,
6798 | { "Number of Sections", "oran_fh_cus.numberOfSections",
6799 | FT_UINT8, BASE_DEC,
6800 | NULL((void*)0), 0x0,
6801 | "The number of section IDs included in this message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6802 | },
6803 |
6804 | /* Section 7.5.2.9 */
6805 | { &hf_oran_sectionType,
6806 | { "Section Type", "oran_fh_cus.sectionType",
6807 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
6808 | RVALS(section_types)((0 ? (const struct _range_string*)0 : ((section_types)))), 0x0,
6809 | "Determines the characteristics of U-plane data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6810 | },
6811 |
6812 | /* Section 7.5.2.10 */
6813 | { &hf_oran_udCompHdr,
6814 | { "udCompHdr", "oran_fh_cus.udCompHdr",
6815 | FT_STRING, BASE_NONE,
6816 | NULL((void*)0), 0x0,
6817 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6818 | },
6819 |
6820 | /* Section 7.5.2.11 */
6821 | { &hf_oran_numberOfUEs,
6822 | { "Number Of UEs", "oran_fh_cus.numberOfUEs",
6823 | FT_UINT8, BASE_DEC,
6824 | NULL((void*)0), 0x0,
6825 | "Indicates number of UEs for which channel info is provided", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6826 | },
6827 |
6828 | /* Section 7.5.2.12 */
6829 | { &hf_oran_timeOffset,
6830 | { "Time Offset", "oran_fh_cus.timeOffset",
6831 | FT_UINT16, BASE_DEC,
6832 | NULL((void*)0), 0x0,
6833 | "from start of the slot to start of CP in samples", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6834 | },
6835 |
6836 | /* Section 7.5.2.13 */
6837 | { &hf_oran_frameStructure_fft,
6838 | { "FFT Size", "oran_fh_cus.frameStructure.fft",
6839 | FT_UINT8, BASE_HEX | BASE_RANGE_STRING0x00000100,
6840 | RVALS(frame_structure_fft)((0 ? (const struct _range_string*)0 : ((frame_structure_fft) ))), 0xf0,
6841 | "The FFT/iFFT size being used for all IQ data processing related to this message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6842 | },
6843 |
6844 | /* Section 7.5.2.13 */
6845 | { &hf_oran_frameStructure_subcarrier_spacing,
6846 | { "Subcarrier Spacing", "oran_fh_cus.frameStructure.spacing",
6847 | FT_UINT8, BASE_HEX | BASE_RANGE_STRING0x00000100,
6848 | RVALS(subcarrier_spacings)((0 ? (const struct _range_string*)0 : ((subcarrier_spacings) ))), 0x0f,
6849 | "The sub carrier spacing as well as the number of slots per 1ms sub-frame",
6850 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6851 | },
6852 |
6853 | /* Section 7.5.2.14 */
6854 | { &hf_oran_cpLength,
6855 | { "cpLength", "oran_fh_cus.cpLength",
6856 | FT_UINT16, BASE_DEC,
6857 | NULL((void*)0), 0x0,
6858 | "cyclic prefix length", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6859 | },
6860 |
6861 | { &hf_oran_timing_header,
6862 | { "Timing Header", "oran_fh_cus.timingHeader",
6863 | FT_STRING, BASE_NONE,
6864 | NULL((void*)0), 0x0,
6865 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6866 | },
6867 |
6868 | /* Section 7.5.3.1 */
6869 | { &hf_oran_section_id,
6870 | { "sectionId", "oran_fh_cus.sectionId",
6871 | FT_UINT16, BASE_DEC,
6872 | NULL((void*)0), 0xfff0,
6873 | "section identifier of data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6874 | },
6875 |
6876 | /* Section 7.5.3.2 */
6877 | { &hf_oran_rb,
6878 | { "rb", "oran_fh_cus.rb",
6879 | FT_UINT8, BASE_DEC,
6880 | VALS(rb_vals)((0 ? (const struct _value_string*)0 : ((rb_vals)))), 0x08,
6881 | "resource block indicator", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6882 | },
6883 |
6884 | /* Section 7.5.5.3 */
6885 | { &hf_oran_symInc,
6886 | { "symInc", "oran_fh_cus.symInc",
6887 | FT_UINT8, BASE_DEC,
6888 | VALS(sym_inc_vals)((0 ? (const struct _value_string*)0 : ((sym_inc_vals)))), 0x04,
6889 | "Symbol Number Increment Command", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6890 | },
6891 |
6892 | /* Section 7.5.3.4 */
6893 | { &hf_oran_startPrbc,
6894 | { "startPrbc", "oran_fh_cus.startPrbc",
6895 | FT_UINT16, BASE_DEC,
6896 | NULL((void*)0), 0x03ff,
6897 | "Starting PRB of Control Plane Section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6898 | },
6899 |
6900 | /* Section 7.5.3.5 */
6901 | { &hf_oran_reMask_re1,
6902 | { "RE 1", "oran_fh_cus.reMask-RE1",
6903 | FT_BOOLEAN, 16,
6904 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x8000,
6905 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6906 | },
6907 | { &hf_oran_reMask_re2,
6908 | { "RE 2", "oran_fh_cus.reMask-RE2",
6909 | FT_BOOLEAN, 16,
6910 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x4000,
6911 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6912 | },
6913 | { &hf_oran_reMask_re3,
6914 | { "RE 3", "oran_fh_cus.reMask-RE3",
6915 | FT_BOOLEAN, 16,
6916 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x2000,
6917 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6918 | },
6919 | { &hf_oran_reMask_re4,
6920 | { "RE 4", "oran_fh_cus.reMask-RE4",
6921 | FT_BOOLEAN, 16,
6922 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x1000,
6923 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6924 | },
6925 | { &hf_oran_reMask_re5,
6926 | { "RE 5", "oran_fh_cus.reMask-RE5",
6927 | FT_BOOLEAN, 16,
6928 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0800,
6929 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6930 | },
6931 | { &hf_oran_reMask_re6,
6932 | { "RE 6", "oran_fh_cus.reMask-RE6",
6933 | FT_BOOLEAN, 16,
6934 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0400,
6935 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6936 | },
6937 | { &hf_oran_reMask_re7,
6938 | { "RE 7", "oran_fh_cus.reMask-RE7",
6939 | FT_BOOLEAN, 16,
6940 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0200,
6941 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6942 | },
6943 | { &hf_oran_reMask_re8,
6944 | { "RE 8", "oran_fh_cus.reMask-RE8",
6945 | FT_BOOLEAN, 16,
6946 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0100,
6947 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6948 | },
6949 | { &hf_oran_reMask_re9,
6950 | { "RE 9", "oran_fh_cus.reMask-RE9",
6951 | FT_BOOLEAN, 16,
6952 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0080,
6953 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6954 | },
6955 | { &hf_oran_reMask_re10,
6956 | { "RE 10", "oran_fh_cus.reMask-RE10",
6957 | FT_BOOLEAN, 16,
6958 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0040,
6959 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6960 | },
6961 | { &hf_oran_reMask_re11,
6962 | { "RE 11", "oran_fh_cus.reMask-RE11",
6963 | FT_BOOLEAN, 16,
6964 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0020,
6965 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6966 | },
6967 | { &hf_oran_reMask_re12,
6968 | { "RE 12", "oran_fh_cus.reMask-RE12",
6969 | FT_BOOLEAN, 16,
6970 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0010,
6971 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6972 | },
6973 | { &hf_oran_reMask,
6974 | { "RE Mask", "oran_fh_cus.reMask",
6975 | FT_UINT16, BASE_HEX,
6976 | NULL((void*)0), 0xfff0,
6977 | "The Resource Element (RE) mask within a PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6978 | },
6979 |
6980 | /* Section 7.5.3.6 */
6981 | { &hf_oran_numPrbc,
6982 | { "numPrbc", "oran_fh_cus.numPrbc",
6983 | FT_UINT8, BASE_DEC,
6984 | NULL((void*)0), 0x0,
6985 | "Number of contiguous PRBs per data section description", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6986 | },
6987 |
6988 | /* Section 7.5.3.7 */
6989 | { &hf_oran_numSymbol,
6990 | { "Number of Symbols", "oran_fh_cus.numSymbol",
6991 | FT_UINT8, BASE_DEC,
6992 | NULL((void*)0), 0x0f,
6993 | "Defines number of symbols to which the section control is applicable", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6994 | },
6995 |
6996 | /* Section 7.5.3.8 */
6997 | { &hf_oran_ef,
6998 | { "Extension Flag", "oran_fh_cus.ef",
6999 | FT_BOOLEAN, 8,
7000 | NULL((void*)0), 0x80,
7001 | "Indicates if more section extensions follow", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7002 | },
7003 |
7004 | /* Section 7.5.3.9 */
7005 | { &hf_oran_beamId,
7006 | { "Beam ID", "oran_fh_cus.beamId",
7007 | FT_UINT16, BASE_DEC,
7008 | NULL((void*)0), 0x7fff,
7009 | "Defines the beam pattern to be applied to the U-Plane data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7010 | },
7011 |
7012 | { &hf_oran_extension,
7013 | { "Extension", "oran_fh_cus.extension",
7014 | FT_STRING, BASE_NONE,
7015 | NULL((void*)0), 0x0,
7016 | "Section extension", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7017 | },
7018 |
7019 | /* Section 7.6.2.1 */
7020 | { &hf_oran_exttype,
7021 | { "extType", "oran_fh_cus.extType",
7022 | FT_UINT8, BASE_DEC,
7023 | VALS(exttype_vals)((0 ? (const struct _value_string*)0 : ((exttype_vals)))), 0x7f,
7024 | "The extension type, which provides additional parameters specific to subject data extension", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7025 | },
7026 |
7027 | /* Section 7.6.2.3 */
7028 | { &hf_oran_extlen,
7029 | { "extLen", "oran_fh_cus.extLen",
7030 | FT_UINT16, BASE_DEC,
7031 | NULL((void*)0), 0x0,
7032 | "Extension length in 32-bit words", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7033 | },
7034 |
7035 | /* Section 7.7.1 */
7036 | { &hf_oran_bfw,
7037 | { "bfw", "oran_fh_cus.bfw",
7038 | FT_STRING, BASE_NONE,
7039 | NULL((void*)0), 0x0,
7040 | "Set of weights for a particular antenna", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7041 | },
7042 | { &hf_oran_bfw_bundle,
7043 | { "Bundle", "oran_fh_cus.bfw.bundle",
7044 | FT_STRING, BASE_NONE,
7045 | NULL((void*)0), 0x0,
7046 | "Bundle of BFWs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7047 | },
7048 | { &hf_oran_bfw_bundle_id,
7049 | { "Bundle Id", "oran_fh_cus.bfw.bundleId",
7050 | FT_UINT32, BASE_DEC,
7051 | NULL((void*)0), 0x0,
7052 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7053 | },
7054 | /* Section 7.7.1.4 */
7055 | { &hf_oran_bfw_i,
7056 | { "bfwI", "oran_fh_cus.bfwI",
7057 | FT_FLOAT, BASE_NONE,
7058 | NULL((void*)0), 0x0,
7059 | "In-phase", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7060 | },
7061 | /* Section 7.7.1.5 */
7062 | { &hf_oran_bfw_q,
7063 | { "bfwQ", "oran_fh_cus.bfwQ",
7064 | FT_FLOAT, BASE_NONE,
7065 | NULL((void*)0), 0x0,
7066 | "Quadrature", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7067 | },
7068 |
7069 | /* Section 7.5.3.10 */
7070 | { &hf_oran_ueId,
7071 | { "UE ID", "oran_fh_cus.ueId",
7072 | FT_UINT16, BASE_DEC,
7073 | NULL((void*)0), 0x7fff,
7074 | "logical identifier for set of channel info", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7075 | },
7076 |
7077 | /* Section 7.5.3.11 */
7078 | { &hf_oran_freqOffset,
7079 | { "Frequency Offset", "oran_fh_cus.freqOffset",
7080 | FT_UINT24, BASE_DEC,
7081 | NULL((void*)0), 0x0,
7082 | "with respect to the carrier center frequency before additional filtering", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7083 | },
7084 |
7085 | /* Section 7.5.3.12 */
7086 | { &hf_oran_regularizationFactor,
7087 | { "Regularization Factor", "oran_fh_cus.regularizationFactor",
7088 | FT_INT16, BASE_DEC,
7089 | NULL((void*)0), 0x0,
7090 | "Signed value to support MMSE operation within O-RU", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7091 | },
7092 |
7093 | /* Section 7.5.3.14 */
7094 | { &hf_oran_laaMsgType,
7095 | { "LAA Message Type", "oran_fh_cus.laaMsgType",
7096 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
7097 | RVALS(laaMsgTypes)((0 ? (const struct _range_string*)0 : ((laaMsgTypes)))), 0xf0,
7098 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7099 | },
7100 |
7101 | /* Section 7.5.3.15 */
7102 | { &hf_oran_laaMsgLen,
7103 | { "LAA Message Length", "oran_fh_cus.laaMsgLen",
7104 | FT_UINT8, BASE_DEC,
7105 | NULL((void*)0), 0x0f,
7106 | "number of 32-bit words in the LAA section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7107 | },
7108 |
7109 | /* Section 7.5.3.16 */
7110 | { &hf_oran_lbtHandle,
7111 | { "LBT Handle", "oran_fh_cus.lbtHandle",
7112 | FT_UINT16, BASE_HEX,
7113 | NULL((void*)0), 0x0,
7114 | "label to identify transaction", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7115 | },
7116 |
7117 | /* Section 7.5.3.17 */
7118 | { &hf_oran_lbtDeferFactor,
7119 | { "Defer Factor", "oran_fh_cus.lbtDeferFactor",
7120 | FT_UINT8, BASE_DEC,
7121 | NULL((void*)0), 0x07,
7122 | "Defer factor in sensing slots as described in 3GPP TS 36.213 Section 15.1.1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7123 | },
7124 |
7125 | /* Section 7.5.3.18 */
7126 | { &hf_oran_lbtBackoffCounter,
7127 | { "Backoff Counter", "oran_fh_cus.lbtBackoffCounter",
7128 | FT_UINT16, BASE_DEC,
7129 | NULL((void*)0), 0xffc0,
7130 | "LBT backoff counter in sensing slots as described in 3GPP TS 36.213 Section 15.1.1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7131 | },
7132 |
7133 | /* Section 7.5.3.19 */
7134 | { &hf_oran_lbtOffset,
7135 | { "LBT Offset", "oran_fh_cus.lbtOffset",
7136 | FT_UINT16, BASE_DEC,
7137 | NULL((void*)0), 0xffc0,
7138 | "LBT start time in microseconds from the beginning of the subframe scheduled by this message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7139 | },
7140 |
7141 | /* Section 7.5.3.20 */
7142 | { &hf_oran_MCOT,
7143 | { "Maximum Channel Occupancy Time", "oran_fh_cus.MCOT",
7144 | FT_UINT8, BASE_DEC,
7145 | NULL((void*)0), 0x3c,
7146 | "LTE TXOP duration in subframes as described in 3GPP TS 36.213 Section 15.1.1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7147 | },
7148 |
7149 | /* Section 7.5.3.21 */
7150 | { &hf_oran_lbtMode,
7151 | { "LBT Mode", "oran_fh_cus.lbtMode",
7152 | FT_UINT8, BASE_DEC,
7153 | VALS(lbtMode_vals)((0 ? (const struct _value_string*)0 : ((lbtMode_vals)))), 0x0,
7154 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7155 | },
7156 |
7157 | /* Section 7.5.3.22 */
7158 | { &hf_oran_lbtPdschRes,
7159 | { "lbtPdschRes", "oran_fh_cus.lbtPdschRes",
7160 | FT_UINT8, BASE_DEC,
7161 | VALS(lbtPdschRes_vals)((0 ? (const struct _value_string*)0 : ((lbtPdschRes_vals)))), 0xc0,
7162 | "LBT result of SFN/SF", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7163 | },
7164 |
7165 | /* Section 7.5.3.23 */
7166 | { &hf_oran_sfStatus,
7167 | { "sfStatus", "oran_fh_cus.sfStatus",
7168 | FT_BOOLEAN, 8,
7169 | TFS(&tfs_sfStatus)((0 ? (const struct true_false_string*)0 : ((&tfs_sfStatus )))), 0x10,
7170 | "Indicates whether the subframe was dropped or transmitted", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7171 | },
7172 |
7173 | /* Section 7.5.3.22 */
7174 | { &hf_oran_lbtDrsRes,
7175 | { "lbtDrsRes", "oran_fh_cus.lbtDrsRes",
7176 | FT_BOOLEAN, 8,
7177 | TFS(&tfs_fail_success)((0 ? (const struct true_false_string*)0 : ((&tfs_fail_success )))), 0x80,
7178 | "Indicates whether the subframe was dropped or transmitted", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7179 | },
7180 |
7181 | /* Section 7.5.3.25 */
7182 | { &hf_oran_initialPartialSF,
7183 | { "Initial partial SF", "oran_fh_cus.initialPartialSF",
7184 | FT_BOOLEAN, 8,
7185 | TFS(&tfs_partial_full_sf)((0 ? (const struct true_false_string*)0 : ((&tfs_partial_full_sf )))), 0x40,
7186 | "Indicates whether the initial SF in the LBT process is full or partial", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7187 | },
7188 |
7189 | /* Section 7.5.3.26. */
7190 | { &hf_oran_lbtBufErr,
7191 | { "lbtBufErr", "oran_fh_cus.lbtBufErr",
7192 | FT_BOOLEAN, 8,
7193 | TFS(&tfs_lbtBufErr)((0 ? (const struct true_false_string*)0 : ((&tfs_lbtBufErr )))), 0x80,
7194 | "LBT buffer error", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7195 | },
7196 |
7197 | /* Section 7.5.3.27 */
7198 | { &hf_oran_sfnSfEnd,
7199 | { "SFN/SF End", "oran_fh_cus.sfnSfEnd",
7200 | FT_UINT16, BASE_DEC,
7201 | NULL((void*)0), 0x0fff,
7202 | "SFN/SF by which the DRS window must end", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7203 | },
7204 |
7205 | /* Section 7.5.3.28 */
7206 | { &hf_oran_lbtCWConfig_H,
7207 | { "lbtCWConfig_H", "oran_fh_cus.lbtCWConfig_H",
7208 | FT_UINT8, BASE_DEC,
7209 | NULL((void*)0), 0x0,
7210 | "HARQ parameters for congestion window management", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7211 | },
7212 |
7213 | /* Section 7.5.3.29 */
7214 | { &hf_oran_lbtCWConfig_T,
7215 | { "lbtCWConfig_T", "oran_fh_cus.lbtCWConfig_T",
7216 | FT_UINT8, BASE_DEC,
7217 | NULL((void*)0), 0x0,
7218 | "TB parameters for congestion window management", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7219 | },
7220 |
7221 | /* Section 7.5.3.30 */
7222 | { &hf_oran_lbtTrafficClass,
7223 | { "lbtTrafficClass", "oran_fh_cus.lbtTrafficClass",
7224 | FT_UINT8, BASE_DEC,
7225 | VALS(lbtTrafficClass_vals)((0 ? (const struct _value_string*)0 : ((lbtTrafficClass_vals )))), 0x38,
7226 | "Traffic class priority for congestion window management", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7227 | },
7228 |
7229 | /* Section 7.5.3.31 */
7230 | { &hf_oran_lbtCWR_Rst,
7231 | { "lbtCWR_Rst", "oran_fh_cus.lbtCWR_Rst",
7232 | FT_BOOLEAN, 8,
7233 | TFS(&tfs_fail_success)((0 ? (const struct true_false_string*)0 : ((&tfs_fail_success )))), 0x80,
7234 | "notification about packet reception successful or not", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7235 | },
7236 |
7237 | /* Reserved fields */
7238 | { &hf_oran_reserved,
7239 | { "reserved", "oran_fh_cus.reserved",
7240 | FT_UINT64, BASE_HEX,
7241 | NULL((void*)0), 0x0,
7242 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7243 | },
7244 |
7245 | { &hf_oran_reserved_1bit,
7246 | { "reserved", "oran_fh_cus.reserved",
7247 | FT_UINT8, BASE_HEX,
7248 | NULL((void*)0), 0x80,
7249 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7250 | },
7251 | { &hf_oran_reserved_2bits,
7252 | { "reserved", "oran_fh_cus.reserved",
7253 | FT_UINT8, BASE_HEX,
7254 | NULL((void*)0), 0xc0,
7255 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7256 | },
7257 | { &hf_oran_reserved_3bits,
7258 | { "reserved", "oran_fh_cus.reserved",
7259 | FT_UINT8, BASE_HEX,
7260 | NULL((void*)0), 0xe0,
7261 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7262 | },
7263 | { &hf_oran_reserved_4bits,
7264 | { "reserved", "oran_fh_cus.reserved",
7265 | FT_UINT8, BASE_HEX,
7266 | NULL((void*)0), 0xf0,
7267 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7268 | },
7269 | { &hf_oran_reserved_last_4bits,
7270 | { "reserved", "oran_fh_cus.reserved",
7271 | FT_UINT8, BASE_HEX,
7272 | NULL((void*)0), 0x0f,
7273 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7274 | },
7275 | { &hf_oran_reserved_last_5bits,
7276 | { "reserved", "oran_fh_cus.reserved",
7277 | FT_UINT8, BASE_HEX,
7278 | NULL((void*)0), 0x1f,
7279 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7280 | },
7281 | { &hf_oran_reserved_6bits,
7282 | { "reserved", "oran_fh_cus.reserved",
7283 | FT_UINT8, BASE_HEX,
7284 | NULL((void*)0), 0xfc,
7285 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7286 | },
7287 | { &hf_oran_reserved_last_6bits,
7288 | { "reserved", "oran_fh_cus.reserved",
7289 | FT_UINT8, BASE_HEX,
7290 | NULL((void*)0), 0x3f,
7291 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7292 | },
7293 | { &hf_oran_reserved_7bits,
7294 | { "reserved", "oran_fh_cus.reserved",
7295 | FT_UINT8, BASE_HEX,
7296 | NULL((void*)0), 0xfe,
7297 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7298 | },
7299 | { &hf_oran_reserved_last_7bits,
7300 | { "reserved", "oran_fh_cus.reserved",
7301 | FT_UINT8, BASE_HEX,
7302 | NULL((void*)0), 0x7f,
7303 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7304 | },
7305 | { &hf_oran_reserved_8bits,
7306 | { "reserved", "oran_fh_cus.reserved",
7307 | FT_UINT8, BASE_HEX,
7308 | NULL((void*)0), 0x0,
7309 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7310 | },
7311 | { &hf_oran_reserved_16bits,
7312 | { "reserved", "oran_fh_cus.reserved",
7313 | FT_UINT16, BASE_HEX,
7314 | NULL((void*)0), 0x0,
7315 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7316 | },
7317 | { &hf_oran_reserved_15bits,
7318 | { "reserved", "oran_fh_cus.reserved",
7319 | FT_UINT16, BASE_HEX,
7320 | NULL((void*)0), 0x7fff,
7321 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7322 | },
7323 | { &hf_oran_reserved_bit1,
7324 | { "reserved", "oran_fh_cus.reserved",
7325 | FT_UINT8, BASE_HEX,
7326 | NULL((void*)0), 0x40,
7327 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7328 | },
7329 | { &hf_oran_reserved_bit2,
7330 | { "reserved", "oran_fh_cus.reserved",
7331 | FT_UINT8, BASE_HEX,
7332 | NULL((void*)0), 0x20,
7333 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7334 | },
7335 | { &hf_oran_reserved_bit4,
7336 | { "reserved", "oran_fh_cus.reserved",
7337 | FT_UINT8, BASE_HEX,
7338 | NULL((void*)0), 0x08,
7339 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7340 | },
7341 | { &hf_oran_reserved_bit5,
7342 | { "reserved", "oran_fh_cus.reserved",
7343 | FT_UINT8, BASE_HEX,
7344 | NULL((void*)0), 0x04,
7345 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7346 | },
7347 | { &hf_oran_reserved_bits123,
7348 | { "reserved", "oran_fh_cus.reserved",
7349 | FT_UINT8, BASE_HEX,
7350 | NULL((void*)0), 0x70,
7351 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7352 | },
7353 | { &hf_oran_reserved_bits456,
7354 | { "reserved", "oran_fh_cus.reserved",
7355 | FT_UINT8, BASE_HEX,
7356 | NULL((void*)0), 0x0e,
7357 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7358 | },
7359 |
7360 |
7361 | /* 7.7.11.10 */
7362 | { &hf_oran_bundle_offset,
7363 | { "BundleOffset", "oran_fh_cus.bundleOffset",
7364 | FT_UINT8, BASE_DEC,
7365 | NULL((void*)0), 0x3f,
7366 | "offset between start of first PRB bundle and startPrbc", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7367 | },
7368 | /* 7.7.11.9 */
7369 | { &hf_oran_cont_ind,
7370 | { "contInd", "oran_fh_cus.contInd",
7371 | FT_BOOLEAN, 8,
7372 | TFS(&continuity_indication_tfs)((0 ? (const struct true_false_string*)0 : ((&continuity_indication_tfs )))), 0x80,
7373 | "PRB region continuity flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7374 | },
7375 |
7376 | /* 7.7.1.2 bfwCompHdr (beamforming weight compression header) */
7377 | { &hf_oran_bfwCompHdr,
7378 | { "bfwCompHdr", "oran_fh_cus.bfwCompHdr",
7379 | FT_STRING, BASE_NONE,
7380 | NULL((void*)0), 0x0,
7381 | "Compression method and IQ bit width for beamforming weights", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7382 | },
7383 | { &hf_oran_bfwCompHdr_iqWidth,
7384 | { "IQ Bit Width", "oran_fh_cus.bfwCompHdr_iqWidth",
7385 | FT_UINT8, BASE_HEX,
7386 | VALS(bfw_comp_headers_iq_width)((0 ? (const struct _value_string*)0 : ((bfw_comp_headers_iq_width )))), 0xf0,
7387 | "IQ bit width for the beamforming weights", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7388 | },
7389 | { &hf_oran_bfwCompHdr_compMeth,
7390 | { "Compression Method", "oran_fh_cus.bfwCompHdr_compMeth",
7391 | FT_UINT8, BASE_HEX,
7392 | VALS(bfw_comp_headers_comp_meth)((0 ? (const struct _value_string*)0 : ((bfw_comp_headers_comp_meth )))), 0x0f,
7393 | "compression method for the beamforming weights", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7394 | },
7395 |
7396 | /* 7.5.3.32 */
7397 | { &hf_oran_ciCompParam,
7398 | { "ciCompParam", "oran_fh_cus.ciCompParam",
7399 | FT_STRING, BASE_NONE,
7400 | NULL((void*)0), 0x0,
7401 | "channel information compression parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7402 | },
7403 |
7404 | /* Table 7.5.3.32-1 */
7405 | { &hf_oran_blockScaler,
7406 | { "blockScaler", "oran_fh_cus.blockScaler",
7407 | FT_UINT8, BASE_HEX,
7408 | NULL((void*)0), 0x0,
7409 | "unsigned, 1 integer bit, 7 fractional bits", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7410 | },
7411 | { &hf_oran_compBitWidth,
7412 | { "compBitWidth", "oran_fh_cus.compBitWidth",
7413 | FT_UINT8, BASE_DEC,
7414 | NULL((void*)0), 0xf0,
7415 | "Length of I bits and length of Q bits after compression over entire PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7416 | },
7417 | { &hf_oran_compShift,
7418 | { "compShift", "oran_fh_cus.compShift",
7419 | FT_UINT8, BASE_DEC,
7420 | NULL((void*)0), 0x0f,
7421 | "The shift applied to the entire PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7422 | },
7423 |
7424 | { &hf_oran_active_beamspace_coefficient_n1,
7425 | { "N1", "oran_fh_cus.activeBeamspace_Coefficient_n1",
7426 | FT_BOOLEAN, 8,
7427 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x80,
7428 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7429 | },
7430 | { &hf_oran_active_beamspace_coefficient_n2,
7431 | { "N2", "oran_fh_cus.activeBeamspace_Coefficient_n2",
7432 | FT_BOOLEAN, 8,
7433 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x40,
7434 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7435 | },
7436 | { &hf_oran_active_beamspace_coefficient_n3,
7437 | { "N3", "oran_fh_cus.activeBeamspace_Coefficient_n3",
7438 | FT_BOOLEAN, 8,
7439 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x20,
7440 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7441 | },
7442 | { &hf_oran_active_beamspace_coefficient_n4,
7443 | { "N4", "oran_fh_cus.activeBeamspace_Coefficient_n4",
7444 | FT_BOOLEAN, 8,
7445 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x10,
7446 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7447 | },
7448 | { &hf_oran_active_beamspace_coefficient_n5,
7449 | { "N5", "oran_fh_cus.activeBeamspace_Coefficient_n5",
7450 | FT_BOOLEAN, 8,
7451 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x08,
7452 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7453 | },
7454 | { &hf_oran_active_beamspace_coefficient_n6,
7455 | { "N6", "oran_fh_cus.activeBeamspace_Coefficient_n6",
7456 | FT_BOOLEAN, 8,
7457 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x04,
7458 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7459 | },
7460 | { &hf_oran_active_beamspace_coefficient_n7,
7461 | { "N7", "oran_fh_cus.activeBeamspace_Coefficient_n7",
7462 | FT_BOOLEAN, 8,
7463 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x02,
7464 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7465 | },
7466 | { &hf_oran_active_beamspace_coefficient_n8,
7467 | { "N8", "oran_fh_cus.activeBeamspace_Coefficient_n8",
7468 | FT_BOOLEAN, 8,
7469 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x01,
7470 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7471 | },
7472 |
7473 | { &hf_oran_activeBeamspaceCoefficientMask,
7474 | { "activeBeamspaceCoefficientMask", "oran_fh_cus.activeBeamspaceCoefficientMask",
7475 | FT_UINT8, BASE_HEX,
7476 | NULL((void*)0), 0xff,
7477 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7478 | },
7479 | { &hf_oran_activeBeamspaceCoefficientMask_bits_set,
7480 | { "Array elements set", "oran_fh_cus.activeBeamspaceCoefficientMask.bits-set",
7481 | FT_UINT32, BASE_DEC,
7482 | NULL((void*)0), 0x0,
7483 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7484 | },
7485 |
7486 | /* Section 7.7.6.6 */
7487 | { &hf_oran_se6_repetition,
7488 | { "repetition", "oran_fh_cus.repetition",
7489 | FT_BOOLEAN, BASE_NONE,
7490 | TFS(&repetition_se6_tfs)((0 ? (const struct true_false_string*)0 : ((&repetition_se6_tfs )))), 0x0,
7491 | "Repetition of a highest priority data section for C-Plane", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7492 | },
7493 | /* 7.7.20.9 */
7494 | { &hf_oran_rbgSize,
7495 | { "rbgSize", "oran_fh_cus.rbgSize",
7496 | FT_UINT8, BASE_HEX,
7497 | VALS(rbg_size_vals)((0 ? (const struct _value_string*)0 : ((rbg_size_vals)))), 0x70,
7498 | "Number of PRBs of the resource block groups allocated by the bit mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7499 | },
7500 | /* 7.7.20.10 */
7501 | { &hf_oran_rbgMask,
7502 | { "rbgMask", "oran_fh_cus.rbgMask",
7503 | FT_UINT32, BASE_HEX,
7504 | NULL((void*)0), 0x0fffffff,
7505 | "Each bit indicates whether a corresponding resource block group is present", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7506 | },
7507 | /* 7.7.6.5. Also 7.7.12.3 and 7.7.19.5 */
7508 | { &hf_oran_noncontig_priority,
7509 | { "priority", "oran_fh_cus.priority",
7510 | FT_UINT8, BASE_HEX,
7511 | VALS(priority_vals)((0 ? (const struct _value_string*)0 : ((priority_vals)))), 0xc0,
7512 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7513 | },
7514 |
7515 | /* 7.7.6.4 */
7516 | { &hf_oran_symbol_mask,
7517 | { "symbolMask", "oran_fh_cus.symbolMask",
7518 | FT_UINT16, BASE_HEX,
7519 | NULL((void*)0), 0x3fff,
7520 | "Each bit indicates whether the rbgMask applies to a given symbol in the slot", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7521 | },
7522 | { &hf_oran_symbol_mask_s13,
7523 | { "symbol 13", "oran_fh_cus.symbolMask.symbol-13",
7524 | FT_BOOLEAN, 16,
7525 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x2000,
7526 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7527 | },
7528 | { &hf_oran_symbol_mask_s12,
7529 | { "symbol 12", "oran_fh_cus.symbolMask.symbol-12",
7530 | FT_BOOLEAN, 16,
7531 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x1000,
7532 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7533 | },
7534 | { &hf_oran_symbol_mask_s11,
7535 | { "symbol 11", "oran_fh_cus.symbolMask.symbol-11",
7536 | FT_BOOLEAN, 16,
7537 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0800,
7538 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7539 | },
7540 | { &hf_oran_symbol_mask_s10,
7541 | { "symbol 10", "oran_fh_cus.symbolMask.symbol-10",
7542 | FT_BOOLEAN, 16,
7543 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0400,
7544 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7545 | },
7546 | { &hf_oran_symbol_mask_s9,
7547 | { "symbol 9", "oran_fh_cus.symbolMask.symbol-9",
7548 | FT_BOOLEAN, 16,
7549 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0200,
7550 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7551 | },
7552 | { &hf_oran_symbol_mask_s8,
7553 | { "symbol 8", "oran_fh_cus.symbolMask.symbol-8",
7554 | FT_BOOLEAN, 16,
7555 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0100,
7556 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7557 | },
7558 | { &hf_oran_symbol_mask_s7,
7559 | { "symbol 7", "oran_fh_cus.symbolMask.symbol-7",
7560 | FT_BOOLEAN, 16,
7561 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0080,
7562 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7563 | },
7564 | { &hf_oran_symbol_mask_s6,
7565 | { "symbol 6", "oran_fh_cus.symbolMask.symbol-6",
7566 | FT_BOOLEAN, 16,
7567 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0040,
7568 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7569 | },
7570 | { &hf_oran_symbol_mask_s5,
7571 | { "symbol 5", "oran_fh_cus.symbolMask.symbol-5",
7572 | FT_BOOLEAN, 16,
7573 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0020,
7574 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7575 | },
7576 | { &hf_oran_symbol_mask_s4,
7577 | { "symbol 4", "oran_fh_cus.symbolMask.symbol-4",
7578 | FT_BOOLEAN, 16,
7579 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0010,
7580 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7581 | },
7582 | { &hf_oran_symbol_mask_s3,
7583 | { "symbol 3", "oran_fh_cus.symbolMask.symbol-3",
7584 | FT_BOOLEAN, 16,
7585 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0008,
7586 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7587 | },
7588 | { &hf_oran_symbol_mask_s2,
7589 | { "symbol 2", "oran_fh_cus.symbolMask.symbol-2",
7590 | FT_BOOLEAN, 16,
7591 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0004,
7592 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7593 | },
7594 | { &hf_oran_symbol_mask_s1,
7595 | { "symbol 1", "oran_fh_cus.symbolMask.symbol-1",
7596 | FT_BOOLEAN, 16,
7597 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0002,
7598 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7599 | },
7600 | { &hf_oran_symbol_mask_s0,
7601 | { "symbol 0", "oran_fh_cus.symbolMask.symbol-0",
7602 | FT_BOOLEAN, 16,
7603 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0001,
7604 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7605 | },
7606 |
7607 |
7608 | /* 7.7.22.2 */
7609 | { &hf_oran_ack_nack_req_id,
7610 | { "ackNackReqId", "oran_fh_cus.ackNackReqId",
7611 | FT_UINT16, BASE_HEX,
7612 | NULL((void*)0), 0x0,
7613 | "Indicates the ACK/NACK request ID of a section description", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7614 | },
7615 |
7616 | /* Subtree for next 2 items */
7617 | { &hf_oran_frequency_range,
7618 | { "Frequency Range", "oran_fh_cus.frequencyRange",
7619 | FT_STRING, BASE_NONE,
7620 | NULL((void*)0), 0x0,
7621 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7622 | },
7623 |
7624 | /* 7.7.12.4 */
7625 | { &hf_oran_off_start_prb,
7626 | { "offStartPrb", "oran_fh_cus.offStartPrb",
7627 | FT_UINT8, BASE_DEC,
7628 | NULL((void*)0), 0x0,
7629 | "Offset of PRB range start", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7630 | },
7631 | /* 7.7.12.5 */
7632 | { &hf_oran_num_prb,
7633 | { "numPrb", "oran_fh_cus.numPrb",
7634 | FT_UINT8, BASE_DEC,
7635 | NULL((void*)0), 0x0,
7636 | "Number of PRBs in PRB range", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7637 | },
7638 |
7639 | /* symbolId 8.3.3.7 */
7640 | { &hf_oran_symbolId,
7641 | { "Symbol Identifier", "oran_fh_cus.symbolId",
7642 | FT_UINT8, BASE_DEC,
7643 | NULL((void*)0), 0x3f,
7644 | "Identifies a symbol number within a slot", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7645 | },
7646 |
7647 | /* startPrbu 8.3.3.11 */
7648 | { &hf_oran_startPrbu,
7649 | { "startPrbu", "oran_fh_cus.startPrbu",
7650 | FT_UINT16, BASE_DEC,
7651 | NULL((void*)0), 0x03ff,
7652 | "starting PRB of user plane section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7653 | },
7654 |
7655 | /* numPrbu 8.3.3.12 */
7656 | { &hf_oran_numPrbu,
7657 | { "numPrbu", "oran_fh_cus.numPrbu",
7658 | FT_UINT8, BASE_DEC,
7659 | NULL((void*)0), 0x0,
7660 | "number of PRBs per user plane section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7661 | },
7662 |
7663 | /* 7.7.1.3 */
7664 | { &hf_oran_bfwCompParam,
7665 | { "bfwCompParam", "oran_fh_cus.bfwCompParam",
7666 | FT_STRING, BASE_NONE,
7667 | NULL((void*)0), 0x0,
7668 | "Beamforming weight compression parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7669 | },
7670 |
7671 | /* 6.3.3.13 */
7672 | { &hf_oran_udCompHdrMeth,
7673 | { "User Data Compression Method", "oran_fh_cus.udCompHdrMeth",
7674 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
7675 | RVALS(ud_comp_header_meth)((0 ? (const struct _range_string*)0 : ((ud_comp_header_meth) ))), 0x0f,
7676 | "Defines the compression method for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7677 | },
7678 | { &hf_oran_udCompHdrMeth_pref,
7679 | { "User Data Compression Method", "oran_fh_cus.udCompHdrMeth",
7680 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
7681 | RVALS(ud_comp_header_meth)((0 ? (const struct _range_string*)0 : ((ud_comp_header_meth) ))), 0x0,
7682 | "Defines the compression method for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7683 | },
7684 | /* 8.3.3.18 */
7685 | { &hf_oran_udCompLen,
7686 | { "udCompLen", "oran_fh_cus.udCompLen",
7687 | FT_UINT16, BASE_DEC,
7688 | NULL((void*)0), 0x0,
7689 | "PRB field length in octets", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7690 | },
7691 |
7692 | /* 6.3.3.13 */
7693 | { &hf_oran_udCompHdrIqWidth,
7694 | { "User Data IQ width", "oran_fh_cus.udCompHdrWidth",
7695 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
7696 | RVALS(ud_comp_header_width)((0 ? (const struct _range_string*)0 : ((ud_comp_header_width )))), 0xf0,
7697 | "Defines the IQ bit width for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7698 | },
7699 | { &hf_oran_udCompHdrIqWidth_pref,
7700 | { "User Data IQ width", "oran_fh_cus.udCompHdrWidth",
7701 | FT_UINT8, BASE_DEC,
7702 | NULL((void*)0), 0x0,
7703 | "Defines the IQ bit width for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7704 | },
7705 |
7706 | { &hf_oran_sinrCompHdrIqWidth_pref,
7707 | { "SINR IQ width", "oran_fh_cus.sinrCompHdrWidth",
7708 | FT_UINT8, BASE_DEC,
7709 | NULL((void*)0), 0x0,
7710 | "Defines the IQ bit width for SINR data in section type 9", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7711 | },
7712 | { &hf_oran_sinrCompHdrMeth_pref,
7713 | { "SINR Compression Method", "oran_fh_cus.sinrCompHdrMeth",
7714 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
7715 | RVALS(ud_comp_header_meth)((0 ? (const struct _range_string*)0 : ((ud_comp_header_meth) ))), 0x0,
7716 | "Defines the compression method for SINR data in section type 9", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7717 | },
7718 |
7719 | /* Section 8.3.3.15 (not always present - depends upon meth) */
7720 | { &hf_oran_udCompParam,
7721 | { "User Data Compression Parameter", "oran_fh_cus.udCompParam",
7722 | FT_STRING, BASE_NONE,
7723 | NULL((void*)0), 0x0,
7724 | "Applies to whatever compression method is specified by the associated sectionID's compMeth value", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7725 | },
7726 | /* 8.3.3.18 */
7727 | { &hf_oran_sReSMask,
7728 | { "sReSMask", "oran_fh_cus.sReSMask",
7729 | FT_UINT16, BASE_HEX,
7730 | NULL((void*)0), 0xf0ff,
7731 | "selective RE sending mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7732 | },
7733 |
7734 | { &hf_oran_sReSMask_re12,
7735 | { "RE-12", "oran_fh_cus.sReSMask-re12",
7736 | FT_BOOLEAN, 16,
7737 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x8000,
7738 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7739 | },
7740 | { &hf_oran_sReSMask_re11,
7741 | { "RE-11", "oran_fh_cus.sReSMask-re11",
7742 | FT_BOOLEAN, 16,
7743 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x4000,
7744 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7745 | },
7746 | { &hf_oran_sReSMask_re10,
7747 | { "RE-10", "oran_fh_cus.sReSMask-re10",
7748 | FT_BOOLEAN, 16,
7749 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x2000,
7750 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7751 | },
7752 | { &hf_oran_sReSMask_re9,
7753 | { "RE-9", "oran_fh_cus.sReSMask-re9",
7754 | FT_BOOLEAN, 16,
7755 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x1000,
7756 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7757 | },
7758 | { &hf_oran_sReSMask_re8,
7759 | { "RE-8", "oran_fh_cus.sReSMask-re8",
7760 | FT_BOOLEAN, 16,
7761 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0080,
7762 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7763 | },
7764 | { &hf_oran_sReSMask_re7,
7765 | { "RE-7", "oran_fh_cus.sReSMask-re7",
7766 | FT_BOOLEAN, 16,
7767 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0040,
7768 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7769 | },
7770 | { &hf_oran_sReSMask_re6,
7771 | { "RE-6", "oran_fh_cus.sReSMask-re6",
7772 | FT_BOOLEAN, 16,
7773 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0020,
7774 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7775 | },
7776 | { &hf_oran_sReSMask_re5,
7777 | { "RE-5", "oran_fh_cus.sReSMask-re5",
7778 | FT_BOOLEAN, 16,
7779 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0010,
7780 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7781 | },
7782 | { &hf_oran_sReSMask_re4,
7783 | { "RE-4", "oran_fh_cus.sReSMask-re4",
7784 | FT_BOOLEAN, 16,
7785 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0008,
7786 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7787 | },
7788 | { &hf_oran_sReSMask_re3,
7789 | { "RE-3", "oran_fh_cus.sReSMask-re3",
7790 | FT_BOOLEAN, 16,
7791 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0004,
7792 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7793 | },
7794 | { &hf_oran_sReSMask_re2,
7795 | { "RE-2", "oran_fh_cus.sReSMask-re2",
7796 | FT_BOOLEAN, 16,
7797 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0002,
7798 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7799 | },
7800 | { &hf_oran_sReSMask_re1,
7801 | { "RE-1", "oran_fh_cus.sReSMask-re1",
7802 | FT_BOOLEAN, 16,
7803 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0001,
7804 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7805 | },
7806 |
7807 | /* 8.3.3.20 */
7808 | { &hf_oran_sReSMask1,
7809 | { "sReSMask1", "oran_fh_cus.sReSMask1",
7810 | FT_UINT16, BASE_HEX,
7811 | NULL((void*)0), 0x0fff,
7812 | "selective RE sending mask 1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7813 | },
7814 | /* 8.3.3.21 */
7815 | { &hf_oran_sReSMask2,
7816 | { "sReSMask2", "oran_fh_cus.sReSMask2",
7817 | FT_UINT16, BASE_HEX,
7818 | NULL((void*)0), 0x0fff,
7819 | "selective RE sending mask 2", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7820 | },
7821 |
7822 | { &hf_oran_sReSMask1_2_re12,
7823 | { "RE-12", "oran_fh_cus.sReSMask-re12",
7824 | FT_BOOLEAN, 16,
7825 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0800,
7826 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7827 | },
7828 | { &hf_oran_sReSMask1_2_re11,
7829 | { "RE-11", "oran_fh_cus.sReSMask-re11",
7830 | FT_BOOLEAN, 16,
7831 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0400,
7832 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7833 | },
7834 | { &hf_oran_sReSMask1_2_re10,
7835 | { "RE-10", "oran_fh_cus.sReSMask-re10",
7836 | FT_BOOLEAN, 16,
7837 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0200,
7838 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7839 | },
7840 | { &hf_oran_sReSMask1_2_re9,
7841 | { "RE-9", "oran_fh_cus.sReSMask-re9",
7842 | FT_BOOLEAN, 16,
7843 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0100,
7844 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7845 | },
7846 |
7847 | /* Section 6.3.3.15 */
7848 | { &hf_oran_iSample,
7849 | { "iSample", "oran_fh_cus.iSample",
7850 | FT_FLOAT, BASE_NONE,
7851 | NULL((void*)0), 0x0,
7852 | "In-phase Sample value", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7853 | },
7854 |
7855 | /* Section 6.3.3.16 */
7856 | { &hf_oran_qSample,
7857 | { "qSample", "oran_fh_cus.qSample",
7858 | FT_FLOAT, BASE_NONE,
7859 | NULL((void*)0), 0x0,
7860 | "Quadrature Sample value", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7861 | },
7862 |
7863 | { &hf_oran_exponent,
7864 | { "Exponent", "oran_fh_cus.exponent",
7865 | FT_UINT8, BASE_DEC,
7866 | NULL((void*)0), 0x0f,
7867 | "Exponent applicable to the I & Q mantissas", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7868 | },
7869 |
7870 | { &hf_oran_iq_user_data,
7871 | { "IQ User Data", "oran_fh_cus.iq_user_data",
7872 | FT_BYTES, BASE_NONE,
7873 | NULL((void*)0), 0x0,
7874 | "Used for the In-phase and Quadrature sample mantissa", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7875 | },
7876 |
7877 |
7878 | { &hf_oran_u_section_ul_symbol_time,
7879 | { "Microseconds since first UL U-plane frame for this symbol", "oran_fh_cus.us-since-first-ul-frame",
7880 | FT_UINT32, BASE_DEC,
7881 | NULL((void*)0), 0x0,
7882 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7883 | },
7884 | { &hf_oran_u_section_ul_symbol_frames,
7885 | { "Number of UL frames sent for this symbol", "oran_fh_cus.number-ul-frames-in-symbol",
7886 | FT_UINT32, BASE_DEC,
7887 | NULL((void*)0), 0x0,
7888 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7889 | },
7890 | { &hf_oran_u_section_ul_symbol_first_frame,
7891 | { "First UL frame for this symbol", "oran_fh_cus.first-ul-frame-in-symbol",
7892 | FT_FRAMENUM, BASE_NONE,
7893 | FRAMENUM_TYPE(FT_FRAMENUM_NONE)((gpointer) (glong) (FT_FRAMENUM_NONE)), 0x0,
7894 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7895 | },
7896 | { &hf_oran_u_section_ul_symbol_last_frame,
7897 | { "Last UL frame for this symbol", "oran_fh_cus.last-ul-frame-in-symbol",
7898 | FT_FRAMENUM, BASE_NONE,
7899 | FRAMENUM_TYPE(FT_FRAMENUM_NONE)((gpointer) (glong) (FT_FRAMENUM_NONE)), 0x0,
7900 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7901 | },
7902 |
7903 | { &hf_oran_c_eAxC_ID,
7904 | { "c_eAxC_ID", "oran_fh_cus.c_eaxc_id",
7905 | FT_STRING, BASE_NONE,
7906 | NULL((void*)0), 0x0,
7907 | "This is a calculated field for the c_eAxC ID, which identifies the message stream", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7908 | },
7909 |
7910 | { &hf_oran_refa,
7911 | { "RefA", "oran_fh_cus.refa",
7912 | FT_STRING, BASE_NONE,
7913 | NULL((void*)0), 0x0,
7914 | "This is a calculated field for the RefA ID, which provides a reference in time", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7915 | },
7916 |
7917 |
7918 | /* Section 7.5.2.15 */
7919 | { &hf_oran_ciCompHdr,
7920 | { "ciCompHdr", "oran_fh_cus.ciCompHdr",
7921 | FT_STRING, BASE_NONE,
7922 | NULL((void*)0), 0x0,
7923 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7924 | },
7925 | { &hf_oran_ciCompHdrMeth,
7926 | { "User Data Compression Method", "oran_fh_cus.ciCompHdrMeth",
7927 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
7928 | RVALS(ud_comp_header_meth)((0 ? (const struct _range_string*)0 : ((ud_comp_header_meth) ))), 0x0e,
7929 | "Defines the compression method for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7930 | },
7931 | { &hf_oran_ciCompHdrIqWidth,
7932 | { "User Data IQ width", "oran_fh_cus.udCompHdrWidth",
7933 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
7934 | RVALS(ud_comp_header_width)((0 ? (const struct _range_string*)0 : ((ud_comp_header_width )))), 0xf0,
7935 | "Defines the IQ bit width for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7936 | },
7937 | { &hf_oran_ciCompOpt,
7938 | { "ciCompOpt", "oran_fh_cus.ciCompOpt",
7939 | FT_UINT8, BASE_DEC,
7940 | VALS(ci_comp_opt_vals)((0 ? (const struct _value_string*)0 : ((ci_comp_opt_vals)))), 0x01,
7941 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7942 | },
7943 |
7944 | /* 7.7.11.7 */
7945 | { &hf_oran_disable_bfws,
7946 | { "disableBFWs", "oran_fh_cus.disableBFWs",
7947 | FT_BOOLEAN, 8,
7948 | NULL((void*)0), 0x80,
7949 | "Indicate if BFWs under section extension are disabled", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7950 | },
7951 | /* 7.7.11.8 */
7952 | { &hf_oran_rad,
7953 | { "RAD", "oran_fh_cus.rad",
7954 | FT_BOOLEAN, 8,
7955 | NULL((void*)0), 0x40,
7956 | "Reset After PRB Discontinuity", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7957 | },
7958 | /* 7.7.11.4 */
7959 | { &hf_oran_num_bund_prbs,
7960 | { "numBundPrb", "oran_fh_cus.numBundPrb",
7961 | FT_UINT8, BASE_DEC,
7962 | NULL((void*)0), 0x0,
7963 | "Number of bundled PRBs per BFWs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7964 | },
7965 | { &hf_oran_beam_id,
7966 | { "beamId", "oran_fh_cus.beamId",
7967 | FT_UINT16, BASE_DEC,
7968 | NULL((void*)0), 0x7fff,
7969 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7970 | },
7971 | { &hf_oran_num_weights_per_bundle,
7972 | { "Num weights per bundle", "oran_fh_cus.num_weights_per_bundle",
7973 | FT_UINT16, BASE_DEC,
7974 | NULL((void*)0), 0x0,
7975 | "From dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7976 | },
7977 |
7978 | { &hf_oran_samples_prb,
7979 | {"PRB", "oran_fh_cus.prb",
7980 | FT_STRING, BASE_NONE,
7981 | NULL((void*)0), 0x0,
7982 | "Grouping of samples for a particular Physical Resource Block", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7983 | },
7984 |
7985 | /* 7.5.3.13 */
7986 | { &hf_oran_ciSample,
7987 | { "ciSample", "oran_fh_cus.ciSample",
7988 | FT_STRING, BASE_NONE,
7989 | NULL((void*)0), 0x0,
7990 | "Sample (I and Q values)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7991 | },
7992 | { &hf_oran_ciIsample,
7993 | { "ciIsample", "oran_fh_cus.ciISample",
7994 | FT_FLOAT, BASE_NONE,
7995 | NULL((void*)0), 0x0,
7996 | "Channel information complex value - I part", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7997 | },
7998 | { &hf_oran_ciQsample,
7999 | { "ciQsample", "oran_fh_cus.ciQSample",
8000 | FT_FLOAT, BASE_NONE,
8001 | NULL((void*)0), 0x0,
8002 | "Channel information complex value - Q part", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8003 | },
8004 |
8005 | /* 7.7.10.2 */
8006 | { &hf_oran_beamGroupType,
8007 | { "beamGroupType", "oran_fh_cus.beamGroupType",
8008 | FT_UINT8, BASE_DEC,
8009 | VALS(beam_group_type_vals)((0 ? (const struct _value_string*)0 : ((beam_group_type_vals )))), 0xc0,
8010 | "The type of beam grouping", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8011 | },
8012 | /* 7.7.10.3 */
8013 | { &hf_oran_numPortc,
8014 | { "numPortc", "oran_fh_cus.numPortc",
8015 | FT_UINT8, BASE_DEC,
8016 | NULL((void*)0), 0x3f,
8017 | "The number of eAxC ports", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8018 | },
8019 |
8020 | /* 7.7.4.2 (1 bit) */
8021 | { &hf_oran_csf,
8022 | { "csf", "oran_fh_cus.csf",
8023 | FT_BOOLEAN, BASE_NONE,
8024 | NULL((void*)0), 0x0,
8025 | "constellation shift flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8026 | },
8027 | /* 7.7.4.3 */
8028 | { &hf_oran_modcompscaler,
8029 | { "modCompScaler", "oran_fh_cus.modcompscaler",
8030 | FT_UINT16, BASE_DEC,
8031 | NULL((void*)0), 0x7fff,
8032 | "modulation compression scaler value", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8033 | },
8034 |
8035 | /* 7.7.5.1 */
8036 | { &hf_oran_modcomp_param_set,
8037 | { "Set", "oran_fh_cus.modcomp-param-set",
8038 | FT_STRING, BASE_NONE,
8039 | NULL((void*)0), 0x0,
8040 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8041 | },
8042 |
8043 | /* mcScaleReMask 7.7.5.2 (12 bits) */
8044 | { &hf_oran_mc_scale_re_mask,
8045 | { "mcScaleReMask", "oran_fh_cus.mcscaleremask",
8046 | FT_BOOLEAN, BASE_NONE,
8047 | NULL((void*)0), 0x0,
8048 | "modulation compression power scale RE mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8049 | },
8050 | /* mcScaleOffset 7.7.5.4 (15 bits) */
8051 | { &hf_oran_mc_scale_offset,
8052 | { "mcScaleOffset", "oran_fh_cus.mcscaleoffset",
8053 | FT_UINT24, BASE_DEC,
8054 | NULL((void*)0), 0x0,
8055 | "scaling value for modulation compression", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8056 | },
8057 | /* eAxCmask (7.7.7.2) */
8058 | { &hf_oran_eAxC_mask,
8059 | { "eAxC Mask", "oran_fh_cus.eaxcmask",
8060 | FT_UINT16, BASE_HEX,
8061 | NULL((void*)0), 0xffff,
8062 | "Which eAxC_ID values the C-Plane message applies to", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8063 | },
8064 | /* technology (interface name) 7.7.9.2 */
8065 | { &hf_oran_technology,
8066 | { "Technology", "oran_fh_cus.technology",
8067 | FT_UINT8, BASE_DEC,
8068 | VALS(interface_name_vals)((0 ? (const struct _value_string*)0 : ((interface_name_vals) ))), 0x0,
8069 | "Interface name (that C-PLane section applies to)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8070 | },
8071 | /* Exttype 14 (7.7.14.2) */
8072 | { &hf_oran_nullLayerInd,
8073 | { "nullLayerInd", "oran_fh_cus.nulllayerind",
8074 | FT_BOOLEAN, BASE_NONE,
8075 | NULL((void*)0), 0x0,
8076 | "Whether corresponding layer is nulling-layer or not", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8077 | },
8078 |
8079 | /* Exttype 19 */
8080 | /* 7.7.19.3 */
8081 | { &hf_oran_se19_repetition,
8082 | { "repetition", "oran_fh_cus.repetition",
8083 | FT_BOOLEAN, BASE_NONE,
8084 | TFS(&repetition_se19_tfs)((0 ? (const struct true_false_string*)0 : ((&repetition_se19_tfs )))), 0x0,
8085 | "repeat port info flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8086 | },
8087 | /* 7.7.19.8 */
8088 | /* TODO: break down into each RE as done for 7.5.3.5 ? */
8089 | { &hf_oran_portReMask,
8090 | { "portReMask", "oran_fh_cus.portReMask",
8091 | FT_BOOLEAN, 16,
8092 | TFS(&tfs_set_notset)((0 ? (const struct true_false_string*)0 : ((&tfs_set_notset )))), 0x0fff,
8093 | "RE bitmask per port", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8094 | },
8095 | /* 7.7.19.9 */
8096 | { &hf_oran_portSymbolMask,
8097 | { "portSymbolMask", "oran_fh_cus.portSymbolMask",
8098 | FT_BOOLEAN, 16,
8099 | TFS(&tfs_set_notset)((0 ? (const struct true_false_string*)0 : ((&tfs_set_notset )))), 0x3fff,
8100 | "Symbol bitmask port port", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8101 | },
8102 |
8103 | { &hf_oran_ext19_port,
8104 | {"Port", "oran_fh_cus.ext19.port",
8105 | FT_STRING, BASE_NONE,
8106 | NULL((void*)0), 0x0,
8107 | "Entry for a given port in ext19", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8108 | },
8109 |
8110 | /* Ext 13 */
8111 | { &hf_oran_prb_allocation,
8112 | {"PRB allocation", "oran_fh_cus.prb-allocation",
8113 | FT_STRING, BASE_NONE,
8114 | NULL((void*)0), 0x0,
8115 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8116 | },
8117 | /* 7.7.13.2 */
8118 | { &hf_oran_nextSymbolId,
8119 | { "nextSymbolId", "oran_fh_cus.nextSymbolId",
8120 | FT_UINT8, BASE_DEC,
8121 | NULL((void*)0), 0x3c,
8122 | "offset of PRB range start", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8123 | },
8124 | /* 7.7.13.3 */
8125 | { &hf_oran_nextStartPrbc,
8126 | { "nextStartPrbc", "oran_fh_cus.nextStartPrbc",
8127 | FT_UINT16, BASE_DEC,
8128 | NULL((void*)0), 0x03ff,
8129 | "number of PRBs in PRB range", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8130 | },
8131 |
8132 | /* Puncturing patters as appears in SE 20 */
8133 | { &hf_oran_puncPattern,
8134 | { "puncPattern", "oran_fh_cus.puncPattern",
8135 | FT_STRING, BASE_NONE,
8136 | NULL((void*)0), 0x0,
8137 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8138 | },
8139 |
8140 | /* 7.7.20.2 numPuncPatterns */
8141 | { &hf_oran_numPuncPatterns,
8142 | { "numPuncPatterns", "oran_fh_cus.numPuncPatterns",
8143 | FT_UINT8, BASE_DEC,
8144 | NULL((void*)0), 0x0,
8145 | "number of puncturing patterns", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8146 | },
8147 | /* 7.7.20.3 symbolMask */
8148 | { &hf_oran_symbolMask_ext20,
8149 | { "symbolMask", "oran_fh_cus.symbolMask",
8150 | FT_UINT16, BASE_HEX,
8151 | NULL((void*)0), 0xfffc,
8152 | "Bitmask where each bit indicates the symbols associated with the puncturing pattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8153 | },
8154 | /* 7.7.20.4 startPuncPrb */
8155 | { &hf_oran_startPuncPrb,
8156 | { "startPuncPrb", "oran_fh_cus.startPuncPrb",
8157 | FT_UINT16, BASE_DEC,
8158 | NULL((void*)0), 0x03ff,
8159 | "starting PRB to which one puncturing pattern applies", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8160 | },
8161 | /* 7.7.20.5 numPuncPrb */
8162 | { &hf_oran_numPuncPrb,
8163 | { "numPuncPrb", "oran_fh_cus.numPuncPrb",
8164 | FT_UINT8, BASE_DEC,
8165 | NULL((void*)0), 0x0,
8166 | "the number of PRBs of the puncturing pattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8167 | },
8168 | /* 7.7.20.6 puncReMask */
8169 | { &hf_oran_puncReMask,
8170 | { "puncReMask", "oran_fh_cus.puncReMask",
8171 | FT_UINT16, BASE_DEC,
8172 | NULL((void*)0), 0xffc0,
8173 | "puncturing pattern RE mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8174 | },
8175 | /* 7.7.20.12 multiSDScope */
8176 | { &hf_oran_multiSDScope,
8177 | { "multiSDScope", "oran_fh_cus.multiSDScope",
8178 | FT_BOOLEAN, 8,
8179 | TFS(&multi_sd_scope_tfs)((0 ? (const struct true_false_string*)0 : ((&multi_sd_scope_tfs )))), 0x02,
8180 | "multiple section description scope flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8181 | },
8182 | /* 7.7.20.4 rbgIncl */
8183 | { &hf_oran_RbgIncl,
8184 | { "rbgIncl", "oran_fh_cus.rbgIncl",
8185 | FT_BOOLEAN, 8,
8186 | NULL((void*)0), 0x01,
8187 | "rbg included flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8188 | },
8189 |
8190 | /* 7.7.21.2 ciPrbGroupSize */
8191 | { &hf_oran_ci_prb_group_size,
8192 | { "ciPrbGroupSize", "oran_fh_cus.ciPrbGroupSize",
8193 | FT_UINT8, BASE_DEC,
8194 | NULL((void*)0), 0x0,
8195 | "channel information PRB group size", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8196 | },
8197 | /* 7.21.3 */
8198 | { &hf_oran_prg_size_st5,
8199 | { "prgSize", "oran_fh_cus.prgSize",
8200 | FT_UINT8, BASE_DEC,
8201 | VALS(prg_size_st5_vals)((0 ? (const struct _value_string*)0 : ((prg_size_st5_vals))) ), 0x03,
8202 | "precoding resource block group size", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8203 | },
8204 | { &hf_oran_prg_size_st6,
8205 | { "prgSize", "oran_fh_cus.prgSize",
8206 | FT_UINT8, BASE_DEC,
8207 | VALS(prg_size_st6_vals)((0 ? (const struct _value_string*)0 : ((prg_size_st6_vals))) ), 0x03,
8208 | "precoding resource block group size", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8209 | },
8210 |
8211 | /* 7.7.17.2 numUeID */
8212 | { &hf_oran_num_ueid,
8213 | { "numUeID", "oran_fh_cus.numUeID",
8214 | FT_UINT8, BASE_DEC,
8215 | NULL((void*)0), 0x0,
8216 | "number of ueIDs per user", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8217 | },
8218 |
8219 | /* 7.7.16.2 antMask */
8220 | { &hf_oran_antMask,
8221 | { "antMask", "oran_fh_cus.antMask",
8222 | FT_UINT64, BASE_HEX,
8223 | NULL((void*)0), 0xffffffffffffffff,
8224 | "indices of antennas to be pre-combined per RX endpoint", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8225 | },
8226 |
8227 | /* 7.7.18.2 transmissionWindowOffset */
8228 | { &hf_oran_transmissionWindowOffset,
8229 | { "transmissionWindowOffset", "oran_fh_cus.transmissionWindowOffset",
8230 | FT_UINT16, BASE_DEC,
8231 | NULL((void*)0), 0x0,
8232 | "start of the transmission window as an offset to when the transmission window would have been without this parameter, i.e. (Ta3_max - Ta3_min)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8233 | },
8234 | /* 7.7.18.3 transmissionWindowSize */
8235 | { &hf_oran_transmissionWindowSize,
8236 | { "transmissionWindowSize", "oran_fh_cus.transmissionWindowSize",
8237 | FT_UINT16, BASE_DEC,
8238 | NULL((void*)0), 0x3fff,
8239 | "size of the transmission window in resolution µs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8240 | },
8241 | /* 7.7.18.4 toT */
8242 | { &hf_oran_toT,
8243 | { "toT", "oran_fh_cus.toT",
8244 | FT_UINT8, BASE_DEC,
8245 | VALS(type_of_transmission_vals)((0 ? (const struct _value_string*)0 : ((type_of_transmission_vals )))), 0x03,
8246 | "type of transmission", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8247 | },
8248 |
8249 | /* 7.7.2.2 bfaCompHdr */
8250 | { &hf_oran_bfaCompHdr,
8251 | { "bfaCompHdr", "oran_fh_cus.bfaCompHdr",
8252 | FT_STRING, BASE_NONE,
8253 | NULL((void*)0), 0x0,
8254 | "beamforming attributes compression header", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8255 | },
8256 | /* 7.7.2.2-2: bfAzPtWidth */
8257 | { &hf_oran_bfAzPtWidth,
8258 | { "bfAzPtWidth", "oran_fh_cus.bfAzPtWidth",
8259 | FT_UINT8, BASE_DEC,
8260 | VALS(bfa_bw_vals)((0 ? (const struct _value_string*)0 : ((bfa_bw_vals)))), 0x38,
8261 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8262 | },
8263 | /* 7.7.2.2-3: bfZePtWidth */
8264 | { &hf_oran_bfZePtWidth,
8265 | { "bfZePtWidth", "oran_fh_cus.bfZePtWidth",
8266 | FT_UINT8, BASE_DEC,
8267 | VALS(bfa_bw_vals)((0 ? (const struct _value_string*)0 : ((bfa_bw_vals)))), 0x07,
8268 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8269 | },
8270 | /* 7.7.2.2-4: bfAz3ddWidth */
8271 | { &hf_oran_bfAz3ddWidth,
8272 | { "bfAz3ddWidth", "oran_fh_cus.bfAz3ddWidth",
8273 | FT_UINT8, BASE_DEC,
8274 | VALS(bfa_bw_vals)((0 ? (const struct _value_string*)0 : ((bfa_bw_vals)))), 0x38,
8275 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8276 | },
8277 | /* 7.7.2.2-5: bfZe3ddWidth */
8278 | { &hf_oran_bfZe3ddWidth,
8279 | { "bfZe3ddWidth", "oran_fh_cus.bfZe3ddWidth",
8280 | FT_UINT8, BASE_DEC,
8281 | VALS(bfa_bw_vals)((0 ? (const struct _value_string*)0 : ((bfa_bw_vals)))), 0x07,
8282 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8283 | },
8284 |
8285 | /* 7.7.2.3 bfAzPt */
8286 | { &hf_oran_bfAzPt,
8287 | { "bfAzPt", "oran_fh_cus.bfAzPt",
8288 | FT_UINT8, BASE_DEC,
8289 | NULL((void*)0), 0x0,
8290 | "beamforming azimuth pointing parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8291 | },
8292 | /* 7.7.2.4 bfZePt */
8293 | { &hf_oran_bfZePt,
8294 | { "bfZePt", "oran_fh_cus.bfZePt",
8295 | FT_UINT8, BASE_DEC,
8296 | NULL((void*)0), 0x0,
8297 | "beamforming zenith pointing parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8298 | },
8299 | /* 7.7.2.5 bfAz3dd */
8300 | { &hf_oran_bfAz3dd,
8301 | { "bfAz3dd", "oran_fh_cus.bfAz3dd",
8302 | FT_UINT8, BASE_DEC,
8303 | NULL((void*)0), 0x0,
8304 | "beamforming azimuth beamwidth parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8305 | },
8306 | /* 7.7.2.6 bfZe3dd */
8307 | { &hf_oran_bfZe3dd,
8308 | { "bfZe3dd", "oran_fh_cus.bfZe3dd",
8309 | FT_UINT8, BASE_DEC,
8310 | NULL((void*)0), 0x0,
8311 | "beamforming zenith beamwidth parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8312 | },
8313 |
8314 | /* 7.7.2.7 bfAzSl */
8315 | { &hf_oran_bfAzSl,
8316 | { "bfAzSl", "oran_fh_cus.bfAzSl",
8317 | FT_UINT8, BASE_DEC,
8318 | VALS(sidelobe_suppression_vals)((0 ? (const struct _value_string*)0 : ((sidelobe_suppression_vals )))), 0x38,
8319 | "beamforming azimuth sidelobe parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8320 | },
8321 | /* 7.7.2.8 bfZeSl */
8322 | { &hf_oran_bfZeSl,
8323 | { "bfZeSl", "oran_fh_cus.bfZeSl",
8324 | FT_UINT8, BASE_DEC,
8325 | VALS(sidelobe_suppression_vals)((0 ? (const struct _value_string*)0 : ((sidelobe_suppression_vals )))), 0x07,
8326 | "beamforming zenith sidelobe parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8327 | },
8328 |
8329 | /* 7.5.2.17 */
8330 | { &hf_oran_cmd_scope,
8331 | { "cmdScope", "oran_fh_cus.cmdScope",
8332 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8333 | RVALS(cmd_scope_vals)((0 ? (const struct _range_string*)0 : ((cmd_scope_vals)))), 0x0f,
8334 | "command scope", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8335 | },
8336 | /* 7.5.2.18 */
8337 | { &hf_oran_number_of_st4_cmds,
8338 | { "numberOfST4Cmds", "oran_fh_cus.numberOfST4Cmds",
8339 | FT_UINT8, BASE_DEC,
8340 | NULL((void*)0), 0x0,
8341 | "Number of Section Type 4 commands", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8342 | },
8343 |
8344 | { &hf_oran_st4_cmd_header,
8345 | { "Command common header", "oran_fh_cus.st4CmdCommonHeader",
8346 | FT_STRING, BASE_NONE,
8347 | NULL((void*)0), 0x0,
8348 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8349 | },
8350 |
8351 | /* 7.5.3.38 */
8352 | { &hf_oran_st4_cmd_type,
8353 | { "st4CmdType", "oran_fh_cus.st4CmdType",
8354 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8355 | RVALS(st4_cmd_type_vals)((0 ? (const struct _range_string*)0 : ((st4_cmd_type_vals))) ), 0x0,
8356 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8357 | },
8358 | /* 7.5.3.39 */
8359 | { &hf_oran_st4_cmd_len,
8360 | { "st4CmdLen", "oran_fh_cus.st4CmdLen",
8361 | FT_UINT16, BASE_DEC,
8362 | NULL((void*)0), 0x0,
8363 | "Length of command in 32-bit words", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8364 | },
8365 | /* 7.5.3.40 */
8366 | { &hf_oran_st4_cmd_num_slots,
8367 | { "numSlots", "oran_fh_cus.st4NumSlots",
8368 | FT_UINT8, BASE_DEC,
8369 | NULL((void*)0), 0x0,
8370 | "Contiguous slots for which command is applicable", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8371 | },
8372 | /* 7.5.3.41 */
8373 | { &hf_oran_st4_cmd_ack_nack_req_id,
8374 | { "ackNackReqId", "oran_fh_cus.ackNackReqId",
8375 | FT_UINT16, BASE_DEC,
8376 | NULL((void*)0), 0x0,
8377 | "ACK/NACK Request Id", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8378 | },
8379 |
8380 | { &hf_oran_st4_cmd,
8381 | { "Command", "oran_fh_cus.st4Cmd",
8382 | FT_STRING, BASE_NONE,
8383 | NULL((void*)0), 0x0,
8384 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8385 | },
8386 |
8387 | /* 7.5.3.52 */
8388 | { &hf_oran_sleepmode_trx,
8389 | { "sleepMode", "oran_fh_cus.sleepMode",
8390 | FT_UINT8, BASE_HEX,
8391 | VALS(sleep_mode_trx_vals)((0 ? (const struct _value_string*)0 : ((sleep_mode_trx_vals) ))), 0x03,
8392 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8393 | },
8394 | { &hf_oran_sleepmode_asm,
8395 | { "sleepMode", "oran_fh_cus.sleepMode",
8396 | FT_UINT8, BASE_HEX,
8397 | VALS(sleep_mode_asm_vals)((0 ? (const struct _value_string*)0 : ((sleep_mode_asm_vals) ))), 0x03,
8398 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8399 | },
8400 |
8401 | /* 7.5.3.51 */
8402 | { &hf_oran_log2maskbits,
8403 | { "log2MaskBits", "oran_fh_cus.log2MaskBits",
8404 | FT_UINT8, BASE_HEX,
8405 | VALS(log2maskbits_vals)((0 ? (const struct _value_string*)0 : ((log2maskbits_vals))) ), 0x3c,
8406 | "Number of bits to appear in antMask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8407 | },
8408 | /* 7.5.3.53 */
8409 | { &hf_oran_num_slots_ext,
8410 | { "numSlotsExt", "oran_fh_cus.numSlotsExt",
8411 | FT_UINT24, BASE_HEX,
8412 | NULL((void*)0), 0x0fffff,
8413 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8414 | },
8415 | /* 7.5.3.54 */
8416 | { &hf_oran_antMask_trx_control,
8417 | { "antMask", "oran_fh_cus.trxControl.antMask",
8418 | FT_BYTES, BASE_NONE,
8419 | NULL((void*)0), 0x0,
8420 | "which antennas should sleep or wake-up", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8421 | },
8422 | /* 7.5.3.55 */
8423 | { &hf_oran_ready,
8424 | { "ready", "oran_fh_cus.ready",
8425 | FT_BOOLEAN, 8,
8426 | TFS(&ready_tfs)((0 ? (const struct true_false_string*)0 : ((&ready_tfs)) )), 0x01,
8427 | "wake-up ready indicator", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8428 | },
8429 | /* 7.5.3.34 */
8430 | { &hf_oran_number_of_acks,
8431 | { "numberOfAcks", "oran_fh_cus.numberOfAcks",
8432 | FT_UINT8, BASE_DEC,
8433 | NULL((void*)0), 0x0,
8434 | "number of ACKs for one eAxC_ID", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8435 | },
8436 | /* 7.5.3.35 */
8437 | { &hf_oran_number_of_nacks,
8438 | { "numberOfNacks", "oran_fh_cus.numberOfNacks",
8439 | FT_UINT8, BASE_DEC,
8440 | NULL((void*)0), 0x0,
8441 | "number of NACKs for one eAxC_ID", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8442 | },
8443 | /* 7.5.3.36 */
8444 | { &hf_oran_ackid,
8445 | { "ackId", "oran_fh_cus.ackId",
8446 | FT_UINT16, BASE_DEC,
8447 | NULL((void*)0), 0x0,
8448 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8449 | },
8450 | /* 7.5.3.37 */
8451 | { &hf_oran_nackid,
8452 | { "nackId", "oran_fh_cus.nackId",
8453 | FT_UINT16, BASE_DEC,
8454 | NULL((void*)0), 0x0,
8455 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8456 | },
8457 |
8458 | /* Links between acknack requests & responses */
8459 | { &hf_oran_acknack_request_frame,
8460 | { "Request Frame", "oran_fh_cus.ackNackId.request-frame",
8461 | FT_FRAMENUM, BASE_NONE,
8462 | FRAMENUM_TYPE(FT_FRAMENUM_REQUEST)((gpointer) (glong) (FT_FRAMENUM_REQUEST)), 0x0,
8463 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8464 | },
8465 | { &hf_oran_acknack_request_time,
8466 | { "Time since request in ms", "oran_fh_cus.ackNackId.time-since-request",
8467 | FT_UINT32, BASE_DEC,
8468 | NULL((void*)0), 0x0,
8469 | "Time between request and response", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8470 | },
8471 | { &hf_oran_acknack_request_type,
8472 | { "Request Type", "oran_fh_cus.ackNackId.request-type",
8473 | FT_UINT32, BASE_DEC,
8474 | VALS(acknack_type_vals)((0 ? (const struct _value_string*)0 : ((acknack_type_vals))) ), 0x0,
8475 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8476 | },
8477 | { &hf_oran_acknack_response_frame,
8478 | { "Response Frame", "oran_fh_cus.ackNackId.response-frame",
8479 | FT_FRAMENUM, BASE_NONE,
8480 | FRAMENUM_TYPE(FT_FRAMENUM_RESPONSE)((gpointer) (glong) (FT_FRAMENUM_RESPONSE)), 0x0,
8481 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8482 | },
8483 | { &hf_oran_acknack_response_time,
8484 | { "Time to response in ms", "oran_fh_cus.ackNackId.time-to-response",
8485 | FT_UINT32, BASE_DEC,
8486 | NULL((void*)0), 0x0,
8487 | "Time between request and response", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8488 | },
8489 |
8490 | /* 7.5.3.43 */
8491 | { &hf_oran_disable_tdbfns,
8492 | { "disableTDBFNs", "oran_fh_cus.disableTDBFNs",
8493 | FT_BOOLEAN, 8,
8494 | TFS(&disable_tdbfns_tfs)((0 ? (const struct true_false_string*)0 : ((&disable_tdbfns_tfs )))), 0x80,
8495 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8496 | },
8497 |
8498 | /* 7.5.3.44 */
8499 | { &hf_oran_td_beam_group,
8500 | { "tdBeamGrp", "oran_fh_cus.tdBeamGrp",
8501 | FT_UINT16, BASE_HEX,
8502 | NULL((void*)0), 0x7fff,
8503 | "Applies to symbolMask in command header", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8504 | },
8505 | /* 7.5.3.43 */
8506 | { &hf_oran_disable_tdbfws,
8507 | { "disableTDBFWs", "oran_fh_cus.disableTDBFWs",
8508 | FT_BOOLEAN, 8,
8509 | TFS(&beam_numbers_included_tfs)((0 ? (const struct true_false_string*)0 : ((&beam_numbers_included_tfs )))), 0x80,
8510 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8511 | },
8512 |
8513 | /* 7.5.3.56 */
8514 | { &hf_oran_td_beam_num,
8515 | { "tdBeamNum", "oran_fh_cus.tdBeamNum",
8516 | FT_UINT16, BASE_HEX,
8517 | NULL((void*)0), 0x7fff,
8518 | "time-domain beam number", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8519 | },
8520 |
8521 | /* 7.5.3.49 */
8522 | { &hf_oran_dir_pattern,
8523 | { "dirPattern", "oran_fh_cus.dirPattern",
8524 | FT_BOOLEAN, 16,
8525 | TFS(&symbol_direction_tfs)((0 ? (const struct true_false_string*)0 : ((&symbol_direction_tfs )))), 0x3fff,
8526 | "symbol data direction (gNB Tx/Rx) pattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8527 | },
8528 | /* 7.5.3.50 */
8529 | { &hf_oran_guard_pattern,
8530 | { "guardPattern", "oran_fh_cus.guardPattern",
8531 | FT_BOOLEAN, 16,
8532 | TFS(&symbol_guard_tfs)((0 ? (const struct true_false_string*)0 : ((&symbol_guard_tfs )))), 0x3fff,
8533 | "guard pattern bitmask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8534 | },
8535 |
8536 | /* For convenient filtering */
8537 | { &hf_oran_cplane,
8538 | { "C-Plane", "oran_fh_cus.c-plane",
8539 | FT_NONE, BASE_NONE,
8540 | NULL((void*)0), 0x0,
8541 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8542 | },
8543 | { &hf_oran_uplane,
8544 | { "U-Plane", "oran_fh_cus.u-plane",
8545 | FT_NONE, BASE_NONE,
8546 | NULL((void*)0), 0x0,
8547 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8548 | },
8549 | { &hf_oran_bf,
8550 | { "BeamForming", "oran_fh_cus.bf",
8551 | FT_NONE, BASE_NONE,
8552 | NULL((void*)0), 0x0,
8553 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8554 | },
8555 | { &hf_oran_zero_prb,
8556 | { "Zero PRB", "oran_fh_cus.zero-prb",
8557 | FT_NONE, BASE_NONE,
8558 | NULL((void*)0), 0x0,
8559 | "All of the REs in this PRB are zero", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8560 | },
8561 |
8562 | /* 5.1.3.2.7 */
8563 | { &hf_oran_ecpri_pcid,
8564 | { "ecpriPcid", "oran_fh_cus.ecpriPcid",
8565 | FT_NONE, BASE_NONE,
8566 | NULL((void*)0), 0x0,
8567 | "IQ data transfer message series identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8568 | },
8569 | { &hf_oran_ecpri_rtcid,
8570 | { "ecpriRtcid", "oran_fh_cus.ecpriRtcid",
8571 | FT_NONE, BASE_NONE,
8572 | NULL((void*)0), 0x0,
8573 | "Real time control data identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8574 | },
8575 | /* 5.1.3.2.8 */
8576 | { &hf_oran_ecpri_seqid,
8577 | { "ecpriSeqid", "oran_fh_cus.ecpriSeqid",
8578 | FT_NONE, BASE_NONE,
8579 | NULL((void*)0), 0x0,
8580 | "message identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8581 | },
8582 |
8583 | /* 7.7.23.2 */
8584 | { &hf_oran_num_sym_prb_pattern,
8585 | { "numSymPrbPattern", "oran_fh_cus.numSymPrbPattern",
8586 | FT_UINT8, BASE_DEC,
8587 | NULL((void*)0), 0xf0,
8588 | "number of symbol and resource block patterns", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8589 | },
8590 | /* 7.7.23.11 */
8591 | { &hf_oran_prb_mode,
8592 | { "prbMode", "oran_fh_cus.prbMode",
8593 | FT_BOOLEAN, 8,
8594 | TFS(&prb_mode_tfs)((0 ? (const struct true_false_string*)0 : ((&prb_mode_tfs )))), 0x01,
8595 | "PRB Mode", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8596 | },
8597 |
8598 | { &hf_oran_sym_prb_pattern,
8599 | { "symPrbPattern", "oran_fh_cus.symPrbPattern",
8600 | FT_STRING, BASE_NONE,
8601 | NULL((void*)0), 0x0,
8602 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8603 | },
8604 |
8605 | /* 7.7.23.3 */
8606 | { &hf_oran_sym_mask,
8607 | { "symMask", "oran_fh_cus.symMask",
8608 | FT_UINT16, BASE_HEX,
8609 | NULL((void*)0), 0x3fff,
8610 | "symbol mask part of symPrbPattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8611 | },
8612 | /* 7.7.23.5 */
8613 | {&hf_oran_num_mc_scale_offset,
8614 | {"numMcScaleOffset", "oran_fh_cus.numMcScaleOffset",
8615 | FT_UINT8, BASE_DEC,
8616 | NULL((void*)0), 0xf0,
8617 | "number of modulation compression scaling value per symPrbPattern",
8618 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8619 | },
8620 | /* 7.7.23.4 */
8621 | { &hf_oran_prb_pattern,
8622 | { "prbPattern", "oran_fh_cus.prbPattern",
8623 | FT_UINT8, BASE_DEC,
8624 | NULL((void*)0), 0x0f,
8625 | "resource block pattern part of symPrbPattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8626 | },
8627 |
8628 | /* 7.7.3.2 */
8629 | { &hf_oran_codebook_index,
8630 | { "codebookIndex", "oran_fh_cus.codebookIndex",
8631 | FT_UINT8, BASE_DEC,
8632 | NULL((void*)0), 0x0,
8633 | "precoder codebook used for transmission", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8634 | },
8635 | /* 7.7.3.3 */
8636 | { &hf_oran_layerid,
8637 | { "layerID", "oran_fh_cus.layerID",
8638 | FT_UINT8, BASE_DEC,
8639 | NULL((void*)0), 0xf0,
8640 | "Layer ID for DL transmission", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8641 | },
8642 | /* 7.7.3.5 */
8643 | { &hf_oran_numlayers,
8644 | { "numLayers", "oran_fh_cus.numLayers",
8645 | FT_UINT8, BASE_DEC,
8646 | NULL((void*)0), 0x0f,
8647 | "number of layers for DL transmission", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8648 | },
8649 | /* 7.7.3.4 */
8650 | { &hf_oran_txscheme,
8651 | { "txScheme", "oran_fh_cus.txScheme",
8652 | FT_UINT8, BASE_DEC,
8653 | NULL((void*)0), 0xf0,
8654 | "transmission scheme", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8655 | },
8656 | /* 7.7.3.6 */
8657 | { &hf_oran_crs_remask,
8658 | { "crsReMask", "oran_fh_cus.crsReMask",
8659 | FT_UINT16, BASE_HEX,
8660 | NULL((void*)0), 0x0fff,
8661 | "CRS resource element mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8662 | },
8663 | /* 7.7.3.8 */
8664 | { &hf_oran_crs_shift,
8665 | { "crsShift", "oran_fh_cus.crsShift",
8666 | FT_UINT8, BASE_HEX,
8667 | NULL((void*)0), 0x80,
8668 | "CRS resource element mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8669 | },
8670 | /* 7.7.3.7 */
8671 | { &hf_oran_crs_symnum,
8672 | { "crsSymNum", "oran_fh_cus.crsSymNum",
8673 | FT_UINT8, BASE_DEC,
8674 | NULL((void*)0), 0x0f,
8675 | "CRS symbol number indication", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8676 | },
8677 | /* 7.7.3.9 */
8678 | { &hf_oran_beamid_ap1,
8679 | { "beamIdAP1", "oran_fh_cus.beamIdAP1",
8680 | FT_UINT16, BASE_DEC,
8681 | NULL((void*)0), 0x7f,
8682 | "beam id to be used for antenna port 1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8683 | },
8684 | /* 7.7.3.10 */
8685 | { &hf_oran_beamid_ap2,
8686 | { "beamIdAP2", "oran_fh_cus.beamIdAP2",
8687 | FT_UINT16, BASE_DEC,
8688 | NULL((void*)0), 0x7f,
8689 | "beam id to be used for antenna port 2", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8690 | },
8691 | /* 7.7.3.11 */
8692 | { &hf_oran_beamid_ap3,
8693 | { "beamIdAP3", "oran_fh_cus.beamIdAP3",
8694 | FT_UINT16, BASE_DEC,
8695 | NULL((void*)0), 0x7f,
8696 | "beam id to be used for antenna port 3", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8697 | },
8698 |
8699 | /* 7.7.10.3a */
8700 | { &hf_oran_port_list_index,
8701 | { "portListIndex", "oran_fh_cus.portListIndex",
8702 | FT_UINT8, BASE_DEC,
8703 | NULL((void*)0), 0x0,
8704 | "the index of an eAxC_ID in the port-list", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8705 | },
8706 |
8707 | { &hf_oran_alpn_per_sym,
8708 | { "alpnPerSym", "oran_fh_cus.alpnPerSym",
8709 | FT_UINT8, BASE_HEX,
8710 | VALS(alpn_per_sym_vals)((0 ? (const struct _value_string*)0 : ((alpn_per_sym_vals))) ), 0x80,
8711 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8712 | },
8713 | { &hf_oran_ant_dmrs_snr,
8714 | { "antDmrsSnr", "oran_fh_cus.antDmrsSnr",
8715 | FT_UINT8, BASE_HEX,
8716 | VALS(ant_dmrs_snr_vals)((0 ? (const struct _value_string*)0 : ((ant_dmrs_snr_vals))) ), 0x40,
8717 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8718 | },
8719 |
8720 | /* 7.7.24.6 */
8721 | { &hf_oran_user_group_size,
8722 | { "userGroupSize", "oran_fh_cus.userGroupSize",
8723 | FT_UINT8, BASE_DEC,
8724 | NULL((void*)0), 0x1f,
8725 | "number of UE data layers in the user group identified by userGroupId", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8726 | },
8727 | /* 7.7.24.7 */
8728 | { &hf_oran_user_group_id,
8729 | { "userGroupId", "oran_fh_cus.userGroupId",
8730 | FT_UINT8, BASE_DEC,
8731 | NULL((void*)0), 0x0,
8732 | "indicates user group described by the section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8733 | },
8734 | /* 7.7.24.8 */
8735 | { &hf_oran_entry_type,
8736 | { "entryType", "oran_fh_cus.entryType",
8737 | FT_UINT8, BASE_DEC,
8738 | VALS(entry_type_vals)((0 ? (const struct _value_string*)0 : ((entry_type_vals)))), 0xe0,
8739 | "indicates format of the entry", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8740 | },
8741 | /* 7.7.24.9 */
8742 | { &hf_oran_dmrs_port_number,
8743 | { "dmrsPortNumber", "oran_fh_cus.dmrsPortNumber",
8744 | FT_UINT8, BASE_DEC,
8745 | NULL((void*)0), 0x1f,
8746 | "DMRS antenna port number for the associated ueId", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8747 | },
8748 | /* 7.7.24.10 */
8749 | { &hf_oran_ueid_reset,
8750 | { "ueidReset", "oran_fh_cus.ueidReset",
8751 | FT_BOOLEAN, 8,
8752 | TFS(&tfs_ueid_reset)((0 ? (const struct true_false_string*)0 : ((&tfs_ueid_reset )))), 0x80,
8753 | "same UEID as the previous slot", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8754 | },
8755 | /* 7.7.24.11 */
8756 | { &hf_oran_dmrs_symbol_mask,
8757 | { "dmrsSymbolMask", "oran_fh_cus.dmrsSymbolMask",
8758 | FT_UINT16, BASE_HEX,
8759 | NULL((void*)0), 0x3fff,
8760 | "symbols within the slot containing DMRS", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8761 | },
8762 | { &hf_oran_dmrs_symbol_mask_s13,
8763 | { "symbol 13", "oran_fh_cus.dmrsSymbolMask.symbol-13",
8764 | FT_BOOLEAN, 16,
8765 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x2000,
8766 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8767 | },
8768 | { &hf_oran_dmrs_symbol_mask_s12,
8769 | { "symbol 12", "oran_fh_cus.dmrsSymbolMask.symbol-12",
8770 | FT_BOOLEAN, 16,
8771 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x1000,
8772 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8773 | },
8774 | { &hf_oran_dmrs_symbol_mask_s11,
8775 | { "symbol 11", "oran_fh_cus.dmrsSymbolMask.symbol-11",
8776 | FT_BOOLEAN, 16,
8777 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0800,
8778 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8779 | },
8780 | { &hf_oran_dmrs_symbol_mask_s10,
8781 | { "symbol 10", "oran_fh_cus.dmrsSymbolMask.symbol-10",
8782 | FT_BOOLEAN, 16,
8783 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0400,
8784 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8785 | },
8786 | { &hf_oran_dmrs_symbol_mask_s9,
8787 | { "symbol 9", "oran_fh_cus.dmrsSymbolMask.symbol-9",
8788 | FT_BOOLEAN, 16,
8789 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0200,
8790 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8791 | },
8792 | { &hf_oran_dmrs_symbol_mask_s8,
8793 | { "symbol 8", "oran_fh_cus.dmrsSymbolMask.symbol-8",
8794 | FT_BOOLEAN, 16,
8795 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0100,
8796 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8797 | },
8798 | { &hf_oran_dmrs_symbol_mask_s7,
8799 | { "symbol 7", "oran_fh_cus.dmrsSymbolMask.symbol-7",
8800 | FT_BOOLEAN, 16,
8801 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0080,
8802 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8803 | },
8804 | { &hf_oran_dmrs_symbol_mask_s6,
8805 | { "symbol 6", "oran_fh_cus.dmrsSymbolMask.symbol-6",
8806 | FT_BOOLEAN, 16,
8807 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0040,
8808 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8809 | },
8810 | { &hf_oran_dmrs_symbol_mask_s5,
8811 | { "symbol 5", "oran_fh_cus.dmrsSymbolMask.symbol-5",
8812 | FT_BOOLEAN, 16,
8813 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0020,
8814 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8815 | },
8816 | { &hf_oran_dmrs_symbol_mask_s4,
8817 | { "symbol 4", "oran_fh_cus.dmrsSymbolMask.symbol-4",
8818 | FT_BOOLEAN, 16,
8819 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0010,
8820 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8821 | },
8822 | { &hf_oran_dmrs_symbol_mask_s3,
8823 | { "symbol 3", "oran_fh_cus.dmrsSymbolMask.symbol-3",
8824 | FT_BOOLEAN, 16,
8825 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0008,
8826 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8827 | },
8828 | { &hf_oran_dmrs_symbol_mask_s2,
8829 | { "symbol 2", "oran_fh_cus.dmrsSymbolMask.symbol-2",
8830 | FT_BOOLEAN, 16,
8831 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0004,
8832 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8833 | },
8834 | { &hf_oran_dmrs_symbol_mask_s1,
8835 | { "symbol 1", "oran_fh_cus.dmrsSymbolMask.symbol-1",
8836 | FT_BOOLEAN, 16,
8837 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0002,
8838 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8839 | },
8840 | { &hf_oran_dmrs_symbol_mask_s0,
8841 | { "symbol 0", "oran_fh_cus.dmrsSymbolMask.symbol-0",
8842 | FT_BOOLEAN, 16,
8843 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0001,
8844 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8845 | },
8846 |
8847 | /* 7.7.24.12 */
8848 | { &hf_oran_scrambling,
8849 | { "scrambling", "oran_fh_cus.scrambling",
8850 | FT_UINT16, BASE_HEX,
8851 | NULL((void*)0), 0x0,
8852 | "used to calculate the seed value required to initialize pseudo-random generator", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8853 | },
8854 | /* 7.7.24.13 */
8855 | { &hf_oran_nscid,
8856 | { "nscid", "oran_fh_cus.nscid",
8857 | FT_UINT8, BASE_HEX,
8858 | NULL((void*)0), 0x80,
8859 | "used to calculate the seed value for pseudo-random generator", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8860 | },
8861 | /* 7.7.24.14 */
8862 | { &hf_oran_dtype,
8863 | { "dType", "oran_fh_cus.dType",
8864 | FT_UINT8, BASE_HEX,
8865 | VALS(dtype_vals)((0 ? (const struct _value_string*)0 : ((dtype_vals)))), 0x40,
8866 | "PUSCH DMRS configuration type", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8867 | },
8868 | /* 7.7.24.15 */
8869 | { &hf_oran_cmd_without_data,
8870 | { "cmdWithoutData", "oran_fh_cus.cmdWithoutData",
8871 | FT_UINT8, BASE_HEX,
8872 | NULL((void*)0), 0x30,
8873 | "number of DMRS CDM groups without data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8874 | },
8875 | /* 7.7.24.16 */
8876 | { &hf_oran_lambda,
8877 | { "lambda", "oran_fh_cus.lambda",
8878 | FT_UINT8, BASE_HEX,
8879 | NULL((void*)0), 0x0c,
8880 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8881 | },
8882 | /* 7.7.24.19 */
8883 | { &hf_oran_first_prb,
8884 | { "firstPrb", "oran_fh_cus.firstPrb",
8885 | FT_UINT16, BASE_DEC,
8886 | NULL((void*)0), 0x03fe,
8887 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8888 | },
8889 | /* 7.7.24.20 */
8890 | { &hf_oran_last_prb,
8891 | { "lastPrb", "oran_fh_cus.lastPrb",
8892 | FT_UINT16, BASE_DEC,
8893 | NULL((void*)0), 0x01ff,
8894 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8895 | },
8896 |
8897 | /* 7.7.24.17 */
8898 | /* TODO: add value_string */
8899 | { &hf_oran_low_papr_type,
8900 | { "lowPaprType", "oran_fh_cus.lowPaprType",
8901 | FT_UINT8, BASE_HEX,
8902 | VALS(papr_type_vals)((0 ? (const struct _value_string*)0 : ((papr_type_vals)))), 0x30,
8903 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8904 | },
8905 | /* 7.7.24.18 */
8906 | { &hf_oran_hopping_mode,
8907 | { "hoppingMode", "oran_fh_cus.hoppingMode",
8908 | FT_UINT8, BASE_HEX,
8909 | VALS(hopping_mode_vals)((0 ? (const struct _value_string*)0 : ((hopping_mode_vals))) ), 0x0c,
8910 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8911 | },
8912 |
8913 | { &hf_oran_tx_win_for_on_air_symbol_l,
8914 | { "txWinForOnAirSymbol", "oran_fh_cus.txWinForOnAirSymbol",
8915 | FT_UINT8, BASE_DEC,
8916 | NULL((void*)0), 0xf0,
8917 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8918 | },
8919 | { &hf_oran_tx_win_for_on_air_symbol_r,
8920 | { "txWinForOnAirSymbol", "oran_fh_cus.txWinForOnAirSymbol",
8921 | FT_UINT8, BASE_DEC,
8922 | NULL((void*)0), 0x0f,
8923 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8924 | },
8925 | /* 7.7.26.2 */
8926 | { &hf_oran_num_fo_fb,
8927 | { "numFoFb", "oran_fh_cus.numFoFb",
8928 | FT_UINT8, BASE_DEC,
8929 | NULL((void*)0), 0x7f,
8930 | "number of frequency offset feedback", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8931 | },
8932 | /* 7.7.26.3 */
8933 | { &hf_oran_freq_offset_fb,
8934 | { "freqOffsetFb", "oran_fh_cus.freqOffsetFb",
8935 | FT_UINT16, BASE_HEX_DEC | BASE_RANGE_STRING0x00000100,
8936 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
8937 | "UE frequency offset feedback", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8938 | },
8939 |
8940 | /* 7.7.28.2 */
8941 | { &hf_oran_num_ue_sinr_rpt,
8942 | { "numUeSinrRpt", "oran_fh_cus.numUeSinrRpt",
8943 | FT_UINT8, BASE_DEC,
8944 | NULL((void*)0), 0x1f,
8945 | "number of sinr reported UEs {1 - 12}", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8946 | },
8947 |
8948 | /* 7.5.2.19 */
8949 | { &hf_oran_num_sinr_per_prb,
8950 | { "numSinrPerPrb", "oran_fh_cus.numSinrPerPrb",
8951 | FT_UINT8, BASE_DEC,
8952 | VALS(num_sinr_per_prb_vals)((0 ? (const struct _value_string*)0 : ((num_sinr_per_prb_vals )))), 0x70,
8953 | "number of SINR values per PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8954 | },
8955 | { &hf_oran_num_sinr_per_prb_right,
8956 | { "numSinrPerPrb", "oran_fh_cus.numSinrPerPrb",
8957 | FT_UINT8, BASE_DEC,
8958 | VALS(num_sinr_per_prb_vals)((0 ? (const struct _value_string*)0 : ((num_sinr_per_prb_vals )))), 0x07,
8959 | "number of SINR values per PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8960 | },
8961 |
8962 | /* 7.5.3.68 */
8963 | { &hf_oran_sinr_value,
8964 | { "sinrValue", "oran_fh_cus.sinrValue",
8965 | FT_FLOAT, BASE_NONE,
8966 | NULL((void*)0), 0x0,
8967 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8968 | },
8969 |
8970 | { &hf_oran_measurement_report,
8971 | { "Measurement Report", "oran_fh_cus.measurement-report",
8972 | FT_STRING, BASE_NONE,
8973 | NULL((void*)0), 0x0,
8974 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8975 | },
8976 | /* 7.5.3.57 */
8977 | { &hf_oran_mf,
8978 | { "mf", "oran_fh_cus.mf",
8979 | FT_BOOLEAN, 8,
8980 | TFS(&measurement_flag_tfs)((0 ? (const struct true_false_string*)0 : ((&measurement_flag_tfs )))), 0x80,
8981 | "measurement flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8982 | },
8983 | /* 7.5.3.59 */
8984 | { &hf_oran_meas_data_size,
8985 | { "measDataSize", "oran_fh_cus.measDataSize",
8986 | FT_UINT16, BASE_DEC,
8987 | NULL((void*)0), 0x0,
8988 | "measurement data size (in words)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8989 | },
8990 |
8991 | /* 7.5.3.58 */
8992 | { &hf_oran_meas_type_id,
8993 | { "measTypeId", "oran_fh_cus.measTypeId",
8994 | FT_UINT8, BASE_DEC,
8995 | VALS(meas_type_id_vals)((0 ? (const struct _value_string*)0 : ((meas_type_id_vals))) ), 0x7F,
8996 | "measurement report type identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8997 | },
8998 | /* 7.5.3.66 */
8999 | { &hf_oran_num_elements,
9000 | { "numElements", "oran_fh_cus.numElements",
9001 | FT_UINT8, BASE_DEC,
9002 | NULL((void*)0), 0x0,
9003 | "measurement report type identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9004 | },
9005 | /* 7.5.3.60 */
9006 | { &hf_oran_ue_tae,
9007 | { "ueTae", "oran_fh_cus.ueTae",
9008 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
9009 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
9010 | "UE Timing Advance Error", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9011 | },
9012 | /* 7.5.3.61 */
9013 | { &hf_oran_ue_layer_power,
9014 | { "ueLayerPower", "oran_fh_cus.ueLayerPower",
9015 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
9016 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
9017 | "UE Layer Power", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9018 | },
9019 |
9020 | /* 7.5.3.62 */
9021 | { &hf_oran_ue_freq_offset,
9022 | { "ueFreqOffset", "oran_fh_cus.ueFreqOffset",
9023 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
9024 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
9025 | "UE frequency offset", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9026 | },
9027 | /* 7.5.3.63 */
9028 | { &hf_oran_ipn_power,
9029 | { "ipnPower", "oran_fh_cus.ipnPower",
9030 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
9031 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
9032 | "Interference plus Noise power", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9033 | },
9034 | /* 7.5.3.64 */
9035 | { &hf_oran_ant_dmrs_snr_val,
9036 | { "antDmrsSnrVal", "oran_fh_cus.antDmrsSnrVal",
9037 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
9038 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
9039 | "antenna DMRS-SNR", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9040 | },
9041 |
9042 | { &hf_oran_measurement_command,
9043 | { "Measurement Command", "oran_fh_cus.measurement-command",
9044 | FT_STRING, BASE_NONE,
9045 | NULL((void*)0), 0x0,
9046 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9047 | },
9048 |
9049 | /* 7.5.27.2 */
9050 | { &hf_oran_beam_type,
9051 | {"beamType", "oran_fh_cus.beamType",
9052 | FT_UINT16, BASE_DEC,
9053 | VALS(beam_type_vals)((0 ? (const struct _value_string*)0 : ((beam_type_vals)))), 0xc0,
9054 | NULL((void*)0),
9055 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9056 | },
9057 | /* 7.5.3.65 */
9058 | { &hf_oran_meas_cmd_size,
9059 | {"measCmdSize", "oran_fh_cus.measCmdSize",
9060 | FT_UINT16, BASE_DEC,
9061 | NULL((void*)0), 0x0,
9062 | "measurement command size in words",
9063 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9064 | },
9065 |
9066 | { &hf_oran_symbol_reordering_layer,
9067 | { "Layer", "oran_fh_cus.layer",
9068 | FT_STRING, BASE_NONE,
9069 | NULL((void*)0), 0x0,
9070 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9071 | },
9072 | { &hf_oran_dmrs_entry,
9073 | { "Entry", "oran_fh_cus.dmrs-entry",
9074 | FT_STRING, BASE_NONE,
9075 | NULL((void*)0), 0x0,
9076 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9077 | },
9078 |
9079 | { &hf_oran_c_section_common,
9080 | { "Common Section", "oran_fh_cus.c-plane.section.common",
9081 | FT_STRING, BASE_NONE,
9082 | NULL((void*)0), 0x0,
9083 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9084 | },
9085 | { &hf_oran_c_section,
9086 | { "Section", "oran_fh_cus.c-plane.section",
9087 | FT_STRING, BASE_NONE,
9088 | NULL((void*)0), 0x0,
9089 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9090 | },
9091 | { &hf_oran_u_section,
9092 | { "Section", "oran_fh_cus.u-plane.section",
9093 | FT_STRING, BASE_NONE,
9094 | NULL((void*)0), 0x0,
9095 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9096 | },
9097 |
9098 | /* Link back to UL C-plane where udCompHdr was recorded */
9099 | { &hf_oran_ul_cplane_ud_comp_hdr_frame,
9100 | { "C-Plane UL udCompHdr frame", "oran_fh_cus.ul-cplane.udCompHdr",
9101 | FT_FRAMENUM, BASE_NONE,
9102 | FRAMENUM_TYPE(FT_FRAMENUM_REQUEST)((gpointer) (glong) (FT_FRAMENUM_REQUEST)), 0x0,
9103 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9104 | },
9105 | };
9106 |
9107 | /* Setup protocol subtree array */
9108 | static int *ett[] = {
9109 | &ett_oran,
9110 | &ett_oran_ecpri_pcid,
9111 | &ett_oran_ecpri_rtcid,
9112 | &ett_oran_ecpri_seqid,
9113 | &ett_oran_section_type,
9114 | &ett_oran_u_timing,
9115 | &ett_oran_u_section,
9116 | &ett_oran_u_prb,
9117 | &ett_oran_section,
9118 | &ett_oran_iq,
9119 | &ett_oran_bfw_bundle,
9120 | &ett_oran_bfw,
9121 | &ett_oran_frequency_range,
9122 | &ett_oran_prb_cisamples,
9123 | &ett_oran_cisample,
9124 | &ett_oran_udcomphdr,
9125 | &ett_oran_udcompparam,
9126 | &ett_oran_cicomphdr,
9127 | &ett_oran_cicompparam,
9128 | &ett_oran_bfwcomphdr,
9129 | &ett_oran_bfwcompparam,
9130 | &ett_oran_ext19_port,
9131 | &ett_oran_prb_allocation,
9132 | &ett_oran_punc_pattern,
9133 | &ett_oran_bfacomphdr,
9134 | &ett_oran_modcomp_param_set,
9135 | &ett_oran_st4_cmd_header,
9136 | &ett_oran_st4_cmd,
9137 | &ett_oran_sym_prb_pattern,
9138 | &ett_oran_measurement_report,
9139 | &ett_oran_measurement_command,
9140 | &ett_oran_sresmask,
9141 | &ett_oran_c_section_common,
9142 | &ett_oran_c_section,
9143 | &ett_oran_remask,
9144 | &ett_oran_symbol_reordering_layer,
9145 | &ett_oran_dmrs_entry,
9146 | &ett_oran_dmrs_symbol_mask,
9147 | &ett_oran_symbol_mask,
9148 | &ett_active_beamspace_coefficient_mask
9149 | };
9150 |
9151 | static int *ext_ett[HIGHEST_EXTTYPE28];
9152 | for (unsigned extno=0; extno<HIGHEST_EXTTYPE28; extno++) {
9153 | ext_ett[extno] = &ett_oran_c_section_extension[extno];
9154 | }
9155 |
9156 | expert_module_t* expert_oran;
9157 |
9158 | static ei_register_info ei[] = {
9159 | { &ei_oran_unsupported_bfw_compression_method, { "oran_fh_cus.unsupported_bfw_compression_method", PI_UNDECODED0x05000000, PI_WARN0x00600000, "Unsupported BFW Compression Method", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9160 | { &ei_oran_invalid_sample_bit_width, { "oran_fh_cus.invalid_sample_bit_width", PI_UNDECODED0x05000000, PI_ERROR0x00800000, "Unsupported sample bit width", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9161 | { &ei_oran_reserved_numBundPrb, { "oran_fh_cus.reserved_numBundPrb", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "Reserved value of numBundPrb", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9162 | { &ei_oran_extlen_wrong, { "oran_fh_cus.extlen_wrong", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "extlen doesn't match number of dissected bytes", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9163 | { &ei_oran_invalid_eaxc_bit_width, { "oran_fh_cus.invalid_eaxc_bit_width", PI_UNDECODED0x05000000, PI_ERROR0x00800000, "Inconsistent eAxC bit width", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9164 | { &ei_oran_extlen_zero, { "oran_fh_cus.extlen_zero", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "extlen - zero is reserved value", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9165 | { &ei_oran_rbg_size_reserved, { "oran_fh_cus.rbg_size_reserved", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "rbgSize - zero is reserved value", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9166 | { &ei_oran_frame_length, { "oran_fh_cus.frame_length", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "there should be 0-3 bytes remaining after PDU in frame", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9167 | { &ei_oran_numprbc_ext21_zero, { "oran_fh_cus.numprbc_ext21_zero", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "numPrbc shall not be set to 0 when ciPrbGroupSize is configured", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9168 | { &ei_oran_ci_prb_group_size_reserved, { "oran_fh_cus.ci_prb_group_size_reserved", PI_MALFORMED0x07000000, PI_WARN0x00600000, "ciPrbGroupSize should be 2-254", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9169 | { &ei_oran_st8_nackid, { "oran_fh_cus.st8_nackid", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "operation for this ackId failed", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9170 | { &ei_oran_st4_no_cmds, { "oran_fh_cus.st4_nackid", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "Not valid to have no commands in ST4", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9171 | { &ei_oran_st4_zero_len_cmd, { "oran_fh_cus.st4_zero_len_cmd", PI_MALFORMED0x07000000, PI_WARN0x00600000, "ST4 cmd with length 0 is reserved", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9172 | { &ei_oran_st4_wrong_len_cmd, { "oran_fh_cus.st4_wrong_len_cmd", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "ST4 cmd with length not matching contents", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9173 | { &ei_oran_st4_unknown_cmd, { "oran_fh_cus.st4_unknown_cmd", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "ST4 cmd with unknown command code", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9174 | { &ei_oran_mcot_out_of_range, { "oran_fh_cus.mcot_out_of_range", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "MCOT should be 1-10", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9175 | { &ei_oran_se10_unknown_beamgrouptype, { "oran_fh_cus.se10_unknown_beamgrouptype", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE10 - unknown BeamGroupType value", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9176 | { &ei_oran_se10_not_allowed, { "oran_fh_cus.se10_not_allowed", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE10 - type not allowed for sectionType", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9177 | { &ei_oran_start_symbol_id_not_zero, { "oran_fh_cus.startsymbolid_shall_be_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "For ST4 commands 3&4, startSymbolId shall be 0", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9178 | { &ei_oran_trx_control_cmd_scope, { "oran_fh_cus.trx_command.bad_cmdscope", PI_MALFORMED0x07000000, PI_WARN0x00600000, "TRX command must have cmdScope of ARRAY-COMMAND", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9179 | { &ei_oran_unhandled_se, { "oran_fh_cus.se_not_handled", PI_UNDECODED0x05000000, PI_WARN0x00600000, "SE not recognised/handled by dissector", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9180 | { &ei_oran_bad_symbolmask, { "oran_fh_cus.bad_symbol_mask", PI_MALFORMED0x07000000, PI_WARN0x00600000, "For non-zero sleepMode, symbolMask must be 0x0 or 0x3ffff", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9181 | { &ei_oran_numslots_not_zero, { "oran_fh_cus.numslots_not_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "For ST4 TIME_DOMAIN_BEAM_WEIGHTS, numSlots should be 0", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9182 | { &ei_oran_version_unsupported, { "oran_fh_cus.version_unsupported", PI_UNDECODED0x05000000, PI_WARN0x00600000, "Protocol version unsupported", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9183 | { &ei_oran_laa_msg_type_unsupported, { "oran_fh_cus.laa_msg_type_unsupported", PI_UNDECODED0x05000000, PI_WARN0x00600000, "laaMsgType unsupported", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9184 | { &ei_oran_se_on_unsupported_st, { "oran_fh_cus.se_on_unsupported_st", PI_MALFORMED0x07000000, PI_WARN0x00600000, "Section Extension should not appear on this Section Type", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9185 | { &ei_oran_cplane_unexpected_sequence_number_ul, { "oran_fh_cus.unexpected_seq_no_cplane.ul", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Unexpected sequence number seen in C-Plane UL", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9186 | { &ei_oran_cplane_unexpected_sequence_number_dl, { "oran_fh_cus.unexpected_seq_no_cplane.dl", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Unexpected sequence number seen in C-Plane DL", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9187 | { &ei_oran_uplane_unexpected_sequence_number_ul, { "oran_fh_cus.unexpected_seq_no_uplane.ul", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Unexpected sequence number seen in U-Plane UL", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9188 | { &ei_oran_uplane_unexpected_sequence_number_dl, { "oran_fh_cus.unexpected_seq_no_uplane.dl", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Unexpected sequence number seen in U-Plane DL", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9189 | { &ei_oran_acknack_no_request, { "oran_fh_cus.acknack_no_request", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Have ackNackId response, but no request", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9190 | { &ei_oran_udpcomphdr_should_be_zero, { "oran_fh_cus.udcomphdr_should_be_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "C-Plane udCompHdr in DL should be set to 0", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9191 | { &ei_oran_radio_fragmentation_c_plane, { "oran_fh_cus.radio_fragmentation_c_plane", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "Radio fragmentation not allowed in C-PLane", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9192 | { &ei_oran_radio_fragmentation_u_plane, { "oran_fh_cus.radio_fragmentation_u_plane", PI_UNDECODED0x05000000, PI_WARN0x00600000, "Radio fragmentation in C-PLane not yet supported", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9193 | { &ei_oran_lastRbdid_out_of_range, { "oran_fh_cus.lastrbdid_out_of_range", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE 6 has bad rbgSize", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9194 | { &ei_oran_rbgMask_beyond_last_rbdid, { "oran_fh_cus.rbgmask_beyond_lastrbdid", PI_MALFORMED0x07000000, PI_WARN0x00600000, "rbgMask has bits set beyond lastRbgId", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9195 | { &ei_oran_unexpected_measTypeId, { "oran_fh_cus.unexpected_meastypeid", PI_MALFORMED0x07000000, PI_WARN0x00600000, "unexpected measTypeId", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9196 | { &ei_oran_unsupported_compression_method, { "oran_fh_cus.compression_type_unsupported", PI_UNDECODED0x05000000, PI_WARN0x00600000, "Unsupported compression type", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9197 | { &ei_oran_ud_comp_len_wrong_size, { "oran_fh_cus.ud_comp_len_wrong_size", PI_MALFORMED0x07000000, PI_WARN0x00600000, "udCompLen does not match length of U-Plane section", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9198 | { &ei_oran_sresmask2_not_zero_with_rb, { "oran_fh_cus.sresmask2_not_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "sReSMask2 should be zero when rb set", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9199 | { &ei_oran_st6_rb_shall_be_0, { "oran_fh_cus.st6_rb_set", PI_MALFORMED0x07000000, PI_WARN0x00600000, "rb should not be set for Section Type 6", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9200 | { &ei_oran_st9_not_ul, { "oran_fh_cus.st9_not_ul", PI_MALFORMED0x07000000, PI_WARN0x00600000, "Section Type 9 should only be sent in uplink direction", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9201 | { &ei_oran_st10_numsymbol_not_14, { "oran_fh_cus.st10_numsymbol_not_14", PI_MALFORMED0x07000000, PI_WARN0x00600000, "numSymbol should be 14 for Section Type 10", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9202 | { &ei_oran_st10_startsymbolid_not_0, { "oran_fh_cus.st10_startsymbolid_not_0", PI_MALFORMED0x07000000, PI_WARN0x00600000, "startSymbolId should be 0 for Section Type 10", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9203 | { &ei_oran_st10_not_ul, { "oran_fh_cus.st10_not_ul", PI_MALFORMED0x07000000, PI_WARN0x00600000, "Section Type 10 should only be sent in uplink direction", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9204 | { &ei_oran_se24_nothing_to_inherit, { "oran_fh_cus.se24_nothing_to_inherit", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE10 doesn't have type 2 or 3 before trying to inherit", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9205 | { &ei_oran_num_sinr_per_prb_unknown, { "oran_fh_cus.unexpected_num_sinr_per_prb", PI_MALFORMED0x07000000, PI_WARN0x00600000, "invalid numSinrPerPrb value", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9206 | { &ei_oran_start_symbol_id_bits_ignored, { "oran_fh_cus.start_symbol_id_bits_ignored", PI_MALFORMED0x07000000, PI_WARN0x00600000, "some startSymbolId lower bits ignored", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9207 | { &ei_oran_user_group_id_reserved_value, { "oran_fh_cus.user_group_id.reserved_value", PI_MALFORMED0x07000000, PI_WARN0x00600000, "userGroupId value 255 is reserved", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9208 | { &ei_oran_port_list_index_zero, { "oran_fh_cus.port_list_index.zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "portListIndex should not be zero", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9209 | { &ei_oran_ul_uplane_symbol_too_long, { "oran_fh_cus.ul_uplane_symbol_tx_too_slow", PI_RECEIVE0x0f000000, PI_WARN0x00600000, "UL U-Plane Tx took too long for symbol (limit set in preference)", EXPFILL0, ((void*)0), 0, {0, {((void*)0), ((void*)0), FT_NONE, BASE_NONE , ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE, -1, ((void *)0)}} }},
9210 | };
9211 |
9212 | /* Register the protocol name and description */
9213 | proto_oran = proto_register_protocol("O-RAN Fronthaul CUS", "O-RAN FH CUS", "oran_fh_cus");
9214 |
9215 | /* Allow dissector to find be found by name. */
9216 | register_dissector("oran_fh_cus", dissect_oran, proto_oran);
9217 |
9218 | /* Register the tap name. */
9219 | oran_tap = register_tap("oran-fh-cus");
9220 |
9221 | /* Required function calls to register the header fields and subtrees */
9222 | proto_register_field_array(proto_oran, hf, array_length(hf)(sizeof (hf) / sizeof (hf)[0]));
9223 | proto_register_subtree_array(ett, array_length(ett)(sizeof (ett) / sizeof (ett)[0]));
9224 | proto_register_subtree_array(ext_ett, array_length(ext_ett)(sizeof (ext_ett) / sizeof (ext_ett)[0]));
9225 |
9226 |
9227 | expert_oran = expert_register_protocol(proto_oran);
9228 | expert_register_field_array(expert_oran, ei, array_length(ei)(sizeof (ei) / sizeof (ei)[0]));
9229 |
9230 | module_t * oran_module = prefs_register_protocol(proto_oran, NULL((void*)0));
9231 |
9232 | /* prefs_register_static_text_preference(oran_module, "oran.stream", "", ""); */
9233 |
9234 | /* Register bit width/compression preferences separately by direction. */
9235 | prefs_register_uint_preference(oran_module, "oran.du_port_id_bits", "DU Port ID bits [a]",
9236 | "The bit width of DU Port ID - sum of a,b,c&d (eAxC) must be 16", 10, &pref_du_port_id_bits);
9237 | prefs_register_uint_preference(oran_module, "oran.bandsector_id_bits", "BandSector ID bits [b]",
9238 | "The bit width of BandSector ID - sum of a,b,c&d (eAxC) must be 16", 10, &pref_bandsector_id_bits);
9239 | prefs_register_uint_preference(oran_module, "oran.cc_id_bits", "CC ID bits [c]",
9240 | "The bit width of CC ID - sum of a,b,c&d (eAxC) must be 16", 10, &pref_cc_id_bits);
9241 | prefs_register_uint_preference(oran_module, "oran.ru_port_id_bits", "RU Port ID bits [d]",
9242 | "The bit width of RU Port ID - sum of a,b,c&d (eAxC) must be 16", 10, &pref_ru_port_id_bits);
9243 |
9244 | prefs_register_static_text_preference(oran_module, "oran.ul", "", "");
9245 |
9246 | /* Uplink userplane */
9247 | prefs_register_uint_preference(oran_module, "oran.iq_bitwidth_up", "IQ Bitwidth Uplink",
9248 | "The bit width of a sample in the Uplink (if no udcompHdr and no C-Plane)", 10, &pref_sample_bit_width_uplink);
9249 | prefs_register_enum_preference(oran_module, "oran.ud_comp_up", "Uplink User Data Compression",
9250 | "Uplink User Data Compression (if no udcompHdr and no C-Plane)", &pref_iqCompressionUplink, ul_compression_options, false0);
9251 | prefs_register_enum_preference(oran_module, "oran.ud_comp_hdr_up", "udCompHdr field is present for uplink",
9252 | "The udCompHdr field in U-Plane messages may or may not be present, depending on the "
9253 | "configuration of the O-RU. This preference instructs the dissector to expect "
9254 | "this field to be present in uplink messages",
9255 | &pref_includeUdCompHeaderUplink, udcomphdr_present_options, false0);
9256 | prefs_register_uint_preference(oran_module, "oran.ul_slot_us_limit", "Microseconds allowed for UL tx in symbol",
9257 | "Maximum number of microseconds allowed for UL slot transmission before expert warning (zero to disable). N.B. timing relative to first frame seen for same symbol",
9258 | 10, &us_allowed_for_ul_in_symbol);
9259 |
9260 |
9261 |
9262 | prefs_register_static_text_preference(oran_module, "oran.dl", "", "");
9263 |
9264 | /* Downlink userplane */
9265 | prefs_register_uint_preference(oran_module, "oran.iq_bitwidth_down", "IQ Bitwidth Downlink",
9266 | "The bit width of a sample in the Downlink (if no udcompHdr)", 10, &pref_sample_bit_width_downlink);
9267 | prefs_register_enum_preference(oran_module, "oran.ud_comp_down", "Downlink User Data Compression",
9268 | "Downlink User Data Compression", &pref_iqCompressionDownlink, dl_compression_options, false0);
9269 | prefs_register_enum_preference(oran_module, "oran.ud_comp_hdr_down", "udCompHdr field is present for downlink",
9270 | "The udCompHdr field in U-Plane messages may or may not be present, depending on the "
9271 | "configuration of the O-RU. This preference instructs the dissector to expect "
9272 | "this field to be present in downlink messages",
9273 | &pref_includeUdCompHeaderDownlink, udcomphdr_present_options, false0);
9274 |
9275 | prefs_register_static_text_preference(oran_module, "oran.sinr", "", "");
9276 |
9277 | /* SINR */
9278 | prefs_register_uint_preference(oran_module, "oran.iq_bitwidth_sinr", "IQ Bitwidth SINR",
9279 | "The bit width of a sample in SINR", 10, &pref_sample_bit_width_sinr);
9280 | prefs_register_enum_preference(oran_module, "oran.ud_comp_sinr", "SINR Compression",
9281 | "SINR Compression", &pref_iqCompressionSINR, ul_compression_options, false0);
9282 |
9283 |
9284 | /* BF-related */
9285 | prefs_register_static_text_preference(oran_module, "oran.bf", "", "");
9286 |
9287 | prefs_register_obsolete_preference(oran_module, "oran.num_weights_per_bundle");
9288 |
9289 | prefs_register_uint_preference(oran_module, "oran.num_bf_antennas", "Number of beam weights",
9290 | "Number of array elements that BF weights will be provided for", 10, &pref_num_bf_antennas);
9291 |
9292 | prefs_register_obsolete_preference(oran_module, "oran.num_bf_weights");
9293 |
9294 | prefs_register_bool_preference(oran_module, "oran.st6_4byte_alignment_required", "Use 4-byte alignment for ST6 sections",
9295 | "Default is 1-byte alignment", &st6_4byte_alignment);
9296 |
9297 |
9298 | /* Misc (and will seldom need to be accessed) */
9299 | prefs_register_static_text_preference(oran_module, "oran.misc", "", "");
9300 |
9301 | prefs_register_bool_preference(oran_module, "oran.show_iq_samples", "Show IQ Sample values",
9302 | "When enabled, for U-Plane frames show each I and Q value in PRB", &pref_showIQSampleValues);
9303 |
9304 | prefs_register_enum_preference(oran_module, "oran.support_udcomplen", "udCompLen supported",
9305 | "When enabled, U-Plane messages with relevant compression schemes will include udCompLen",
9306 | &pref_support_udcompLen, udcomplen_support_options, false0);
9307 |
9308 | prefs_register_uint_preference(oran_module, "oran.rbs_in_uplane_section", "Total RBs in User-Plane data section",
9309 | "This is used if numPrbu is signalled as 0", 10, &pref_data_plane_section_total_rbs);
9310 |
9311 | prefs_register_bool_preference(oran_module, "oran.unscaled_iq", "Show unscaled I/Q values",
9312 | "", &show_unscaled_values);
9313 |
9314 | prefs_register_obsolete_preference(oran_module, "oran.k_antenna_ports");
9315 |
9316 |
9317 | flow_states_table = wmem_tree_new_autoreset(wmem_epan_scope(), wmem_file_scope());
9318 | flow_results_table = wmem_tree_new_autoreset(wmem_epan_scope(), wmem_file_scope());
9319 | ul_symbol_timing = wmem_tree_new_autoreset(wmem_epan_scope(), wmem_file_scope());
9320 |
9321 | register_init_routine(&oran_init_protocol);
9322 | }
9323 |
9324 | /* Simpler form of proto_reg_handoff_oran which can be used if there are
9325 | * no prefs-dependent registration function calls. */
9326 | void
9327 | proto_reg_handoff_oran(void)
9328 | {
9329 | }
9330 |
9331 | /*
9332 | * Editor modelines - http://www.wireshark.org/tools/modelines.html
9333 | *
9334 | * Local Variables:
9335 | * c-basic-offset: 4
9336 | * tab-width: 8
9337 | * indent-tabs-mode: nil
9338 | * End:
9339 | *
9340 | * ex: set shiftwidth=4 tabstop=8 expandtab:
9341 | * :indentSize=4:tabSize=8:noTabs=true:
9342 | */