### Bug Summary

File: | epan/dissectors/packet-nmea0183.c
Warning: | line 1630, column 5 Value stored to 'offset' is never read

### Annotated Source Code

Press '?' to see keyboard shortcuts

Show analyzer invocation
clang -cc1 -cc1 -triple x86_64-pc-linux-gnu -analyze -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name packet-nmea0183.c -analyzer-checker=core -analyzer-checker=apiModeling -analyzer-checker=unix -analyzer-checker=deadcode -analyzer-checker=security.insecureAPI.UncheckedReturn -analyzer-checker=security.insecureAPI.getpw -analyzer-checker=security.insecureAPI.gets -analyzer-checker=security.insecureAPI.mktemp -analyzer-checker=security.insecureAPI.mkstemp -analyzer-checker=security.insecureAPI.vfork -analyzer-checker=nullability.NullPassedToNonnull -analyzer-checker=nullability.NullReturnedFromNonnull -analyzer-output plist -w -setup-static-analyzer -mrelocation-model pic -pic-level 2 -fhalf-no-semantic-interposition -fno-delete-null-pointer-checks -mframe-pointer=all -relaxed-aliasing -fmath-errno -ffp-contract=on -fno-rounding-math -ffloat16-excess-precision=fast -fbfloat16-excess-precision=fast -mconstructor-aliases -funwind-tables=2 -target-cpu x86-64 -tune-cpu generic -debugger-tuning=gdb -fdebug-compilation-dir=/builds/wireshark/wireshark/build -fcoverage-compilation-dir=/builds/wireshark/wireshark/build -resource-dir /usr/lib/llvm-21/lib/clang/21 -isystem /usr/include/glib-2.0 -isystem /usr/lib/x86_64-linux-gnu/glib-2.0/include -isystem /builds/wireshark/wireshark/epan/dissectors -isystem /builds/wireshark/wireshark/build/epan/dissectors -isystem /usr/include/mit-krb5 -isystem /usr/include/libxml2 -isystem /builds/wireshark/wireshark/epan -D G_DISABLE_DEPRECATED -D G_DISABLE_SINGLE_INCLUDES -D WS_BUILD_DLL -D WS_DEBUG -D WS_DEBUG_UTF_8 -I /builds/wireshark/wireshark/build -I /builds/wireshark/wireshark -I /builds/wireshark/wireshark/include -D _GLIBCXX_ASSERTIONS -internal-isystem /usr/lib/llvm-21/lib/clang/21/include -internal-isystem /usr/local/include -internal-isystem /usr/lib/gcc/x86_64-linux-gnu/14/../../../../x86_64-linux-gnu/include -internal-externc-isystem /usr/include/x86_64-linux-gnu -internal-externc-isystem /include -internal-externc-isystem /usr/include -fmacro-prefix-map=/builds/wireshark/wireshark/= -fmacro-prefix-map=/builds/wireshark/wireshark/build/= -fmacro-prefix-map=../= -Wno-format-nonliteral -std=gnu11 -ferror-limit 19 -fvisibility=hidden -fwrapv -fwrapv-pointer -fstrict-flex-arrays=3 -stack-protector 2 -fstack-clash-protection -fcf-protection=full -fgnuc-version=4.2.1 -fskip-odr-check-in-gmf -fexceptions -fcolor-diagnostics -analyzer-output=html -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -o /builds/wireshark/wireshark/sbout/2025-12-12-100324-3573-1 -x c /builds/wireshark/wireshark/epan/dissectors/packet-nmea0183.c

Keyboard shortcuts:

- Use 'j/k' keys for keyboard navigation
- Use 'Shift+S' to show/hide relevant lines
- Use '?' to toggle this window

Close
Show only relevant lines Show control flow arrows

1 | /* packet-nmea0183.c
2 | * Routines for NMEA 0183 protocol dissection
3 | * Copyright 2024 Casper Meijn <casper@meijn.net>
4 | *
5 | * Wireshark - Network traffic analyzer
6 | * By Gerald Combs <gerald@wireshark.org>
7 | * Copyright 1998 Gerald Combs
8 | *
9 | * SPDX-License-Identifier: GPL-2.0-or-later
10 | */
11 |
12 | #include "config.h"
13 | #include <epan/packet.h>
14 | #include <epan/expert.h>
15 |
16 |
17 | /*
18 | * null-terminated sentence prefix string "UdPbC"
19 | */
20 | #define UDPBC"UdPbC" "UdPbC"
21 | #define RRUDP"RrUdP" "RrUdP"
22 | #define RAUDP"RaUdp" "RaUdp"
23 | #define RPUDP"RpUdP" "RpUdP"
24 | #define NMEA0183_CRLF0x0d0a 0x0d0a
25 |
26 | static int hf_nmea0183_talker_id;
27 | static int hf_nmea0183_sentence_id;
28 | static int hf_nmea0183_unknown_field;
29 | static int hf_nmea0183_checksum;
30 | static int hf_nmea0183_checksum_calculated;
31 |
32 | static int hf_nmea0183_dpt_depth;
33 | static int hf_nmea0183_dpt_offset;
34 | static int hf_nmea0183_dpt_max_range;
35 |
36 | static int hf_nmea0183_hdt_heading;
37 | static int hf_nmea0183_hdt_unit;
38 |
39 | static int hf_nmea0183_alr_time;
40 | static int hf_nmea0183_alr_time_hour;
41 | static int hf_nmea0183_alr_time_minute;
42 | static int hf_nmea0183_alr_time_second;
43 | static int hf_nmea0183_alr_alarm_id;
44 | static int hf_nmea0183_alr_alarm_cond;
45 | static int hf_nmea0183_alr_alarm_ack_st;
46 | static int hf_nmea0183_alr_alarm_desc_txt;
47 |
48 | static int hf_nmea0183_gga_time;
49 | static int hf_nmea0183_gga_time_hour;
50 | static int hf_nmea0183_gga_time_minute;
51 | static int hf_nmea0183_gga_time_second;
52 | static int hf_nmea0183_gga_latitude;
53 | static int hf_nmea0183_gga_latitude_degree;
54 | static int hf_nmea0183_gga_latitude_minute;
55 | static int hf_nmea0183_gga_latitude_direction;
56 | static int hf_nmea0183_gga_longitude;
57 | static int hf_nmea0183_gga_longitude_degree;
58 | static int hf_nmea0183_gga_longitude_minute;
59 | static int hf_nmea0183_gga_longitude_direction;
60 | static int hf_nmea0183_gga_quality;
61 | static int hf_nmea0183_gga_number_satellites;
62 | static int hf_nmea0183_gga_horizontal_dilution;
63 | static int hf_nmea0183_gga_altitude;
64 | static int hf_nmea0183_gga_altitude_unit;
65 | static int hf_nmea0183_gga_geoidal_separation;
66 | static int hf_nmea0183_gga_geoidal_separation_unit;
67 | static int hf_nmea0183_gga_age_dgps;
68 | static int hf_nmea0183_gga_dgps_station;
69 |
70 | static int hf_nmea0183_gll_latitude;
71 | static int hf_nmea0183_gll_latitude_degree;
72 | static int hf_nmea0183_gll_latitude_minute;
73 | static int hf_nmea0183_gll_latitude_direction;
74 | static int hf_nmea0183_gll_longitude;
75 | static int hf_nmea0183_gll_longitude_degree;
76 | static int hf_nmea0183_gll_longitude_minute;
77 | static int hf_nmea0183_gll_longitude_direction;
78 | static int hf_nmea0183_gll_time;
79 | static int hf_nmea0183_gll_time_hour;
80 | static int hf_nmea0183_gll_time_minute;
81 | static int hf_nmea0183_gll_time_second;
82 | static int hf_nmea0183_gll_status;
83 | static int hf_nmea0183_gll_mode;
84 |
85 | static int hf_nmea0183_gst_time;
86 | static int hf_nmea0183_gst_time_hour;
87 | static int hf_nmea0183_gst_time_minute;
88 | static int hf_nmea0183_gst_time_second;
89 | static int hf_nmea0183_gst_rms_total_sd;
90 | static int hf_nmea0183_gst_ellipse_major_sd;
91 | static int hf_nmea0183_gst_ellipse_minor_sd;
92 | static int hf_nmea0183_gst_ellipse_orientation;
93 | static int hf_nmea0183_gst_latitude_sd;
94 | static int hf_nmea0183_gst_longitude_sd;
95 | static int hf_nmea0183_gst_altitude_sd;
96 |
97 | static int hf_nmea0183_rot_rate_of_turn;
98 | static int hf_nmea0183_rot_valid;
99 | static int hf_nmea0183_txt_num;
100 | static int hf_nmea0183_txt_sent_num;
101 | static int hf_nmea0183_txt_id;
102 | static int hf_nmea0183_txt_msg;
103 |
104 | static int hf_nmea0183_vbw_water_speed_longitudinal;
105 | static int hf_nmea0183_vbw_water_speed_transverse;
106 | static int hf_nmea0183_vbw_water_speed_valid;
107 | static int hf_nmea0183_vbw_ground_speed_longitudinal;
108 | static int hf_nmea0183_vbw_ground_speed_transverse;
109 | static int hf_nmea0183_vbw_ground_speed_valid;
110 | static int hf_nmea0183_vbw_stern_water_speed;
111 | static int hf_nmea0183_vbw_stern_water_speed_valid;
112 | static int hf_nmea0183_vbw_stern_ground_speed;
113 | static int hf_nmea0183_vbw_stern_ground_speed_valid;
114 |
115 | static int hf_nmea0183_vhw_true_heading;
116 | static int hf_nmea0183_vhw_true_heading_unit;
117 | static int hf_nmea0183_vhw_magnetic_heading;
118 | static int hf_nmea0183_vhw_magnetic_heading_unit;
119 | static int hf_nmea0183_vhw_water_speed_knot;
120 | static int hf_nmea0183_vhw_water_speed_knot_unit;
121 | static int hf_nmea0183_vhw_water_speed_kilometer;
122 | static int hf_nmea0183_vhw_water_speed_kilometer_unit;
123 |
124 | static int hf_nmea0183_vlw_cumulative_water;
125 | static int hf_nmea0183_vlw_cumulative_water_unit;
126 | static int hf_nmea0183_vlw_trip_water;
127 | static int hf_nmea0183_vlw_trip_water_unit;
128 | static int hf_nmea0183_vlw_cumulative_ground;
129 | static int hf_nmea0183_vlw_cumulative_ground_unit;
130 | static int hf_nmea0183_vlw_trip_ground;
131 | static int hf_nmea0183_vlw_trip_ground_unit;
132 |
133 | static int hf_nmea0183_vtg_true_course;
134 | static int hf_nmea0183_vtg_true_course_unit;
135 | static int hf_nmea0183_vtg_magnetic_course;
136 | static int hf_nmea0183_vtg_magnetic_course_unit;
137 | static int hf_nmea0183_vtg_ground_speed_knot;
138 | static int hf_nmea0183_vtg_ground_speed_knot_unit;
139 | static int hf_nmea0183_vtg_ground_speed_kilometer;
140 | static int hf_nmea0183_vtg_ground_speed_kilometer_unit;
141 | static int hf_nmea0183_vtg_mode;
142 |
143 | static int hf_nmea0183_zda_time;
144 | static int hf_nmea0183_zda_time_hour;
145 | static int hf_nmea0183_zda_time_minute;
146 | static int hf_nmea0183_zda_time_second;
147 | static int hf_nmea0183_zda_date_day;
148 | static int hf_nmea0183_zda_date_month;
149 | static int hf_nmea0183_zda_date_year;
150 | static int hf_nmea0183_zda_local_zone_hour;
151 | static int hf_nmea0183_zda_local_zone_minute;
152 |
153 | static int hf_nmea0183_sentence_prefix;
154 | static int hf_nmea0183_tag_block;
155 | static int hf_nmea0183_bin_version;
156 | static int hf_nmea0183_bin_srcid;
157 | static int hf_nmea0183_bin_dstid;
158 | static int hf_nmea0183_bin_mtype;
159 | static int hf_nmea0183_bin_blockid;
160 | static int hf_nmea0183_bin_seqnum;
161 | static int hf_nmea0183_bin_max_seqnum;
162 | static int hf_nmea0183_bin_data;
163 | static int hf_nmea0183_bin_file_descriptor;
164 | static int hf_nmea0183_bin_file_descriptor_len;
165 | static int hf_nmea0183_bin_file_length;
166 | static int hf_nmea0183_bin_stat_of_acquisition;
167 | static int hf_nmea0183_bin_device;
168 | static int hf_nmea0183_bin_channel;
169 | static int hf_nmea0183_bin_type_len;
170 | static int hf_nmea0183_bin_data_type;
171 | static int hf_nmea0183_bin_status_and_info;
172 |
173 | static int ett_nmea0183;
174 | static int ett_nmea0183_checksum;
175 | static int ett_nmea0183_sentence;
176 | static int ett_nmea0183_zda_time;
177 | static int ett_nmea0183_alr_time;
178 | static int ett_nmea0183_gga_time;
179 | static int ett_nmea0183_gga_latitude;
180 | static int ett_nmea0183_gga_longitude;
181 | static int ett_nmea0183_gll_time;
182 | static int ett_nmea0183_gll_latitude;
183 | static int ett_nmea0183_gll_longitude;
184 | static int ett_nmea0183_gst_time;
185 | static int ett_nmea0183_tag_block;
186 | static int ett_nmea0183_fd;
187 |
188 | static expert_field ei_nmea0183_invalid_first_character;
189 | static expert_field ei_nmea0183_missing_checksum_character;
190 | static expert_field ei_nmea0183_invalid_end_of_line;
191 | static expert_field ei_nmea0183_checksum_incorrect;
192 | static expert_field ei_nmea0183_sentence_too_long;
193 | static expert_field ei_nmea0183_field_time_too_short;
194 | static expert_field ei_nmea0183_field_latitude_too_short;
195 | static expert_field ei_nmea0183_field_longitude_too_short;
196 | static expert_field ei_nmea0183_field_missing;
197 | static expert_field ei_nmea0183_gga_altitude_unit_incorrect;
198 | static expert_field ei_nmea0183_gga_geoidal_separation_unit_incorrect;
199 | static expert_field ei_nmea0183_hdt_unit_incorrect;
200 | static expert_field ei_nmea0183_vhw_true_heading_unit_incorrect;
201 | static expert_field ei_nmea0183_vhw_magnetic_heading_unit_incorrect;
202 | static expert_field ei_nmea0183_vhw_water_speed_knot_unit_incorrect;
203 | static expert_field ei_nmea0183_vhw_water_speed_kilometer_unit_incorrect;
204 | static expert_field ei_nmea0183_vlw_cumulative_water_unit_incorrect;
205 | static expert_field ei_nmea0183_vlw_trip_water_unit_incorrect;
206 | static expert_field ei_nmea0183_vlw_cumulative_ground_unit_incorrect;
207 | static expert_field ei_nmea0183_vlw_trip_ground_unit_incorrect;
208 | static expert_field ei_nmea0183_vtg_true_course_unit_incorrect;
209 | static expert_field ei_nmea0183_vtg_magnetic_course_unit_incorrect;
210 | static expert_field ei_nmea0183_vtg_ground_speed_knot_unit_incorrect;
211 | static expert_field ei_nmea0183_vtg_ground_speed_kilometer_unit_incorrect;
212 |
213 | static int proto_nmea0183;
214 | static int proto_nmea0183_bin;
215 |
216 | static dissector_handle_t nmea0183_handle;
217 |
218 | // List of known Talker IDs (Source: NMEA Revealed by Eric S. Raymond, https://gpsd.gitlab.io/gpsd/NMEA.html, retrieved 2023-01-26)
219 | static const string_string known_talker_ids[] = {
220 | {"AB", "Independent AIS Base Station"},
221 | {"AD", "Dependent AIS Base Station"},
222 | {"AG", "Autopilot - General"},
223 | {"AI", "Mobile AIS Station"},
224 | {"AN", "AIS Aid to Navigation"},
225 | {"AP", "Autopilot - Magnetic"},
226 | {"AR", "AIS Receiving Station"},
227 | {"AT", "AIS Transmitting Station"},
228 | {"AX", "AIS Simplex Repeater"},
229 | {"BD", "BeiDou (China)"},
230 | {"BI", "Bilge System"},
231 | {"BN", "Bridge navigational watch alarm system"},
232 | {"BS", "Base AIS Station"},
233 | {"CA", "Central Alarm"},
234 | {"CC", "Computer - Programmed Calculator (obsolete)"},
235 | {"CD", "Communications - Digital Selective Calling (DSC)"},
236 | {"CM", "Computer - Memory Data (obsolete)"},
237 | {"CR", "Communications - Data Receiver"},
238 | {"CS", "Communications - Satellite"},
239 | {"CT", "Communications - Radio-Telephone (MF/HF)"},
240 | {"CV", "Communications - Radio-Telephone (VHF)"},
241 | {"CX", "Communications - Scanning Receiver"},
242 | {"DE", "DECCA Navigation (obsolete)"},
243 | {"DF", "Direction Finder"},
244 | {"DM", "Velocity Sensor, Speed Log, Water, Magnetic"},
245 | {"DP", "Dynamiv Position"},
246 | {"DU", "Duplex repeater station"},
247 | {"EC", "Electronic Chart System (ECS)"},
248 | {"EI", "Electronic Chart Display & Information System (ECDIS)"},
249 | {"EP", "Emergency Position Indicating Beacon (EPIRB)"},
250 | {"ER", "Engine Room Monitoring Systems"},
251 | {"FD", "Fire Door"},
252 | {"FE", "Fire Extinguisher System"},
253 | {"FR", "Fire Detection System"},
254 | {"FS", "Fire Sprinkler"},
255 | {"GA", "Galileo Positioning System"},
256 | {"GB", "BeiDou (China)"},
257 | {"GI", "NavIC, IRNSS (India)"},
258 | {"GL", "GLONASS, according to IEIC 61162-1"},
259 | {"GN", "Combination of multiple satellite systems (NMEA 1083)"},
260 | {"GP", "Global Positioning System receiver"},
261 | {"GQ", "QZSS regional GPS augmentation system (Japan)"},
262 | {"HC", "Heading - Magnetic Compass"},
263 | {"HD", "Hull Door"},
264 | {"HE", "Heading - North Seeking Gyro"},
265 | {"HF", "Heading - Fluxgate"},
266 | {"HN", "Heading - Non North Seeking Gyro"},
267 | {"HS", "Hull Stress"},
268 | {"II", "Integrated Instrumentation"},
269 | {"IN", "Integrated Navigation"},
270 | {"JA", "Alarm and Monitoring"},
271 | {"JB", "Water Monitoring"},
272 | {"JC", "Power Management"},
273 | {"JD", "Propulsion Control"},
274 | {"JE", "Engine Control"},
275 | {"JF", "Propulsion Boiler"},
276 | {"JG", "Aux Boiler"},
277 | {"JH", "Engine Governor"},
278 | {"LA", "Loran A (obsolete)"},
279 | {"LC", "Loran C (obsolete)"},
280 | {"MP", "Microwave Positioning System (obsolete)"},
281 | {"MX", "Multiplexer"},
282 | {"NL", "Navigation light controller"},
283 | {"NV", "Night Vision"},
284 | {"OM", "OMEGA Navigation System (obsolete)"},
285 | {"OS", "Distress Alarm System (obsolete)"},
286 | {"P ", "Vendor specific"},
287 | {"QZ", "QZSS regional GPS augmentation system (Japan)"},
288 | {"RA", "RADAR and/or ARPA"},
289 | {"RB", "Record Book"},
290 | {"RC", "Propulsion Machinery including Remote Control"},
291 | {"RI", "Rudder Angle Indicator"},
292 | {"SA", "Physical Shore AUS Station"},
293 | {"SC", "Steering Control System/Device"},
294 | {"SD", "Depth Sounder"},
295 | {"SG", "Steering Gear"},
296 | {"SN", "Electronic Positioning System, other/general"},
297 | {"SS", "Scanning Sounder"},
298 | {"ST", "Skytraq debug output"},
299 | {"TC", "Track Control"},
300 | {"TI", "Turn Rate Indicator"},
301 | {"TR", "TRANSIT Navigation System"},
302 | {"U0", "User Configured 0"},
303 | {"U1", "User Configured 1"},
304 | {"U2", "User Configured 2"},
305 | {"U3", "User Configured 3"},
306 | {"U4", "User Configured 4"},
307 | {"U5", "User Configured 5"},
308 | {"U6", "User Configured 6"},
309 | {"U7", "User Configured 7"},
310 | {"U8", "User Configured 8"},
311 | {"U9", "User Configured 9"},
312 | {"UP", "Microprocessor controller"},
313 | {"VA", "VHF Data Exchange System (VDES), ASM"},
314 | {"VD", "Velocity Sensor, Doppler, other/general"},
315 | {"VM", "Velocity Sensor, Speed Log, Water, Magnetic"},
316 | {"VR", "Voyage Data recorder"},
317 | {"VS", "VHF Data Exchange System (VDES), Satellite"},
318 | {"VT", "VHF Data Exchange System (VDES), Terrestrial"},
319 | {"VW", "Velocity Sensor, Speed Log, Water, Mechanical"},
320 | {"WD", "Watertight Door"},
321 | {"WI", "Weather Instruments"},
322 | {"WL", "Water Level"},
323 | {"YC", "Transducer - Temperature (obsolete)"},
324 | {"YD", "Transducer - Displacement, Angular or Linear (obsolete)"},
325 | {"YF", "Transducer - Frequency (obsolete)"},
326 | {"YL", "Transducer - Level (obsolete)"},
327 | {"YP", "Transducer - Pressure (obsolete)"},
328 | {"YR", "Transducer - Flow Rate (obsolete)"},
329 | {"YT", "Transducer - Tachometer (obsolete)"},
330 | {"YV", "Transducer - Volume (obsolete)"},
331 | {"YX", "Transducer"},
332 | {"ZA", "Timekeeper - Atomic Clock"},
333 | {"ZC", "Timekeeper - Chronometer"},
334 | {"ZQ", "Timekeeper - Quartz"},
335 | {"ZV", "Timekeeper - Radio Update, WWV or WWVH"},
336 | {NULL((void*)0), NULL((void*)0)}};
337 |
338 | // List of known Sentence IDs (Source: NMEA Revealed by Eric S. Raymond, https://gpsd.gitlab.io/gpsd/NMEA.html, retrieved 2023-01-26)
339 | static const string_string known_sentence_ids[] = {
340 | {"AAM", "Waypoint Arrival Alarm"},
341 | {"ABK", "UAIS Addressed and Binary Broadcast Acknowledgement"},
342 | {"ACA", "UAIS Regional Channel Assignment Message"},
343 | {"ACF", "General AtoN Station Configuration Command"},
344 | {"ACG", "Extended General AtoN Station Configuration Command"},
345 | {"ACK", "Alarm Acknowledgement"},
346 | {"ACM", "Preparation and Initiation of an AIS Base Station Addressed Channel Management Message (Message 22)"},
347 | {"ACS", "UAIS Channel Management Information Source"},
348 | {"ADS", "Automatic Device Status"},
349 | {"AFB", "AtoN Forced Broadcast Command"},
350 | {"AGA", "Preparation and Initiation of an AIS Base Station Broadcast of a Group Assignment Message (Message 23)"},
351 | {"AID", "AtoN Identification Configuration Command"},
352 | {"AIR", "UAIS Interrogation Request"},
353 | {"AKD", "Acknowledge Detail Alarm Condition"},
354 | {"ALA", "Set Detail Alarm Condition"},
355 | {"ALM", "GPS Almanac Data"},
356 | {"ALR", "Set Alarm State"},
357 | {"ARC", "Alert Command Refused"},
358 | {"APA", "Autopilot Sentence A"},
359 | {"APB", "Autopilot Sentence B"},
360 | {"ASD", "Autopilot System Data"},
361 | {"ASN", "Preparation and Initiation of an AIS Base Station Broadcast of Assignment VDL (Message 16)"},
362 | {"BBM", "AIS Broadcast BinaryMessage"},
363 | {"BCG", "Base Station Configuration, General Command"},
364 | {"BCL", "Base Station Configuration, Location Command"},
365 | {"BEC", "Bearing & Distance to Waypoint - Dead Reckoning"},
366 | {"BER", "Bearing & Distance to Waypoint, Dead Reckoning, Rhumb Line"},
367 | {"BOD", "Bearing - Waypoint to Waypoint"},
368 | {"BPI", "Bearing & Distance to Point of Interest"},
369 | {"BWC", "Bearing & Distance to Waypoint - Great Circle"},
370 | {"BWR", "Bearing and Distance to Waypoint - Rhumb Line"},
371 | {"BWW", "Bearing - Waypoint to Waypoint"},
372 | {"CBR", "Configure Broadcast Rates for AIS AtoN Station Message Command"},
373 | {"CEK", "Configure Encryption Key Command"},
374 | {"COP", "Configure the Operational Period, Command"},
375 | {"CPC", "Configure Parameter-Code for UNIX Time Parameter (c)"},
376 | {"CPD", "Configure Parameter-Code for Destination-Identification Parameter (d)"},
377 | {"CPG", "Configure Parameter-Code for the Sentence-Grouping Parameter (g)"},
378 | {"CPN", "Configure Parameter-Code for the Line-Count Parameter (n)"},
379 | {"CPR", "Configure Parameter-Code for Relative Time Parameter (r)"},
380 | {"CPS", "Configure Parameter-Code for the Source-Identification Parameter (s)"},
381 | {"CPT", "Configure Parameter-Code for General Alphanumeric String Parameter (t)"},
382 | {"CUR", "Water Current Layer"},
383 | {"DBK", "Echosounder - Depth Below Keel"},
384 | {"DBS", "Echosounder - Depth Below Surface"},
385 | {"DBT", "Echosounder - Depth Below Transducer"},
386 | {"DCN", "DECCA Position"},
387 | {"DCR", "Device Capability Report"},
388 | {"DDC", "Display Dimming Control"},
389 | {"DLM", "Data Link Management Slot Allocations for Base Station"},
390 | {"DOR", "Door Status Detection"},
391 | {"DPT", "Depth of Water"},
392 | {"DRU", "Dual Doppler Auxiliary Data"},
393 | {"DSC", "Digital Selective Calling Information"},
394 | {"DSE", "Extended DSC"},
395 | {"DSI", "DSC Transponder Initiate"},
396 | {"DSR", "DSC Transponder Response"},
397 | {"DTM", "Datum Reference"},
398 | {"ECB", "Configure Broadcast Rates for Base Station Messages with Epoch Planning Support"},
399 | {"ETL", "Engine Telegraph Operation Status"},
400 | {"EVE", "General Event Message"},
401 | {"FIR", "Fire Detection"},
402 | {"FSI", "Frequency Set Information"},
403 | {"FSR", "Frame Summary of AIS Reception"},
404 | {"GAL", "Galileo Almanac Data"},
405 | {"GBS", "GPS Satellite Fault Detection"},
406 | {"GDA", "Dead Reckoning Positions"},
407 | {"GEN", "Generic Binary/Status Information"},
408 | {"GFA", "GNSS Fix Accuracy and Integrity"},
409 | {"GGA", "Global Positioning System Fix Data"},
410 | {"GLA", "Loran-C Positions"},
411 | {"GLC", "Geographic Position, Loran-C"},
412 | {"GLL", "Geographic Position - Latitude/Longitude"},
413 | {"GMP", "GNSS Map Projection Fix Data"},
414 | {"GNS", "GNSS Fix data"},
415 | {"GOA", "OMEGA Positions"},
416 | {"GRS", "GNSS Range Residuals"},
417 | {"GSA", "GNSS DOP and Active Satellites"},
418 | {"GST", "GNSS Pseudorange Noise Statistics"},
419 | {"GSV", "GNSS Satellites in View"},
420 | {"GTD", "Geographic Location in Time Differences"},
421 | {"GXA", "TRANSIT Position"},
422 | {"HBT", "Heartbeat Supervision Report"},
423 | {"HCC", "Compass Heading"},
424 | {"HCD", "Heading and Deviation"},
425 | {"HDG", "Heading - Deviation & Variation"},
426 | {"HDM", "Heading - Magnetic"},
427 | {"HDT", "Heading - True"},
428 | {"HFB", "Trawl Headrope to Footrope and Bottom"},
429 | {"HMR", "Heading, Monitor Receive"},
430 | {"HMS", "Heading, Monitor Set"},
431 | {"HSC", "Heading Steering Command"},
432 | {"HSS", "Hull Stress Surveillance Systems"},
433 | {"HTC", "Heading/Track Control Command"},
434 | {"HTD", "Heading/Track Control Data"},
435 | {"HVD", "Magnetic Variation, Automatic"},
436 | {"HVM", "Magnetic Variation, Manually Set"},
437 | {"IMA", "Vessel Identification"},
438 | {"ITS", "Trawl Door Spread 2 Distance"},
439 | {"LCD", "Loran-C Signal Data"},
440 | {"LR1", "UAIS Long-range Reply Sentence 1"},
441 | {"LR2", "UAIS Long-range Reply Sentence 2"},
442 | {"LR3", "UAIS Long-range Reply Sentence 3"},
443 | {"LRF", "UAIS Long-Range Function"},
444 | {"LRI", "UAIS Long-Range Interrogation"},
445 | {"LTI", "UAIS Long-Range Interrogation"},
446 | {"MDA", "Meteorological Composite"},
447 | {"MEB", "Message Input for Broadcast, Command"},
448 | {"MHU", "Humidity"},
449 | {"MLA", "GLONASS Almanac Data"},
450 | {"MMB", "Barometer"},
451 | {"MSK", "Control for a Beacon Receiver"},
452 | {"MSS", "Beacon Receiver Status"},
453 | {"MTA", "Air Temperature"},
454 | {"MTW", "Mean Temperature of Water"},
455 | {"MWD", "Wind Direction & Speed"},
456 | {"MWH", "Wave Height"},
457 | {"MWS", "Wind & Sea State"},
458 | {"MWV", "Wind Speed and Angle"},
459 | {"NAK", "Negative Acknowledgement"},
460 | {"NRM", "NAVTEX Receiver Mask"},
461 | {"NRX", "NAVTEX Received Message"},
462 | {"ODC", "Echosounder - ODEC DPT Format"},
463 | {"OLN", "Omega Lane Numbers"},
464 | {"OLW", "Omega Lane Width"},
465 | {"OMP", "Omega Position"},
466 | {"OSD", "Own Ship Data"},
467 | {"OZN", "Omega Zone Number"},
468 | {"POS", "Device Position and Ship Dimensions Report or Configuration Command"},
469 | {"PRC", "Propulsion Remote Control Status"},
470 | {"R00", "Waypoints in active route"},
471 | {"RLM", "Return Link Message"},
472 | {"RMA", "Recommended Minimum Specific Loran-C Data"},
473 | {"RMB", "Recommended Minimum Navigation Information"},
474 | {"RMC", "Recommended Minimum Specific GNSS Data"},
475 | {"RNN", "Routes"},
476 | {"ROO", "Waypoints in Active Route"},
477 | {"ROR", "Rudder Order Status"},
478 | {"ROT", "Rate Of Turn"},
479 | {"RPM", "Revolutions"},
480 | {"RSA", "Rudder Sensor Angle"},
481 | {"RSD", "RADAR System Data"},
482 | {"RST", "Equipment Reset Command"},
483 | {"RTE", "Routes"},
484 | {"SBK", "Loran-C Blink Status"},
485 | {"SCD", "Loran-C ECDs"},
486 | {"SCY", "Loran-C Cycle Lock Status"},
487 | {"SDB", "Loran-C Signal Strength"},
488 | {"SFI", "Scanning Frequency Information"},
489 | {"SGD", "Position Accuracy Estimate"},
490 | {"SGR", "Loran-C Chain Identifier"},
491 | {"SID", "Set an Equipment's Identification, Command"},
492 | {"SIU", "Loran-C Stations in Use"},
493 | {"SLC", "Loran-C Status"},
494 | {"SPO", "Select AIS Device's Processing and Output"},
495 | {"SNC", "Navigation Calculation Basis"},
496 | {"SNU", "Loran-C SNR Status"},
497 | {"SPO", "Select AIS Device's Processing and Output"},
498 | {"SPS", "Loran-C Predicted Signal Strength"},
499 | {"SSD", "UAIS Ship Static Data"},
500 | {"SSF", "Position Correction Offset"},
501 | {"STC", "Time Constant"},
502 | {"STN", "Multiple Data ID"},
503 | {"STR", "Tracking Reference"},
504 | {"SYS", "Hybrid System Configuration"},
505 | {"TBR", "TAG Block Report"},
506 | {"TBS", "TAG Block Listener Source-Identification Configuration Command"},
507 | {"TDS", "Trawl Door Spread Distance"},
508 | {"TEC", "TRANSIT Satellite Error Code & Doppler Count"},
509 | {"TEP", "TRANSIT Satellite Predicted Elevation"},
510 | {"TFI", "Trawl Filling Indicator"},
511 | {"TFR", "Transmit Feedback Report"},
512 | {"TGA", "TRANSIT Satellite Antenna & Geoidal Heights"},
513 | {"THS", "True Heading and Status"},
514 | {"TIF", "TRANSIT Satellite Initial Flag"},
515 | {"TLB", "Target Label"},
516 | {"TLL", "Target Latitude and Longitude"},
517 | {"TPC", "Trawl Position Cartesian Coordinates"},
518 | {"TPR", "Trawl Position Relative Vessel"},
519 | {"TPT", "Trawl Position True"},
520 | {"TRC", "Thruster Control Data"},
521 | {"TRD", "Thruster Response Data"},
522 | {"TRF", "TRANSIT Fix Data"},
523 | {"TRP", "TRANSIT Satellite Predicted Direction of Rise"},
524 | {"TRS", "TRANSIT Satellite Operating Status"},
525 | {"TSA", "Transmit Slot Assignment"},
526 | {"TSP", "Transmit Slot Prohibit"},
527 | {"TSR", "Transmit Slot Prohibit - Status Report"},
528 | {"TTD", "Tracked Target Data"},
529 | {"TTM", "Tracked Target Message"},
530 | {"TUT", "Transmission of Multi-Language Text"},
531 | {"TXT", "Text Transmission"},
532 | {"UID", "User Identification Code Transmission"},
533 | {"VBW", "Dual Ground/Water Speed"},
534 | {"VCD", "Current at Selected Depth"},
535 | {"VDR", "Set and Drift"},
536 | {"VER", "Version"},
537 | {"VHW", "Water Speed and Heading"},
538 | {"VLW", "Distance Traveled through Water"},
539 | {"VPE", "Speed, Dead Reckoned Parallel to True Wind"},
540 | {"VPW", "Speed, Measured Parallel to Wind"},
541 | {"VSD", "UAIS Voyage Static Data"},
542 | {"VSI", "VDL Signal Information"},
543 | {"VTA", "Actual Track"},
544 | {"VTG", "Track made good and Ground speed"},
545 | {"VTI", "Intended Track"},
546 | {"VWE", "Wind Track Efficiency"},
547 | {"VWR", "Relative Wind Speed and Angle"},
548 | {"VWT", "True Wind Speed and Angle"},
549 | {"WAT", "Water Level Detection"},
550 | {"WCV", "Waypoint Closure Velocity"},
551 | {"WDC", "Distance to Waypoint - Great Circle"},
552 | {"WDR", "Distance to Waypoint - Rhumb Line"},
553 | {"WFM", "Route Following Mode"},
554 | {"WNC", "Distance - Waypoint to Waypoint"},
555 | {"WNR", "Waypoint-to-Waypoint Distance, Rhumb Line"},
556 | {"WPL", "Waypoint Location"},
557 | {"XDR", "Transducer Measurement"},
558 | {"XTE", "Cross-Track Error, Measured"},
559 | {"XTR", "Cross Track Error - Dead Reckoning"},
560 | {"YWP", "Water Propagation Speed"},
561 | {"YWS", "Water Profile"},
562 | {"ZAA", "Time, Elapsed/Estimated"},
563 | {"ZCD", "Timer"},
564 | {"ZDA", "Time & Date - UTC, day, month, year and local time zone"},
565 | {"ZDL", "Time and Distance to Variable Point"},
566 | {"ZEV", "Event Timer"},
567 | {"ZFO", "UTC & Time from origin Waypoint"},
568 | {"ZLZ", "Time of Day"},
569 | {"ZTG", "UTC & Time to Destination Waypoint"},
570 | {"ZZU", "Time, UTC"},
571 | {NULL((void*)0), NULL((void*)0)}};
572 |
573 | /* Proprietary Manufacturer Mnemonic Coder lookup table */
574 | /* https://web.nmea.org/External/WCPages/WCWebContent/webcontentpage.aspx?ContentID=364 */
575 | static const string_string manufacturer_vals[] = {
576 | {"3SN", "3-S Navigation"},
577 | {"AAB", "ASM Selective Addressed Message (Reserved for Future Use)"},
578 | {"AAR", "Asian American Resources"},
579 | {"ABB", "ASM Broadcast Message (Reserved for Future Use)"},
580 | {"ACE", "Auto-Comm Engineering Corporation"},
581 | {"ACR", "ACR Electronics, Inc."},
582 | {"ACS", "Arco Solar Inc."},
583 | {"ACT", "Advanced Control Technology"},
584 | {"ADI", "Aditel"},
585 | {"ADM", "ASM VHF Data-Link Message (Reserved for Future Use)"},
586 | {"ADN", "AD Navigation"},
587 | {"ADO", "ASM VHF Data-Link Own-Vessel Report (Reserved for Future Use"},
588 | {"AGB", "ASM Geographical Multicast Message (Reserved for Future Use"},
589 | {"AGI", "Airguide Instrument Co."},
590 | {"AGL", "Alert Group List (Reserved for Future Use)"},
591 | {"AHA", "Autohelm of America"},
592 | {"AIP", "AIPHONE Corporation"},
593 | {"ALD", "Alden Electronics, Inc."},
594 | {"AMB", "Ambarella, Inc. "},
595 | {"AMC", "AllTek Marine Electronics Corp."},
596 | {"AMI", "Advanced Marine Instrumentation, Ltd."},
597 | {"AMK", "ASM Addressed and Broadcast Message Acknowledgement (Reserved for Future Use)"},
598 | {"AMM", "Aquametro Oil & Marine"},
599 | {"AMR", "AMR Systems"},
600 | {"AMT", "Airmar Technology Corporation"},
601 | {"AND", "Andrew Corporation"},
602 | {"ANI", "Autonautic Instrumental Sl. (Spain)"},
603 | {"ANS", "Antenna Specialists"},
604 | {"ANX", "Analytyx Electronic Systems"},
605 | {"ANZ", "Anschutz of America"},
606 | {"AOB", "Aerobytes, Ltd."},
607 | {"APC", "Apelco Electronics & Navigation"},
608 | {"APN", "American Pioneer, Inc."},
609 | {"APO", "Automated Procedure Options (Reserved for Future Use)"},
610 | {"APW", "Pharos Marine Automatic Power"},
611 | {"APX", "Amperex, Inc."},
612 | {"AQC", "Aqua-Chem, Inc."},
613 | {"AQD", "AquaDynamics, Inc."},
614 | {"AQM", "Aqua Meter Instrument Corp."},
615 | {"ARL", "Active Research, Ltd."},
616 | {"ART", "Arlt Technologies, GmbH (Germany)"},
617 | {"ARV", "Arvento Mobile Systems"},
618 | {"ASH", "Ashtech"},
619 | {"ASP", "American Solar Power"},
620 | {"ATC", "Advanced C Technology, Ltd."},
621 | {"ATE", "Aetna Engineering"},
622 | {"ATM", "Atlantic Marketing Company"},
623 | {"ATR", "Airtron"},
624 | {"ATV", "Activation, Inc."},
625 | {"AUC", "Automated Procedure Control (Reserved for Future Use)"},
626 | {"AUP", "Automated Procedure Query (Reserved for Future Use)"},
627 | {"AUS", "Automated Procedure Status (Reserved for Future Use)"},
628 | {"AVN", "Advanced Navigation, Inc."},
629 | {"AWA", "Awa New Zealand, Ltd."},
630 | {"AXN", "Axiom Navigation, Inc."},
631 | {"BBG", "BBG, Inc."},
632 | {"BBL", "BBL Industries, Inc."},
633 | {"BBR", "BBR and Associates"},
634 | {"BDV", "Brisson Development, Inc."},
635 | {"BEC", "Boat Electric Corporation"},
636 | {"BFA", "Blueflow Americas"},
637 | {"BGG", "Bodensee Gravitymeter Geo-Systems (BGS)"},
638 | {"BGS", "Barringer Geoservice"},
639 | {"BGT", "Brookes and Gatehouse, Inc."},
640 | {"BHE", "BH Electronics"},
641 | {"BHR", "Bahr Technologies, Inc."},
642 | {"BLB", "Bay Laboratories"},
643 | {"BMC", "BMC"},
644 | {"BME", "Bartel Marine Electronics"},
645 | {"BMS", "Becker Marine Systems"},
646 | {"BMT", "Aventics GmbH (formerly Bosch Rexroth AG Marine Technique) (Germany)"},
647 | {"BNI", "Neil Brown Instrument Systems"},
648 | {"BNS", "Bowditch Navigation Systems"},
649 | {"BRM", "Mel Barr Company"},
650 | {"BRO", "Broadgate, Ltd."},
651 | {"BRY", "Byrd Industries"},
652 | {"BTH", "Benthos, Inc."},
653 | {"BTK", "Baltek Corporation"},
654 | {"BTS", "Boat Sentry, Inc."},
655 | {"BVE", "BV Engineering"},
656 | {"BXA", "Bendix-Avalex, Inc."},
657 | {"CAI", "Cambridge Aero Instruments"},
658 | {"CAT", "Catel"},
659 | {"CBN", "Cybernet Marine Products"},
660 | {"CCA", "Copal Corporation of America"},
661 | {"CCC", "Coastel Communications Company"},
662 | {"CCL", "Coastal Climate Company"},
663 | {"CCM", "Coastal Communications"},
664 | {"CDC", "Cordic Company"},
665 | {"CDI", "Chetco Digital Instruments"},
666 | {"CDL", "Teledyne CDL (CDLTD), Inc."},
667 | {"CDS", "Central Dimming Set (Reserved for Future Use)"},
668 | {"CEC", "Ceco Communications, Inc."},
669 | {"CEI", "Cambridge Engineering, Inc."},
670 | {"CFS", "Carlisle and Finch Company"},
671 | {"CHI", "Charles Industries, Ltd."},
672 | {"CIN", "Canadian Automotive Instruments"},
673 | {"CKM", "Cinkel Marine Electronics"},
674 | {"CLR", "Colorlight AB"},
675 | {"CMA", "Soc Nouvelle D'equip Calvados"},
676 | {"CMC", "Coe Manufacturing Company"},
677 | {"CME", "Cushman Electronics, Inc."},
678 | {"CML", "CML Microsystems PLC"},
679 | {"CMN", "ComNav Marine, Ltd."},
680 | {"CMP", "C-MAP, s.r.l. (Italy)"},
681 | {"CMS", "Coastal Marine Sales Company"},
682 | {"CMV", "Coursemaster USA, Inc."},
683 | {"CNI", "Continental Instruments"},
684 | {"CNS", "CNS Systems AB (Sweden)"},
685 | {"CNV", "Coastal Navigator"},
686 | {"CNX", "Cynex Manufacturing Company"},
687 | {"CPL", "Computrol, Inc."},
688 | {"CPN", "CompuNav"},
689 | {"CPS", "Columbus Positioning, Ltd."},
690 | {"CPT", "CPT, Inc."},
691 | {"CRE", "Crystal Electronics, Ltd."},
692 | {"CRO", "The Caro Group"},
693 | {"CRY", "Crystek Crystals Corporation"},
694 | {"CSI", "Communication Systems International"},
695 | {"CSM", "COMSAT Maritime Services"},
696 | {"CSR", "CSR Stockholm"},
697 | {"CSS", "CNS, Inc."},
698 | {"CST", "CAST, Inc."},
699 | {"CSV", "Combined Services"},
700 | {"CTA", "Current Alternatives"},
701 | {"CTB", "Cetec Benmar"},
702 | {"CTC", "Cell-Tech Communications"},
703 | {"CTE", "Castle Electronics"},
704 | {"CTL", "C-Tech, Ltd."},
705 | {"CTS", "C-Tech Systems"},
706 | {"CUL", "Cyclic Procedure List (Reserved for Future Use)"},
707 | {"CUS", "Customware"},
708 | {"CWD", "Cubic Western Data"},
709 | {"CWF", "Hamilton Jet"},
710 | {"CWV", "Celwave RF, Inc."},
711 | {"CYL", "Cyclic Procedure List (Reserved for Future Use)"},
712 | {"CYZ", "CYZ, Inc."},
713 | {"DAN", "Danelec Marine A/S (Denmark)"},
714 | {"DAS", "Dassault Sercel Navigation-Positioning"},
715 | {"DBM", "Deep Blue Marine"},
716 | {"DCC", "Dolphin Components Corporation"},
717 | {"DEB", "Debeg GmbH (Germany)"},
718 | {"DEC", "Decca Division, Litton Marine Systems BV"},
719 | {"DFI", "Defender Industries, Inc."},
720 | {"DGC", "Digicourse, Inc."},
721 | {"DGY", "Digital Yacht, Ltd."},
722 | {"DGP", "Digpilot A/S (Norway)"},
723 | {"DME", "Delorme"},
724 | {"DMI", "Datamarine International"},
725 | {"DNS", "Dornier System"},
726 | {"DNT", "Del Norte Technology, Inc."},
727 | {"DOI", "Digital Oceans, Inc."},
728 | {"DPC", "Data Panel Corporation"},
729 | {"DPS", "Danaplus, Inc."},
730 | {"DRL", "RL Drake Company"},
731 | {"DSC", "Dynascan Corporation"},
732 | {"DTN", "Dytechna, Ltd."},
733 | {"DYN", "Dynamote Corporation"},
734 | {"DYT", "Dytek Laboratories, Inc."},
735 | {"EAN", "EuroAvionics Navigation Systems GmbH (Germany)"},
736 | {"EBC", "Emergency Beacon Corporation"},
737 | {"ECI", "Enhanced Selective Calling Information (Reserved for Future Use)"},
738 | {"ECR", "Escort, Inc."},
739 | {"ECT", "Echotec, Inc."},
740 | {"EDO", "EDO Corporation, Electroacoustics Division"},
741 | {"EEL", "Electronica Eutimio Sl. (Spain)"},
742 | {"EEV", "EEV, Inc."},
743 | {"EFC", "Efcom Communication Systems"},
744 | {"EKC", "Eastman Kodak"},
745 | {"ELA", "Wartsila Elac Nautik GmbH (Germany)"},
746 | {"ELD", "Electronic Devices, Inc."},
747 | {"ELM", "ELMAN, s.r.l. (Italy)"},
748 | {"EMC", "Electric Motion Company"},
749 | {"EMK", "E-Marine Company, Ltd."},
750 | {"EMR", "EMRI A/S (Denmark)"},
751 | {"EMS", "Electro Marine Systems, Inc."},
752 | {"ENA", "Energy Analysts, Inc."},
753 | {"ENC", "Encron, Inc."},
754 | {"EPM", "EPSCO Marine"},
755 | {"EPT", "Eastprint, Inc."},
756 | {"ERC", "The Ericsson Corporation"},
757 | {"ERD", "eRide, Inc."},
758 | {"ESA", "European Space Agency"},
759 | {"ESC", "Electronics Emporium Division of ESC Products"},
760 | {"ESY", "E-Systems ECI Division"},
761 | {"FDN", "FluiDyne"},
762 | {"FEC", "Furuno Electric Company"},
763 | {"FHE", "Fish Hawk Electronics"},
764 | {"FJN", "Jon Fluke Company"},
765 | {"FLA", "Flarm Technology GmbH (Germany)"},
766 | {"FLO", "Floscan, Inc."},
767 | {"FMM", "First Mate Marine Autopilots"},
768 | {"FMS", "Fugro Seastar A/S (MarineStar)"},
769 | {"FNT", "Franklin Net and Twine, Ltd."},
770 | {"FRC", "The Fredericks Company"},
771 | {"FSS", "Frequency Selection (Reserved for Future Use)"},
772 | {"FST", "Fastrax OY (Switzerland)"},
773 | {"FTG", "Thomas G Faria Corporation"},
774 | {"FTT", "FT-TEC"},
775 | {"FUG", "Fugro Intersite BV (Netherlands)"},
776 | {"FUJ", "Fujitsu Ten Corporation of America"},
777 | {"FUR", "Furuno USA, Inc."},
778 | {"FWG", "Forschungsbereich Wasserchall and Geophysik WTD 71 (German Armed Forces Research Institute) (Germany)"},
779 | {"GAM", "GRE America, Inc."},
780 | {"GCA", "Gulf Cellular Associates"},
781 | {"GDC", "GNSS Differential Correction (Reserved for Future Use)"},
782 | {"GEC", "GEC Plessey Semiconductors"},
783 | {"GES", "Geostar Corporation"},
784 | {"GFC", "Graphic Controls Corporation"},
785 | {"GFV", "GFV Marine, Ltd."},
786 | {"GIL", "Gill Instruments Limited"},
787 | {"GIS", "Galax Integrated Systems"},
788 | {"GNV", "Geonav International"},
789 | {"GPI", "Global Positioning Instrument Corporation"},
790 | {"GPP", "GEO++ GmbH (Germany)"},
791 | {"GPR", "Global Positioning System Joint Program Office (Rockwell Collins)"},
792 | {"GRF", "Grafinta (Spain)"},
793 | {"GRM", "Garmin Corporation"},
794 | {"GSC", "Gold Star Company, Ltd."},
795 | {"GTI", "Genesis Technology International, Ltd."},
796 | {"GTO", "GRO Electronics"},
797 | {"GVE", "Guest Corporation"},
798 | {"GVT", "Great Valley Technology"},
799 | {"HAI", "Hydragraphic Associates, Ltd."},
800 | {"HAL", "HAL Communications Corporation"},
801 | {"HAR", "Harris Corporation"},
802 | {"HHS", "Hydel Hellas Skaltsaris, Ltd. (Shanghai)"},
803 | {"HIG", "Hy-Gain"},
804 | {"HIL", "Philips Navigation A/S (Denmark)"},
805 | {"HIT", "Hi-Tec"},
806 | {"HMS", "Hyde Marine Systems, Inc."},
807 | {"HOM", "Hoppe Marine GmbH (Germany)"},
808 | {"HPK", "Hewlett-Packard"},
809 | {"HRC", "Harco Manufacturing Company"},
810 | {"HRM", "[Unnamed]"},
811 | {"HRT", "Hart Systems, Inc."},
812 | {"HTI", "Heart Interface, Inc."},
813 | {"HUL", "Hull Electronics Company"},
814 | {"HWM", "Honeywell Marine Systems"},
815 | {"IBM", "IBM Microelectronics"},
816 | {"ICO", "Icom of America, Inc."},
817 | {"ICG", "Initiative Computing USA, Inc. / Initiative Computing AG"},
818 | {"IDS", "ICAN Marine (Canada)"},
819 | {"IFD", "International Fishing Devices"},
820 | {"IFI", "Instruments for Industry"},
821 | {"ILS", "Ideal Teknoloji Bilisim Cozumleri A/S (Turkey)"},
822 | {"IME", "Imperial Marine Equipment"},
823 | {"IMI", "International Marine Instruments"},
824 | {"IMM", "ITT Mackay Marine"},
825 | {"IMP", "Impulse Manufacturing, Inc."},
826 | {"IMR", "Ideal Technologies, Inc."},
827 | {"IMT", "International Marketing and Trading, Inc."},
828 | {"INM", "Inmar Electronics and Sales"},
829 | {"INT", "Intech, Inc."},
830 | {"IRT", "Intera Technologies, Ltd."},
831 | {"IST", "Innerspace Technology, Inc."},
832 | {"ITM", "Intermarine Electronics, Inc."},
833 | {"ITR", "Itera, Ltd."},
834 | {"IWW", "Inland Waterways (Germany)"},
835 | {"IXB", "iXblue"},
836 | {"JAN", "Jan Crystals"},
837 | {"JAS", "Jasco Research, Ltd."},
838 | {"JFR", "Ray Jefferson"},
839 | {"JLD", "Jargoon Limited"},
840 | {"JMT", "Japan Marine Telecommunications"},
841 | {"JPI", "JP Instruments"},
842 | {"JRC", "Japan Radio Company, Ltd."},
843 | {"JRI", "J-R Industries, Inc."},
844 | {"JTC", "J-Tech Associates, Inc."},
845 | {"JTR", "Jotron Radiosearch, Ltd."},
846 | {"KBE", "KB Electronics, Ltd."},
847 | {"KBM", "Kennebec Marine Company"},
848 | {"KEL", "Knudsen Engineering, Ltd."},
849 | {"KHU", "Kelvin Hughes, Ltd."},
850 | {"KLA", "Klein Associates, Inc."},
851 | {"KME", "Kyushu Matsushita Electric"},
852 | {"KML", "Kongsberg Mesotech, Ltd. (Canada)"},
853 | {"KMO", "Kongsberg Maritime A/S (Norway)"},
854 | {"KMR", "King Marine Radio Corporation"},
855 | {"KMS", "Kongsberg Maritime Subsea (Norway)"},
856 | {"KNC", "Kongsberg Norcontrols (Norway)"},
857 | {"KNG", "King Radio Corporation"},
858 | {"KOD", "Koden Electronics Company, Ltd."},
859 | {"KRA", "EDV Krajka (Germany)"},
860 | {"KRP", "Krupp International, Inc."},
861 | {"KST", "Kongsberg Seatex A/S (Norway)"},
862 | {"KVH", "KVH Company"},
863 | {"KYI", "Kyocera International, Inc."},
864 | {"L3A", "L3 Communications Recorders Division"},
865 | {"LAT", "Latitude Corporation"},
866 | {"L3I", "L-3 Interstate Electronics Corporation"},
867 | {"LCI", "Lasercraft, Inc."},
868 | {"LEC", "Lorain Electronics Corporation"},
869 | {"LEI", "Leica Geosystems Pty, Ltd."},
870 | {"LIT", "Litton Laser Systems"},
871 | {"LMM", "Lamarche Manufacturing Company"},
872 | {"LRD", "Lorad"},
873 | {"LSE", "Littlemore Scientific (ELSEC) Engineering"},
874 | {"LSP", "Laser Plot, Inc."},
875 | {"LST", "Lite Systems Engineering"},
876 | {"LTH", "Lars Thrane A/S (Denmark)"},
877 | {"LTF", "Littlefuse, Inc."},
878 | {"LTI", "Laser Technology, Inc."},
879 | {"LWR", "Lowrance Electronics Corporation"},
880 | {"MCA", "Canadian Marconi Company"},
881 | {"MCI", "Matsushita Communications (Japan)"},
882 | {"MCL", "Micrologic, Inc."},
883 | {"MDL", "Medallion Instruments, Inc."},
884 | {"MDS", "Marine Data Systems"},
885 | {"MEC", "Marine Engine Center, Inc."},
886 | {"MEG", "Maritec Engineering GmbH (Germany)"},
887 | {"MES", "Marine Electronics Services, Inc."},
888 | {"MEW", "Matsushita Electric Works (Japan)"},
889 | {"MFR", "Modern Products, Ltd."},
890 | {"MFW", "Frank W. Murphy Manufacturing"},
891 | {"MGN", "Magellen Systems Corporation"},
892 | {"MGS", "MG Electronic Sales Corporation"},
893 | {"MIE", "Mieco, Inc."},
894 | {"MIK", "Mikrolab GmbH (Germany)"},
895 | {"MIR", "Miros A/S (Norway)"},
896 | {"MIM", "Marconi International Marine"},
897 | {"MLE", "Martha Lake Electronics"},
898 | {"MLN", "Matlin Company"},
899 | {"MLP", "Marlin Products"},
900 | {"MLT", "Miller Technologies"},
901 | {"MMB", "Marsh-McBirney, Inc."},
902 | {"MME", "Marks Marine Engineering"},
903 | {"MMI", "Microwave Monolithics"},
904 | {"MMM", "Madman Marine"},
905 | {"MMP", "Metal Marine Pilot, Inc."},
906 | {"MMS", "Mars Marine Systems"},
907 | {"MMT", "Micro Modular Technologies"},
908 | {"MNI", "Micro-Now Instrument Company"},
909 | {"MNT", "Marine Technology"},
910 | {"MNX", "Marinex"},
911 | {"MOT", "Motorola Communications & Electronics"},
912 | {"MPI", "Megapulse, Inc."},
913 | {"MPN", "Memphis Net and Twine Company, Inc."},
914 | {"MQS", "Marquis Industries, Inc."},
915 | {"MRC", "Marinecomp, Inc."},
916 | {"MRE", "Morad Electronics Corporation"},
917 | {"MRP", "Mooring Products of New England"},
918 | {"MRR", "II Morrow, Inc."},
919 | {"MRS", "Marine Radio Service"},
920 | {"MSB", "Mitsubishi Electric Company, Ltd."},
921 | {"MSE", "Master Electronics"},
922 | {"MSF", "Microsoft Corporation"},
923 | {"MSM", "Master Mariner, Inc."},
924 | {"MST", "Mesotech Systems, Ltd."},
925 | {"MTA", "Marine Technical Associates"},
926 | {"MTD", "Maritel Data Services"},
927 | {"MTG", "Marine Technical Assistance Group"},
928 | {"MTI", "Mobile Telesystems, Inc."},
929 | {"MTK", "Martech, Inc."},
930 | {"MTL", "Marine Technologies, LLC"},
931 | {"MTR", "The MITRE Corporation"},
932 | {"MTS", "Mets, Inc."},
933 | {"MUR", "Murata Erie North America"},
934 | {"MVX", "Magnavox Advanced Products and Systems Company"},
935 | {"MXS", "Maxsea International"},
936 | {"MXX", "Maxxima Marine"},
937 | {"MYS", "Marine Electronics Company (South Korea)"},
938 | {"NAG", "Noris Automation GmbH (Germany)"},
939 | {"NAT", "Nautech, Ltd."},
940 | {"NAU", "Nauticast (a.k.a. Nauticall)"},
941 | {"NAV", "Navtec, Inc."},
942 | {"NCG", "Navcert, GmbH (Germany)"},
943 | {"NCT", "Navcom Technology, Inc."},
944 | {"NEC", "NEC Corporation"},
945 | {"NEF", "New England Fishing Gear"},
946 | {"NGC", "Northrop Grumman Maritime Systems"},
947 | {"NGS", "Navigation Sciences, Inc."},
948 | {"NIX", "L-3 Nautronix"},
949 | {"NLS", "Navigation Light Status (Reserved for Future Use)"},
950 | {"NMR", "Newmar"},
951 | {"NMX", "Nanometrics"},
952 | {"NOM", "Nav-Com, Inc."},
953 | {"NOR", "Nortech Surveys (Canada)"},
954 | {"NOS", "Northern Solutions A/S (Norway)"},
955 | {"NOV", "NovAtel Communications, Ltd."},
956 | {"NSI", "Noregon Systems, Inc."},
957 | {"NSL", "Navitron Systems, Ltd."},
958 | {"NSM", "Northstar Marine"},
959 | {"NTI", "Northstar Technologies, Inc."},
960 | {"NTK", "Novatech Designs, Ltd."},
961 | {"NTS", "Navtech Systems"},
962 | {"NUT", "Nautitech Pty, Ltd."},
963 | {"NVC", "Navico"},
964 | {"NVG", "NVS Technologies AG (Switzerland)"},
965 | {"NVL", "Navelec Marine Systems Sl. (Spain)"},
966 | {"NVO", "Navionics, s.p.a. (Italy)"},
967 | {"NVS", "Navstar"},
968 | {"NVT", "Novariant, Inc."},
969 | {"NWC", "Naval Warfare Center"},
970 | {"OAR", "On-Line Applications Research (OAR) Corporation"},
971 | {"OBS", "Observator Instruments"},
972 | {"OCC", "Occupation Control (Reserved for Future Use)"},
973 | {"ODE", "Ocean Data Equipment Corporation"},
974 | {"ODN", "Odin Electronics, Inc."},
975 | {"OHB", "OHB Systems"},
976 | {"OIN", "Ocean Instruments, Inc."},
977 | {"OKI", "Oki Electric Industry Company, Ltd."},
978 | {"OLY", "Navstard, Ltd. (Polytechnic Electronics)"},
979 | {"OMN", "Omnetics Corporation"},
980 | {"OMT", "Omnitech A/S (Norway)"},
981 | {"ONI", "Omskiy Nauchno Issledovatelskiy Institut Priborostroeniya (Russia)"},
982 | {"ORB", "Orbcomm"},
983 | {"ORE", "Ocean Research"},
984 | {"OSG", "Ocean Signal, Ltd."},
985 | {"OSI", "OSI Maritime Systems (was Offshore Systems International)"},
986 | {"OSL", "OSI Maritime Systems (was Offshore Systems, Ltd.)"},
987 | {"OSS", "Ocean Solution Systems"},
988 | {"OTK", "Ocean Technology"},
989 | {"PCE", "Pace"},
990 | {"PCM", "P-Sea Marine Systems"},
991 | {"PDC", "Pan Delta Controls, Ltd."},
992 | {"PDM", "Prodelco Marine Systems"},
993 | {"PLA", "Plath C Division of Litton Industries"},
994 | {"PLI", "Pilot Instruments"},
995 | {"PMI", "Pernicka Marine Instruments"},
996 | {"PMP", "Pacific Marine Products"},
997 | {"PNI", "PNI Sensors, Inc."},
998 | {"PNL", "Points North, Ltd."},
999 | {"POM", "POMS Engineering"},
1000 | {"PPL", "Pamarine Private, Ltd."},
1001 | {"PRK", "Perko, Inc."},
1002 | {"PSM", "Pearce-Simpson, Inc."},
1003 | {"PST", "Pointstar A/S (Denmark)"},
1004 | {"PTC", "Petro-Com"},
1005 | {"PTG", "PTI/Guest"},
1006 | {"PTH", "Pathcom, Inc."},
1007 | {"PVS", "Planevision Systems"},
1008 | {"QNQ", "QinetiQ (United Kingdom)"},
1009 | {"QRC", "QinetiQ (United Kingdom)"},
1010 | {"QWE", "Qwerty Elektronik AB (Sweden)"},
1011 | {"QZM", "[Unnamed]"},
1012 | {"Q2N", "QQN Navigation ABS"},
1013 | {"RAC", "Racal Marine, Inc."},
1014 | {"RAE", "RCA Astro-Electronics"},
1015 | {"RAF", "Robins Air Force (USAF)"},
1016 | {"RAK", "Rockson Automation Kiel"},
1017 | {"RAY", "Raytheon Marine Company"},
1018 | {"RCA", "RCA Service Company"},
1019 | {"RCH", "Roach Engineering"},
1020 | {"RCI", "Rochester Instruments, Inc."},
1021 | {"RCQ", "QinetiQ (United Kingdom)"},
1022 | {"RDC", "U.S. Coast Guard Research & Development Center"},
1023 | {"RDI", "Radar Devices"},
1024 | {"RDM", "Ray-Dar Manufacturing Company"},
1025 | {"REC", "Ross Engineering Company"},
1026 | {"RFP", "Rolfite Products, Inc."},
1027 | {"RGC", "RCA Global Communications"},
1028 | {"RGL", "Riegl Laser Measurement Systems"},
1029 | {"RGY", "Regency Electronics, Inc."},
1030 | {"RHO", "Rhotheta Elektronik GmbH (Germany)"},
1031 | {"RHM", "RH Marine"},
1032 | {"RLK", "Reelektronika NL (Netherlands)"},
1033 | {"RME", "Racal Marine Electronics"},
1034 | {"RMR", "RCA Missile and Radar"},
1035 | {"RSL", "Ross Laboratories, Inc."},
1036 | {"RSM", "Robertson-Shipmate USA"},
1037 | {"RTH", "Parthus"},
1038 | {"RTN", "Robertson Tritech Nyaskaien (Norway)"},
1039 | {"RWC", "Rockwell Collins"},
1040 | {"RWI", "Rockwell International"},
1041 | {"SAA", "Satronika Sl. (Spain)"},
1042 | {"SAB", "VDE Satellite Selective Addressed Binary and Safety Related Message (Reserved for Future Use)"},
1043 | {"SAE", "STN Atlas Elektronik GmbH (Germany)"},
1044 | {"SAF", "Safemine"},
1045 | {"SAI", "SAIT, Inc."},
1046 | {"SAJ", "SAJ Instrument AB (Finland)"},
1047 | {"SAM", "SAM Electronics GmbH (Germany)"},
1048 | {"SAL", "Consilium Marine AB (Sweden)"},
1049 | {"SAP", "Systems Engineering & Assessment, Ltd."},
1050 | {"SAT", "Satloc"},
1051 | {"SBB", "VDE Satellite Broadcast Binary Message (Reserved for Future Use)"},
1052 | {"SBG", "SBG Systems"},
1053 | {"SBR", "Sea-Bird Electronics, Inc."},
1054 | {"SCL", "Sokkia Company, Ltd."},
1055 | {"SCM", "Scandinavian Microsystems A/S (Norway)"},
1056 | {"SCO", "Simoco Telecommunications, Ltd."},
1057 | {"SCR", "Signalcrafters, Inc."},
1058 | {"SDM", "VDE Satellite VHF Data-Link Message (Reserved for Future Use)"},
1059 | {"SDN", "Sapien Design"},
1060 | {"SDO", "VDE Satellite VHF Data-Link Own-Vessel Report (Reserved for Future Use)"},
1061 | {"SEA", "Sea, Inc."},
1062 | {"SEC", "Sercel Electronics of Canada"},
1063 | {"SEE", "Seetrac (a.k.a. Global Marine Tracking)"},
1064 | {"SEL", "Selection Report (Reserved for Future Use)"},
1065 | {"SEM", "Semtech, Ltd."},
1066 | {"SEP", "Steel and Engine Products"},
1067 | {"SER", "Sercel France"},
1068 | {"SFN", "Seafarer Navigation International"},
1069 | {"SGB", "VDE Satellite Geographical Addressed Binary and Safety Message (Reserved for Future Use)"},
1070 | {"SGC", "SGC, Inc."},
1071 | {"SGN", "Signav"},
1072 | {"SHI", "Shine Micro, Inc."},
1073 | {"SIG", "Signet, Inc."},
1074 | {"SIM", "Simrad, Inc."},
1075 | {"SKA", "Skantek Corporation"},
1076 | {"SKP", "Skipper Electronics A/S (Norway)"},
1077 | {"SLI", "Starlink, Inc."},
1078 | {"SLM", "Steering Location Mode (Reserved for Future Use)"},
1079 | {"SMC", "Solis Marine Consultants"},
1080 | {"SMD", "ShipModul Customware (Netherlands)"},
1081 | {"SME", "Shakespeare Marine Electronics"},
1082 | {"SMF", "Seattle Marine and Fishing Supply Company"},
1083 | {"SMI", "Sperry Marine, Inc."},
1084 | {"SMK", "VDE Satellite Addressed and Broadcast Message Acknowledgement (Reserved for Future Use)"},
1085 | {"SML", "Simerl Instruments"},
1086 | {"SMT", "SRT Marine Technology, Ltd. (United Kingdom)"},
1087 | {"SMV", "SafetyNet Message Vessel (Reserved for Future Use)"},
1088 | {"SNP", "Science Applications International Corporation"},
1089 | {"SNV", "STARNAV Corporation (Canada)"},
1090 | {"SNY", "Sony Corporation - Mobile Electronics"},
1091 | {"SOM", "Sound Marine Electronics"},
1092 | {"SON", "Sonardyne International, Ltd. (United Kingdom)"},
1093 | {"SOV", "Sell Overseas America"},
1094 | {"SPL", "Spelmar"},
1095 | {"SPT", "Sound Powered Telephone"},
1096 | {"SRC", "Stellar Research Group"},
1097 | {"SRD", "SRD Labs"},
1098 | {"SRF", "SIRF Technology, Inc."},
1099 | {"SRP", "System Function ID Resolution Protocol (Reserved for Future Use)"},
1100 | {"SRS", "Scientific Radio Systems, Inc."},
1101 | {"SRT", "Standard Radio and Telefon AB (Sweden)"},
1102 | {"SRV", "(Reserved for Future Use)"},
1103 | {"SSA", "(Reserved for Future Use)"},
1104 | {"SSC", "Swedish Space Corporation"},
1105 | {"SSD", "Saab AB, Security & Defense Solutions, Command and Control Systems Division (Sweden)"},
1106 | {"SSE", "Seven Star Electronics"},
1107 | {"SSI", "Sea Scout Industries"},
1108 | {"SSN", "Septentrio"},
1109 | {"STC", "Standard Communications"},
1110 | {"STI", "Sea-Temp Instrument Corporation"},
1111 | {"STK", "Seatechnik, Ltd. (a.k.a. Trelleborg Marine Systems) (United Kingdom)"},
1112 | {"STL", "Streamline Technology, Ltd."},
1113 | {"STM", "SI-TEX Marine Electronics"},
1114 | {"STO", "Stowe Marine Electronics"},
1115 | {"STT", "Saab TransponderTech AB (Sweden)"},
1116 | {"SVY", "Savoy Electronics"},
1117 | {"SWI", "Swoffer Marine Instruments"},
1118 | {"SWT", "Swift Navigation, Inc."},
1119 | {"SYE", "Samyung ENC Company, Ltd. (South Korea)"},
1120 | {"SYN", "Synergy Systems, LLC"},
1121 | {"TAB", "VDE Terrestrial Selective Addressed Binary and Safety Related Message (Reserved for Future Use)"},
1122 | {"TBB", "Thompson Brothers Boat Manufacturing"},
1123 | {"TBM", "VDE Terrestrial Broadcast Binary Message (Reserved for Future Use)"},
1124 | {"TCN", "Trade Commission of Norway"},
1125 | {"TDI", "Teledyne RD Instruments, Inc."},
1126 | {"TDL", "Tideland Signal"},
1127 | {"TDM", "VDE Terrestrial VHF Data-Link Message (Reserved for Future Use)"},
1128 | {"TDO", "VDE Terrestrial VHF Data-Link Own-Vessel Report (Reserved for Future Use)"},
1129 | {"TEL", "Plessey Tellumat (South Africa)"},
1130 | {"TES", "Thales Electronic Systems GmbH (Germany)"},
1131 | {"TGB", "VDE Terrestrial Geographical Addressed Binary and Safety Message (Reserved for Future Use)"},
1132 | {"THR", "Thrane and Thrane A/A (Denmark)"},
1133 | {"TKI", "Tokyo Keiki, Inc. (Japan)"},
1134 | {"TLS", "Telesystems"},
1135 | {"TMK", "VDE Terrestrial Addressed and Broadcast Message Acknowledgement (Reserved for Future Use)"},
1136 | {"TMS", "Trelleborg Marine Systems"},
1137 | {"TMT", "Tamtech, Ltd."},
1138 | {"TNL", "Trimble Navigation, Inc."},
1139 | {"TOP", "Topcon Positioning Systems, Inc."},
1140 | {"TPL", "Totem Plus, Ltd."},
1141 | {"TRC", "Tracor, Inc."},
1142 | {"TRS", "Travroute Software"},
1143 | {"TSG", "(Reserved for Future Use)"},
1144 | {"TSI", "Techsonic Industries, Inc."},
1145 | {"TSS", "Teledyne TSS, Ltd. (United Kingdom)"},
1146 | {"TTK", "Talon Technology Corporation"},
1147 | {"TTS", "Transtector Systems, Inc."},
1148 | {"TYC", "Vincotech GmbH (formerly Tyco Electronics) (Germany)"},
1149 | {"TWC", "Transworld Communications"},
1150 | {"TWS", "Telit Location Solutions, a Division of Telit Wireless Solutions"},
1151 | {"TXI", "Texas Instruments, Inc."},
1152 | {"UBX", "u-blox AG (Switzerland)"},
1153 | {"UCG", "United States Coast Guard"},
1154 | {"UEL", "Ultra Electronics, Ltd."},
1155 | {"UME", "UMEC"},
1156 | {"UNF", "Uniforce Electronics Company"},
1157 | {"UNI", "Uniden Corporation of America"},
1158 | {"UNP", "Unipas, Inc."},
1159 | {"URS", "UrsaNav, Inc."},
1160 | {"VAN", "Vanner, Inc."},
1161 | {"VAR", "Varian Eimac Associates"},
1162 | {"VBC", "Docking Speed Log (Reserved for Future Use)"},
1163 | {"VCM", "Videocom"},
1164 | {"VDB", "Bertold Vandenbergh"},
1165 | {"VEA", "Vard Electro A/S (Norway)"},
1166 | {"VEC", "Vectron International"},
1167 | {"VEX", "Vexilar"},
1168 | {"VIS", "Vessel Information Systems"},
1169 | {"VMR", "Vast Marketing Corporation"},
1170 | {"VSP", "Vesper Marine"},
1171 | {"VXS", "Vertex Standard"},
1172 | {"WAL", "Walport USA"},
1173 | {"WBE", "Wamblee, s.r.l. (Italy)"},
1174 | {"WBG", "Westberg Manufacturing"},
1175 | {"WBR", "Wesbar Corporation"},
1176 | {"WEC", "Westinghouse Electric Corporation"},
1177 | {"WEI", "Weidmueller Interface GmbH (Germany)"},
1178 | {"WCI", "Wi-Sys Communications"},
1179 | {"WDC", "Weatherdock Corporation"},
1180 | {"WHA", "W-H Autopilots, Inc."},
1181 | {"WMM", "Wait Manufacturing and Marine Sales Company"},
1182 | {"WMR", "Wesmar Electronics"},
1183 | {"WNG", "Winegard Company"},
1184 | {"WOE", "Woosung Engineering Company, Ltd. (South Korea)"},
1185 | {"WSE", "Wilson Electronics Corporation"},
1186 | {"WST", "West Electronics, Ltd."},
1187 | {"WTC", "Watercom"},
1188 | {"XEL", "3XEL Electronics and Navigation Systems, s.r.l. (Italy)"},
1189 | {"YAS", "Yaesu Electronics (Japan)"},
1190 | {"YDK", "Yokogawa Denshikiki Company, Ltd. (Japan)"},
1191 | {"YSH", "Standard Horizon Yaesu"},
1192 | {"ZNS", "Zinnos, Inc. (South Korea)"},
1193 | {NULL((void*)0), NULL((void*)0)}};
1194 |
1195 | // List of GPS Quality Indicator (Source: NMEA Revealed by Eric S. Raymond, https://gpsd.gitlab.io/gpsd/NMEA.html, retrieved 2023-01-26)
1196 | static const string_string known_gps_quality_indicators[] = {
1197 | {"0", "Fix not available"},
1198 | {"1", "GPS fix"},
1199 | {"2", "Differential GPS fix"},
1200 | {"3", "PPS fix"},
1201 | {"4", "Real Time Kinematic"},
1202 | {"5", "Float Real Time Kinematic"},
1203 | {"6", "Estimated (dead reckoning)"},
1204 | {"7", "Manual input mode"},
1205 | {"8", "Simulation mode"},
1206 | {NULL((void*)0), NULL((void*)0)}};
1207 |
1208 | // List of status indicators (Source: NMEA Revealed by Eric S. Raymond, https://gpsd.gitlab.io/gpsd/NMEA.html, retrieved 2024-04-19)
1209 | static const string_string known_status_indicators[] = {
1210 | {"A", "Valid/Active"},
1211 | {"V", "Invalid/Void"},
1212 | {NULL((void*)0), NULL((void*)0)}};
1213 |
1214 | // List of FAA Mode Indicator (Source: NMEA Revealed by Eric S. Raymond, https://gpsd.gitlab.io/gpsd/NMEA.html, retrieved 2024-04-19)
1215 | static const string_string known_faa_mode_indicators[] = {
1216 | {"A", "Autonomous mode"},
1217 | {"C", "Quectel Querk, Caution"},
1218 | {"D", "Differential Mode"},
1219 | {"E", "Estimated (dead-reckoning) mode"},
1220 | {"F", "RTK Float mode"},
1221 | {"M", "Manual Input Mode"},
1222 | {"N", "Data Not Valid"},
1223 | {"P", "Precise"},
1224 | {"R", "RTK Integer mode"},
1225 | {"S", "Simulated Mode"},
1226 | {"U", "Quectel Querk, Unsafe"},
1227 | {NULL((void*)0), NULL((void*)0)}};
1228 |
1229 | static uint8_t calculate_checksum(tvbuff_t *tvb, const int start, const int length)
1230 | {
1231 | uint8_t checksum = 0;
1232 | for (int i = start; i < start + length; i++)
1233 | {
1234 | checksum ^= tvb_get_uint8(tvb, i);
1235 | }
1236 | return checksum;
1237 | }
1238 |
1239 | /* Find first occurrence of a field separator in tvbuff, starting at offset. Searches
1240 | * to end of tvbuff.
1241 | * Returns the offset of the found separator.
1242 | * If separator is not found, return the offset of end of tvbuff.
1243 | * If offset is out of bounds, return the offset of end of tvbuff.
1244 | **/
1245 | static int
1246 | tvb_find_end_of_nmea0183_field(tvbuff_t *tvb, const int offset)
1247 | {
1248 | if (tvb_captured_length_remaining(tvb, offset) == 0)
1249 | {
1250 | return tvb_captured_length(tvb);
1251 | }
1252 |
1253 | int end_of_field_offset = tvb_find_uint8(tvb, offset, -1, ',');
1254 | if (end_of_field_offset == -1)
1255 | {
1256 | return tvb_captured_length(tvb);
1257 | }
1258 | return end_of_field_offset;
1259 | }
1260 |
1261 | /* Add a zero length item which indicates an expected but missing field */
1262 | static proto_item *
1263 | proto_tree_add_missing_field(proto_tree *tree, packet_info *pinfo, int hf, tvbuff_t *tvb,
1264 | const int offset)
1265 | {
1266 | proto_item *ti = NULL((void*)0);
1267 | ti = proto_tree_add_item(tree, hf, tvb, offset, 0, ENC_ASCII0x00000000);
1268 | proto_item_append_text(ti, "[missing]");
1269 | expert_add_info(pinfo, ti, &ei_nmea0183_field_missing);
1270 | return ti;
1271 | }
1272 |
1273 | /* Dissect a time field. The field is split into a tree with hour, minute and second elements.
1274 | * Returns length including separator
1275 | **/
1276 | static int
1277 | dissect_nmea0183_field_time(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, int offset,
1278 | int hf_time, int hf_hour, int hf_minute, int hf_second, int ett_time)
1279 | {
1280 | if (offset > (int)tvb_captured_length(tvb))
1281 | {
1282 | proto_tree_add_missing_field(tree, pinfo, hf_time, tvb, tvb_captured_length(tvb));
1283 | return 0;
1284 | }
1285 |
1286 | proto_item *ti = NULL((void*)0);
1287 | int end_of_field_offset = tvb_find_end_of_nmea0183_field(tvb, offset);
1288 | ti = proto_tree_add_item(tree, hf_time, tvb, offset, end_of_field_offset - offset, ENC_ASCII0x00000000);
1289 | if (end_of_field_offset - offset == 0)
1290 | {
1291 | proto_item_append_text(ti, ": [empty]");
1292 | }
1293 | else if (end_of_field_offset - offset >= 6)
1294 | {
1295 | const uint8_t *hour = NULL((void*)0);
1296 | const uint8_t *minute = NULL((void*)0);
1297 | const uint8_t *second = NULL((void*)0);
1298 | proto_tree *time_subtree = proto_item_add_subtree(ti, ett_time);
1299 |
1300 | proto_tree_add_item_ret_string(time_subtree, hf_hour,
1301 | tvb, offset, 2, ENC_ASCII0x00000000,
1302 | pinfo->pool, &hour);
1303 |
1304 | proto_tree_add_item_ret_string(time_subtree, hf_minute,
1305 | tvb, offset + 2, 2, ENC_ASCII0x00000000,
1306 | pinfo->pool, &minute);
1307 |
1308 | proto_tree_add_item_ret_string(time_subtree, hf_second,
1309 | tvb, offset + 4, end_of_field_offset - offset - 4,
1310 | ENC_ASCII0x00000000, pinfo->pool, &second);
1311 |
1312 | proto_item_append_text(ti, ": %s:%s:%s", hour, minute, second);
1313 | }
1314 | else
1315 | {
1316 | expert_add_info(pinfo, ti, &ei_nmea0183_field_time_too_short);
1317 | }
1318 | return end_of_field_offset - offset + 1;
1319 | }
1320 |
1321 | /* Dissect a single field containing a dimensionless value. Returns length including separator */
1322 | static int
1323 | dissect_nmea0183_field(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, int offset, int hf, const char *suffix, const string_string *str_str)
1324 | {
1325 | const char* field_str = NULL((void*)0);
1326 |
1327 | if (offset > (int)tvb_captured_length(tvb))
1328 | {
1329 | proto_tree_add_missing_field(tree, pinfo, hf, tvb, tvb_captured_length(tvb));
1330 | return 0;
1331 | }
1332 |
1333 | proto_item *ti = NULL((void*)0);
1334 | int end_of_field_offset = tvb_find_end_of_nmea0183_field(tvb, offset);
1335 | ti = proto_tree_add_item_ret_string(tree, hf, tvb, offset, end_of_field_offset - offset, ENC_ASCII0x00000000, pinfo->pool, (const uint8_t**)&field_str);
1336 | if (end_of_field_offset - offset == 0)
1337 | {
1338 | proto_item_append_text(ti, "[empty]");
1339 | }
1340 | else if (suffix != NULL((void*)0))
1341 | {
1342 | proto_item_append_text(ti, " %s", suffix);
1343 | }
1344 | if ((str_str)&&(field_str)) {
1345 | proto_item_append_text(ti, " - %s", str_to_str_wmem(pinfo->pool, field_str, str_str, " "));
1346 | }
1347 | return end_of_field_offset - offset + 1;
1348 | }
1349 |
1350 | /* Dissect a latitude/longitude direction field.
1351 | * Returns length including separator
1352 | **/
1353 | static int
1354 | dissect_nmea0183_field_latlong_direction(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree,
1355 | int offset, int hf,
1356 | wmem_allocator_t *scope, const uint8_t **retval)
1357 | {
1358 | if (offset > (int)tvb_captured_length(tvb))
1359 | {
1360 | proto_tree_add_missing_field(tree, pinfo, hf, tvb, tvb_captured_length(tvb));
1361 | return 0;
1362 | }
1363 |
1364 | int end_of_field_offset = tvb_find_end_of_nmea0183_field(tvb, offset);
1365 | proto_item *ti = proto_tree_add_item_ret_string(tree, hf,
1366 | tvb, offset, end_of_field_offset - offset, ENC_ASCII0x00000000,
1367 | scope, retval);
1368 | if (end_of_field_offset - offset == 0)
1369 | {
1370 | if (retval == NULL((void*)0))
1371 | {
1372 | proto_item_append_text(ti, "[empty]");
1373 | }
1374 | else
1375 | {
1376 | proto_item_append_text(ti, "[missing]");
1377 | expert_add_info(pinfo, ti, &ei_nmea0183_field_missing);
1378 | }
1379 | }
1380 | return end_of_field_offset - offset + 1;
1381 | }
1382 |
1383 | /* Dissect a latitude field + direction field. The fields are split into a tree with degree, minute and direction elements.
1384 | * Returns length including separator
1385 | **/
1386 | static int
1387 | dissect_nmea0183_field_latitude(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, int offset,
1388 | int hf_latitude, int hf_degree, int hf_minute, int hf_direction, int ett_latitude)
1389 | {
1390 | if (offset > (int)tvb_captured_length(tvb))
1391 | {
1392 | proto_tree_add_missing_field(tree, pinfo, hf_latitude, tvb, tvb_captured_length(tvb));
1393 | return 0;
1394 | }
1395 |
1396 | proto_item *ti = NULL((void*)0);
1397 | int end_of_field_offset = tvb_find_end_of_nmea0183_field(tvb, offset);
1398 | ti = proto_tree_add_item(tree, hf_latitude, tvb, offset, end_of_field_offset - offset, ENC_ASCII0x00000000);
1399 | if (end_of_field_offset - offset == 0)
1400 | {
1401 | proto_item_append_text(ti, ": [empty]");
1402 |
1403 | end_of_field_offset += dissect_nmea0183_field_latlong_direction(tvb, pinfo, tree, end_of_field_offset + 1, hf_direction, NULL((void*)0), NULL((void*)0));
1404 | }
1405 | else if (end_of_field_offset - offset >= 4)
1406 | {
1407 | const uint8_t *degree = NULL((void*)0);
1408 | const uint8_t *minute = NULL((void*)0);
1409 | const uint8_t *direction = NULL((void*)0);
1410 | proto_tree *latitude_subtree = proto_item_add_subtree(ti, ett_latitude);
1411 |
1412 | proto_tree_add_item_ret_string(latitude_subtree, hf_degree,
1413 | tvb, offset, 2,
1414 | ENC_ASCII0x00000000, pinfo->pool, &degree);
1415 |
1416 | proto_tree_add_item_ret_string(latitude_subtree, hf_minute,
1417 | tvb, offset + 2, end_of_field_offset - offset - 2,
1418 | ENC_ASCII0x00000000, pinfo->pool, &minute);
1419 |
1420 | end_of_field_offset += dissect_nmea0183_field_latlong_direction(tvb, pinfo, latitude_subtree, end_of_field_offset + 1, hf_direction, pinfo->pool, &direction);
1421 |
1422 | proto_item_append_text(ti, ": %s° %s' %s", degree, minute, direction);
1423 | }
1424 | else
1425 | {
1426 | expert_add_info(pinfo, ti, &ei_nmea0183_field_latitude_too_short);
1427 |
1428 | end_of_field_offset += dissect_nmea0183_field_latlong_direction(tvb, pinfo, tree, end_of_field_offset + 1, hf_direction, NULL((void*)0), NULL((void*)0));
1429 | }
1430 | return end_of_field_offset - offset + 1;
1431 | }
1432 |
1433 | /* Dissect a longitude field + direction field. The fields are split into a tree with degree, minute and direction elements.
1434 | * Returns length including separator
1435 | **/
1436 | static int
1437 | dissect_nmea0183_field_longitude(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, int offset,
1438 | int hf_longitude, int hf_degree, int hf_minute, int hf_direction, int ett_latitude)
1439 | {
1440 | if (offset > (int)tvb_captured_length(tvb))
1441 | {
1442 | proto_tree_add_missing_field(tree, pinfo, hf_longitude, tvb, tvb_captured_length(tvb));
1443 | return 0;
1444 | }
1445 |
1446 | proto_item *ti = NULL((void*)0);
1447 | int end_of_field_offset = tvb_find_end_of_nmea0183_field(tvb, offset);
1448 | ti = proto_tree_add_item(tree, hf_longitude, tvb, offset, end_of_field_offset - offset, ENC_ASCII0x00000000);
1449 | if (end_of_field_offset - offset == 0)
1450 | {
1451 | proto_item_append_text(ti, ": [empty]");
1452 |
1453 | end_of_field_offset += dissect_nmea0183_field_latlong_direction(tvb, pinfo, tree, end_of_field_offset + 1, hf_direction, NULL((void*)0), NULL((void*)0));
1454 | }
1455 | else if (end_of_field_offset - offset >= 5)
1456 | {
1457 | const uint8_t *degree = NULL((void*)0);
1458 | const uint8_t *minute = NULL((void*)0);
1459 | const uint8_t *direction = NULL((void*)0);
1460 | proto_tree *longitude_subtree = proto_item_add_subtree(ti, ett_latitude);
1461 |
1462 | proto_tree_add_item_ret_string(longitude_subtree, hf_degree,
1463 | tvb, offset, 3,
1464 | ENC_ASCII0x00000000, pinfo->pool, &degree);
1465 |
1466 | proto_tree_add_item_ret_string(longitude_subtree, hf_minute,
1467 | tvb, offset + 3, end_of_field_offset - offset - 3,
1468 | ENC_ASCII0x00000000, pinfo->pool, &minute);
1469 |
1470 | end_of_field_offset += dissect_nmea0183_field_latlong_direction(tvb, pinfo, longitude_subtree, end_of_field_offset + 1, hf_direction, pinfo->pool, &direction);
1471 |
1472 | proto_item_append_text(ti, ": %s° %s' %s", degree, minute, direction);
1473 | }
1474 | else
1475 | {
1476 | expert_add_info(pinfo, ti, &ei_nmea0183_field_longitude_too_short);
1477 |
1478 | end_of_field_offset += dissect_nmea0183_field_latlong_direction(tvb, pinfo, tree, end_of_field_offset + 1, hf_direction, NULL((void*)0), NULL((void*)0));
1479 | }
1480 | return end_of_field_offset - offset + 1;
1481 | }
1482 |
1483 | /* Dissect a required gps quality field. Returns length including separator */
1484 | static int
1485 | dissect_nmea0183_field_gps_quality(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, int offset, int hf)
1486 | {
1487 | if (offset > (int)tvb_captured_length(tvb))
1488 | {
1489 | proto_tree_add_missing_field(tree, pinfo, hf, tvb, tvb_captured_length(tvb));
1490 | return 0;
1491 | }
1492 |
1493 | proto_item *ti = NULL((void*)0);
1494 | int end_of_field_offset = tvb_find_end_of_nmea0183_field(tvb, offset);
1495 | const char *quality = NULL((void*)0);
1496 | ti = proto_tree_add_item_ret_string(tree, hf,
1497 | tvb, offset, end_of_field_offset - offset, ENC_ASCII0x00000000,
1498 | pinfo->pool, (const uint8_t**)&quality);
1499 | if (end_of_field_offset - offset == 0)
1500 | {
1501 | proto_item_append_text(ti, "[missing]");
1502 | expert_add_info(pinfo, ti, &ei_nmea0183_field_missing);
1503 | }
1504 | else
1505 | {
1506 | proto_item_append_text(ti, " (%s)", str_to_str_wmem(pinfo->pool, quality, known_gps_quality_indicators, "Unknown quality"));
1507 | }
1508 | return end_of_field_offset - offset + 1;
1509 | }
1510 |
1511 | /* Dissect a single field containing a fixed text.
1512 | The text of the field must match the `expected_text` or expert info `invalid_ei` is
1513 | added to the field. An empty field is allowed. Returns length including separator */
1514 | static int
1515 | dissect_nmea0183_field_fixed_text(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, int offset, int hf,
1516 | const char *expected_text, expert_field *invalid_ei)
1517 | {
1518 | if (offset > (int)tvb_captured_length(tvb))
1519 | {
1520 | proto_tree_add_missing_field(tree, pinfo, hf, tvb, tvb_captured_length(tvb));
1521 | return 0;
1522 | }
1523 |
1524 | proto_item *ti = NULL((void*)0);
1525 | const char *text = NULL((void*)0);
1526 | int end_of_field_offset = tvb_find_end_of_nmea0183_field(tvb, offset);
1527 | ti = proto_tree_add_item_ret_string(tree, hf,
1528 | tvb, offset, end_of_field_offset - offset, ENC_ASCII0x00000000,
1529 | pinfo->pool, (const uint8_t**)&text);
1530 | if (end_of_field_offset - offset == 0)
1531 | {
1532 | proto_item_append_text(ti, "[empty]");
1533 | }
1534 | else if (g_ascii_strcasecmp(text, expected_text) != 0)
1535 | {
1536 | expert_add_info(pinfo, ti, invalid_ei);
1537 | }
1538 | return end_of_field_offset - offset + 1;
1539 | }
1540 |
1541 | /* Dissect a optional FAA mode indicator field. Returns length including separator */
1542 | static int
1543 | dissect_nmea0183_field_faa_mode(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, int offset, int hf)
1544 | {
1545 | if (offset > (int)tvb_captured_length(tvb))
1546 | {
1547 | proto_tree_add_missing_field(tree, pinfo, hf, tvb, tvb_captured_length(tvb));
1548 | return 0;
1549 | }
1550 |
1551 | proto_item *ti = NULL((void*)0);
1552 | int end_of_field_offset = tvb_find_end_of_nmea0183_field(tvb, offset);
1553 | const char *mode = NULL((void*)0);
1554 | ti = proto_tree_add_item_ret_string(tree, hf,
1555 | tvb, offset, end_of_field_offset - offset, ENC_ASCII0x00000000,
1556 | pinfo->pool, (const uint8_t**)&mode);
1557 | if (end_of_field_offset - offset == 0)
1558 | {
1559 | proto_item_append_text(ti, "[empty]");
1560 | }
1561 | else
1562 | {
1563 | proto_item_append_text(ti, " (%s)", str_to_str_wmem(pinfo->pool, mode, known_faa_mode_indicators, "Unknown FAA mode"));
1564 | }
1565 | return end_of_field_offset - offset + 1;
1566 | }
1567 |
1568 | /* Dissect a optional A/V status field. Returns length including separator */
1569 | static int
1570 | dissect_nmea0183_field_status(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, int offset, int hf)
1571 | {
1572 | if (offset > (int)tvb_captured_length(tvb))
1573 | {
1574 | proto_tree_add_missing_field(tree, pinfo, hf, tvb, tvb_captured_length(tvb));
1575 | return 0;
1576 | }
1577 |
1578 | proto_item *ti = NULL((void*)0);
1579 | int end_of_field_offset = tvb_find_end_of_nmea0183_field(tvb, offset);
1580 | const char *mode = NULL((void*)0);
1581 | ti = proto_tree_add_item_ret_string(tree, hf,
1582 | tvb, offset, end_of_field_offset - offset, ENC_ASCII0x00000000,
1583 | pinfo->pool, (const uint8_t**)&mode);
1584 | if (end_of_field_offset - offset == 0)
1585 | {
1586 | proto_item_append_text(ti, "[empty]");
1587 | }
1588 | else
1589 | {
1590 | proto_item_append_text(ti, " (%s)", str_to_str_wmem(pinfo->pool, mode, known_status_indicators, "Unknown status"));
1591 | }
1592 | return end_of_field_offset - offset + 1;
1593 | }
1594 |
1595 | /* Dissect a ALR sentence. */
1596 | /*
1597 | * $--ALR,hhmmss.ss,xxx,A,A,c--c*hh<CR><LF>
1598 | */
1599 | static const string_string alarm_condition_str[] = {
1600 | {"A", "Threshold exceeded"},
1601 | {"V", "Threshold not exceeded"},
1602 | { NULL((void*)0), NULL((void*)0)},
1603 | };
1604 |
1605 | static const string_string alarm_ack_state_str[] = {
1606 | {"A", "Acknowledged"},
1607 | {"V", "Unacknowledged"},
1608 | { NULL((void*)0), NULL((void*)0)},
1609 | };
1610 |
1611 | static int
1612 | dissect_nmea0183_sentence_alr(tvbuff_t* tvb, packet_info* pinfo, proto_tree* tree)
1613 | {
1614 | int offset = 0;
1615 |
1616 | proto_tree* subtree = proto_tree_add_subtree(tree, tvb, offset,
1617 | tvb_captured_length(tvb), ett_nmea0183_sentence, NULL((void*)0), "ALR sentence - Set Alarm State");
1618 |
1619 | /* hhmmss.ss */
1620 | offset += dissect_nmea0183_field_time(tvb, pinfo, subtree, offset, hf_nmea0183_alr_time,
1621 | hf_nmea0183_alr_time_hour, hf_nmea0183_alr_time_minute,
1622 | hf_nmea0183_alr_time_second, ett_nmea0183_alr_time);
1623 | /* xxx Unique alarm number (identifier) at alarm source */
1624 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_alr_alarm_id, NULL((void*)0), NULL((void*)0));
1625 | /* Alarm condition (A = threshold exceeded, V = not exceeded) */
1626 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_alr_alarm_cond, NULL((void*)0), alarm_condition_str);
1627 | /* Alarm’s acknowledge state, A= acknowledged, V= unacknowledged*/
1628 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_alr_alarm_ack_st, NULL((void*)0), alarm_ack_state_str);
1629 | /* c--c Alarm’s description text*/
1630 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_alr_alarm_desc_txt, NULL((void*)0), NULL((void*)0));
| Value stored to 'offset' is never read
1631 |
1632 | return tvb_captured_length(tvb);
1633 | }
1634 |
1635 | /* Dissect a DPT sentence. */
1636 | static int
1637 | dissect_nmea0183_sentence_dpt(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree)
1638 | {
1639 | int offset = 0;
1640 |
1641 | proto_tree *subtree = proto_tree_add_subtree(tree, tvb, offset,
1642 | tvb_captured_length(tvb), ett_nmea0183_sentence, NULL((void*)0), "DPT sentence - Depth of Water");
1643 |
1644 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_dpt_depth, "meter", NULL((void*)0));
1645 |
1646 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_dpt_offset, "meter", NULL((void*)0));
1647 |
1648 | dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_dpt_max_range, "meter", NULL((void*)0));
1649 |
1650 | return tvb_captured_length(tvb);
1651 | }
1652 |
1653 | /* Dissect a GGA sentence. The time, latitude and longitude fields is split into individual parts. */
1654 | static int
1655 | dissect_nmea0183_sentence_gga(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree)
1656 | {
1657 | int offset = 0;
1658 |
1659 | proto_tree *subtree = proto_tree_add_subtree(tree, tvb, offset,
1660 | tvb_captured_length(tvb), ett_nmea0183_sentence,
1661 | NULL((void*)0), "GGA sentence - Global Positioning System Fix");
1662 |
1663 | offset += dissect_nmea0183_field_time(tvb, pinfo, subtree, offset, hf_nmea0183_gga_time,
1664 | hf_nmea0183_gga_time_hour, hf_nmea0183_gga_time_minute,
1665 | hf_nmea0183_gga_time_second, ett_nmea0183_gga_time);
1666 |
1667 | offset += dissect_nmea0183_field_latitude(tvb, pinfo, subtree, offset, hf_nmea0183_gga_latitude,
1668 | hf_nmea0183_gga_latitude_degree, hf_nmea0183_gga_latitude_minute,
1669 | hf_nmea0183_gga_latitude_direction, ett_nmea0183_gga_latitude);
1670 |
1671 | offset += dissect_nmea0183_field_longitude(tvb, pinfo, subtree, offset, hf_nmea0183_gga_longitude,
1672 | hf_nmea0183_gga_longitude_degree, hf_nmea0183_gga_longitude_minute,
1673 | hf_nmea0183_gga_longitude_direction, ett_nmea0183_gga_longitude);
1674 |
1675 | offset += dissect_nmea0183_field_gps_quality(tvb, pinfo, subtree, offset, hf_nmea0183_gga_quality);
1676 |
1677 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gga_number_satellites, NULL((void*)0), NULL((void*)0));
1678 |
1679 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gga_horizontal_dilution, "meter", NULL((void*)0));
1680 |
1681 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gga_altitude, "meter", NULL((void*)0));
1682 |
1683 | offset += dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_gga_altitude_unit,
1684 | "M", &ei_nmea0183_gga_altitude_unit_incorrect);
1685 |
1686 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gga_geoidal_separation, "meter", NULL((void*)0));
1687 |
1688 | offset += dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_gga_geoidal_separation_unit,
1689 | "M", &ei_nmea0183_gga_geoidal_separation_unit_incorrect);
1690 |
1691 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gga_age_dgps, "second", NULL((void*)0));
1692 |
1693 | dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gga_dgps_station, NULL((void*)0), NULL((void*)0));
1694 |
1695 | return tvb_captured_length(tvb);
1696 | }
1697 |
1698 | /* Dissect a GLL sentence. The latitude, longitude and time fields is split into individual parts. */
1699 | static int
1700 | dissect_nmea0183_sentence_gll(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree)
1701 | {
1702 | int offset = 0;
1703 |
1704 | proto_tree *subtree = proto_tree_add_subtree(tree, tvb, offset,
1705 | tvb_captured_length(tvb), ett_nmea0183_sentence,
1706 | NULL((void*)0), "GLL sentence - Geographic Position");
1707 |
1708 | offset += dissect_nmea0183_field_latitude(tvb, pinfo, subtree, offset, hf_nmea0183_gll_latitude,
1709 | hf_nmea0183_gll_latitude_degree, hf_nmea0183_gll_latitude_minute,
1710 | hf_nmea0183_gll_latitude_direction, ett_nmea0183_gll_latitude);
1711 |
1712 | offset += dissect_nmea0183_field_longitude(tvb, pinfo, subtree, offset, hf_nmea0183_gll_longitude,
1713 | hf_nmea0183_gll_longitude_degree, hf_nmea0183_gll_longitude_minute,
1714 | hf_nmea0183_gll_longitude_direction, ett_nmea0183_gll_longitude);
1715 |
1716 | offset += dissect_nmea0183_field_time(tvb, pinfo, subtree, offset, hf_nmea0183_gll_time,
1717 | hf_nmea0183_gll_time_hour, hf_nmea0183_gll_time_minute,
1718 | hf_nmea0183_gll_time_second, ett_nmea0183_gll_time);
1719 |
1720 | offset += dissect_nmea0183_field_status(tvb, pinfo, subtree, offset, hf_nmea0183_gll_status);
1721 |
1722 | dissect_nmea0183_field_faa_mode(tvb, pinfo, subtree, offset, hf_nmea0183_gll_mode);
1723 |
1724 | return tvb_captured_length(tvb);
1725 | }
1726 |
1727 | /* Dissect a GST sentence. The time field is split into individual parts. */
1728 | static int
1729 | dissect_nmea0183_sentence_gst(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree)
1730 | {
1731 | int offset = 0;
1732 |
1733 | proto_tree *subtree = proto_tree_add_subtree(tree, tvb, offset,
1734 | tvb_captured_length(tvb), ett_nmea0183_sentence,
1735 | NULL((void*)0), "GST sentence - GPS Pseudorange Noise Statistics");
1736 |
1737 | offset += dissect_nmea0183_field_time(tvb, pinfo, subtree, offset, hf_nmea0183_gst_time,
1738 | hf_nmea0183_gst_time_hour, hf_nmea0183_gst_time_minute,
1739 | hf_nmea0183_gst_time_second, ett_nmea0183_gst_time);
1740 |
1741 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gst_rms_total_sd, NULL((void*)0), NULL((void*)0));
1742 |
1743 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gst_ellipse_major_sd, "meter", NULL((void*)0));
1744 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gst_ellipse_minor_sd, "meter", NULL((void*)0));
1745 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gst_ellipse_orientation, "degree (true north)", NULL((void*)0));
1746 |
1747 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gst_latitude_sd, "meter", NULL((void*)0));
1748 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gst_longitude_sd, "meter", NULL((void*)0));
1749 | dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_gst_altitude_sd, "meter", NULL((void*)0));
1750 |
1751 | return tvb_captured_length(tvb);
1752 | }
1753 |
1754 | /* Dissect a HDT sentence. */
1755 | static int
1756 | dissect_nmea0183_sentence_hdt(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree)
1757 | {
1758 | int offset = 0;
1759 |
1760 | proto_tree *subtree = proto_tree_add_subtree(tree, tvb, offset,
1761 | tvb_captured_length(tvb), ett_nmea0183_sentence,
1762 | NULL((void*)0), "HDT sentence - True Heading");
1763 |
1764 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_hdt_heading, "degree", NULL((void*)0));
1765 |
1766 | dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_hdt_unit,
1767 | "T", &ei_nmea0183_hdt_unit_incorrect);
1768 |
1769 | return tvb_captured_length(tvb);
1770 | }
1771 |
1772 | /* Dissect a ROT sentence. */
1773 | static int
1774 | dissect_nmea0183_sentence_rot(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree)
1775 | {
1776 | int offset = 0;
1777 |
1778 | proto_tree *subtree = proto_tree_add_subtree(tree, tvb, offset,
1779 | tvb_captured_length(tvb), ett_nmea0183_sentence,
1780 | NULL((void*)0), "ROT sentence - Rate Of Turn");
1781 |
1782 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_rot_rate_of_turn, "degree per minute", NULL((void*)0));
1783 |
1784 | dissect_nmea0183_field_status(tvb, pinfo, subtree, offset, hf_nmea0183_rot_valid);
1785 |
1786 | return tvb_captured_length(tvb);
1787 | }
1788 |
1789 | /* Dissect a TXT sentence */
1790 | static int
1791 | dissect_nmea0183_sentence_txt(tvbuff_t* tvb, packet_info* pinfo, proto_tree* tree)
1792 | {
1793 | int offset = 0;
1794 |
1795 | proto_tree* subtree = proto_tree_add_subtree(tree, tvb, offset,
1796 | tvb_captured_length(tvb), ett_nmea0183_sentence,
1797 | NULL((void*)0), "TXT sentence - Text Transmission");
1798 |
1799 | /* Total number of sentences, 01 to 99 */
1800 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_txt_num, NULL((void*)0), NULL((void*)0));
1801 | /* Sentence number */
1802 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_txt_sent_num, NULL((void*)0), NULL((void*)0));
1803 | /* Text identifier */
1804 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_txt_id, NULL((void*)0), NULL((void*)0));
1805 | /* Text message */
1806 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_txt_msg, NULL((void*)0), NULL((void*)0));
1807 |
1808 | return tvb_captured_length(tvb);
1809 | }
1810 |
1811 |
1812 | /* Dissect a VHW sentence. */
1813 | static int
1814 | dissect_nmea0183_sentence_vhw(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree)
1815 | {
1816 | int offset = 0;
1817 |
1818 | proto_tree *subtree = proto_tree_add_subtree(tree, tvb, offset,
1819 | tvb_captured_length(tvb), ett_nmea0183_sentence,
1820 | NULL((void*)0), "VHW sentence - Water speed and heading");
1821 |
1822 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vhw_true_heading, "degree", NULL((void*)0));
1823 |
1824 | offset += dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_vhw_true_heading_unit,
1825 | "T", &ei_nmea0183_vhw_true_heading_unit_incorrect);
1826 |
1827 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vhw_magnetic_heading, "degree", NULL((void*)0));
1828 |
1829 | offset += dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_vhw_magnetic_heading_unit,
1830 | "M", &ei_nmea0183_vhw_magnetic_heading_unit_incorrect);
1831 |
1832 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vhw_water_speed_knot, "knot", NULL((void*)0));
1833 |
1834 | offset += dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_vhw_water_speed_knot_unit,
1835 | "N", &ei_nmea0183_vhw_water_speed_knot_unit_incorrect);
1836 |
1837 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vhw_water_speed_kilometer, "kilometer per hour", NULL((void*)0));
1838 |
1839 | dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_vhw_water_speed_kilometer_unit,
1840 | "K", &ei_nmea0183_vhw_water_speed_kilometer_unit_incorrect);
1841 |
1842 | return tvb_captured_length(tvb);
1843 | }
1844 |
1845 | /* Dissect a VBW sentence. */
1846 | static int
1847 | dissect_nmea0183_sentence_vbw(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree)
1848 | {
1849 | int offset = 0;
1850 |
1851 | proto_tree *subtree = proto_tree_add_subtree(tree, tvb, offset,
1852 | tvb_captured_length(tvb), ett_nmea0183_sentence,
1853 | NULL((void*)0), "VBW sentence - Dual Ground/Water Speed");
1854 |
1855 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vbw_water_speed_longitudinal, "knot", NULL((void*)0));
1856 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vbw_water_speed_transverse, "knot", NULL((void*)0));
1857 | offset += dissect_nmea0183_field_status(tvb, pinfo, subtree, offset, hf_nmea0183_vbw_water_speed_valid);
1858 |
1859 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vbw_ground_speed_longitudinal, "knot", NULL((void*)0));
1860 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vbw_ground_speed_transverse, "knot", NULL((void*)0));
1861 | offset += dissect_nmea0183_field_status(tvb, pinfo, subtree, offset, hf_nmea0183_vbw_ground_speed_valid);
1862 |
1863 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vbw_stern_water_speed, "knot", NULL((void*)0));
1864 | offset += dissect_nmea0183_field_status(tvb, pinfo, subtree, offset, hf_nmea0183_vbw_stern_water_speed_valid);
1865 |
1866 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vbw_stern_ground_speed, "knot", NULL((void*)0));
1867 | dissect_nmea0183_field_status(tvb, pinfo, subtree, offset, hf_nmea0183_vbw_stern_ground_speed_valid);
1868 |
1869 | return tvb_captured_length(tvb);
1870 | }
1871 |
1872 | /* Dissect a VLW sentence. */
1873 | static int
1874 | dissect_nmea0183_sentence_vlw(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree)
1875 | {
1876 | int offset = 0;
1877 |
1878 | proto_tree *subtree = proto_tree_add_subtree(tree, tvb, offset,
1879 | tvb_captured_length(tvb), ett_nmea0183_sentence,
1880 | NULL((void*)0), "VLW sentence - Distance Traveled through Water");
1881 |
1882 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vlw_cumulative_water, "nautical miles", NULL((void*)0));
1883 |
1884 | offset += dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_vlw_cumulative_water_unit,
1885 | "N", &ei_nmea0183_vlw_cumulative_water_unit_incorrect);
1886 |
1887 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vlw_trip_water, "nautical miles", NULL((void*)0));
1888 |
1889 | offset += dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_vlw_trip_water_unit,
1890 | "N", &ei_nmea0183_vlw_trip_water_unit_incorrect);
1891 |
1892 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vlw_cumulative_ground, "nautical miles", NULL((void*)0));
1893 |
1894 | offset += dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_vlw_cumulative_ground_unit,
1895 | "N", &ei_nmea0183_vlw_cumulative_ground_unit_incorrect);
1896 |
1897 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vlw_trip_ground, "nautical miles", NULL((void*)0));
1898 |
1899 | dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_vlw_trip_ground_unit,
1900 | "N", &ei_nmea0183_vlw_trip_ground_unit_incorrect);
1901 |
1902 | return tvb_captured_length(tvb);
1903 | }
1904 |
1905 | /* Dissect a VTG sentence. */
1906 | static int
1907 | dissect_nmea0183_sentence_vtg(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree)
1908 | {
1909 | int offset = 0;
1910 |
1911 | proto_tree *subtree = proto_tree_add_subtree(tree, tvb, offset,
1912 | tvb_captured_length(tvb), ett_nmea0183_sentence,
1913 | NULL((void*)0), "VTG sentence - Track made good and Ground speed");
1914 |
1915 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vtg_true_course, "degree", NULL((void*)0));
1916 |
1917 | offset += dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_vtg_true_course_unit,
1918 | "T", &ei_nmea0183_vtg_true_course_unit_incorrect);
1919 |
1920 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vtg_magnetic_course, "degree", NULL((void*)0));
1921 |
1922 | offset += dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_vtg_magnetic_course_unit,
1923 | "M", &ei_nmea0183_vtg_magnetic_course_unit_incorrect);
1924 |
1925 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vtg_ground_speed_knot, "knot", NULL((void*)0));
1926 |
1927 | offset += dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_vtg_ground_speed_knot_unit,
1928 | "N", &ei_nmea0183_vtg_ground_speed_knot_unit_incorrect);
1929 |
1930 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_vtg_ground_speed_kilometer, "kilometer per hour", NULL((void*)0));
1931 |
1932 | offset += dissect_nmea0183_field_fixed_text(tvb, pinfo, subtree, offset, hf_nmea0183_vtg_ground_speed_kilometer_unit,
1933 | "K", &ei_nmea0183_vtg_ground_speed_kilometer_unit_incorrect);
1934 |
1935 | dissect_nmea0183_field_faa_mode(tvb, pinfo, subtree, offset, hf_nmea0183_vtg_mode);
1936 |
1937 | return tvb_captured_length(tvb);
1938 | }
1939 |
1940 | /* Dissect a ZDA (Time & Date) sentence. The time field is split into individual parts. */
1941 | static int
1942 | dissect_nmea0183_sentence_zda(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree)
1943 | {
1944 | int offset = 0;
1945 | proto_tree *subtree = proto_tree_add_subtree(tree, tvb, offset,
1946 | tvb_captured_length(tvb), ett_nmea0183_sentence,
1947 | NULL((void*)0), "ZDA sentence - Time & Date");
1948 |
1949 | offset += dissect_nmea0183_field_time(tvb, pinfo, subtree, offset, hf_nmea0183_zda_time,
1950 | hf_nmea0183_zda_time_hour, hf_nmea0183_zda_time_minute,
1951 | hf_nmea0183_zda_time_second, ett_nmea0183_zda_time);
1952 |
1953 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_zda_date_day, NULL((void*)0), NULL((void*)0));
1954 |
1955 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_zda_date_month, NULL((void*)0), NULL((void*)0));
1956 |
1957 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_zda_date_year, NULL((void*)0), NULL((void*)0));
1958 |
1959 | offset += dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_zda_local_zone_hour, NULL((void*)0), NULL((void*)0));
1960 |
1961 | dissect_nmea0183_field(tvb, pinfo, subtree, offset, hf_nmea0183_zda_local_zone_minute, NULL((void*)0), NULL((void*)0));
1962 |
1963 | return tvb_captured_length(tvb);
1964 | }
1965 |
1966 | /* Dissect a sentence where the sentence id is unknown. Each field is shown as an generic field. */
1967 | static int
1968 | dissect_nmea0183_sentence_unknown(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree)
1969 | {
1970 | int offset = 0;
1971 |
1972 | proto_tree *subtree = proto_tree_add_subtree(tree, tvb, offset,
1973 | tvb_captured_length(tvb), ett_nmea0183_sentence,
1974 | NULL((void*)0), "Unknown sentence");
1975 |
1976 | /* In an unknown sentence, the name of each field is unknown. Find all field by splitting at a comma. */
1977 | while (tvb_captured_length_remaining(tvb, offset) > 0)
1978 | {
1979 | int end_of_field_offset = tvb_find_end_of_nmea0183_field(tvb, offset);
1980 | proto_item *ti = proto_tree_add_item(subtree, hf_nmea0183_unknown_field,
1981 | tvb, offset, end_of_field_offset - offset, ENC_ASCII0x00000000);
1982 | if (end_of_field_offset - offset == 0)
1983 | {
1984 | proto_item_append_text(ti, "[empty]");
1985 | }
1986 | offset = end_of_field_offset + 1;
1987 | }
1988 | return tvb_captured_length(tvb);
1989 | }
1990 |
1991 |
1992 | /* <tag block 1>,<tagblock2>, … <tagblock n>*<tagblocks CS> */
1993 | //static void
1994 | //dissect_nmea0183_tag_block(tvbuff_t* tvb, packet_info* pinfo, proto_tree* tree)
1995 | //{
1996 | // int offset = 0, chk_sum_off, comma_off;
1997 | //
1998 | // chk_sum_off = tvb_find_uint8(tvb, offset, -1, '*');
1999 | // if (chk_sum_off == -1) {
2000 | // /* No checksum ??*/
2001 | // return;
2002 | // }
2003 | // while (offset < chk_sum_off) {
2004 | // comma_off = tvb_find_uint8(tvb, offset, -1, ',');
2005 | // if (comma_off == -1) {
2006 | //
2007 | // }
2008 | //
2009 | // }
2010 | //
2011 | //}
2012 | static int
2013 | dissect_nmea0183_tag_blocks(tvbuff_t* tvb, packet_info* pinfo _U___attribute__((unused)), proto_tree* tree, int offset) {
2014 |
2015 | int start_offset;
2016 | int end_offset;
2017 |
2018 | while (tvb_get_uint8(tvb, offset) == '\\') {
2019 | start_offset = offset;
2020 | offset++;
2021 | end_offset = tvb_find_uint8(tvb, offset, -1, '\\');
2022 | if (end_offset == -1) {
2023 | // Add expert info
2024 | return tvb_captured_length(tvb);
2025 | }
2026 | proto_tree_add_item(tree, hf_nmea0183_tag_block, tvb, start_offset, (end_offset - start_offset) + 1, ENC_ASCII0x00000000);
2027 | //proto_tree* tree = proto_item_add_subtree(ti, ett_nmea0183_tag_block);
2028 | offset = end_offset + 1;
2029 | }
2030 | return offset;
2031 | }
2032 |
2033 | static int
2034 | dissect_nmea0183_msg(tvbuff_t* tvb, packet_info* pinfo, proto_tree* tree)
2035 | {
2036 | proto_item* ti;
2037 | int offset = 0,start_offset;
2038 | int start_checksum_offset = 0;
2039 | const char* talker_id = NULL((void*)0);
2040 | const char* sentence_id = NULL((void*)0);
2041 | const char* checksum = NULL((void*)0);
2042 | uint8_t start_delimiter;
2043 |
2044 | /* Start delimiter */
2045 | start_delimiter = tvb_get_uint8(tvb, offset);
2046 | if ((start_delimiter != '$') && (start_delimiter != '!'))
2047 | {
2048 | expert_add_info(pinfo, tree, &ei_nmea0183_invalid_first_character);
2049 | }
2050 |
2051 | offset += 1;
2052 | start_offset = offset;
2053 | /* Talker id */
2054 | ti = proto_tree_add_item_ret_string(tree, hf_nmea0183_talker_id,
2055 | tvb, offset, 2, ENC_ASCII0x00000000,
2056 | pinfo->pool, (const uint8_t**)&talker_id);
2057 |
2058 | proto_item_append_text(ti, " (%s)", str_to_str_wmem(pinfo->pool, talker_id, known_talker_ids, "Unknown talker ID"));
2059 |
2060 | col_append_fstr(pinfo->cinfo, COL_INFO, "Talker %s", str_to_str_wmem(pinfo->pool, talker_id, known_talker_ids, "Unknown talker ID"));
2061 |
2062 | offset += 2;
2063 |
2064 | /* Sentence id */
2065 | ti = proto_tree_add_item_ret_string(tree, hf_nmea0183_sentence_id,
2066 | tvb, offset, 3, ENC_ASCII0x00000000,
2067 | pinfo->pool, (const uint8_t**)&sentence_id);
2068 |
2069 | proto_item_append_text(ti, " (%s)", str_to_str_wmem(pinfo->pool, sentence_id, known_sentence_ids, "Unknown sentence ID"));
2070 |
2071 | col_append_fstr(pinfo->cinfo, COL_INFO, ", Sentence %s", str_to_str_wmem(pinfo->pool, sentence_id, known_sentence_ids, "Unknown sentence ID"));
2072 |
2073 | offset += 3;
2074 |
2075 | /* Start of checksum */
2076 | start_checksum_offset = tvb_find_uint8(tvb, offset, -1, '*');
2077 | if (start_checksum_offset == -1)
2078 | {
2079 | expert_add_info(pinfo, tree, &ei_nmea0183_missing_checksum_character);
2080 | return tvb_captured_length(tvb);
2081 | }
2082 |
2083 | /* Data */
2084 | offset += 1;
2085 | tvbuff_t *data_tvb = tvb_new_subset_length(tvb, offset, start_checksum_offset - offset);
2086 | if (g_ascii_strcasecmp(sentence_id, "ALR") == 0)
2087 | {
2088 | offset += dissect_nmea0183_sentence_alr(data_tvb, pinfo, tree);
2089 | }
2090 | else if (g_ascii_strcasecmp(sentence_id, "DPT") == 0)
2091 | {
2092 | offset += dissect_nmea0183_sentence_dpt(data_tvb, pinfo, tree);
2093 | }
2094 | else if (g_ascii_strcasecmp(sentence_id, "GGA") == 0)
2095 | {
2096 | offset += dissect_nmea0183_sentence_gga(data_tvb, pinfo, tree);
2097 | }
2098 | else if (g_ascii_strcasecmp(sentence_id, "GLL") == 0)
2099 | {
2100 | offset += dissect_nmea0183_sentence_gll(data_tvb, pinfo, tree);
2101 | }
2102 | else if (g_ascii_strcasecmp(sentence_id, "GST") == 0)
2103 | {
2104 | offset += dissect_nmea0183_sentence_gst(data_tvb, pinfo, tree);
2105 | }
2106 | else if (g_ascii_strcasecmp(sentence_id, "HDT") == 0)
2107 | {
2108 | offset += dissect_nmea0183_sentence_hdt(data_tvb, pinfo, tree);
2109 | }
2110 | else if (g_ascii_strcasecmp(sentence_id, "ROT") == 0)
2111 | {
2112 | offset += dissect_nmea0183_sentence_rot(data_tvb, pinfo, tree);
2113 | }
2114 | else if (g_ascii_strcasecmp(sentence_id, "TXT") == 0)
2115 | {
2116 | offset += dissect_nmea0183_sentence_txt(data_tvb, pinfo, tree);
2117 | }
2118 | else if (g_ascii_strcasecmp(sentence_id, "VBW") == 0)
2119 | {
2120 | offset += dissect_nmea0183_sentence_vbw(data_tvb, pinfo, tree);
2121 | }
2122 | else if (g_ascii_strcasecmp(sentence_id, "VHW") == 0)
2123 | {
2124 | offset += dissect_nmea0183_sentence_vhw(data_tvb, pinfo, tree);
2125 | }
2126 | else if (g_ascii_strcasecmp(sentence_id, "VLW") == 0)
2127 | {
2128 | offset += dissect_nmea0183_sentence_vlw(data_tvb, pinfo, tree);
2129 | }
2130 | else if (g_ascii_strcasecmp(sentence_id, "VTG") == 0)
2131 | {
2132 | offset += dissect_nmea0183_sentence_vtg(data_tvb, pinfo, tree);
2133 | }
2134 | else if (g_ascii_strcasecmp(sentence_id, "ZDA") == 0)
2135 | {
2136 | offset += dissect_nmea0183_sentence_zda(data_tvb, pinfo, tree);
2137 | }
2138 | else
2139 | {
2140 | offset += dissect_nmea0183_sentence_unknown(data_tvb, pinfo, tree);
2141 | }
2142 |
2143 | /* Checksum */
2144 | offset += 1;
2145 | ti = proto_tree_add_item_ret_string(tree, hf_nmea0183_checksum,
2146 | tvb, offset, 2, ENC_ASCII0x00000000,
2147 | pinfo->pool, (const uint8_t**)&checksum);
2148 |
2149 | uint8_t received_checksum = (uint8_t)strtol(checksum, NULL((void*)0), 16);
2150 | uint8_t calculated_checksum;
2151 |
2152 | //calculated_checksum = calculate_checksum(tvb, 1, offset - 2);
2153 | calculated_checksum = calculate_checksum(tvb, start_offset, (offset - start_offset-1));
2154 |
2155 | if (received_checksum == calculated_checksum)
2156 | {
2157 | proto_item_append_text(ti, " [correct]");
2158 | }
2159 | else
2160 | {
2161 | proto_item_append_text(ti, " [INCORRECT]");
2162 | expert_add_info(pinfo, ti, &ei_nmea0183_checksum_incorrect);
2163 | }
2164 |
2165 | // Calculated checksum highlights 2 bytes, which is the ascii hex value of a 1 byte checksum
2166 | proto_item *checksum_tree = proto_item_add_subtree(ti, ett_nmea0183_checksum);
2167 | ti = proto_tree_add_uint(checksum_tree, hf_nmea0183_checksum_calculated,
2168 | tvb, offset, 2, calculated_checksum);
2169 |
2170 | proto_item_set_generated(ti);
2171 |
2172 | offset += 2;
2173 |
2174 | /* End of line */
2175 | if (tvb_captured_length_remaining(tvb, offset) < 2 ||
2176 | tvb_get_uint8(tvb, offset) != '\r' ||
2177 | tvb_get_uint8(tvb, offset + 1) != '\n')
2178 | {
2179 | expert_add_info(pinfo, tree, &ei_nmea0183_invalid_end_of_line);
2180 | }
2181 | offset += 2;
2182 |
2183 | /* Check sentence length */
2184 | if (offset > 82)
2185 | {
2186 | expert_add_info(pinfo, tree, &ei_nmea0183_sentence_too_long);
2187 | }
2188 |
2189 | return tvb_captured_length(tvb);
2190 | }
2191 |
2192 | static const value_string nmea0183_bin_mtype_vals[] = {
2193 | { 1, "Data"},
2194 | { 2, "Query"},
2195 | { 3, "Ack"},
2196 | { 0, NULL((void*)0) },
2197 | };
2198 |
2199 | static int
2200 | dissect_nmea0183_bin(tvbuff_t* tvb, packet_info* pinfo, proto_tree* tree, void* data _U___attribute__((unused)))
2201 | {
2202 | proto_item* ti;
2203 | proto_tree* nmea0183_tree, *fd_tree;
2204 | uint32_t mtype, seqnum, file_descriptor_len, type_len;
2205 |
2206 | int offset = 0;
2207 |
2208 | col_set_str(pinfo->cinfo, COL_PROTOCOL, "NMEA 0183 Binary");
2209 | /* Clear the info column */
2210 | col_clear(pinfo->cinfo, COL_INFO);
2211 |
2212 | ti = proto_tree_add_item(tree, proto_nmea0183_bin, tvb, 0, -1, ENC_NA0x00000000);
2213 | nmea0183_tree = proto_item_add_subtree(ti, ett_nmea0183);
2214 |
2215 | proto_tree_add_item(nmea0183_tree, hf_nmea0183_sentence_prefix, tvb, offset, 6, ENC_ASCII0x00000000);
2216 | offset += 6;
2217 | proto_tree_add_item(nmea0183_tree, hf_nmea0183_bin_version, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
2218 | offset+=2;
2219 | proto_tree_add_item(nmea0183_tree, hf_nmea0183_bin_srcid, tvb, offset, 6, ENC_ASCII0x00000000);
2220 | offset += 6;
2221 | proto_tree_add_item(nmea0183_tree, hf_nmea0183_bin_dstid, tvb, offset, 6, ENC_ASCII0x00000000);
2222 | offset += 6;
2223 | proto_tree_add_item_ret_uint(nmea0183_tree, hf_nmea0183_bin_mtype, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &mtype);
2224 | offset += 2;
2225 | proto_tree_add_item(nmea0183_tree, hf_nmea0183_bin_blockid, tvb, offset, 4, ENC_BIG_ENDIAN0x00000000);
2226 | offset += 4;
2227 | proto_tree_add_item_ret_uint(nmea0183_tree, hf_nmea0183_bin_seqnum, tvb, offset, 4, ENC_BIG_ENDIAN0x00000000, &seqnum);
2228 | offset += 4;
2229 | proto_tree_add_item(nmea0183_tree, hf_nmea0183_bin_max_seqnum, tvb, offset, 4, ENC_BIG_ENDIAN0x00000000);
2230 | offset += 4;
2231 | if (offset < (int)tvb_reported_length(tvb)) {
2232 | if ((mtype == 1) && (seqnum == 1)) {
2233 | /* binary file descriptor*/
2234 | ti = proto_tree_add_item(nmea0183_tree, hf_nmea0183_bin_file_descriptor, tvb, offset, -1, ENC_ASCII0x00000000);
2235 | fd_tree = proto_item_add_subtree(ti, ett_nmea0183_fd);
2236 | proto_tree_add_item_ret_uint(fd_tree, hf_nmea0183_bin_file_descriptor_len, tvb, offset, 4, ENC_BIG_ENDIAN0x00000000, &file_descriptor_len);
2237 | proto_item_set_len(ti, file_descriptor_len);
2238 | offset += 4;
2239 | proto_tree_add_item(fd_tree, hf_nmea0183_bin_file_length, tvb, offset, 4, ENC_BIG_ENDIAN0x00000000);
2240 | offset += 4;
2241 | proto_tree_add_item(fd_tree, hf_nmea0183_bin_stat_of_acquisition, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
2242 | offset += 2;
2243 | proto_tree_add_item(fd_tree, hf_nmea0183_bin_device, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2244 | offset++;
2245 | proto_tree_add_item(fd_tree, hf_nmea0183_bin_channel, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2246 | offset++;
2247 | proto_tree_add_item_ret_uint(fd_tree, hf_nmea0183_bin_type_len, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &type_len);
2248 | offset++;
2249 | proto_tree_add_item(fd_tree, hf_nmea0183_bin_data_type, tvb, offset, type_len, ENC_ASCII0x00000000);
2250 | offset += type_len;
2251 | proto_tree_add_item(fd_tree, hf_nmea0183_bin_status_and_info, tvb, offset, file_descriptor_len - type_len - 13, ENC_ASCII0x00000000);
2252 | offset += file_descriptor_len - type_len - 13;
2253 | }
2254 | proto_tree_add_item(nmea0183_tree, hf_nmea0183_bin_data, tvb, offset, -1, ENC_NA0x00000000);
2255 | }
2256 |
2257 |
2258 | return tvb_reported_length(tvb);
2259 | }
2260 |
2261 | static int
2262 | dissect_nmea0183(tvbuff_t* tvb, packet_info* pinfo, proto_tree* tree, void* data)
2263 | {
2264 | proto_item* ti;
2265 | proto_tree* nmea0183_tree = NULL((void*)0);
2266 | int offset = 0;
2267 | int end_offset;
2268 | bool_Bool first_msg = true1;
2269 |
2270 | col_set_str(pinfo->cinfo, COL_PROTOCOL, "NMEA 0183");
2271 | /* Clear the info column */
2272 | col_clear(pinfo->cinfo, COL_INFO);
2273 |
2274 | /* Find end of nmea message */
2275 | end_offset = tvb_find_uint16(tvb, 0, -1, NMEA0183_CRLF0x0d0a);
2276 | if (end_offset == -1) {
2277 | end_offset = tvb_reported_length(tvb);
2278 | }
2279 | /* Add CRLF */
2280 | end_offset += 2;
2281 |
2282 |
2283 | /* UdPbC\<tag block 1>,<tagblock2>, … <tagblock n>*<tagblocks CS>\<NMEA message>*/
2284 | if (tvb_strneql(tvb, 0, UDPBC"UdPbC", strlen(UDPBC"UdPbC")) == 0) {
2285 | if (first_msg == true1) {
2286 | ti = proto_tree_add_item(tree, proto_nmea0183, tvb, 0, end_offset, ENC_NA0x00000000);
2287 | nmea0183_tree = proto_item_add_subtree(ti, ett_nmea0183);
2288 | }
2289 | proto_tree_add_item(nmea0183_tree, hf_nmea0183_sentence_prefix, tvb, offset, 6, ENC_ASCII0x00000000);
2290 | offset += 6;
2291 | while (offset < (int)tvb_reported_length(tvb)) {
2292 | if (first_msg != true1) {
2293 | end_offset = tvb_find_uint16(tvb, offset, -1, NMEA0183_CRLF0x0d0a);
2294 | if (end_offset == -1) {
2295 | end_offset = tvb_reported_length(tvb);
2296 | }
2297 | /* Add CRLF */
2298 | end_offset += 2;
2299 |
2300 | ti = proto_tree_add_item(tree, proto_nmea0183, tvb, offset, end_offset, ENC_NA0x00000000);
2301 | nmea0183_tree = proto_item_add_subtree(ti, ett_nmea0183);
2302 | }
2303 | offset = dissect_nmea0183_tag_blocks(tvb, pinfo, nmea0183_tree, offset);
2304 | tvbuff_t* msg_tvb = tvb_new_subset_length(tvb, offset, end_offset - offset);
2305 | dissect_nmea0183_msg(msg_tvb, pinfo, nmea0183_tree);
2306 | offset += (end_offset - offset);
2307 | first_msg = false0;
2308 | }
2309 | return offset;
2310 | } else if (tvb_strneql(tvb, 0, RRUDP"RrUdP", strlen(RRUDP"RrUdP")) == 0) {
2311 | /* Binary nmea0183 */
2312 | offset = dissect_nmea0183_bin(tvb, pinfo, tree, data);
2313 | return offset;
2314 | } else if (tvb_strneql(tvb, 0, RAUDP"RaUdp", strlen(RAUDP"RaUdp")) == 0) {
2315 | /* Binary nmea0183 */
2316 | offset = dissect_nmea0183_bin(tvb, pinfo, tree, data);
2317 | return offset;
2318 | } else if (tvb_strneql(tvb, 0, RPUDP"RpUdP", strlen(RPUDP"RpUdP")) == 0) {
2319 | /* Binary nmea0183 */
2320 | offset = dissect_nmea0183_bin(tvb, pinfo, tree, data);
2321 | return offset;
2322 | }
2323 |
2324 | ti = proto_tree_add_item(tree, proto_nmea0183, tvb, 0, end_offset, ENC_NA0x00000000);
2325 | nmea0183_tree = proto_item_add_subtree(ti, ett_nmea0183);
2326 |
2327 | tvbuff_t *msg_tvb = tvb_new_subset_length(tvb, offset, end_offset - offset);
2328 | offset = dissect_nmea0183_msg(msg_tvb, pinfo, nmea0183_tree);
2329 |
2330 | return offset;
2331 | }
2332 |
2333 | /* Try to detect NMEA 0183 heuristically */
2334 | static bool_Bool dissect_nmea0183_heur(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, void *data)
2335 | {
2336 | char *sent_type;
2337 | const char *talker, *t_val, *p_val, *m_val, *manuf;
2338 |
2339 | /* Have to have at least 11 bytes:
2340 | * 1-byte sentence type character ('!' or '$')
2341 | * 2-byte TALKER lookup value
2342 | * 2-byte TALKER (for Query sentences) or 3-byte FORMATTER
2343 | * variable number of bytes for delimiters and data fields (minimum would be a single ',' byte)
2344 | * '*' delimeter byte, 2-bytes for checksum, and 2-bytes for EOM "\r\n" */
2345 | if(tvb_reported_length(tvb) < 11 || tvb_captured_length(tvb) < 5){
2346 | return false0;
2347 | }
2348 | /* See if we have a UDP brodcast message */
2349 | if (tvb_strneql(tvb, 0, UDPBC"UdPbC", strlen(UDPBC"UdPbC")) == 0) {
2350 | return (dissect_nmea0183(tvb, pinfo, tree, data) != 0);
2351 | }
2352 | if (tvb_strneql(tvb, 0, RRUDP"RrUdP", strlen(RRUDP"RrUdP")) == 0) {
2353 | return (dissect_nmea0183_bin(tvb, pinfo, tree, data) != 0);
2354 | }
2355 | if (tvb_strneql(tvb, 0, RAUDP"RaUdp", strlen(RAUDP"RaUdp")) == 0) {
2356 | return (dissect_nmea0183_bin(tvb, pinfo, tree, data) != 0);
2357 | }
2358 | if (tvb_strneql(tvb, 0, RPUDP"RpUdP", strlen(RPUDP"RpUdP")) == 0) {
2359 | return (dissect_nmea0183_bin(tvb, pinfo, tree, data) != 0);
2360 | }
2361 | /* Grab the first byte and check the first character */
2362 | sent_type = (char*)tvb_get_string_enc(pinfo->pool, tvb, 0, 1, ENC_ASCII0x00000000);
2363 |
2364 | /* Sentence type character ('!' or '$') */
2365 | if( (sent_type[0] != '!') && (sent_type[0] != '$') ){
2366 | return false0;
2367 | }
2368 |
2369 | /* We either have a 'P' and corresponding manufacturer 3-byte value OR
2370 | * we have a non-proprietary 2-byte TALKER field */
2371 | //TODO: Implement encapsulation and proprietary message parsing
2372 |
2373 | /* Do a lookup for the 2-byte TALKER field */
2374 | t_val = (char*)tvb_get_string_enc(pinfo->pool, tvb, 1, 2, ENC_ASCII0x00000000);
2375 | talker = try_str_to_str(t_val, known_talker_ids);
2376 |
2377 | /* Do a lookup for the 3-byte manufacturer if the 2nd byte in the PDU is 'P' */
2378 | p_val = (char*)tvb_get_string_enc(pinfo->pool, tvb, 1, 1, ENC_ASCII0x00000000);
2379 | m_val = (char*)tvb_get_string_enc(pinfo->pool, tvb, 2, 3, ENC_ASCII0x00000000);
2380 | manuf = try_str_to_str(m_val, manufacturer_vals);
2381 |
2382 | /* If one of the two conditions are true then try to dissect NMEA 0183 */
2383 | if( ((p_val[0] == 'P') && (manuf != NULL((void*)0))) ||
2384 | (talker != NULL((void*)0)) ){
2385 | /* Looks like NMEA 0183 so let's give it a try */
2386 | return (dissect_nmea0183(tvb, pinfo, tree, data) != 0);
2387 | }
2388 | /* If neither conditions are met then we return false */
2389 | else{
2390 | return false0;
2391 | }
2392 | }
2393 |
2394 | void proto_register_nmea0183(void)
2395 | {
2396 | expert_module_t *expert_nmea0183;
2397 |
2398 | static hf_register_info hf[] = {
2399 | {&hf_nmea0183_talker_id,
2400 | {"Talker ID", "nmea0183.talker",
2401 | FT_STRING, BASE_NONE,
2402 | NULL((void*)0), 0x0,
2403 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2404 | {&hf_nmea0183_sentence_id,
2405 | {"Sentence ID", "nmea0183.sentence",
2406 | FT_STRING, BASE_NONE,
2407 | NULL((void*)0), 0x0,
2408 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2409 | {&hf_nmea0183_unknown_field,
2410 | {"Field", "nmea0183.unknown_field",
2411 | FT_STRING, BASE_NONE,
2412 | NULL((void*)0), 0x0,
2413 | "NMEA 0183 Unknown field", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2414 | {&hf_nmea0183_checksum,
2415 | {"Checksum", "nmea0183.checksum",
2416 | FT_STRING, BASE_NONE,
2417 | NULL((void*)0), 0x0,
2418 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2419 | {&hf_nmea0183_checksum_calculated,
2420 | {"Calculated checksum", "nmea0183.checksum_calculated",
2421 | FT_UINT8, BASE_HEX,
2422 | NULL((void*)0), 0x0,
2423 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2424 | {&hf_nmea0183_dpt_depth,
2425 | {"Water depth", "nmea0183.dpt_depth",
2426 | FT_STRING, BASE_NONE,
2427 | NULL((void*)0), 0x0,
2428 | "NMEA 0183 DPT Water depth relative to transducer", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2429 | {&hf_nmea0183_dpt_offset,
2430 | {"Offset", "nmea0183.dpt_offset",
2431 | FT_STRING, BASE_NONE,
2432 | NULL((void*)0), 0x0,
2433 | "NMEA 0183 DPT Offset from transducer, positive means distance from transducer to water line, negative means distance from transducer to keel", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2434 | {&hf_nmea0183_dpt_max_range,
2435 | {"Maximum range", "nmea0183.dpt_max_range",
2436 | FT_STRING, BASE_NONE,
2437 | NULL((void*)0), 0x0,
2438 | "NMEA 0183 DPT Maximum range scale in use (NMEA 3.0 and above)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2439 | {&hf_nmea0183_alr_time,
2440 | {"UTC Time of alarm condition change", "nmea0183.alr_time",
2441 | FT_NONE, BASE_NONE,
2442 | NULL((void*)0), 0x0,
2443 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2444 | {&hf_nmea0183_alr_time_hour,
2445 | {"Hour", "nmea0183.alr_time_hour",
2446 | FT_STRING, BASE_NONE,
2447 | NULL((void*)0), 0x0,
2448 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2449 | {&hf_nmea0183_alr_time_minute,
2450 | {"Minute", "nmea0183.alr_time_minute",
2451 | FT_STRING, BASE_NONE,
2452 | NULL((void*)0), 0x0,
2453 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2454 | {&hf_nmea0183_alr_time_second,
2455 | {"Second", "nmea0183.alr_time_second",
2456 | FT_STRING, BASE_NONE,
2457 | NULL((void*)0), 0x0,
2458 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2459 | {&hf_nmea0183_alr_alarm_id,
2460 | {"Alarm id", "nmea0183.alr_id",
2461 | FT_STRING, BASE_NONE,
2462 | NULL((void*)0), 0x0,
2463 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2464 | {&hf_nmea0183_alr_alarm_cond,
2465 | {"Alarm condition", "nmea0183.alr_alarm_cond",
2466 | FT_STRING, BASE_NONE,
2467 | NULL((void*)0), 0x0,
2468 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2469 | {&hf_nmea0183_alr_alarm_ack_st,
2470 | {"Alarm’s acknowledge state", "nmea0183.alr_alarm_ack_st",
2471 | FT_STRING, BASE_NONE,
2472 | NULL((void*)0), 0x0,
2473 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2474 | {&hf_nmea0183_alr_alarm_desc_txt,
2475 | {"Alarm’s description text", "nmea0183.alr_alarm_desc_txt",
2476 | FT_STRING, BASE_NONE,
2477 | NULL((void*)0), 0x0,
2478 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2479 | {&hf_nmea0183_gga_time,
2480 | {"UTC Time of position", "nmea0183.gga_time",
2481 | FT_NONE, BASE_NONE,
2482 | NULL((void*)0), 0x0,
2483 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2484 | {&hf_nmea0183_gga_time_hour,
2485 | {"Hour", "nmea0183.gga_time_hour",
2486 | FT_STRING, BASE_NONE,
2487 | NULL((void*)0), 0x0,
2488 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2489 | {&hf_nmea0183_gga_time_minute,
2490 | {"Minute", "nmea0183.gga_time_minute",
2491 | FT_STRING, BASE_NONE,
2492 | NULL((void*)0), 0x0,
2493 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2494 | {&hf_nmea0183_gga_time_second,
2495 | {"Second", "nmea0183.gga_time_second",
2496 | FT_STRING, BASE_NONE,
2497 | NULL((void*)0), 0x0,
2498 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2499 | {&hf_nmea0183_gga_latitude,
2500 | {"Latitude", "nmea0183.gga_latitude",
2501 | FT_NONE, BASE_NONE,
2502 | NULL((void*)0), 0x0,
2503 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2504 | {&hf_nmea0183_gga_latitude_degree,
2505 | {"Degree", "nmea0183.gga_latitude_degree",
2506 | FT_STRING, BASE_NONE,
2507 | NULL((void*)0), 0x0,
2508 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2509 | {&hf_nmea0183_gga_latitude_minute,
2510 | {"Minute", "nmea0183.gga_latitude_minute",
2511 | FT_STRING, BASE_NONE,
2512 | NULL((void*)0), 0x0,
2513 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2514 | {&hf_nmea0183_gga_latitude_direction,
2515 | {"Direction", "nmea0183.gga_latitude_direction",
2516 | FT_STRING, BASE_NONE,
2517 | NULL((void*)0), 0x0,
2518 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2519 | {&hf_nmea0183_gga_longitude,
2520 | {"Longitude", "nmea0183.gga_longitude",
2521 | FT_NONE, BASE_NONE,
2522 | NULL((void*)0), 0x0,
2523 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2524 | {&hf_nmea0183_gga_longitude_degree,
2525 | {"Degree", "nmea0183.gga_longitude_degree",
2526 | FT_STRING, BASE_NONE,
2527 | NULL((void*)0), 0x0,
2528 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2529 | {&hf_nmea0183_gga_longitude_minute,
2530 | {"Minute", "nmea0183.gga_longitude_minute",
2531 | FT_STRING, BASE_NONE,
2532 | NULL((void*)0), 0x0,
2533 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2534 | {&hf_nmea0183_gga_longitude_direction,
2535 | {"Direction", "nmea0183.gga_longitude_direction",
2536 | FT_STRING, BASE_NONE,
2537 | NULL((void*)0), 0x0,
2538 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2539 | {&hf_nmea0183_gga_quality,
2540 | {"Quality indicator", "nmea0183.gga_quality",
2541 | FT_STRING, BASE_NONE,
2542 | NULL((void*)0), 0x0,
2543 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2544 | {&hf_nmea0183_gga_number_satellites,
2545 | {"Number of satellites", "nmea0183.gga_number_satellites",
2546 | FT_STRING, BASE_NONE,
2547 | NULL((void*)0), 0x0,
2548 | "NMEA 0183 GGA Number of satellites in use", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2549 | {&hf_nmea0183_gga_horizontal_dilution,
2550 | {"Horizontal Dilution", "nmea0183.gga_horizontal_dilution",
2551 | FT_STRING, BASE_NONE,
2552 | NULL((void*)0), 0x0,
2553 | "NMEA 0183 GGA Horizontal Dilution of precision", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2554 | {&hf_nmea0183_gga_altitude,
2555 | {"Altitude", "nmea0183.gga_altitude",
2556 | FT_STRING, BASE_NONE,
2557 | NULL((void*)0), 0x0,
2558 | "NMEA 0183 GGA Antenna Altitude above mean-sea-level", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2559 | {&hf_nmea0183_gga_altitude_unit,
2560 | {"Altitude unit", "nmea0183.gga_altitude_unit",
2561 | FT_STRING, BASE_NONE,
2562 | NULL((void*)0), 0x0,
2563 | "NMEA 0183 GGA Units of antenna altitude", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2564 | {&hf_nmea0183_gga_geoidal_separation,
2565 | {"Geoidal separation", "nmea0183.gga_geoidal_separation",
2566 | FT_STRING, BASE_NONE,
2567 | NULL((void*)0), 0x0,
2568 | "NMEA 0183 GGA Geoidal separation, the difference between the WGS-84 earth ellipsoid and mean-sea-level", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2569 | {&hf_nmea0183_gga_geoidal_separation_unit,
2570 | {"Geoidal separation unit", "nmea0183.gga_geoidal_separation_unit",
2571 | FT_STRING, BASE_NONE,
2572 | NULL((void*)0), 0x0,
2573 | "NMEA 0183 GGA Units of geoidal separation, meters", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2574 | {&hf_nmea0183_gga_age_dgps,
2575 | {"Age of differential GPS", "nmea0183.gga_age_dgps",
2576 | FT_STRING, BASE_NONE,
2577 | NULL((void*)0), 0x0,
2578 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2579 | {&hf_nmea0183_gga_dgps_station,
2580 | {"Differential GPS station id", "nmea0183.gga_dgps_station",
2581 | FT_STRING, BASE_NONE,
2582 | NULL((void*)0), 0x0,
2583 | "NMEA 0183 GGA Differential reference station ID", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2584 | {&hf_nmea0183_gll_latitude,
2585 | {"Latitude", "nmea0183.gll_latitude",
2586 | FT_NONE, BASE_NONE,
2587 | NULL((void*)0), 0x0,
2588 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2589 | {&hf_nmea0183_gll_latitude_degree,
2590 | {"Degree", "nmea0183.gll_latitude_degree",
2591 | FT_STRING, BASE_NONE,
2592 | NULL((void*)0), 0x0,
2593 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2594 | {&hf_nmea0183_gll_latitude_minute,
2595 | {"Minute", "nmea0183.gll_latitude_minute",
2596 | FT_STRING, BASE_NONE,
2597 | NULL((void*)0), 0x0,
2598 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2599 | {&hf_nmea0183_gll_latitude_direction,
2600 | {"Direction", "nmea0183.gll_latitude_direction",
2601 | FT_STRING, BASE_NONE,
2602 | NULL((void*)0), 0x0,
2603 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2604 | {&hf_nmea0183_gll_longitude,
2605 | {"Longitude", "nmea0183.gll_longitude",
2606 | FT_NONE, BASE_NONE,
2607 | NULL((void*)0), 0x0,
2608 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2609 | {&hf_nmea0183_gll_longitude_degree,
2610 | {"Degree", "nmea0183.gll_longitude_degree",
2611 | FT_STRING, BASE_NONE,
2612 | NULL((void*)0), 0x0,
2613 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2614 | {&hf_nmea0183_gll_longitude_minute,
2615 | {"Minute", "nmea0183.gll_longitude_minute",
2616 | FT_STRING, BASE_NONE,
2617 | NULL((void*)0), 0x0,
2618 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2619 | {&hf_nmea0183_gll_longitude_direction,
2620 | {"Direction", "nmea0183.gll_longitude_direction",
2621 | FT_STRING, BASE_NONE,
2622 | NULL((void*)0), 0x0,
2623 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2624 | {&hf_nmea0183_gll_time,
2625 | {"UTC Time of position", "nmea0183.gll_time",
2626 | FT_NONE, BASE_NONE,
2627 | NULL((void*)0), 0x0,
2628 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2629 | {&hf_nmea0183_gll_time_hour,
2630 | {"Hour", "nmea0183.gll_time_hour",
2631 | FT_STRING, BASE_NONE,
2632 | NULL((void*)0), 0x0,
2633 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2634 | {&hf_nmea0183_gll_time_minute,
2635 | {"Minute", "nmea0183.gll_time_minute",
2636 | FT_STRING, BASE_NONE,
2637 | NULL((void*)0), 0x0,
2638 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2639 | {&hf_nmea0183_gll_time_second,
2640 | {"Second", "nmea0183.gll_time_second",
2641 | FT_STRING, BASE_NONE,
2642 | NULL((void*)0), 0x0,
2643 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2644 | {&hf_nmea0183_gll_status,
2645 | {"Status", "nmea0183.gll_status",
2646 | FT_STRING, BASE_NONE,
2647 | NULL((void*)0), 0x0,
2648 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2649 | {&hf_nmea0183_gll_mode,
2650 | {"FAA mode", "nmea0183.gll_mode",
2651 | FT_STRING, BASE_NONE,
2652 | NULL((void*)0), 0x0,
2653 | "NMEA 0183 GLL FAA mode indicator (NMEA 2.3 and later)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2654 | {&hf_nmea0183_gst_time,
2655 | {"UTC Time of position", "nmea0183.gst_time",
2656 | FT_NONE, BASE_NONE,
2657 | NULL((void*)0), 0x0,
2658 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2659 | {&hf_nmea0183_gst_time_hour,
2660 | {"Hour", "nmea0183.gst_time_hour",
2661 | FT_STRING, BASE_NONE,
2662 | NULL((void*)0), 0x0,
2663 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2664 | {&hf_nmea0183_gst_time_minute,
2665 | {"Minute", "nmea0183.gst_time_minute",
2666 | FT_STRING, BASE_NONE,
2667 | NULL((void*)0), 0x0,
2668 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2669 | {&hf_nmea0183_gst_time_second,
2670 | {"Second", "nmea0183.gst_time_second",
2671 | FT_STRING, BASE_NONE,
2672 | NULL((void*)0), 0x0,
2673 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2674 | {&hf_nmea0183_gst_rms_total_sd,
2675 | {"Total RMS standard deviation", "nmea0183.gst_sd_rms_total",
2676 | FT_STRING, BASE_NONE,
2677 | NULL((void*)0), 0x0,
2678 | "NMEA 0183 GST Total RMS standard deviation of ranges inputs to the navigation solution", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2679 | {&hf_nmea0183_gst_ellipse_major_sd,
2680 | {"Standard deviation of semi-major axis of error", "nmea0183.gst_ellipse_major_sd",
2681 | FT_STRING, BASE_NONE,
2682 | NULL((void*)0), 0x0,
2683 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2684 | {&hf_nmea0183_gst_ellipse_minor_sd,
2685 | {"Standard deviation of semi-minor axis of error ellipse", "nmea0183.gst_ellipse_minor_sd",
2686 | FT_STRING, BASE_NONE,
2687 | NULL((void*)0), 0x0,
2688 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2689 | {&hf_nmea0183_gst_ellipse_orientation,
2690 | {"Orientation of semi-major axis of error ellipse", "nmea0183.gst_ellipse_orientation",
2691 | FT_STRING, BASE_NONE,
2692 | NULL((void*)0), 0x0,
2693 | "NMEA 0183 GST Orientation of semi-major axis of error ellipse (true north degrees)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2694 | {&hf_nmea0183_gst_latitude_sd,
2695 | {"Standard deviation of latitude error", "nmea0183.gst_sd_latitude",
2696 | FT_STRING, BASE_NONE,
2697 | NULL((void*)0), 0x0,
2698 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2699 | {&hf_nmea0183_gst_longitude_sd,
2700 | {"Standard deviation of longitude error", "nmea0183.gst_sd_longitude",
2701 | FT_STRING, BASE_NONE,
2702 | NULL((void*)0), 0x0,
2703 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2704 | {&hf_nmea0183_gst_altitude_sd,
2705 | {"Standard deviation of altitude error", "nmea0183.gst_sd_altitude",
2706 | FT_STRING, BASE_NONE,
2707 | NULL((void*)0), 0x0,
2708 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2709 | {&hf_nmea0183_hdt_heading,
2710 | {"True heading", "nmea0183.hdt_heading",
2711 | FT_STRING, BASE_NONE,
2712 | NULL((void*)0), 0x0,
2713 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2714 | {&hf_nmea0183_hdt_unit,
2715 | {"Heading unit", "nmea0183.hdt_unit",
2716 | FT_STRING, BASE_NONE,
2717 | NULL((void*)0), 0x0,
2718 | "NMEA 0183 HDT Heading unit, must be T", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2719 | {&hf_nmea0183_rot_rate_of_turn,
2720 | {"Rate of turn", "nmea0183.rot_rate_of_turn",
2721 | FT_STRING, BASE_NONE,
2722 | NULL((void*)0), 0x0,
2723 | "NMEA 0183 ROT Rate Of Turn, degrees per minute, negative value means bow turns to port", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2724 | { &hf_nmea0183_txt_num,
2725 | {"Total number of sentences", "nmea0183.txt.num",
2726 | FT_STRING, BASE_NONE,
2727 | NULL((void*)0), 0x0,
2728 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)} },
2729 | { &hf_nmea0183_txt_sent_num,
2730 | {"Sentence number", "nmea0183.txt.sent_num",
2731 | FT_STRING, BASE_NONE,
2732 | NULL((void*)0), 0x0,
2733 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)} },
2734 | { &hf_nmea0183_txt_id,
2735 | {"Text identifier", "nmea0183.txt.id",
2736 | FT_STRING, BASE_NONE,
2737 | NULL((void*)0), 0x0,
2738 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)} },
2739 | { &hf_nmea0183_txt_msg,
2740 | {"Text message", "nmea0183.txt.msg",
2741 | FT_STRING, BASE_NONE,
2742 | NULL((void*)0), 0x0,
2743 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)} },
2744 | {&hf_nmea0183_rot_valid,
2745 | {"Validity", "nmea0183.rot_valid",
2746 | FT_STRING, BASE_NONE,
2747 | NULL((void*)0), 0x0,
2748 | "NMEA 0183 ROT Status, A means data is valid", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2749 | {&hf_nmea0183_vbw_water_speed_longitudinal,
2750 | {"Longitudinal water speed", "nmea0183.vbw_water_speed_longitudinal",
2751 | FT_STRING, BASE_NONE,
2752 | NULL((void*)0), 0x0,
2753 | "NMEA 0183 VBW Longitudinal water speed, negative value means astern, knots", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2754 | {&hf_nmea0183_vbw_water_speed_transverse,
2755 | {"Transverse water speed", "nmea0183.vbw_water_speed_transverse",
2756 | FT_STRING, BASE_NONE,
2757 | NULL((void*)0), 0x0,
2758 | "NMEA 0183 VBW Transverse water speed, negative value means port, knots", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2759 | {&hf_nmea0183_vbw_water_speed_valid,
2760 | {"Water speed validity", "nmea0183.vbw_water_speed_valid",
2761 | FT_STRING, BASE_NONE,
2762 | NULL((void*)0), 0x0,
2763 | "NMEA 0183 VBW Water speed status, A means data is valid", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2764 | {&hf_nmea0183_vbw_ground_speed_longitudinal,
2765 | {"Longitudinal ground speed", "nmea0183.vbw_ground_speed_longitudinal",
2766 | FT_STRING, BASE_NONE,
2767 | NULL((void*)0), 0x0,
2768 | "NMEA 0183 VBW Longitudinal ground speed, negative value means astern, knots", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2769 | {&hf_nmea0183_vbw_ground_speed_transverse,
2770 | {"Transverse ground speed", "nmea0183.vbw_ground_speed_transverse",
2771 | FT_STRING, BASE_NONE,
2772 | NULL((void*)0), 0x0,
2773 | "NMEA 0183 VBW Transverse ground speed, negative value means port, knots", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2774 | {&hf_nmea0183_vbw_ground_speed_valid,
2775 | {"Ground speed validity", "nmea0183.vbw_ground_speed_valid",
2776 | FT_STRING, BASE_NONE,
2777 | NULL((void*)0), 0x0,
2778 | "NMEA 0183 VBW Ground speed status, A means data is valid", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2779 | {&hf_nmea0183_vbw_stern_water_speed,
2780 | {"Stern water speed", "nmea0183.vbw_stern_water_speed",
2781 | FT_STRING, BASE_NONE,
2782 | NULL((void*)0), 0x0,
2783 | "NMEA 0183 VBW Stern traverse water ground speed, negative value means port, knots", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2784 | {&hf_nmea0183_vbw_stern_water_speed_valid,
2785 | {"Stern water speed validity", "nmea0183.vbw_stern_water_speed_valid",
2786 | FT_STRING, BASE_NONE,
2787 | NULL((void*)0), 0x0,
2788 | "NMEA 0183 VBW Stern traverse water speed status, A means data is valid", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2789 | {&hf_nmea0183_vbw_stern_ground_speed,
2790 | {"Stern ground speed", "nmea0183.vbw_stern_ground_speed",
2791 | FT_STRING, BASE_NONE,
2792 | NULL((void*)0), 0x0,
2793 | "NMEA 0183 VBW Stern traverse ground ground speed, negative value means port, knots", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2794 | {&hf_nmea0183_vbw_stern_ground_speed_valid,
2795 | {"Stern ground speed validity", "nmea0183.vbw_stern_ground_speed_valid",
2796 | FT_STRING, BASE_NONE,
2797 | NULL((void*)0), 0x0,
2798 | "NMEA 0183 VBW Stern traverse ground speed status, A means data is valid", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2799 | {&hf_nmea0183_vhw_true_heading,
2800 | {"True heading", "nmea0183.vhw_true_heading",
2801 | FT_STRING, BASE_NONE,
2802 | NULL((void*)0), 0x0,
2803 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2804 | {&hf_nmea0183_vhw_true_heading_unit,
2805 | {"Heading unit", "nmea0183.vhw_true_heading_unit",
2806 | FT_STRING, BASE_NONE,
2807 | NULL((void*)0), 0x0,
2808 | "NMEA 0183 VHW Heading unit, must be T", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2809 | {&hf_nmea0183_vhw_magnetic_heading,
2810 | {"Magnetic heading", "nmea0183.vhw_magnetic_heading",
2811 | FT_STRING, BASE_NONE,
2812 | NULL((void*)0), 0x0,
2813 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2814 | {&hf_nmea0183_vhw_magnetic_heading_unit,
2815 | {"Heading unit", "nmea0183.vhw_magnetic_heading_unit",
2816 | FT_STRING, BASE_NONE,
2817 | NULL((void*)0), 0x0,
2818 | "NMEA 0183 VHW Heading unit, must be M", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2819 | {&hf_nmea0183_vhw_water_speed_knot,
2820 | {"Water speed", "nmea0183.vhw_water_speed_knot",
2821 | FT_STRING, BASE_NONE,
2822 | NULL((void*)0), 0x0,
2823 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2824 | {&hf_nmea0183_vhw_water_speed_knot_unit,
2825 | {"Speed unit", "nmea0183.vhw_water_speed_knot_unit",
2826 | FT_STRING, BASE_NONE,
2827 | NULL((void*)0), 0x0,
2828 | "NMEA 0183 VHW Water speed unit, must be N", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2829 | {&hf_nmea0183_vhw_water_speed_kilometer,
2830 | {"Water speed", "nmea0183.vhw_water_speed_kilometer",
2831 | FT_STRING, BASE_NONE,
2832 | NULL((void*)0), 0x0,
2833 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2834 | {&hf_nmea0183_vhw_water_speed_kilometer_unit,
2835 | {"Speed unit", "nmea0183.vhw_water_speed_kilometer_unit",
2836 | FT_STRING, BASE_NONE,
2837 | NULL((void*)0), 0x0,
2838 | "NMEA 0183 VHW Water speed unit, must be K", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2839 | {&hf_nmea0183_vlw_cumulative_water,
2840 | {"Cumulative water distance", "nmea0183.vlw_hf_nmea0183_vlw_cumulative_water",
2841 | FT_STRING, BASE_NONE,
2842 | NULL((void*)0), 0x0,
2843 | "NMEA 0183 VLW Total cumulative water distance, nautical miles", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2844 | {&hf_nmea0183_vlw_cumulative_water_unit,
2845 | {"Distance unit", "nmea0183.vlw_cumulative_water_unit",
2846 | FT_STRING, BASE_NONE,
2847 | NULL((void*)0), 0x0,
2848 | "NMEA 0183 VLW Distance unit, must be N", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2849 | {&hf_nmea0183_vlw_trip_water,
2850 | {"Trip water distance", "nmea0183.vlw_hf_nmea0183_vlw_trip_water",
2851 | FT_STRING, BASE_NONE,
2852 | NULL((void*)0), 0x0,
2853 | "NMEA 0183 VLW Water distance since Reset, nautical miles", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2854 | {&hf_nmea0183_vlw_trip_water_unit,
2855 | {"Distance unit", "nmea0183.vlw_trip_water_unit",
2856 | FT_STRING, BASE_NONE,
2857 | NULL((void*)0), 0x0,
2858 | "NMEA 0183 VLW Distance unit, must be N", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2859 | {&hf_nmea0183_vlw_cumulative_ground,
2860 | {"Cumulative ground distance", "nmea0183.vlw_hf_nmea0183_vlw_cumulative_ground",
2861 | FT_STRING, BASE_NONE,
2862 | NULL((void*)0), 0x0,
2863 | "NMEA 0183 VLW Total cumulative ground distance, nautical miles (NMEA 3 and above)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2864 | {&hf_nmea0183_vlw_cumulative_ground_unit,
2865 | {"Distance unit", "nmea0183.vlw_cumulative_ground_unit",
2866 | FT_STRING, BASE_NONE,
2867 | NULL((void*)0), 0x0,
2868 | "NMEA 0183 VLW Distance unit, must be N", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2869 | {&hf_nmea0183_vlw_trip_ground,
2870 | {"Trip ground distance", "nmea0183.vlw_hf_nmea0183_vlw_trip_ground",
2871 | FT_STRING, BASE_NONE,
2872 | NULL((void*)0), 0x0,
2873 | "NMEA 0183 VLW Ground distance since Reset, nautical miles (NMEA 3 and above)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2874 | {&hf_nmea0183_vlw_trip_ground_unit,
2875 | {"Distance unit", "nmea0183.vlw_trip_ground_unit",
2876 | FT_STRING, BASE_NONE,
2877 | NULL((void*)0), 0x0,
2878 | "NMEA 0183 VLW Distance unit, must be N", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2879 | {&hf_nmea0183_vtg_true_course,
2880 | {"True course over ground", "nmea0183.vtg_true_course",
2881 | FT_STRING, BASE_NONE,
2882 | NULL((void*)0), 0x0,
2883 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2884 | {&hf_nmea0183_vtg_true_course_unit,
2885 | {"Course unit", "nmea0183.vtg_true_course_unit",
2886 | FT_STRING, BASE_NONE,
2887 | NULL((void*)0), 0x0,
2888 | "NMEA 0183 VTG Course unit, must be T", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2889 | {&hf_nmea0183_vtg_magnetic_course,
2890 | {"Magnetic course over ground", "nmea0183.vtg_magnetic_course",
2891 | FT_STRING, BASE_NONE,
2892 | NULL((void*)0), 0x0,
2893 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2894 | {&hf_nmea0183_vtg_magnetic_course_unit,
2895 | {"Course unit", "nmea0183.vtg_magnetic_course_unit",
2896 | FT_STRING, BASE_NONE,
2897 | NULL((void*)0), 0x0,
2898 | "NMEA 0183 VTG Course unit, must be M", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2899 | {&hf_nmea0183_vtg_ground_speed_knot,
2900 | {"Speed over ground", "nmea0183.vtg_ground_speed_knot",
2901 | FT_STRING, BASE_NONE,
2902 | NULL((void*)0), 0x0,
2903 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2904 | {&hf_nmea0183_vtg_ground_speed_knot_unit,
2905 | {"Speed unit", "nmea0183.vtg_ground_speed_knot_unit",
2906 | FT_STRING, BASE_NONE,
2907 | NULL((void*)0), 0x0,
2908 | "NMEA 0183 VTG Ground speed unit, must be N", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2909 | {&hf_nmea0183_vtg_ground_speed_kilometer,
2910 | {"Speed over ground", "nmea0183.vtg_ground_speed_kilometer",
2911 | FT_STRING, BASE_NONE,
2912 | NULL((void*)0), 0x0,
2913 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2914 | {&hf_nmea0183_vtg_ground_speed_kilometer_unit,
2915 | {"Speed unit", "nmea0183.vtg_ground_speed_kilometer_unit",
2916 | FT_STRING, BASE_NONE,
2917 | NULL((void*)0), 0x0,
2918 | "NMEA 0183 VTG Ground speed unit, must be K", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2919 | {&hf_nmea0183_vtg_mode,
2920 | {"FAA mode", "nmea0183.vtg_mode",
2921 | FT_STRING, BASE_NONE,
2922 | NULL((void*)0), 0x0,
2923 | "NMEA 0183 VTG FAA mode indicator (NMEA 2.3 and later)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2924 | {&hf_nmea0183_zda_time,
2925 | {"UTC Time", "nmea0183.zda_time",
2926 | FT_NONE, BASE_NONE,
2927 | NULL((void*)0), 0x0,
2928 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2929 | {&hf_nmea0183_zda_time_hour,
2930 | {"Hour", "nmea0183.zda_time_hour",
2931 | FT_STRING, BASE_NONE,
2932 | NULL((void*)0), 0x0,
2933 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2934 | {&hf_nmea0183_zda_time_minute,
2935 | {"Minute", "nmea0183.zda_time_minute",
2936 | FT_STRING, BASE_NONE,
2937 | NULL((void*)0), 0x0,
2938 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2939 | {&hf_nmea0183_zda_time_second,
2940 | {"Second", "nmea0183.zda_time_second",
2941 | FT_STRING, BASE_NONE,
2942 | NULL((void*)0), 0x0,
2943 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2944 | {&hf_nmea0183_zda_date_day,
2945 | {"Day", "nmea0183.zda_date_day",
2946 | FT_STRING, BASE_NONE,
2947 | NULL((void*)0), 0x0,
2948 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2949 | {&hf_nmea0183_zda_date_month,
2950 | {"Month", "nmea0183.zda_date_month",
2951 | FT_STRING, BASE_NONE,
2952 | NULL((void*)0), 0x0,
2953 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2954 | {&hf_nmea0183_zda_date_year,
2955 | {"Year", "nmea0183.zda_date_year",
2956 | FT_STRING, BASE_NONE,
2957 | NULL((void*)0), 0x0,
2958 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2959 | {&hf_nmea0183_zda_local_zone_hour,
2960 | {"Local zone hour", "nmea0183.zda_local_zone_hour",
2961 | FT_STRING, BASE_NONE,
2962 | NULL((void*)0), 0x0,
2963 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2964 | { &hf_nmea0183_zda_local_zone_minute,
2965 | {"Local zone minute", "nmea0183.zda_local_zone_minute",
2966 | FT_STRING, BASE_NONE,
2967 | NULL((void*)0), 0x0,
2968 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}},
2969 | { &hf_nmea0183_sentence_prefix,
2970 | { "Sentence prefix", "nmea0183.sentence_prefix",
2971 | FT_STRING, BASE_NONE,
2972 | NULL((void*)0), 0x0,
2973 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2974 | { &hf_nmea0183_tag_block,
2975 | { "Tag block", "nmea0183.tag_block",
2976 | FT_STRING, BASE_NONE,
2977 | NULL((void*)0), 0x0,
2978 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2979 | { &hf_nmea0183_bin_version,
2980 | { "Version", "nmea0183.bin.version",
2981 | FT_UINT16, BASE_DEC,
2982 | NULL((void*)0), 0x0,
2983 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2984 | { &hf_nmea0183_bin_srcid,
2985 | { "Source Id", "nmea0183.bin.src_id",
2986 | FT_STRING, BASE_NONE,
2987 | NULL((void*)0), 0x0,
2988 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2989 | { &hf_nmea0183_bin_dstid,
2990 | { "Destination Id", "nmea0183.bin.dst_id",
2991 | FT_STRING, BASE_NONE,
2992 | NULL((void*)0), 0x0,
2993 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
2994 | { &hf_nmea0183_bin_mtype,
2995 | { "Mtype", "nmea0183.bin.mtype",
2996 | FT_UINT16, BASE_DEC,
2997 | VALS(nmea0183_bin_mtype_vals)((0 ? (const struct _value_string*)0 : ((nmea0183_bin_mtype_vals )))), 0x0,
2998 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
2999 | { &hf_nmea0183_bin_blockid,
3000 | { "Blockid", "nmea0183.bin.blockid",
3001 | FT_UINT32, BASE_DEC,
3002 | NULL((void*)0), 0x0,
3003 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3004 | { &hf_nmea0183_bin_seqnum,
3005 | { "Sequence number", "nmea0183.bin.seqnum",
3006 | FT_UINT32, BASE_DEC,
3007 | NULL((void*)0), 0x0,
3008 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3009 | { &hf_nmea0183_bin_max_seqnum,
3010 | { "Max Sequence number", "nmea0183.bin.maxseqnum",
3011 | FT_UINT32, BASE_DEC,
3012 | NULL((void*)0), 0x0,
3013 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3014 | { &hf_nmea0183_bin_data,
3015 | { "Data", "nmea0183.bin.data",
3016 | FT_BYTES, BASE_NONE,
3017 | NULL((void*)0), 0x0,
3018 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3019 | { &hf_nmea0183_bin_file_descriptor,
3020 | { "File descriptor", "nmea0183.bin.file_descriptor",
3021 | FT_STRING, BASE_NONE,
3022 | NULL((void*)0), 0x0,
3023 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3024 | { &hf_nmea0183_bin_file_descriptor_len,
3025 | { "File descriptor length", "nmea0183.bin.fd_len",
3026 | FT_UINT32, BASE_DEC,
3027 | NULL((void*)0), 0x0,
3028 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3029 | { &hf_nmea0183_bin_file_length,
3030 | { "File length", "nmea0183.bin.file_len",
3031 | FT_UINT32, BASE_DEC,
3032 | NULL((void*)0), 0x0,
3033 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3034 | { &hf_nmea0183_bin_stat_of_acquisition,
3035 | { "Status of acquisition", "nmea0183.bin.stat_of_acquisition",
3036 | FT_UINT16, BASE_DEC,
3037 | NULL((void*)0), 0x0,
3038 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3039 | { &hf_nmea0183_bin_device,
3040 | { "Device", "nmea0183.bin.device",
3041 | FT_UINT8, BASE_HEX,
3042 | NULL((void*)0), 0x0,
3043 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3044 | { &hf_nmea0183_bin_channel,
3045 | { "Channel", "nmea0183.bin.channel",
3046 | FT_UINT8, BASE_HEX,
3047 | NULL((void*)0), 0x0,
3048 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3049 | { &hf_nmea0183_bin_type_len,
3050 | { "Type length", "nmea0183.bin.type_len",
3051 | FT_UINT8, BASE_DEC,
3052 | NULL((void*)0), 0x0,
3053 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3054 | { &hf_nmea0183_bin_data_type,
3055 | { "Data type", "nmea0183.bin.data_type",
3056 | FT_STRING, BASE_NONE,
3057 | NULL((void*)0), 0x0,
3058 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3059 | { &hf_nmea0183_bin_status_and_info,
3060 | { "Status and information text", "nmea0183.bin.status_and_info",
3061 | FT_STRING, BASE_NONE,
3062 | NULL((void*)0), 0x0,
3063 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
3064 | };
3065 |
3066 | /* Setup protocol subtree array */
3067 | static int *ett[] = {
3068 | &ett_nmea0183,
3069 | &ett_nmea0183_checksum,
3070 | &ett_nmea0183_sentence,
3071 | &ett_nmea0183_zda_time,
3072 | &ett_nmea0183_alr_time,
3073 | &ett_nmea0183_gga_time,
3074 | &ett_nmea0183_gga_latitude,
3075 | &ett_nmea0183_gga_longitude,
3076 | &ett_nmea0183_gll_time,
3077 | &ett_nmea0183_gll_latitude,
3078 | &ett_nmea0183_gll_longitude,
3079 | &ett_nmea0183_gst_time,
3080 | &ett_nmea0183_tag_block,
3081 | &ett_nmea0183_fd
3082 | };
3083 |
3084 | static ei_register_info ei[] = {
3085 | {&ei_nmea0183_invalid_first_character,
3086 | {"nmea0183.invalid_first_character", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3087 | "First character should be '$'", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3088 | {&ei_nmea0183_missing_checksum_character,
3089 | {"nmea0183.missing_checksum_character", PI_MALFORMED0x07000000, PI_ERROR0x00800000,
3090 | "Missing begin of checksum character '*'", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3091 | {&ei_nmea0183_invalid_end_of_line,
3092 | {"nmea0183.invalid_end_of_line", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3093 | "Sentence should end with <CR><LF>", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3094 | {&ei_nmea0183_checksum_incorrect,
3095 | {"nmea0183.checksum_incorrect", PI_CHECKSUM0x01000000, PI_WARN0x00600000,
3096 | "Incorrect checksum", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3097 | {&ei_nmea0183_sentence_too_long,
3098 | {"nmea0183.sentence_too_long", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3099 | "Sentence is too long. Maximum is 82 bytes including $ and <CR><LF>", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3100 | {&ei_nmea0183_field_time_too_short,
3101 | {"nmea0183.field_time_too_short", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3102 | "Field containing time is too short. Field should be at least 6 characters", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3103 | {&ei_nmea0183_field_latitude_too_short,
3104 | {"nmea0183.field_latitude_too_short", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3105 | "Field containing latitude is too short. Field should be at least 4 characters", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3106 | {&ei_nmea0183_field_longitude_too_short,
3107 | {"nmea0183.field_longitude_too_short", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3108 | "Field containing longitude is too short. Field should be at least 5 characters", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3109 | {&ei_nmea0183_field_missing,
3110 | {"nmea0183.field_missing", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3111 | "Field expected, but not found", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3112 | {&ei_nmea0183_gga_altitude_unit_incorrect,
3113 | {"nmea0183.gga_altitude_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3114 | "Incorrect altitude unit (should be 'M')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3115 | {&ei_nmea0183_gga_geoidal_separation_unit_incorrect,
3116 | {"nmea0183.gga_geoidal_separation_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3117 | "Incorrect geoidal separation unit (should be 'M')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3118 | {&ei_nmea0183_hdt_unit_incorrect,
3119 | {"nmea0183.hdt_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3120 | "Incorrect heading unit (should be 'T')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3121 | {&ei_nmea0183_vhw_true_heading_unit_incorrect,
3122 | {"nmea0183.vhw_true_heading_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3123 | "Incorrect heading unit (should be 'T')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3124 | {&ei_nmea0183_vhw_magnetic_heading_unit_incorrect,
3125 | {"nmea0183.vhw_magnetic_heading_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3126 | "Incorrect heading unit (should be 'M')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3127 | {&ei_nmea0183_vhw_water_speed_knot_unit_incorrect,
3128 | {"nmea0183.vhw_water_speed_knot_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3129 | "Incorrect speed unit (should be 'N')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3130 | {&ei_nmea0183_vhw_water_speed_kilometer_unit_incorrect,
3131 | {"nmea0183.vhw_water_speed_kilometer_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3132 | "Incorrect speed unit (should be 'K')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3133 | {&ei_nmea0183_vlw_cumulative_water_unit_incorrect,
3134 | {"nmea0183.vlw_cumulative_water_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3135 | "Incorrect distance unit (should be 'N')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3136 | {&ei_nmea0183_vlw_trip_water_unit_incorrect,
3137 | {"nmea0183.vlw_trip_water_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3138 | "Incorrect distance unit (should be 'N')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3139 | {&ei_nmea0183_vlw_cumulative_ground_unit_incorrect,
3140 | {"nmea0183.vlw_cumulative_ground_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3141 | "Incorrect distance unit (should be 'N')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3142 | {&ei_nmea0183_vlw_trip_ground_unit_incorrect,
3143 | {"nmea0183.vlw_trip_ground_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3144 | "Incorrect distance unit (should be 'N')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3145 | {&ei_nmea0183_vtg_true_course_unit_incorrect,
3146 | {"nmea0183.vtg_true_course_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3147 | "Incorrect course unit (should be 'T')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3148 | {&ei_nmea0183_vtg_magnetic_course_unit_incorrect,
3149 | {"nmea0183.vtg_magnetic_course_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3150 | "Incorrect course unit (should be 'M')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3151 | {&ei_nmea0183_vtg_ground_speed_knot_unit_incorrect,
3152 | {"nmea0183.vtg_ground_speed_knot_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3153 | "Incorrect speed unit (should be 'N')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}},
3154 | {&ei_nmea0183_vtg_ground_speed_kilometer_unit_incorrect,
3155 | {"nmea0183.vtg_ground_speed_kilometer_unit_incorrect", PI_PROTOCOL0x09000000, PI_WARN0x00600000,
3156 | "Incorrect speed unit (should be 'K')", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}}}};
3157 |
3158 | proto_nmea0183 = proto_register_protocol("NMEA 0183 protocol", "NMEA 0183", "nmea0183");
3159 | proto_nmea0183_bin = proto_register_protocol("NMEA 0183 binary protocol", "NMEA 0183 BIN", "nmea0183_bin");
3160 |
3161 | proto_register_field_array(proto_nmea0183, hf, array_length(hf)(sizeof (hf) / sizeof (hf)[0]));
3162 | proto_register_subtree_array(ett, array_length(ett)(sizeof (ett) / sizeof (ett)[0]));
3163 | expert_nmea0183 = expert_register_protocol(proto_nmea0183);
3164 | expert_register_field_array(expert_nmea0183, ei, array_length(ei)(sizeof (ei) / sizeof (ei)[0]));
3165 |
3166 | nmea0183_handle = register_dissector("nmea0183", dissect_nmea0183, proto_nmea0183);
3167 | }
3168 |
3169 | void proto_reg_handoff_nmea0183(void)
3170 | {
3171 | /* Register the UDP PDU NMEA0183 handle for heuristic dissection */
3172 | heur_dissector_add("udp", dissect_nmea0183_heur, "NMEA0183 over UDP",
3173 | "nmea0183_udp", proto_nmea0183, HEURISTIC_DISABLE);
3174 | dissector_add_for_decode_as_with_preference("udp.port", nmea0183_handle);
3175 | }