### Bug Summary

File: | epan/proto.c
Warning: | line 13567, column 39 The result of left shift is undefined because the right operand '64' is not smaller than 64, the capacity of 'uint64_t'

### Annotated Source Code

Press '?' to see keyboard shortcuts

Show analyzer invocation
clang -cc1 -cc1 -triple x86_64-pc-linux-gnu -analyze -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name proto.c -analyzer-checker=core -analyzer-checker=apiModeling -analyzer-checker=unix -analyzer-checker=deadcode -analyzer-checker=security.insecureAPI.UncheckedReturn -analyzer-checker=security.insecureAPI.getpw -analyzer-checker=security.insecureAPI.gets -analyzer-checker=security.insecureAPI.mktemp -analyzer-checker=security.insecureAPI.mkstemp -analyzer-checker=security.insecureAPI.vfork -analyzer-checker=nullability.NullPassedToNonnull -analyzer-checker=nullability.NullReturnedFromNonnull -analyzer-output plist -w -setup-static-analyzer -mrelocation-model pic -pic-level 2 -fhalf-no-semantic-interposition -fno-delete-null-pointer-checks -mframe-pointer=all -relaxed-aliasing -fmath-errno -ffp-contract=on -fno-rounding-math -ffloat16-excess-precision=fast -fbfloat16-excess-precision=fast -mconstructor-aliases -funwind-tables=2 -target-cpu x86-64 -tune-cpu generic -debugger-tuning=gdb -fdebug-compilation-dir=/builds/wireshark/wireshark/build -fcoverage-compilation-dir=/builds/wireshark/wireshark/build -resource-dir /usr/lib/llvm-21/lib/clang/21 -isystem /usr/include/glib-2.0 -isystem /usr/lib/x86_64-linux-gnu/glib-2.0/include -isystem /builds/wireshark/wireshark/epan -isystem /builds/wireshark/wireshark/build/epan -isystem /usr/include/mit-krb5 -isystem /usr/include/libxml2 -isystem /usr/include/lua5.4 -D G_DISABLE_DEPRECATED -D G_DISABLE_SINGLE_INCLUDES -D WS_BUILD_DLL -D WS_DEBUG -D WS_DEBUG_UTF_8 -D epan_EXPORTS -I /builds/wireshark/wireshark/build -I /builds/wireshark/wireshark -I /builds/wireshark/wireshark/include -I /builds/wireshark/wireshark/wiretap -D _GLIBCXX_ASSERTIONS -internal-isystem /usr/lib/llvm-21/lib/clang/21/include -internal-isystem /usr/local/include -internal-isystem /usr/lib/gcc/x86_64-linux-gnu/14/../../../../x86_64-linux-gnu/include -internal-externc-isystem /usr/include/x86_64-linux-gnu -internal-externc-isystem /include -internal-externc-isystem /usr/include -fmacro-prefix-map=/builds/wireshark/wireshark/= -fmacro-prefix-map=/builds/wireshark/wireshark/build/= -fmacro-prefix-map=../= -Wno-format-nonliteral -std=gnu11 -ferror-limit 19 -fvisibility=hidden -fwrapv -fwrapv-pointer -fstrict-flex-arrays=3 -stack-protector 2 -fstack-clash-protection -fcf-protection=full -fgnuc-version=4.2.1 -fskip-odr-check-in-gmf -fexceptions -fcolor-diagnostics -analyzer-output=html -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -o /builds/wireshark/wireshark/sbout/2026-01-15-100408-3603-1 -x c /builds/wireshark/wireshark/epan/proto.c

Keyboard shortcuts:

- Use 'j/k' keys for keyboard navigation
- Use 'Shift+S' to show/hide relevant lines
- Use '?' to toggle this window

Close
Show only relevant lines Show control flow arrows

1 | /* proto.c
2 | * Routines for protocol tree
3 | *
4 | * Wireshark - Network traffic analyzer
5 | * By Gerald Combs <gerald@wireshark.org>
6 | * Copyright 1998 Gerald Combs
7 | *
8 | * SPDX-License-Identifier: GPL-2.0-or-later
9 | */
10 |
11 | #include "config.h"
12 | #define WS_LOG_DOMAIN"Epan" LOG_DOMAIN_EPAN"Epan"
13 | #include "wireshark.h"
14 |
15 | #include <float.h>
16 | #include <errno(*__errno_location ()).h>
17 |
18 | #include <epan/tfs.h>
19 | #include <epan/unit_strings.h>
20 |
21 | #include <wsutil/array.h>
22 | #include <wsutil/bits_ctz.h>
23 | #include <wsutil/bits_count_ones.h>
24 | #include <wsutil/sign_ext.h>
25 | #include <wsutil/utf8_entities.h>
26 | #include <wsutil/json_dumper.h>
27 | #include <wsutil/pint.h>
28 | #include <wsutil/unicode-utils.h>
29 | #include <wsutil/dtoa.h>
30 | #include <wsutil/filesystem.h>
31 | #ifdef HAVE_UNISTD_H1
32 | #include <unistd.h>
33 | #endif
34 |
35 | #include <ftypes/ftypes.h>
36 | #include <ftypes/ftypes-int.h>
37 |
38 | #include <epan/packet.h>
39 | #include "exceptions.h"
40 | #include "ptvcursor.h"
41 | #include "strutil.h"
42 | #include "addr_resolv.h"
43 | #include "address_types.h"
44 | #include "oids.h"
45 | #include "proto.h"
46 | #include "epan_dissect.h"
47 | #include "dfilter/dfilter.h"
48 | #include "tvbuff.h"
49 | #include "charsets.h"
50 | #include "column-info.h"
51 | #include "to_str.h"
52 | #include "osi-utils.h"
53 | #include "expert.h"
54 | #include "show_exception.h"
55 | #include "in_cksum.h"
56 |
57 | #include <wsutil/crash_info.h>
58 | #include <wsutil/epochs.h>
59 |
60 | /* Ptvcursor limits */
61 | #define SUBTREE_ONCE_ALLOCATION_NUMBER8 8
62 | #define SUBTREE_MAX_LEVELS256 256
63 |
64 | typedef struct __subtree_lvl {
65 | int cursor_offset;
66 | proto_item *it;
67 | proto_tree *tree;
68 | } subtree_lvl;
69 |
70 | struct ptvcursor {
71 | wmem_allocator_t *scope;
72 | subtree_lvl *pushed_tree;
73 | uint8_t pushed_tree_index;
74 | uint8_t pushed_tree_max;
75 | proto_tree *tree;
76 | tvbuff_t *tvb;
77 | int offset;
78 | };
79 |
80 | #define cVALS(x)(const value_string*)(x) (const value_string*)(x)
81 |
82 | /** See inlined comments.
83 | @param tree the tree to append this item to
84 | @param free_block a code block to call to free resources if this returns
85 | @return NULL if 'tree' is null */
86 | #define CHECK_FOR_NULL_TREE_AND_FREE(tree, free_block)if (!tree) { free_block; return ((void*)0); } \
87 | if (!tree) { \
88 | free_block; \
89 | return NULL((void*)0); \
90 | }
91 |
92 | /** See inlined comments.
93 | @param tree the tree to append this item to
94 | @return NULL if 'tree' is null */
95 | #define CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); } \
96 | CHECK_FOR_NULL_TREE_AND_FREE(tree, ((void)0))if (!tree) { ((void)0); return ((void*)0); }
97 |
98 | /** See inlined comments.
99 | @param length the length of this item
100 | @param cleanup_block a code block to call to free resources if this returns
101 | @return NULL if 'length' is lower -1 or equal 0 */
102 | #define CHECK_FOR_ZERO_OR_MINUS_LENGTH_AND_CLEANUP(length, cleanup_block)if (length < -1 || length == 0 ) { cleanup_block; return ( (void*)0); } \
103 | if (length < -1 || length == 0 ) { \
104 | cleanup_block; \
105 | return NULL((void*)0); \
106 | }
107 |
108 | /** See inlined comments.
109 | @param length the length of this item
110 | @return NULL if 'length' is lower -1 or equal 0 */
111 | #define CHECK_FOR_ZERO_OR_MINUS_LENGTH(length)if (length < -1 || length == 0 ) { ((void)0); return ((void *)0); } \
112 | CHECK_FOR_ZERO_OR_MINUS_LENGTH_AND_CLEANUP(length, ((void)0))if (length < -1 || length == 0 ) { ((void)0); return ((void *)0); }
113 |
114 | /** See inlined comments.
115 | @param tree the tree to append this item to
116 | @param hfindex field index
117 | @param hfinfo header_field
118 | @param free_block a code block to call to free resources if this returns
119 | @return the header field matching 'hfinfo' */
120 | #define TRY_TO_FAKE_THIS_ITEM_OR_FREE(tree, hfindex, hfinfo, free_block)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 120 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 120, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 120, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { free_block; if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 120, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { free_block; return proto_tree_add_fake_node(tree, hfinfo ); } } } \
121 | /* If the tree is not visible and this item is not referenced \
122 | we don't have to do much work at all but we should still \
123 | return a node so that referenced field items below this node \
124 | (think proto_item_add_subtree()) will still have somewhere \
125 | to attach to or else filtering will not work (they would be \
126 | ignored since tree would be NULL). \
127 | DON'T try to fake a node where PTREE_FINFO(tree) is visible \
128 | because that means we can change its length or repr, and we \
129 | don't want to do so with calls intended for this faked new \
130 | item, so this item needs a new (hidden) child node. \
131 | We fake FT_PROTOCOL unless some clients have requested us \
132 | not to do so. \
133 | */ \
134 | PTREE_DATA(tree)((tree)->tree_data)->count++; \
135 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 135, __func__, "Unregistered hf! index=%d", hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 135, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 135, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; \
136 | if (PTREE_DATA(tree)((tree)->tree_data)->count > prefs.gui_max_tree_items) { \
137 | free_block; \
138 | if (wireshark_abort_on_too_many_items) \
139 | ws_error("Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)", \ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 140 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items)
140 | hfinfo->abbrev, prefs.gui_max_tree_items)ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 140 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); \
141 | /* Let the exception handler add items to the tree */ \
142 | PTREE_DATA(tree)((tree)->tree_data)->count = 0; \
143 | THROW_MESSAGE(DissectorError, \except_throw(1, (6), (wmem_strdup_printf(((tree)->tree_data ->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items)))
144 | wmem_strdup_printf(PNODE_POOL(tree), \except_throw(1, (6), (wmem_strdup_printf(((tree)->tree_data ->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items)))
145 | "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)", \except_throw(1, (6), (wmem_strdup_printf(((tree)->tree_data ->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items)))
146 | hfinfo->abbrev, prefs.gui_max_tree_items))except_throw(1, (6), (wmem_strdup_printf(((tree)->tree_data ->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); \
147 | } \
148 | if (!(PTREE_DATA(tree)((tree)->tree_data)->visible)) { \
149 | if (PROTO_ITEM_IS_HIDDEN(tree)proto_item_is_hidden((tree))) { \
150 | if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) \
151 | && (hfinfo->ref_type != HF_REF_TYPE_PRINT) \
152 | && (hfinfo->type != FT_PROTOCOL || \
153 | PTREE_DATA(tree)((tree)->tree_data)->fake_protocols)) { \
154 | free_block; \
155 | /* return fake node with no field info */\
156 | return proto_tree_add_fake_node(tree, hfinfo); \
157 | } \
158 | } \
159 | }
160 |
161 | /** See inlined comments.
162 | @param tree the tree to append this item to
163 | @param hfindex field index
164 | @param hfinfo header_field
165 | @return the header field matching 'hfinfo' */
166 | #define TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 166 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 166, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 166, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 166, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } } \
167 | TRY_TO_FAKE_THIS_ITEM_OR_FREE(tree, hfindex, hfinfo, ((void)0))((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 167 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 167, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 167, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 167, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } }
168 |
169 |
170 | /** See inlined comments.
171 | @param pi the created protocol item we're about to return */
172 | #define TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 172, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; } \
173 | ws_assert(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 173, __func__, "assertion failed: %s", "pi" ); } while (0); \
174 | if (!PITEM_FINFO(pi)((pi)->finfo)) \
175 | return pi; \
176 | if (!(PTREE_DATA(pi)((pi)->tree_data)->visible) && \
177 | PROTO_ITEM_IS_HIDDEN(pi)proto_item_is_hidden((pi))) { \
178 | /* If the tree (GUI) or item isn't visible it's pointless for \
179 | * us to generate the protocol item's string representation */ \
180 | return pi; \
181 | }
182 | /* Same as above but returning void */
183 | #define TRY_TO_FAKE_THIS_REPR_VOID(pi)if (!pi || !((pi)->finfo)) return; if (!(((pi)->tree_data )->visible) && proto_item_is_hidden((pi))) { return ; } \
184 | if (!pi || !PITEM_FINFO(pi)((pi)->finfo)) \
185 | return; \
186 | if (!(PTREE_DATA(pi)((pi)->tree_data)->visible) && \
187 | PROTO_ITEM_IS_HIDDEN(pi)proto_item_is_hidden((pi))) { \
188 | /* If the tree (GUI) or item isn't visible it's pointless for \
189 | * us to generate the protocol item's string representation */ \
190 | return; \
191 | }
192 | /* Similar to above, but allows a NULL tree */
193 | #define TRY_TO_FAKE_THIS_REPR_NESTED(pi)if ((pi == ((void*)0)) || (((pi)->finfo) == ((void*)0)) || (!(((pi)->tree_data)->visible) && proto_item_is_hidden ((pi)))) { return pi; } \
194 | if ((pi == NULL((void*)0)) || (PITEM_FINFO(pi)((pi)->finfo) == NULL((void*)0)) || (!(PTREE_DATA(pi)((pi)->tree_data)->visible) && \
195 | PROTO_ITEM_IS_HIDDEN(pi)proto_item_is_hidden((pi)))) { \
196 | /* If the tree (GUI) or item isn't visible it's pointless for \
197 | * us to generate the protocol item's string representation */ \
198 | return pi; \
199 | }
200 |
201 | #ifdef ENABLE_CHECK_FILTER
202 | #define CHECK_HF_VALUE(type, spec, start_values) \
203 | { \
204 | const type *current; \
205 | int n, m; \
206 | current = start_values; \
207 | for (n=0; current; n++, current++) { \
208 | /* Drop out if we reached the end. */ \
209 | if ((current->value == 0) && (current->strptr == NULL((void*)0))) { \
210 | break; \
211 | } \
212 | /* Check value against all previous */ \
213 | for (m=0; m < n; m++) { \
214 | /* There are lots of duplicates with the same string, \
215 | so only report if different... */ \
216 | if ((start_values[m].value == current->value) && \
217 | (strcmp(start_values[m].strptr, current->strptr) != 0)) { \
218 | ws_error("Field '%s' (%s) has a conflicting entry in its" \ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 221 , __func__, "Field '%s' (%s) has a conflicting entry in its" " value_string: %" spec " is at indices %u (%s) and %u (%s)", hfinfo->name, hfinfo ->abbrev, current->value, m, start_values[m].strptr, n, current->strptr)
219 | " value_string: %" spec " is at indices %u (%s) and %u (%s)", \ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 221 , __func__, "Field '%s' (%s) has a conflicting entry in its" " value_string: %" spec " is at indices %u (%s) and %u (%s)", hfinfo->name, hfinfo ->abbrev, current->value, m, start_values[m].strptr, n, current->strptr)
220 | hfinfo->name, hfinfo->abbrev, \ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 221 , __func__, "Field '%s' (%s) has a conflicting entry in its" " value_string: %" spec " is at indices %u (%s) and %u (%s)", hfinfo->name, hfinfo ->abbrev, current->value, m, start_values[m].strptr, n, current->strptr)
221 | current->value, m, start_values[m].strptr, n, current->strptr)ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 221 , __func__, "Field '%s' (%s) has a conflicting entry in its" " value_string: %" spec " is at indices %u (%s) and %u (%s)", hfinfo->name, hfinfo ->abbrev, current->value, m, start_values[m].strptr, n, current->strptr); \
222 | } \
223 | } \
224 | } \
225 | }
226 | #endif
227 |
228 | /* The longest NUMBER-like field label we have is for BASE_OUI, which
229 | * can have up to 64 bytes for the manufacturer name if resolved plus
230 | * 11 bytes for the "XX:XX:XX ()" part = 75 octets.
231 | */
232 | #define NUMBER_LABEL_LENGTH80 80
233 |
234 | static const char *hf_try_val_to_str(uint32_t value, const header_field_info *hfinfo);
235 | static const char *hf_try_val64_to_str(uint64_t value, const header_field_info *hfinfo);
236 | static const char *hf_try_val_to_str_const(uint32_t value, const header_field_info *hfinfo, const char *unknown_str);
237 | static const char *hf_try_val64_to_str_const(uint64_t value, const header_field_info *hfinfo, const char *unknown_str);
238 | static int hfinfo_bitoffset(const header_field_info *hfinfo);
239 | static int hfinfo_mask_bitwidth(const header_field_info *hfinfo);
240 | static int hfinfo_container_bitwidth(const header_field_info *hfinfo);
241 |
242 | #define label_concat(dst, pos, src)ws_label_strcpy(dst, 240, pos, src, 0) \
243 | ws_label_strcpy(dst, ITEM_LABEL_LENGTH240, pos, src, 0)
244 |
245 | static void mark_truncated(char *label_str, size_t name_pos, const size_t size, size_t *value_pos);
246 | static void label_mark_truncated(char *label_str, size_t name_pos, size_t *value_pos);
247 |
248 | static void fill_label_boolean(const field_info *fi, char *label_str, size_t *value_pos);
249 | static void fill_label_bitfield_char(const field_info *fi, char *label_str, size_t *value_pos);
250 | static void fill_label_bitfield(const field_info *fi, char *label_str, size_t *value_pos, bool_Bool is_signed);
251 | static void fill_label_bitfield64(const field_info *fi, char *label_str, size_t *value_pos, bool_Bool is_signed);
252 | static void fill_label_char(const field_info *fi, char *label_str, size_t *value_pos);
253 | static void fill_label_number(const field_info *fi, char *label_str, size_t *value_pos, bool_Bool is_signed);
254 | static void fill_label_number64(const field_info *fi, char *label_str, size_t *value_pos, bool_Bool is_signed);
255 |
256 | static size_t fill_display_label_float(const field_info *fi, char *label_str, const int label_str_size);
257 | static void fill_label_float(const field_info *fi, char *label_str, size_t *value_pos);
258 | static size_t fill_display_label_ieee_11073_float(const field_info *fi, char *label_str, const int label_str_size);
259 | static void fill_label_ieee_11073_float(const field_info *fi, char *label_str, size_t *value_pos);
260 |
261 | static const char *hfinfo_number_value_format_display(const header_field_info *hfinfo, int display, char buf[NUMBER_LABEL_LENGTH80], uint32_t value);
262 | static const char *hfinfo_number_value_format_display64(const header_field_info *hfinfo, int display, char buf[NUMBER_LABEL_LENGTH80], uint64_t value);
263 | static const char *hfinfo_char_vals_format(const header_field_info *hfinfo, char buf[32], uint32_t value);
264 | static const char* hfinfo_char_value_format_display(int display, char buf[7], uint32_t value);
265 | static const char *hfinfo_number_vals_format(const header_field_info *hfinfo, char buf[NUMBER_LABEL_LENGTH80], uint32_t value);
266 | static const char *hfinfo_number_vals_format64(const header_field_info *hfinfo, char buf[NUMBER_LABEL_LENGTH80], uint64_t value);
267 | static const char *hfinfo_number_value_format(const header_field_info *hfinfo, char buf[NUMBER_LABEL_LENGTH80], uint32_t value);
268 | static const char *hfinfo_number_value_format64(const header_field_info *hfinfo, char buf[NUMBER_LABEL_LENGTH80], uint64_t value);
269 | static const char *hfinfo_char_value_format(const header_field_info *hfinfo, char buf[32], uint32_t value);
270 | static const char *hfinfo_numeric_value_format(const header_field_info *hfinfo, char buf[NUMBER_LABEL_LENGTH80], uint32_t value);
271 | static const char *hfinfo_numeric_value_format64(const header_field_info *hfinfo, char buf[NUMBER_LABEL_LENGTH80], uint64_t value);
272 |
273 | static void proto_cleanup_base(void);
274 |
275 | static proto_item *
276 | proto_tree_add_node(proto_tree *tree, field_info *fi);
277 |
278 | static proto_item *
279 | proto_tree_add_fake_node(proto_tree *tree, const header_field_info *hfinfo);
280 |
281 | static void
282 | get_hfi_length(header_field_info *hfinfo, tvbuff_t *tvb, const int start, int *length,
283 | int *item_length, const unsigned encoding);
284 |
285 | static int
286 | get_full_length(header_field_info *hfinfo, tvbuff_t *tvb, const int start,
287 | int length, unsigned item_length, const int encoding);
288 |
289 | static field_info *
290 | new_field_info(proto_tree *tree, header_field_info *hfinfo, tvbuff_t *tvb,
291 | const int start, const int item_length);
292 |
293 | static proto_item *
294 | proto_tree_add_pi(proto_tree *tree, header_field_info *hfinfo, tvbuff_t *tvb,
295 | int start, int *length);
296 |
297 | static void
298 | proto_tree_set_representation_value(proto_item *pi, const char *format, va_list ap);
299 | static void
300 | proto_tree_set_representation(proto_item *pi, const char *format, va_list ap);
301 |
302 | static void
303 | proto_tree_set_protocol_tvb(field_info *fi, tvbuff_t *tvb, const char* field_data, int length);
304 | static void
305 | proto_tree_set_bytes(field_info *fi, const uint8_t* start_ptr, int length);
306 | static void
307 | proto_tree_set_bytes_tvb(field_info *fi, tvbuff_t *tvb, int offset, int length);
308 | static void
309 | proto_tree_set_bytes_gbytearray(field_info *fi, const GByteArray *value);
310 | static void
311 | proto_tree_set_time(field_info *fi, const nstime_t *value_ptr);
312 | static void
313 | proto_tree_set_string(field_info *fi, const char* value);
314 | static void
315 | proto_tree_set_ax25(field_info *fi, const uint8_t* value);
316 | static void
317 | proto_tree_set_ax25_tvb(field_info *fi, tvbuff_t *tvb, int start);
318 | static void
319 | proto_tree_set_vines(field_info *fi, const uint8_t* value);
320 | static void
321 | proto_tree_set_vines_tvb(field_info *fi, tvbuff_t *tvb, int start);
322 | static void
323 | proto_tree_set_ether(field_info *fi, const uint8_t* value);
324 | static void
325 | proto_tree_set_ether_tvb(field_info *fi, tvbuff_t *tvb, int start);
326 | static void
327 | proto_tree_set_ipxnet(field_info *fi, uint32_t value);
328 | static void
329 | proto_tree_set_ipv4(field_info *fi, ws_in4_addr value);
330 | static void
331 | proto_tree_set_ipv6(field_info *fi, const ws_in6_addr* value);
332 | static void
333 | proto_tree_set_ipv6_tvb(field_info *fi, tvbuff_t *tvb, int start, int length);
334 | static void
335 | proto_tree_set_fcwwn_tvb(field_info *fi, tvbuff_t *tvb, int start, int length);
336 | static void
337 | proto_tree_set_guid(field_info *fi, const e_guid_t *value_ptr);
338 | static void
339 | proto_tree_set_guid_tvb(field_info *fi, tvbuff_t *tvb, int start, const unsigned encoding);
340 | static void
341 | proto_tree_set_oid(field_info *fi, const uint8_t* value_ptr, int length);
342 | static void
343 | proto_tree_set_oid_tvb(field_info *fi, tvbuff_t *tvb, int start, int length);
344 | static void
345 | proto_tree_set_system_id(field_info *fi, const uint8_t* value_ptr, int length);
346 | static void
347 | proto_tree_set_system_id_tvb(field_info *fi, tvbuff_t *tvb, int start, int length);
348 | static void
349 | proto_tree_set_boolean(field_info *fi, uint64_t value);
350 | static void
351 | proto_tree_set_float(field_info *fi, float value);
352 | static void
353 | proto_tree_set_double(field_info *fi, double value);
354 | static void
355 | proto_tree_set_uint(field_info *fi, uint32_t value);
356 | static void
357 | proto_tree_set_int(field_info *fi, int32_t value);
358 | static void
359 | proto_tree_set_uint64(field_info *fi, uint64_t value);
360 | static void
361 | proto_tree_set_int64(field_info *fi, int64_t value);
362 | static void
363 | proto_tree_set_eui64(field_info *fi, const uint64_t value);
364 | static void
365 | proto_tree_set_eui64_tvb(field_info *fi, tvbuff_t *tvb, int start, const unsigned encoding);
366 |
367 | /* Handle type length mismatch (now filterable) expert info */
368 | static int proto_type_length_mismatch;
369 | static expert_field ei_type_length_mismatch_error;
370 | static expert_field ei_type_length_mismatch_warn;
371 | static void register_type_length_mismatch(void);
372 |
373 | /* Handle byte array string decoding errors with expert info */
374 | static int proto_byte_array_string_decoding_error;
375 | static expert_field ei_byte_array_string_decoding_failed_error;
376 | static void register_byte_array_string_decodinws_error(void);
377 |
378 | /* Handle date and time string decoding errors with expert info */
379 | static int proto_date_time_string_decoding_error;
380 | static expert_field ei_date_time_string_decoding_failed_error;
381 | static void register_date_time_string_decodinws_error(void);
382 |
383 | /* Handle string errors expert info */
384 | static int proto_string_errors;
385 | static expert_field ei_string_trailing_characters;
386 | static void register_string_errors(void);
387 |
388 | static int proto_register_field_init(header_field_info *hfinfo, const int parent);
389 |
390 | /* special-case header field used within proto.c */
391 | static header_field_info hfi_text_only =
392 | { "Text item", "text", FT_NONE, BASE_NONE, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) };
393 | int hf_text_only;
394 |
395 | /* Structure for information about a protocol */
396 | struct _protocol {
397 | const char *name; /* long description */
398 | const char *short_name; /* short description */
399 | const char *filter_name; /* name of this protocol in filters */
400 | GPtrArray *fields; /* fields for this protocol */
401 | int proto_id; /* field ID for this protocol */
402 | bool_Bool is_enabled; /* true if protocol is enabled */
403 | bool_Bool enabled_by_default; /* true if protocol is enabled by default */
404 | bool_Bool can_toggle; /* true if is_enabled can be changed */
405 | int parent_proto_id; /* Used to identify "pino"s (Protocol In Name Only).
406 | For dissectors that need a protocol name so they
407 | can be added to a dissector table, but use the
408 | parent_proto_id for things like enable/disable */
409 | GList *heur_list; /* Heuristic dissectors associated with this protocol */
410 | };
411 |
412 | /* List of all protocols */
413 | static GList *protocols;
414 |
415 | /* Structure stored for deregistered g_slice */
416 | struct g_slice_data {
417 | size_t block_size;
418 | void *mem_block;
419 | };
420 |
421 | /* Deregistered fields */
422 | static GPtrArray *deregistered_fields;
423 | static GPtrArray *deregistered_data;
424 | static GPtrArray *deregistered_slice;
425 |
426 | /* indexed by prefix, contains initializers */
427 | static GHashTable* prefixes;
428 |
429 | /* Contains information about a field when a dissector calls
430 | * proto_tree_add_item. */
431 | #define FIELD_INFO_NEW(pool, fi)fi = ((field_info*)wmem_alloc((pool), sizeof(field_info))) fi = wmem_new(pool, field_info)((field_info*)wmem_alloc((pool), sizeof(field_info)))
432 | #define FIELD_INFO_FREE(pool, fi)wmem_free(pool, fi) wmem_free(pool, fi)
433 |
434 | /* Contains the space for proto_nodes. */
435 | #define PROTO_NODE_INIT(node)node->first_child = ((void*)0); node->last_child = ((void *)0); node->next = ((void*)0); \
436 | node->first_child = NULL((void*)0); \
437 | node->last_child = NULL((void*)0); \
438 | node->next = NULL((void*)0);
439 |
440 | #define PROTO_NODE_FREE(pool, node)wmem_free(pool, node) \
441 | wmem_free(pool, node)
442 |
443 | /* String space for protocol and field items for the GUI */
444 | #define ITEM_LABEL_NEW(pool, il)il = ((item_label_t*)wmem_alloc((pool), sizeof(item_label_t)) ); il->value_pos = 0; il->value_len = 0; \
445 | il = wmem_new(pool, item_label_t)((item_label_t*)wmem_alloc((pool), sizeof(item_label_t))); \
446 | il->value_pos = 0; \
447 | il->value_len = 0;
448 | #define ITEM_LABEL_FREE(pool, il)wmem_free(pool, il); \
449 | wmem_free(pool, il);
450 |
451 | #define PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 451, __func__, "Unregistered hf! index=%d", hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 451, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 451, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex]; \
452 | if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) \
453 | ws_error("Unregistered hf! index=%d", hfindex)ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 453 , __func__, "Unregistered hf! index=%d", hfindex); \
454 | DISSECTOR_ASSERT_HINT(hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len, "Unregistered hf!")((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo .len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 454, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))); \
455 | DISSECTOR_ASSERT_HINT(gpa_hfinfo.hfi[hfindex] != NULL, "Unregistered hf!")((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : ( proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 455, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))); \
456 | hfinfo = gpa_hfinfo.hfi[hfindex];
457 |
458 | #define PROTO_PRE_ALLOC_HF_FIELDS_MEM(300000+5000) (300000+PRE_ALLOC_EXPERT_FIELDS_MEM5000)
459 |
460 | /* List which stores protocols and fields that have been registered */
461 | typedef struct _gpa_hfinfo_t {
462 | uint32_t len;
463 | uint32_t allocated_len;
464 | header_field_info **hfi;
465 | } gpa_hfinfo_t;
466 |
467 | static gpa_hfinfo_t gpa_hfinfo;
468 |
469 | /* Hash table of abbreviations and IDs */
470 | static wmem_map_t *gpa_name_map;
471 | static header_field_info *same_name_hfinfo;
472 |
473 | /* Hash table protocol aliases. const char * -> const char * */
474 | static GHashTable *gpa_protocol_aliases;
475 |
476 | /*
477 | * We're called repeatedly with the same field name when sorting a column.
478 | * Cache our last gpa_name_map hit for faster lookups.
479 | */
480 | static char *last_field_name;
481 | static header_field_info *last_hfinfo;
482 |
483 | /* Points to the first element of an array of bits, indexed by
484 | a subtree item type; that array element is true if subtrees of
485 | an item of that type are to be expanded. */
486 | static uint32_t *tree_is_expanded;
487 |
488 | /* Number of elements in that array. The entry with index 0 is not used. */
489 | int num_tree_types = 1;
490 |
491 | /* Name hashtables for fast detection of duplicate names */
492 | static GHashTable* proto_names;
493 | static GHashTable* proto_short_names;
494 | static GHashTable* proto_filter_names;
495 |
496 | static const char * const reserved_filter_names[] = {
497 | /* Display filter keywords. */
498 | "eq",
499 | "ne",
500 | "all_eq",
501 | "any_eq",
502 | "all_ne",
503 | "any_ne",
504 | "gt",
505 | "ge",
506 | "lt",
507 | "le",
508 | "bitand",
509 | "bitwise_and",
510 | "contains",
511 | "matches",
512 | "not",
513 | "and",
514 | "or",
515 | "xor",
516 | "in",
517 | "any",
518 | "all",
519 | "true",
520 | "false",
521 | "nan",
522 | "inf",
523 | "infinity",
524 | NULL((void*)0)
525 | };
526 |
527 | static GHashTable *proto_reserved_filter_names;
528 | static GQueue* saved_dir_queue;
529 |
530 | static int
531 | proto_compare_name(const void *p1_arg, const void *p2_arg)
532 | {
533 | const protocol_t *p1 = (const protocol_t *)p1_arg;
534 | const protocol_t *p2 = (const protocol_t *)p2_arg;
535 |
536 | return g_ascii_strcasecmp(p1->short_name, p2->short_name);
537 | }
538 |
539 | static GSList *dissector_plugins;
540 |
541 | #ifdef HAVE_PLUGINS1
542 | void
543 | proto_register_plugin(const proto_plugin *plug)
544 | {
545 | dissector_plugins = g_slist_prepend(dissector_plugins, (proto_plugin *)plug);
546 | }
547 | #else /* HAVE_PLUGINS */
548 | void
549 | proto_register_plugin(const proto_plugin *plug _U___attribute__((unused)))
550 | {
551 | ws_warning("proto_register_plugin: built without support for binary plugins")do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 551, __func__, "proto_register_plugin: built without support for binary plugins" ); } } while (0);
552 | }
553 | #endif /* HAVE_PLUGINS */
554 |
555 | static void
556 | call_plugin_register_protoinfo(void *data, void *user_data _U___attribute__((unused)))
557 | {
558 | proto_plugin *plug = (proto_plugin *)data;
559 |
560 | if (plug->register_protoinfo) {
561 | plug->register_protoinfo();
562 | }
563 | }
564 |
565 | static void
566 | call_plugin_register_handoff(void *data, void *user_data _U___attribute__((unused)))
567 | {
568 | proto_plugin *plug = (proto_plugin *)data;
569 |
570 | if (plug->register_handoff) {
571 | plug->register_handoff();
572 | }
573 | }
574 |
575 | void proto_pre_init(void)
576 | {
577 | saved_dir_queue = g_queue_new();
578 |
579 | proto_names = g_hash_table_new(wmem_str_hash, g_str_equal);
580 | proto_short_names = g_hash_table_new(wmem_str_hash, g_str_equal);
581 | proto_filter_names = g_hash_table_new(wmem_str_hash, g_str_equal);
582 |
583 | proto_reserved_filter_names = g_hash_table_new(wmem_str_hash, g_str_equal);
584 | for (const char* const * ptr = reserved_filter_names; *ptr != NULL((void*)0); ptr++) {
585 | /* GHashTable has no key destructor so the cast is safe. */
586 | g_hash_table_add(proto_reserved_filter_names, *(char**)ptr);
587 | }
588 |
589 | gpa_hfinfo.len = 0;
590 | gpa_hfinfo.allocated_len = 0;
591 | gpa_hfinfo.hfi = NULL((void*)0);
592 | gpa_name_map = wmem_map_new(wmem_epan_scope(), wmem_str_hash, g_str_equal);
593 | wmem_map_reserve(gpa_name_map, PROTO_PRE_ALLOC_HF_FIELDS_MEM(300000+5000));
594 | gpa_protocol_aliases = g_hash_table_new(wmem_str_hash, g_str_equal);
595 | deregistered_fields = g_ptr_array_new();
596 | deregistered_data = g_ptr_array_new();
597 | deregistered_slice = g_ptr_array_new();
598 | }
599 |
600 | /* initialize data structures and register protocols and fields */
601 | void
602 | proto_init(GSList *register_all_plugin_protocols_list,
603 | GSList *register_all_plugin_handoffs_list,
604 | register_entity_func register_func, register_entity_func handoff_func,
605 | register_cb cb,
606 | void *client_data)
607 | {
608 | /* Initialize the ftype subsystem */
609 | ftypes_initialize();
610 |
611 | /* Initialize the address type subsystem */
612 | address_types_initialize();
613 |
614 | /* Register one special-case FT_TEXT_ONLY field for use when
615 | converting wireshark to new-style proto_tree. These fields
616 | are merely strings on the GUI tree; they are not filterable */
617 | hf_text_only = proto_register_field_init(&hfi_text_only, -1);
618 |
619 | /* Register the pseudo-protocols used for exceptions. */
620 | register_show_exception();
621 | register_type_length_mismatch();
622 | register_byte_array_string_decodinws_error();
623 | register_date_time_string_decodinws_error();
624 | register_string_errors();
625 | ftypes_register_pseudofields();
626 | col_register_protocol();
627 |
628 | /* Have each built-in dissector register its protocols, fields,
629 | dissector tables, and dissectors to be called through a
630 | handle, and do whatever one-time initialization it needs to
631 | do. */
632 | if (register_func != NULL((void*)0))
633 | register_func(cb, client_data);
634 |
635 | /* Now call the registration routines for all epan plugins. */
636 | for (GSList *l = register_all_plugin_protocols_list; l != NULL((void*)0); l = l->next) {
637 | ((void (*)(register_cb, void *))l->data)(cb, client_data);
638 | }
639 |
640 | /* Now call the registration routines for all dissector plugins. */
641 | if (cb)
642 | (*cb)(RA_PLUGIN_REGISTER, NULL((void*)0), client_data);
643 | g_slist_foreach(dissector_plugins, call_plugin_register_protoinfo, NULL((void*)0));
644 |
645 | /* Now call the "handoff registration" routines of all built-in
646 | dissectors; those routines register the dissector in other
647 | dissectors' handoff tables, and fetch any dissector handles
648 | they need. */
649 | if (handoff_func != NULL((void*)0))
650 | handoff_func(cb, client_data);
651 |
652 | /* Now do the same with epan plugins. */
653 | for (GSList *l = register_all_plugin_handoffs_list; l != NULL((void*)0); l = l->next) {
654 | ((void (*)(register_cb, void *))l->data)(cb, client_data);
655 | }
656 |
657 | /* Now do the same with dissector plugins. */
658 | if (cb)
659 | (*cb)(RA_PLUGIN_HANDOFF, NULL((void*)0), client_data);
660 | g_slist_foreach(dissector_plugins, call_plugin_register_handoff, NULL((void*)0));
661 |
662 | /* sort the protocols by protocol name */
663 | protocols = g_list_sort(protocols, proto_compare_name);
664 |
665 | /* sort the dissector handles in dissector tables (for -G reports
666 | * and -d error messages. The GUI sorts the handles itself.) */
667 | packet_all_tables_sort_handles();
668 |
669 | /* We've assigned all the subtree type values; allocate the array
670 | for them, and zero it out. */
671 | tree_is_expanded = g_new0(uint32_t, (num_tree_types/32)+1)((uint32_t *) g_malloc0_n (((num_tree_types/32)+1), sizeof (uint32_t )));
672 | }
673 |
674 | static void
675 | proto_cleanup_base(void)
676 | {
677 | protocol_t *protocol;
678 | header_field_info *hfinfo;
679 |
680 | /* Free the abbrev/ID hash table */
681 | if (gpa_name_map) {
682 | // XXX - We don't have a wmem_map_destroy, but
683 | // it does get cleaned up when epan scope is
684 | // destroyed
685 | //g_hash_table_destroy(gpa_name_map);
686 | gpa_name_map = NULL((void*)0);
687 | }
688 | if (gpa_protocol_aliases) {
689 | g_hash_table_destroy(gpa_protocol_aliases);
690 | gpa_protocol_aliases = NULL((void*)0);
691 | }
692 | g_free(last_field_name);
693 | last_field_name = NULL((void*)0);
694 |
695 | while (protocols) {
696 | protocol = (protocol_t *)protocols->data;
697 | PROTO_REGISTRAR_GET_NTH(protocol->proto_id, hfinfo)if((protocol->proto_id == 0 || (unsigned)protocol->proto_id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 697 , __func__, "Unregistered hf! index=%d", protocol->proto_id ); ((void) ((protocol->proto_id > 0 && (unsigned )protocol->proto_id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 697, "protocol->proto_id > 0 && (unsigned)protocol->proto_id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[protocol-> proto_id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 697, "gpa_hfinfo.hfi[protocol->proto_id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[protocol-> proto_id];;
698 | DISSECTOR_ASSERT(protocol->proto_id == hfinfo->id)((void) ((protocol->proto_id == hfinfo->id) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 698, "protocol->proto_id == hfinfo->id" ))));
699 |
700 | g_slice_free(header_field_info, hfinfo)do { if (1) g_slice_free1 (sizeof (header_field_info), (hfinfo )); else (void) ((header_field_info*) 0 == (hfinfo)); } while (0);
701 | if (protocol->parent_proto_id != -1) {
702 | // pino protocol
703 | DISSECTOR_ASSERT(protocol->fields == NULL)((void) ((protocol->fields == ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 703, "protocol->fields == ((void*)0)" )))); //helpers should not have any registered fields
704 | DISSECTOR_ASSERT(protocol->heur_list == NULL)((void) ((protocol->heur_list == ((void*)0)) ? (void)0 : ( proto_report_dissector_bug("%s:%u: failed assertion \"%s\"", "epan/proto.c" , 704, "protocol->heur_list == ((void*)0)")))); //helpers should not have a heuristic list
705 | } else {
706 | if (protocol->fields) {
707 | g_ptr_array_free(protocol->fields, true1);
708 | }
709 | g_list_free(protocol->heur_list);
710 | }
711 | protocols = g_list_remove(protocols, protocol);
712 | g_free(protocol);
713 | }
714 |
715 | if (proto_names) {
716 | g_hash_table_destroy(proto_names);
717 | proto_names = NULL((void*)0);
718 | }
719 |
720 | if (proto_short_names) {
721 | g_hash_table_destroy(proto_short_names);
722 | proto_short_names = NULL((void*)0);
723 | }
724 |
725 | if (proto_filter_names) {
726 | g_hash_table_destroy(proto_filter_names);
727 | proto_filter_names = NULL((void*)0);
728 | }
729 |
730 | if (proto_reserved_filter_names) {
731 | g_hash_table_destroy(proto_reserved_filter_names);
732 | proto_reserved_filter_names = NULL((void*)0);
733 | }
734 |
735 | if (gpa_hfinfo.allocated_len) {
736 | gpa_hfinfo.len = 0;
737 | gpa_hfinfo.allocated_len = 0;
738 | g_free(gpa_hfinfo.hfi);
739 | gpa_hfinfo.hfi = NULL((void*)0);
740 | }
741 |
742 | if (deregistered_fields) {
743 | g_ptr_array_free(deregistered_fields, true1);
744 | deregistered_fields = NULL((void*)0);
745 | }
746 |
747 | if (deregistered_data) {
748 | g_ptr_array_free(deregistered_data, true1);
749 | deregistered_data = NULL((void*)0);
750 | }
751 |
752 | if (deregistered_slice) {
753 | g_ptr_array_free(deregistered_slice, true1);
754 | deregistered_slice = NULL((void*)0);
755 | }
756 |
757 | g_free(tree_is_expanded);
758 | tree_is_expanded = NULL((void*)0);
759 |
760 | if (prefixes)
761 | g_hash_table_destroy(prefixes);
762 |
763 | if (saved_dir_queue != NULL((void*)0)) {
764 | g_queue_clear_full(saved_dir_queue, g_free);
765 | g_queue_free(saved_dir_queue);
766 | saved_dir_queue = NULL((void*)0);
767 | }
768 | }
769 |
770 | void
771 | proto_cleanup(void)
772 | {
773 | proto_free_deregistered_fields();
774 | proto_cleanup_base();
775 |
776 | g_slist_free(dissector_plugins);
777 | dissector_plugins = NULL((void*)0);
778 | }
779 |
780 | static bool_Bool
781 | ws_pushd(const char* dir)
782 | {
783 | //Save the current working directory
784 | const char* save_wd = get_current_working_dir();
785 | if (save_wd != NULL((void*)0))
786 | g_queue_push_head(saved_dir_queue, g_strdup(save_wd)g_strdup_inline (save_wd));
787 |
788 | //Change to the new one
789 | #ifdef _WIN32
790 | SetCurrentDirectory(utf_8to16(dir));
791 | return true1;
792 | #else
793 | return (chdir(dir) == 0);
794 | #endif
795 | }
796 |
797 | static bool_Bool
798 | ws_popd(void)
799 | {
800 | int ret = 0;
801 | char* saved_wd = g_queue_pop_head(saved_dir_queue);
802 | if (saved_wd == NULL((void*)0))
803 | return false0;
804 |
805 | //Restore the previous one
806 | #ifdef _WIN32
807 | SetCurrentDirectory(utf_8to16(saved_wd));
808 | #else
809 | ret = chdir(saved_wd);
810 | #endif
811 | g_free(saved_wd);
812 | return (ret == 0);
813 | }
814 |
815 | void
816 | proto_execute_in_directory(const char* dir, proto_execute_in_directory_func func, void* param)
817 | {
818 | if (ws_pushd(dir))
819 | {
820 | func(param);
821 | ws_popd();
822 | }
823 | }
824 |
825 | static bool_Bool
826 | // NOLINTNEXTLINE(misc-no-recursion)
827 | proto_tree_traverse_pre_order(proto_tree *tree, proto_tree_traverse_func func,
828 | void *data)
829 | {
830 | proto_node *pnode = tree;
831 | proto_node *child;
832 | proto_node *current;
833 |
834 | if (func(pnode, data))
835 | return true1;
836 |
837 | child = pnode->first_child;
838 | while (child != NULL((void*)0)) {
839 | /*
840 | * The routine we call might modify the child, e.g. by
841 | * freeing it, so we get the child's successor before
842 | * calling that routine.
843 | */
844 | current = child;
845 | child = current->next;
846 | // We recurse here, but we're limited by prefs.gui_max_tree_depth
847 | if (proto_tree_traverse_pre_order((proto_tree *)current, func, data))
848 | return true1;
849 | }
850 |
851 | return false0;
852 | }
853 |
854 | void
855 | proto_tree_children_foreach(proto_tree *tree, proto_tree_foreach_func func,
856 | void *data)
857 | {
858 | proto_node *node = tree;
859 | proto_node *current;
860 |
861 | if (!node)
862 | return;
863 |
864 | node = node->first_child;
865 | while (node != NULL((void*)0)) {
866 | current = node;
867 | node = current->next;
868 | func((proto_tree *)current, data);
869 | }
870 | }
871 |
872 | static void
873 | free_GPtrArray_value(void *key, void *value, void *user_data _U___attribute__((unused)))
874 | {
875 | GPtrArray *ptrs = (GPtrArray *)value;
876 | int hfid = GPOINTER_TO_UINT(key)((guint) (gulong) (key));
877 | header_field_info *hfinfo;
878 |
879 | PROTO_REGISTRAR_GET_NTH(hfid, hfinfo)if((hfid == 0 || (unsigned)hfid > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 879, __func__, "Unregistered hf! index=%d", hfid); ((void) ((hfid > 0 && (unsigned)hfid < gpa_hfinfo .len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 879, "hfid > 0 && (unsigned)hfid < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfid] != ( (void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 879, "gpa_hfinfo.hfi[hfid] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[hfid];;
880 | if (hfinfo->ref_type != HF_REF_TYPE_NONE) {
881 | /* when a field is referenced by a filter this also
882 | affects the refcount for the parent protocol so we need
883 | to adjust the refcount for the parent as well
884 | */
885 | if (hfinfo->parent != -1) {
886 | header_field_info *parent_hfinfo;
887 | PROTO_REGISTRAR_GET_NTH(hfinfo->parent, parent_hfinfo)if((hfinfo->parent == 0 || (unsigned)hfinfo->parent > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 887 , __func__, "Unregistered hf! index=%d", hfinfo->parent); ( (void) ((hfinfo->parent > 0 && (unsigned)hfinfo ->parent < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 887, "hfinfo->parent > 0 && (unsigned)hfinfo->parent < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> parent] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 887, "gpa_hfinfo.hfi[hfinfo->parent] != ((void*)0)" , "Unregistered hf!")))) ; parent_hfinfo = gpa_hfinfo.hfi[hfinfo ->parent];;
888 | parent_hfinfo->ref_type = HF_REF_TYPE_NONE;
889 | }
890 | hfinfo->ref_type = HF_REF_TYPE_NONE;
891 | }
892 |
893 | g_ptr_array_free(ptrs, true1);
894 | }
895 |
896 | static void
897 | proto_tree_free_node(proto_node *node, void *data _U___attribute__((unused)))
898 | {
899 | field_info *finfo = PNODE_FINFO(node)((node)->finfo);
900 |
901 | proto_tree_children_foreach(node, proto_tree_free_node, NULL((void*)0));
902 |
903 | if (finfo) {
904 | fvalue_free(finfo->value);
905 | finfo->value = NULL((void*)0);
906 | }
907 | }
908 |
909 | void
910 | proto_tree_reset(proto_tree *tree)
911 | {
912 | tree_data_t *tree_data = PTREE_DATA(tree)((tree)->tree_data);
913 |
914 | proto_tree_children_foreach(tree, proto_tree_free_node, NULL((void*)0));
915 |
916 | /* free tree data */
917 | if (tree_data->interesting_hfids) {
918 | /* Free all the GPtrArray's in the interesting_hfids hash. */
919 | g_hash_table_foreach(tree_data->interesting_hfids,
920 | free_GPtrArray_value, NULL((void*)0));
921 |
922 | /* And then remove all values. */
923 | g_hash_table_remove_all(tree_data->interesting_hfids);
924 | }
925 |
926 | /* Reset track of the number of children */
927 | tree_data->count = 0;
928 |
929 | /* Reset our loop checks */
930 | tree_data->idle_count_ds_tvb = NULL((void*)0);
931 | tree_data->max_start = 0;
932 | tree_data->start_idle_count = 0;
933 |
934 | PROTO_NODE_INIT(tree)tree->first_child = ((void*)0); tree->last_child = ((void *)0); tree->next = ((void*)0);;
935 | }
936 |
937 | /* frees the resources that the dissection a proto_tree uses */
938 | void
939 | proto_tree_free(proto_tree *tree)
940 | {
941 | tree_data_t *tree_data = PTREE_DATA(tree)((tree)->tree_data);
942 |
943 | proto_tree_children_foreach(tree, proto_tree_free_node, NULL((void*)0));
944 |
945 | /* free tree data */
946 | if (tree_data->interesting_hfids) {
947 | /* Free all the GPtrArray's in the interesting_hfids hash. */
948 | g_hash_table_foreach(tree_data->interesting_hfids,
949 | free_GPtrArray_value, NULL((void*)0));
950 |
951 | /* And then destroy the hash. */
952 | g_hash_table_destroy(tree_data->interesting_hfids);
953 | }
954 |
955 | g_slice_free(tree_data_t, tree_data)do { if (1) g_slice_free1 (sizeof (tree_data_t), (tree_data)) ; else (void) ((tree_data_t*) 0 == (tree_data)); } while (0);
956 |
957 | g_slice_free(proto_tree, tree)do { if (1) g_slice_free1 (sizeof (proto_tree), (tree)); else (void) ((proto_tree*) 0 == (tree)); } while (0);
958 | }
959 |
960 | /* Is the parsing being done for a visible proto_tree or an invisible one?
961 | * By setting this correctly, the proto_tree creation is sped up by not
962 | * having to call vsnprintf and copy strings around.
963 | */
964 | bool_Bool
965 | proto_tree_set_visible(proto_tree *tree, bool_Bool visible)
966 | {
967 | bool_Bool old_visible = PTREE_DATA(tree)((tree)->tree_data)->visible;
968 |
969 | PTREE_DATA(tree)((tree)->tree_data)->visible = visible;
970 |
971 | return old_visible;
972 | }
973 |
974 | void
975 | proto_tree_set_fake_protocols(proto_tree *tree, bool_Bool fake_protocols)
976 | {
977 | if (tree)
978 | PTREE_DATA(tree)((tree)->tree_data)->fake_protocols = fake_protocols;
979 | }
980 |
981 | /* Assume dissector set only its protocol fields.
982 | This function is called by dissectors and allows the speeding up of filtering
983 | in wireshark; if this function returns false it is safe to reset tree to NULL
984 | and thus skip calling most of the expensive proto_tree_add_...()
985 | functions.
986 | If the tree is visible we implicitly assume the field is referenced.
987 | */
988 | bool_Bool
989 | proto_field_is_referenced(proto_tree *tree, int proto_id)
990 | {
991 | register header_field_info *hfinfo;
992 |
993 |
994 | if (!tree)
995 | return false0;
996 |
997 | if (PTREE_DATA(tree)((tree)->tree_data)->visible)
998 | return true1;
999 |
1000 | PROTO_REGISTRAR_GET_NTH(proto_id, hfinfo)if((proto_id == 0 || (unsigned)proto_id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 1000, __func__, "Unregistered hf! index=%d" , proto_id); ((void) ((proto_id > 0 && (unsigned)proto_id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 1000, "proto_id > 0 && (unsigned)proto_id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[proto_id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 1000, "gpa_hfinfo.hfi[proto_id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[proto_id];;
1001 | if (hfinfo->ref_type != HF_REF_TYPE_NONE)
1002 | return true1;
1003 |
1004 | if (hfinfo->type == FT_PROTOCOL && !PTREE_DATA(tree)((tree)->tree_data)->fake_protocols)
1005 | return true1;
1006 |
1007 | return false0;
1008 | }
1009 |
1010 |
1011 | /* Finds a record in the hfinfo array by id. */
1012 | header_field_info *
1013 | proto_registrar_get_nth(unsigned hfindex)
1014 | {
1015 | register header_field_info *hfinfo;
1016 |
1017 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 1017, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 1017, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 1017, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
1018 | return hfinfo;
1019 | }
1020 |
1021 |
1022 | /* Prefix initialization
1023 | * this allows for a dissector to register a display filter name prefix
1024 | * so that it can delay the initialization of the hf array as long as
1025 | * possible.
1026 | */
1027 |
1028 | /* compute a hash for the part before the dot of a display filter */
1029 | static unsigned
1030 | prefix_hash (const void *key) {
1031 | /* end the string at the dot and compute its hash */
1032 | char* copy = g_strdup((const char *)key)g_strdup_inline ((const char *)key);
1033 | char* c = copy;
1034 | unsigned tmp;
1035 |
1036 | for (; *c; c++) {
1037 | if (*c == '.') {
1038 | *c = 0;
1039 | break;
1040 | }
1041 | }
1042 |
1043 | tmp = wmem_str_hash(copy);
1044 | g_free(copy);
1045 | return tmp;
1046 | }
1047 |
1048 | /* are both strings equal up to the end or the dot? */
1049 | static gboolean
1050 | prefix_equal (const void *ap, const void *bp) {
1051 | const char* a = (const char *)ap;
1052 | const char* b = (const char *)bp;
1053 |
1054 | do {
1055 | char ac = *a++;
1056 | char bc = *b++;
1057 |
1058 | if ( (ac == '.' || ac == '\0') && (bc == '.' || bc == '\0') ) return TRUE(!(0));
1059 |
1060 | if ( (ac == '.' || ac == '\0') && ! (bc == '.' || bc == '\0') ) return FALSE(0);
1061 | if ( (bc == '.' || bc == '\0') && ! (ac == '.' || ac == '\0') ) return FALSE(0);
1062 |
1063 | if (ac != bc) return FALSE(0);
1064 | } while (1);
1065 |
1066 | return FALSE(0);
1067 | }
1068 |
1069 | /* Register a new prefix for "delayed" initialization of field arrays */
1070 | void
1071 | proto_register_prefix(const char *prefix, prefix_initializer_t pi ) {
1072 | if (! prefixes ) {
1073 | prefixes = g_hash_table_new(prefix_hash, prefix_equal);
1074 | }
1075 |
1076 | g_hash_table_insert(prefixes, (void *)prefix, (void *)pi);
1077 | }
1078 |
1079 | /* helper to call all prefix initializers */
1080 | static gboolean
1081 | initialize_prefix(void *k, void *v, void *u _U___attribute__((unused))) {
1082 | ((prefix_initializer_t)v)((const char *)k);
1083 | return TRUE(!(0));
1084 | }
1085 |
1086 | /** Initialize every remaining uninitialized prefix. */
1087 | void
1088 | proto_initialize_all_prefixes(void) {
1089 | g_hash_table_foreach_remove(prefixes, initialize_prefix, NULL((void*)0));
1090 | }
1091 |
1092 | /* Finds a record in the hfinfo array by name.
1093 | * If it fails to find it in the already registered fields,
1094 | * it tries to find and call an initializer in the prefixes
1095 | * table and if so it looks again.
1096 | */
1097 |
1098 | header_field_info *
1099 | proto_registrar_get_byname(const char *field_name)
1100 | {
1101 | header_field_info *hfinfo;
1102 | prefix_initializer_t pi;
1103 |
1104 | if (!field_name)
1105 | return NULL((void*)0);
1106 |
1107 | if (g_strcmp0(field_name, last_field_name) == 0) {
1108 | return last_hfinfo;
1109 | }
1110 |
1111 | hfinfo = (header_field_info *)wmem_map_lookup(gpa_name_map, field_name);
1112 |
1113 | if (hfinfo) {
1114 | g_free(last_field_name);
1115 | last_field_name = g_strdup(field_name)g_strdup_inline (field_name);
1116 | last_hfinfo = hfinfo;
1117 | return hfinfo;
1118 | }
1119 |
1120 | if (!prefixes)
1121 | return NULL((void*)0);
1122 |
1123 | if ((pi = (prefix_initializer_t)g_hash_table_lookup(prefixes, field_name) ) != NULL((void*)0)) {
1124 | pi(field_name);
1125 | g_hash_table_remove(prefixes, field_name);
1126 | } else {
1127 | return NULL((void*)0);
1128 | }
1129 |
1130 | hfinfo = (header_field_info *)wmem_map_lookup(gpa_name_map, field_name);
1131 |
1132 | if (hfinfo) {
1133 | g_free(last_field_name);
1134 | last_field_name = g_strdup(field_name)g_strdup_inline (field_name);
1135 | last_hfinfo = hfinfo;
1136 | }
1137 | return hfinfo;
1138 | }
1139 |
1140 | header_field_info*
1141 | proto_registrar_get_byalias(const char *alias_name)
1142 | {
1143 | if (!alias_name) {
1144 | return NULL((void*)0);
1145 | }
1146 |
1147 | /* Find our aliased protocol. */
1148 | char *an_copy = g_strdup(alias_name)g_strdup_inline (alias_name);
1149 | char *dot = strchr(an_copy, '.');
1150 | if (dot) {
1151 | *dot = '\0';
1152 | }
1153 | const char *proto_pfx = (const char *) g_hash_table_lookup(gpa_protocol_aliases, an_copy);
1154 | if (!proto_pfx) {
1155 | g_free(an_copy);
1156 | return NULL((void*)0);
1157 | }
1158 |
1159 | /* Construct our aliased field and look it up. */
1160 | GString *filter_name = g_string_new(proto_pfx);
1161 | if (dot) {
1162 | g_string_append_printf(filter_name, ".%s", dot+1);
1163 | }
1164 | header_field_info *hfinfo = proto_registrar_get_byname(filter_name->str);
1165 | g_free(an_copy);
1166 | g_string_free(filter_name, TRUE)(__builtin_constant_p ((!(0))) ? (((!(0))) ? (g_string_free) ( (filter_name), ((!(0)))) : g_string_free_and_steal (filter_name )) : (g_string_free) ((filter_name), ((!(0)))));
1167 |
1168 | return hfinfo;
1169 | }
1170 |
1171 | int
1172 | proto_registrar_get_id_byname(const char *field_name)
1173 | {
1174 | header_field_info *hfinfo;
1175 |
1176 | hfinfo = proto_registrar_get_byname(field_name);
1177 |
1178 | if (!hfinfo)
1179 | return -1;
1180 |
1181 | return hfinfo->id;
1182 | }
1183 |
1184 | static int
1185 | label_strcat_flags(const header_field_info *hfinfo)
1186 | {
1187 | if (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF) & BASE_STR_WSP)
1188 | return FORMAT_LABEL_REPLACE_SPACE(0x1 << 0);
1189 |
1190 | return 0;
1191 | }
1192 |
1193 | static char *
1194 | format_bytes_hfinfo_maxlen(wmem_allocator_t *scope, const header_field_info *hfinfo,
1195 | const uint8_t *bytes, unsigned length, size_t max_str_len)
1196 | {
1197 | char *str = NULL((void*)0);
1198 | const uint8_t *p;
1199 | bool_Bool is_printable;
1200 |
1201 | if (bytes) {
1202 | if (hfinfo->display & BASE_SHOW_UTF_8_PRINTABLE0x00020000) {
1203 | /*
1204 | * If all bytes are valid and printable UTF-8, show the
1205 | * bytes as a string - in quotes to indicate that it's
1206 | * a string.
1207 | */
1208 | if (isprint_utf8_string((const char*)bytes, length)) {
1209 | str = wmem_strdup_printf(scope, "\"%.*s\"",
1210 | (int)length, bytes);
1211 | return str;
1212 | }
1213 | } else if (hfinfo->display & BASE_SHOW_ASCII_PRINTABLE0x00010000) {
1214 | /*
1215 | * Check whether all bytes are printable.
1216 | */
1217 | is_printable = true1;
1218 | for (p = bytes; p < bytes+length; p++) {
1219 | if (!g_ascii_isprint(*p)((g_ascii_table[(guchar) (*p)] & G_ASCII_PRINT) != 0)) {
1220 | /* Not printable. */
1221 | is_printable = false0;
1222 | break;
1223 | }
1224 | }
1225 |
1226 | /*
1227 | * If all bytes are printable ASCII, show the bytes
1228 | * as a string - in quotes to indicate that it's
1229 | * a string.
1230 | */
1231 | if (is_printable) {
1232 | str = wmem_strdup_printf(scope, "\"%.*s\"",
1233 | (int)length, bytes);
1234 | return str;
1235 | }
1236 | }
1237 |
1238 | /*
1239 | * Either it's not printable ASCII, or we don't care whether
1240 | * it's printable ASCII; show it as hex bytes.
1241 | */
1242 | switch (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF)) {
1243 | case SEP_DOT:
1244 | str = bytes_to_str_punct_maxlen(scope, bytes, length, '.', max_str_len/3);
1245 | break;
1246 | case SEP_DASH:
1247 | str = bytes_to_str_punct_maxlen(scope, bytes, length, '-', max_str_len/3);
1248 | break;
1249 | case SEP_COLON:
1250 | str = bytes_to_str_punct_maxlen(scope, bytes, length, ':', max_str_len/3);
1251 | break;
1252 | case SEP_SPACE:
1253 | str = bytes_to_str_punct_maxlen(scope, bytes, length, ' ', max_str_len/3);
1254 | break;
1255 | case BASE_NONE:
1256 | default:
1257 | if (prefs.display_byte_fields_with_spaces) {
1258 | str = bytes_to_str_punct_maxlen(scope, bytes, length, ' ', max_str_len/3);
1259 | } else {
1260 | str = bytes_to_str_maxlen(scope, bytes, length, max_str_len/2);
1261 | }
1262 | break;
1263 | }
1264 | }
1265 | else {
1266 | if (hfinfo->display & BASE_ALLOW_ZERO0x00000800) {
1267 | str = wmem_strdup(scope, "<none>");
1268 | } else {
1269 | str = wmem_strdup(scope, "<MISSING>");
1270 | }
1271 | }
1272 | return str;
1273 | }
1274 |
1275 | static char *
1276 | format_bytes_hfinfo(wmem_allocator_t *scope, const header_field_info *hfinfo,
1277 | const uint8_t *bytes, unsigned length)
1278 | {
1279 | return format_bytes_hfinfo_maxlen(scope, hfinfo, bytes, length, ITEM_LABEL_LENGTH240);
1280 | }
1281 |
1282 | static void
1283 | ptvcursor_new_subtree_levels(ptvcursor_t *ptvc)
1284 | {
1285 | subtree_lvl *pushed_tree;
1286 |
1287 | DISSECTOR_ASSERT(ptvc->pushed_tree_max <= SUBTREE_MAX_LEVELS-SUBTREE_ONCE_ALLOCATION_NUMBER)((void) ((ptvc->pushed_tree_max <= 256 -8) ? (void)0 : ( proto_report_dissector_bug("%s:%u: failed assertion \"%s\"", "epan/proto.c" , 1287, "ptvc->pushed_tree_max <= 256-8"))));
1288 | ptvc->pushed_tree_max += SUBTREE_ONCE_ALLOCATION_NUMBER8;
1289 |
1290 | pushed_tree = (subtree_lvl *)wmem_realloc(ptvc->scope, (void *)ptvc->pushed_tree, sizeof(subtree_lvl) * ptvc->pushed_tree_max);
1291 | DISSECTOR_ASSERT(pushed_tree != NULL)((void) ((pushed_tree != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 1291, "pushed_tree != ((void*)0)" ))));
1292 | ptvc->pushed_tree = pushed_tree;
1293 | }
1294 |
1295 | static void
1296 | ptvcursor_free_subtree_levels(ptvcursor_t *ptvc)
1297 | {
1298 | ptvc->pushed_tree = NULL((void*)0);
1299 | ptvc->pushed_tree_max = 0;
1300 | DISSECTOR_ASSERT(ptvc->pushed_tree_index == 0)((void) ((ptvc->pushed_tree_index == 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 1300, "ptvc->pushed_tree_index == 0" ))));
1301 | ptvc->pushed_tree_index = 0;
1302 | }
1303 |
1304 | /* Allocates an initializes a ptvcursor_t with 3 variables:
1305 | * proto_tree, tvbuff, and offset. */
1306 | ptvcursor_t *
1307 | ptvcursor_new(wmem_allocator_t *scope, proto_tree *tree, tvbuff_t *tvb, int offset)
1308 | {
1309 | ptvcursor_t *ptvc;
1310 |
1311 | ptvc = wmem_new(scope, ptvcursor_t)((ptvcursor_t*)wmem_alloc((scope), sizeof(ptvcursor_t)));
1312 | ptvc->scope = scope;
1313 | ptvc->tree = tree;
1314 | ptvc->tvb = tvb;
1315 | ptvc->offset = offset;
1316 | ptvc->pushed_tree = NULL((void*)0);
1317 | ptvc->pushed_tree_max = 0;
1318 | ptvc->pushed_tree_index = 0;
1319 | return ptvc;
1320 | }
1321 |
1322 |
1323 | /* Frees memory for ptvcursor_t, but nothing deeper than that. */
1324 | void
1325 | ptvcursor_free(ptvcursor_t *ptvc)
1326 | {
1327 | ptvcursor_free_subtree_levels(ptvc);
1328 | /*g_free(ptvc);*/
1329 | }
1330 |
1331 | /* Returns tvbuff. */
1332 | tvbuff_t *
1333 | ptvcursor_tvbuff(ptvcursor_t *ptvc)
1334 | {
1335 | return ptvc->tvb;
1336 | }
1337 |
1338 | /* Returns current offset. */
1339 | int
1340 | ptvcursor_current_offset(ptvcursor_t *ptvc)
1341 | {
1342 | return ptvc->offset;
1343 | }
1344 |
1345 | proto_tree *
1346 | ptvcursor_tree(ptvcursor_t *ptvc)
1347 | {
1348 | if (!ptvc)
1349 | return NULL((void*)0);
1350 |
1351 | return ptvc->tree;
1352 | }
1353 |
1354 | void
1355 | ptvcursor_set_tree(ptvcursor_t *ptvc, proto_tree *tree)
1356 | {
1357 | ptvc->tree = tree;
1358 | }
1359 |
1360 | /* creates a subtree, sets it as the working tree and pushes the old working tree */
1361 | proto_tree *
1362 | ptvcursor_push_subtree(ptvcursor_t *ptvc, proto_item *it, int ett_subtree)
1363 | {
1364 | subtree_lvl *subtree;
1365 | if (ptvc->pushed_tree_index >= ptvc->pushed_tree_max)
1366 | ptvcursor_new_subtree_levels(ptvc);
1367 |
1368 | subtree = ptvc->pushed_tree + ptvc->pushed_tree_index;
1369 | subtree->tree = ptvc->tree;
1370 | subtree->it= NULL((void*)0);
1371 | ptvc->pushed_tree_index++;
1372 | return ptvcursor_set_subtree(ptvc, it, ett_subtree);
1373 | }
1374 |
1375 | /* pops a subtree */
1376 | void
1377 | ptvcursor_pop_subtree(ptvcursor_t *ptvc)
1378 | {
1379 | subtree_lvl *subtree;
1380 |
1381 | if (ptvc->pushed_tree_index <= 0)
1382 | return;
1383 |
1384 | ptvc->pushed_tree_index--;
1385 | subtree = ptvc->pushed_tree + ptvc->pushed_tree_index;
1386 | if (subtree->it != NULL((void*)0))
1387 | proto_item_set_len(subtree->it, ptvcursor_current_offset(ptvc) - subtree->cursor_offset);
1388 |
1389 | ptvc->tree = subtree->tree;
1390 | }
1391 |
1392 | /* saves the current tvb offset and the item in the current subtree level */
1393 | static void
1394 | ptvcursor_subtree_set_item(ptvcursor_t *ptvc, proto_item *it)
1395 | {
1396 | subtree_lvl *subtree;
1397 |
1398 | DISSECTOR_ASSERT(ptvc->pushed_tree_index > 0)((void) ((ptvc->pushed_tree_index > 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 1398, "ptvc->pushed_tree_index > 0" ))));
1399 |
1400 | subtree = ptvc->pushed_tree + ptvc->pushed_tree_index - 1;
1401 | subtree->it = it;
1402 | subtree->cursor_offset = ptvcursor_current_offset(ptvc);
1403 | }
1404 |
1405 | /* Creates a subtree and adds it to the cursor as the working tree but does not
1406 | * save the old working tree */
1407 | proto_tree *
1408 | ptvcursor_set_subtree(ptvcursor_t *ptvc, proto_item *it, int ett_subtree)
1409 | {
1410 | ptvc->tree = proto_item_add_subtree(it, ett_subtree);
1411 | return ptvc->tree;
1412 | }
1413 |
1414 | static proto_tree *
1415 | ptvcursor_add_subtree_item(ptvcursor_t *ptvc, proto_item *it, int ett_subtree, int length)
1416 | {
1417 | ptvcursor_push_subtree(ptvc, it, ett_subtree);
1418 | if (length == SUBTREE_UNDEFINED_LENGTH-1)
1419 | ptvcursor_subtree_set_item(ptvc, it);
1420 | return ptvcursor_tree(ptvc);
1421 | }
1422 |
1423 | /* Add an item to the tree and create a subtree
1424 | * If the length is unknown, length may be defined as SUBTREE_UNDEFINED_LENGTH.
1425 | * In this case, when the subtree will be closed, the parent item length will
1426 | * be equal to the advancement of the cursor since the creation of the subtree.
1427 | */
1428 | proto_tree *
1429 | ptvcursor_add_with_subtree(ptvcursor_t *ptvc, int hfindex, int length,
1430 | const unsigned encoding, int ett_subtree)
1431 | {
1432 | proto_item *it;
1433 |
1434 | it = ptvcursor_add_no_advance(ptvc, hfindex, length, encoding);
1435 | return ptvcursor_add_subtree_item(ptvc, it, ett_subtree, length);
1436 | }
1437 |
1438 | static proto_item *
1439 | proto_tree_add_text_node(proto_tree *tree, tvbuff_t *tvb, int start, int length);
1440 |
1441 | /* Add a text node to the tree and create a subtree
1442 | * If the length is unknown, length may be defined as SUBTREE_UNDEFINED_LENGTH.
1443 | * In this case, when the subtree will be closed, the item length will be equal
1444 | * to the advancement of the cursor since the creation of the subtree.
1445 | */
1446 | proto_tree *
1447 | ptvcursor_add_text_with_subtree(ptvcursor_t *ptvc, int length,
1448 | int ett_subtree, const char *format, ...)
1449 | {
1450 | proto_item *pi;
1451 | va_list ap;
1452 | header_field_info *hfinfo;
1453 | proto_tree *tree;
1454 |
1455 | tree = ptvcursor_tree(ptvc);
1456 |
1457 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
1458 |
1459 | TRY_TO_FAKE_THIS_ITEM(tree, hf_text_only, hfinfo)((tree)->tree_data)->count++; if((hf_text_only == 0 || ( unsigned)hf_text_only > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 1459 , __func__, "Unregistered hf! index=%d", hf_text_only); ((void ) ((hf_text_only > 0 && (unsigned)hf_text_only < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 1459, "hf_text_only > 0 && (unsigned)hf_text_only < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hf_text_only ] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 1459, "gpa_hfinfo.hfi[hf_text_only] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hf_text_only ];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 1459, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
1460 |
1461 | pi = proto_tree_add_text_node(tree, ptvcursor_tvbuff(ptvc),
1462 | ptvcursor_current_offset(ptvc), length);
1463 |
1464 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 1464, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
1465 |
1466 | va_start(ap, format)__builtin_va_start(ap, format);
1467 | proto_tree_set_representation(pi, format, ap);
1468 | va_end(ap)__builtin_va_end(ap);
1469 |
1470 | return ptvcursor_add_subtree_item(ptvc, pi, ett_subtree, length);
1471 | }
1472 |
1473 | /* Add a text-only node, leaving it to our caller to fill the text in */
1474 | static proto_item *
1475 | proto_tree_add_text_node(proto_tree *tree, tvbuff_t *tvb, int start, int length)
1476 | {
1477 | proto_item *pi;
1478 |
1479 | if (tree == NULL((void*)0))
1480 | return NULL((void*)0);
1481 |
1482 | pi = proto_tree_add_pi(tree, &hfi_text_only, tvb, start, &length);
1483 |
1484 | return pi;
1485 | }
1486 |
1487 | /* (INTERNAL USE ONLY) Add a text-only node to the proto_tree */
1488 | proto_item *
1489 | proto_tree_add_text_internal(proto_tree *tree, tvbuff_t *tvb, int start, int length,
1490 | const char *format, ...)
1491 | {
1492 | proto_item *pi;
1493 | va_list ap;
1494 | header_field_info *hfinfo;
1495 |
1496 | if (length == -1) {
1497 | length = tvb_captured_length(tvb) ? tvb_ensure_captured_length_remaining(tvb, start) : 0;
1498 | } else {
1499 | tvb_ensure_bytes_exist(tvb, start, length);
1500 | }
1501 |
1502 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
1503 |
1504 | TRY_TO_FAKE_THIS_ITEM(tree, hf_text_only, hfinfo)((tree)->tree_data)->count++; if((hf_text_only == 0 || ( unsigned)hf_text_only > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 1504 , __func__, "Unregistered hf! index=%d", hf_text_only); ((void ) ((hf_text_only > 0 && (unsigned)hf_text_only < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 1504, "hf_text_only > 0 && (unsigned)hf_text_only < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hf_text_only ] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 1504, "gpa_hfinfo.hfi[hf_text_only] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hf_text_only ];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 1504, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
1505 |
1506 | pi = proto_tree_add_text_node(tree, tvb, start, length);
1507 |
1508 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 1508, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
1509 |
1510 | va_start(ap, format)__builtin_va_start(ap, format);
1511 | proto_tree_set_representation(pi, format, ap);
1512 | va_end(ap)__builtin_va_end(ap);
1513 |
1514 | return pi;
1515 | }
1516 |
1517 | /* (INTERNAL USE ONLY) Add a text-only node to the proto_tree (va_list version) */
1518 | proto_item *
1519 | proto_tree_add_text_valist_internal(proto_tree *tree, tvbuff_t *tvb, int start,
1520 | int length, const char *format, va_list ap)
1521 | {
1522 | proto_item *pi;
1523 | header_field_info *hfinfo;
1524 |
1525 | /* proto_tree_add_text_node calls proto_tree_add_pi() with the
1526 | * FT_NONE hf_text_only, which calls get_hfi_length, which adjusts
1527 | * the length to be what's in the tvbuff if length is -1, and the
1528 | * minimum of length and what's in the tvbuff if not.
1529 | */
1530 |
1531 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
1532 |
1533 | TRY_TO_FAKE_THIS_ITEM(tree, hf_text_only, hfinfo)((tree)->tree_data)->count++; if((hf_text_only == 0 || ( unsigned)hf_text_only > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 1533 , __func__, "Unregistered hf! index=%d", hf_text_only); ((void ) ((hf_text_only > 0 && (unsigned)hf_text_only < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 1533, "hf_text_only > 0 && (unsigned)hf_text_only < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hf_text_only ] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 1533, "gpa_hfinfo.hfi[hf_text_only] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hf_text_only ];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 1533, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
1534 |
1535 | pi = proto_tree_add_text_node(tree, tvb, start, length);
1536 |
1537 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 1537, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
1538 |
1539 | proto_tree_set_representation(pi, format, ap);
1540 |
1541 | return pi;
1542 | }
1543 |
1544 | /* Add a text-only node that creates a subtree underneath.
1545 | */
1546 | proto_tree *
1547 | proto_tree_add_subtree(proto_tree *tree, tvbuff_t *tvb, int start, int length, int idx, proto_item **tree_item, const char *text)
1548 | {
1549 | return proto_tree_add_subtree_format(tree, tvb, start, length, idx, tree_item, "%s", text);
1550 | }
1551 |
1552 | /* Add a text-only node that creates a subtree underneath.
1553 | */
1554 | proto_tree *
1555 | proto_tree_add_subtree_format(proto_tree *tree, tvbuff_t *tvb, int start, int length, int idx, proto_item **tree_item, const char *format, ...)
1556 | {
1557 | proto_tree *pt;
1558 | proto_item *pi;
1559 | va_list ap;
1560 |
1561 | va_start(ap, format)__builtin_va_start(ap, format);
1562 | pi = proto_tree_add_text_valist_internal(tree, tvb, start, length, format, ap);
1563 | va_end(ap)__builtin_va_end(ap);
1564 |
1565 | if (tree_item != NULL((void*)0))
1566 | *tree_item = pi;
1567 |
1568 | pt = proto_item_add_subtree(pi, idx);
1569 |
1570 | return pt;
1571 | }
1572 |
1573 | /* Add a text-only node for debugging purposes. The caller doesn't need
1574 | * to worry about tvbuff, start, or length. Debug message gets sent to
1575 | * STDOUT, too */
1576 | proto_item *
1577 | proto_tree_add_debug_text(proto_tree *tree, const char *format, ...)
1578 | {
1579 | proto_item *pi;
1580 | va_list ap;
1581 |
1582 | pi = proto_tree_add_text_node(tree, NULL((void*)0), 0, 0);
1583 |
1584 | if (pi) {
1585 | va_start(ap, format)__builtin_va_start(ap, format);
1586 | proto_tree_set_representation(pi, format, ap);
1587 | va_end(ap)__builtin_va_end(ap);
1588 | }
1589 | va_start(ap, format)__builtin_va_start(ap, format);
1590 | vprintf(format, ap);
1591 | va_end(ap)__builtin_va_end(ap);
1592 | printf("\n");
1593 |
1594 | return pi;
1595 | }
1596 |
1597 | proto_item *
1598 | proto_tree_add_format_text(proto_tree *tree, tvbuff_t *tvb, int start, int length)
1599 | {
1600 | proto_item *pi;
1601 | header_field_info *hfinfo;
1602 |
1603 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
1604 |
1605 | TRY_TO_FAKE_THIS_ITEM(tree, hf_text_only, hfinfo)((tree)->tree_data)->count++; if((hf_text_only == 0 || ( unsigned)hf_text_only > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 1605 , __func__, "Unregistered hf! index=%d", hf_text_only); ((void ) ((hf_text_only > 0 && (unsigned)hf_text_only < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 1605, "hf_text_only > 0 && (unsigned)hf_text_only < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hf_text_only ] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 1605, "gpa_hfinfo.hfi[hf_text_only] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hf_text_only ];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 1605, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
1606 |
1607 | pi = proto_tree_add_text_node(tree, tvb, start, length);
1608 |
1609 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 1609, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
1610 |
1611 | proto_item_set_text(pi, "%s", tvb_format_text(tree->tree_data->pinfo->pool, tvb, start, length));
1612 |
1613 | return pi;
1614 | }
1615 |
1616 | proto_item *
1617 | proto_tree_add_format_wsp_text(proto_tree *tree, tvbuff_t *tvb, int start, int length)
1618 | {
1619 | proto_item *pi;
1620 | header_field_info *hfinfo;
1621 | char *str;
1622 |
1623 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
1624 |
1625 | TRY_TO_FAKE_THIS_ITEM(tree, hf_text_only, hfinfo)((tree)->tree_data)->count++; if((hf_text_only == 0 || ( unsigned)hf_text_only > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 1625 , __func__, "Unregistered hf! index=%d", hf_text_only); ((void ) ((hf_text_only > 0 && (unsigned)hf_text_only < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 1625, "hf_text_only > 0 && (unsigned)hf_text_only < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hf_text_only ] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 1625, "gpa_hfinfo.hfi[hf_text_only] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hf_text_only ];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 1625, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
1626 |
1627 | pi = proto_tree_add_text_node(tree, tvb, start, length);
1628 |
1629 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 1629, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
1630 |
1631 | str = tvb_format_text_wsp(NULL((void*)0), tvb, start, length);
1632 | proto_item_set_text(pi, "%s", str);
1633 | wmem_free(NULL((void*)0), str);
1634 |
1635 | return pi;
1636 | }
1637 |
1638 | void proto_report_dissector_bug(const char *format, ...)
1639 | {
1640 | va_list args;
1641 |
1642 | if (wireshark_abort_on_dissector_bug) {
1643 | /*
1644 | * Try to have the error message show up in the crash
1645 | * information.
1646 | */
1647 | va_start(args, format)__builtin_va_start(args, format);
1648 | ws_vadd_crash_info(format, args);
1649 | va_end(args)__builtin_va_end(args);
1650 |
1651 | /*
1652 | * Print the error message.
1653 | */
1654 | va_start(args, format)__builtin_va_start(args, format);
1655 | vfprintf(stderrstderr, format, args);
1656 | va_end(args)__builtin_va_end(args);
1657 | putc('\n', stderrstderr);
1658 |
1659 | /*
1660 | * And crash.
1661 | */
1662 | abort();
1663 | } else {
1664 | va_start(args, format)__builtin_va_start(args, format);
1665 | VTHROW_FORMATTED(DissectorError, format, args)except_vthrowf(1, (6), format, args);
1666 | va_end(args)__builtin_va_end(args);
1667 | ws_assert_not_reached()ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 1667 , __func__, "assertion \"not reached\" failed"); /* GCC 12 with ASAN needs this. */
1668 | }
1669 | }
1670 |
1671 | /* We could probably get away with changing is_error to a minimum length value. */
1672 | static void
1673 | report_type_length_mismatch(proto_tree *tree, const char *descr, int length, bool_Bool is_error)
1674 | {
1675 | if (is_error) {
1676 | expert_add_info_format(NULL((void*)0), tree, &ei_type_length_mismatch_error, "Trying to fetch %s with length %d", descr, length);
1677 | } else {
1678 | expert_add_info_format(NULL((void*)0), tree, &ei_type_length_mismatch_warn, "Trying to fetch %s with length %d", descr, length);
1679 | }
1680 |
1681 | if (is_error) {
1682 | THROW(ReportedBoundsError)except_throw(1, (3), ((void*)0));
1683 | }
1684 | }
1685 |
1686 | static uint32_t
1687 | get_uint_value(proto_tree *tree, tvbuff_t *tvb, int offset, int length, const unsigned encoding)
1688 | {
1689 | uint32_t value;
1690 | bool_Bool length_error;
1691 |
1692 | switch (length) {
1693 |
1694 | case 1:
1695 | value = tvb_get_uint8(tvb, offset);
1696 | if (encoding & ENC_ZIGBEE0x40000000) {
1697 | if (value == 0xFF) { /* Invalid Zigbee length, set to 0 */
1698 | value = 0;
1699 | }
1700 | }
1701 | break;
1702 |
1703 | case 2:
1704 | value = (encoding & ENC_LITTLE_ENDIAN0x80000000) ? tvb_get_letohs(tvb, offset)
1705 | : tvb_get_ntohs(tvb, offset);
1706 | if (encoding & ENC_ZIGBEE0x40000000) {
1707 | if (value == 0xFFFF) { /* Invalid Zigbee length, set to 0 */
1708 | value = 0;
1709 | }
1710 | }
1711 | break;
1712 |
1713 | case 3:
1714 | value = (encoding & ENC_LITTLE_ENDIAN0x80000000) ? tvb_get_letoh24(tvb, offset)
1715 | : tvb_get_ntoh24(tvb, offset);
1716 | break;
1717 |
1718 | case 4:
1719 | value = (encoding & ENC_LITTLE_ENDIAN0x80000000) ? tvb_get_letohl(tvb, offset)
1720 | : tvb_get_ntohl(tvb, offset);
1721 | break;
1722 |
1723 | default:
1724 | if (length < 1) {
1725 | length_error = true1;
1726 | value = 0;
1727 | } else {
1728 | length_error = false0;
1729 | value = (encoding & ENC_LITTLE_ENDIAN0x80000000) ? tvb_get_letohl(tvb, offset)
1730 | : tvb_get_ntohl(tvb, offset);
1731 | }
1732 | report_type_length_mismatch(tree, "an unsigned integer", length, length_error);
1733 | break;
1734 | }
1735 | return value;
1736 | }
1737 |
1738 | static inline uint64_t
1739 | get_uint64_value(proto_tree *tree, tvbuff_t *tvb, int offset, unsigned length, const unsigned encoding)
1740 | {
1741 | uint64_t value;
1742 |
1743 | value = tvb_get_uint64_with_length(tvb, offset, length, encoding);
1744 |
1745 | if (length < 1 || length > 8) {
1746 | report_type_length_mismatch(tree, "an unsigned integer", length, (length < 1));
1747 | }
1748 |
1749 | return value;
1750 | }
1751 |
1752 | static int32_t
1753 | get_int_value(proto_tree *tree, tvbuff_t *tvb, int offset, int length, const unsigned encoding)
1754 | {
1755 | int32_t value;
1756 | bool_Bool length_error;
1757 |
1758 | switch (length) {
1759 |
1760 | case 1:
1761 | value = tvb_get_int8(tvb, offset);
1762 | break;
1763 |
1764 | case 2:
1765 | value = encoding ? tvb_get_letohis(tvb, offset)
1766 | : tvb_get_ntohis(tvb, offset);
1767 | break;
1768 |
1769 | case 3:
1770 | value = encoding ? tvb_get_letohi24(tvb, offset)
1771 | : tvb_get_ntohi24(tvb, offset);
1772 | break;
1773 |
1774 | case 4:
1775 | value = encoding ? tvb_get_letohil(tvb, offset)
1776 | : tvb_get_ntohil(tvb, offset);
1777 | break;
1778 |
1779 | default:
1780 | if (length < 1) {
1781 | length_error = true1;
1782 | value = 0;
1783 | } else {
1784 | length_error = false0;
1785 | value = encoding ? tvb_get_letohil(tvb, offset)
1786 | : tvb_get_ntohil(tvb, offset);
1787 | }
1788 | report_type_length_mismatch(tree, "a signed integer", length, length_error);
1789 | break;
1790 | }
1791 | return value;
1792 | }
1793 |
1794 | /* Note: this returns an unsigned int64, but with the appropriate bit(s) set to
1795 | * be cast-able as a int64_t. This is weird, but what the code has always done.
1796 | */
1797 | static inline uint64_t
1798 | get_int64_value(proto_tree *tree, tvbuff_t *tvb, int start, unsigned length, const unsigned encoding)
1799 | {
1800 | uint64_t value = get_uint64_value(tree, tvb, start, length, encoding);
1801 |
1802 | switch (length) {
1803 | case 7:
1804 | value = ws_sign_ext64(value, 56);
1805 | break;
1806 | case 6:
1807 | value = ws_sign_ext64(value, 48);
1808 | break;
1809 | case 5:
1810 | value = ws_sign_ext64(value, 40);
1811 | break;
1812 | case 4:
1813 | value = ws_sign_ext64(value, 32);
1814 | break;
1815 | case 3:
1816 | value = ws_sign_ext64(value, 24);
1817 | break;
1818 | case 2:
1819 | value = ws_sign_ext64(value, 16);
1820 | break;
1821 | case 1:
1822 | value = ws_sign_ext64(value, 8);
1823 | break;
1824 | }
1825 |
1826 | return value;
1827 | }
1828 |
1829 | /* For FT_STRING */
1830 | static inline const uint8_t *
1831 | get_string_value(wmem_allocator_t *scope, tvbuff_t *tvb, int start,
1832 | int length, int *ret_length, const unsigned encoding)
1833 | {
1834 | if (length == -1) {
1835 | length = tvb_ensure_captured_length_remaining(tvb, start);
1836 | }
1837 | *ret_length = length;
1838 | return tvb_get_string_enc(scope, tvb, start, length, encoding);
1839 | }
1840 |
1841 | /* For FT_STRINGZ */
1842 | static inline const uint8_t *
1843 | get_stringz_value(wmem_allocator_t *scope, proto_tree *tree, tvbuff_t *tvb,
1844 | int start, int length, int *ret_length, const unsigned encoding)
1845 | {
1846 | const uint8_t *value;
1847 |
1848 | if (length < -1) {
1849 | report_type_length_mismatch(tree, "a string", length, true1);
1850 | }
1851 |
1852 | /* XXX - Ideally, every "null-terminated string which fits into a
1853 | * known length" should be either FT_STRINGZPAD or FT_STRINGZTRUNC
1854 | * as appropriate, not a FT_STRINGZ. If so, then we could always call
1855 | * tvb_get_stringz_enc here. Failing that, we could treat length 0
1856 | * as unknown length as well (since there is a trailing '\0', the real
1857 | * length is never zero), allowing switching to unsigned lengths.
1858 | */
1859 | if (length == -1) {
1860 | /* This can throw an exception */
1861 | value = tvb_get_stringz_enc(scope, tvb, start, (unsigned*)&length, encoding);
1862 | } else {
1863 | /* In this case, length signifies the length of the string.
1864 | *
1865 | * This could either be a null-padded string, which doesn't
1866 | * necessarily have a '\0' at the end, or a null-terminated
1867 | * string, with a trailing '\0'. (Yes, there are cases
1868 | * where you have a string that's both counted and null-
1869 | * terminated.)
1870 | *
1871 | * In the first case, we must allocate a buffer of length
1872 | * "length+1", to make room for a trailing '\0'.
1873 | *
1874 | * In the second case, we don't assume that there is a
1875 | * trailing '\0' there, as the packet might be malformed.
1876 | * (XXX - should we throw an exception if there's no
1877 | * trailing '\0'?) Therefore, we allocate a buffer of
1878 | * length "length+1", and put in a trailing '\0', just to
1879 | * be safe.
1880 | *
1881 | * (XXX - this would change if we made string values counted
1882 | * rather than null-terminated.)
1883 | */
1884 | value = tvb_get_string_enc(scope, tvb, start, length, encoding);
1885 | }
1886 | *ret_length = length;
1887 | return value;
1888 | }
1889 |
1890 | /* For FT_UINT_STRING */
1891 | static inline const uint8_t *
1892 | get_uint_string_value(wmem_allocator_t *scope, proto_tree *tree,
1893 | tvbuff_t *tvb, int start, int length, int *ret_length,
1894 | const unsigned encoding)
1895 | {
1896 | uint32_t n;
1897 | const uint8_t *value;
1898 |
1899 | /* I believe it's ok if this is called with a NULL tree */
1900 | n = get_uint_value(tree, tvb, start, length, encoding & ~ENC_CHARENCODING_MASK0x0000FFFE);
1901 | value = tvb_get_string_enc(scope, tvb, start + length, n, encoding);
1902 | length += n;
1903 | *ret_length = length;
1904 | return value;
1905 | }
1906 |
1907 | /* For FT_STRINGZPAD */
1908 | static inline const uint8_t *
1909 | get_stringzpad_value(wmem_allocator_t *scope, tvbuff_t *tvb, int start,
1910 | int length, int *ret_length, const unsigned encoding)
1911 | {
1912 | /*
1913 | * XXX - currently, string values are null-
1914 | * terminated, so a "zero-padded" string
1915 | * isn't special. If we represent string
1916 | * values as something that includes a counted
1917 | * array of bytes, we'll need to strip the
1918 | * trailing NULs.
1919 | */
1920 | if (length == -1) {
1921 | length = tvb_ensure_captured_length_remaining(tvb, start);
1922 | }
1923 | *ret_length = length;
1924 | return tvb_get_string_enc(scope, tvb, start, length, encoding);
1925 | }
1926 |
1927 | /* For FT_STRINGZTRUNC */
1928 | static inline const uint8_t *
1929 | get_stringztrunc_value(wmem_allocator_t *scope, tvbuff_t *tvb, int start,
1930 | int length, int *ret_length, const unsigned encoding)
1931 | {
1932 | /*
1933 | * XXX - currently, string values are null-
1934 | * terminated, so a "zero-truncated" string
1935 | * isn't special. If we represent string
1936 | * values as something that includes a counted
1937 | * array of bytes, we'll need to strip everything
1938 | * starting with the terminating NUL.
1939 | */
1940 | if (length == -1) {
1941 | length = tvb_ensure_captured_length_remaining(tvb, start);
1942 | }
1943 | *ret_length = length;
1944 | return tvb_get_string_enc(scope, tvb, start, length, encoding);
1945 | }
1946 |
1947 | /*
1948 | * Deltas between the epochs for various non-UN*X time stamp formats and
1949 | * the January 1, 1970, 00:00:00 (proleptic?) UTC epoch for the UN*X time
1950 | * stamp format.
1951 | */
1952 |
1953 | /*
1954 | * NTP Era 0: the epoch is January 1, 1900, 00:00:00 (proleptic?) UTC.
1955 | * XXX - if it's OK if this is unsigned, can we just use
1956 | * EPOCH_DELTA_1900_01_01_00_00_00_UTC?
1957 | */
1958 | #define NTP_TIMEDIFF1900TO1970SEC2208988800L INT64_C(2208988800)2208988800L
1959 |
1960 | /*
1961 | * NTP Era 1: the epoch is February 7, 2036, 06:28:16 UTC.
1962 | */
1963 | #define NTP_TIMEDIFF1970TO2036SEC2085978496L INT64_C(2085978496)2085978496L
1964 |
1965 | /* this can be called when there is no tree, so tree may be null */
1966 | static void
1967 | get_time_value(proto_tree *tree, tvbuff_t *tvb, const int start,
1968 | const int length, const unsigned encoding, nstime_t *time_stamp,
1969 | const bool_Bool is_relative)
1970 | {
1971 | uint32_t tmpsecs;
1972 | uint64_t tmp64secs;
1973 | uint64_t todusecs;
1974 |
1975 | switch (encoding) {
1976 |
1977 | case ENC_TIME_SECS_NSECS0x00000000|ENC_BIG_ENDIAN0x00000000:
1978 | /*
1979 | * If the length is 16, 8-byte seconds, followed
1980 | * by 8-byte fractional time in nanoseconds,
1981 | * both big-endian.
1982 | *
1983 | * If the length is 12, 8-byte seconds, followed
1984 | * by 4-byte fractional time in nanoseconds,
1985 | * both big-endian.
1986 | *
1987 | * If the length is 8, 4-byte seconds, followed
1988 | * by 4-byte fractional time in nanoseconds,
1989 | * both big-endian.
1990 | *
1991 | * For absolute times, the seconds are seconds
1992 | * since the UN*X epoch.
1993 | */
1994 | if (length == 16) {
1995 | time_stamp->secs = (time_t)tvb_get_ntoh64(tvb, start);
1996 | time_stamp->nsecs = (uint32_t)tvb_get_ntoh64(tvb, start+8);
1997 | } else if (length == 12) {
1998 | time_stamp->secs = (time_t)tvb_get_ntoh64(tvb, start);
1999 | time_stamp->nsecs = tvb_get_ntohl(tvb, start+8);
2000 | } else if (length == 8) {
2001 | time_stamp->secs = (time_t)tvb_get_ntohl(tvb, start);
2002 | time_stamp->nsecs = tvb_get_ntohl(tvb, start+4);
2003 | } else if (length == 4) {
2004 | /*
2005 | * Backwards compatibility.
2006 | * ENC_TIME_SECS_NSECS is 0; using
2007 | * ENC_BIG_ENDIAN by itself with a 4-byte
2008 | * time-in-seconds value was done in the
2009 | * past.
2010 | */
2011 | time_stamp->secs = (time_t)tvb_get_ntohl(tvb, start);
2012 | time_stamp->nsecs = 0;
2013 | } else {
2014 | time_stamp->secs = 0;
2015 | time_stamp->nsecs = 0;
2016 | report_type_length_mismatch(tree, "a timespec", length, (length < 4));
2017 | }
2018 | break;
2019 |
2020 | case ENC_TIME_SECS_NSECS0x00000000|ENC_LITTLE_ENDIAN0x80000000:
2021 | /*
2022 | * If the length is 16, 8-byte seconds, followed
2023 | * by 8-byte fractional time in nanoseconds,
2024 | * both little-endian.
2025 | *
2026 | * If the length is 12, 8-byte seconds, followed
2027 | * by 4-byte fractional time in nanoseconds,
2028 | * both little-endian.
2029 | *
2030 | * If the length is 8, 4-byte seconds, followed
2031 | * by 4-byte fractional time in nanoseconds,
2032 | * both little-endian.
2033 | *
2034 | * For absolute times, the seconds are seconds
2035 | * since the UN*X epoch.
2036 | */
2037 | if (length == 16) {
2038 | time_stamp->secs = (time_t)tvb_get_letoh64(tvb, start);
2039 | time_stamp->nsecs = (uint32_t)tvb_get_letoh64(tvb, start+8);
2040 | } else if (length == 12) {
2041 | time_stamp->secs = (time_t)tvb_get_letoh64(tvb, start);
2042 | time_stamp->nsecs = tvb_get_letohl(tvb, start+8);
2043 | } else if (length == 8) {
2044 | time_stamp->secs = (time_t)tvb_get_letohl(tvb, start);
2045 | time_stamp->nsecs = tvb_get_letohl(tvb, start+4);
2046 | } else if (length == 4) {
2047 | /*
2048 | * Backwards compatibility.
2049 | * ENC_TIME_SECS_NSECS is 0; using
2050 | * ENC_LITTLE_ENDIAN by itself with a 4-byte
2051 | * time-in-seconds value was done in the
2052 | * past.
2053 | */
2054 | time_stamp->secs = (time_t)tvb_get_letohl(tvb, start);
2055 | time_stamp->nsecs = 0;
2056 | } else {
2057 | time_stamp->secs = 0;
2058 | time_stamp->nsecs = 0;
2059 | report_type_length_mismatch(tree, "a timespec", length, (length < 4));
2060 | }
2061 | break;
2062 |
2063 | case ENC_TIME_NTP0x00000002|ENC_BIG_ENDIAN0x00000000:
2064 | /*
2065 | * NTP time stamp, big-endian.
2066 | * Only supported for absolute times.
2067 | */
2068 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2068, "!is_relative" ))));
2069 |
2070 | /* We need a temporary variable here so the unsigned math
2071 | * works correctly (for years > 2036 according to RFC 2030
2072 | * chapter 3).
2073 | *
2074 | * If bit 0 is set, the UTC time is in the range 1968-2036 and
2075 | * UTC time is reckoned from 0h 0m 0s UTC on 1 January 1900.
2076 | * If bit 0 is not set, the time is in the range 2036-2104 and
2077 | * UTC time is reckoned from 6h 28m 16s UTC on 7 February 2036.
2078 | */
2079 | tmpsecs = tvb_get_ntohl(tvb, start);
2080 | if ((tmpsecs & 0x80000000) != 0)
2081 | time_stamp->secs = (time_t)((int64_t)tmpsecs - NTP_TIMEDIFF1900TO1970SEC2208988800L);
2082 | else
2083 | time_stamp->secs = (time_t)((int64_t)tmpsecs + NTP_TIMEDIFF1970TO2036SEC2085978496L);
2084 |
2085 | if (length == 8) {
2086 | tmp64secs = tvb_get_ntoh64(tvb, start);
2087 | if (tmp64secs == 0) {
2088 | //This is "NULL" time
2089 | time_stamp->secs = 0;
2090 | time_stamp->nsecs = 0;
2091 | } else {
2092 | /*
2093 | * Convert 1/2^32s of a second to
2094 | * nanoseconds.
2095 | */
2096 | time_stamp->nsecs = (int)(1000000000*(tvb_get_ntohl(tvb, start+4)/4294967296.0));
2097 | }
2098 | } else if (length == 4) {
2099 | /*
2100 | * Backwards compatibility.
2101 | */
2102 | if (tmpsecs == 0) {
2103 | //This is "NULL" time
2104 | time_stamp->secs = 0;
2105 | }
2106 | time_stamp->nsecs = 0;
2107 | } else {
2108 | time_stamp->secs = 0;
2109 | time_stamp->nsecs = 0;
2110 | report_type_length_mismatch(tree, "an NTP time stamp", length, (length < 4));
2111 | }
2112 | break;
2113 |
2114 | case ENC_TIME_NTP0x00000002|ENC_LITTLE_ENDIAN0x80000000:
2115 | /*
2116 | * NTP time stamp, little-endian.
2117 | * Only supported for absolute times.
2118 | *
2119 | * NTP doesn't use this, because it's an Internet format
2120 | * and hence big-endian. Any implementation must decide
2121 | * whether the NTP timestamp is a 64-bit unsigned fixed
2122 | * point number (RFC 1305, RFC 4330) or a 64-bit struct
2123 | * with a 32-bit unsigned seconds field followed by a
2124 | * 32-bit fraction field (cf. RFC 5905, which obsoletes
2125 | * the previous two).
2126 | *
2127 | * XXX: We do the latter, but no dissector uses this format.
2128 | * OTOH, ERF timestamps do the former, so perhaps we
2129 | * should switch the interpretation so that packet-erf.c
2130 | * could use this directly?
2131 | */
2132 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2132, "!is_relative" ))));
2133 |
2134 | /* We need a temporary variable here so the unsigned math
2135 | * works correctly (for years > 2036 according to RFC 2030
2136 | * chapter 3).
2137 | *
2138 | * If bit 0 is set, the UTC time is in the range 1968-2036 and
2139 | * UTC time is reckoned from 0h 0m 0s UTC on 1 January 1900.
2140 | * If bit 0 is not set, the time is in the range 2036-2104 and
2141 | * UTC time is reckoned from 6h 28m 16s UTC on 7 February 2036.
2142 | */
2143 | tmpsecs = tvb_get_letohl(tvb, start);
2144 | if ((tmpsecs & 0x80000000) != 0)
2145 | time_stamp->secs = (time_t)((int64_t)tmpsecs - NTP_TIMEDIFF1900TO1970SEC2208988800L);
2146 | else
2147 | time_stamp->secs = (time_t)((int64_t)tmpsecs + NTP_TIMEDIFF1970TO2036SEC2085978496L);
2148 |
2149 | if (length == 8) {
2150 | tmp64secs = tvb_get_letoh64(tvb, start);
2151 | if (tmp64secs == 0) {
2152 | //This is "NULL" time
2153 | time_stamp->secs = 0;
2154 | time_stamp->nsecs = 0;
2155 | } else {
2156 | /*
2157 | * Convert 1/2^32s of a second to
2158 | * nanoseconds.
2159 | */
2160 | time_stamp->nsecs = (int)(1000000000*(tvb_get_letohl(tvb, start+4)/4294967296.0));
2161 | }
2162 | } else if (length == 4) {
2163 | /*
2164 | * Backwards compatibility.
2165 | */
2166 | if (tmpsecs == 0) {
2167 | //This is "NULL" time
2168 | time_stamp->secs = 0;
2169 | }
2170 | time_stamp->nsecs = 0;
2171 | } else {
2172 | time_stamp->secs = 0;
2173 | time_stamp->nsecs = 0;
2174 | report_type_length_mismatch(tree, "an NTP time stamp", length, (length < 4));
2175 | }
2176 | break;
2177 |
2178 | case ENC_TIME_TOD0x00000004|ENC_BIG_ENDIAN0x00000000:
2179 | /*
2180 | * S/3x0 and z/Architecture TOD clock time stamp,
2181 | * big-endian. The epoch is January 1, 1900,
2182 | * 00:00:00 (proleptic?) UTC.
2183 | *
2184 | * Only supported for absolute times.
2185 | */
2186 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2186, "!is_relative" ))));
2187 | DISSECTOR_ASSERT(length == 8)((void) ((length == 8) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2187, "length == 8" ))));
2188 |
2189 | if (length == 8) {
2190 | todusecs = tvb_get_ntoh64(tvb, start) >> 12;
2191 | time_stamp->secs = (time_t)((todusecs / 1000000) - EPOCH_DELTA_1900_01_01_00_00_00_UTC2208988800U);
2192 | time_stamp->nsecs = (int)((todusecs % 1000000) * 1000);
2193 | } else {
2194 | time_stamp->secs = 0;
2195 | time_stamp->nsecs = 0;
2196 | report_type_length_mismatch(tree, "a TOD clock time stamp", length, (length < 4));
2197 | }
2198 | break;
2199 |
2200 | case ENC_TIME_TOD0x00000004|ENC_LITTLE_ENDIAN0x80000000:
2201 | /*
2202 | * S/3x0 and z/Architecture TOD clock time stamp,
2203 | * little-endian. The epoch is January 1, 1900,
2204 | * 00:00:00 (proleptic?) UTC.
2205 | *
2206 | * Only supported for absolute times.
2207 | */
2208 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2208, "!is_relative" ))));
2209 |
2210 | if (length == 8) {
2211 | todusecs = tvb_get_letoh64(tvb, start) >> 12 ;
2212 | time_stamp->secs = (time_t)((todusecs / 1000000) - EPOCH_DELTA_1900_01_01_00_00_00_UTC2208988800U);
2213 | time_stamp->nsecs = (int)((todusecs % 1000000) * 1000);
2214 | } else {
2215 | time_stamp->secs = 0;
2216 | time_stamp->nsecs = 0;
2217 | report_type_length_mismatch(tree, "a TOD clock time stamp", length, (length < 4));
2218 | }
2219 | break;
2220 |
2221 | case ENC_TIME_RTPS0x00000008|ENC_BIG_ENDIAN0x00000000:
2222 | /*
2223 | * Time stamp using the same seconds/fraction format
2224 | * as NTP, but with the origin of the time stamp being
2225 | * the UNIX epoch rather than the NTP epoch; big-
2226 | * endian.
2227 | *
2228 | * Only supported for absolute times.
2229 | */
2230 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2230, "!is_relative" ))));
2231 |
2232 | if (length == 8) {
2233 | time_stamp->secs = (time_t)tvb_get_ntohl(tvb, start);
2234 | /*
2235 | * Convert 1/2^32s of a second to nanoseconds.
2236 | */
2237 | time_stamp->nsecs = (int)(1000000000*(tvb_get_ntohl(tvb, start+4)/4294967296.0));
2238 | } else {
2239 | time_stamp->secs = 0;
2240 | time_stamp->nsecs = 0;
2241 | report_type_length_mismatch(tree, "an RTPS time stamp", length, (length < 4));
2242 | }
2243 | break;
2244 |
2245 | case ENC_TIME_RTPS0x00000008|ENC_LITTLE_ENDIAN0x80000000:
2246 | /*
2247 | * Time stamp using the same seconds/fraction format
2248 | * as NTP, but with the origin of the time stamp being
2249 | * the UNIX epoch rather than the NTP epoch; little-
2250 | * endian.
2251 | *
2252 | * Only supported for absolute times.
2253 | *
2254 | * The RTPS specification explicitly supports Little
2255 | * Endian encoding. In one place, it states that its
2256 | * Time_t representation "is the one defined by ...
2257 | * RFC 1305", but in another explicitly defines it as
2258 | * a struct consisting of an 32 bit unsigned seconds
2259 | * field and a 32 bit unsigned fraction field, not a 64
2260 | * bit fixed point, so we do that here.
2261 | * https://www.omg.org/spec/DDSI-RTPS/2.5/PDF
2262 | */
2263 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2263, "!is_relative" ))));
2264 |
2265 | if (length == 8) {
2266 | time_stamp->secs = (time_t)tvb_get_letohl(tvb, start);
2267 | /*
2268 | * Convert 1/2^32s of a second to nanoseconds.
2269 | */
2270 | time_stamp->nsecs = (int)(1000000000*(tvb_get_letohl(tvb, start+4)/4294967296.0));
2271 | } else {
2272 | time_stamp->secs = 0;
2273 | time_stamp->nsecs = 0;
2274 | report_type_length_mismatch(tree, "an RTPS time stamp", length, (length < 4));
2275 | }
2276 | break;
2277 |
2278 | case ENC_TIME_MIP60x00000024 | ENC_BIG_ENDIAN0x00000000:
2279 | /*
2280 | * MIP6 time stamp, big-endian.
2281 | * A 64-bit unsigned integer field containing a timestamp. The
2282 | * value indicates the number of seconds since January 1, 1970,
2283 | * 00:00 UTC, by using a fixed point format. In this format, the
2284 | * integer number of seconds is contained in the first 48 bits of
2285 | * the field, and the remaining 16 bits indicate the number of
2286 | * 1/65536 fractions of a second.
2287 |
2288 | * Only supported for absolute times.
2289 | */
2290 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2290, "!is_relative" ))));
2291 |
2292 | if (length == 8) {
2293 | /* We need a temporary variable here so the casting and fractions
2294 | * of a second work correctly.
2295 | */
2296 | tmp64secs = tvb_get_ntoh48(tvb, start);
2297 | tmpsecs = tvb_get_ntohs(tvb, start + 6);
2298 | tmpsecs <<= 16;
2299 |
2300 | if ((tmp64secs == 0) && (tmpsecs == 0)) {
2301 | //This is "NULL" time
2302 | time_stamp->secs = 0;
2303 | time_stamp->nsecs = 0;
2304 | } else {
2305 | time_stamp->secs = (time_t)tmp64secs;
2306 | time_stamp->nsecs = (int)((tmpsecs / 4294967296.0) * 1000000000);
2307 | }
2308 | } else {
2309 | time_stamp->secs = 0;
2310 | time_stamp->nsecs = 0;
2311 | report_type_length_mismatch(tree, "an NTP time stamp", length, (length != 8));
2312 | }
2313 | break;
2314 |
2315 | case ENC_TIME_SECS_USECS0x00000010|ENC_BIG_ENDIAN0x00000000:
2316 | /*
2317 | * If the length is 16, 8-byte seconds, followed
2318 | * by 8-byte fractional time in microseconds,
2319 | * both big-endian.
2320 | *
2321 | * If the length is 12, 8-byte seconds, followed
2322 | * by 4-byte fractional time in microseconds,
2323 | * both big-endian.
2324 | *
2325 | * If the length is 8, 4-byte seconds, followed
2326 | * by 4-byte fractional time in microseconds,
2327 | * both big-endian.
2328 | *
2329 | * For absolute times, the seconds are seconds
2330 | * since the UN*X epoch.
2331 | */
2332 | if (length == 16) {
2333 | time_stamp->secs = (time_t)tvb_get_ntoh64(tvb, start);
2334 | time_stamp->nsecs = (uint32_t)tvb_get_ntoh64(tvb, start+8)*1000;
2335 | } else if (length == 12) {
2336 | time_stamp->secs = (time_t)tvb_get_ntoh64(tvb, start);
2337 | time_stamp->nsecs = tvb_get_ntohl(tvb, start+8)*1000;
2338 | } else if (length == 8) {
2339 | time_stamp->secs = (time_t)tvb_get_ntohl(tvb, start);
2340 | time_stamp->nsecs = tvb_get_ntohl(tvb, start+4)*1000;
2341 | } else {
2342 | time_stamp->secs = 0;
2343 | time_stamp->nsecs = 0;
2344 | report_type_length_mismatch(tree, "a timeval", length, (length < 4));
2345 | }
2346 | break;
2347 |
2348 | case ENC_TIME_SECS_USECS0x00000010|ENC_LITTLE_ENDIAN0x80000000:
2349 | /*
2350 | * If the length is 16, 8-byte seconds, followed
2351 | * by 8-byte fractional time in microseconds,
2352 | * both little-endian.
2353 | *
2354 | * If the length is 12, 8-byte seconds, followed
2355 | * by 4-byte fractional time in microseconds,
2356 | * both little-endian.
2357 | *
2358 | * If the length is 8, 4-byte seconds, followed
2359 | * by 4-byte fractional time in microseconds,
2360 | * both little-endian.
2361 | *
2362 | * For absolute times, the seconds are seconds
2363 | * since the UN*X epoch.
2364 | */
2365 | if (length == 16) {
2366 | time_stamp->secs = (time_t)tvb_get_letoh64(tvb, start);
2367 | time_stamp->nsecs = (uint32_t)tvb_get_letoh64(tvb, start+8)*1000;
2368 | } else if (length == 12) {
2369 | time_stamp->secs = (time_t)tvb_get_letoh64(tvb, start);
2370 | time_stamp->nsecs = tvb_get_letohl(tvb, start+8)*1000;
2371 | } else if (length == 8) {
2372 | time_stamp->secs = (time_t)tvb_get_letohl(tvb, start);
2373 | time_stamp->nsecs = tvb_get_letohl(tvb, start+4)*1000;
2374 | } else {
2375 | time_stamp->secs = 0;
2376 | time_stamp->nsecs = 0;
2377 | report_type_length_mismatch(tree, "a timeval", length, (length < 4));
2378 | }
2379 | break;
2380 |
2381 | case ENC_TIME_SECS0x00000012|ENC_BIG_ENDIAN0x00000000:
2382 | case ENC_TIME_SECS0x00000012|ENC_LITTLE_ENDIAN0x80000000:
2383 | /*
2384 | * Seconds, 1 to 8 bytes.
2385 | * For absolute times, it's seconds since the
2386 | * UN*X epoch.
2387 | */
2388 | if (length >= 1 && length <= 8) {
2389 | time_stamp->secs = (time_t)get_uint64_value(tree, tvb, start, length, encoding);
2390 | time_stamp->nsecs = 0;
2391 | } else {
2392 | time_stamp->secs = 0;
2393 | time_stamp->nsecs = 0;
2394 | report_type_length_mismatch(tree, "a time-in-seconds time stamp", length, (length < 4));
2395 | }
2396 | break;
2397 |
2398 | case ENC_TIME_MSECS0x00000014|ENC_BIG_ENDIAN0x00000000:
2399 | case ENC_TIME_MSECS0x00000014|ENC_LITTLE_ENDIAN0x80000000:
2400 | /*
2401 | * Milliseconds, 1 to 8 bytes.
2402 | * For absolute times, it's milliseconds since the
2403 | * UN*X epoch.
2404 | */
2405 | if (length >= 1 && length <= 8) {
2406 | uint64_t msecs;
2407 |
2408 | msecs = get_uint64_value(tree, tvb, start, length, encoding);
2409 | time_stamp->secs = (time_t)(msecs / 1000);
2410 | time_stamp->nsecs = (int)(msecs % 1000)*1000000;
2411 | } else {
2412 | time_stamp->secs = 0;
2413 | time_stamp->nsecs = 0;
2414 | report_type_length_mismatch(tree, "a time-in-milliseconds time stamp", length, (length < 4));
2415 | }
2416 | break;
2417 |
2418 | case ENC_TIME_USECS0x00000030|ENC_BIG_ENDIAN0x00000000:
2419 | case ENC_TIME_USECS0x00000030|ENC_LITTLE_ENDIAN0x80000000:
2420 | /*
2421 | * Microseconds, 1 to 8 bytes.
2422 | * For absolute times, it's microseconds since the
2423 | * UN*X epoch.
2424 | */
2425 | if (length >= 1 && length <= 8) {
2426 | uint64_t usecs;
2427 |
2428 | usecs = get_uint64_value(tree, tvb, start, length, encoding);
2429 | time_stamp->secs = (time_t)(usecs / 1000000);
2430 | time_stamp->nsecs = (int)(usecs % 1000000)*1000;
2431 | } else {
2432 | time_stamp->secs = 0;
2433 | time_stamp->nsecs = 0;
2434 | report_type_length_mismatch(tree, "a time-in-microseconds time stamp", length, (length < 4));
2435 | }
2436 | break;
2437 |
2438 | case ENC_TIME_NSECS0x00000028|ENC_BIG_ENDIAN0x00000000:
2439 | case ENC_TIME_NSECS0x00000028|ENC_LITTLE_ENDIAN0x80000000:
2440 | /*
2441 | * nanoseconds, 1 to 8 bytes.
2442 | * For absolute times, it's nanoseconds since the
2443 | * UN*X epoch.
2444 | */
2445 |
2446 | if (length >= 1 && length <= 8) {
2447 | uint64_t nsecs;
2448 |
2449 | nsecs = get_uint64_value(tree, tvb, start, length, encoding);
2450 | time_stamp->secs = (time_t)(nsecs / 1000000000);
2451 | time_stamp->nsecs = (int)(nsecs % 1000000000);
2452 | } else {
2453 | time_stamp->secs = 0;
2454 | time_stamp->nsecs = 0;
2455 | report_type_length_mismatch(tree, "a time-in-nanoseconds time stamp", length, (length < 4));
2456 | }
2457 | break;
2458 |
2459 | case ENC_TIME_RFC_39710x00000020|ENC_BIG_ENDIAN0x00000000:
2460 | /*
2461 | * 1/64ths of a second since the UN*X epoch,
2462 | * big-endian.
2463 | *
2464 | * Only supported for absolute times.
2465 | */
2466 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2466, "!is_relative" ))));
2467 |
2468 | if (length == 8) {
2469 | /*
2470 | * The upper 48 bits are seconds since the
2471 | * UN*X epoch.
2472 | */
2473 | time_stamp->secs = (time_t)tvb_get_ntoh48(tvb, start);
2474 | /*
2475 | * The lower 16 bits are 1/2^16s of a second;
2476 | * convert them to nanoseconds.
2477 | *
2478 | * XXX - this may give the impression of higher
2479 | * precision than you actually get.
2480 | */
2481 | time_stamp->nsecs = (int)(1000000000*(tvb_get_ntohs(tvb, start+6)/65536.0));
2482 | } else {
2483 | time_stamp->secs = 0;
2484 | time_stamp->nsecs = 0;
2485 | report_type_length_mismatch(tree, "an RFC 3971-style time stamp", length, (length < 4));
2486 | }
2487 | break;
2488 |
2489 | case ENC_TIME_RFC_39710x00000020|ENC_LITTLE_ENDIAN0x80000000:
2490 | /*
2491 | * 1/64ths of a second since the UN*X epoch,
2492 | * little-endian.
2493 | *
2494 | * Only supported for absolute times.
2495 | */
2496 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2496, "!is_relative" ))));
2497 |
2498 | if (length == 8) {
2499 | /*
2500 | * XXX - this is assuming that, if anybody
2501 | * were ever to use this format - RFC 3971
2502 | * doesn't, because that's an Internet
2503 | * protocol, and those use network byte
2504 | * order, i.e. big-endian - they'd treat it
2505 | * as a 64-bit count of 1/2^16s of a second,
2506 | * putting the upper 48 bits at the end.
2507 | *
2508 | * The lower 48 bits are seconds since the
2509 | * UN*X epoch.
2510 | */
2511 | time_stamp->secs = (time_t)tvb_get_letoh48(tvb, start+2);
2512 | /*
2513 | * The upper 16 bits are 1/2^16s of a second;
2514 | * convert them to nanoseconds.
2515 | *
2516 | * XXX - this may give the impression of higher
2517 | * precision than you actually get.
2518 | */
2519 | time_stamp->nsecs = (int)(1000000000*(tvb_get_letohs(tvb, start)/65536.0));
2520 | } else {
2521 | time_stamp->secs = 0;
2522 | time_stamp->nsecs = 0;
2523 | report_type_length_mismatch(tree, "an RFC 3971-style time stamp", length, (length < 4));
2524 | }
2525 | break;
2526 |
2527 | case ENC_TIME_SECS_NTP0x00000018|ENC_BIG_ENDIAN0x00000000:
2528 | /*
2529 | * NTP time stamp, with 1-second resolution (i.e.,
2530 | * seconds since the NTP epoch), big-endian.
2531 | * Only supported for absolute times.
2532 | */
2533 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2533, "!is_relative" ))));
2534 |
2535 | if (length == 4) {
2536 | /*
2537 | * We need a temporary variable here so the unsigned math
2538 | * works correctly (for years > 2036 according to RFC 2030
2539 | * chapter 3).
2540 | *
2541 | * If bit 0 is set, the UTC time is in the range 1968-2036 and
2542 | * UTC time is reckoned from 0h 0m 0s UTC on 1 January 1900.
2543 | * If bit 0 is not set, the time is in the range 2036-2104 and
2544 | * UTC time is reckoned from 6h 28m 16s UTC on 7 February 2036.
2545 | */
2546 | tmpsecs = tvb_get_ntohl(tvb, start);
2547 | if ((tmpsecs & 0x80000000) != 0)
2548 | time_stamp->secs = (time_t)((int64_t)tmpsecs - NTP_TIMEDIFF1900TO1970SEC2208988800L);
2549 | else
2550 | time_stamp->secs = (time_t)((int64_t)tmpsecs + NTP_TIMEDIFF1970TO2036SEC2085978496L);
2551 | time_stamp->nsecs = 0;
2552 | } else {
2553 | time_stamp->secs = 0;
2554 | time_stamp->nsecs = 0;
2555 | report_type_length_mismatch(tree, "an NTP seconds-only time stamp", length, (length < 4));
2556 | }
2557 | break;
2558 |
2559 | case ENC_TIME_SECS_NTP0x00000018|ENC_LITTLE_ENDIAN0x80000000:
2560 | /*
2561 | * NTP time stamp, with 1-second resolution (i.e.,
2562 | * seconds since the NTP epoch), little-endian.
2563 | * Only supported for absolute times.
2564 | */
2565 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2565, "!is_relative" ))));
2566 |
2567 | /*
2568 | * We need a temporary variable here so the unsigned math
2569 | * works correctly (for years > 2036 according to RFC 2030
2570 | * chapter 3).
2571 | *
2572 | * If bit 0 is set, the UTC time is in the range 1968-2036 and
2573 | * UTC time is reckoned from 0h 0m 0s UTC on 1 January 1900.
2574 | * If bit 0 is not set, the time is in the range 2036-2104 and
2575 | * UTC time is reckoned from 6h 28m 16s UTC on 7 February 2036.
2576 | */
2577 | if (length == 4) {
2578 | tmpsecs = tvb_get_letohl(tvb, start);
2579 | if ((tmpsecs & 0x80000000) != 0)
2580 | time_stamp->secs = (time_t)((int64_t)tmpsecs - NTP_TIMEDIFF1900TO1970SEC2208988800L);
2581 | else
2582 | time_stamp->secs = (time_t)((int64_t)tmpsecs + NTP_TIMEDIFF1970TO2036SEC2085978496L);
2583 | time_stamp->nsecs = 0;
2584 | } else {
2585 | time_stamp->secs = 0;
2586 | time_stamp->nsecs = 0;
2587 | report_type_length_mismatch(tree, "an NTP seconds-only time stamp", length, (length < 4));
2588 | }
2589 | break;
2590 |
2591 | case ENC_TIME_MSEC_NTP0x00000022 | ENC_BIG_ENDIAN0x00000000:
2592 | /*
2593 | * Milliseconds, 6 to 8 bytes.
2594 | * For absolute times, it's milliseconds since the
2595 | * NTP epoch.
2596 | *
2597 | * ETSI TS 129.274 8.119 defines this as:
2598 | * "a 48 bit unsigned integer in network order format
2599 | * ...encoded as the number of milliseconds since
2600 | * 00:00:00 January 1, 1900 00:00 UTC, i.e. as the
2601 | * rounded value of 1000 x the value of the 64-bit
2602 | * timestamp (Seconds + (Fraction / (1<<32))) defined
2603 | * in clause 6 of IETF RFC 5905."
2604 | *
2605 | * Taken literally, the part after "i.e." would
2606 | * mean that the value rolls over before reaching
2607 | * 2^32 * 1000 = 4294967296000 = 0x3e800000000
2608 | * when the 64 bit timestamp rolls over, and we have
2609 | * to pick an NTP Era equivalence class to support
2610 | * (such as 1968-01-20 to 2104-02-06).
2611 | *
2612 | * OTOH, the extra room might be used to store Era
2613 | * information instead, in which case times until
2614 | * 10819-08-03 can be represented with 6 bytes without
2615 | * ambiguity. We handle both implementations, and assume
2616 | * that times before 1968-01-20 are not represented.
2617 | *
2618 | * Only 6 bytes or more makes sense as an absolute
2619 | * time. 5 bytes or fewer could express a span of
2620 | * less than 35 years, either 1900-1934 or 2036-2070.
2621 | */
2622 | if (length >= 6 && length <= 8) {
2623 | uint64_t msecs;
2624 |
2625 | msecs = get_uint64_value(tree, tvb, start, length, encoding);
2626 | tmp64secs = (msecs / 1000);
2627 | /*
2628 | * Assume that times in the first half of NTP
2629 | * Era 0 really represent times in the NTP
2630 | * Era 1.
2631 | */
2632 | if (tmp64secs >= 0x80000000)
2633 | time_stamp->secs = (time_t)((int64_t)tmp64secs - NTP_TIMEDIFF1900TO1970SEC2208988800L);
2634 | else
2635 | time_stamp->secs = (time_t)((int64_t)tmp64secs + NTP_TIMEDIFF1970TO2036SEC2085978496L);
2636 | time_stamp->nsecs = (int)(msecs % 1000)*1000000;
2637 | }
2638 | else {
2639 | time_stamp->secs = 0;
2640 | time_stamp->nsecs = 0;
2641 | report_type_length_mismatch(tree, "a time-in-milliseconds NTP time stamp", length, (length < 6));
2642 | }
2643 | break;
2644 |
2645 | case ENC_TIME_MP4_FILE_SECS0x00000026|ENC_BIG_ENDIAN0x00000000:
2646 | /*
2647 | * MP4 file time stamps, big-endian.
2648 | * Only supported for absolute times.
2649 | */
2650 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2650, "!is_relative" ))));
2651 |
2652 | if (length == 8) {
2653 | tmp64secs = tvb_get_ntoh64(tvb, start);
2654 | time_stamp->secs = (time_t)(int64_t)(tmp64secs - EPOCH_DELTA_1904_01_01_00_00_00_UTC2082844800U);
2655 | time_stamp->nsecs = 0;
2656 | } else if (length == 4) {
2657 | tmpsecs = tvb_get_ntohl(tvb, start);
2658 | time_stamp->secs = (time_t)(int32_t)(tmpsecs - EPOCH_DELTA_1904_01_01_00_00_00_UTC2082844800U);
2659 | time_stamp->nsecs = 0;
2660 | } else {
2661 | time_stamp->secs = 0;
2662 | time_stamp->nsecs = 0;
2663 | report_type_length_mismatch(tree, "an MP4 time stamp", length, (length < 4));
2664 | }
2665 | break;
2666 |
2667 | case ENC_TIME_ZBEE_ZCL0x00000032 | ENC_BIG_ENDIAN0x00000000:
2668 | /*
2669 | * Zigbee ZCL time stamps, big-endian.
2670 | * Only supported for absolute times.
2671 | */
2672 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2672, "!is_relative" ))));
2673 |
2674 | if (length == 8) {
2675 | tmp64secs = tvb_get_ntoh64(tvb, start);
2676 | time_stamp->secs = (time_t)(int64_t)(tmp64secs + EPOCH_DELTA_2000_01_01_00_00_00_UTC((3*365 + 366)*7 + 2*365)*24*3600UL);
2677 | time_stamp->nsecs = 0;
2678 | } else if (length == 4) {
2679 | tmpsecs = tvb_get_ntohl(tvb, start);
2680 | time_stamp->secs = (time_t)(tmpsecs + EPOCH_DELTA_2000_01_01_00_00_00_UTC((3*365 + 366)*7 + 2*365)*24*3600UL);
2681 | time_stamp->nsecs = 0;
2682 | } else {
2683 | time_stamp->secs = 0;
2684 | time_stamp->nsecs = 0;
2685 | report_type_length_mismatch(tree, "a Zigbee ZCL time stamp", length, (length < 4));
2686 | }
2687 | break;
2688 |
2689 | case ENC_TIME_ZBEE_ZCL0x00000032 | ENC_LITTLE_ENDIAN0x80000000:
2690 | /*
2691 | * Zigbee ZCL time stamps, little-endian.
2692 | * Only supported for absolute times.
2693 | */
2694 | DISSECTOR_ASSERT(!is_relative)((void) ((!is_relative) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 2694, "!is_relative" ))));
2695 |
2696 | if (length == 8) {
2697 | tmp64secs = tvb_get_letoh64(tvb, start);
2698 | time_stamp->secs = (time_t)(int64_t)(tmp64secs + EPOCH_DELTA_2000_01_01_00_00_00_UTC((3*365 + 366)*7 + 2*365)*24*3600UL);
2699 | time_stamp->nsecs = 0;
2700 | } else if (length == 4) {
2701 | tmpsecs = tvb_get_letohl(tvb, start);
2702 | time_stamp->secs = (time_t)(tmpsecs + EPOCH_DELTA_2000_01_01_00_00_00_UTC((3*365 + 366)*7 + 2*365)*24*3600UL);
2703 | time_stamp->nsecs = 0;
2704 | } else {
2705 | time_stamp->secs = 0;
2706 | time_stamp->nsecs = 0;
2707 | report_type_length_mismatch(tree, "a Zigbee ZCL time stamp", length, (length < 4));
2708 | }
2709 | break;
2710 |
2711 | default:
2712 | DISSECTOR_ASSERT_NOT_REACHED()(proto_report_dissector_bug("%s:%u: failed assertion \"DISSECTOR_ASSERT_NOT_REACHED\"" , "epan/proto.c", 2712));
2713 | break;
2714 | }
2715 | }
2716 |
2717 | static void
2718 | tree_data_add_maybe_interesting_field(tree_data_t *tree_data, field_info *fi)
2719 | {
2720 | const header_field_info *hfinfo = fi->hfinfo;
2721 |
2722 | if (hfinfo->ref_type == HF_REF_TYPE_DIRECT || hfinfo->ref_type == HF_REF_TYPE_PRINT) {
2723 | GPtrArray *ptrs = NULL((void*)0);
2724 |
2725 | if (tree_data->interesting_hfids == NULL((void*)0)) {
2726 | /* Initialize the hash because we now know that it is needed */
2727 | tree_data->interesting_hfids =
2728 | g_hash_table_new(g_direct_hash, NULL((void*)0) /* g_direct_equal */);
2729 | } else if (g_hash_table_size(tree_data->interesting_hfids)) {
2730 | ptrs = (GPtrArray *)g_hash_table_lookup(tree_data->interesting_hfids,
2731 | GINT_TO_POINTER(hfinfo->id)((gpointer) (glong) (hfinfo->id)));
2732 | }
2733 |
2734 | if (!ptrs) {
2735 | /* First element triggers the creation of pointer array */
2736 | ptrs = g_ptr_array_new();
2737 | g_hash_table_insert(tree_data->interesting_hfids,
2738 | GINT_TO_POINTER(hfinfo->id)((gpointer) (glong) (hfinfo->id)), ptrs);
2739 | }
2740 |
2741 | g_ptr_array_add(ptrs, fi);
2742 | }
2743 | }
2744 |
2745 |
2746 | /*
2747 | * Validates that field length bytes are available starting from
2748 | * start (pos/neg). Throws an exception if they aren't.
2749 | */
2750 | static void
2751 | test_length(header_field_info *hfinfo, tvbuff_t *tvb,
2752 | int start, int length, const unsigned encoding)
2753 | {
2754 | int size = length;
2755 |
2756 | if (!tvb)
2757 | return;
2758 |
2759 | if ((hfinfo->type == FT_STRINGZ) ||
2760 | ((encoding & ENC_VARINT_MASK(0x00000002|0x00000004|0x00000008|0x00000010)) &&
2761 | (FT_IS_UINT(hfinfo->type)(((hfinfo->type) == FT_CHAR || (hfinfo->type) == FT_UINT8 || (hfinfo->type) == FT_UINT16 || (hfinfo->type) == FT_UINT24 || (hfinfo->type) == FT_UINT32 || (hfinfo->type) == FT_FRAMENUM ) || ((hfinfo->type) == FT_UINT40 || (hfinfo->type) == FT_UINT48 || (hfinfo->type) == FT_UINT56 || (hfinfo->type) == FT_UINT64 )) || FT_IS_INT(hfinfo->type)(((hfinfo->type) == FT_INT8 || (hfinfo->type) == FT_INT16 || (hfinfo->type) == FT_INT24 || (hfinfo->type) == FT_INT32 ) || ((hfinfo->type) == FT_INT40 || (hfinfo->type) == FT_INT48 || (hfinfo->type) == FT_INT56 || (hfinfo->type) == FT_INT64 ))))) {
2762 | /* If we're fetching until the end of the TVB, only validate
2763 | * that the offset is within range.
2764 | */
2765 | if (length == -1)
2766 | size = 0;
2767 | }
2768 |
2769 | tvb_ensure_bytes_exist(tvb, start, size);
2770 | }
2771 |
2772 | static void
2773 | detect_trailing_stray_characters(unsigned encoding, const char *string, int length, proto_item *pi)
2774 | {
2775 | bool_Bool found_stray_character = false0;
2776 |
2777 | if (!string)
2778 | return;
2779 |
2780 | switch (encoding & ENC_CHARENCODING_MASK0x0000FFFE) {
2781 | case ENC_ASCII0x00000000:
2782 | case ENC_UTF_80x00000002:
2783 | for (int i = (int)strlen(string); i < length; i++) {
2784 | if (string[i] != '\0') {
2785 | found_stray_character = true1;
2786 | break;
2787 | }
2788 | }
2789 | break;
2790 |
2791 | default:
2792 | break;
2793 | }
2794 |
2795 | if (found_stray_character) {
2796 | expert_add_info(NULL((void*)0), pi, &ei_string_trailing_characters);
2797 | }
2798 | }
2799 |
2800 | static void
2801 | free_fvalue_cb(void *data)
2802 | {
2803 | fvalue_t *fv = (fvalue_t*)data;
2804 | fvalue_free(fv);
2805 | }
2806 |
2807 | /* Add an item to a proto_tree, using the text label registered to that item;
2808 | the item is extracted from the tvbuff handed to it. */
2809 | static proto_item *
2810 | proto_tree_new_item(field_info *new_fi, proto_tree *tree,
2811 | tvbuff_t *tvb, int start, int length,
2812 | unsigned encoding)
2813 | {
2814 | proto_item *pi;
2815 | uint32_t value, n;
2816 | uint64_t value64;
2817 | ws_in4_addr ipv4_value;
2818 | float floatval;
2819 | double doubleval;
2820 | const char *stringval = NULL((void*)0);
2821 | nstime_t time_stamp;
2822 | bool_Bool length_error;
2823 |
2824 | /* Ensure that the newly created fvalue_t is freed if we throw an
2825 | * exception before adding it to the tree. (gcc creates clobbering
2826 | * when it optimizes the equivalent TRY..EXCEPT implementation.)
2827 | * XXX: Move the new_field_info() call inside here?
2828 | */
2829 | CLEANUP_PUSH(free_fvalue_cb, new_fi->value){ struct except_stacknode except_sn; struct except_cleanup except_cl ; except_setup_clean(&except_sn, &except_cl, (free_fvalue_cb ), (new_fi->value));
2830 |
2831 | switch (new_fi->hfinfo->type) {
2832 | case FT_NONE:
2833 | /* no value to set for FT_NONE */
2834 | break;
2835 |
2836 | case FT_PROTOCOL:
2837 | proto_tree_set_protocol_tvb(new_fi, tvb, new_fi->hfinfo->name, length);
2838 | break;
2839 |
2840 | case FT_BYTES:
2841 | proto_tree_set_bytes_tvb(new_fi, tvb, start, length);
2842 | break;
2843 |
2844 | case FT_UINT_BYTES:
2845 | n = get_uint_value(tree, tvb, start, length, encoding);
2846 | proto_tree_set_bytes_tvb(new_fi, tvb, start + length, n);
2847 |
2848 | /* Instead of calling proto_item_set_len(), since we don't yet
2849 | * have a proto_item, we set the field_info's length ourselves. */
2850 | new_fi->length = n + length;
2851 | break;
2852 |
2853 | case FT_BOOLEAN:
2854 | /*
2855 | * Map all non-zero values to little-endian for
2856 | * backwards compatibility.
2857 | */
2858 | if (encoding)
2859 | encoding = ENC_LITTLE_ENDIAN0x80000000;
2860 | proto_tree_set_boolean(new_fi,
2861 | get_uint64_value(tree, tvb, start, length, encoding));
2862 | break;
2863 |
2864 | case FT_CHAR:
2865 | /* XXX - make these just FT_UINT? */
2866 | case FT_UINT8:
2867 | case FT_UINT16:
2868 | case FT_UINT24:
2869 | case FT_UINT32:
2870 | if (encoding & ENC_VARINT_MASK(0x00000002|0x00000004|0x00000008|0x00000010)) {
2871 | new_fi->length = tvb_get_varint(tvb, start, (length == -1) ? FT_VARINT_MAX_LEN10 : length, &value64, encoding);
2872 | value = (uint32_t)value64;
2873 | if (!(encoding & ENC_VARINT_QUIC0x00000004)) {
2874 | new_fi->flags |= FI_VARINT0x00040000;
2875 | }
2876 | }
2877 | else {
2878 | /*
2879 | * Map all non-zero values to little-endian for
2880 | * backwards compatibility.
2881 | */
2882 | if (encoding)
2883 | encoding = ENC_LITTLE_ENDIAN0x80000000;
2884 |
2885 | value = get_uint_value(tree, tvb, start, length, encoding);
2886 | }
2887 | proto_tree_set_uint(new_fi, value);
2888 | break;
2889 |
2890 | case FT_UINT40:
2891 | case FT_UINT48:
2892 | case FT_UINT56:
2893 | case FT_UINT64:
2894 | if (encoding & ENC_VARINT_MASK(0x00000002|0x00000004|0x00000008|0x00000010)) {
2895 | new_fi->length = tvb_get_varint(tvb, start, (length == -1) ? FT_VARINT_MAX_LEN10 : length, &value64, encoding);
2896 | if (!(encoding & ENC_VARINT_QUIC0x00000004)) {
2897 | new_fi->flags |= FI_VARINT0x00040000;
2898 | }
2899 | }
2900 | else {
2901 | /*
2902 | * Map all other non-zero values to little-endian for
2903 | * backwards compatibility.
2904 | */
2905 | if (encoding)
2906 | encoding = ENC_LITTLE_ENDIAN0x80000000;
2907 |
2908 | value64 = get_uint64_value(tree, tvb, start, length, encoding);
2909 | }
2910 | proto_tree_set_uint64(new_fi, value64);
2911 | break;
2912 |
2913 | /* XXX - make these just FT_INT? */
2914 | case FT_INT8:
2915 | case FT_INT16:
2916 | case FT_INT24:
2917 | case FT_INT32:
2918 | /*
2919 | * Map all non-zero values to little-endian for
2920 | * backwards compatibility.
2921 | */
2922 | if (encoding)
2923 | encoding = ENC_LITTLE_ENDIAN0x80000000;
2924 | proto_tree_set_int(new_fi,
2925 | get_int_value(tree, tvb, start, length, encoding));
2926 | break;
2927 |
2928 | case FT_INT40:
2929 | case FT_INT48:
2930 | case FT_INT56:
2931 | case FT_INT64:
2932 | /*
2933 | * Map all non-zero values to little-endian for
2934 | * backwards compatibility.
2935 | */
2936 | if (encoding)
2937 | encoding = ENC_LITTLE_ENDIAN0x80000000;
2938 | proto_tree_set_int64(new_fi,
2939 | get_int64_value(tree, tvb, start, length, encoding));
2940 | break;
2941 |
2942 | case FT_IPv4:
2943 | /*
2944 | * Map all non-zero values to little-endian for
2945 | * backwards compatibility.
2946 | */
2947 | if (encoding)
2948 | encoding = ENC_LITTLE_ENDIAN0x80000000;
2949 | if (length != FT_IPv4_LEN4) {
2950 | length_error = length < FT_IPv4_LEN4 ? true1 : false0;
2951 | report_type_length_mismatch(tree, "an IPv4 address", length, length_error);
2952 | }
2953 | ipv4_value = tvb_get_ipv4(tvb, start);
2954 | /*
2955 | * NOTE: to support code written when
2956 | * proto_tree_add_item() took a bool as its
2957 | * last argument, with false meaning "big-endian"
2958 | * and true meaning "little-endian", we treat any
2959 | * non-zero value of "encoding" as meaning
2960 | * "little-endian".
2961 | */
2962 | proto_tree_set_ipv4(new_fi, encoding ? GUINT32_SWAP_LE_BE(ipv4_value)(((guint32) ( (((guint32) (ipv4_value) & (guint32) 0x000000ffU ) << 24) | (((guint32) (ipv4_value) & (guint32) 0x0000ff00U ) << 8) | (((guint32) (ipv4_value) & (guint32) 0x00ff0000U ) >> 8) | (((guint32) (ipv4_value) & (guint32) 0xff000000U ) >> 24)))) : ipv4_value);
2963 | break;
2964 |
2965 | case FT_IPXNET:
2966 | if (length != FT_IPXNET_LEN4) {
2967 | length_error = length < FT_IPXNET_LEN4 ? true1 : false0;
2968 | report_type_length_mismatch(tree, "an IPXNET address", length, length_error);
2969 | }
2970 | proto_tree_set_ipxnet(new_fi,
2971 | get_uint_value(tree, tvb, start, FT_IPXNET_LEN4, ENC_BIG_ENDIAN0x00000000));
2972 | break;
2973 |
2974 | case FT_IPv6:
2975 | if (length != FT_IPv6_LEN16) {
2976 | length_error = length < FT_IPv6_LEN16 ? true1 : false0;
2977 | report_type_length_mismatch(tree, "an IPv6 address", length, length_error);
2978 | }
2979 | proto_tree_set_ipv6_tvb(new_fi, tvb, start, length);
2980 | break;
2981 |
2982 | case FT_FCWWN:
2983 | if (length != FT_FCWWN_LEN8) {
2984 | length_error = length < FT_FCWWN_LEN8 ? true1 : false0;
2985 | report_type_length_mismatch(tree, "an FCWWN address", length, length_error);
2986 | }
2987 | proto_tree_set_fcwwn_tvb(new_fi, tvb, start, length);
2988 | break;
2989 |
2990 | case FT_AX25:
2991 | if (length != 7) {
2992 | length_error = length < 7 ? true1 : false0;
2993 | report_type_length_mismatch(tree, "an AX.25 address", length, length_error);
2994 | }
2995 | proto_tree_set_ax25_tvb(new_fi, tvb, start);
2996 | break;
2997 |
2998 | case FT_VINES:
2999 | if (length != VINES_ADDR_LEN6) {
3000 | length_error = length < VINES_ADDR_LEN6 ? true1 : false0;
3001 | report_type_length_mismatch(tree, "a Vines address", length, length_error);
3002 | }
3003 | proto_tree_set_vines_tvb(new_fi, tvb, start);
3004 | break;
3005 |
3006 | case FT_ETHER:
3007 | if (length != FT_ETHER_LEN6) {
3008 | length_error = length < FT_ETHER_LEN6 ? true1 : false0;
3009 | report_type_length_mismatch(tree, "a MAC address", length, length_error);
3010 | }
3011 | proto_tree_set_ether_tvb(new_fi, tvb, start);
3012 | break;
3013 |
3014 | case FT_EUI64:
3015 | /*
3016 | * Map all non-zero values to little-endian for
3017 | * backwards compatibility.
3018 | */
3019 | if (encoding)
3020 | encoding = ENC_LITTLE_ENDIAN0x80000000;
3021 | if (length != FT_EUI64_LEN8) {
3022 | length_error = length < FT_EUI64_LEN8 ? true1 : false0;
3023 | report_type_length_mismatch(tree, "an EUI-64 address", length, length_error);
3024 | }
3025 | proto_tree_set_eui64_tvb(new_fi, tvb, start, encoding);
3026 | break;
3027 | case FT_GUID:
3028 | /*
3029 | * Map all non-zero values to little-endian for
3030 | * backwards compatibility.
3031 | */
3032 | if (encoding)
3033 | encoding = ENC_LITTLE_ENDIAN0x80000000;
3034 | if (length != FT_GUID_LEN16) {
3035 | length_error = length < FT_GUID_LEN16 ? true1 : false0;
3036 | report_type_length_mismatch(tree, "a GUID", length, length_error);
3037 | }
3038 | proto_tree_set_guid_tvb(new_fi, tvb, start, encoding);
3039 | break;
3040 |
3041 | case FT_OID:
3042 | case FT_REL_OID:
3043 | proto_tree_set_oid_tvb(new_fi, tvb, start, length);
3044 | break;
3045 |
3046 | case FT_SYSTEM_ID:
3047 | proto_tree_set_system_id_tvb(new_fi, tvb, start, length);
3048 | break;
3049 |
3050 | case FT_FLOAT:
3051 | /*
3052 | * NOTE: to support code written when
3053 | * proto_tree_add_item() took a bool as its
3054 | * last argument, with false meaning "big-endian"
3055 | * and true meaning "little-endian", we treat any
3056 | * non-zero value of "encoding" as meaning
3057 | * "little-endian".
3058 | *
3059 | * At some point in the future, we might
3060 | * support non-IEEE-binary floating-point
3061 | * formats in the encoding as well
3062 | * (IEEE decimal, System/3x0, VAX).
3063 | */
3064 | if (encoding)
3065 | encoding = ENC_LITTLE_ENDIAN0x80000000;
3066 | if (length != 4) {
3067 | length_error = length < 4 ? true1 : false0;
3068 | report_type_length_mismatch(tree, "a single-precision floating point number", length, length_error);
3069 | }
3070 | if (encoding)
3071 | floatval = tvb_get_letohieee_float(tvb, start);
3072 | else
3073 | floatval = tvb_get_ntohieee_float(tvb, start);
3074 | proto_tree_set_float(new_fi, floatval);
3075 | break;
3076 |
3077 | case FT_DOUBLE:
3078 | /*
3079 | * NOTE: to support code written when
3080 | * proto_tree_add_item() took a bool as its
3081 | * last argument, with false meaning "big-endian"
3082 | * and true meaning "little-endian", we treat any
3083 | * non-zero value of "encoding" as meaning
3084 | * "little-endian".
3085 | *
3086 | * At some point in the future, we might
3087 | * support non-IEEE-binary floating-point
3088 | * formats in the encoding as well
3089 | * (IEEE decimal, System/3x0, VAX).
3090 | */
3091 | if (encoding == true1)
3092 | encoding = ENC_LITTLE_ENDIAN0x80000000;
3093 | if (length != 8) {
3094 | length_error = length < 8 ? true1 : false0;
3095 | report_type_length_mismatch(tree, "a double-precision floating point number", length, length_error);
3096 | }
3097 | if (encoding)
3098 | doubleval = tvb_get_letohieee_double(tvb, start);
3099 | else
3100 | doubleval = tvb_get_ntohieee_double(tvb, start);
3101 | proto_tree_set_double(new_fi, doubleval);
3102 | break;
3103 |
3104 | case FT_STRING:
3105 | stringval = (const char*)get_string_value(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool),
3106 | tvb, start, length, &length, encoding);
3107 | proto_tree_set_string(new_fi, stringval);
3108 |
3109 | /* Instead of calling proto_item_set_len(), since we
3110 | * don't yet have a proto_item, we set the
3111 | * field_info's length ourselves.
3112 | *
3113 | * XXX - our caller can't use that length to
3114 | * advance an offset unless they arrange that
3115 | * there always be a protocol tree into which
3116 | * we're putting this item.
3117 | */
3118 | new_fi->length = length;
3119 | break;
3120 |
3121 | case FT_STRINGZ:
3122 | stringval = (const char*)get_stringz_value(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool),
3123 | tree, tvb, start, length, &length, encoding);
3124 | proto_tree_set_string(new_fi, stringval);
3125 |
3126 | /* Instead of calling proto_item_set_len(),
3127 | * since we don't yet have a proto_item, we
3128 | * set the field_info's length ourselves.
3129 | *
3130 | * XXX - our caller can't use that length to
3131 | * advance an offset unless they arrange that
3132 | * there always be a protocol tree into which
3133 | * we're putting this item.
3134 | */
3135 | new_fi->length = length;
3136 | break;
3137 |
3138 | case FT_UINT_STRING:
3139 | /*
3140 | * NOTE: to support code written when
3141 | * proto_tree_add_item() took a bool as its
3142 | * last argument, with false meaning "big-endian"
3143 | * and true meaning "little-endian", if the
3144 | * encoding value is true, treat that as
3145 | * ASCII with a little-endian length.
3146 | *
3147 | * This won't work for code that passes
3148 | * arbitrary non-zero values; that code
3149 | * will need to be fixed.
3150 | */
3151 | if (encoding == true1)
3152 | encoding = ENC_ASCII0x00000000|ENC_LITTLE_ENDIAN0x80000000;
3153 | stringval = (const char*)get_uint_string_value(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool),
3154 | tree, tvb, start, length, &length, encoding);
3155 | proto_tree_set_string(new_fi, stringval);
3156 |
3157 | /* Instead of calling proto_item_set_len(), since we
3158 | * don't yet have a proto_item, we set the
3159 | * field_info's length ourselves.
3160 | *
3161 | * XXX - our caller can't use that length to
3162 | * advance an offset unless they arrange that
3163 | * there always be a protocol tree into which
3164 | * we're putting this item.
3165 | */
3166 | new_fi->length = length;
3167 | break;
3168 |
3169 | case FT_STRINGZPAD:
3170 | stringval = (const char*)get_stringzpad_value(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool),
3171 | tvb, start, length, &length, encoding);
3172 | proto_tree_set_string(new_fi, stringval);
3173 |
3174 | /* Instead of calling proto_item_set_len(), since we
3175 | * don't yet have a proto_item, we set the
3176 | * field_info's length ourselves.
3177 | *
3178 | * XXX - our caller can't use that length to
3179 | * advance an offset unless they arrange that
3180 | * there always be a protocol tree into which
3181 | * we're putting this item.
3182 | */
3183 | new_fi->length = length;
3184 | break;
3185 |
3186 | case FT_STRINGZTRUNC:
3187 | stringval = (const char*)get_stringztrunc_value(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool),
3188 | tvb, start, length, &length, encoding);
3189 | proto_tree_set_string(new_fi, stringval);
3190 |
3191 | /* Instead of calling proto_item_set_len(), since we
3192 | * don't yet have a proto_item, we set the
3193 | * field_info's length ourselves.
3194 | *
3195 | * XXX - our caller can't use that length to
3196 | * advance an offset unless they arrange that
3197 | * there always be a protocol tree into which
3198 | * we're putting this item.
3199 | */
3200 | new_fi->length = length;
3201 | break;
3202 |
3203 | case FT_ABSOLUTE_TIME:
3204 | /*
3205 | * Absolute times can be in any of a number of
3206 | * formats, and they can be big-endian or
3207 | * little-endian.
3208 | *
3209 | * Historically FT_TIMEs were only timespecs;
3210 | * the only question was whether they were stored
3211 | * in big- or little-endian format.
3212 | *
3213 | * For backwards compatibility, we interpret an
3214 | * encoding of 1 as meaning "little-endian timespec",
3215 | * so that passing true is interpreted as that.
3216 | */
3217 | if (encoding == true1)
3218 | encoding = ENC_TIME_SECS_NSECS0x00000000|ENC_LITTLE_ENDIAN0x80000000;
3219 |
3220 | get_time_value(tree, tvb, start, length, encoding, &time_stamp, false0);
3221 |
3222 | proto_tree_set_time(new_fi, &time_stamp);
3223 | break;
3224 |
3225 | case FT_RELATIVE_TIME:
3226 | /*
3227 | * Relative times can be in any of a number of
3228 | * formats, and they can be big-endian or
3229 | * little-endian.
3230 | *
3231 | * Historically FT_TIMEs were only timespecs;
3232 | * the only question was whether they were stored
3233 | * in big- or little-endian format.
3234 | *
3235 | * For backwards compatibility, we interpret an
3236 | * encoding of 1 as meaning "little-endian timespec",
3237 | * so that passing true is interpreted as that.
3238 | */
3239 | if (encoding == true1)
3240 | encoding = ENC_TIME_SECS_NSECS0x00000000|ENC_LITTLE_ENDIAN0x80000000;
3241 |
3242 | get_time_value(tree, tvb, start, length, encoding, &time_stamp, true1);
3243 |
3244 | proto_tree_set_time(new_fi, &time_stamp);
3245 | break;
3246 | case FT_IEEE_11073_SFLOAT:
3247 | if (encoding)
3248 | encoding = ENC_LITTLE_ENDIAN0x80000000;
3249 | if (length != 2) {
3250 | length_error = length < 2 ? true1 : false0;
3251 | report_type_length_mismatch(tree, "a IEEE 11073 SFLOAT", length, length_error);
3252 | }
3253 |
3254 | fvalue_set_uinteger(new_fi->value, tvb_get_uint16(tvb, start, encoding));
3255 |
3256 | break;
3257 | case FT_IEEE_11073_FLOAT:
3258 | if (encoding)
3259 | encoding = ENC_LITTLE_ENDIAN0x80000000;
3260 | if (length != 4) {
3261 | length_error = length < 4 ? true1 : false0;
3262 | report_type_length_mismatch(tree, "a IEEE 11073 FLOAT", length, length_error);
3263 | }
3264 | fvalue_set_uinteger(new_fi->value, tvb_get_uint32(tvb, start, encoding));
3265 |
3266 | break;
3267 | default:
3268 | REPORT_DISSECTOR_BUG("field %s is of unknown type %d (%s)",proto_report_dissector_bug("field %s is of unknown type %d (%s)" , new_fi->hfinfo->abbrev, new_fi->hfinfo->type, ftype_name (new_fi->hfinfo->type))
3269 | new_fi->hfinfo->abbrev,proto_report_dissector_bug("field %s is of unknown type %d (%s)" , new_fi->hfinfo->abbrev, new_fi->hfinfo->type, ftype_name (new_fi->hfinfo->type))
3270 | new_fi->hfinfo->type,proto_report_dissector_bug("field %s is of unknown type %d (%s)" , new_fi->hfinfo->abbrev, new_fi->hfinfo->type, ftype_name (new_fi->hfinfo->type))
3271 | ftype_name(new_fi->hfinfo->type))proto_report_dissector_bug("field %s is of unknown type %d (%s)" , new_fi->hfinfo->abbrev, new_fi->hfinfo->type, ftype_name (new_fi->hfinfo->type));
3272 | break;
3273 | }
3274 | FI_SET_FLAG(new_fi, (encoding & ENC_LITTLE_ENDIAN) ? FI_LITTLE_ENDIAN : FI_BIG_ENDIAN)do { if (new_fi) (new_fi)->flags = (new_fi)->flags | (( encoding & 0x80000000) ? 0x00000008 : 0x00000010); } while (0);
3275 |
3276 | /* Don't add new node to proto_tree until now so that any exceptions
3277 | * raised by a tvbuff access method doesn't leave junk in the proto_tree. */
3278 | /* XXX. wouldn't be better to add this item to tree, with some special
3279 | * flag (FI_EXCEPTION?) to know which item caused exception? For
3280 | * strings and bytes, we would have to set new_fi->value to something
3281 | * non-NULL, or otherwise ensure that proto_item_fill_display_label
3282 | * could handle NULL values. */
3283 | CLEANUP_POPexcept_pop(); if (0) except_cl.except_func(except_cl.except_context ); }
3284 | pi = proto_tree_add_node(tree, new_fi);
3285 |
3286 | switch (new_fi->hfinfo->type) {
3287 |
3288 | case FT_STRING:
3289 | /* XXX: trailing stray character detection should be done
3290 | * _before_ conversion to UTF-8, because conversion can change
3291 | * the length, or else get_string_length should return a value
3292 | * for the "length in bytes of the string after conversion
3293 | * including internal nulls." (Noting that we do, for other
3294 | * reasons, still need the "length in bytes in the field",
3295 | * especially for FT_STRINGZ.)
3296 | *
3297 | * This is true even for ASCII and UTF-8, because
3298 | * substituting REPLACEMENT CHARACTERS for illegal characters
3299 | * can also do so (and for UTF-8 possibly even make the
3300 | * string _shorter_).
3301 | */
3302 | detect_trailing_stray_characters(encoding, stringval, length, pi);
3303 | break;
3304 |
3305 | default:
3306 | break;
3307 | }
3308 |
3309 | return pi;
3310 | }
3311 |
3312 | proto_item *
3313 | proto_tree_add_item_ret_int(proto_tree *tree, int hfindex, tvbuff_t *tvb,
3314 | const int start, int length,
3315 | const unsigned encoding, int32_t *retval)
3316 | {
3317 | header_field_info *hfinfo;
3318 | field_info *new_fi;
3319 | int32_t value;
3320 |
3321 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 3321, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3321, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3321, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
3322 |
3323 | switch (hfinfo->type) {
3324 | case FT_INT8:
3325 | case FT_INT16:
3326 | case FT_INT24:
3327 | case FT_INT32:
3328 | break;
3329 | case FT_INT64:
3330 | REPORT_DISSECTOR_BUG("64-bit signed integer field %s used with proto_tree_add_item_ret_int()",proto_report_dissector_bug("64-bit signed integer field %s used with proto_tree_add_item_ret_int()" , hfinfo->abbrev)
3331 | hfinfo->abbrev)proto_report_dissector_bug("64-bit signed integer field %s used with proto_tree_add_item_ret_int()" , hfinfo->abbrev);
3332 | default:
3333 | REPORT_DISSECTOR_BUG("Non-signed-integer field %s used with proto_tree_add_item_ret_int()",proto_report_dissector_bug("Non-signed-integer field %s used with proto_tree_add_item_ret_int()" , hfinfo->abbrev)
3334 | hfinfo->abbrev)proto_report_dissector_bug("Non-signed-integer field %s used with proto_tree_add_item_ret_int()" , hfinfo->abbrev);
3335 | }
3336 |
3337 | CHECK_FOR_ZERO_OR_MINUS_LENGTH_AND_CLEANUP(length,if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3338 | {if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3339 | if(retval)if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3340 | {if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3341 | *retval = 0;if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3342 | }if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3343 | } )if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); };
3344 |
3345 | if (encoding & ENC_STRING0x03000000) {
3346 | REPORT_DISSECTOR_BUG("wrong encoding")proto_report_dissector_bug("wrong encoding");
3347 | }
3348 | /* I believe it's ok if this is called with a NULL tree */
3349 | value = get_int_value(tree, tvb, start, length, encoding);
3350 |
3351 | if (retval) {
3352 | int no_of_bits;
3353 | *retval = value;
3354 | if (hfinfo->bitmask) {
3355 | /* Mask out irrelevant portions */
3356 | *retval &= (uint32_t)(hfinfo->bitmask);
3357 | /* Shift bits */
3358 | *retval >>= hfinfo_bitshift(hfinfo);
3359 | }
3360 | no_of_bits = ws_count_ones(hfinfo->bitmask);
3361 | *retval = ws_sign_ext32(*retval, no_of_bits);
3362 | }
3363 |
3364 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
3365 |
3366 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3366 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3366, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3366, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3366, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
3367 |
3368 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
3369 |
3370 | proto_tree_set_int(new_fi, value);
3371 |
3372 | new_fi->flags |= (encoding & ENC_LITTLE_ENDIAN0x80000000) ? FI_LITTLE_ENDIAN0x00000008 : FI_BIG_ENDIAN0x00000010;
3373 |
3374 | return proto_tree_add_node(tree, new_fi);
3375 | }
3376 |
3377 | proto_item *
3378 | proto_tree_add_item_ret_uint(proto_tree *tree, int hfindex, tvbuff_t *tvb,
3379 | const int start, int length,
3380 | const unsigned encoding, uint32_t *retval)
3381 | {
3382 | header_field_info *hfinfo;
3383 | field_info *new_fi;
3384 | uint32_t value;
3385 |
3386 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 3386, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3386, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3386, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
3387 |
3388 | switch (hfinfo->type) {
3389 | case FT_CHAR:
3390 | case FT_UINT8:
3391 | case FT_UINT16:
3392 | case FT_UINT24:
3393 | case FT_UINT32:
3394 | break;
3395 | default:
3396 | REPORT_DISSECTOR_BUG("field %s is not of type FT_CHAR, FT_UINT8, FT_UINT16, FT_UINT24, or FT_UINT32",proto_report_dissector_bug("field %s is not of type FT_CHAR, FT_UINT8, FT_UINT16, FT_UINT24, or FT_UINT32" , hfinfo->abbrev)
3397 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_CHAR, FT_UINT8, FT_UINT16, FT_UINT24, or FT_UINT32" , hfinfo->abbrev);
3398 | }
3399 |
3400 | CHECK_FOR_ZERO_OR_MINUS_LENGTH_AND_CLEANUP(length,if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3401 | {if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3402 | if(retval)if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3403 | {if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3404 | *retval = 0;if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3405 | }if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3406 | } )if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); };
3407 |
3408 | if (encoding & ENC_STRING0x03000000) {
3409 | REPORT_DISSECTOR_BUG("wrong encoding")proto_report_dissector_bug("wrong encoding");
3410 | }
3411 | /* I believe it's ok if this is called with a NULL tree */
3412 | /* XXX - modify if we ever support EBCDIC FT_CHAR */
3413 | if (encoding & ENC_VARINT_MASK(0x00000002|0x00000004|0x00000008|0x00000010)) {
3414 | uint64_t temp64;
3415 | tvb_get_varint(tvb, start, length, &temp64, encoding);
3416 | value = (uint32_t)temp64;
3417 | } else {
3418 | value = get_uint_value(tree, tvb, start, length, encoding);
3419 | }
3420 |
3421 | if (retval) {
3422 | *retval = value;
3423 | if (hfinfo->bitmask) {
3424 | /* Mask out irrelevant portions */
3425 | *retval &= (uint32_t)(hfinfo->bitmask);
3426 | /* Shift bits */
3427 | *retval >>= hfinfo_bitshift(hfinfo);
3428 | }
3429 | }
3430 |
3431 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
3432 |
3433 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3433 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3433, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3433, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3433, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
3434 |
3435 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
3436 |
3437 | proto_tree_set_uint(new_fi, value);
3438 |
3439 | new_fi->flags |= (encoding & ENC_LITTLE_ENDIAN0x80000000) ? FI_LITTLE_ENDIAN0x00000008 : FI_BIG_ENDIAN0x00000010;
3440 | if (encoding & (ENC_VARINT_PROTOBUF0x00000002|ENC_VARINT_ZIGZAG0x00000008|ENC_VARINT_SDNV0x00000010)) {
3441 | new_fi->flags |= FI_VARINT0x00040000;
3442 | }
3443 | return proto_tree_add_node(tree, new_fi);
3444 | }
3445 |
3446 | /* Gets data from tvbuff, adds it to proto_tree, increments offset,
3447 | * and returns proto_item* and uint value retrieved*/
3448 | proto_item *
3449 | ptvcursor_add_ret_uint(ptvcursor_t *ptvc, int hfindex, int length,
3450 | const unsigned encoding, uint32_t *retval)
3451 | {
3452 | field_info *new_fi;
3453 | header_field_info *hfinfo;
3454 | int item_length;
3455 | int offset;
3456 | uint32_t value;
3457 |
3458 | offset = ptvc->offset;
3459 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 3459, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3459, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3459, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
3460 |
3461 | switch (hfinfo->type) {
3462 | case FT_CHAR:
3463 | case FT_UINT8:
3464 | case FT_UINT16:
3465 | case FT_UINT24:
3466 | case FT_UINT32:
3467 | break;
3468 | default:
3469 | REPORT_DISSECTOR_BUG("field %s is not of type FT_CHAR, FT_UINT8, FT_UINT16, FT_UINT24, or FT_UINT32",proto_report_dissector_bug("field %s is not of type FT_CHAR, FT_UINT8, FT_UINT16, FT_UINT24, or FT_UINT32" , hfinfo->abbrev)
3470 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_CHAR, FT_UINT8, FT_UINT16, FT_UINT24, or FT_UINT32" , hfinfo->abbrev);
3471 | }
3472 |
3473 | get_hfi_length(hfinfo, ptvc->tvb, offset, &length, &item_length, encoding);
3474 | test_length(hfinfo, ptvc->tvb, offset, item_length, encoding);
3475 |
3476 | /* I believe it's ok if this is called with a NULL tree */
3477 | /* XXX - modify if we ever support EBCDIC FT_CHAR */
3478 | value = get_uint_value(ptvc->tree, ptvc->tvb, offset, item_length, encoding);
3479 |
3480 | if (retval) {
3481 | *retval = value;
3482 | if (hfinfo->bitmask) {
3483 | /* Mask out irrelevant portions */
3484 | *retval &= (uint32_t)(hfinfo->bitmask);
3485 | /* Shift bits */
3486 | *retval >>= hfinfo_bitshift(hfinfo);
3487 | }
3488 | }
3489 |
3490 | ptvcursor_advance(ptvc, get_full_length(hfinfo, ptvc->tvb, offset, length, item_length, encoding));
3491 |
3492 | CHECK_FOR_NULL_TREE(ptvc->tree)if (!ptvc->tree) { ((void)0); return ((void*)0); };
3493 |
3494 | /* Coast clear. Try and fake it */
3495 | TRY_TO_FAKE_THIS_ITEM(ptvc->tree, hfindex, hfinfo)((ptvc->tree)->tree_data)->count++; if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3495 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3495, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3495, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((ptvc->tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3495, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((ptvc->tree )->tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((ptvc->tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((ptvc ->tree)->tree_data)->visible)) { if (proto_item_is_hidden ((ptvc->tree))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT ) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo->type != FT_PROTOCOL || ((ptvc->tree)->tree_data )->fake_protocols)) { ((void)0); return proto_tree_add_fake_node (ptvc->tree, hfinfo); } } };
3496 |
3497 | new_fi = new_field_info(ptvc->tree, hfinfo, ptvc->tvb, offset, item_length);
3498 |
3499 | return proto_tree_new_item(new_fi, ptvc->tree, ptvc->tvb,
3500 | offset, length, encoding);
3501 | }
3502 |
3503 | /* Gets data from tvbuff, adds it to proto_tree, increments offset,
3504 | * and returns proto_item* and int value retrieved*/
3505 | proto_item *
3506 | ptvcursor_add_ret_int(ptvcursor_t *ptvc, int hfindex, int length,
3507 | const unsigned encoding, int32_t *retval)
3508 | {
3509 | field_info *new_fi;
3510 | header_field_info *hfinfo;
3511 | int item_length;
3512 | int offset;
3513 | uint32_t value;
3514 |
3515 | offset = ptvc->offset;
3516 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 3516, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3516, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3516, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
3517 |
3518 | switch (hfinfo->type) {
3519 | case FT_INT8:
3520 | case FT_INT16:
3521 | case FT_INT24:
3522 | case FT_INT32:
3523 | break;
3524 | default:
3525 | REPORT_DISSECTOR_BUG("field %s is not of type FT_INT8, FT_INT16, FT_INT24, or FT_INT32",proto_report_dissector_bug("field %s is not of type FT_INT8, FT_INT16, FT_INT24, or FT_INT32" , hfinfo->abbrev)
3526 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_INT8, FT_INT16, FT_INT24, or FT_INT32" , hfinfo->abbrev);
3527 | }
3528 |
3529 | get_hfi_length(hfinfo, ptvc->tvb, offset, &length, &item_length, encoding);
3530 | test_length(hfinfo, ptvc->tvb, offset, item_length, encoding);
3531 |
3532 | /* I believe it's ok if this is called with a NULL tree */
3533 | /* XXX - modify if we ever support EBCDIC FT_CHAR */
3534 | value = get_int_value(ptvc->tree, ptvc->tvb, offset, item_length, encoding);
3535 |
3536 | if (retval) {
3537 | int no_of_bits;
3538 | *retval = value;
3539 | if (hfinfo->bitmask) {
3540 | /* Mask out irrelevant portions */
3541 | *retval &= (uint32_t)(hfinfo->bitmask);
3542 | /* Shift bits */
3543 | *retval >>= hfinfo_bitshift(hfinfo);
3544 | }
3545 | no_of_bits = ws_count_ones(hfinfo->bitmask);
3546 | *retval = ws_sign_ext32(*retval, no_of_bits);
3547 | }
3548 |
3549 | ptvcursor_advance(ptvc, get_full_length(hfinfo, ptvc->tvb, offset, length, item_length, encoding));
3550 |
3551 | CHECK_FOR_NULL_TREE(ptvc->tree)if (!ptvc->tree) { ((void)0); return ((void*)0); };
3552 |
3553 | /* Coast clear. Try and fake it */
3554 | TRY_TO_FAKE_THIS_ITEM(ptvc->tree, hfindex, hfinfo)((ptvc->tree)->tree_data)->count++; if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3554 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3554, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3554, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((ptvc->tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3554, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((ptvc->tree )->tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((ptvc->tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((ptvc ->tree)->tree_data)->visible)) { if (proto_item_is_hidden ((ptvc->tree))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT ) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo->type != FT_PROTOCOL || ((ptvc->tree)->tree_data )->fake_protocols)) { ((void)0); return proto_tree_add_fake_node (ptvc->tree, hfinfo); } } };
3555 |
3556 | new_fi = new_field_info(ptvc->tree, hfinfo, ptvc->tvb, offset, item_length);
3557 |
3558 | return proto_tree_new_item(new_fi, ptvc->tree, ptvc->tvb,
3559 | offset, length, encoding);
3560 | }
3561 |
3562 | /* Gets data from tvbuff, adds it to proto_tree, increments offset,
3563 | * and returns proto_item* and string value retrieved */
3564 | proto_item*
3565 | ptvcursor_add_ret_string(ptvcursor_t* ptvc, int hf, int length, const unsigned encoding, wmem_allocator_t *scope, const uint8_t **retval)
3566 | {
3567 | header_field_info *hfinfo;
3568 | field_info *new_fi;
3569 | const uint8_t *value;
3570 | int item_length;
3571 | int offset;
3572 |
3573 | offset = ptvc->offset;
3574 |
3575 | PROTO_REGISTRAR_GET_NTH(hf, hfinfo)if((hf == 0 || (unsigned)hf > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3575 , __func__, "Unregistered hf! index=%d", hf); ((void) ((hf > 0 && (unsigned)hf < gpa_hfinfo.len) ? (void)0 : ( proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3575, "hf > 0 && (unsigned)hf < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hf] != (( void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3575, "gpa_hfinfo.hfi[hf] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[hf];;
3576 |
3577 | switch (hfinfo->type) {
3578 | case FT_STRING:
3579 | value = get_string_value(scope, ptvc->tvb, offset, length, &item_length, encoding);
3580 | break;
3581 | case FT_STRINGZ:
3582 | value = get_stringz_value(scope, ptvc->tree, ptvc->tvb, offset, length, &item_length, encoding);
3583 | break;
3584 | case FT_UINT_STRING:
3585 | value = get_uint_string_value(scope, ptvc->tree, ptvc->tvb, offset, length, &item_length, encoding);
3586 | break;
3587 | case FT_STRINGZPAD:
3588 | value = get_stringzpad_value(scope, ptvc->tvb, offset, length, &item_length, encoding);
3589 | break;
3590 | case FT_STRINGZTRUNC:
3591 | value = get_stringztrunc_value(scope, ptvc->tvb, offset, length, &item_length, encoding);
3592 | break;
3593 | default:
3594 | REPORT_DISSECTOR_BUG("field %s is not of type FT_STRING, FT_STRINGZ, FT_UINT_STRING, FT_STRINGZPAD, or FT_STRINGZTRUNC",proto_report_dissector_bug("field %s is not of type FT_STRING, FT_STRINGZ, FT_UINT_STRING, FT_STRINGZPAD, or FT_STRINGZTRUNC" , hfinfo->abbrev)
3595 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_STRING, FT_STRINGZ, FT_UINT_STRING, FT_STRINGZPAD, or FT_STRINGZTRUNC" , hfinfo->abbrev);
3596 | }
3597 |
3598 | if (retval)
3599 | *retval = value;
3600 |
3601 | ptvcursor_advance(ptvc, item_length);
3602 |
3603 | CHECK_FOR_NULL_TREE(ptvc->tree)if (!ptvc->tree) { ((void)0); return ((void*)0); };
3604 |
3605 | TRY_TO_FAKE_THIS_ITEM(ptvc->tree, hfinfo->id, hfinfo)((ptvc->tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 3605, __func__, "Unregistered hf! index=%d" , hfinfo->id); ((void) ((hfinfo->id > 0 && ( unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3605, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3605, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((ptvc->tree)->tree_data)->count > prefs .gui_max_tree_items) { ((void)0); if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3605 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((ptvc->tree )->tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((ptvc->tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((ptvc ->tree)->tree_data)->visible)) { if (proto_item_is_hidden ((ptvc->tree))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT ) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo->type != FT_PROTOCOL || ((ptvc->tree)->tree_data )->fake_protocols)) { ((void)0); return proto_tree_add_fake_node (ptvc->tree, hfinfo); } } };
3606 |
3607 | new_fi = new_field_info(ptvc->tree, hfinfo, ptvc->tvb, offset, item_length);
3608 |
3609 | return proto_tree_new_item(new_fi, ptvc->tree, ptvc->tvb,
3610 | offset, length, encoding);
3611 | }
3612 |
3613 | /* Gets data from tvbuff, adds it to proto_tree, increments offset,
3614 | * and returns proto_item* and boolean value retrieved */
3615 | proto_item*
3616 | ptvcursor_add_ret_boolean(ptvcursor_t* ptvc, int hfindex, int length, const unsigned encoding, bool_Bool *retval)
3617 | {
3618 | header_field_info *hfinfo;
3619 | field_info *new_fi;
3620 | int item_length;
3621 | int offset;
3622 | uint64_t value, bitval;
3623 |
3624 | offset = ptvc->offset;
3625 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 3625, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3625, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3625, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
3626 |
3627 | if (hfinfo->type != FT_BOOLEAN) {
3628 | REPORT_DISSECTOR_BUG("field %s is not of type FT_BOOLEAN",proto_report_dissector_bug("field %s is not of type FT_BOOLEAN" , hfinfo->abbrev)
3629 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_BOOLEAN" , hfinfo->abbrev);
3630 | }
3631 |
3632 | CHECK_FOR_ZERO_OR_MINUS_LENGTH_AND_CLEANUP(length,if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3633 | {if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3634 | if(retval)if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3635 | {if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3636 | *retval = false;if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3637 | }if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3638 | } )if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); };
3639 |
3640 | if (encoding & ENC_STRING0x03000000) {
3641 | REPORT_DISSECTOR_BUG("wrong encoding")proto_report_dissector_bug("wrong encoding");
3642 | }
3643 |
3644 | get_hfi_length(hfinfo, ptvc->tvb, offset, &length, &item_length, encoding);
3645 | test_length(hfinfo, ptvc->tvb, offset, item_length, encoding);
3646 |
3647 | /* I believe it's ok if this is called with a NULL tree */
3648 | value = get_uint64_value(ptvc->tree, ptvc->tvb, offset, length, encoding);
3649 |
3650 | if (retval) {
3651 | bitval = value;
3652 | if (hfinfo->bitmask) {
3653 | /* Mask out irrelevant portions */
3654 | bitval &= hfinfo->bitmask;
3655 | }
3656 | *retval = (bitval != 0);
3657 | }
3658 |
3659 | ptvcursor_advance(ptvc, get_full_length(hfinfo, ptvc->tvb, offset, length, item_length, encoding));
3660 |
3661 | CHECK_FOR_NULL_TREE(ptvc->tree)if (!ptvc->tree) { ((void)0); return ((void*)0); };
3662 |
3663 | TRY_TO_FAKE_THIS_ITEM(ptvc->tree, hfinfo->id, hfinfo)((ptvc->tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 3663, __func__, "Unregistered hf! index=%d" , hfinfo->id); ((void) ((hfinfo->id > 0 && ( unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3663, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3663, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((ptvc->tree)->tree_data)->count > prefs .gui_max_tree_items) { ((void)0); if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3663 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((ptvc->tree )->tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((ptvc->tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((ptvc ->tree)->tree_data)->visible)) { if (proto_item_is_hidden ((ptvc->tree))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT ) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo->type != FT_PROTOCOL || ((ptvc->tree)->tree_data )->fake_protocols)) { ((void)0); return proto_tree_add_fake_node (ptvc->tree, hfinfo); } } };
3664 |
3665 | new_fi = new_field_info(ptvc->tree, hfinfo, ptvc->tvb, offset, item_length);
3666 |
3667 | return proto_tree_new_item(new_fi, ptvc->tree, ptvc->tvb,
3668 | offset, length, encoding);
3669 | }
3670 |
3671 | proto_item *
3672 | proto_tree_add_item_ret_uint64(proto_tree *tree, int hfindex, tvbuff_t *tvb,
3673 | const int start, int length, const unsigned encoding, uint64_t *retval)
3674 | {
3675 | header_field_info *hfinfo;
3676 | field_info *new_fi;
3677 | uint64_t value;
3678 |
3679 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 3679, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3679, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3679, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
3680 |
3681 | switch (hfinfo->type) {
3682 | case FT_UINT40:
3683 | case FT_UINT48:
3684 | case FT_UINT56:
3685 | case FT_UINT64:
3686 | break;
3687 | default:
3688 | REPORT_DISSECTOR_BUG("field %s is not of type FT_UINT40, FT_UINT48, FT_UINT56, or FT_UINT64",proto_report_dissector_bug("field %s is not of type FT_UINT40, FT_UINT48, FT_UINT56, or FT_UINT64" , hfinfo->abbrev)
3689 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_UINT40, FT_UINT48, FT_UINT56, or FT_UINT64" , hfinfo->abbrev);
3690 | }
3691 |
3692 | CHECK_FOR_ZERO_OR_MINUS_LENGTH_AND_CLEANUP(length,if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3693 | {if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3694 | if(retval)if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3695 | {if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3696 | *retval = 0;if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3697 | }if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3698 | } )if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); };
3699 |
3700 | if (encoding & ENC_STRING0x03000000) {
3701 | REPORT_DISSECTOR_BUG("wrong encoding")proto_report_dissector_bug("wrong encoding");
3702 | }
3703 | /* I believe it's ok if this is called with a NULL tree */
3704 | if (encoding & ENC_VARINT_MASK(0x00000002|0x00000004|0x00000008|0x00000010)) {
3705 | tvb_get_varint(tvb, start, length, &value, encoding);
3706 | } else {
3707 | value = get_uint64_value(tree, tvb, start, length, encoding);
3708 | }
3709 |
3710 | if (retval) {
3711 | *retval = value;
3712 | if (hfinfo->bitmask) {
3713 | /* Mask out irrelevant portions */
3714 | *retval &= hfinfo->bitmask;
3715 | /* Shift bits */
3716 | *retval >>= hfinfo_bitshift(hfinfo);
3717 | }
3718 | }
3719 |
3720 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
3721 |
3722 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3722 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3722, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3722, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3722, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
3723 |
3724 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
3725 |
3726 | proto_tree_set_uint64(new_fi, value);
3727 |
3728 | new_fi->flags |= (encoding & ENC_LITTLE_ENDIAN0x80000000) ? FI_LITTLE_ENDIAN0x00000008 : FI_BIG_ENDIAN0x00000010;
3729 | if (encoding & (ENC_VARINT_PROTOBUF0x00000002|ENC_VARINT_ZIGZAG0x00000008|ENC_VARINT_SDNV0x00000010)) {
3730 | new_fi->flags |= FI_VARINT0x00040000;
3731 | }
3732 |
3733 | return proto_tree_add_node(tree, new_fi);
3734 | }
3735 |
3736 | proto_item *
3737 | proto_tree_add_item_ret_int64(proto_tree *tree, int hfindex, tvbuff_t *tvb,
3738 | const int start, int length, const unsigned encoding, int64_t *retval)
3739 | {
3740 | header_field_info *hfinfo;
3741 | field_info *new_fi;
3742 | int64_t value;
3743 |
3744 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 3744, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3744, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3744, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
3745 |
3746 | switch (hfinfo->type) {
3747 | case FT_INT40:
3748 | case FT_INT48:
3749 | case FT_INT56:
3750 | case FT_INT64:
3751 | break;
3752 | default:
3753 | REPORT_DISSECTOR_BUG("field %s is not of type FT_INT40, FT_INT48, FT_INT56, or FT_INT64",proto_report_dissector_bug("field %s is not of type FT_INT40, FT_INT48, FT_INT56, or FT_INT64" , hfinfo->abbrev)
3754 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_INT40, FT_INT48, FT_INT56, or FT_INT64" , hfinfo->abbrev);
3755 | }
3756 |
3757 | CHECK_FOR_ZERO_OR_MINUS_LENGTH_AND_CLEANUP(length,if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3758 | {if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3759 | if(retval)if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3760 | {if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3761 | *retval = 0;if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3762 | }if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3763 | } )if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); };
3764 |
3765 | if (encoding & ENC_STRING0x03000000) {
3766 | REPORT_DISSECTOR_BUG("wrong encoding")proto_report_dissector_bug("wrong encoding");
3767 | }
3768 | /* I believe it's ok if this is called with a NULL tree */
3769 | if (encoding & ENC_VARINT_MASK(0x00000002|0x00000004|0x00000008|0x00000010)) {
3770 | tvb_get_varint(tvb, start, length, (uint64_t*)&value, encoding);
3771 | }
3772 | else {
3773 | value = get_int64_value(tree, tvb, start, length, encoding);
3774 | }
3775 |
3776 | if (retval) {
3777 | *retval = value;
3778 | }
3779 |
3780 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
3781 |
3782 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3782 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3782, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3782, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3782, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
3783 |
3784 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
3785 |
3786 | proto_tree_set_int64(new_fi, value);
3787 |
3788 | new_fi->flags |= (encoding & ENC_LITTLE_ENDIAN0x80000000) ? FI_LITTLE_ENDIAN0x00000008 : FI_BIG_ENDIAN0x00000010;
3789 | if (encoding & (ENC_VARINT_PROTOBUF0x00000002|ENC_VARINT_ZIGZAG0x00000008|ENC_VARINT_SDNV0x00000010)) {
3790 | new_fi->flags |= FI_VARINT0x00040000;
3791 | }
3792 |
3793 | return proto_tree_add_node(tree, new_fi);
3794 | }
3795 |
3796 | proto_item *
3797 | proto_tree_add_item_ret_varint(proto_tree *tree, int hfindex, tvbuff_t *tvb,
3798 | const int start, int length, const unsigned encoding, uint64_t *retval, int *lenretval)
3799 | {
3800 | header_field_info *hfinfo;
3801 | field_info *new_fi;
3802 | uint64_t value;
3803 |
3804 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 3804, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3804, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3804, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
3805 |
3806 | if ((!FT_IS_INT(hfinfo->type)(((hfinfo->type) == FT_INT8 || (hfinfo->type) == FT_INT16 || (hfinfo->type) == FT_INT24 || (hfinfo->type) == FT_INT32 ) || ((hfinfo->type) == FT_INT40 || (hfinfo->type) == FT_INT48 || (hfinfo->type) == FT_INT56 || (hfinfo->type) == FT_INT64 ))) && (!FT_IS_UINT(hfinfo->type)(((hfinfo->type) == FT_CHAR || (hfinfo->type) == FT_UINT8 || (hfinfo->type) == FT_UINT16 || (hfinfo->type) == FT_UINT24 || (hfinfo->type) == FT_UINT32 || (hfinfo->type) == FT_FRAMENUM ) || ((hfinfo->type) == FT_UINT40 || (hfinfo->type) == FT_UINT48 || (hfinfo->type) == FT_UINT56 || (hfinfo->type) == FT_UINT64 )))) {
3807 | REPORT_DISSECTOR_BUG("field %s is not of type FT_UINT or FT_INT",proto_report_dissector_bug("field %s is not of type FT_UINT or FT_INT" , hfinfo->abbrev)
3808 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_UINT or FT_INT" , hfinfo->abbrev);
3809 | }
3810 |
3811 | /* length validation for native number encoding caught by get_uint64_value() */
3812 | /* length has to be -1 or > 0 regardless of encoding */
3813 | if (length == 0)
3814 | REPORT_DISSECTOR_BUG("Invalid length %d passed to proto_tree_add_item_ret_varint",proto_report_dissector_bug("Invalid length %d passed to proto_tree_add_item_ret_varint" , length)
3815 | length)proto_report_dissector_bug("Invalid length %d passed to proto_tree_add_item_ret_varint" , length);
3816 |
3817 | if (encoding & ENC_STRING0x03000000) {
3818 | REPORT_DISSECTOR_BUG("wrong encoding")proto_report_dissector_bug("wrong encoding");
3819 | }
3820 |
3821 | length = tvb_get_varint(tvb, start, (length == -1) ? FT_VARINT_MAX_LEN10 : length, &value, encoding);
3822 |
3823 | if (retval) {
3824 | *retval = value;
3825 | if (hfinfo->bitmask) {
3826 | /* Mask out irrelevant portions */
3827 | *retval &= hfinfo->bitmask;
3828 | /* Shift bits */
3829 | *retval >>= hfinfo_bitshift(hfinfo);
3830 | }
3831 | }
3832 |
3833 | if (lenretval) {
3834 | *lenretval = length;
3835 | }
3836 |
3837 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
3838 |
3839 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3839 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3839, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3839, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3839, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
3840 |
3841 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
3842 |
3843 | proto_tree_set_uint64(new_fi, value);
3844 |
3845 | new_fi->flags |= (encoding & ENC_LITTLE_ENDIAN0x80000000) ? FI_LITTLE_ENDIAN0x00000008 : FI_BIG_ENDIAN0x00000010;
3846 | if (encoding & (ENC_VARINT_PROTOBUF0x00000002|ENC_VARINT_ZIGZAG0x00000008|ENC_VARINT_SDNV0x00000010)) {
3847 | new_fi->flags |= FI_VARINT0x00040000;
3848 | }
3849 |
3850 | return proto_tree_add_node(tree, new_fi);
3851 |
3852 | }
3853 |
3854 | proto_item *
3855 | proto_tree_add_item_ret_boolean(proto_tree *tree, int hfindex, tvbuff_t *tvb,
3856 | const int start, int length,
3857 | const unsigned encoding, bool_Bool *retval)
3858 | {
3859 | header_field_info *hfinfo;
3860 | field_info *new_fi;
3861 | uint64_t value, bitval;
3862 |
3863 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 3863, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3863, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3863, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
3864 |
3865 | if (hfinfo->type != FT_BOOLEAN) {
3866 | REPORT_DISSECTOR_BUG("field %s is not of type FT_BOOLEAN",proto_report_dissector_bug("field %s is not of type FT_BOOLEAN" , hfinfo->abbrev)
3867 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_BOOLEAN" , hfinfo->abbrev);
3868 | }
3869 |
3870 | CHECK_FOR_ZERO_OR_MINUS_LENGTH_AND_CLEANUP(length,if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3871 | {if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3872 | if(retval)if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3873 | {if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3874 | *retval = false;if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3875 | }if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); }
3876 | } )if (length < -1 || length == 0 ) { { if(retval) { *retval = 0; } }; return ((void*)0); };
3877 |
3878 | if (encoding & ENC_STRING0x03000000) {
3879 | REPORT_DISSECTOR_BUG("wrong encoding")proto_report_dissector_bug("wrong encoding");
3880 | }
3881 | /* I believe it's ok if this is called with a NULL tree */
3882 | value = get_uint64_value(tree, tvb, start, length, encoding);
3883 |
3884 | if (retval) {
3885 | bitval = value;
3886 | if (hfinfo->bitmask) {
3887 | /* Mask out irrelevant portions */
3888 | bitval &= hfinfo->bitmask;
3889 | }
3890 | *retval = (bitval != 0);
3891 | }
3892 |
3893 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
3894 |
3895 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3895 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3895, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3895, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3895, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
3896 |
3897 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
3898 |
3899 | proto_tree_set_boolean(new_fi, value);
3900 |
3901 | new_fi->flags |= (encoding & ENC_LITTLE_ENDIAN0x80000000) ? FI_LITTLE_ENDIAN0x00000008 : FI_BIG_ENDIAN0x00000010;
3902 |
3903 | return proto_tree_add_node(tree, new_fi);
3904 | }
3905 |
3906 | proto_item *
3907 | proto_tree_add_item_ret_float(proto_tree *tree, int hfindex, tvbuff_t *tvb,
3908 | const int start, int length,
3909 | const unsigned encoding, float *retval)
3910 | {
3911 | header_field_info *hfinfo = proto_registrar_get_nth(hfindex);
3912 | field_info *new_fi;
3913 | float value;
3914 |
3915 | DISSECTOR_ASSERT_HINT(hfinfo != NULL, "Not passed hfi!")((void) ((hfinfo != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3915, "hfinfo != ((void*)0)", "Not passed hfi!"))));
3916 |
3917 | if (hfinfo->type != FT_FLOAT) {
3918 | REPORT_DISSECTOR_BUG("field %s is not of type FT_FLOAT", hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_FLOAT" , hfinfo->abbrev);
3919 | }
3920 |
3921 | if (length != 4) {
3922 | report_type_length_mismatch(tree, "a single-precision floating point number", length, true1);
3923 | }
3924 |
3925 | /* treat any nonzero encoding as little endian for backwards compatibility */
3926 | value = encoding ? tvb_get_letohieee_float(tvb, start) : tvb_get_ntohieee_float(tvb, start);
3927 | if (retval) {
3928 | *retval = value;
3929 | }
3930 |
3931 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
3932 |
3933 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3933 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3933, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3933, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3933, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
3934 |
3935 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
3936 | if (encoding) {
3937 | new_fi->flags |= FI_LITTLE_ENDIAN0x00000008;
3938 | }
3939 |
3940 | proto_tree_set_float(new_fi, value);
3941 |
3942 | return proto_tree_add_node(tree, new_fi);
3943 | }
3944 |
3945 | proto_item *
3946 | proto_tree_add_item_ret_double(proto_tree *tree, int hfindex, tvbuff_t *tvb,
3947 | const int start, int length,
3948 | const unsigned encoding, double *retval)
3949 | {
3950 | header_field_info *hfinfo = proto_registrar_get_nth(hfindex);
3951 | field_info *new_fi;
3952 | double value;
3953 |
3954 | DISSECTOR_ASSERT_HINT(hfinfo != NULL, "Not passed hfi!")((void) ((hfinfo != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3954, "hfinfo != ((void*)0)", "Not passed hfi!"))));
3955 |
3956 | if (hfinfo->type != FT_DOUBLE) {
3957 | REPORT_DISSECTOR_BUG("field %s is not of type FT_DOUBLE", hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_DOUBLE" , hfinfo->abbrev);
3958 | }
3959 |
3960 | if (length != 8) {
3961 | report_type_length_mismatch(tree, "a double-precision floating point number", length, true1);
3962 | }
3963 |
3964 | /* treat any nonzero encoding as little endian for backwards compatibility */
3965 | value = encoding ? tvb_get_letohieee_double(tvb, start) : tvb_get_ntohieee_double(tvb, start);
3966 | if (retval) {
3967 | *retval = value;
3968 | }
3969 |
3970 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
3971 |
3972 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3972 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3972, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3972, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 3972, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
3973 |
3974 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
3975 | if (encoding) {
3976 | new_fi->flags |= FI_LITTLE_ENDIAN0x00000008;
3977 | }
3978 |
3979 | proto_tree_set_double(new_fi, value);
3980 |
3981 | return proto_tree_add_node(tree, new_fi);
3982 | }
3983 |
3984 | proto_item *
3985 | proto_tree_add_item_ret_ipv4(proto_tree *tree, int hfindex, tvbuff_t *tvb,
3986 | const int start, int length,
3987 | const unsigned encoding, ws_in4_addr *retval)
3988 | {
3989 | header_field_info *hfinfo;
3990 | field_info *new_fi;
3991 | ws_in4_addr value;
3992 |
3993 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 3993, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 3993, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 3993, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
3994 |
3995 | switch (hfinfo->type) {
3996 | case FT_IPv4:
3997 | break;
3998 | default:
3999 | REPORT_DISSECTOR_BUG("field %s is not of type FT_IPv4",proto_report_dissector_bug("field %s is not of type FT_IPv4", hfinfo->abbrev)
4000 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_IPv4", hfinfo->abbrev);
4001 | }
4002 |
4003 | if (length != FT_IPv4_LEN4)
4004 | REPORT_DISSECTOR_BUG("Invalid length %d passed to proto_tree_add_item_ret_ipv4",proto_report_dissector_bug("Invalid length %d passed to proto_tree_add_item_ret_ipv4" , length)
4005 | length)proto_report_dissector_bug("Invalid length %d passed to proto_tree_add_item_ret_ipv4" , length);
4006 |
4007 | if (encoding & (ENC_STRING0x03000000 | ENC_VARINT_MASK(0x00000002|0x00000004|0x00000008|0x00000010))) {
4008 | REPORT_DISSECTOR_BUG("wrong encoding")proto_report_dissector_bug("wrong encoding");
4009 | }
4010 |
4011 | /*
4012 | * NOTE: to support code written when proto_tree_add_item() took
4013 | * a bool as its last argument, with false meaning "big-endian"
4014 | * and true meaning "little-endian", we treat any non-zero value
4015 | * of "encoding" as meaning "little-endian".
4016 | */
4017 | value = tvb_get_ipv4(tvb, start);
4018 | if (encoding)
4019 | value = GUINT32_SWAP_LE_BE(value)(((guint32) ( (((guint32) (value) & (guint32) 0x000000ffU ) << 24) | (((guint32) (value) & (guint32) 0x0000ff00U ) << 8) | (((guint32) (value) & (guint32) 0x00ff0000U ) >> 8) | (((guint32) (value) & (guint32) 0xff000000U ) >> 24))));
4020 |
4021 | if (retval) {
4022 | *retval = value;
4023 | }
4024 |
4025 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4026 |
4027 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4027 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4027, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4027, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4027, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4028 |
4029 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
4030 |
4031 | proto_tree_set_ipv4(new_fi, value);
4032 |
4033 | new_fi->flags |= encoding ? FI_LITTLE_ENDIAN0x00000008 : FI_BIG_ENDIAN0x00000010;
4034 | return proto_tree_add_node(tree, new_fi);
4035 | }
4036 |
4037 | proto_item *
4038 | proto_tree_add_item_ret_ipv6(proto_tree *tree, int hfindex, tvbuff_t *tvb,
4039 | const int start, int length,
4040 | const unsigned encoding, ws_in6_addr *addr)
4041 | {
4042 | header_field_info *hfinfo = proto_registrar_get_nth(hfindex);
4043 | field_info *new_fi;
4044 |
4045 | DISSECTOR_ASSERT_HINT(hfinfo != NULL, "Not passed hfi!")((void) ((hfinfo != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4045, "hfinfo != ((void*)0)", "Not passed hfi!"))));
4046 |
4047 | switch (hfinfo->type) {
4048 | case FT_IPv6:
4049 | break;
4050 | default:
4051 | REPORT_DISSECTOR_BUG("field %s is not of type FT_IPv6",proto_report_dissector_bug("field %s is not of type FT_IPv6", hfinfo->abbrev)
4052 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_IPv6", hfinfo->abbrev);
4053 | }
4054 |
4055 | if (length != FT_IPv6_LEN16)
4056 | REPORT_DISSECTOR_BUG("Invalid length %d passed to proto_tree_add_item_ret_ipv6",proto_report_dissector_bug("Invalid length %d passed to proto_tree_add_item_ret_ipv6" , length)
4057 | length)proto_report_dissector_bug("Invalid length %d passed to proto_tree_add_item_ret_ipv6" , length);
4058 |
4059 | if (encoding) {
4060 | REPORT_DISSECTOR_BUG("Encodings not yet implemented for proto_tree_add_item_ret_ipv6")proto_report_dissector_bug("Encodings not yet implemented for proto_tree_add_item_ret_ipv6" );
4061 | }
4062 |
4063 | tvb_get_ipv6(tvb, start, addr);
4064 |
4065 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4066 |
4067 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4067 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4067, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4067, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4067, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4068 |
4069 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
4070 |
4071 | proto_tree_set_ipv6(new_fi, addr);
4072 |
4073 | return proto_tree_add_node(tree, new_fi);
4074 | }
4075 |
4076 | proto_item *
4077 | proto_tree_add_item_ret_ether(proto_tree *tree, int hfindex, tvbuff_t *tvb,
4078 | const int start, int length, const unsigned encoding, uint8_t *retval) {
4079 |
4080 | header_field_info *hfinfo = proto_registrar_get_nth(hfindex);
4081 | field_info *new_fi;
4082 |
4083 | DISSECTOR_ASSERT_HINT(hfinfo != NULL, "Not passed hfi!")((void) ((hfinfo != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4083, "hfinfo != ((void*)0)", "Not passed hfi!"))));
4084 |
4085 | switch (hfinfo->type) {
4086 | case FT_ETHER:
4087 | break;
4088 | default:
4089 | REPORT_DISSECTOR_BUG("field %s is not of type FT_ETHER",proto_report_dissector_bug("field %s is not of type FT_ETHER" , hfinfo->abbrev)
4090 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_ETHER" , hfinfo->abbrev);
4091 | }
4092 |
4093 | if (length != FT_ETHER_LEN6)
4094 | REPORT_DISSECTOR_BUG("Invalid length %d passed to proto_tree_add_item_ret_ether",proto_report_dissector_bug("Invalid length %d passed to proto_tree_add_item_ret_ether" , length)
4095 | length)proto_report_dissector_bug("Invalid length %d passed to proto_tree_add_item_ret_ether" , length);
4096 |
4097 | if (encoding) {
4098 | REPORT_DISSECTOR_BUG("Encodings not yet implemented for proto_tree_add_item_ret_ether")proto_report_dissector_bug("Encodings not yet implemented for proto_tree_add_item_ret_ether" );
4099 | }
4100 |
4101 | tvb_memcpy(tvb, retval, start, length);
4102 |
4103 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4104 |
4105 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4105 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4105, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4105, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4105, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4106 |
4107 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
4108 |
4109 | proto_tree_set_ether(new_fi, retval);
4110 |
4111 | return proto_tree_add_node(tree, new_fi);
4112 | }
4113 |
4114 |
4115 | proto_item *
4116 | proto_tree_add_item_ret_string_and_length(proto_tree *tree, int hfindex,
4117 | tvbuff_t *tvb,
4118 | const int start, int length,
4119 | const unsigned encoding,
4120 | wmem_allocator_t *scope,
4121 | const uint8_t **retval,
4122 | int *lenretval)
4123 | {
4124 | proto_item *pi;
4125 | header_field_info *hfinfo;
4126 | field_info *new_fi;
4127 | const uint8_t *value;
4128 |
4129 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4129, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4129, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4129, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
4130 |
4131 | switch (hfinfo->type) {
4132 | case FT_STRING:
4133 | value = get_string_value(scope, tvb, start, length, lenretval, encoding);
4134 | break;
4135 | case FT_STRINGZ:
4136 | value = get_stringz_value(scope, tree, tvb, start, length, lenretval, encoding);
4137 | break;
4138 | case FT_UINT_STRING:
4139 | value = get_uint_string_value(scope, tree, tvb, start, length, lenretval, encoding);
4140 | break;
4141 | case FT_STRINGZPAD:
4142 | value = get_stringzpad_value(scope, tvb, start, length, lenretval, encoding);
4143 | break;
4144 | case FT_STRINGZTRUNC:
4145 | value = get_stringztrunc_value(scope, tvb, start, length, lenretval, encoding);
4146 | break;
4147 | default:
4148 | REPORT_DISSECTOR_BUG("field %s is not of type FT_STRING, FT_STRINGZ, FT_UINT_STRING, FT_STRINGZPAD, or FT_STRINGZTRUNC",proto_report_dissector_bug("field %s is not of type FT_STRING, FT_STRINGZ, FT_UINT_STRING, FT_STRINGZPAD, or FT_STRINGZTRUNC" , hfinfo->abbrev)
4149 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_STRING, FT_STRINGZ, FT_UINT_STRING, FT_STRINGZPAD, or FT_STRINGZTRUNC" , hfinfo->abbrev);
4150 | }
4151 |
4152 | if (retval)
4153 | *retval = value;
4154 |
4155 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4156 |
4157 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4157 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4157, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4157, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4157, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4158 |
4159 | new_fi = new_field_info(tree, hfinfo, tvb, start, *lenretval);
4160 |
4161 | proto_tree_set_string(new_fi, (const char*)value);
4162 |
4163 | new_fi->flags |= (encoding & ENC_LITTLE_ENDIAN0x80000000) ? FI_LITTLE_ENDIAN0x00000008 : FI_BIG_ENDIAN0x00000010;
4164 |
4165 | pi = proto_tree_add_node(tree, new_fi);
4166 |
4167 | switch (hfinfo->type) {
4168 |
4169 | case FT_STRINGZ:
4170 | case FT_STRINGZPAD:
4171 | case FT_STRINGZTRUNC:
4172 | case FT_UINT_STRING:
4173 | break;
4174 |
4175 | case FT_STRING:
4176 | detect_trailing_stray_characters(encoding, (const char*)value, length, pi);
4177 | break;
4178 |
4179 | default:
4180 | ws_assert_not_reached()ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4180 , __func__, "assertion \"not reached\" failed");
4181 | }
4182 |
4183 | return pi;
4184 | }
4185 |
4186 | proto_item *
4187 | proto_tree_add_item_ret_string(proto_tree *tree, int hfindex, tvbuff_t *tvb,
4188 | const int start, int length,
4189 | const unsigned encoding, wmem_allocator_t *scope,
4190 | const uint8_t **retval)
4191 | {
4192 | return proto_tree_add_item_ret_string_and_length(tree, hfindex,
4193 | tvb, start, length, encoding, scope, retval, &length);
4194 | }
4195 |
4196 | proto_item *
4197 | proto_tree_add_item_ret_display_string_and_length(proto_tree *tree, int hfindex,
4198 | tvbuff_t *tvb,
4199 | const int start, int length,
4200 | const unsigned encoding,
4201 | wmem_allocator_t *scope,
4202 | char **retval,
4203 | int *lenretval)
4204 | {
4205 | proto_item *pi;
4206 | header_field_info *hfinfo;
4207 | field_info *new_fi;
4208 | const uint8_t *value;
4209 | uint32_t n = 0;
4210 |
4211 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4211, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4211, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4211, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
4212 |
4213 | switch (hfinfo->type) {
4214 | case FT_STRING:
4215 | value = get_string_value(scope, tvb, start, length, lenretval, encoding);
4216 | *retval = wmem_alloc(scope, ITEM_LABEL_LENGTH240);
4217 | ws_label_strcpy(*retval, ITEM_LABEL_LENGTH240, 0, value, label_strcat_flags(hfinfo));
4218 | break;
4219 | case FT_STRINGZ:
4220 | value = get_stringz_value(scope, tree, tvb, start, length, lenretval, encoding);
4221 | *retval = wmem_alloc(scope, ITEM_LABEL_LENGTH240);
4222 | ws_label_strcpy(*retval, ITEM_LABEL_LENGTH240, 0, value, label_strcat_flags(hfinfo));
4223 | break;
4224 | case FT_UINT_STRING:
4225 | value = get_uint_string_value(scope, tree, tvb, start, length, lenretval, encoding);
4226 | *retval = wmem_alloc(scope, ITEM_LABEL_LENGTH240);
4227 | ws_label_strcpy(*retval, ITEM_LABEL_LENGTH240, 0, value, label_strcat_flags(hfinfo));
4228 | break;
4229 | case FT_STRINGZPAD:
4230 | value = get_stringzpad_value(scope, tvb, start, length, lenretval, encoding);
4231 | *retval = wmem_alloc(scope, ITEM_LABEL_LENGTH240);
4232 | ws_label_strcpy(*retval, ITEM_LABEL_LENGTH240, 0, value, label_strcat_flags(hfinfo));
4233 | break;
4234 | case FT_STRINGZTRUNC:
4235 | value = get_stringztrunc_value(scope, tvb, start, length, lenretval, encoding);
4236 | *retval = wmem_alloc(scope, ITEM_LABEL_LENGTH240);
4237 | ws_label_strcpy(*retval, ITEM_LABEL_LENGTH240, 0, value, label_strcat_flags(hfinfo));
4238 | break;
4239 | case FT_BYTES:
4240 | tvb_ensure_bytes_exist(tvb, start, length);
4241 | value = tvb_get_ptr(tvb, start, length);
4242 | *retval = format_bytes_hfinfo(scope, hfinfo, value, length);
4243 | *lenretval = length;
4244 | break;
4245 | case FT_UINT_BYTES:
4246 | n = get_uint_value(tree, tvb, start, length, encoding);
4247 | tvb_ensure_bytes_exist(tvb, start + length, n);
4248 | value = tvb_get_ptr(tvb, start + length, n);
4249 | *retval = format_bytes_hfinfo(scope, hfinfo, value, n);
4250 | *lenretval = length + n;
4251 | break;
4252 | default:
4253 | REPORT_DISSECTOR_BUG("field %s is not of type FT_STRING, FT_STRINGZ, FT_UINT_STRING, FT_STRINGZPAD, FT_STRINGZTRUNC, FT_BYTES, or FT_UINT_BYTES",proto_report_dissector_bug("field %s is not of type FT_STRING, FT_STRINGZ, FT_UINT_STRING, FT_STRINGZPAD, FT_STRINGZTRUNC, FT_BYTES, or FT_UINT_BYTES" , hfinfo->abbrev)
4254 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_STRING, FT_STRINGZ, FT_UINT_STRING, FT_STRINGZPAD, FT_STRINGZTRUNC, FT_BYTES, or FT_UINT_BYTES" , hfinfo->abbrev);
4255 | }
4256 |
4257 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4258 |
4259 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4259 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4259, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4259, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4259, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4260 |
4261 | new_fi = new_field_info(tree, hfinfo, tvb, start, *lenretval);
4262 |
4263 | switch (hfinfo->type) {
4264 |
4265 | case FT_STRING:
4266 | case FT_STRINGZ:
4267 | case FT_UINT_STRING:
4268 | case FT_STRINGZPAD:
4269 | case FT_STRINGZTRUNC:
4270 | proto_tree_set_string(new_fi, (const char*)value);
4271 | break;
4272 |
4273 | case FT_BYTES:
4274 | proto_tree_set_bytes(new_fi, value, length);
4275 | break;
4276 |
4277 | case FT_UINT_BYTES:
4278 | proto_tree_set_bytes(new_fi, value, n);
4279 | break;
4280 |
4281 | default:
4282 | ws_assert_not_reached()ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4282 , __func__, "assertion \"not reached\" failed");
4283 | }
4284 |
4285 | new_fi->flags |= (encoding & ENC_LITTLE_ENDIAN0x80000000) ? FI_LITTLE_ENDIAN0x00000008 : FI_BIG_ENDIAN0x00000010;
4286 |
4287 | pi = proto_tree_add_node(tree, new_fi);
4288 |
4289 | switch (hfinfo->type) {
4290 |
4291 | case FT_STRINGZ:
4292 | case FT_STRINGZPAD:
4293 | case FT_STRINGZTRUNC:
4294 | case FT_UINT_STRING:
4295 | break;
4296 |
4297 | case FT_STRING:
4298 | detect_trailing_stray_characters(encoding, (const char*)value, length, pi);
4299 | break;
4300 |
4301 | case FT_BYTES:
4302 | case FT_UINT_BYTES:
4303 | break;
4304 |
4305 | default:
4306 | ws_assert_not_reached()ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4306 , __func__, "assertion \"not reached\" failed");
4307 | }
4308 |
4309 | return pi;
4310 | }
4311 |
4312 | proto_item *
4313 | proto_tree_add_item_ret_display_string(proto_tree *tree, int hfindex,
4314 | tvbuff_t *tvb,
4315 | const int start, int length,
4316 | const unsigned encoding,
4317 | wmem_allocator_t *scope,
4318 | char **retval)
4319 | {
4320 | return proto_tree_add_item_ret_display_string_and_length(tree, hfindex,
4321 | tvb, start, length, encoding, scope, retval, &length);
4322 | }
4323 |
4324 | proto_item *
4325 | proto_tree_add_item_ret_time_string(proto_tree *tree, int hfindex,
4326 | tvbuff_t *tvb,
4327 | const int start, int length, const unsigned encoding,
4328 | wmem_allocator_t *scope, char **retval)
4329 | {
4330 | header_field_info *hfinfo;
4331 | field_info *new_fi;
4332 | nstime_t time_stamp;
4333 | int flags;
4334 |
4335 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4335, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4335, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4335, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
4336 |
4337 | switch (hfinfo->type) {
4338 | case FT_ABSOLUTE_TIME:
4339 | get_time_value(tree, tvb, start, length, encoding, &time_stamp, false0);
4340 | flags = ABS_TIME_TO_STR_SHOW_ZONE(1U << 0);
4341 | if (prefs.display_abs_time_ascii < ABS_TIME_ASCII_TREE) {
4342 | flags |= ABS_TIME_TO_STR_ISO8601(1U << 3);
4343 | }
4344 | *retval = abs_time_to_str_ex(scope, &time_stamp, hfinfo->display, flags);
4345 | break;
4346 | case FT_RELATIVE_TIME:
4347 | get_time_value(tree, tvb, start, length, encoding, &time_stamp, true1);
4348 | *retval = rel_time_to_secs_str(scope, &time_stamp);
4349 | break;
4350 | default:
4351 | REPORT_DISSECTOR_BUG("field %s is not of type FT_ABSOLUTE_TIME or FT_RELATIVE_TIME",proto_report_dissector_bug("field %s is not of type FT_ABSOLUTE_TIME or FT_RELATIVE_TIME" , hfinfo->abbrev)
4352 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_ABSOLUTE_TIME or FT_RELATIVE_TIME" , hfinfo->abbrev);
4353 | }
4354 |
4355 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4356 |
4357 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4357 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4357, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4357, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4357, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4358 |
4359 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
4360 |
4361 | switch (hfinfo->type) {
4362 |
4363 | case FT_ABSOLUTE_TIME:
4364 | case FT_RELATIVE_TIME:
4365 | proto_tree_set_time(new_fi, &time_stamp);
4366 | break;
4367 | default:
4368 | ws_assert_not_reached()ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4368 , __func__, "assertion \"not reached\" failed");
4369 | }
4370 |
4371 | new_fi->flags |= (encoding & ENC_LITTLE_ENDIAN0x80000000) ? FI_LITTLE_ENDIAN0x00000008 : FI_BIG_ENDIAN0x00000010;
4372 |
4373 | return proto_tree_add_node(tree, new_fi);
4374 | }
4375 |
4376 | /* Gets data from tvbuff, adds it to proto_tree, increments offset,
4377 | and returns proto_item* */
4378 | proto_item *
4379 | ptvcursor_add(ptvcursor_t *ptvc, int hfindex, int length,
4380 | const unsigned encoding)
4381 | {
4382 | field_info *new_fi;
4383 | header_field_info *hfinfo;
4384 | int item_length;
4385 | int offset;
4386 |
4387 | offset = ptvc->offset;
4388 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4388, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4388, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4388, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
4389 | get_hfi_length(hfinfo, ptvc->tvb, offset, &length, &item_length, encoding);
4390 | test_length(hfinfo, ptvc->tvb, offset, item_length, encoding);
4391 |
4392 | ptvcursor_advance(ptvc, get_full_length(hfinfo, ptvc->tvb, offset, length, item_length, encoding));
4393 |
4394 | CHECK_FOR_NULL_TREE(ptvc->tree)if (!ptvc->tree) { ((void)0); return ((void*)0); };
4395 |
4396 | /* Coast clear. Try and fake it */
4397 | TRY_TO_FAKE_THIS_ITEM(ptvc->tree, hfindex, hfinfo)((ptvc->tree)->tree_data)->count++; if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4397 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4397, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4397, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((ptvc->tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4397, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((ptvc->tree )->tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((ptvc->tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((ptvc ->tree)->tree_data)->visible)) { if (proto_item_is_hidden ((ptvc->tree))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT ) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo->type != FT_PROTOCOL || ((ptvc->tree)->tree_data )->fake_protocols)) { ((void)0); return proto_tree_add_fake_node (ptvc->tree, hfinfo); } } };
4398 |
4399 | new_fi = new_field_info(ptvc->tree, hfinfo, ptvc->tvb, offset, item_length);
4400 |
4401 | return proto_tree_new_item(new_fi, ptvc->tree, ptvc->tvb,
4402 | offset, length, encoding);
4403 | }
4404 |
4405 | /* Add an item to a proto_tree, using the text label registered to that item;
4406 | the item is extracted from the tvbuff handed to it. */
4407 | proto_item *
4408 | proto_tree_add_item_new(proto_tree *tree, header_field_info *hfinfo, tvbuff_t *tvb,
4409 | const int start, int length, const unsigned encoding)
4410 | {
4411 | field_info *new_fi;
4412 | int item_length;
4413 |
4414 | DISSECTOR_ASSERT_HINT(hfinfo != NULL, "Not passed hfi!")((void) ((hfinfo != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4414, "hfinfo != ((void*)0)", "Not passed hfi!"))));
4415 |
4416 | get_hfi_length(hfinfo, tvb, start, &length, &item_length, encoding);
4417 | test_length(hfinfo, tvb, start, item_length, encoding);
4418 |
4419 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4420 |
4421 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4421 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4421, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4421, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4421, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4422 |
4423 | new_fi = new_field_info(tree, hfinfo, tvb, start, item_length);
4424 |
4425 | return proto_tree_new_item(new_fi, tree, tvb, start, length, encoding);
4426 | }
4427 |
4428 | proto_item *
4429 | proto_tree_add_item(proto_tree *tree, int hfindex, tvbuff_t *tvb,
4430 | const int start, int length, const unsigned encoding)
4431 | {
4432 | register header_field_info *hfinfo;
4433 |
4434 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4434, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4434, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4434, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
4435 | return proto_tree_add_item_new(tree, hfinfo, tvb, start, length, encoding);
4436 | }
4437 |
4438 | /* Add an item to a proto_tree, using the text label registered to that item;
4439 | the item is extracted from the tvbuff handed to it.
4440 |
4441 | Return the length of the item through the pointer. */
4442 | proto_item *
4443 | proto_tree_add_item_new_ret_length(proto_tree *tree, header_field_info *hfinfo,
4444 | tvbuff_t *tvb, const int start,
4445 | int length, const unsigned encoding,
4446 | int *lenretval)
4447 | {
4448 | field_info *new_fi;
4449 | int item_length;
4450 | proto_item *item;
4451 |
4452 | DISSECTOR_ASSERT_HINT(hfinfo != NULL, "Not passed hfi!")((void) ((hfinfo != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4452, "hfinfo != ((void*)0)", "Not passed hfi!"))));
4453 |
4454 | get_hfi_length(hfinfo, tvb, start, &length, &item_length, encoding);
4455 | test_length(hfinfo, tvb, start, item_length, encoding);
4456 |
4457 | if (!tree) {
4458 | /*
4459 | * We need to get the correct item length here.
4460 | * That's normally done by proto_tree_new_item(),
4461 | * but we won't be calling it.
4462 | */
4463 | *lenretval = get_full_length(hfinfo, tvb, start, length,
4464 | item_length, encoding);
4465 | return NULL((void*)0);
4466 | }
4467 |
4468 | TRY_TO_FAKE_THIS_ITEM_OR_FREE(tree, hfinfo->id, hfinfo, {((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; return proto_tree_add_fake_node( tree, hfinfo); } } }
4469 | /*((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; return proto_tree_add_fake_node( tree, hfinfo); } } }
4470 | * Even if the tree item is not referenced (and thus faked),((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; return proto_tree_add_fake_node( tree, hfinfo); } } }
4471 | * the caller must still be informed of the actual length.((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; return proto_tree_add_fake_node( tree, hfinfo); } } }
4472 | */((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; return proto_tree_add_fake_node( tree, hfinfo); } } }
4473 | *lenretval = get_full_length(hfinfo, tvb, start, length,((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; return proto_tree_add_fake_node( tree, hfinfo); } } }
4474 | item_length, encoding);((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; return proto_tree_add_fake_node( tree, hfinfo); } } }
4475 | })((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4475, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4475 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { *lenretval = get_full_length(hfinfo, tvb, start, length , item_length, encoding); }; return proto_tree_add_fake_node( tree, hfinfo); } } };
4476 |
4477 | new_fi = new_field_info(tree, hfinfo, tvb, start, item_length);
4478 |
4479 | item = proto_tree_new_item(new_fi, tree, tvb, start, length, encoding);
4480 | *lenretval = new_fi->length;
4481 | return item;
4482 | }
4483 |
4484 | proto_item *
4485 | proto_tree_add_item_ret_length(proto_tree *tree, int hfindex, tvbuff_t *tvb,
4486 | const int start, int length,
4487 | const unsigned encoding, int *lenretval)
4488 | {
4489 | register header_field_info *hfinfo;
4490 |
4491 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4491, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4491, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4491, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
4492 | return proto_tree_add_item_new_ret_length(tree, hfinfo, tvb, start, length, encoding, lenretval);
4493 | }
4494 |
4495 | /* which FT_ types can use proto_tree_add_bytes_item() */
4496 | static inline bool_Bool
4497 | validate_proto_tree_add_bytes_ftype(const enum ftenum type)
4498 | {
4499 | return (type == FT_BYTES ||
4500 | type == FT_UINT_BYTES ||
4501 | type == FT_OID ||
4502 | type == FT_REL_OID ||
4503 | type == FT_SYSTEM_ID );
4504 | }
4505 |
4506 | /* Note: this does no validation that the byte array of an FT_OID or
4507 | FT_REL_OID is actually valid; and neither does proto_tree_add_item(),
4508 | so I think it's ok to continue not validating it?
4509 | */
4510 | proto_item *
4511 | proto_tree_add_bytes_item(proto_tree *tree, int hfindex, tvbuff_t *tvb,
4512 | const unsigned start, unsigned length,
4513 | const unsigned encoding,
4514 | GByteArray *retval, unsigned *endoff, int *err)
4515 | {
4516 | field_info *new_fi;
4517 | GByteArray *bytes = retval;
4518 | GByteArray *created_bytes = NULL((void*)0);
4519 | bool_Bool failed = false0;
4520 | uint32_t n = 0;
4521 | header_field_info *hfinfo;
4522 | bool_Bool generate = (bytes || tree) ? true1 : false0;
4523 |
4524 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4524, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4524, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4524, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
4525 |
4526 | DISSECTOR_ASSERT_HINT(hfinfo != NULL, "Not passed hfi!")((void) ((hfinfo != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4526, "hfinfo != ((void*)0)", "Not passed hfi!"))));
4527 |
4528 | DISSECTOR_ASSERT_HINT(validate_proto_tree_add_bytes_ftype(hfinfo->type),((void) ((validate_proto_tree_add_bytes_ftype(hfinfo->type )) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4529, "validate_proto_tree_add_bytes_ftype(hfinfo->type)" , "Called proto_tree_add_bytes_item but not a bytes-based FT_XXX type" ))))
4529 | "Called proto_tree_add_bytes_item but not a bytes-based FT_XXX type")((void) ((validate_proto_tree_add_bytes_ftype(hfinfo->type )) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4529, "validate_proto_tree_add_bytes_ftype(hfinfo->type)" , "Called proto_tree_add_bytes_item but not a bytes-based FT_XXX type" ))));
4530 |
4531 | if (length == 0) {
4532 | return NULL((void*)0);
4533 | }
4534 |
4535 | if (encoding & ENC_STR_NUM0x01000000) {
4536 | REPORT_DISSECTOR_BUG("Decoding number strings for byte arrays is not supported")proto_report_dissector_bug("Decoding number strings for byte arrays is not supported" );
4537 | }
4538 |
4539 | if (generate && (encoding & ENC_STR_HEX0x02000000)) {
4540 | if (hfinfo->type == FT_UINT_BYTES) {
4541 | /* can't decode FT_UINT_BYTES from strings */
4542 | REPORT_DISSECTOR_BUG("proto_tree_add_bytes_item called for "proto_report_dissector_bug("proto_tree_add_bytes_item called for " "FT_UINT_BYTES type, but as ENC_STR_HEX")
4543 | "FT_UINT_BYTES type, but as ENC_STR_HEX")proto_report_dissector_bug("proto_tree_add_bytes_item called for " "FT_UINT_BYTES type, but as ENC_STR_HEX");
4544 | }
4545 |
4546 | unsigned hex_encoding = encoding;
4547 | if (!(encoding & ENC_SEP_MASK0x001F0000)) {
4548 | /* If none of the separator values are used,
4549 | * assume no separator (the common case). */
4550 | hex_encoding |= ENC_SEP_NONE0x00010000;
4551 | #if 0
4552 | REPORT_DISSECTOR_BUG("proto_tree_add_bytes_item called "proto_report_dissector_bug("proto_tree_add_bytes_item called " "with ENC_STR_HEX but no ENC_SEP_XXX value")
4553 | "with ENC_STR_HEX but no ENC_SEP_XXX value")proto_report_dissector_bug("proto_tree_add_bytes_item called " "with ENC_STR_HEX but no ENC_SEP_XXX value");
4554 | #endif
4555 | }
4556 |
4557 | if (!bytes) {
4558 | /* caller doesn't care about return value, but we need it to
4559 | call tvb_get_string_bytes() and set the tree later */
4560 | bytes = created_bytes = g_byte_array_new();
4561 | }
4562 |
4563 | /*
4564 | * bytes might be NULL after this, but can't add expert
4565 | * error until later; if it's NULL, just note that
4566 | * it failed.
4567 | */
4568 | bytes = tvb_get_string_bytes(tvb, start, length, hex_encoding, bytes, endoff);
4569 | if (bytes == NULL((void*)0))
4570 | failed = true1;
4571 | }
4572 | else if (generate) {
4573 | tvb_ensure_bytes_exist(tvb, start, length);
4574 |
4575 | if (hfinfo->type == FT_UINT_BYTES) {
4576 | n = length; /* n is now the "header" length */
4577 | length = get_uint_value(tree, tvb, start, n, encoding);
4578 | /* length is now the value's length; only store the value in the array */
4579 | tvb_ensure_bytes_exist(tvb, start + n, length);
4580 | if (!bytes) {
4581 | /* caller doesn't care about return value, but
4582 | * we may need it to set the tree later */
4583 | bytes = created_bytes = g_byte_array_new();
4584 | }
4585 | g_byte_array_append(bytes, tvb_get_ptr(tvb, start + n, length), length);
4586 | }
4587 | else if (length > 0) {
4588 | if (!bytes) {
4589 | /* caller doesn't care about return value, but
4590 | * we may need it to set the tree later */
4591 | bytes = created_bytes = g_byte_array_new();
4592 | }
4593 | g_byte_array_append(bytes, tvb_get_ptr(tvb, start, length), length);
4594 | }
4595 |
4596 | if (endoff)
4597 | *endoff = start + n + length;
4598 | }
4599 |
4600 | if (err)
4601 | *err = failed ? EINVAL22 : 0;
4602 |
4603 | CHECK_FOR_NULL_TREE_AND_FREE(tree,if (!tree) { { if (created_bytes) g_byte_array_free(created_bytes , 1); created_bytes = ((void*)0); bytes = ((void*)0); }; return ((void*)0); }
4604 | {if (!tree) { { if (created_bytes) g_byte_array_free(created_bytes , 1); created_bytes = ((void*)0); bytes = ((void*)0); }; return ((void*)0); }
4605 | if (created_bytes)if (!tree) { { if (created_bytes) g_byte_array_free(created_bytes , 1); created_bytes = ((void*)0); bytes = ((void*)0); }; return ((void*)0); }
4606 | g_byte_array_free(created_bytes, true);if (!tree) { { if (created_bytes) g_byte_array_free(created_bytes , 1); created_bytes = ((void*)0); bytes = ((void*)0); }; return ((void*)0); }
4607 | created_bytes = NULL;if (!tree) { { if (created_bytes) g_byte_array_free(created_bytes , 1); created_bytes = ((void*)0); bytes = ((void*)0); }; return ((void*)0); }
4608 | bytes = NULL;if (!tree) { { if (created_bytes) g_byte_array_free(created_bytes , 1); created_bytes = ((void*)0); bytes = ((void*)0); }; return ((void*)0); }
4609 | } )if (!tree) { { if (created_bytes) g_byte_array_free(created_bytes , 1); created_bytes = ((void*)0); bytes = ((void*)0); }; return ((void*)0); };
4610 |
4611 | TRY_TO_FAKE_THIS_ITEM_OR_FREE(tree, hfinfo->id, hfinfo,((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { if (created_bytes) g_byte_array_free(created_bytes, 1); created_bytes = ((void*)0); bytes = ((void*)0); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { if (created_bytes) g_byte_array_free(created_bytes, 1) ; created_bytes = ((void*)0); bytes = ((void*)0); }; return proto_tree_add_fake_node (tree, hfinfo); } } }
4612 | {((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { if (created_bytes) g_byte_array_free(created_bytes, 1); created_bytes = ((void*)0); bytes = ((void*)0); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { if (created_bytes) g_byte_array_free(created_bytes, 1) ; created_bytes = ((void*)0); bytes = ((void*)0); }; return proto_tree_add_fake_node (tree, hfinfo); } } }
4613 | if (created_bytes)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { if (created_bytes) g_byte_array_free(created_bytes, 1); created_bytes = ((void*)0); bytes = ((void*)0); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { if (created_bytes) g_byte_array_free(created_bytes, 1) ; created_bytes = ((void*)0); bytes = ((void*)0); }; return proto_tree_add_fake_node (tree, hfinfo); } } }
4614 | g_byte_array_free(created_bytes, true);((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { if (created_bytes) g_byte_array_free(created_bytes, 1); created_bytes = ((void*)0); bytes = ((void*)0); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { if (created_bytes) g_byte_array_free(created_bytes, 1) ; created_bytes = ((void*)0); bytes = ((void*)0); }; return proto_tree_add_fake_node (tree, hfinfo); } } }
4615 | created_bytes = NULL;((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { if (created_bytes) g_byte_array_free(created_bytes, 1); created_bytes = ((void*)0); bytes = ((void*)0); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { if (created_bytes) g_byte_array_free(created_bytes, 1) ; created_bytes = ((void*)0); bytes = ((void*)0); }; return proto_tree_add_fake_node (tree, hfinfo); } } }
4616 | bytes = NULL;((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { if (created_bytes) g_byte_array_free(created_bytes, 1); created_bytes = ((void*)0); bytes = ((void*)0); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { if (created_bytes) g_byte_array_free(created_bytes, 1) ; created_bytes = ((void*)0); bytes = ((void*)0); }; return proto_tree_add_fake_node (tree, hfinfo); } } }
4617 | } )((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4617, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { { if (created_bytes) g_byte_array_free(created_bytes, 1); created_bytes = ((void*)0); bytes = ((void*)0); }; if (wireshark_abort_on_too_many_items ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4617 , __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { { if (created_bytes) g_byte_array_free(created_bytes, 1) ; created_bytes = ((void*)0); bytes = ((void*)0); }; return proto_tree_add_fake_node (tree, hfinfo); } } };
4618 |
4619 | /* n will be zero except when it's a FT_UINT_BYTES */
4620 | new_fi = new_field_info(tree, hfinfo, tvb, start, n + length);
4621 |
4622 | if (encoding & ENC_STRING0x03000000) {
4623 | if (failed)
4624 | expert_add_info(NULL((void*)0), tree, &ei_byte_array_string_decoding_failed_error);
4625 |
4626 | if (bytes)
4627 | proto_tree_set_bytes_gbytearray(new_fi, bytes);
4628 | else
4629 | proto_tree_set_bytes(new_fi, NULL((void*)0), 0);
4630 |
4631 | if (created_bytes)
4632 | g_byte_array_free(created_bytes, true1);
4633 | }
4634 | else {
4635 | /* n will be zero except when it's a FT_UINT_BYTES */
4636 | proto_tree_set_bytes_tvb(new_fi, tvb, start + n, length);
4637 |
4638 | /* XXX: If we have a non-NULL tree but NULL retval, we don't
4639 | * use the byte array created above in this case.
4640 | */
4641 | if (created_bytes)
4642 | g_byte_array_free(created_bytes, true1);
4643 |
4644 | FI_SET_FLAG(new_fi,do { if (new_fi) (new_fi)->flags = (new_fi)->flags | (( encoding & 0x80000000) ? 0x00000008 : 0x00000010); } while (0)
4645 | (encoding & ENC_LITTLE_ENDIAN) ? FI_LITTLE_ENDIAN : FI_BIG_ENDIAN)do { if (new_fi) (new_fi)->flags = (new_fi)->flags | (( encoding & 0x80000000) ? 0x00000008 : 0x00000010); } while (0);
4646 | }
4647 |
4648 | return proto_tree_add_node(tree, new_fi);
4649 | }
4650 |
4651 |
4652 | proto_item *
4653 | proto_tree_add_time_item(proto_tree *tree, int hfindex, tvbuff_t *tvb,
4654 | const unsigned start, const unsigned length,
4655 | const unsigned encoding,
4656 | nstime_t *retval, unsigned *endoff, int *err)
4657 | {
4658 | field_info *new_fi;
4659 | nstime_t time_stamp;
4660 | int saved_err = 0;
4661 | header_field_info *hfinfo;
4662 |
4663 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4663, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4663, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4663, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
4664 |
4665 | DISSECTOR_ASSERT_HINT(hfinfo != NULL, "Not passed hfi!")((void) ((hfinfo != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4665, "hfinfo != ((void*)0)", "Not passed hfi!"))));
4666 |
4667 | if (length == 0) {
4668 | if(retval) {
4669 | nstime_set_zero(retval);
4670 | }
4671 | return NULL((void*)0);
4672 | }
4673 |
4674 | nstime_set_zero(&time_stamp);
4675 |
4676 | if (encoding & ENC_STR_TIME_MASK0x001F0000) {
4677 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_ABSOLUTE_TIME)((void) (((hfinfo)->type == FT_ABSOLUTE_TIME) ? (void)0 : ( proto_report_dissector_bug("%s:%u: field %s is not of type ""FT_ABSOLUTE_TIME" , "epan/proto.c", 4677, ((hfinfo))->abbrev))));
4678 | /* The only string format that could be a relative time is
4679 | * ENC_ISO_8601_TIME, and that is treated as an absolute time
4680 | * relative to "now" currently.
4681 | */
4682 | if (!tvb_get_string_time(tvb, start, length, encoding, &time_stamp, endoff))
4683 | saved_err = EINVAL22;
4684 | }
4685 | else {
4686 | DISSECTOR_ASSERT_FIELD_TYPE_IS_TIME(hfinfo)((void) (((hfinfo)->type == FT_ABSOLUTE_TIME || (hfinfo)-> type == FT_RELATIVE_TIME) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type FT_ABSOLUTE_TIME or FT_RELATIVE_TIME" , "epan/proto.c", 4686, ((hfinfo))->abbrev))));
4687 | const bool_Bool is_relative = (hfinfo->type == FT_RELATIVE_TIME) ? true1 : false0;
4688 |
4689 | tvb_ensure_bytes_exist(tvb, start, length);
4690 | get_time_value(tree, tvb, start, length, encoding, &time_stamp, is_relative);
4691 | if (endoff) *endoff = start + length;
4692 | }
4693 |
4694 | if (err) *err = saved_err;
4695 |
4696 | if (retval) {
4697 | retval->secs = time_stamp.secs;
4698 | retval->nsecs = time_stamp.nsecs;
4699 | }
4700 |
4701 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4702 |
4703 | TRY_TO_FAKE_THIS_ITEM(tree, hfinfo->id, hfinfo)((tree)->tree_data)->count++; if((hfinfo->id == 0 || (unsigned)hfinfo->id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4703 , __func__, "Unregistered hf! index=%d", hfinfo->id); ((void ) ((hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4703, "hfinfo->id > 0 && (unsigned)hfinfo->id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4703, "gpa_hfinfo.hfi[hfinfo->id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> id];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4703, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4704 |
4705 | new_fi = new_field_info(tree, hfinfo, tvb, start, length);
4706 |
4707 | proto_tree_set_time(new_fi, &time_stamp);
4708 |
4709 | if (encoding & ENC_STRING0x03000000) {
4710 | if (saved_err)
4711 | expert_add_info(NULL((void*)0), tree, &ei_date_time_string_decoding_failed_error);
4712 | }
4713 | else {
4714 | FI_SET_FLAG(new_fi,do { if (new_fi) (new_fi)->flags = (new_fi)->flags | (( encoding & 0x80000000) ? 0x00000008 : 0x00000010); } while (0)
4715 | (encoding & ENC_LITTLE_ENDIAN) ? FI_LITTLE_ENDIAN : FI_BIG_ENDIAN)do { if (new_fi) (new_fi)->flags = (new_fi)->flags | (( encoding & 0x80000000) ? 0x00000008 : 0x00000010); } while (0);
4716 | }
4717 |
4718 | return proto_tree_add_node(tree, new_fi);
4719 | }
4720 |
4721 | /* Add a FT_NONE to a proto_tree */
4722 | proto_item *
4723 | proto_tree_add_none_format(proto_tree *tree, const int hfindex, tvbuff_t *tvb,
4724 | const int start, int length, const char *format,
4725 | ...)
4726 | {
4727 | proto_item *pi;
4728 | va_list ap;
4729 | header_field_info *hfinfo;
4730 |
4731 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4732 |
4733 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4733 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4733, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4733, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4733, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4734 |
4735 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_NONE)((void) (((hfinfo)->type == FT_NONE) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_NONE", "epan/proto.c", 4735 , ((hfinfo))->abbrev))));
4736 |
4737 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
4738 |
4739 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4739, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
4740 |
4741 | va_start(ap, format)__builtin_va_start(ap, format);
4742 | proto_tree_set_representation(pi, format, ap);
4743 | va_end(ap)__builtin_va_end(ap);
4744 |
4745 | /* no value to set for FT_NONE */
4746 | return pi;
4747 | }
4748 |
4749 | /* Gets data from tvbuff, adds it to proto_tree, *DOES NOT* increment
4750 | * offset, and returns proto_item* */
4751 | proto_item *
4752 | ptvcursor_add_no_advance(ptvcursor_t* ptvc, int hf, int length,
4753 | const unsigned encoding)
4754 | {
4755 | proto_item *item;
4756 |
4757 | item = proto_tree_add_item(ptvc->tree, hf, ptvc->tvb, ptvc->offset,
4758 | length, encoding);
4759 |
4760 | return item;
4761 | }
4762 |
4763 | /* Advance the ptvcursor's offset within its tvbuff without
4764 | * adding anything to the proto_tree. */
4765 | void
4766 | ptvcursor_advance(ptvcursor_t* ptvc, int length)
4767 | {
4768 | if (ckd_add(&ptvc->offset, ptvc->offset, length)__builtin_add_overflow((ptvc->offset), (length), (&ptvc ->offset))) {
4769 | THROW(ReportedBoundsError)except_throw(1, (3), ((void*)0));
4770 | }
4771 | }
4772 |
4773 |
4774 | static void
4775 | proto_tree_set_protocol_tvb(field_info *fi, tvbuff_t *tvb, const char* field_data, int length)
4776 | {
4777 | fvalue_set_protocol(fi->value, tvb, field_data, length);
4778 | }
4779 |
4780 | /* Add a FT_PROTOCOL to a proto_tree */
4781 | proto_item *
4782 | proto_tree_add_protocol_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
4783 | int start, int length, const char *format, ...)
4784 | {
4785 | proto_item *pi;
4786 | tvbuff_t *protocol_tvb;
4787 | va_list ap;
4788 | header_field_info *hfinfo;
4789 | char* protocol_rep;
4790 |
4791 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4792 |
4793 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4793 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4793, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4793, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4793, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4794 |
4795 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_PROTOCOL)((void) (((hfinfo)->type == FT_PROTOCOL) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_PROTOCOL", "epan/proto.c" , 4795, ((hfinfo))->abbrev))));
4796 |
4797 | /*
4798 | * This can throw an exception, so do it before we allocate anything.
4799 | */
4800 | protocol_tvb = (start == 0 ? tvb : tvb_new_subset_length(tvb, start, length));
4801 |
4802 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
4803 |
4804 | va_start(ap, format)__builtin_va_start(ap, format);
4805 | protocol_rep = ws_strdup_vprintf(format, ap)wmem_strdup_vprintf(((void*)0), format, ap);
4806 | proto_tree_set_protocol_tvb(PNODE_FINFO(pi)((pi)->finfo), protocol_tvb, protocol_rep, length);
4807 | g_free(protocol_rep);
4808 | va_end(ap)__builtin_va_end(ap);
4809 |
4810 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4810, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
4811 |
4812 | va_start(ap, format)__builtin_va_start(ap, format);
4813 | proto_tree_set_representation(pi, format, ap);
4814 | va_end(ap)__builtin_va_end(ap);
4815 |
4816 | return pi;
4817 | }
4818 |
4819 | /* Add a FT_BYTES to a proto_tree */
4820 | proto_item *
4821 | proto_tree_add_bytes(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
4822 | int length, const uint8_t *start_ptr)
4823 | {
4824 | proto_item *pi;
4825 | header_field_info *hfinfo;
4826 | int item_length;
4827 |
4828 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4828, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4828, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4828, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
4829 | get_hfi_length(hfinfo, tvb, start, &length, &item_length, ENC_NA0x00000000);
4830 | test_length(hfinfo, tvb, start, item_length, ENC_NA0x00000000);
4831 |
4832 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4833 |
4834 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4834 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4834, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4834, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4834, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4835 |
4836 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_BYTES)((void) (((hfinfo)->type == FT_BYTES) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_BYTES", "epan/proto.c", 4836, ((hfinfo))->abbrev))));
4837 |
4838 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
4839 | proto_tree_set_bytes(PNODE_FINFO(pi)((pi)->finfo), start_ptr, length);
4840 |
4841 | return pi;
4842 | }
4843 |
4844 | /* Add a FT_BYTES to a proto_tree */
4845 | proto_item *
4846 | proto_tree_add_bytes_with_length(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
4847 | int tvbuff_length, const uint8_t *start_ptr, int ptr_length)
4848 | {
4849 | proto_item *pi;
4850 | header_field_info *hfinfo;
4851 | int item_length;
4852 |
4853 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4853, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 4853, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4853, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
4854 | get_hfi_length(hfinfo, tvb, start, &tvbuff_length, &item_length, ENC_NA0x00000000);
4855 | test_length(hfinfo, tvb, start, item_length, ENC_NA0x00000000);
4856 |
4857 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4858 |
4859 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4859 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4859, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4859, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4859, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4860 |
4861 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_BYTES)((void) (((hfinfo)->type == FT_BYTES) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_BYTES", "epan/proto.c", 4861, ((hfinfo))->abbrev))));
4862 |
4863 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &tvbuff_length);
4864 | proto_tree_set_bytes(PNODE_FINFO(pi)((pi)->finfo), start_ptr, ptr_length);
4865 |
4866 | return pi;
4867 | }
4868 |
4869 | proto_item *
4870 | proto_tree_add_bytes_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
4871 | int start, int length,
4872 | const uint8_t *start_ptr,
4873 | const char *format, ...)
4874 | {
4875 | proto_item *pi;
4876 | va_list ap;
4877 |
4878 | if (start_ptr == NULL((void*)0))
4879 | start_ptr = tvb_get_ptr(tvb, start, length);
4880 |
4881 | pi = proto_tree_add_bytes(tree, hfindex, tvb, start, length, start_ptr);
4882 |
4883 | TRY_TO_FAKE_THIS_REPR_NESTED(pi)if ((pi == ((void*)0)) || (((pi)->finfo) == ((void*)0)) || (!(((pi)->tree_data)->visible) && proto_item_is_hidden ((pi)))) { return pi; };
4884 |
4885 | va_start(ap, format)__builtin_va_start(ap, format);
4886 | proto_tree_set_representation_value(pi, format, ap);
4887 | va_end(ap)__builtin_va_end(ap);
4888 |
4889 | return pi;
4890 | }
4891 |
4892 | proto_item *
4893 | proto_tree_add_bytes_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
4894 | int start, int length, const uint8_t *start_ptr,
4895 | const char *format, ...)
4896 | {
4897 | proto_item *pi;
4898 | va_list ap;
4899 |
4900 | if (start_ptr == NULL((void*)0))
4901 | start_ptr = tvb_get_ptr(tvb, start, length);
4902 |
4903 | pi = proto_tree_add_bytes(tree, hfindex, tvb, start, length, start_ptr);
4904 |
4905 | TRY_TO_FAKE_THIS_REPR_NESTED(pi)if ((pi == ((void*)0)) || (((pi)->finfo) == ((void*)0)) || (!(((pi)->tree_data)->visible) && proto_item_is_hidden ((pi)))) { return pi; };
4906 |
4907 | va_start(ap, format)__builtin_va_start(ap, format);
4908 | proto_tree_set_representation(pi, format, ap);
4909 | va_end(ap)__builtin_va_end(ap);
4910 |
4911 | return pi;
4912 | }
4913 |
4914 | static void
4915 | proto_tree_set_bytes(field_info *fi, const uint8_t* start_ptr, int length)
4916 | {
4917 | DISSECTOR_ASSERT(length >= 0)((void) ((length >= 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 4917, "length >= 0" ))));
4918 | DISSECTOR_ASSERT(start_ptr != NULL || length == 0)((void) ((start_ptr != ((void*)0) || length == 0) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 4918, "start_ptr != ((void*)0) || length == 0" ))));
4919 |
4920 | fvalue_set_bytes_data(fi->value, start_ptr, length);
4921 | }
4922 |
4923 |
4924 | static void
4925 | proto_tree_set_bytes_tvb(field_info *fi, tvbuff_t *tvb, int offset, int length)
4926 | {
4927 | tvb_ensure_bytes_exist(tvb, offset, length);
4928 | proto_tree_set_bytes(fi, tvb_get_ptr(tvb, offset, length), length);
4929 | }
4930 |
4931 | static void
4932 | proto_tree_set_bytes_gbytearray(field_info *fi, const GByteArray *value)
4933 | {
4934 | GByteArray *bytes;
4935 |
4936 | DISSECTOR_ASSERT(value != NULL)((void) ((value != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 4936, "value != ((void*)0)" ))));
4937 |
4938 | bytes = byte_array_dup(value);
4939 |
4940 | fvalue_set_byte_array(fi->value, bytes);
4941 | }
4942 |
4943 | /* Add a FT_*TIME to a proto_tree */
4944 | proto_item *
4945 | proto_tree_add_time(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
4946 | int length, const nstime_t *value_ptr)
4947 | {
4948 | proto_item *pi;
4949 | header_field_info *hfinfo;
4950 |
4951 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
4952 |
4953 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4953 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4953, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 4953, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 4953, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
4954 |
4955 | DISSECTOR_ASSERT_FIELD_TYPE_IS_TIME(hfinfo)((void) (((hfinfo)->type == FT_ABSOLUTE_TIME || (hfinfo)-> type == FT_RELATIVE_TIME) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type FT_ABSOLUTE_TIME or FT_RELATIVE_TIME" , "epan/proto.c", 4955, ((hfinfo))->abbrev))));
4956 |
4957 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
4958 | proto_tree_set_time(PNODE_FINFO(pi)((pi)->finfo), value_ptr);
4959 |
4960 | return pi;
4961 | }
4962 |
4963 | proto_item *
4964 | proto_tree_add_time_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
4965 | int start, int length, nstime_t *value_ptr,
4966 | const char *format, ...)
4967 | {
4968 | proto_item *pi;
4969 | va_list ap;
4970 |
4971 | pi = proto_tree_add_time(tree, hfindex, tvb, start, length, value_ptr);
4972 | if (pi != tree) {
4973 | va_start(ap, format)__builtin_va_start(ap, format);
4974 | proto_tree_set_representation_value(pi, format, ap);
4975 | va_end(ap)__builtin_va_end(ap);
4976 | }
4977 |
4978 | return pi;
4979 | }
4980 |
4981 | proto_item *
4982 | proto_tree_add_time_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
4983 | int start, int length, nstime_t *value_ptr,
4984 | const char *format, ...)
4985 | {
4986 | proto_item *pi;
4987 | va_list ap;
4988 |
4989 | pi = proto_tree_add_time(tree, hfindex, tvb, start, length, value_ptr);
4990 | if (pi != tree) {
4991 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 4991, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
4992 |
4993 | va_start(ap, format)__builtin_va_start(ap, format);
4994 | proto_tree_set_representation(pi, format, ap);
4995 | va_end(ap)__builtin_va_end(ap);
4996 | }
4997 |
4998 | return pi;
4999 | }
5000 |
5001 | /* Set the FT_*TIME value */
5002 | static void
5003 | proto_tree_set_time(field_info *fi, const nstime_t *value_ptr)
5004 | {
5005 | DISSECTOR_ASSERT(value_ptr != NULL)((void) ((value_ptr != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 5005, "value_ptr != ((void*)0)" ))));
5006 |
5007 | fvalue_set_time(fi->value, value_ptr);
5008 | }
5009 |
5010 | /* Add a FT_IPXNET to a proto_tree */
5011 | proto_item *
5012 | proto_tree_add_ipxnet(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
5013 | int length, uint32_t value)
5014 | {
5015 | proto_item *pi;
5016 | header_field_info *hfinfo;
5017 |
5018 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
5019 |
5020 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5020 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5020, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5020, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5020, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
5021 |
5022 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_IPXNET)((void) (((hfinfo)->type == FT_IPXNET) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_IPXNET", "epan/proto.c" , 5022, ((hfinfo))->abbrev))));
5023 |
5024 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
5025 | proto_tree_set_ipxnet(PNODE_FINFO(pi)((pi)->finfo), value);
5026 |
5027 | return pi;
5028 | }
5029 |
5030 | proto_item *
5031 | proto_tree_add_ipxnet_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5032 | int start, int length, uint32_t value,
5033 | const char *format, ...)
5034 | {
5035 | proto_item *pi;
5036 | va_list ap;
5037 |
5038 | pi = proto_tree_add_ipxnet(tree, hfindex, tvb, start, length, value);
5039 | if (pi != tree) {
5040 | va_start(ap, format)__builtin_va_start(ap, format);
5041 | proto_tree_set_representation_value(pi, format, ap);
5042 | va_end(ap)__builtin_va_end(ap);
5043 | }
5044 |
5045 | return pi;
5046 | }
5047 |
5048 | proto_item *
5049 | proto_tree_add_ipxnet_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5050 | int start, int length, uint32_t value,
5051 | const char *format, ...)
5052 | {
5053 | proto_item *pi;
5054 | va_list ap;
5055 |
5056 | pi = proto_tree_add_ipxnet(tree, hfindex, tvb, start, length, value);
5057 | if (pi != tree) {
5058 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 5058, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
5059 |
5060 | va_start(ap, format)__builtin_va_start(ap, format);
5061 | proto_tree_set_representation(pi, format, ap);
5062 | va_end(ap)__builtin_va_end(ap);
5063 | }
5064 |
5065 | return pi;
5066 | }
5067 |
5068 | /* Set the FT_IPXNET value */
5069 | static void
5070 | proto_tree_set_ipxnet(field_info *fi, uint32_t value)
5071 | {
5072 | fvalue_set_uinteger(fi->value, value);
5073 | }
5074 |
5075 | /* Add a FT_IPv4 to a proto_tree */
5076 | proto_item *
5077 | proto_tree_add_ipv4(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
5078 | int length, ws_in4_addr value)
5079 | {
5080 | proto_item *pi;
5081 | header_field_info *hfinfo;
5082 |
5083 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
5084 |
5085 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5085 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5085, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5085, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5085, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
5086 |
5087 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_IPv4)((void) (((hfinfo)->type == FT_IPv4) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_IPv4", "epan/proto.c", 5087 , ((hfinfo))->abbrev))));
5088 |
5089 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
5090 | proto_tree_set_ipv4(PNODE_FINFO(pi)((pi)->finfo), value);
5091 |
5092 | return pi;
5093 | }
5094 |
5095 | proto_item *
5096 | proto_tree_add_ipv4_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5097 | int start, int length, ws_in4_addr value,
5098 | const char *format, ...)
5099 | {
5100 | proto_item *pi;
5101 | va_list ap;
5102 |
5103 | pi = proto_tree_add_ipv4(tree, hfindex, tvb, start, length, value);
5104 | if (pi != tree) {
5105 | va_start(ap, format)__builtin_va_start(ap, format);
5106 | proto_tree_set_representation_value(pi, format, ap);
5107 | va_end(ap)__builtin_va_end(ap);
5108 | }
5109 |
5110 | return pi;
5111 | }
5112 |
5113 | proto_item *
5114 | proto_tree_add_ipv4_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5115 | int start, int length, ws_in4_addr value,
5116 | const char *format, ...)
5117 | {
5118 | proto_item *pi;
5119 | va_list ap;
5120 |
5121 | pi = proto_tree_add_ipv4(tree, hfindex, tvb, start, length, value);
5122 | if (pi != tree) {
5123 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 5123, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
5124 |
5125 | va_start(ap, format)__builtin_va_start(ap, format);
5126 | proto_tree_set_representation(pi, format, ap);
5127 | va_end(ap)__builtin_va_end(ap);
5128 | }
5129 |
5130 | return pi;
5131 | }
5132 |
5133 | /* Set the FT_IPv4 value */
5134 | static void
5135 | proto_tree_set_ipv4(field_info *fi, ws_in4_addr value)
5136 | {
5137 | ipv4_addr_and_mask ipv4;
5138 | ws_ipv4_addr_and_mask_init(&ipv4, value, 32);
5139 | fvalue_set_ipv4(fi->value, &ipv4);
5140 | }
5141 |
5142 | /* Add a FT_IPv6 to a proto_tree */
5143 | proto_item *
5144 | proto_tree_add_ipv6(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
5145 | int length, const ws_in6_addr *value)
5146 | {
5147 | proto_item *pi;
5148 | header_field_info *hfinfo;
5149 |
5150 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
5151 |
5152 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5152 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5152, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5152, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5152, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
5153 |
5154 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_IPv6)((void) (((hfinfo)->type == FT_IPv6) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_IPv6", "epan/proto.c", 5154 , ((hfinfo))->abbrev))));
5155 |
5156 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
5157 | proto_tree_set_ipv6(PNODE_FINFO(pi)((pi)->finfo), value);
5158 |
5159 | return pi;
5160 | }
5161 |
5162 | proto_item *
5163 | proto_tree_add_ipv6_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5164 | int start, int length,
5165 | const ws_in6_addr *value_ptr,
5166 | const char *format, ...)
5167 | {
5168 | proto_item *pi;
5169 | va_list ap;
5170 |
5171 | pi = proto_tree_add_ipv6(tree, hfindex, tvb, start, length, value_ptr);
5172 | if (pi != tree) {
5173 | va_start(ap, format)__builtin_va_start(ap, format);
5174 | proto_tree_set_representation_value(pi, format, ap);
5175 | va_end(ap)__builtin_va_end(ap);
5176 | }
5177 |
5178 | return pi;
5179 | }
5180 |
5181 | proto_item *
5182 | proto_tree_add_ipv6_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5183 | int start, int length,
5184 | const ws_in6_addr *value_ptr,
5185 | const char *format, ...)
5186 | {
5187 | proto_item *pi;
5188 | va_list ap;
5189 |
5190 | pi = proto_tree_add_ipv6(tree, hfindex, tvb, start, length, value_ptr);
5191 | if (pi != tree) {
5192 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 5192, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
5193 |
5194 | va_start(ap, format)__builtin_va_start(ap, format);
5195 | proto_tree_set_representation(pi, format, ap);
5196 | va_end(ap)__builtin_va_end(ap);
5197 | }
5198 |
5199 | return pi;
5200 | }
5201 |
5202 | /* Set the FT_IPv6 value */
5203 | static void
5204 | proto_tree_set_ipv6(field_info *fi, const ws_in6_addr *value)
5205 | {
5206 | DISSECTOR_ASSERT(value != NULL)((void) ((value != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 5206, "value != ((void*)0)" ))));
5207 | ipv6_addr_and_prefix ipv6;
5208 | ipv6.addr = *value;
5209 | ipv6.prefix = 128;
5210 | fvalue_set_ipv6(fi->value, &ipv6);
5211 | }
5212 |
5213 | static void
5214 | proto_tree_set_ipv6_tvb(field_info *fi, tvbuff_t *tvb, int start, int length)
5215 | {
5216 | proto_tree_set_ipv6(fi, (const ws_in6_addr *)tvb_get_ptr(tvb, start, length));
5217 | }
5218 |
5219 | /* Set the FT_FCWWN value */
5220 | static void
5221 | proto_tree_set_fcwwn(field_info *fi, const uint8_t* value_ptr)
5222 | {
5223 | DISSECTOR_ASSERT(value_ptr != NULL)((void) ((value_ptr != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 5223, "value_ptr != ((void*)0)" ))));
5224 | fvalue_set_fcwwn(fi->value, value_ptr);
5225 | }
5226 |
5227 | static void
5228 | proto_tree_set_fcwwn_tvb(field_info *fi, tvbuff_t *tvb, int start, int length)
5229 | {
5230 | proto_tree_set_fcwwn(fi, tvb_get_ptr(tvb, start, length));
5231 | }
5232 |
5233 | /* Add a FT_GUID to a proto_tree */
5234 | proto_item *
5235 | proto_tree_add_guid(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
5236 | int length, const e_guid_t *value_ptr)
5237 | {
5238 | proto_item *pi;
5239 | header_field_info *hfinfo;
5240 |
5241 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
5242 |
5243 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5243 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5243, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5243, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5243, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
5244 |
5245 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_GUID)((void) (((hfinfo)->type == FT_GUID) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_GUID", "epan/proto.c", 5245 , ((hfinfo))->abbrev))));
5246 |
5247 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
5248 | proto_tree_set_guid(PNODE_FINFO(pi)((pi)->finfo), value_ptr);
5249 |
5250 | return pi;
5251 | }
5252 |
5253 | proto_item *
5254 | proto_tree_add_guid_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5255 | int start, int length,
5256 | const e_guid_t *value_ptr,
5257 | const char *format, ...)
5258 | {
5259 | proto_item *pi;
5260 | va_list ap;
5261 |
5262 | pi = proto_tree_add_guid(tree, hfindex, tvb, start, length, value_ptr);
5263 | if (pi != tree) {
5264 | va_start(ap, format)__builtin_va_start(ap, format);
5265 | proto_tree_set_representation_value(pi, format, ap);
5266 | va_end(ap)__builtin_va_end(ap);
5267 | }
5268 |
5269 | return pi;
5270 | }
5271 |
5272 | proto_item *
5273 | proto_tree_add_guid_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5274 | int start, int length, const e_guid_t *value_ptr,
5275 | const char *format, ...)
5276 | {
5277 | proto_item *pi;
5278 | va_list ap;
5279 |
5280 | pi = proto_tree_add_guid(tree, hfindex, tvb, start, length, value_ptr);
5281 | if (pi != tree) {
5282 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 5282, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
5283 |
5284 | va_start(ap, format)__builtin_va_start(ap, format);
5285 | proto_tree_set_representation(pi, format, ap);
5286 | va_end(ap)__builtin_va_end(ap);
5287 | }
5288 |
5289 | return pi;
5290 | }
5291 |
5292 | /* Set the FT_GUID value */
5293 | static void
5294 | proto_tree_set_guid(field_info *fi, const e_guid_t *value_ptr)
5295 | {
5296 | DISSECTOR_ASSERT(value_ptr != NULL)((void) ((value_ptr != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 5296, "value_ptr != ((void*)0)" ))));
5297 | fvalue_set_guid(fi->value, value_ptr);
5298 | }
5299 |
5300 | static void
5301 | proto_tree_set_guid_tvb(field_info *fi, tvbuff_t *tvb, int start,
5302 | const unsigned encoding)
5303 | {
5304 | e_guid_t guid;
5305 |
5306 | tvb_get_guid(tvb, start, &guid, encoding);
5307 | proto_tree_set_guid(fi, &guid);
5308 | }
5309 |
5310 | /* Add a FT_OID to a proto_tree */
5311 | proto_item *
5312 | proto_tree_add_oid(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
5313 | int length, const uint8_t* value_ptr)
5314 | {
5315 | proto_item *pi;
5316 | header_field_info *hfinfo;
5317 |
5318 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
5319 |
5320 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5320 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5320, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5320, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5320, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
5321 |
5322 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_OID)((void) (((hfinfo)->type == FT_OID) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_OID", "epan/proto.c", 5322 , ((hfinfo))->abbrev))));
5323 |
5324 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
5325 | proto_tree_set_oid(PNODE_FINFO(pi)((pi)->finfo), value_ptr, length);
5326 |
5327 | return pi;
5328 | }
5329 |
5330 | proto_item *
5331 | proto_tree_add_oid_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5332 | int start, int length,
5333 | const uint8_t* value_ptr,
5334 | const char *format, ...)
5335 | {
5336 | proto_item *pi;
5337 | va_list ap;
5338 |
5339 | pi = proto_tree_add_oid(tree, hfindex, tvb, start, length, value_ptr);
5340 | if (pi != tree) {
5341 | va_start(ap, format)__builtin_va_start(ap, format);
5342 | proto_tree_set_representation_value(pi, format, ap);
5343 | va_end(ap)__builtin_va_end(ap);
5344 | }
5345 |
5346 | return pi;
5347 | }
5348 |
5349 | proto_item *
5350 | proto_tree_add_oid_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5351 | int start, int length, const uint8_t* value_ptr,
5352 | const char *format, ...)
5353 | {
5354 | proto_item *pi;
5355 | va_list ap;
5356 |
5357 | pi = proto_tree_add_oid(tree, hfindex, tvb, start, length, value_ptr);
5358 | if (pi != tree) {
5359 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 5359, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
5360 |
5361 | va_start(ap, format)__builtin_va_start(ap, format);
5362 | proto_tree_set_representation(pi, format, ap);
5363 | va_end(ap)__builtin_va_end(ap);
5364 | }
5365 |
5366 | return pi;
5367 | }
5368 |
5369 | /* Set the FT_OID value */
5370 | static void
5371 | proto_tree_set_oid(field_info *fi, const uint8_t* value_ptr, int length)
5372 | {
5373 | GByteArray *bytes;
5374 |
5375 | DISSECTOR_ASSERT(value_ptr != NULL || length == 0)((void) ((value_ptr != ((void*)0) || length == 0) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 5375, "value_ptr != ((void*)0) || length == 0" ))));
5376 |
5377 | bytes = g_byte_array_new();
5378 | if (length > 0) {
5379 | g_byte_array_append(bytes, value_ptr, length);
5380 | }
5381 | fvalue_set_byte_array(fi->value, bytes);
5382 | }
5383 |
5384 | static void
5385 | proto_tree_set_oid_tvb(field_info *fi, tvbuff_t *tvb, int start, int length)
5386 | {
5387 | proto_tree_set_oid(fi, tvb_get_ptr(tvb, start, length), length);
5388 | }
5389 |
5390 | /* Set the FT_SYSTEM_ID value */
5391 | static void
5392 | proto_tree_set_system_id(field_info *fi, const uint8_t* value_ptr, int length)
5393 | {
5394 | GByteArray *bytes;
5395 |
5396 | DISSECTOR_ASSERT(value_ptr != NULL || length == 0)((void) ((value_ptr != ((void*)0) || length == 0) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 5396, "value_ptr != ((void*)0) || length == 0" ))));
5397 |
5398 | bytes = g_byte_array_new();
5399 | if (length > 0) {
5400 | g_byte_array_append(bytes, value_ptr, length);
5401 | }
5402 | fvalue_set_byte_array(fi->value, bytes);
5403 | }
5404 |
5405 | static void
5406 | proto_tree_set_system_id_tvb(field_info *fi, tvbuff_t *tvb, int start, int length)
5407 | {
5408 | proto_tree_set_system_id(fi, tvb_get_ptr(tvb, start, length), length);
5409 | }
5410 |
5411 | /* Add a FT_STRING, FT_STRINGZ, FT_STRINGZPAD, or FT_STRINGZTRUNC to a
5412 | * proto_tree. Creates own copy of string, and frees it when the proto_tree
5413 | * is destroyed. */
5414 | proto_item *
5415 | proto_tree_add_string(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
5416 | int length, const char* value)
5417 | {
5418 | proto_item *pi;
5419 | header_field_info *hfinfo;
5420 | int item_length;
5421 |
5422 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 5422, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 5422, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5422, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
5423 | get_hfi_length(hfinfo, tvb, start, &length, &item_length, ENC_NA0x00000000);
5424 | /*
5425 | * Special case - if the length is 0, skip the test, so that
5426 | * we can have an empty string right after the end of the
5427 | * packet. (This handles URL-encoded forms where the last field
5428 | * has no value so the form ends right after the =.)
5429 | *
5430 | * XXX - length zero makes sense for FT_STRING, and more or less
5431 | * for FT_STRINGZTRUNC, and FT_STRINGZPAD, but doesn't make sense
5432 | * for FT_STRINGZ (except that a number of fields that should be
5433 | * one of the others are actually registered as FT_STRINGZ.)
5434 | */
5435 | if (item_length != 0)
5436 | test_length(hfinfo, tvb, start, item_length, ENC_NA0x00000000);
5437 |
5438 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
5439 |
5440 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5440 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5440, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5440, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5440, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
5441 |
5442 | DISSECTOR_ASSERT_FIELD_TYPE_IS_STRING(hfinfo)((void) ((((hfinfo)->type) == FT_STRING || ((hfinfo)->type ) == FT_STRINGZ || ((hfinfo)->type) == FT_STRINGZPAD || (( hfinfo)->type) == FT_STRINGZTRUNC || ((hfinfo)->type) == FT_UINT_STRING || ((hfinfo)->type) == FT_AX25) ? (void)0 : (proto_report_dissector_bug("%s:%u: field %s is not of type FT_STRING, FT_STRINGZ, FT_STRINGZPAD, FT_STRINGZTRUNC, or FT_UINT_STRING" , "epan/proto.c", 5442, ((hfinfo))->abbrev))));
5443 |
5444 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
5445 | DISSECTOR_ASSERT(length >= 0)((void) ((length >= 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 5445, "length >= 0" ))));
5446 |
5447 | WS_UTF_8_CHECK(value, -1)do { const char *__uni_endptr; if (1 && (value) != (( void*)0) && !g_utf8_validate(value, -1, &__uni_endptr )) { do { if (1) { ws_log_utf8_full("UTF-8", LOG_LEVEL_DEBUG, "epan/proto.c", 5447, __func__, value, -1, __uni_endptr); } } while (0); } } while (0);
5448 | proto_tree_set_string(PNODE_FINFO(pi)((pi)->finfo), value);
5449 |
5450 | return pi;
5451 | }
5452 |
5453 | proto_item *
5454 | proto_tree_add_string_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5455 | int start, int length, const char* value,
5456 | const char *format,
5457 | ...)
5458 | {
5459 | proto_item *pi;
5460 | va_list ap;
5461 |
5462 | pi = proto_tree_add_string(tree, hfindex, tvb, start, length, value);
5463 | if (pi != tree) {
5464 | va_start(ap, format)__builtin_va_start(ap, format);
5465 | proto_tree_set_representation_value(pi, format, ap);
5466 | va_end(ap)__builtin_va_end(ap);
5467 | }
5468 |
5469 | return pi;
5470 | }
5471 |
5472 | proto_item *
5473 | proto_tree_add_string_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5474 | int start, int length, const char* value,
5475 | const char *format, ...)
5476 | {
5477 | proto_item *pi;
5478 | va_list ap;
5479 |
5480 | pi = proto_tree_add_string(tree, hfindex, tvb, start, length, value);
5481 | if (pi != tree) {
5482 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 5482, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
5483 |
5484 | va_start(ap, format)__builtin_va_start(ap, format);
5485 | proto_tree_set_representation(pi, format, ap);
5486 | va_end(ap)__builtin_va_end(ap);
5487 | }
5488 |
5489 | return pi;
5490 | }
5491 |
5492 | /* Set the FT_STRING value */
5493 | static void
5494 | proto_tree_set_string(field_info *fi, const char* value)
5495 | {
5496 | if (value) {
5497 | fvalue_set_string(fi->value, value);
5498 | } else {
5499 | /*
5500 | * XXX - why is a null value for a string field
5501 | * considered valid?
5502 | */
5503 | fvalue_set_string(fi->value, "[ Null ]");
5504 | }
5505 | }
5506 |
5507 | /* Set the FT_AX25 value */
5508 | static void
5509 | proto_tree_set_ax25(field_info *fi, const uint8_t* value)
5510 | {
5511 | fvalue_set_ax25(fi->value, value);
5512 | }
5513 |
5514 | static void
5515 | proto_tree_set_ax25_tvb(field_info *fi, tvbuff_t *tvb, int start)
5516 | {
5517 | proto_tree_set_ax25(fi, tvb_get_ptr(tvb, start, 7));
5518 | }
5519 |
5520 | /* Set the FT_VINES value */
5521 | static void
5522 | proto_tree_set_vines(field_info *fi, const uint8_t* value)
5523 | {
5524 | fvalue_set_vines(fi->value, value);
5525 | }
5526 |
5527 | static void
5528 | proto_tree_set_vines_tvb(field_info *fi, tvbuff_t *tvb, int start)
5529 | {
5530 | proto_tree_set_vines(fi, tvb_get_ptr(tvb, start, FT_VINES_ADDR_LEN6));
5531 | }
5532 |
5533 | /* Add a FT_ETHER to a proto_tree */
5534 | proto_item *
5535 | proto_tree_add_ether(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
5536 | int length, const uint8_t* value)
5537 | {
5538 | proto_item *pi;
5539 | header_field_info *hfinfo;
5540 |
5541 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
5542 |
5543 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5543 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5543, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5543, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5543, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
5544 |
5545 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_ETHER)((void) (((hfinfo)->type == FT_ETHER) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_ETHER", "epan/proto.c", 5545, ((hfinfo))->abbrev))));
5546 |
5547 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
5548 | proto_tree_set_ether(PNODE_FINFO(pi)((pi)->finfo), value);
5549 |
5550 | return pi;
5551 | }
5552 |
5553 | proto_item *
5554 | proto_tree_add_ether_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5555 | int start, int length, const uint8_t* value,
5556 | const char *format, ...)
5557 | {
5558 | proto_item *pi;
5559 | va_list ap;
5560 |
5561 | pi = proto_tree_add_ether(tree, hfindex, tvb, start, length, value);
5562 | if (pi != tree) {
5563 | va_start(ap, format)__builtin_va_start(ap, format);
5564 | proto_tree_set_representation_value(pi, format, ap);
5565 | va_end(ap)__builtin_va_end(ap);
5566 | }
5567 |
5568 | return pi;
5569 | }
5570 |
5571 | proto_item *
5572 | proto_tree_add_ether_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5573 | int start, int length, const uint8_t* value,
5574 | const char *format, ...)
5575 | {
5576 | proto_item *pi;
5577 | va_list ap;
5578 |
5579 | pi = proto_tree_add_ether(tree, hfindex, tvb, start, length, value);
5580 | if (pi != tree) {
5581 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 5581, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
5582 |
5583 | va_start(ap, format)__builtin_va_start(ap, format);
5584 | proto_tree_set_representation(pi, format, ap);
5585 | va_end(ap)__builtin_va_end(ap);
5586 | }
5587 |
5588 | return pi;
5589 | }
5590 |
5591 | /* Set the FT_ETHER value */
5592 | static void
5593 | proto_tree_set_ether(field_info *fi, const uint8_t* value)
5594 | {
5595 | fvalue_set_ether(fi->value, value);
5596 | }
5597 |
5598 | static void
5599 | proto_tree_set_ether_tvb(field_info *fi, tvbuff_t *tvb, int start)
5600 | {
5601 | proto_tree_set_ether(fi, tvb_get_ptr(tvb, start, FT_ETHER_LEN6));
5602 | }
5603 |
5604 | /* Add a FT_BOOLEAN to a proto_tree */
5605 | proto_item *
5606 | proto_tree_add_boolean(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
5607 | int length, uint64_t value)
5608 | {
5609 | proto_item *pi;
5610 | header_field_info *hfinfo;
5611 |
5612 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
5613 |
5614 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5614 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5614, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5614, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5614, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
5615 |
5616 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_BOOLEAN)((void) (((hfinfo)->type == FT_BOOLEAN) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_BOOLEAN", "epan/proto.c" , 5616, ((hfinfo))->abbrev))));
5617 |
5618 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
5619 | proto_tree_set_boolean(PNODE_FINFO(pi)((pi)->finfo), value);
5620 |
5621 | return pi;
5622 | }
5623 |
5624 | proto_item *
5625 | proto_tree_add_boolean_format_value(proto_tree *tree, int hfindex,
5626 | tvbuff_t *tvb, int start, int length,
5627 | uint64_t value, const char *format, ...)
5628 | {
5629 | proto_item *pi;
5630 | va_list ap;
5631 |
5632 | pi = proto_tree_add_boolean(tree, hfindex, tvb, start, length, value);
5633 | if (pi != tree) {
5634 | va_start(ap, format)__builtin_va_start(ap, format);
5635 | proto_tree_set_representation_value(pi, format, ap);
5636 | va_end(ap)__builtin_va_end(ap);
5637 | }
5638 |
5639 | return pi;
5640 | }
5641 |
5642 | proto_item *
5643 | proto_tree_add_boolean_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5644 | int start, int length, uint64_t value,
5645 | const char *format, ...)
5646 | {
5647 | proto_item *pi;
5648 | va_list ap;
5649 |
5650 | pi = proto_tree_add_boolean(tree, hfindex, tvb, start, length, value);
5651 | if (pi != tree) {
5652 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 5652, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
5653 |
5654 | va_start(ap, format)__builtin_va_start(ap, format);
5655 | proto_tree_set_representation(pi, format, ap);
5656 | va_end(ap)__builtin_va_end(ap);
5657 | }
5658 |
5659 | return pi;
5660 | }
5661 |
5662 | /* Set the FT_BOOLEAN value */
5663 | static void
5664 | proto_tree_set_boolean(field_info *fi, uint64_t value)
5665 | {
5666 | proto_tree_set_uint64(fi, value);
5667 | }
5668 |
5669 | /* Generate, into "buf", a string showing the bits of a bitfield.
5670 | Return a pointer to the character after that string. */
5671 | static char *
5672 | other_decode_bitfield_value(char *buf, const uint64_t val, const uint64_t mask, const int width)
5673 | {
5674 | int i = 0;
5675 | uint64_t bit;
5676 | char *p;
5677 |
5678 | p = buf;
5679 |
5680 | /* This is a devel error. It is safer to stop here. */
5681 | DISSECTOR_ASSERT(width >= 1)((void) ((width >= 1) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 5681, "width >= 1" ))));
5682 |
5683 | bit = UINT64_C(1)1UL << (width - 1);
5684 | for (;;) {
5685 | if (mask & bit) {
5686 | /* This bit is part of the field. Show its value. */
5687 | if (val & bit)
5688 | *p++ = '1';
5689 | else
5690 | *p++ = '0';
5691 | } else {
5692 | /* This bit is not part of the field. */
5693 | *p++ = '.';
5694 | }
5695 | bit >>= 1;
5696 | i++;
5697 | if (i >= width)
5698 | break;
5699 | if (i % 4 == 0)
5700 | *p++ = ' ';
5701 | }
5702 | *p = '\0';
5703 | return p;
5704 | }
5705 |
5706 | static char *
5707 | decode_bitfield_value(char *buf, const uint64_t val, const uint64_t mask, const int width)
5708 | {
5709 | char *p;
5710 |
5711 | p = other_decode_bitfield_value(buf, val, mask, width);
5712 | p = g_stpcpy(p, " = ");
5713 |
5714 | return p;
5715 | }
5716 |
5717 | static char *
5718 | other_decode_bitfield_varint_value(char *buf, uint64_t val, uint64_t mask, const int width)
5719 | {
5720 | int i = 0;
5721 | uint64_t bit;
5722 | char *p;
5723 |
5724 | p = buf;
5725 |
5726 | /* This is a devel error. It is safer to stop here. */
5727 | DISSECTOR_ASSERT(width >= 1)((void) ((width >= 1) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 5727, "width >= 1" ))));
5728 |
5729 | bit = UINT64_C(1)1UL << (width - 1);
5730 | for (;;) {
5731 | if (((8-(i % 8)) != 8) && /* MSB is never used for value. */
5732 | (mask & bit)) {
5733 | /* This bit is part of the field. Show its value. */
5734 | if (val & bit)
5735 | *p++ = '1';
5736 | else
5737 | *p++ = '0';
5738 | } else {
5739 | /* This bit is not part of the field. */
5740 | *p++ = '.';
5741 | }
5742 | bit >>= 1;
5743 | i++;
5744 | if (i >= width)
5745 | break;
5746 | if (i % 4 == 0)
5747 | *p++ = ' ';
5748 | }
5749 |
5750 | *p = '\0';
5751 | return p;
5752 | }
5753 |
5754 | static char *
5755 | decode_bitfield_varint_value(char *buf, const uint64_t val, const uint64_t mask, const int width)
5756 | {
5757 | char *p;
5758 |
5759 | p = other_decode_bitfield_varint_value(buf, val, mask, width);
5760 | p = g_stpcpy(p, " = ");
5761 |
5762 | return p;
5763 | }
5764 |
5765 | /* Add a FT_FLOAT to a proto_tree */
5766 | proto_item *
5767 | proto_tree_add_float(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
5768 | int length, float value)
5769 | {
5770 | proto_item *pi;
5771 | header_field_info *hfinfo;
5772 |
5773 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
5774 |
5775 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5775 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5775, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5775, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5775, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
5776 |
5777 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_FLOAT)((void) (((hfinfo)->type == FT_FLOAT) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_FLOAT", "epan/proto.c", 5777, ((hfinfo))->abbrev))));
5778 |
5779 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
5780 | proto_tree_set_float(PNODE_FINFO(pi)((pi)->finfo), value);
5781 |
5782 | return pi;
5783 | }
5784 |
5785 | proto_item *
5786 | proto_tree_add_float_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5787 | int start, int length, float value,
5788 | const char *format, ...)
5789 | {
5790 | proto_item *pi;
5791 | va_list ap;
5792 |
5793 | pi = proto_tree_add_float(tree, hfindex, tvb, start, length, value);
5794 | if (pi != tree) {
5795 | va_start(ap, format)__builtin_va_start(ap, format);
5796 | proto_tree_set_representation_value(pi, format, ap);
5797 | va_end(ap)__builtin_va_end(ap);
5798 | }
5799 |
5800 | return pi;
5801 | }
5802 |
5803 | proto_item *
5804 | proto_tree_add_float_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5805 | int start, int length, float value,
5806 | const char *format, ...)
5807 | {
5808 | proto_item *pi;
5809 | va_list ap;
5810 |
5811 | pi = proto_tree_add_float(tree, hfindex, tvb, start, length, value);
5812 | if (pi != tree) {
5813 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 5813, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
5814 |
5815 | va_start(ap, format)__builtin_va_start(ap, format);
5816 | proto_tree_set_representation(pi, format, ap);
5817 | va_end(ap)__builtin_va_end(ap);
5818 | }
5819 |
5820 | return pi;
5821 | }
5822 |
5823 | /* Set the FT_FLOAT value */
5824 | static void
5825 | proto_tree_set_float(field_info *fi, float value)
5826 | {
5827 | fvalue_set_floating(fi->value, value);
5828 | }
5829 |
5830 | /* Add a FT_DOUBLE to a proto_tree */
5831 | proto_item *
5832 | proto_tree_add_double(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
5833 | int length, double value)
5834 | {
5835 | proto_item *pi;
5836 | header_field_info *hfinfo;
5837 |
5838 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
5839 |
5840 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5840 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5840, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5840, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5840, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
5841 |
5842 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_DOUBLE)((void) (((hfinfo)->type == FT_DOUBLE) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_DOUBLE", "epan/proto.c" , 5842, ((hfinfo))->abbrev))));
5843 |
5844 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
5845 | proto_tree_set_double(PNODE_FINFO(pi)((pi)->finfo), value);
5846 |
5847 | return pi;
5848 | }
5849 |
5850 | proto_item *
5851 | proto_tree_add_double_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5852 | int start, int length, double value,
5853 | const char *format, ...)
5854 | {
5855 | proto_item *pi;
5856 | va_list ap;
5857 |
5858 | pi = proto_tree_add_double(tree, hfindex, tvb, start, length, value);
5859 | if (pi != tree) {
5860 | va_start(ap, format)__builtin_va_start(ap, format);
5861 | proto_tree_set_representation_value(pi, format, ap);
5862 | va_end(ap)__builtin_va_end(ap);
5863 | }
5864 |
5865 | return pi;
5866 | }
5867 |
5868 | proto_item *
5869 | proto_tree_add_double_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5870 | int start, int length, double value,
5871 | const char *format, ...)
5872 | {
5873 | proto_item *pi;
5874 | va_list ap;
5875 |
5876 | pi = proto_tree_add_double(tree, hfindex, tvb, start, length, value);
5877 | if (pi != tree) {
5878 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 5878, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
5879 |
5880 | va_start(ap, format)__builtin_va_start(ap, format);
5881 | proto_tree_set_representation(pi, format, ap);
5882 | va_end(ap)__builtin_va_end(ap);
5883 | }
5884 |
5885 | return pi;
5886 | }
5887 |
5888 | /* Set the FT_DOUBLE value */
5889 | static void
5890 | proto_tree_set_double(field_info *fi, double value)
5891 | {
5892 | fvalue_set_floating(fi->value, value);
5893 | }
5894 |
5895 | /* Add FT_CHAR or FT_UINT{8,16,24,32} to a proto_tree */
5896 | proto_item *
5897 | proto_tree_add_uint(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
5898 | int length, uint32_t value)
5899 | {
5900 | proto_item *pi = NULL((void*)0);
5901 | header_field_info *hfinfo;
5902 |
5903 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
5904 |
5905 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5905 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5905, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5905, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5905, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
5906 |
5907 | switch (hfinfo->type) {
5908 | case FT_CHAR:
5909 | case FT_UINT8:
5910 | case FT_UINT16:
5911 | case FT_UINT24:
5912 | case FT_UINT32:
5913 | case FT_FRAMENUM:
5914 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
5915 | proto_tree_set_uint(PNODE_FINFO(pi)((pi)->finfo), value);
5916 | break;
5917 |
5918 | default:
5919 | REPORT_DISSECTOR_BUG("field %s is not of type FT_CHAR, FT_UINT8, FT_UINT16, FT_UINT24, FT_UINT32, or FT_FRAMENUM",proto_report_dissector_bug("field %s is not of type FT_CHAR, FT_UINT8, FT_UINT16, FT_UINT24, FT_UINT32, or FT_FRAMENUM" , hfinfo->abbrev)
5920 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_CHAR, FT_UINT8, FT_UINT16, FT_UINT24, FT_UINT32, or FT_FRAMENUM" , hfinfo->abbrev);
5921 | }
5922 |
5923 | return pi;
5924 | }
5925 |
5926 | proto_item *
5927 | proto_tree_add_uint_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5928 | int start, int length, uint32_t value,
5929 | const char *format, ...)
5930 | {
5931 | proto_item *pi;
5932 | va_list ap;
5933 |
5934 | pi = proto_tree_add_uint(tree, hfindex, tvb, start, length, value);
5935 | if (pi != tree) {
5936 | va_start(ap, format)__builtin_va_start(ap, format);
5937 | proto_tree_set_representation_value(pi, format, ap);
5938 | va_end(ap)__builtin_va_end(ap);
5939 | }
5940 |
5941 | return pi;
5942 | }
5943 |
5944 | proto_item *
5945 | proto_tree_add_uint_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
5946 | int start, int length, uint32_t value,
5947 | const char *format, ...)
5948 | {
5949 | proto_item *pi;
5950 | va_list ap;
5951 |
5952 | pi = proto_tree_add_uint(tree, hfindex, tvb, start, length, value);
5953 | if (pi != tree) {
5954 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 5954, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
5955 |
5956 | va_start(ap, format)__builtin_va_start(ap, format);
5957 | proto_tree_set_representation(pi, format, ap);
5958 | va_end(ap)__builtin_va_end(ap);
5959 | }
5960 |
5961 | return pi;
5962 | }
5963 |
5964 | /* Set the FT_UINT{8,16,24,32} value */
5965 | static void
5966 | proto_tree_set_uint(field_info *fi, uint32_t value)
5967 | {
5968 | const header_field_info *hfinfo;
5969 | uint32_t integer;
5970 |
5971 | hfinfo = fi->hfinfo;
5972 | integer = value;
5973 |
5974 | if (hfinfo->bitmask) {
5975 | /* Mask out irrelevant portions */
5976 | integer &= (uint32_t)(hfinfo->bitmask);
5977 |
5978 | /* Shift bits */
5979 | integer >>= hfinfo_bitshift(hfinfo);
5980 |
5981 | FI_SET_FLAG(fi, FI_BITS_OFFSET(hfinfo_bitoffset(hfinfo)))do { if (fi) (fi)->flags = (fi)->flags | ((((hfinfo_bitoffset (hfinfo)) & 63) << 5)); } while(0);
5982 | FI_SET_FLAG(fi, FI_BITS_SIZE(hfinfo_mask_bitwidth(hfinfo)))do { if (fi) (fi)->flags = (fi)->flags | ((((hfinfo_mask_bitwidth (hfinfo)) & 63) << 12)); } while(0);
5983 | }
5984 |
5985 | fvalue_set_uinteger(fi->value, integer);
5986 | }
5987 |
5988 | /* Add FT_UINT{40,48,56,64} to a proto_tree */
5989 | proto_item *
5990 | proto_tree_add_uint64(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
5991 | int length, uint64_t value)
5992 | {
5993 | proto_item *pi = NULL((void*)0);
5994 | header_field_info *hfinfo;
5995 |
5996 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
5997 |
5998 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5998 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5998, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 5998, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 5998, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
5999 |
6000 | switch (hfinfo->type) {
6001 | case FT_UINT40:
6002 | case FT_UINT48:
6003 | case FT_UINT56:
6004 | case FT_UINT64:
6005 | case FT_FRAMENUM:
6006 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
6007 | proto_tree_set_uint64(PNODE_FINFO(pi)((pi)->finfo), value);
6008 | break;
6009 |
6010 | default:
6011 | REPORT_DISSECTOR_BUG("field %s is not of type FT_UINT40, FT_UINT48, FT_UINT56, FT_UINT64, or FT_FRAMENUM",proto_report_dissector_bug("field %s is not of type FT_UINT40, FT_UINT48, FT_UINT56, FT_UINT64, or FT_FRAMENUM" , hfinfo->abbrev)
6012 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_UINT40, FT_UINT48, FT_UINT56, FT_UINT64, or FT_FRAMENUM" , hfinfo->abbrev);
6013 | }
6014 |
6015 | return pi;
6016 | }
6017 |
6018 | proto_item *
6019 | proto_tree_add_uint64_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
6020 | int start, int length, uint64_t value,
6021 | const char *format, ...)
6022 | {
6023 | proto_item *pi;
6024 | va_list ap;
6025 |
6026 | pi = proto_tree_add_uint64(tree, hfindex, tvb, start, length, value);
6027 | if (pi != tree) {
6028 | va_start(ap, format)__builtin_va_start(ap, format);
6029 | proto_tree_set_representation_value(pi, format, ap);
6030 | va_end(ap)__builtin_va_end(ap);
6031 | }
6032 |
6033 | return pi;
6034 | }
6035 |
6036 | proto_item *
6037 | proto_tree_add_uint64_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
6038 | int start, int length, uint64_t value,
6039 | const char *format, ...)
6040 | {
6041 | proto_item *pi;
6042 | va_list ap;
6043 |
6044 | pi = proto_tree_add_uint64(tree, hfindex, tvb, start, length, value);
6045 | if (pi != tree) {
6046 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 6046, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
6047 |
6048 | va_start(ap, format)__builtin_va_start(ap, format);
6049 | proto_tree_set_representation(pi, format, ap);
6050 | va_end(ap)__builtin_va_end(ap);
6051 | }
6052 |
6053 | return pi;
6054 | }
6055 |
6056 | /* Set the FT_UINT{40,48,56,64} value */
6057 | static void
6058 | proto_tree_set_uint64(field_info *fi, uint64_t value)
6059 | {
6060 | const header_field_info *hfinfo;
6061 | uint64_t integer;
6062 |
6063 | hfinfo = fi->hfinfo;
6064 | integer = value;
6065 |
6066 | if (hfinfo->bitmask) {
6067 | /* Mask out irrelevant portions */
6068 | integer &= hfinfo->bitmask;
6069 |
6070 | /* Shift bits */
6071 | integer >>= hfinfo_bitshift(hfinfo);
6072 |
6073 | FI_SET_FLAG(fi, FI_BITS_OFFSET(hfinfo_bitoffset(hfinfo)))do { if (fi) (fi)->flags = (fi)->flags | ((((hfinfo_bitoffset (hfinfo)) & 63) << 5)); } while(0);
6074 | FI_SET_FLAG(fi, FI_BITS_SIZE(hfinfo_mask_bitwidth(hfinfo)))do { if (fi) (fi)->flags = (fi)->flags | ((((hfinfo_mask_bitwidth (hfinfo)) & 63) << 12)); } while(0);
6075 | }
6076 |
6077 | fvalue_set_uinteger64(fi->value, integer);
6078 | }
6079 |
6080 | /* Add FT_INT{8,16,24,32} to a proto_tree */
6081 | proto_item *
6082 | proto_tree_add_int(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
6083 | int length, int32_t value)
6084 | {
6085 | proto_item *pi = NULL((void*)0);
6086 | header_field_info *hfinfo;
6087 |
6088 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
6089 |
6090 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 6090 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 6090, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 6090, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 6090, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
6091 |
6092 | switch (hfinfo->type) {
6093 | case FT_INT8:
6094 | case FT_INT16:
6095 | case FT_INT24:
6096 | case FT_INT32:
6097 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
6098 | proto_tree_set_int(PNODE_FINFO(pi)((pi)->finfo), value);
6099 | break;
6100 |
6101 | default:
6102 | REPORT_DISSECTOR_BUG("field %s is not of type FT_INT8, FT_INT16, FT_INT24, or FT_INT32",proto_report_dissector_bug("field %s is not of type FT_INT8, FT_INT16, FT_INT24, or FT_INT32" , hfinfo->abbrev)
6103 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_INT8, FT_INT16, FT_INT24, or FT_INT32" , hfinfo->abbrev);
6104 | }
6105 |
6106 | return pi;
6107 | }
6108 |
6109 | proto_item *
6110 | proto_tree_add_int_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
6111 | int start, int length, int32_t value,
6112 | const char *format, ...)
6113 | {
6114 | proto_item *pi;
6115 | va_list ap;
6116 |
6117 | pi = proto_tree_add_int(tree, hfindex, tvb, start, length, value);
6118 | if (pi != tree) {
6119 | va_start(ap, format)__builtin_va_start(ap, format);
6120 | proto_tree_set_representation_value(pi, format, ap);
6121 | va_end(ap)__builtin_va_end(ap);
6122 | }
6123 |
6124 | return pi;
6125 | }
6126 |
6127 | proto_item *
6128 | proto_tree_add_int_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
6129 | int start, int length, int32_t value,
6130 | const char *format, ...)
6131 | {
6132 | proto_item *pi;
6133 | va_list ap;
6134 |
6135 | pi = proto_tree_add_int(tree, hfindex, tvb, start, length, value);
6136 | if (pi != tree) {
6137 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 6137, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
6138 |
6139 | va_start(ap, format)__builtin_va_start(ap, format);
6140 | proto_tree_set_representation(pi, format, ap);
6141 | va_end(ap)__builtin_va_end(ap);
6142 | }
6143 |
6144 | return pi;
6145 | }
6146 |
6147 | /* Set the FT_INT{8,16,24,32} value */
6148 | static void
6149 | proto_tree_set_int(field_info *fi, int32_t value)
6150 | {
6151 | const header_field_info *hfinfo;
6152 | uint32_t integer;
6153 | int no_of_bits;
6154 |
6155 | hfinfo = fi->hfinfo;
6156 | integer = (uint32_t) value;
6157 |
6158 | if (hfinfo->bitmask) {
6159 | /* Mask out irrelevant portions */
6160 | integer &= (uint32_t)(hfinfo->bitmask);
6161 |
6162 | /* Shift bits */
6163 | integer >>= hfinfo_bitshift(hfinfo);
6164 |
6165 | no_of_bits = ws_count_ones(hfinfo->bitmask);
6166 | integer = ws_sign_ext32(integer, no_of_bits);
6167 |
6168 | FI_SET_FLAG(fi, FI_BITS_OFFSET(hfinfo_bitoffset(hfinfo)))do { if (fi) (fi)->flags = (fi)->flags | ((((hfinfo_bitoffset (hfinfo)) & 63) << 5)); } while(0);
6169 | FI_SET_FLAG(fi, FI_BITS_SIZE(hfinfo_mask_bitwidth(hfinfo)))do { if (fi) (fi)->flags = (fi)->flags | ((((hfinfo_mask_bitwidth (hfinfo)) & 63) << 12)); } while(0);
6170 | }
6171 |
6172 | fvalue_set_sinteger(fi->value, integer);
6173 | }
6174 |
6175 | /* Add FT_INT{40,48,56,64} to a proto_tree */
6176 | proto_item *
6177 | proto_tree_add_int64(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
6178 | int length, int64_t value)
6179 | {
6180 | proto_item *pi = NULL((void*)0);
6181 | header_field_info *hfinfo;
6182 |
6183 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
6184 |
6185 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 6185 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 6185, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 6185, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 6185, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
6186 |
6187 | switch (hfinfo->type) {
6188 | case FT_INT40:
6189 | case FT_INT48:
6190 | case FT_INT56:
6191 | case FT_INT64:
6192 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
6193 | proto_tree_set_int64(PNODE_FINFO(pi)((pi)->finfo), value);
6194 | break;
6195 |
6196 | default:
6197 | REPORT_DISSECTOR_BUG("field %s is not of type FT_INT40, FT_INT48, FT_INT56, or FT_INT64",proto_report_dissector_bug("field %s is not of type FT_INT40, FT_INT48, FT_INT56, or FT_INT64" , hfinfo->abbrev)
6198 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_INT40, FT_INT48, FT_INT56, or FT_INT64" , hfinfo->abbrev);
6199 | }
6200 |
6201 | return pi;
6202 | }
6203 |
6204 | proto_item *
6205 | proto_tree_add_int64_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
6206 | int start, int length, int64_t value,
6207 | const char *format, ...)
6208 | {
6209 | proto_item *pi;
6210 | va_list ap;
6211 |
6212 | pi = proto_tree_add_int64(tree, hfindex, tvb, start, length, value);
6213 | if (pi != tree) {
6214 | va_start(ap, format)__builtin_va_start(ap, format);
6215 | proto_tree_set_representation_value(pi, format, ap);
6216 | va_end(ap)__builtin_va_end(ap);
6217 | }
6218 |
6219 | return pi;
6220 | }
6221 |
6222 | /* Set the FT_INT{40,48,56,64} value */
6223 | static void
6224 | proto_tree_set_int64(field_info *fi, int64_t value)
6225 | {
6226 | const header_field_info *hfinfo;
6227 | uint64_t integer;
6228 | int no_of_bits;
6229 |
6230 | hfinfo = fi->hfinfo;
6231 | integer = value;
6232 |
6233 | if (hfinfo->bitmask) {
6234 | /* Mask out irrelevant portions */
6235 | integer &= hfinfo->bitmask;
6236 |
6237 | /* Shift bits */
6238 | integer >>= hfinfo_bitshift(hfinfo);
6239 |
6240 | no_of_bits = ws_count_ones(hfinfo->bitmask);
6241 | integer = ws_sign_ext64(integer, no_of_bits);
6242 |
6243 | FI_SET_FLAG(fi, FI_BITS_OFFSET(hfinfo_bitoffset(hfinfo)))do { if (fi) (fi)->flags = (fi)->flags | ((((hfinfo_bitoffset (hfinfo)) & 63) << 5)); } while(0);
6244 | FI_SET_FLAG(fi, FI_BITS_SIZE(hfinfo_mask_bitwidth(hfinfo)))do { if (fi) (fi)->flags = (fi)->flags | ((((hfinfo_mask_bitwidth (hfinfo)) & 63) << 12)); } while(0);
6245 | }
6246 |
6247 | fvalue_set_sinteger64(fi->value, integer);
6248 | }
6249 |
6250 | proto_item *
6251 | proto_tree_add_int64_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
6252 | int start, int length, int64_t value,
6253 | const char *format, ...)
6254 | {
6255 | proto_item *pi;
6256 | va_list ap;
6257 |
6258 | pi = proto_tree_add_int64(tree, hfindex, tvb, start, length, value);
6259 | if (pi != tree) {
6260 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 6260, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
6261 |
6262 | va_start(ap, format)__builtin_va_start(ap, format);
6263 | proto_tree_set_representation(pi, format, ap);
6264 | va_end(ap)__builtin_va_end(ap);
6265 | }
6266 |
6267 | return pi;
6268 | }
6269 |
6270 | /* Add a FT_EUI64 to a proto_tree */
6271 | proto_item *
6272 | proto_tree_add_eui64(proto_tree *tree, int hfindex, tvbuff_t *tvb, int start,
6273 | int length, const uint64_t value)
6274 | {
6275 | proto_item *pi;
6276 | header_field_info *hfinfo;
6277 |
6278 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
6279 |
6280 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 6280 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 6280, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 6280, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 6280, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
6281 |
6282 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_EUI64)((void) (((hfinfo)->type == FT_EUI64) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_EUI64", "epan/proto.c", 6282, ((hfinfo))->abbrev))));
6283 |
6284 | pi = proto_tree_add_pi(tree, hfinfo, tvb, start, &length);
6285 | proto_tree_set_eui64(PNODE_FINFO(pi)((pi)->finfo), value);
6286 |
6287 | return pi;
6288 | }
6289 |
6290 | proto_item *
6291 | proto_tree_add_eui64_format_value(proto_tree *tree, int hfindex, tvbuff_t *tvb,
6292 | int start, int length, const uint64_t value,
6293 | const char *format, ...)
6294 | {
6295 | proto_item *pi;
6296 | va_list ap;
6297 |
6298 | pi = proto_tree_add_eui64(tree, hfindex, tvb, start, length, value);
6299 | if (pi != tree) {
6300 | va_start(ap, format)__builtin_va_start(ap, format);
6301 | proto_tree_set_representation_value(pi, format, ap);
6302 | va_end(ap)__builtin_va_end(ap);
6303 | }
6304 |
6305 | return pi;
6306 | }
6307 |
6308 | proto_item *
6309 | proto_tree_add_eui64_format(proto_tree *tree, int hfindex, tvbuff_t *tvb,
6310 | int start, int length, const uint64_t value,
6311 | const char *format, ...)
6312 | {
6313 | proto_item *pi;
6314 | va_list ap;
6315 |
6316 | pi = proto_tree_add_eui64(tree, hfindex, tvb, start, length, value);
6317 | if (pi != tree) {
6318 | TRY_TO_FAKE_THIS_REPR(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 6318, __func__, "assertion failed: %s", "pi" ); } while (0); if (!((pi)->finfo)) return pi; if (!(((pi) ->tree_data)->visible) && proto_item_is_hidden( (pi))) { return pi; };
6319 |
6320 | va_start(ap, format)__builtin_va_start(ap, format);
6321 | proto_tree_set_representation(pi, format, ap);
6322 | va_end(ap)__builtin_va_end(ap);
6323 | }
6324 |
6325 | return pi;
6326 | }
6327 |
6328 | /* Set the FT_EUI64 value */
6329 | static void
6330 | proto_tree_set_eui64(field_info *fi, const uint64_t value)
6331 | {
6332 | uint8_t v[FT_EUI64_LEN8];
6333 | phtonu64(v, value);
6334 | fvalue_set_bytes_data(fi->value, v, FT_EUI64_LEN8);
6335 | }
6336 |
6337 | static void
6338 | proto_tree_set_eui64_tvb(field_info *fi, tvbuff_t *tvb, int start, const unsigned encoding)
6339 | {
6340 | if (encoding)
6341 | {
6342 | proto_tree_set_eui64(fi, tvb_get_letoh64(tvb, start));
6343 | } else {
6344 | proto_tree_set_eui64(fi, tvb_get_ntoh64(tvb, start));
6345 | }
6346 | }
6347 |
6348 | proto_item *
6349 | proto_tree_add_mac48_detail(const mac_hf_list_t *list_specific,
6350 | const mac_hf_list_t *list_generic,
6351 | int idx, tvbuff_t *tvb,
6352 | proto_tree *tree, int offset)
6353 | {
6354 | uint8_t addr[6];
6355 | const char *addr_name = NULL((void*)0);
6356 | const char *oui_name = NULL((void*)0);
6357 | proto_item *addr_item = NULL((void*)0);
6358 | proto_tree *addr_tree = NULL((void*)0);
6359 | proto_item *ret_val = NULL((void*)0);
6360 |
6361 | if (tree == NULL((void*)0) || list_specific == NULL((void*)0)) {
6362 | return NULL((void*)0);
6363 | }
6364 |
6365 | /* Resolve what we can of the address */
6366 | tvb_memcpy(tvb, addr, offset, sizeof addr);
6367 | if (list_specific->hf_addr_resolved || (list_generic && list_generic->hf_addr_resolved)) {
6368 | addr_name = get_ether_name(addr);
6369 | }
6370 | if (list_specific->hf_oui_resolved || (list_generic && list_generic->hf_oui_resolved)) {
6371 | oui_name = get_manuf_name_if_known(addr, sizeof(addr));
6372 | }
6373 |
6374 | /* Add the item for the specific address type */
6375 | ret_val = proto_tree_add_item(tree, *list_specific->hf_addr, tvb, offset, 6, ENC_BIG_ENDIAN0x00000000);
6376 | if (idx >= 0) {
6377 | addr_tree = proto_item_add_subtree(ret_val, idx);
6378 | }
6379 | else {
6380 | addr_tree = tree;
6381 | }
6382 |
6383 | if (list_specific->hf_addr_resolved != NULL((void*)0)) {
6384 | addr_item = proto_tree_add_string(addr_tree, *list_specific->hf_addr_resolved,
6385 | tvb, offset, 6, addr_name);
6386 | proto_item_set_generated(addr_item);
6387 | proto_item_set_hidden(addr_item);
6388 | }
6389 |
6390 | if (list_specific->hf_oui != NULL((void*)0)) {
6391 | addr_item = proto_tree_add_item(addr_tree, *list_specific->hf_oui, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000);
6392 | proto_item_set_generated(addr_item);
6393 | proto_item_set_hidden(addr_item);
6394 |
6395 | if (oui_name != NULL((void*)0) && list_specific->hf_oui_resolved != NULL((void*)0)) {
6396 | addr_item = proto_tree_add_string(addr_tree, *list_specific->hf_oui_resolved, tvb, offset, 6, oui_name);
6397 | proto_item_set_generated(addr_item);
6398 | proto_item_set_hidden(addr_item);
6399 | }
6400 | }
6401 |
6402 | if (list_specific->hf_lg != NULL((void*)0)) {
6403 | proto_tree_add_item(addr_tree, *list_specific->hf_lg, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000);
6404 | }
6405 | if (list_specific->hf_ig != NULL((void*)0)) {
6406 | proto_tree_add_item(addr_tree, *list_specific->hf_ig, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000);
6407 | }
6408 |
6409 | /* Were we given a list for generic address fields? If not, stop here */
6410 | if (list_generic == NULL((void*)0)) {
6411 | return ret_val;
6412 | }
6413 |
6414 | addr_item = proto_tree_add_item(addr_tree, *list_generic->hf_addr, tvb, offset, 6, ENC_BIG_ENDIAN0x00000000);
6415 | proto_item_set_hidden(addr_item);
6416 |
6417 | if (list_generic->hf_addr_resolved != NULL((void*)0)) {
6418 | addr_item = proto_tree_add_string(addr_tree, *list_generic->hf_addr_resolved,
6419 | tvb, offset, 6, addr_name);
6420 | proto_item_set_generated(addr_item);
6421 | proto_item_set_hidden(addr_item);
6422 | }
6423 |
6424 | if (list_generic->hf_oui != NULL((void*)0)) {
6425 | addr_item = proto_tree_add_item(addr_tree, *list_generic->hf_oui, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000);
6426 | proto_item_set_generated(addr_item);
6427 | proto_item_set_hidden(addr_item);
6428 |
6429 | if (oui_name != NULL((void*)0) && list_generic->hf_oui_resolved != NULL((void*)0)) {
6430 | addr_item = proto_tree_add_string(addr_tree, *list_generic->hf_oui_resolved, tvb, offset, 6, oui_name);
6431 | proto_item_set_generated(addr_item);
6432 | proto_item_set_hidden(addr_item);
6433 | }
6434 | }
6435 |
6436 | if (list_generic->hf_lg != NULL((void*)0)) {
6437 | addr_item = proto_tree_add_item(addr_tree, *list_generic->hf_lg, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000);
6438 | proto_item_set_hidden(addr_item);
6439 | }
6440 | if (list_generic->hf_ig != NULL((void*)0)) {
6441 | addr_item = proto_tree_add_item(addr_tree, *list_generic->hf_ig, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000);
6442 | proto_item_set_hidden(addr_item);
6443 | }
6444 | return ret_val;
6445 | }
6446 |
6447 | static proto_item *
6448 | proto_tree_add_fake_node(proto_tree *tree, const header_field_info *hfinfo)
6449 | {
6450 | proto_node *pnode, *tnode, *sibling;
6451 | field_info *tfi;
6452 | unsigned depth = 1;
6453 |
6454 | ws_assert(tree)do { if ((1) && !(tree)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 6454, __func__, "assertion failed: %s", "tree" ); } while (0);
6455 |
6456 | /*
6457 | * Restrict our depth. proto_tree_traverse_pre_order and
6458 | * proto_tree_traverse_post_order (and possibly others) are recursive
6459 | * so we need to be mindful of our stack size.
6460 | */
6461 | if (tree->first_child == NULL((void*)0)) {
6462 | for (tnode = tree; tnode != NULL((void*)0); tnode = tnode->parent) {
6463 | depth++;
6464 | if (G_UNLIKELY(depth > prefs.gui_max_tree_depth)(depth > prefs.gui_max_tree_depth)) {
6465 | THROW_MESSAGE(DissectorError, wmem_strdup_printf(PNODE_POOL(tree),except_throw(1, (6), (wmem_strdup_printf(((tree)->tree_data ->pinfo->pool), "Maximum tree depth %d exceeded for \"%s\" - \"%s\" (%s:%u) (Maximum depth can be increased in advanced preferences)" , prefs.gui_max_tree_depth, hfinfo->name, hfinfo->abbrev , ((const char*) (__func__)), 6468)))
6466 | "Maximum tree depth %d exceeded for \"%s\" - \"%s\" (%s:%u) (Maximum depth can be increased in advanced preferences)",except_throw(1, (6), (wmem_strdup_printf(((tree)->tree_data ->pinfo->pool), "Maximum tree depth %d exceeded for \"%s\" - \"%s\" (%s:%u) (Maximum depth can be increased in advanced preferences)" , prefs.gui_max_tree_depth, hfinfo->name, hfinfo->abbrev , ((const char*) (__func__)), 6468)))
6467 | prefs.gui_max_tree_depth,except_throw(1, (6), (wmem_strdup_printf(((tree)->tree_data ->pinfo->pool), "Maximum tree depth %d exceeded for \"%s\" - \"%s\" (%s:%u) (Maximum depth can be increased in advanced preferences)" , prefs.gui_max_tree_depth, hfinfo->name, hfinfo->abbrev , ((const char*) (__func__)), 6468)))
6468 | hfinfo->name, hfinfo->abbrev, G_STRFUNC, __LINE__))except_throw(1, (6), (wmem_strdup_printf(((tree)->tree_data ->pinfo->pool), "Maximum tree depth %d exceeded for \"%s\" - \"%s\" (%s:%u) (Maximum depth can be increased in advanced preferences)" , prefs.gui_max_tree_depth, hfinfo->name, hfinfo->abbrev , ((const char*) (__func__)), 6468)));
6469 | }
6470 | }
6471 | }
6472 |
6473 | /*
6474 | * Make sure "tree" is ready to have subtrees under it, by
6475 | * checking whether it's been given an ett_ value.
6476 | *
6477 | * "PNODE_FINFO(tnode)" may be null; that's the case for the root
6478 | * node of the protocol tree. That node is not displayed,
6479 | * so it doesn't need an ett_ value to remember whether it
6480 | * was expanded.
6481 | */
6482 | tnode = tree;
6483 | tfi = PNODE_FINFO(tnode)((tnode)->finfo);
6484 | if (tfi != NULL((void*)0) && (tfi->tree_type < 0 || tfi->tree_type >= num_tree_types)) {
6485 | REPORT_DISSECTOR_BUG("\"%s\" - \"%s\" tfi->tree_type: %d invalid (%s:%u)",proto_report_dissector_bug("\"%s\" - \"%s\" tfi->tree_type: %d invalid (%s:%u)" , hfinfo->name, hfinfo->abbrev, tfi->tree_type, "epan/proto.c" , 6486)
6486 | hfinfo->name, hfinfo->abbrev, tfi->tree_type, __FILE__, __LINE__)proto_report_dissector_bug("\"%s\" - \"%s\" tfi->tree_type: %d invalid (%s:%u)" , hfinfo->name, hfinfo->abbrev, tfi->tree_type, "epan/proto.c" , 6486);
6487 | /* XXX - is it safe to continue here? */
6488 | }
6489 |
6490 | pnode = wmem_new(PNODE_POOL(tree), proto_node)((proto_node*)wmem_alloc((((tree)->tree_data->pinfo-> pool)), sizeof(proto_node)));
6491 | PROTO_NODE_INIT(pnode)pnode->first_child = ((void*)0); pnode->last_child = (( void*)0); pnode->next = ((void*)0);;
6492 | pnode->parent = tnode;
6493 | PNODE_HFINFO(pnode)((pnode)->hfinfo) = hfinfo;
6494 | PNODE_FINFO(pnode)((pnode)->finfo) = NULL((void*)0); // Faked
6495 | pnode->tree_data = PTREE_DATA(tree)((tree)->tree_data);
6496 |
6497 | if (tnode->last_child != NULL((void*)0)) {
6498 | sibling = tnode->last_child;
6499 | DISSECTOR_ASSERT(sibling->next == NULL)((void) ((sibling->next == ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 6499, "sibling->next == ((void*)0)" ))));
6500 | sibling->next = pnode;
6501 | } else
6502 | tnode->first_child = pnode;
6503 | tnode->last_child = pnode;
6504 |
6505 | /* We should not be adding a fake node for an interesting field */
6506 | ws_assert(hfinfo->ref_type != HF_REF_TYPE_DIRECT && hfinfo->ref_type != HF_REF_TYPE_PRINT)do { if ((1) && !(hfinfo->ref_type != HF_REF_TYPE_DIRECT && hfinfo->ref_type != HF_REF_TYPE_PRINT)) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 6506, __func__, "assertion failed: %s" , "hfinfo->ref_type != HF_REF_TYPE_DIRECT && hfinfo->ref_type != HF_REF_TYPE_PRINT" ); } while (0);
6507 |
6508 | /* XXX - Should the proto_item have a header_field_info member, at least
6509 | * for faked items, to know what hfi was faked? (Some dissectors look at
6510 | * the tree items directly.)
6511 | */
6512 | return (proto_item *)pnode;
6513 | }
6514 |
6515 | /* Add a field_info struct to the proto_tree, encapsulating it in a proto_node */
6516 | static proto_item *
6517 | proto_tree_add_node(proto_tree *tree, field_info *fi)
6518 | {
6519 | proto_node *pnode, *tnode, *sibling;
6520 | field_info *tfi;
6521 | unsigned depth = 1;
6522 |
6523 | ws_assert(tree)do { if ((1) && !(tree)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 6523, __func__, "assertion failed: %s", "tree" ); } while (0);
6524 |
6525 | /*
6526 | * Restrict our depth. proto_tree_traverse_pre_order and
6527 | * proto_tree_traverse_post_order (and possibly others) are recursive
6528 | * so we need to be mindful of our stack size.
6529 | */
6530 | if (tree->first_child == NULL((void*)0)) {
6531 | for (tnode = tree; tnode != NULL((void*)0); tnode = tnode->parent) {
6532 | depth++;
6533 | if (G_UNLIKELY(depth > prefs.gui_max_tree_depth)(depth > prefs.gui_max_tree_depth)) {
6534 | fvalue_free(fi->value);
6535 | fi->value = NULL((void*)0);
6536 | THROW_MESSAGE(DissectorError, wmem_strdup_printf(PNODE_POOL(tree),except_throw(1, (6), (wmem_strdup_printf(((tree)->tree_data ->pinfo->pool), "Maximum tree depth %d exceeded for \"%s\" - \"%s\" (%s:%u) (Maximum depth can be increased in advanced preferences)" , prefs.gui_max_tree_depth, fi->hfinfo->name, fi->hfinfo ->abbrev, ((const char*) (__func__)), 6539)))
6537 | "Maximum tree depth %d exceeded for \"%s\" - \"%s\" (%s:%u) (Maximum depth can be increased in advanced preferences)",except_throw(1, (6), (wmem_strdup_printf(((tree)->tree_data ->pinfo->pool), "Maximum tree depth %d exceeded for \"%s\" - \"%s\" (%s:%u) (Maximum depth can be increased in advanced preferences)" , prefs.gui_max_tree_depth, fi->hfinfo->name, fi->hfinfo ->abbrev, ((const char*) (__func__)), 6539)))
6538 | prefs.gui_max_tree_depth,except_throw(1, (6), (wmem_strdup_printf(((tree)->tree_data ->pinfo->pool), "Maximum tree depth %d exceeded for \"%s\" - \"%s\" (%s:%u) (Maximum depth can be increased in advanced preferences)" , prefs.gui_max_tree_depth, fi->hfinfo->name, fi->hfinfo ->abbrev, ((const char*) (__func__)), 6539)))
6539 | fi->hfinfo->name, fi->hfinfo->abbrev, G_STRFUNC, __LINE__))except_throw(1, (6), (wmem_strdup_printf(((tree)->tree_data ->pinfo->pool), "Maximum tree depth %d exceeded for \"%s\" - \"%s\" (%s:%u) (Maximum depth can be increased in advanced preferences)" , prefs.gui_max_tree_depth, fi->hfinfo->name, fi->hfinfo ->abbrev, ((const char*) (__func__)), 6539)));
6540 | }
6541 | }
6542 | }
6543 |
6544 | /*
6545 | * Make sure "tree" is ready to have subtrees under it, by
6546 | * checking whether it's been given an ett_ value.
6547 | *
6548 | * "PNODE_FINFO(tnode)" may be null; that's the case for the root
6549 | * node of the protocol tree. That node is not displayed,
6550 | * so it doesn't need an ett_ value to remember whether it
6551 | * was expanded.
6552 | */
6553 | tnode = tree;
6554 | tfi = PNODE_FINFO(tnode)((tnode)->finfo);
6555 | if (tfi != NULL((void*)0) && (tfi->tree_type < 0 || tfi->tree_type >= num_tree_types)) {
6556 | /* Since we are not adding fi to a node, its fvalue won't get
6557 | * freed by proto_tree_free_node(), so free it now.
6558 | */
6559 | fvalue_free(fi->value);
6560 | fi->value = NULL((void*)0);
6561 | REPORT_DISSECTOR_BUG("\"%s\" - \"%s\" tfi->tree_type: %d invalid (%s:%u)",proto_report_dissector_bug("\"%s\" - \"%s\" tfi->tree_type: %d invalid (%s:%u)" , fi->hfinfo->name, fi->hfinfo->abbrev, tfi->tree_type , "epan/proto.c", 6562)
6562 | fi->hfinfo->name, fi->hfinfo->abbrev, tfi->tree_type, __FILE__, __LINE__)proto_report_dissector_bug("\"%s\" - \"%s\" tfi->tree_type: %d invalid (%s:%u)" , fi->hfinfo->name, fi->hfinfo->abbrev, tfi->tree_type , "epan/proto.c", 6562);
6563 | /* XXX - is it safe to continue here? */
6564 | }
6565 |
6566 | pnode = wmem_new(PNODE_POOL(tree), proto_node)((proto_node*)wmem_alloc((((tree)->tree_data->pinfo-> pool)), sizeof(proto_node)));
6567 | PROTO_NODE_INIT(pnode)pnode->first_child = ((void*)0); pnode->last_child = (( void*)0); pnode->next = ((void*)0);;
6568 | pnode->parent = tnode;
6569 | PNODE_HFINFO(pnode)((pnode)->hfinfo) = fi->hfinfo;
6570 | PNODE_FINFO(pnode)((pnode)->finfo) = fi;
6571 | pnode->tree_data = PTREE_DATA(tree)((tree)->tree_data);
6572 |
6573 | if (tnode->last_child != NULL((void*)0)) {
6574 | sibling = tnode->last_child;
6575 | DISSECTOR_ASSERT(sibling->next == NULL)((void) ((sibling->next == ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 6575, "sibling->next == ((void*)0)" ))));
6576 | sibling->next = pnode;
6577 | } else
6578 | tnode->first_child = pnode;
6579 | tnode->last_child = pnode;
6580 |
6581 | tree_data_add_maybe_interesting_field(pnode->tree_data, fi);
6582 |
6583 | return (proto_item *)pnode;
6584 | }
6585 |
6586 |
6587 | /* Generic way to allocate field_info and add to proto_tree.
6588 | * Sets *pfi to address of newly-allocated field_info struct */
6589 | static proto_item *
6590 | proto_tree_add_pi(proto_tree *tree, header_field_info *hfinfo, tvbuff_t *tvb, int start,
6591 | int *length)
6592 | {
6593 | proto_item *pi;
6594 | field_info *fi;
6595 | int item_length;
6596 |
6597 | get_hfi_length(hfinfo, tvb, start, length, &item_length, ENC_NA0x00000000);
6598 | fi = new_field_info(tree, hfinfo, tvb, start, item_length);
6599 | pi = proto_tree_add_node(tree, fi);
6600 |
6601 | return pi;
6602 | }
6603 |
6604 |
6605 | static void
6606 | get_hfi_length(header_field_info *hfinfo, tvbuff_t *tvb, const int start, int *length,
6607 | int *item_length, const unsigned encoding)
6608 | {
6609 | int length_remaining;
6610 |
6611 | /*
6612 | * We only allow a null tvbuff if the item has a zero length,
6613 | * i.e. if there's no data backing it.
6614 | */
6615 | DISSECTOR_ASSERT(tvb != NULL || *length == 0)((void) ((tvb != ((void*)0) || *length == 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 6615, "tvb != ((void*)0) || *length == 0" ))));
6616 |
6617 | /*
6618 | * XXX - in some protocols, there are 32-bit unsigned length
6619 | * fields, so lengths in protocol tree and tvbuff routines
6620 | * should really be unsigned. We should have, for those
6621 | * field types for which "to the end of the tvbuff" makes sense,
6622 | * additional routines that take no length argument and
6623 | * add fields that run to the end of the tvbuff.
6624 | */
6625 | if (*length == -1) {
6626 | /*
6627 | * For FT_NONE, FT_PROTOCOL, FT_BYTES, FT_STRING,
6628 | * FT_STRINGZPAD, and FT_STRINGZTRUNC fields, a length
6629 | * of -1 means "set the length to what remains in the
6630 | * tvbuff".
6631 | *
6632 | * The assumption is either that
6633 | *
6634 | * 1) the length of the item can only be determined
6635 | * by dissection (typically true of items with
6636 | * subitems, which are probably FT_NONE or
6637 | * FT_PROTOCOL)
6638 | *
6639 | * or
6640 | *
6641 | * 2) if the tvbuff is "short" (either due to a short
6642 | * snapshot length or due to lack of reassembly of
6643 | * fragments/segments/whatever), we want to display
6644 | * what's available in the field (probably FT_BYTES
6645 | * or FT_STRING) and then throw an exception later
6646 | *
6647 | * or
6648 | *
6649 | * 3) the field is defined to be "what's left in the
6650 | * packet"
6651 | *
6652 | * so we set the length to what remains in the tvbuff so
6653 | * that, if we throw an exception while dissecting, it
6654 | * has what is probably the right value.
6655 | *
6656 | * For FT_STRINGZ, it means "the string is null-terminated,
6657 | * not null-padded; set the length to the actual length
6658 | * of the string", and if the tvbuff if short, we just
6659 | * throw an exception.
6660 | *
6661 | * For ENC_VARINT_PROTOBUF|ENC_VARINT_QUIC|ENC_VARIANT_ZIGZAG|ENC_VARINT_SDNV,
6662 | * it means "find the end of the string",
6663 | * and if the tvbuff if short, we just throw an exception.
6664 | *
6665 | * It's not valid for any other type of field. For those
6666 | * fields, we treat -1 the same way we treat other
6667 | * negative values - we assume the length is a Really
6668 | * Big Positive Number, and throw a ReportedBoundsError
6669 | * exception, under the assumption that the Really Big
6670 | * Length would run past the end of the packet.
6671 | */
6672 | if ((FT_IS_INT(hfinfo->type)(((hfinfo->type) == FT_INT8 || (hfinfo->type) == FT_INT16 || (hfinfo->type) == FT_INT24 || (hfinfo->type) == FT_INT32 ) || ((hfinfo->type) == FT_INT40 || (hfinfo->type) == FT_INT48 || (hfinfo->type) == FT_INT56 || (hfinfo->type) == FT_INT64 ))) || (FT_IS_UINT(hfinfo->type)(((hfinfo->type) == FT_CHAR || (hfinfo->type) == FT_UINT8 || (hfinfo->type) == FT_UINT16 || (hfinfo->type) == FT_UINT24 || (hfinfo->type) == FT_UINT32 || (hfinfo->type) == FT_FRAMENUM ) || ((hfinfo->type) == FT_UINT40 || (hfinfo->type) == FT_UINT48 || (hfinfo->type) == FT_UINT56 || (hfinfo->type) == FT_UINT64 )))) {
6673 | if (encoding & (ENC_VARINT_PROTOBUF0x00000002|ENC_VARINT_ZIGZAG0x00000008|ENC_VARINT_SDNV0x00000010)) {
6674 | /*
6675 | * Leave the length as -1, so our caller knows
6676 | * it was -1.
6677 | */
6678 | *item_length = *length;
6679 | return;
6680 | } else if (encoding & ENC_VARINT_QUIC0x00000004) {
6681 | switch (tvb_get_uint8(tvb, start) >> 6)
6682 | {
6683 | case 0: /* 0b00 => 1 byte length (6 bits Usable) */
6684 | *item_length = 1;
6685 | break;
6686 | case 1: /* 0b01 => 2 bytes length (14 bits Usable) */
6687 | *item_length = 2;
6688 | break;
6689 | case 2: /* 0b10 => 4 bytes length (30 bits Usable) */
6690 | *item_length = 4;
6691 | break;
6692 | case 3: /* 0b11 => 8 bytes length (62 bits Usable) */
6693 | *item_length = 8;
6694 | break;
6695 | }
6696 | }
6697 | }
6698 |
6699 | switch (hfinfo->type) {
6700 |
6701 | case FT_PROTOCOL:
6702 | case FT_NONE:
6703 | case FT_BYTES:
6704 | case FT_STRING:
6705 | case FT_STRINGZPAD:
6706 | case FT_STRINGZTRUNC:
6707 | /*
6708 | * We allow FT_PROTOCOLs to be zero-length -
6709 | * for example, an ONC RPC NULL procedure has
6710 | * neither arguments nor reply, so the
6711 | * payload for that protocol is empty.
6712 | *
6713 | * We also allow the others to be zero-length -
6714 | * because that's the way the code has been for a
6715 | * long, long time.
6716 | *
6717 | * However, we want to ensure that the start
6718 | * offset is not *past* the byte past the end
6719 | * of the tvbuff: we throw an exception in that
6720 | * case.
6721 | */
6722 | *length = tvb_captured_length(tvb) ? tvb_ensure_captured_length_remaining(tvb, start) : 0;
6723 | DISSECTOR_ASSERT(*length >= 0)((void) ((*length >= 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 6723, "*length >= 0" ))));
6724 | break;
6725 |
6726 | case FT_STRINGZ:
6727 | /*
6728 | * Leave the length as -1, so our caller knows
6729 | * it was -1.
6730 | */
6731 | break;
6732 |
6733 | default:
6734 | THROW(ReportedBoundsError)except_throw(1, (3), ((void*)0));
6735 | DISSECTOR_ASSERT_NOT_REACHED()(proto_report_dissector_bug("%s:%u: failed assertion \"DISSECTOR_ASSERT_NOT_REACHED\"" , "epan/proto.c", 6735));
6736 | }
6737 | *item_length = *length;
6738 | } else {
6739 | *item_length = *length;
6740 | if (hfinfo->type == FT_PROTOCOL || hfinfo->type == FT_NONE) {
6741 | /*
6742 | * These types are for interior nodes of the
6743 | * tree, and don't have data associated with
6744 | * them; if the length is negative (XXX - see
6745 | * above) or goes past the end of the tvbuff,
6746 | * cut it short at the end of the tvbuff.
6747 | * That way, if this field is selected in
6748 | * Wireshark, we don't highlight stuff past
6749 | * the end of the data.
6750 | */
6751 | /* XXX - what to do, if we don't have a tvb? */
6752 | if (tvb) {
6753 | length_remaining = tvb_captured_length_remaining(tvb, start);
6754 | if (*item_length < 0 ||
6755 | (*item_length > 0 &&
6756 | (length_remaining < *item_length)))
6757 | *item_length = length_remaining;
6758 | }
6759 | }
6760 | if (*item_length < 0) {
6761 | THROW(ReportedBoundsError)except_throw(1, (3), ((void*)0));
6762 | }
6763 | }
6764 | }
6765 |
6766 | static int
6767 | get_full_length(header_field_info *hfinfo, tvbuff_t *tvb, const int start,
6768 | int length, unsigned item_length, const int encoding)
6769 | {
6770 | uint32_t n;
6771 |
6772 | /*
6773 | * We need to get the correct item length here.
6774 | * That's normally done by proto_tree_new_item(),
6775 | * but we won't be calling it.
6776 | */
6777 | switch (hfinfo->type) {
6778 |
6779 | case FT_NONE:
6780 | case FT_PROTOCOL:
6781 | case FT_BYTES:
6782 | /*
6783 | * The length is the specified length.
6784 | */
6785 | break;
6786 |
6787 | case FT_UINT_BYTES:
6788 | n = get_uint_value(NULL((void*)0), tvb, start, length, encoding);
6789 | item_length += n;
6790 | if ((int)item_length < length) {
6791 | THROW(ReportedBoundsError)except_throw(1, (3), ((void*)0));
6792 | }
6793 | break;
6794 |
6795 | /* XXX - make these just FT_UINT? */
6796 | case FT_UINT8:
6797 | case FT_UINT16:
6798 | case FT_UINT24:
6799 | case FT_UINT32:
6800 | case FT_UINT40:
6801 | case FT_UINT48:
6802 | case FT_UINT56:
6803 | case FT_UINT64:
6804 | /* XXX - make these just FT_INT? */
6805 | case FT_INT8:
6806 | case FT_INT16:
6807 | case FT_INT24:
6808 | case FT_INT32:
6809 | case FT_INT40:
6810 | case FT_INT48:
6811 | case FT_INT56:
6812 | case FT_INT64:
6813 | if (encoding & ENC_VARINT_MASK(0x00000002|0x00000004|0x00000008|0x00000010)) {
6814 | if (length < -1) {
6815 | report_type_length_mismatch(NULL((void*)0), "a FT_[U]INT", length, true1);
6816 | }
6817 | if (length == -1) {
6818 | uint64_t dummy;
6819 | /* This can throw an exception */
6820 | /* XXX - do this without fetching the varint? */
6821 | length = tvb_get_varint(tvb, start, FT_VARINT_MAX_LEN10, &dummy, encoding);
6822 | if (length == 0) {
6823 | THROW(ReportedBoundsError)except_throw(1, (3), ((void*)0));
6824 | }
6825 | }
6826 | item_length = length;
6827 | break;
6828 | }
6829 |
6830 | /*
6831 | * The length is the specified length.
6832 | */
6833 | break;
6834 |
6835 | case FT_BOOLEAN:
6836 | case FT_CHAR:
6837 | case FT_IPv4:
6838 | case FT_IPXNET:
6839 | case FT_IPv6:
6840 | case FT_FCWWN:
6841 | case FT_AX25:
6842 | case FT_VINES:
6843 | case FT_ETHER:
6844 | case FT_EUI64:
6845 | case FT_GUID:
6846 | case FT_OID:
6847 | case FT_REL_OID:
6848 | case FT_SYSTEM_ID:
6849 | case FT_FLOAT:
6850 | case FT_DOUBLE:
6851 | case FT_STRING:
6852 | /*
6853 | * The length is the specified length.
6854 | */
6855 | break;
6856 |
6857 | case FT_STRINGZ:
6858 | if (length < -1) {
6859 | report_type_length_mismatch(NULL((void*)0), "a string", length, true1);
6860 | }
6861 | if (length == -1) {
6862 | /* This can throw an exception */
6863 | item_length = tvb_strsize_enc(tvb, start, encoding);
6864 | }
6865 | break;
6866 |
6867 | case FT_UINT_STRING:
6868 | n = get_uint_value(NULL((void*)0), tvb, start, length, encoding & ~ENC_CHARENCODING_MASK0x0000FFFE);
6869 | item_length += n;
6870 | if ((int)item_length < length) {
6871 | THROW(ReportedBoundsError)except_throw(1, (3), ((void*)0));
6872 | }
6873 | break;
6874 |
6875 | case FT_STRINGZPAD:
6876 | case FT_STRINGZTRUNC:
6877 | case FT_ABSOLUTE_TIME:
6878 | case FT_RELATIVE_TIME:
6879 | case FT_IEEE_11073_SFLOAT:
6880 | case FT_IEEE_11073_FLOAT:
6881 | /*
6882 | * The length is the specified length.
6883 | */
6884 | break;
6885 |
6886 | default:
6887 | REPORT_DISSECTOR_BUG("field %s has type %d (%s) not handled in gset_full_length()",proto_report_dissector_bug("field %s has type %d (%s) not handled in gset_full_length()" , hfinfo->abbrev, hfinfo->type, ftype_name(hfinfo->type ))
6888 | hfinfo->abbrev,proto_report_dissector_bug("field %s has type %d (%s) not handled in gset_full_length()" , hfinfo->abbrev, hfinfo->type, ftype_name(hfinfo->type ))
6889 | hfinfo->type,proto_report_dissector_bug("field %s has type %d (%s) not handled in gset_full_length()" , hfinfo->abbrev, hfinfo->type, ftype_name(hfinfo->type ))
6890 | ftype_name(hfinfo->type))proto_report_dissector_bug("field %s has type %d (%s) not handled in gset_full_length()" , hfinfo->abbrev, hfinfo->type, ftype_name(hfinfo->type ));
6891 | break;
6892 | }
6893 | return item_length;
6894 | }
6895 |
6896 | // This was arbitrarily chosen, but if you're adding 50K items to the tree
6897 | // without advancing the offset you should probably take a long, hard look
6898 | // at what you're doing.
6899 | // We *could* make this a configurable option, but I (Gerald) would like to
6900 | // avoid adding yet another nerd knob.
6901 | # define PROTO_TREE_MAX_IDLE50000 50000
6902 | static field_info *
6903 | new_field_info(proto_tree *tree, header_field_info *hfinfo, tvbuff_t *tvb,
6904 | const int start, const int item_length)
6905 | {
6906 | field_info *fi;
6907 |
6908 | FIELD_INFO_NEW(PNODE_POOL(tree), fi)fi = ((field_info*)wmem_alloc((((tree)->tree_data->pinfo ->pool)), sizeof(field_info)));
6909 |
6910 | fi->hfinfo = hfinfo;
6911 | fi->start = start;
6912 | fi->start += (tvb)?tvb_raw_offset(tvb):0;
6913 | /* add the data source tvbuff */
6914 | fi->ds_tvb = tvb ? tvb_get_ds_tvb(tvb) : NULL((void*)0);
6915 |
6916 | // If our start offset hasn't advanced after adding many items it probably
6917 | // means we're in a large or infinite loop.
6918 | if (fi->start > 0) {
6919 | if (fi->ds_tvb == PTREE_DATA(tree)((tree)->tree_data)->idle_count_ds_tvb && fi->start <= PTREE_DATA(tree)((tree)->tree_data)->max_start) {
6920 | PTREE_DATA(tree)((tree)->tree_data)->start_idle_count++;
6921 | DISSECTOR_ASSERT_HINT(PTREE_DATA(tree)->start_idle_count < PROTO_TREE_MAX_IDLE, fi->hfinfo->abbrev)((void) ((((tree)->tree_data)->start_idle_count < 50000 ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 6921, "((tree)->tree_data)->start_idle_count < 50000" , fi->hfinfo->abbrev))));
6922 | } else {
6923 | PTREE_DATA(tree)((tree)->tree_data)->idle_count_ds_tvb = fi->ds_tvb;
6924 | PTREE_DATA(tree)((tree)->tree_data)->max_start = fi->start;
6925 | PTREE_DATA(tree)((tree)->tree_data)->start_idle_count = 0;
6926 | }
6927 | }
6928 | fi->length = item_length;
6929 | fi->tree_type = -1;
6930 | fi->flags = 0;
6931 | if (!PTREE_DATA(tree)((tree)->tree_data)->visible) {
6932 | /* If the tree is not visible, set the item hidden, unless we
6933 | * need the representation or length and can't fake them.
6934 | */
6935 | if (hfinfo->ref_type != HF_REF_TYPE_PRINT && (hfinfo->type != FT_PROTOCOL || PTREE_DATA(tree)((tree)->tree_data)->fake_protocols)) {
6936 | FI_SET_FLAG(fi, FI_HIDDEN)do { if (fi) (fi)->flags = (fi)->flags | (0x00000001); } while(0);
6937 | }
6938 | }
6939 | fi->value = fvalue_new(fi->hfinfo->type);
6940 | fi->rep = NULL((void*)0);
6941 |
6942 | fi->appendix_start = 0;
6943 | fi->appendix_length = 0;
6944 |
6945 | fi->total_layer_num = tree->tree_data->pinfo->curr_layer_num;
6946 | fi->proto_layer_num = tree->tree_data->pinfo->curr_proto_layer_num;
6947 |
6948 | return fi;
6949 | }
6950 |
6951 | static size_t proto_find_value_pos(const header_field_info *hfinfo, const char *representation)
6952 | {
6953 | if (hfinfo->display & BASE_NO_DISPLAY_VALUE0x00002000) {
6954 | return 0;
6955 | }
6956 |
6957 | /* Search for field name */
6958 | char *ptr = strstr(representation, hfinfo->name);
6959 | if (!ptr) {
6960 | return 0;
6961 | }
6962 |
6963 | /* Check if field name ends with the ": " delimiter */
6964 | ptr += strlen(hfinfo->name);
6965 | if (strncmp(ptr, ": ", 2) == 0) {
6966 | ptr += 2;
6967 | }
6968 |
6969 | /* Return offset to after field name */
6970 | return ptr - representation;
6971 | }
6972 |
6973 | static size_t label_find_name_pos(const item_label_t *rep)
6974 | {
6975 | size_t name_pos = 0;
6976 |
6977 | /* If the value_pos is too small or too large, we can't find the expected format */
6978 | if (rep->value_pos <= 2 || rep->value_pos >= sizeof(rep->representation)) {
6979 | return 0;
6980 | }
6981 |
6982 | /* Check if the format looks like "label: value", then set name_pos before ':'. */
6983 | if (rep->representation[rep->value_pos-2] == ':') {
6984 | name_pos = rep->value_pos - 2;
6985 | }
6986 |
6987 | return name_pos;
6988 | }
6989 |
6990 | /* If the protocol tree is to be visible, set the representation of a
6991 | proto_tree entry with the name of the field for the item and with
6992 | the value formatted with the supplied printf-style format and
6993 | argument list. */
6994 | static void
6995 | proto_tree_set_representation_value(proto_item *pi, const char *format, va_list ap)
6996 | {
6997 | ws_assert(pi)do { if ((1) && !(pi)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 6997, __func__, "assertion failed: %s", "pi" ); } while (0);
6998 |
6999 | /* If the tree (GUI) or item isn't visible it's pointless for us to generate the protocol
7000 | * items string representation */
7001 | if (PTREE_DATA(pi)((pi)->tree_data)->visible || !proto_item_is_hidden(pi)) {
7002 | size_t name_pos, ret = 0;
7003 | char *str;
7004 | field_info *fi = PITEM_FINFO(pi)((pi)->finfo);
7005 | const header_field_info *hf;
7006 |
7007 | DISSECTOR_ASSERT(fi)((void) ((fi) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 7007, "fi"))));
7008 |
7009 | hf = fi->hfinfo;
7010 |
7011 | ITEM_LABEL_NEW(PNODE_POOL(pi), fi->rep)fi->rep = ((item_label_t*)wmem_alloc((((pi)->tree_data-> pinfo->pool)), sizeof(item_label_t))); fi->rep->value_pos = 0; fi->rep->value_len = 0;;
7012 | if (hf->bitmask && (hf->type == FT_BOOLEAN || FT_IS_UINT(hf->type)(((hf->type) == FT_CHAR || (hf->type) == FT_UINT8 || (hf ->type) == FT_UINT16 || (hf->type) == FT_UINT24 || (hf-> type) == FT_UINT32 || (hf->type) == FT_FRAMENUM) || ((hf-> type) == FT_UINT40 || (hf->type) == FT_UINT48 || (hf->type ) == FT_UINT56 || (hf->type) == FT_UINT64)))) {
7013 | uint64_t val;
7014 | char *p;
7015 |
7016 | if (FT_IS_UINT32(hf->type)((hf->type) == FT_CHAR || (hf->type) == FT_UINT8 || (hf ->type) == FT_UINT16 || (hf->type) == FT_UINT24 || (hf-> type) == FT_UINT32 || (hf->type) == FT_FRAMENUM))
7017 | val = fvalue_get_uinteger(fi->value);
7018 | else
7019 | val = fvalue_get_uinteger64(fi->value);
7020 |
7021 | val <<= hfinfo_bitshift(hf);
7022 |
7023 | p = decode_bitfield_value(fi->rep->representation, val, hf->bitmask, hfinfo_container_bitwidth(hf));
7024 | ret = (p - fi->rep->representation);
7025 | }
7026 |
7027 | /* put in the hf name */
7028 | name_pos = ret = label_concat(fi->rep->representation, ret, (const uint8_t*)hf->name)ws_label_strcpy(fi->rep->representation, 240, ret, (const uint8_t*)hf->name, 0);
7029 |
7030 | ret = label_concat(fi->rep->representation, ret, (const uint8_t*)": ")ws_label_strcpy(fi->rep->representation, 240, ret, (const uint8_t*)": ", 0);
7031 | /* If possible, Put in the value of the string */
7032 | str = wmem_strdup_vprintf(PNODE_POOL(pi)((pi)->tree_data->pinfo->pool), format, ap);
7033 | WS_UTF_8_CHECK(str, -1)do { const char *__uni_endptr; if (1 && (str) != ((void *)0) && !g_utf8_validate(str, -1, &__uni_endptr)) { do { if (1) { ws_log_utf8_full("UTF-8", LOG_LEVEL_DEBUG, "epan/proto.c" , 7033, __func__, str, -1, __uni_endptr); } } while (0); } } while (0);
7034 | fi->rep->value_pos = ret;
7035 | ret = ws_label_strcpy(fi->rep->representation, ITEM_LABEL_LENGTH240, ret, (const uint8_t*)str, 0);
7036 | if (ret >= ITEM_LABEL_LENGTH240) {
7037 | /* Uh oh, we don't have enough room. Tell the user
7038 | * that the field is truncated.
7039 | */
7040 | label_mark_truncated(fi->rep->representation, name_pos, &fi->rep->value_pos);
7041 | }
7042 | fi->rep->value_len = strlen(fi->rep->representation) - fi->rep->value_pos;
7043 | }
7044 | }
7045 |
7046 | /* If the protocol tree is to be visible, set the representation of a
7047 | proto_tree entry with the representation formatted with the supplied
7048 | printf-style format and argument list. */
7049 | static void
7050 | proto_tree_set_representation(proto_item *pi, const char *format, va_list ap)
7051 | {
7052 | size_t ret; /*tmp return value */
7053 | char *str;
7054 | field_info *fi = PITEM_FINFO(pi)((pi)->finfo);
7055 |
7056 | DISSECTOR_ASSERT(fi)((void) ((fi) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 7056, "fi"))));
7057 |
7058 | if (!proto_item_is_hidden(pi)) {
7059 | ITEM_LABEL_NEW(PNODE_POOL(pi), fi->rep)fi->rep = ((item_label_t*)wmem_alloc((((pi)->tree_data-> pinfo->pool)), sizeof(item_label_t))); fi->rep->value_pos = 0; fi->rep->value_len = 0;;
7060 |
7061 | str = wmem_strdup_vprintf(PNODE_POOL(pi)((pi)->tree_data->pinfo->pool), format, ap);
7062 | WS_UTF_8_CHECK(str, -1)do { const char *__uni_endptr; if (1 && (str) != ((void *)0) && !g_utf8_validate(str, -1, &__uni_endptr)) { do { if (1) { ws_log_utf8_full("UTF-8", LOG_LEVEL_DEBUG, "epan/proto.c" , 7062, __func__, str, -1, __uni_endptr); } } while (0); } } while (0);
7063 | fi->rep->value_pos = proto_find_value_pos(fi->hfinfo, str);
7064 | ret = ws_label_strcpy(fi->rep->representation, ITEM_LABEL_LENGTH240, 0, (const uint8_t*)str, 0);
7065 | if (ret >= ITEM_LABEL_LENGTH240) {
7066 | /* Uh oh, we don't have enough room. Tell the user that the field is truncated. */
7067 | size_t name_pos = label_find_name_pos(fi->rep);
7068 | label_mark_truncated(fi->rep->representation, name_pos, &fi->rep->value_pos);
7069 | }
7070 | fi->rep->value_len = strlen(fi->rep->representation) - fi->rep->value_pos;
7071 | }
7072 | }
7073 |
7074 | static int
7075 | proto_strlcpy(char *dest, const char *src, size_t dest_size)
7076 | {
7077 | if (dest_size == 0) return 0;
7078 |
7079 | size_t res = g_strlcpy(dest, src, dest_size);
7080 |
7081 | /* At most dest_size - 1 characters will be copied
7082 | * (unless dest_size is 0). */
7083 | if (res >= dest_size)
7084 | res = dest_size - 1;
7085 | return (int) res;
7086 | }
7087 |
7088 | static header_field_info *
7089 | hfinfo_same_name_get_prev(const header_field_info *hfinfo)
7090 | {
7091 | header_field_info *dup_hfinfo;
7092 |
7093 | if (hfinfo->same_name_prev_id == -1)
7094 | return NULL((void*)0);
7095 | PROTO_REGISTRAR_GET_NTH(hfinfo->same_name_prev_id, dup_hfinfo)if((hfinfo->same_name_prev_id == 0 || (unsigned)hfinfo-> same_name_prev_id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 7095 , __func__, "Unregistered hf! index=%d", hfinfo->same_name_prev_id ); ((void) ((hfinfo->same_name_prev_id > 0 && ( unsigned)hfinfo->same_name_prev_id < gpa_hfinfo.len) ? ( void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 7095, "hfinfo->same_name_prev_id > 0 && (unsigned)hfinfo->same_name_prev_id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> same_name_prev_id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 7095, "gpa_hfinfo.hfi[hfinfo->same_name_prev_id] != ((void*)0)" , "Unregistered hf!")))) ; dup_hfinfo = gpa_hfinfo.hfi[hfinfo ->same_name_prev_id];;
7096 | return dup_hfinfo;
7097 | }
7098 |
7099 | static void
7100 | hfinfo_remove_from_gpa_name_map(const header_field_info *hfinfo)
7101 | {
7102 | g_free(last_field_name);
7103 | last_field_name = NULL((void*)0);
7104 |
7105 | if (!hfinfo->same_name_next && hfinfo->same_name_prev_id == -1) {
7106 | /* No hfinfo with the same name */
7107 | wmem_map_remove(gpa_name_map, hfinfo->abbrev);
7108 | return;
7109 | }
7110 |
7111 | if (hfinfo->same_name_next) {
7112 | hfinfo->same_name_next->same_name_prev_id = hfinfo->same_name_prev_id;
7113 | }
7114 |
7115 | if (hfinfo->same_name_prev_id != -1) {
7116 | header_field_info *same_name_prev = hfinfo_same_name_get_prev(hfinfo);
7117 | same_name_prev->same_name_next = hfinfo->same_name_next;
7118 | if (!hfinfo->same_name_next) {
7119 | /* It's always the latest added hfinfo which is stored in gpa_name_map */
7120 | wmem_map_insert(gpa_name_map, (void *) (same_name_prev->abbrev), same_name_prev);
7121 | }
7122 | }
7123 | }
7124 |
7125 | int
7126 | proto_item_fill_display_label(const field_info *finfo, char *display_label_str, const int label_str_size)
7127 | {
7128 | const header_field_info *hfinfo = finfo->hfinfo;
7129 | int label_len = 0;
7130 | char *tmp_str;
7131 | const char *str;
7132 | const uint8_t *bytes;
7133 | uint32_t number;
7134 | uint64_t number64;
7135 | const char *hf_str_val;
7136 | char number_buf[NUMBER_LABEL_LENGTH80];
7137 | const char *number_out;
7138 | address addr;
7139 | const ipv4_addr_and_mask *ipv4;
7140 | const ipv6_addr_and_prefix *ipv6;
7141 |
7142 | switch (hfinfo->type) {
7143 |
7144 | case FT_NONE:
7145 | case FT_PROTOCOL:
7146 | return proto_strlcpy(display_label_str, UTF8_CHECK_MARK"\u2713", label_str_size);
7147 |
7148 | case FT_UINT_BYTES:
7149 | case FT_BYTES:
7150 | tmp_str = format_bytes_hfinfo_maxlen(NULL((void*)0),
7151 | hfinfo,
7152 | fvalue_get_bytes_data(finfo->value),
7153 | (unsigned)fvalue_length2(finfo->value),
7154 | label_str_size);
7155 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7156 | wmem_free(NULL((void*)0), tmp_str);
7157 | break;
7158 |
7159 | case FT_ABSOLUTE_TIME:
7160 | {
7161 | const nstime_t *value = fvalue_get_time(finfo->value);
7162 | int flags = ABS_TIME_TO_STR_SHOW_ZONE(1U << 0);
7163 | if (prefs.display_abs_time_ascii < ABS_TIME_ASCII_COLUMN) {
7164 | flags |= ABS_TIME_TO_STR_ISO8601(1U << 3);
7165 | }
7166 | if (hfinfo->strings) {
7167 | const char *time_string = try_time_val_to_str(value, (const time_value_string*)hfinfo->strings);
7168 | if (time_string != NULL((void*)0)) {
7169 | label_len = proto_strlcpy(display_label_str, time_string, label_str_size);
7170 | break;
7171 | }
7172 | }
7173 | tmp_str = abs_time_to_str_ex(NULL((void*)0), value, hfinfo->display, flags);
7174 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7175 | wmem_free(NULL((void*)0), tmp_str);
7176 | break;
7177 | }
7178 |
7179 | case FT_RELATIVE_TIME:
7180 | tmp_str = rel_time_to_secs_str(NULL((void*)0), fvalue_get_time(finfo->value));
7181 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7182 | wmem_free(NULL((void*)0), tmp_str);
7183 | break;
7184 |
7185 | case FT_BOOLEAN:
7186 | number64 = fvalue_get_uinteger64(finfo->value);
7187 | label_len = proto_strlcpy(display_label_str,
7188 | tfs_get_string(!!number64, hfinfo->strings), label_str_size);
7189 | break;
7190 |
7191 | case FT_CHAR:
7192 | number = fvalue_get_uinteger(finfo->value);
7193 |
7194 | if (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF) == BASE_CUSTOM) {
7195 | char tmp[ITEM_LABEL_LENGTH240];
7196 | custom_fmt_func_t fmtfunc = (custom_fmt_func_t)hfinfo->strings;
7197 |
7198 | DISSECTOR_ASSERT(fmtfunc)((void) ((fmtfunc) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 7198, "fmtfunc"))));
7199 | fmtfunc(tmp, number);
7200 |
7201 | label_len = proto_strlcpy(display_label_str, tmp, label_str_size);
7202 |
7203 | } else if (hfinfo->strings) {
7204 | number_out = hf_try_val_to_str(number, hfinfo);
7205 |
7206 | if (!number_out) {
7207 | number_out = hfinfo_char_value_format_display(BASE_HEX, number_buf, number);
7208 | }
7209 |
7210 | label_len = proto_strlcpy(display_label_str, number_out, label_str_size);
7211 |
7212 | } else {
7213 | number_out = hfinfo_char_value_format(hfinfo, number_buf, number);
7214 |
7215 | label_len = proto_strlcpy(display_label_str, number_out, label_str_size);
7216 | }
7217 |
7218 | break;
7219 |
7220 | /* XXX - make these just FT_NUMBER? */
7221 | case FT_INT8:
7222 | case FT_INT16:
7223 | case FT_INT24:
7224 | case FT_INT32:
7225 | case FT_UINT8:
7226 | case FT_UINT16:
7227 | case FT_UINT24:
7228 | case FT_UINT32:
7229 | case FT_FRAMENUM:
7230 | hf_str_val = NULL((void*)0);
7231 | number = FT_IS_INT(hfinfo->type)(((hfinfo->type) == FT_INT8 || (hfinfo->type) == FT_INT16 || (hfinfo->type) == FT_INT24 || (hfinfo->type) == FT_INT32 ) || ((hfinfo->type) == FT_INT40 || (hfinfo->type) == FT_INT48 || (hfinfo->type) == FT_INT56 || (hfinfo->type) == FT_INT64 )) ?
7232 | (uint32_t) fvalue_get_sinteger(finfo->value) :
7233 | fvalue_get_uinteger(finfo->value);
7234 |
7235 | if (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF) == BASE_CUSTOM) {
7236 | char tmp[ITEM_LABEL_LENGTH240];
7237 | custom_fmt_func_t fmtfunc = (custom_fmt_func_t)hfinfo->strings;
7238 |
7239 | DISSECTOR_ASSERT(fmtfunc)((void) ((fmtfunc) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 7239, "fmtfunc"))));
7240 | fmtfunc(tmp, number);
7241 |
7242 | label_len = proto_strlcpy(display_label_str, tmp, label_str_size);
7243 |
7244 | } else if (hfinfo->strings && hfinfo->type != FT_FRAMENUM) {
7245 | if (hfinfo->display & BASE_UNIT_STRING0x00001000) {
7246 | number_out = hfinfo_numeric_value_format(hfinfo, number_buf, number);
7247 | label_len = proto_strlcpy(display_label_str, number_out, label_str_size);
7248 | hf_str_val = hf_try_val_to_str(number, hfinfo);
7249 | label_len += proto_strlcpy(display_label_str+label_len, hf_str_val, label_str_size-label_len);
7250 | } else {
7251 | number_out = hf_try_val_to_str(number, hfinfo);
7252 |
7253 | if (!number_out) {
7254 | number_out = hfinfo_number_value_format_display(hfinfo, hfinfo->display, number_buf, number);
7255 | }
7256 |
7257 | label_len = proto_strlcpy(display_label_str, number_out, label_str_size);
7258 | }
7259 | } else {
7260 | number_out = hfinfo_number_value_format(hfinfo, number_buf, number);
7261 |
7262 | label_len = proto_strlcpy(display_label_str, number_out, label_str_size);
7263 | }
7264 |
7265 | break;
7266 |
7267 | case FT_INT40:
7268 | case FT_INT48:
7269 | case FT_INT56:
7270 | case FT_INT64:
7271 | case FT_UINT40:
7272 | case FT_UINT48:
7273 | case FT_UINT56:
7274 | case FT_UINT64:
7275 | hf_str_val = NULL((void*)0);
7276 | number64 = FT_IS_INT(hfinfo->type)(((hfinfo->type) == FT_INT8 || (hfinfo->type) == FT_INT16 || (hfinfo->type) == FT_INT24 || (hfinfo->type) == FT_INT32 ) || ((hfinfo->type) == FT_INT40 || (hfinfo->type) == FT_INT48 || (hfinfo->type) == FT_INT56 || (hfinfo->type) == FT_INT64 )) ?
7277 | (uint64_t) fvalue_get_sinteger64(finfo->value) :
7278 | fvalue_get_uinteger64(finfo->value);
7279 |
7280 | if (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF) == BASE_CUSTOM) {
7281 | char tmp[ITEM_LABEL_LENGTH240];
7282 | custom_fmt_func_64_t fmtfunc64 = (custom_fmt_func_64_t)hfinfo->strings;
7283 |
7284 | DISSECTOR_ASSERT(fmtfunc64)((void) ((fmtfunc64) ? (void)0 : (proto_report_dissector_bug( "%s:%u: failed assertion \"%s\"", "epan/proto.c", 7284, "fmtfunc64" ))));
7285 | fmtfunc64(tmp, number64);
7286 |
7287 | label_len = proto_strlcpy(display_label_str, tmp, label_str_size);
7288 | } else if (hfinfo->strings) {
7289 | if (hfinfo->display & BASE_UNIT_STRING0x00001000) {
7290 | number_out = hfinfo_numeric_value_format64(hfinfo, number_buf, number64);
7291 | label_len = proto_strlcpy(display_label_str, number_out, label_str_size);
7292 | hf_str_val = hf_try_val64_to_str(number64, hfinfo);
7293 | label_len += proto_strlcpy(display_label_str+label_len, hf_str_val, label_str_size-label_len);
7294 | } else {
7295 | number_out = hf_try_val64_to_str(number64, hfinfo);
7296 |
7297 | if (!number_out)
7298 | number_out = hfinfo_number_value_format_display64(hfinfo, hfinfo->display, number_buf, number64);
7299 |
7300 | label_len = proto_strlcpy(display_label_str, number_out, label_str_size);
7301 | }
7302 | } else {
7303 | number_out = hfinfo_number_value_format64(hfinfo, number_buf, number64);
7304 |
7305 | label_len = proto_strlcpy(display_label_str, number_out, label_str_size);
7306 | }
7307 |
7308 | break;
7309 |
7310 | case FT_EUI64:
7311 | set_address (&addr, AT_EUI64, EUI64_ADDR_LEN8, fvalue_get_bytes_data(finfo->value));
7312 | tmp_str = address_to_display(NULL((void*)0), &addr);
7313 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7314 | wmem_free(NULL((void*)0), tmp_str);
7315 | break;
7316 |
7317 | case FT_IPv4:
7318 | ipv4 = fvalue_get_ipv4(finfo->value);
7319 | //XXX: Should we ignore the mask?
7320 | set_address_ipv4(&addr, ipv4);
7321 | tmp_str = address_to_display(NULL((void*)0), &addr);
7322 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7323 | wmem_free(NULL((void*)0), tmp_str);
7324 | free_address(&addr);
7325 | break;
7326 |
7327 | case FT_IPv6:
7328 | ipv6 = fvalue_get_ipv6(finfo->value);
7329 | set_address_ipv6(&addr, ipv6);
7330 | tmp_str = address_to_display(NULL((void*)0), &addr);
7331 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7332 | wmem_free(NULL((void*)0), tmp_str);
7333 | free_address(&addr);
7334 | break;
7335 |
7336 | case FT_FCWWN:
7337 | set_address (&addr, AT_FCWWN, FCWWN_ADDR_LEN8, fvalue_get_bytes_data(finfo->value));
7338 | tmp_str = address_to_display(NULL((void*)0), &addr);
7339 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7340 | wmem_free(NULL((void*)0), tmp_str);
7341 | break;
7342 |
7343 | case FT_ETHER:
7344 | set_address (&addr, AT_ETHER, FT_ETHER_LEN6, fvalue_get_bytes_data(finfo->value));
7345 | tmp_str = address_to_display(NULL((void*)0), &addr);
7346 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7347 | wmem_free(NULL((void*)0), tmp_str);
7348 | break;
7349 |
7350 | case FT_GUID:
7351 | tmp_str = guid_to_str(NULL((void*)0), fvalue_get_guid(finfo->value));
7352 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7353 | wmem_free(NULL((void*)0), tmp_str);
7354 | break;
7355 |
7356 | case FT_REL_OID:
7357 | bytes = fvalue_get_bytes_data(finfo->value);
7358 | tmp_str = rel_oid_resolved_from_encoded(NULL((void*)0), bytes, (int)fvalue_length2(finfo->value));
7359 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7360 | wmem_free(NULL((void*)0), tmp_str);
7361 | break;
7362 |
7363 | case FT_OID:
7364 | bytes = fvalue_get_bytes_data(finfo->value);
7365 | tmp_str = oid_resolved_from_encoded(NULL((void*)0), bytes, (int)fvalue_length2(finfo->value));
7366 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7367 | wmem_free(NULL((void*)0), tmp_str);
7368 | break;
7369 |
7370 | case FT_SYSTEM_ID:
7371 | bytes = fvalue_get_bytes_data(finfo->value);
7372 | tmp_str = print_system_id(NULL((void*)0), bytes, (int)fvalue_length2(finfo->value));
7373 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7374 | wmem_free(NULL((void*)0), tmp_str);
7375 | break;
7376 |
7377 | case FT_FLOAT:
7378 | case FT_DOUBLE:
7379 | label_len = (int)fill_display_label_float(finfo, display_label_str, label_str_size);
7380 | break;
7381 |
7382 | case FT_IEEE_11073_SFLOAT:
7383 | case FT_IEEE_11073_FLOAT:
7384 | label_len = (int)fill_display_label_ieee_11073_float(finfo, display_label_str, label_str_size);
7385 | break;
7386 |
7387 | case FT_STRING:
7388 | case FT_STRINGZ:
7389 | case FT_UINT_STRING:
7390 | case FT_STRINGZPAD:
7391 | case FT_STRINGZTRUNC:
7392 | str = fvalue_get_string(finfo->value);
7393 | label_len = (int)ws_label_strcpy(display_label_str, label_str_size, 0, (const uint8_t*)str, label_strcat_flags(hfinfo));
7394 | if (label_len >= label_str_size) {
7395 | /* Truncation occurred. Get the real length
7396 | * copied (not including '\0') */
7397 | label_len = label_str_size ? label_str_size - 1 : 0;
7398 | }
7399 | break;
7400 |
7401 | default:
7402 | /* First try ftype string representation */
7403 | tmp_str = fvalue_to_string_repr(NULL((void*)0), finfo->value, FTREPR_DISPLAY, hfinfo->display);
7404 | if (!tmp_str) {
7405 | /* Default to show as bytes */
7406 | bytes = fvalue_get_bytes_data(finfo->value);
7407 | tmp_str = bytes_to_str(NULL, bytes, fvalue_length2(finfo->value))bytes_to_str_maxlen(((void*)0), bytes, fvalue_length2(finfo-> value), 36);
7408 | }
7409 | label_len = proto_strlcpy(display_label_str, tmp_str, label_str_size);
7410 | wmem_free(NULL((void*)0), tmp_str);
7411 | break;
7412 | }
7413 | return label_len;
7414 | }
7415 |
7416 | const char *
7417 | proto_custom_set(proto_tree* tree, GSList *field_ids, int occurrence, bool_Bool display_details,
7418 | char *result, char *expr, const int size)
7419 | {
7420 | int len, prev_len, last, i, offset_r = 0, offset_e = 0;
7421 | GPtrArray *finfos;
7422 | field_info *finfo = NULL((void*)0);
7423 | header_field_info* hfinfo;
7424 | const char *abbrev = NULL((void*)0);
7425 |
7426 | char *str;
7427 | col_custom_t *field_idx;
7428 | int field_id;
7429 | int ii = 0;
7430 |
7431 | ws_assert(field_ids != NULL)do { if ((1) && !(field_ids != ((void*)0))) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 7431, __func__, "assertion failed: %s" , "field_ids != ((void*)0)"); } while (0);
7432 | while ((field_idx = (col_custom_t *) g_slist_nth_data(field_ids, ii++))) {
7433 | field_id = field_idx->field_id;
7434 | if (field_id == 0) {
7435 | GPtrArray *fvals = NULL((void*)0);
7436 | bool_Bool passed = dfilter_apply_full(field_idx->dfilter, tree, &fvals);
7437 | if (fvals != NULL((void*)0)) {
7438 |
7439 | // XXX - Handling occurrences is unusual when more
7440 | // than one field is involved, e.g. there's four
7441 | // results for tcp.port + tcp.port. We may really
7442 | // want to apply it to the operands, not the output.
7443 | // Note that occurrences are not quite the same as
7444 | // the layer operator (should the grammar support
7445 | // both?)
7446 | /* Calculate single index or set outer boundaries */
7447 | len = g_ptr_array_len(fvals)((fvals) ? (fvals)->len : 0);
7448 | if (occurrence < 0) {
7449 | i = occurrence + len;
7450 | last = i;
7451 | } else if (occurrence > 0) {
7452 | i = occurrence - 1;
7453 | last = i;
7454 | } else {
7455 | i = 0;
7456 | last = len - 1;
7457 | }
7458 | if (i < 0 || i >= len) {
7459 | g_ptr_array_unref(fvals);
7460 | continue;
7461 | }
7462 | for (; i <= last; i++) {
7463 | /* XXX - We could have a "resolved" result
7464 | * for types where the value depends only
7465 | * on the type, e.g. FT_IPv4, and not on
7466 | * hfinfo->strings. Supporting the latter
7467 | * requires knowing which hfinfo matched
7468 | * if there are multiple with the same
7469 | * abbreviation. In any case, we need to
7470 | * know the expected return type of the
7471 | * field expression.
7472 | */
7473 | str = fvalue_to_string_repr(NULL((void*)0), fvals->pdata[i], FTREPR_DISPLAY, BASE_NONE);
7474 | if (offset_r && (offset_r < (size - 1)))
7475 | result[offset_r++] = ',';
7476 | if (offset_e && (offset_e < (size - 1)))
7477 | expr[offset_e++] = ',';
7478 | offset_r += proto_strlcpy(result+offset_r, str, size-offset_r);
7479 | // col_{add,append,set}_* calls ws_label_strcpy
7480 | offset_e = (int) ws_label_strcpy(expr, size, offset_e, (const uint8_t*)str, 0);
7481 |
7482 | g_free(str);
7483 | }
7484 | g_ptr_array_unref(fvals);
7485 | } else if (passed) {
7486 | // XXX - Occurrence doesn't make sense for a test
7487 | // output, it should be applied to the operands.
7488 | if (offset_r && (offset_r < (size - 1)))
7489 | result[offset_r++] = ',';
7490 | if (offset_e && (offset_e < (size - 1)))
7491 | expr[offset_e++] = ',';
7492 | /* Prevent multiple check marks */
7493 | if (strstr(result, UTF8_CHECK_MARK"\u2713" ",") == NULL((void*)0)) {
7494 | offset_r += proto_strlcpy(result+offset_r, UTF8_CHECK_MARK"\u2713", size-offset_r);
7495 | } else {
7496 | result[--offset_r] = '\0'; /* Remove the added trailing ',' */
7497 | }
7498 | if (strstr(expr, UTF8_CHECK_MARK"\u2713" ",") == NULL((void*)0)) {
7499 | offset_e += proto_strlcpy(expr+offset_e, UTF8_CHECK_MARK"\u2713", size-offset_e);
7500 | } else {
7501 | expr[--offset_e] = '\0'; /* Remove the added trailing ',' */
7502 | }
7503 | }
7504 | continue;
7505 | }
7506 | PROTO_REGISTRAR_GET_NTH((unsigned)field_id, hfinfo)if(((unsigned)field_id == 0 || (unsigned)(unsigned)field_id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 7506 , __func__, "Unregistered hf! index=%d", (unsigned)field_id); ((void) (((unsigned)field_id > 0 && (unsigned)(unsigned )field_id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 7506, "(unsigned)field_id > 0 && (unsigned)(unsigned)field_id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[(unsigned )field_id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 7506, "gpa_hfinfo.hfi[(unsigned)field_id] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[(unsigned)field_id];;
7507 |
7508 | /* do we need to rewind ? */
7509 | if (!hfinfo)
7510 | return "";
7511 |
7512 | if (occurrence < 0) {
7513 | /* Search other direction */
7514 | while (hfinfo->same_name_prev_id != -1) {
7515 | PROTO_REGISTRAR_GET_NTH(hfinfo->same_name_prev_id, hfinfo)if((hfinfo->same_name_prev_id == 0 || (unsigned)hfinfo-> same_name_prev_id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 7515 , __func__, "Unregistered hf! index=%d", hfinfo->same_name_prev_id ); ((void) ((hfinfo->same_name_prev_id > 0 && ( unsigned)hfinfo->same_name_prev_id < gpa_hfinfo.len) ? ( void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 7515, "hfinfo->same_name_prev_id > 0 && (unsigned)hfinfo->same_name_prev_id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> same_name_prev_id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 7515, "gpa_hfinfo.hfi[hfinfo->same_name_prev_id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> same_name_prev_id];;
7516 | }
7517 | }
7518 |
7519 | prev_len = 0; /* Reset handled occurrences */
7520 |
7521 | while (hfinfo) {
7522 | finfos = proto_get_finfo_ptr_array(tree, hfinfo->id);
7523 |
7524 | if (!finfos || !(len = g_ptr_array_len(finfos)((finfos) ? (finfos)->len : 0))) {
7525 | if (occurrence < 0) {
7526 | hfinfo = hfinfo->same_name_next;
7527 | } else {
7528 | hfinfo = hfinfo_same_name_get_prev(hfinfo);
7529 | }
7530 | continue;
7531 | }
7532 |
7533 | /* Are there enough occurrences of the field? */
7534 | if (((occurrence - prev_len) > len) || ((occurrence + prev_len) < -len)) {
7535 | if (occurrence < 0) {
7536 | hfinfo = hfinfo->same_name_next;
7537 | } else {
7538 | hfinfo = hfinfo_same_name_get_prev(hfinfo);
7539 | }
7540 | prev_len += len;
7541 | continue;
7542 | }
7543 |
7544 | /* Calculate single index or set outer boundaries */
7545 | if (occurrence < 0) {
7546 | i = occurrence + len + prev_len;
7547 | last = i;
7548 | } else if (occurrence > 0) {
7549 | i = occurrence - 1 - prev_len;
7550 | last = i;
7551 | } else {
7552 | i = 0;
7553 | last = len - 1;
7554 | }
7555 |
7556 | prev_len += len; /* Count handled occurrences */
7557 |
7558 | while (i <= last) {
7559 | finfo = (field_info *)g_ptr_array_index(finfos, i)((finfos)->pdata)[i];
7560 |
7561 | if (offset_r && (offset_r < (size - 1)))
7562 | result[offset_r++] = ',';
7563 |
7564 | if (display_details) {
7565 | char representation[ITEM_LABEL_LENGTH240];
7566 | size_t offset = 0;
7567 |
7568 | if (finfo->rep && finfo->rep->value_len) {
7569 | g_strlcpy(representation, &finfo->rep->representation[finfo->rep->value_pos],
7570 | MIN(finfo->rep->value_len + 1, ITEM_LABEL_LENGTH)(((finfo->rep->value_len + 1) < (240)) ? (finfo-> rep->value_len + 1) : (240)));
7571 | } else {
7572 | proto_item_fill_label(finfo, representation, &offset);
7573 | }
7574 | offset_r += proto_strlcpy(result+offset_r, &representation[offset], size-offset_r);
7575 | } else {
7576 | switch (hfinfo->type) {
7577 |
7578 | case FT_NONE:
7579 | case FT_PROTOCOL:
7580 | /* Prevent multiple check marks */
7581 | if (strstr(result, UTF8_CHECK_MARK"\u2713" ",") == NULL((void*)0)) {
7582 | offset_r += proto_item_fill_display_label(finfo, result+offset_r, size-offset_r);
7583 | } else {
7584 | result[--offset_r] = '\0'; /* Remove the added trailing ',' again */
7585 | }
7586 | break;
7587 |
7588 | default:
7589 | offset_r += proto_item_fill_display_label(finfo, result+offset_r, size-offset_r);
7590 | break;
7591 | }
7592 | }
7593 |
7594 | if (offset_e && (offset_e < (size - 1)))
7595 | expr[offset_e++] = ',';
7596 |
7597 | if (hfinfo->strings && hfinfo->type != FT_FRAMENUM && FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF) == BASE_NONE && (FT_IS_INT(hfinfo->type)(((hfinfo->type) == FT_INT8 || (hfinfo->type) == FT_INT16 || (hfinfo->type) == FT_INT24 || (hfinfo->type) == FT_INT32 ) || ((hfinfo->type) == FT_INT40 || (hfinfo->type) == FT_INT48 || (hfinfo->type) == FT_INT56 || (hfinfo->type) == FT_INT64 )) || FT_IS_UINT(hfinfo->type)(((hfinfo->type) == FT_CHAR || (hfinfo->type) == FT_UINT8 || (hfinfo->type) == FT_UINT16 || (hfinfo->type) == FT_UINT24 || (hfinfo->type) == FT_UINT32 || (hfinfo->type) == FT_FRAMENUM ) || ((hfinfo->type) == FT_UINT40 || (hfinfo->type) == FT_UINT48 || (hfinfo->type) == FT_UINT56 || (hfinfo->type) == FT_UINT64 )))) {
7598 | const char *hf_str_val;
7599 | /* Integer types with BASE_NONE never get the numeric value. */
7600 | if (FT_IS_INT32(hfinfo->type)((hfinfo->type) == FT_INT8 || (hfinfo->type) == FT_INT16 || (hfinfo->type) == FT_INT24 || (hfinfo->type) == FT_INT32 )) {
7601 | hf_str_val = hf_try_val_to_str_const(fvalue_get_sinteger(finfo->value), hfinfo, "Unknown");
7602 | } else if (FT_IS_UINT32(hfinfo->type)((hfinfo->type) == FT_CHAR || (hfinfo->type) == FT_UINT8 || (hfinfo->type) == FT_UINT16 || (hfinfo->type) == FT_UINT24 || (hfinfo->type) == FT_UINT32 || (hfinfo->type) == FT_FRAMENUM )) {
7603 | hf_str_val = hf_try_val_to_str_const(fvalue_get_uinteger(finfo->value), hfinfo, "Unknown");
7604 | } else if (FT_IS_INT64(hfinfo->type)((hfinfo->type) == FT_INT40 || (hfinfo->type) == FT_INT48 || (hfinfo->type) == FT_INT56 || (hfinfo->type) == FT_INT64 )) {
7605 | hf_str_val = hf_try_val64_to_str_const(fvalue_get_sinteger64(finfo->value), hfinfo, "Unknown");
7606 | } else { // if (FT_IS_UINT64(hfinfo->type)) {
7607 | hf_str_val = hf_try_val64_to_str_const(fvalue_get_uinteger64(finfo->value), hfinfo, "Unknown");
7608 | }
7609 | snprintf(expr+offset_e, size-offset_e, "\"%s\"", hf_str_val);
7610 | offset_e = (int)strlen(expr);
7611 | } else if (hfinfo->type == FT_NONE || hfinfo->type == FT_PROTOCOL) {
7612 | /* Prevent multiple check marks */
7613 | if (strstr(expr, UTF8_CHECK_MARK"\u2713" ",") == NULL((void*)0)) {
7614 | offset_e += proto_item_fill_display_label(finfo, expr+offset_e, size-offset_e);
7615 | } else {
7616 | expr[--offset_e] = '\0'; /* Remove the added trailing ',' again */
7617 | }
7618 | } else {
7619 | str = fvalue_to_string_repr(NULL((void*)0), finfo->value, FTREPR_RAW, finfo->hfinfo->display);
7620 | // col_{add,append,set}_* calls ws_label_strcpy
7621 | offset_e = (int) ws_label_strcpy(expr, size, offset_e, (const uint8_t*)str, 0);
7622 | wmem_free(NULL((void*)0), str);
7623 | }
7624 | i++;
7625 | }
7626 |
7627 | /* XXX: Why is only the first abbreviation returned for a multifield
7628 | * custom column? */
7629 | if (!abbrev) {
7630 | /* Store abbrev for return value */
7631 | abbrev = hfinfo->abbrev;
7632 | }
7633 |
7634 | if (occurrence == 0) {
7635 | /* Fetch next hfinfo with same name (abbrev) */
7636 | hfinfo = hfinfo_same_name_get_prev(hfinfo);
7637 | } else {
7638 | hfinfo = NULL((void*)0);
7639 | }
7640 | }
7641 | }
7642 |
7643 | if (offset_r >= (size - 1)) {
7644 | mark_truncated(result, 0, size, NULL((void*)0));
7645 | }
7646 | if (offset_e >= (size - 1)) {
7647 | mark_truncated(expr, 0, size, NULL((void*)0));
7648 | }
7649 | return abbrev ? abbrev : "";
7650 | }
7651 |
7652 | char *
7653 | proto_custom_get_filter(epan_dissect_t* edt, GSList *field_ids, int occurrence)
7654 | {
7655 | int len, prev_len, last, i;
7656 | GPtrArray *finfos;
7657 | field_info *finfo = NULL((void*)0);
7658 | header_field_info* hfinfo;
7659 |
7660 | char *filter = NULL((void*)0);
7661 | GPtrArray *filter_array;
7662 |
7663 | col_custom_t *col_custom;
7664 | int field_id;
7665 |
7666 | ws_assert(field_ids != NULL)do { if ((1) && !(field_ids != ((void*)0))) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 7666, __func__, "assertion failed: %s" , "field_ids != ((void*)0)"); } while (0);
7667 | filter_array = g_ptr_array_new_full(g_slist_length(field_ids), g_free);
7668 | for (GSList *iter = field_ids; iter; iter = iter->next) {
7669 | col_custom = (col_custom_t*)iter->data;
7670 | field_id = col_custom->field_id;
7671 | if (field_id == 0) {
7672 | GPtrArray *fvals = NULL((void*)0);
7673 | bool_Bool passed = dfilter_apply_full(col_custom->dfilter, edt->tree, &fvals);
7674 | if (fvals != NULL((void*)0)) {
7675 | // XXX - Handling occurrences is unusual when more
7676 | // than one field is involved, e.g. there's four
7677 | // results for tcp.port + tcp.port. We really
7678 | // want to apply it to the operands, not the output.
7679 | /* Calculate single index or set outer boundaries */
7680 | len = g_ptr_array_len(fvals)((fvals) ? (fvals)->len : 0);
7681 | if (occurrence < 0) {
7682 | i = occurrence + len;
7683 | last = i;
7684 | } else if (occurrence > 0) {
7685 | i = occurrence - 1;
7686 | last = i;
7687 | } else {
7688 | i = 0;
7689 | last = len - 1;
7690 | }
7691 | if (i < 0 || i >= len) {
7692 | g_ptr_array_unref(fvals);
7693 | continue;
7694 | }
7695 | for (; i <= last; i++) {
7696 | /* XXX - Should multiple values for one
7697 | * field use set membership to reduce
7698 | * verbosity, here and below? */
7699 | char *str = fvalue_to_string_repr(NULL((void*)0), fvals->pdata[i], FTREPR_DFILTER, BASE_NONE);
7700 | filter = wmem_strdup_printf(NULL((void*)0), "%s == %s", col_custom->dftext, str);
7701 | wmem_free(NULL((void*)0), str);
7702 | if (!g_ptr_array_find_with_equal_func(filter_array, filter, g_str_equal, NULL((void*)0))) {
7703 | g_ptr_array_add(filter_array, filter);
7704 | }
7705 | }
7706 | g_ptr_array_unref(fvals);
7707 | } else if (passed) {
7708 | filter = wmem_strdup(NULL((void*)0), col_custom->dftext);
7709 | if (!g_ptr_array_find_with_equal_func(filter_array, filter, g_str_equal, NULL((void*)0))) {
7710 | g_ptr_array_add(filter_array, filter);
7711 | }
7712 | } else {
7713 | filter = wmem_strdup_printf(NULL((void*)0), "!(%s)", col_custom->dftext);
7714 | if (!g_ptr_array_find_with_equal_func(filter_array, filter, g_str_equal, NULL((void*)0))) {
7715 | g_ptr_array_add(filter_array, filter);
7716 | }
7717 | }
7718 | continue;
7719 | }
7720 |
7721 | PROTO_REGISTRAR_GET_NTH((unsigned)field_id, hfinfo)if(((unsigned)field_id == 0 || (unsigned)(unsigned)field_id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 7721 , __func__, "Unregistered hf! index=%d", (unsigned)field_id); ((void) (((unsigned)field_id > 0 && (unsigned)(unsigned )field_id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 7721, "(unsigned)field_id > 0 && (unsigned)(unsigned)field_id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[(unsigned )field_id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 7721, "gpa_hfinfo.hfi[(unsigned)field_id] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[(unsigned)field_id];;
7722 |
7723 | /* do we need to rewind ? */
7724 | if (!hfinfo)
7725 | return NULL((void*)0);
7726 |
7727 | if (occurrence < 0) {
7728 | /* Search other direction */
7729 | while (hfinfo->same_name_prev_id != -1) {
7730 | PROTO_REGISTRAR_GET_NTH(hfinfo->same_name_prev_id, hfinfo)if((hfinfo->same_name_prev_id == 0 || (unsigned)hfinfo-> same_name_prev_id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 7730 , __func__, "Unregistered hf! index=%d", hfinfo->same_name_prev_id ); ((void) ((hfinfo->same_name_prev_id > 0 && ( unsigned)hfinfo->same_name_prev_id < gpa_hfinfo.len) ? ( void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 7730, "hfinfo->same_name_prev_id > 0 && (unsigned)hfinfo->same_name_prev_id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> same_name_prev_id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 7730, "gpa_hfinfo.hfi[hfinfo->same_name_prev_id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfinfo-> same_name_prev_id];;
7731 | }
7732 | }
7733 |
7734 | prev_len = 0; /* Reset handled occurrences */
7735 |
7736 | while (hfinfo) {
7737 | finfos = proto_get_finfo_ptr_array(edt->tree, hfinfo->id);
7738 |
7739 | if (!finfos || !(len = g_ptr_array_len(finfos)((finfos) ? (finfos)->len : 0))) {
7740 | if (occurrence < 0) {
7741 | hfinfo = hfinfo->same_name_next;
7742 | } else {
7743 | hfinfo = hfinfo_same_name_get_prev(hfinfo);
7744 | }
7745 | continue;
7746 | }
7747 |
7748 | /* Are there enough occurrences of the field? */
7749 | if (((occurrence - prev_len) > len) || ((occurrence + prev_len) < -len)) {
7750 | if (occurrence < 0) {
7751 | hfinfo = hfinfo->same_name_next;
7752 | } else {
7753 | hfinfo = hfinfo_same_name_get_prev(hfinfo);
7754 | }
7755 | prev_len += len;
7756 | continue;
7757 | }
7758 |
7759 | /* Calculate single index or set outer boundaries */
7760 | if (occurrence < 0) {
7761 | i = occurrence + len + prev_len;
7762 | last = i;
7763 | } else if (occurrence > 0) {
7764 | i = occurrence - 1 - prev_len;
7765 | last = i;
7766 | } else {
7767 | i = 0;
7768 | last = len - 1;
7769 | }
7770 |
7771 | prev_len += len; /* Count handled occurrences */
7772 |
7773 | while (i <= last) {
7774 | finfo = (field_info *)g_ptr_array_index(finfos, i)((finfos)->pdata)[i];
7775 |
7776 | filter = proto_construct_match_selected_string(finfo, edt);
7777 | if (filter) {
7778 | /* Only add the same expression once (especially for FT_PROTOCOL).
7779 | * The ptr array doesn't have NULL entries so g_str_equal is fine.
7780 | */
7781 | if (!g_ptr_array_find_with_equal_func(filter_array, filter, g_str_equal, NULL((void*)0))) {
7782 | g_ptr_array_add(filter_array, filter);
7783 | }
7784 | }
7785 | i++;
7786 | }
7787 |
7788 | if (occurrence == 0) {
7789 | /* Fetch next hfinfo with same name (abbrev) */
7790 | hfinfo = hfinfo_same_name_get_prev(hfinfo);
7791 | } else {
7792 | hfinfo = NULL((void*)0);
7793 | }
7794 | }
7795 | }
7796 |
7797 | g_ptr_array_add(filter_array, NULL((void*)0));
7798 |
7799 | /* XXX: Should this be || or && ? */
7800 | char *output = g_strjoinv(" || ", (char **)filter_array->pdata);
7801 |
7802 | g_ptr_array_free(filter_array, true1);
7803 |
7804 | return output;
7805 | }
7806 |
7807 | /* Set text of proto_item after having already been created. */
7808 | void
7809 | proto_item_set_text(proto_item *pi, const char *format, ...)
7810 | {
7811 | field_info *fi = NULL((void*)0);
7812 | va_list ap;
7813 |
7814 | TRY_TO_FAKE_THIS_REPR_VOID(pi)if (!pi || !((pi)->finfo)) return; if (!(((pi)->tree_data )->visible) && proto_item_is_hidden((pi))) { return ; };
7815 |
7816 | fi = PITEM_FINFO(pi)((pi)->finfo);
7817 | if (fi == NULL((void*)0))
7818 | return;
7819 |
7820 | if (fi->rep) {
7821 | ITEM_LABEL_FREE(PNODE_POOL(pi), fi->rep)wmem_free(((pi)->tree_data->pinfo->pool), fi->rep );;
7822 | fi->rep = NULL((void*)0);
7823 | }
7824 |
7825 | va_start(ap, format)__builtin_va_start(ap, format);
7826 | proto_tree_set_representation(pi, format, ap);
7827 | va_end(ap)__builtin_va_end(ap);
7828 | }
7829 |
7830 | /* Append to text of proto_item after having already been created. */
7831 | void
7832 | proto_item_append_text(proto_item *pi, const char *format, ...)
7833 | {
7834 | field_info *fi = NULL((void*)0);
7835 | size_t curlen;
7836 | char *str;
7837 | va_list ap;
7838 |
7839 | TRY_TO_FAKE_THIS_REPR_VOID(pi)if (!pi || !((pi)->finfo)) return; if (!(((pi)->tree_data )->visible) && proto_item_is_hidden((pi))) { return ; };
7840 |
7841 | fi = PITEM_FINFO(pi)((pi)->finfo);
7842 | if (fi == NULL((void*)0)) {
7843 | return;
7844 | }
7845 |
7846 | if (!proto_item_is_hidden(pi)) {
7847 | /*
7848 | * If we don't already have a representation,
7849 | * generate the default representation.
7850 | */
7851 | if (fi->rep == NULL((void*)0)) {
7852 | ITEM_LABEL_NEW(PNODE_POOL(pi), fi->rep)fi->rep = ((item_label_t*)wmem_alloc((((pi)->tree_data-> pinfo->pool)), sizeof(item_label_t))); fi->rep->value_pos = 0; fi->rep->value_len = 0;;
7853 | proto_item_fill_label(fi, fi->rep->representation, &fi->rep->value_pos);
7854 | /* Check for special case append value to FT_NONE or FT_PROTOCOL */
7855 | if ((fi->hfinfo->type == FT_NONE || fi->hfinfo->type == FT_PROTOCOL) &&
7856 | (strncmp(format, ": ", 2) == 0)) {
7857 | fi->rep->value_pos += 2;
7858 | }
7859 | }
7860 | if (fi->rep) {
7861 | curlen = strlen(fi->rep->representation);
7862 | /* curlen doesn't include the \0 byte.
7863 | * XXX: If curlen + 4 > ITEM_LABEL_LENGTH, we can't tell if
7864 | * the representation has already been truncated (of an up
7865 | * to 4 byte UTF-8 character) or is just at the maximum length
7866 | * unless we search for " [truncated]" (which may not be
7867 | * at the start.)
7868 | * It's safer to do nothing.
7869 | */
7870 | if (ITEM_LABEL_LENGTH240 > (curlen + 4)) {
7871 | va_start(ap, format)__builtin_va_start(ap, format);
7872 | str = wmem_strdup_vprintf(PNODE_POOL(pi)((pi)->tree_data->pinfo->pool), format, ap);
7873 | va_end(ap)__builtin_va_end(ap);
7874 | WS_UTF_8_CHECK(str, -1)do { const char *__uni_endptr; if (1 && (str) != ((void *)0) && !g_utf8_validate(str, -1, &__uni_endptr)) { do { if (1) { ws_log_utf8_full("UTF-8", LOG_LEVEL_DEBUG, "epan/proto.c" , 7874, __func__, str, -1, __uni_endptr); } } while (0); } } while (0);
7875 | /* Keep fi->rep->value_pos */
7876 | curlen = ws_label_strcpy(fi->rep->representation, ITEM_LABEL_LENGTH240, curlen, (const uint8_t*)str, 0);
7877 | if (curlen >= ITEM_LABEL_LENGTH240) {
7878 | /* Uh oh, we don't have enough room. Tell the user that the field is truncated. */
7879 | size_t name_pos = label_find_name_pos(fi->rep);
7880 | label_mark_truncated(fi->rep->representation, name_pos, &fi->rep->value_pos);
7881 | }
7882 | fi->rep->value_len = strlen(fi->rep->representation) - fi->rep->value_pos;
7883 | }
7884 | }
7885 | }
7886 | }
7887 |
7888 | /* Prepend to text of proto_item after having already been created. */
7889 | void
7890 | proto_item_prepend_text(proto_item *pi, const char *format, ...)
7891 | {
7892 | field_info *fi = NULL((void*)0);
7893 | size_t pos;
7894 | char representation[ITEM_LABEL_LENGTH240];
7895 | char *str;
7896 | va_list ap;
7897 |
7898 | TRY_TO_FAKE_THIS_REPR_VOID(pi)if (!pi || !((pi)->finfo)) return; if (!(((pi)->tree_data )->visible) && proto_item_is_hidden((pi))) { return ; };
7899 |
7900 | fi = PITEM_FINFO(pi)((pi)->finfo);
7901 | if (fi == NULL((void*)0)) {
7902 | return;
7903 | }
7904 |
7905 | if (!proto_item_is_hidden(pi)) {
7906 | /*
7907 | * If we don't already have a representation,
7908 | * generate the default representation.
7909 | */
7910 | if (fi->rep == NULL((void*)0)) {
7911 | ITEM_LABEL_NEW(PNODE_POOL(pi), fi->rep)fi->rep = ((item_label_t*)wmem_alloc((((pi)->tree_data-> pinfo->pool)), sizeof(item_label_t))); fi->rep->value_pos = 0; fi->rep->value_len = 0;;
7912 | proto_item_fill_label(fi, representation, &fi->rep->value_pos);
7913 | } else
7914 | (void) g_strlcpy(representation, fi->rep->representation, ITEM_LABEL_LENGTH240);
7915 |
7916 | va_start(ap, format)__builtin_va_start(ap, format);
7917 | str = wmem_strdup_vprintf(PNODE_POOL(pi)((pi)->tree_data->pinfo->pool), format, ap);
7918 | va_end(ap)__builtin_va_end(ap);
7919 | WS_UTF_8_CHECK(str, -1)do { const char *__uni_endptr; if (1 && (str) != ((void *)0) && !g_utf8_validate(str, -1, &__uni_endptr)) { do { if (1) { ws_log_utf8_full("UTF-8", LOG_LEVEL_DEBUG, "epan/proto.c" , 7919, __func__, str, -1, __uni_endptr); } } while (0); } } while (0);
7920 | fi->rep->value_pos += strlen(str);
7921 | pos = ws_label_strcpy(fi->rep->representation, ITEM_LABEL_LENGTH240, 0, (const uint8_t*)str, 0);
7922 | pos = ws_label_strcpy(fi->rep->representation, ITEM_LABEL_LENGTH240, pos, (const uint8_t*)representation, 0);
7923 | /* XXX: As above, if the old representation is close to the label
7924 | * length, it might already be marked as truncated. */
7925 | if (pos >= ITEM_LABEL_LENGTH240 && (strlen(representation) + 4) <= ITEM_LABEL_LENGTH240) {
7926 | /* Uh oh, we don't have enough room. Tell the user that the field is truncated. */
7927 | size_t name_pos = label_find_name_pos(fi->rep);
7928 | label_mark_truncated(fi->rep->representation, name_pos, &fi->rep->value_pos);
7929 | }
7930 | fi->rep->value_len = strlen(fi->rep->representation) - fi->rep->value_pos;
7931 | }
7932 | }
7933 |
7934 | static void
7935 | finfo_set_len(field_info *fi, const int length)
7936 | {
7937 | int length_remaining;
7938 |
7939 | DISSECTOR_ASSERT_HINT(length >= 0, fi->hfinfo->abbrev)((void) ((length >= 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 7939, "length >= 0", fi->hfinfo->abbrev))));
7940 | length_remaining = tvb_captured_length_remaining(fi->ds_tvb, fi->start);
7941 | if (length > length_remaining)
7942 | fi->length = length_remaining;
7943 | else
7944 | fi->length = length;
7945 |
7946 | /* If we have an FT_PROTOCOL we need to set the length of the fvalue tvbuff as well. */
7947 | if (fvalue_type_ftenum(fi->value) == FT_PROTOCOL) {
7948 | fvalue_set_protocol_length(fi->value, fi->length);
7949 | }
7950 |
7951 | /*
7952 | * You cannot just make the "len" field of a GByteArray
7953 | * larger, if there's no data to back that length;
7954 | * you can only make it smaller.
7955 | */
7956 | if (fvalue_type_ftenum(fi->value) == FT_BYTES && fi->length > 0) {
7957 | GBytes *bytes = fvalue_get_bytes(fi->value);
7958 | size_t size;
7959 | const void *data = g_bytes_get_data(bytes, &size);
7960 | if ((size_t)fi->length <= size) {
7961 | fvalue_set_bytes_data(fi->value, data, fi->length);
7962 | }
7963 | g_bytes_unref(bytes);
7964 | }
7965 | }
7966 |
7967 | void
7968 | proto_item_set_len(proto_item *pi, const int length)
7969 | {
7970 | field_info *fi;
7971 |
7972 | if (pi == NULL((void*)0))
7973 | return;
7974 |
7975 | fi = PITEM_FINFO(pi)((pi)->finfo);
7976 | if (fi == NULL((void*)0))
7977 | return;
7978 |
7979 | finfo_set_len(fi, length);
7980 | }
7981 |
7982 | /*
7983 | * Sets the length of the item based on its start and on the specified
7984 | * offset, which is the offset past the end of the item; as the start
7985 | * in the item is relative to the beginning of the data source tvbuff,
7986 | * we need to pass in a tvbuff - the end offset is relative to the beginning
7987 | * of that tvbuff.
7988 | */
7989 | void
7990 | proto_item_set_end(proto_item *pi, tvbuff_t *tvb, unsigned end)
7991 | {
7992 | field_info *fi;
7993 | int length;
7994 |
7995 | if (pi == NULL((void*)0))
7996 | return;
7997 |
7998 | fi = PITEM_FINFO(pi)((pi)->finfo);
7999 | if (fi == NULL((void*)0))
8000 | return;
8001 |
8002 | end += tvb_raw_offset(tvb);
8003 | DISSECTOR_ASSERT(end >= fi->start)((void) ((end >= fi->start) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 8003, "end >= fi->start" ))));
8004 | length = end - fi->start;
8005 |
8006 | finfo_set_len(fi, length);
8007 | }
8008 |
8009 | int
8010 | proto_item_get_len(const proto_item *pi)
8011 | {
8012 | field_info *fi;
8013 |
8014 | if (!pi)
8015 | return -1;
8016 | fi = PITEM_FINFO(pi)((pi)->finfo);
8017 | if (fi) {
8018 | return fi->length;
8019 | }
8020 | return -1;
8021 | }
8022 |
8023 | void
8024 | proto_item_set_bits_offset_len(proto_item *ti, int bits_offset, int bits_len) {
8025 | if (!ti) {
8026 | return;
8027 | }
8028 | FI_SET_FLAG(PNODE_FINFO(ti), FI_BITS_OFFSET(bits_offset))do { if (((ti)->finfo)) (((ti)->finfo))->flags = ((( ti)->finfo))->flags | ((((bits_offset) & 63) << 5)); } while(0);
8029 | FI_SET_FLAG(PNODE_FINFO(ti), FI_BITS_SIZE(bits_len))do { if (((ti)->finfo)) (((ti)->finfo))->flags = ((( ti)->finfo))->flags | ((((bits_len) & 63) << 12 )); } while(0);
8030 | }
8031 |
8032 | char *
8033 | proto_item_get_display_repr(wmem_allocator_t *scope, proto_item *pi)
8034 | {
8035 | field_info *fi;
8036 |
8037 | if (!pi)
8038 | return wmem_strdup(scope, "");
8039 | fi = PITEM_FINFO(pi)((pi)->finfo);
8040 | if (!fi)
8041 | return wmem_strdup(scope, "");
8042 | DISSECTOR_ASSERT(fi->hfinfo != NULL)((void) ((fi->hfinfo != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 8042, "fi->hfinfo != ((void*)0)" ))));
8043 | return fvalue_to_string_repr(scope, fi->value, FTREPR_DISPLAY, fi->hfinfo->display);
8044 | }
8045 |
8046 | proto_tree *
8047 | proto_tree_create_root(packet_info *pinfo)
8048 | {
8049 | proto_node *pnode;
8050 |
8051 | /* Initialize the proto_node */
8052 | pnode = g_slice_new(proto_tree)((proto_tree*) g_slice_alloc (sizeof (proto_tree)));
8053 | PROTO_NODE_INIT(pnode)pnode->first_child = ((void*)0); pnode->last_child = (( void*)0); pnode->next = ((void*)0);;
8054 | pnode->parent = NULL((void*)0);
8055 | PNODE_FINFO(pnode)((pnode)->finfo) = NULL((void*)0);
8056 | pnode->tree_data = g_slice_new(tree_data_t)((tree_data_t*) g_slice_alloc (sizeof (tree_data_t)));
8057 |
8058 | /* Make sure we can access pinfo everywhere */
8059 | pnode->tree_data->pinfo = pinfo;
8060 |
8061 | /* Don't initialize the tree_data_t. Wait until we know we need it */
8062 | pnode->tree_data->interesting_hfids = NULL((void*)0);
8063 |
8064 | /* Set the default to false so it's easier to
8065 | * find errors; if we expect to see the protocol tree
8066 | * but for some reason the default 'visible' is not
8067 | * changed, then we'll find out very quickly. */
8068 | pnode->tree_data->visible = false0;
8069 |
8070 | /* Make sure that we fake protocols (if possible) */
8071 | pnode->tree_data->fake_protocols = true1;
8072 |
8073 | /* Keep track of the number of children */
8074 | pnode->tree_data->count = 0;
8075 |
8076 | /* Initialize our loop checks */
8077 | pnode->tree_data->idle_count_ds_tvb = NULL((void*)0);
8078 | pnode->tree_data->max_start = 0;
8079 | pnode->tree_data->start_idle_count = 0;
8080 |
8081 | return (proto_tree *)pnode;
8082 | }
8083 |
8084 |
8085 | /* "prime" a proto_tree with a single hfid that a dfilter
8086 | * is interested in. */
8087 | void
8088 | proto_tree_prime_with_hfid(proto_tree *tree _U___attribute__((unused)), const int hfid)
8089 | {
8090 | header_field_info *hfinfo;
8091 |
8092 | PROTO_REGISTRAR_GET_NTH(hfid, hfinfo)if((hfid == 0 || (unsigned)hfid > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 8092, __func__, "Unregistered hf! index=%d" , hfid); ((void) ((hfid > 0 && (unsigned)hfid < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 8092, "hfid > 0 && (unsigned)hfid < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfid] != ( (void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 8092, "gpa_hfinfo.hfi[hfid] != ((void*)0)", "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfid];;
8093 | /* this field is referenced by a filter so increase the refcount.
8094 | also increase the refcount for the parent, i.e the protocol.
8095 | Don't increase the refcount if we're already printing the
8096 | type, as that is a superset of direct reference.
8097 | */
8098 | if (hfinfo->ref_type != HF_REF_TYPE_PRINT) {
8099 | hfinfo->ref_type = HF_REF_TYPE_DIRECT;
8100 | }
8101 | /* only increase the refcount if there is a parent.
8102 | if this is a protocol and not a field then parent will be -1
8103 | and there is no parent to add any refcounting for.
8104 | */
8105 | if (hfinfo->parent != -1) {
8106 | header_field_info *parent_hfinfo;
8107 | PROTO_REGISTRAR_GET_NTH(hfinfo->parent, parent_hfinfo)if((hfinfo->parent == 0 || (unsigned)hfinfo->parent > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 8107 , __func__, "Unregistered hf! index=%d", hfinfo->parent); ( (void) ((hfinfo->parent > 0 && (unsigned)hfinfo ->parent < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 8107, "hfinfo->parent > 0 && (unsigned)hfinfo->parent < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> parent] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 8107, "gpa_hfinfo.hfi[hfinfo->parent] != ((void*)0)", "Unregistered hf!" )))) ; parent_hfinfo = gpa_hfinfo.hfi[hfinfo->parent];;
8108 |
8109 | /* Mark parent as indirectly referenced unless it is already directly
8110 | * referenced, i.e. the user has specified the parent in a filter.
8111 | */
8112 | if (parent_hfinfo->ref_type == HF_REF_TYPE_NONE)
8113 | parent_hfinfo->ref_type = HF_REF_TYPE_INDIRECT;
8114 | }
8115 | }
8116 |
8117 | /* "prime" a proto_tree with a single hfid that a dfilter
8118 | * is interested in. */
8119 | void
8120 | proto_tree_prime_with_hfid_print(proto_tree *tree _U___attribute__((unused)), const int hfid)
8121 | {
8122 | header_field_info *hfinfo;
8123 |
8124 | PROTO_REGISTRAR_GET_NTH(hfid, hfinfo)if((hfid == 0 || (unsigned)hfid > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 8124, __func__, "Unregistered hf! index=%d" , hfid); ((void) ((hfid > 0 && (unsigned)hfid < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 8124, "hfid > 0 && (unsigned)hfid < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfid] != ( (void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 8124, "gpa_hfinfo.hfi[hfid] != ((void*)0)", "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfid];;
8125 | /* this field is referenced by an (output) filter so increase the refcount.
8126 | also increase the refcount for the parent, i.e the protocol.
8127 | */
8128 | hfinfo->ref_type = HF_REF_TYPE_PRINT;
8129 | /* only increase the refcount if there is a parent.
8130 | if this is a protocol and not a field then parent will be -1
8131 | and there is no parent to add any refcounting for.
8132 | */
8133 | if (hfinfo->parent != -1) {
8134 | header_field_info *parent_hfinfo;
8135 | PROTO_REGISTRAR_GET_NTH(hfinfo->parent, parent_hfinfo)if((hfinfo->parent == 0 || (unsigned)hfinfo->parent > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 8135 , __func__, "Unregistered hf! index=%d", hfinfo->parent); ( (void) ((hfinfo->parent > 0 && (unsigned)hfinfo ->parent < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 8135, "hfinfo->parent > 0 && (unsigned)hfinfo->parent < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> parent] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 8135, "gpa_hfinfo.hfi[hfinfo->parent] != ((void*)0)", "Unregistered hf!" )))) ; parent_hfinfo = gpa_hfinfo.hfi[hfinfo->parent];;
8136 |
8137 | /* Mark parent as indirectly referenced unless it is already directly
8138 | * referenced, i.e. the user has specified the parent in a filter.
8139 | */
8140 | if (parent_hfinfo->ref_type == HF_REF_TYPE_NONE)
8141 | parent_hfinfo->ref_type = HF_REF_TYPE_INDIRECT;
8142 | }
8143 | }
8144 |
8145 | proto_tree *
8146 | proto_item_add_subtree(proto_item *pi, const int idx) {
8147 | field_info *fi;
8148 |
8149 | if (!pi)
8150 | return NULL((void*)0);
8151 |
8152 | DISSECTOR_ASSERT(idx >= 0 && idx < num_tree_types)((void) ((idx >= 0 && idx < num_tree_types) ? ( void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 8152, "idx >= 0 && idx < num_tree_types" ))));
8153 |
8154 | fi = PITEM_FINFO(pi)((pi)->finfo);
8155 | if (!fi)
8156 | return (proto_tree *)pi;
8157 |
8158 | fi->tree_type = idx;
8159 |
8160 | return (proto_tree *)pi;
8161 | }
8162 |
8163 | proto_tree *
8164 | proto_item_get_subtree(proto_item *pi) {
8165 | field_info *fi;
8166 |
8167 | if (!pi)
8168 | return NULL((void*)0);
8169 | fi = PITEM_FINFO(pi)((pi)->finfo);
8170 | if ( (fi) && (fi->tree_type == -1) )
8171 | return NULL((void*)0);
8172 | return (proto_tree *)pi;
8173 | }
8174 |
8175 | proto_item *
8176 | proto_item_get_parent(const proto_item *ti) {
8177 | if (!ti)
8178 | return NULL((void*)0);
8179 | return ti->parent;
8180 | }
8181 |
8182 | proto_item *
8183 | proto_item_get_parent_nth(proto_item *ti, int gen) {
8184 | if (!ti)
8185 | return NULL((void*)0);
8186 | while (gen--) {
8187 | ti = ti->parent;
8188 | if (!ti)
8189 | return NULL((void*)0);
8190 | }
8191 | return ti;
8192 | }
8193 |
8194 |
8195 | proto_item *
8196 | proto_tree_get_parent(proto_tree *tree) {
8197 | if (!tree)
8198 | return NULL((void*)0);
8199 | return (proto_item *)tree;
8200 | }
8201 |
8202 | proto_tree *
8203 | proto_tree_get_parent_tree(proto_tree *tree) {
8204 | if (!tree)
8205 | return NULL((void*)0);
8206 |
8207 | /* we're the root tree, there's no parent
8208 | return ourselves so the caller has at least a tree to attach to */
8209 | if (!tree->parent)
8210 | return tree;
8211 |
8212 | return (proto_tree *)tree->parent;
8213 | }
8214 |
8215 | proto_tree *
8216 | proto_tree_get_root(proto_tree *tree) {
8217 | if (!tree)
8218 | return NULL((void*)0);
8219 | while (tree->parent) {
8220 | tree = tree->parent;
8221 | }
8222 | return tree;
8223 | }
8224 |
8225 | void
8226 | proto_tree_move_item(proto_tree *tree, proto_item *fixed_item,
8227 | proto_item *item_to_move)
8228 | {
8229 | /* This function doesn't generate any values. It only reorganizes the protocol tree
8230 | * so we can bail out immediately if it isn't visible. */
8231 | if (!tree || !PTREE_DATA(tree)((tree)->tree_data)->visible)
8232 | return;
8233 |
8234 | DISSECTOR_ASSERT(item_to_move->parent == tree)((void) ((item_to_move->parent == tree) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 8234, "item_to_move->parent == tree" ))));
8235 | DISSECTOR_ASSERT(fixed_item->parent == tree)((void) ((fixed_item->parent == tree) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 8235, "fixed_item->parent == tree" ))));
8236 |
8237 | /*** cut item_to_move out ***/
8238 |
8239 | /* is item_to_move the first? */
8240 | if (tree->first_child == item_to_move) {
8241 | /* simply change first child to next */
8242 | tree->first_child = item_to_move->next;
8243 |
8244 | DISSECTOR_ASSERT(tree->last_child != item_to_move)((void) ((tree->last_child != item_to_move) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 8244, "tree->last_child != item_to_move" ))));
8245 | } else {
8246 | proto_item *curr_item;
8247 | /* find previous and change it's next */
8248 | for (curr_item = tree->first_child; curr_item != NULL((void*)0); curr_item = curr_item->next) {
8249 | if (curr_item->next == item_to_move) {
8250 | break;
8251 | }
8252 | }
8253 |
8254 | DISSECTOR_ASSERT(curr_item)((void) ((curr_item) ? (void)0 : (proto_report_dissector_bug( "%s:%u: failed assertion \"%s\"", "epan/proto.c", 8254, "curr_item" ))));
8255 |
8256 | curr_item->next = item_to_move->next;
8257 |
8258 | /* fix last_child if required */
8259 | if (tree->last_child == item_to_move) {
8260 | tree->last_child = curr_item;
8261 | }
8262 | }
8263 |
8264 | /*** insert to_move after fixed ***/
8265 | item_to_move->next = fixed_item->next;
8266 | fixed_item->next = item_to_move;
8267 | if (tree->last_child == fixed_item) {
8268 | tree->last_child = item_to_move;
8269 | }
8270 | }
8271 |
8272 | void
8273 | proto_tree_set_appendix(proto_tree *tree, tvbuff_t *tvb, int start,
8274 | const int length)
8275 | {
8276 | field_info *fi;
8277 |
8278 | if (tree == NULL((void*)0))
8279 | return;
8280 |
8281 | fi = PTREE_FINFO(tree)((tree)->finfo);
8282 | if (fi == NULL((void*)0))
8283 | return;
8284 |
8285 | start += tvb_raw_offset(tvb);
8286 | DISSECTOR_ASSERT(start >= 0)((void) ((start >= 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 8286, "start >= 0" ))));
8287 | DISSECTOR_ASSERT(length >= 0)((void) ((length >= 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 8287, "length >= 0" ))));
8288 |
8289 | fi->appendix_start = start;
8290 | fi->appendix_length = length;
8291 | }
8292 |
8293 | static void
8294 | check_protocol_filter_name_or_fail(const char *filter_name)
8295 | {
8296 | /* Require at least two characters. */
8297 | if (filter_name[0] == '\0' || filter_name[1] == '\0') {
8298 | REPORT_DISSECTOR_BUG("Protocol filter name \"%s\" cannot have length less than two.", filter_name)proto_report_dissector_bug("Protocol filter name \"%s\" cannot have length less than two." , filter_name);
8299 | }
8300 |
8301 | if (proto_check_field_name(filter_name) != '\0') {
8302 | REPORT_DISSECTOR_BUG("Protocol filter name \"%s\" has one or more invalid characters."proto_report_dissector_bug("Protocol filter name \"%s\" has one or more invalid characters." " Allowed are letters, digits, '-', '_' and non-repeating '.'." " This might be caused by an inappropriate plugin or a development error." , filter_name)
8303 | " Allowed are letters, digits, '-', '_' and non-repeating '.'."proto_report_dissector_bug("Protocol filter name \"%s\" has one or more invalid characters." " Allowed are letters, digits, '-', '_' and non-repeating '.'." " This might be caused by an inappropriate plugin or a development error." , filter_name)
8304 | " This might be caused by an inappropriate plugin or a development error.", filter_name)proto_report_dissector_bug("Protocol filter name \"%s\" has one or more invalid characters." " Allowed are letters, digits, '-', '_' and non-repeating '.'." " This might be caused by an inappropriate plugin or a development error." , filter_name);
8305 | }
8306 |
8307 | /* Check that it doesn't match some very common numeric forms. */
8308 | if (filter_name[0] == '0' &&
8309 | (filter_name[1] == 'x' || filter_name[1] == 'X' ||
8310 | filter_name[1] == 'b' || filter_name[1] == 'B')) {
8311 | REPORT_DISSECTOR_BUG("Protocol filter name \"%s\" cannot start with \"%c%c\".",proto_report_dissector_bug("Protocol filter name \"%s\" cannot start with \"%c%c\"." , filter_name, filter_name[0], filter_name[1])
8312 | filter_name, filter_name[0], filter_name[1])proto_report_dissector_bug("Protocol filter name \"%s\" cannot start with \"%c%c\"." , filter_name, filter_name[0], filter_name[1]);
8313 | }
8314 |
8315 | /* Names starting with a digit must not contain a minus sign (currently not checked at runtime). */
8316 |
8317 | /* Check that it contains at least one letter. */
8318 | bool_Bool have_letter = false0;
8319 | for (const char *s = filter_name; *s != '\0'; s++) {
8320 | if (g_ascii_isalpha(*s)((g_ascii_table[(guchar) (*s)] & G_ASCII_ALPHA) != 0)) {
8321 | have_letter = true1;
8322 | break;
8323 | }
8324 | }
8325 | if (!have_letter) {
8326 | REPORT_DISSECTOR_BUG("Protocol filter name \"%s\" must contain at least one letter a-z.",proto_report_dissector_bug("Protocol filter name \"%s\" must contain at least one letter a-z." , filter_name)
8327 | filter_name)proto_report_dissector_bug("Protocol filter name \"%s\" must contain at least one letter a-z." , filter_name);
8328 | }
8329 |
8330 | /* Check for reserved keywords. */
8331 | if (g_hash_table_contains(proto_reserved_filter_names, filter_name)) {
8332 | REPORT_DISSECTOR_BUG("Protocol filter name \"%s\" is invalid because it is a reserved keyword."proto_report_dissector_bug("Protocol filter name \"%s\" is invalid because it is a reserved keyword." " This might be caused by an inappropriate plugin or a development error." , filter_name)
8333 | " This might be caused by an inappropriate plugin or a development error.", filter_name)proto_report_dissector_bug("Protocol filter name \"%s\" is invalid because it is a reserved keyword." " This might be caused by an inappropriate plugin or a development error." , filter_name);
8334 | }
8335 | }
8336 |
8337 | int
8338 | proto_register_protocol(const char *name, const char *short_name,
8339 | const char *filter_name)
8340 | {
8341 | protocol_t *protocol;
8342 | header_field_info *hfinfo;
8343 |
8344 | check_protocol_filter_name_or_fail(filter_name);
8345 |
8346 | /*
8347 | * Add this protocol to the list of known protocols;
8348 | * the list is sorted by protocol short name.
8349 | */
8350 | protocol = g_new(protocol_t, 1)((protocol_t *) g_malloc_n ((1), sizeof (protocol_t)));
8351 | protocol->name = name;
8352 | protocol->short_name = short_name;
8353 | protocol->filter_name = filter_name;
8354 | protocol->fields = NULL((void*)0); /* Delegate until actually needed */
8355 | protocol->is_enabled = true1; /* protocol is enabled by default */
8356 | protocol->enabled_by_default = true1; /* see previous comment */
8357 | protocol->can_toggle = true1;
8358 | protocol->parent_proto_id = -1;
8359 | protocol->heur_list = NULL((void*)0);
8360 |
8361 | /* List will be sorted later by name, when all protocols completed registering */
8362 | protocols = g_list_prepend(protocols, protocol);
8363 | /*
8364 | * Make sure there's not already a protocol with any of those
8365 | * names. Crash if there is, as that's an error in the code
8366 | * or an inappropriate plugin.
8367 | * This situation has to be fixed to not register more than one
8368 | * protocol with the same name.
8369 | */
8370 | if (!g_hash_table_insert(proto_names, (void *)name, protocol)) {
8371 | /* ws_error will terminate the program */
8372 | REPORT_DISSECTOR_BUG("Duplicate protocol name \"%s\"!"proto_report_dissector_bug("Duplicate protocol name \"%s\"!" " This might be caused by an inappropriate plugin or a development error." , name)
8373 | " This might be caused by an inappropriate plugin or a development error.", name)proto_report_dissector_bug("Duplicate protocol name \"%s\"!" " This might be caused by an inappropriate plugin or a development error." , name);
8374 | }
8375 | if (!g_hash_table_insert(proto_filter_names, (void *)filter_name, protocol)) {
8376 | REPORT_DISSECTOR_BUG("Duplicate protocol filter_name \"%s\"!"proto_report_dissector_bug("Duplicate protocol filter_name \"%s\"!" " This might be caused by an inappropriate plugin or a development error." , filter_name)
8377 | " This might be caused by an inappropriate plugin or a development error.", filter_name)proto_report_dissector_bug("Duplicate protocol filter_name \"%s\"!" " This might be caused by an inappropriate plugin or a development error." , filter_name);
8378 | }
8379 | if (!g_hash_table_insert(proto_short_names, (void *)short_name, protocol)) {
8380 | REPORT_DISSECTOR_BUG("Duplicate protocol short_name \"%s\"!"proto_report_dissector_bug("Duplicate protocol short_name \"%s\"!" " This might be caused by an inappropriate plugin or a development error." , short_name)
8381 | " This might be caused by an inappropriate plugin or a development error.", short_name)proto_report_dissector_bug("Duplicate protocol short_name \"%s\"!" " This might be caused by an inappropriate plugin or a development error." , short_name);
8382 | }
8383 |
8384 | /* Here we allocate a new header_field_info struct */
8385 | hfinfo = g_slice_new(header_field_info)((header_field_info*) g_slice_alloc (sizeof (header_field_info )));
8386 | hfinfo->name = name;
8387 | hfinfo->abbrev = filter_name;
8388 | hfinfo->type = FT_PROTOCOL;
8389 | hfinfo->display = BASE_NONE;
8390 | hfinfo->strings = protocol;
8391 | hfinfo->bitmask = 0;
8392 | hfinfo->ref_type = HF_REF_TYPE_NONE;
8393 | hfinfo->blurb = NULL((void*)0);
8394 | hfinfo->parent = -1; /* This field differentiates protos and fields */
8395 |
8396 | protocol->proto_id = proto_register_field_init(hfinfo, hfinfo->parent);
8397 | return protocol->proto_id;
8398 | }
8399 |
8400 | int
8401 | proto_register_protocol_in_name_only(const char *name, const char *short_name, const char *filter_name, int parent_proto, enum ftenum field_type)
8402 | {
8403 | protocol_t *protocol;
8404 | header_field_info *hfinfo;
8405 |
8406 | /*
8407 | * Helper protocols don't need the strict rules as a "regular" protocol
8408 | * Just register it in a list and make a hf_ field from it
8409 | */
8410 | if ((field_type != FT_PROTOCOL) && (field_type != FT_BYTES)) {
8411 | REPORT_DISSECTOR_BUG("Pino \"%s\" must be of type FT_PROTOCOL or FT_BYTES.", name)proto_report_dissector_bug("Pino \"%s\" must be of type FT_PROTOCOL or FT_BYTES." , name);
8412 | }
8413 |
8414 | if (parent_proto <= 0) {
8415 | REPORT_DISSECTOR_BUG("Must have a valid parent protocol for helper protocol \"%s\"!"proto_report_dissector_bug("Must have a valid parent protocol for helper protocol \"%s\"!" " This might be caused by an inappropriate plugin or a development error." , name)
8416 | " This might be caused by an inappropriate plugin or a development error.", name)proto_report_dissector_bug("Must have a valid parent protocol for helper protocol \"%s\"!" " This might be caused by an inappropriate plugin or a development error." , name);
8417 | }
8418 |
8419 | check_protocol_filter_name_or_fail(filter_name);
8420 |
8421 | /* Add this protocol to the list of helper protocols (just so it can be properly freed) */
8422 | protocol = g_new(protocol_t, 1)((protocol_t *) g_malloc_n ((1), sizeof (protocol_t)));
8423 | protocol->name = name;
8424 | protocol->short_name = short_name;
8425 | protocol->filter_name = filter_name;
8426 | protocol->fields = NULL((void*)0); /* Delegate until actually needed */
8427 |
8428 | /* Enabling and toggling is really determined by parent protocol,
8429 | but provide default values here */
8430 | protocol->is_enabled = true1;
8431 | protocol->enabled_by_default = true1;
8432 | protocol->can_toggle = true1;
8433 |
8434 | protocol->parent_proto_id = parent_proto;
8435 | protocol->heur_list = NULL((void*)0);
8436 |
8437 | /* List will be sorted later by name, when all protocols completed registering */
8438 | protocols = g_list_prepend(protocols, protocol);
8439 |
8440 | /* Here we allocate a new header_field_info struct */
8441 | hfinfo = g_slice_new(header_field_info)((header_field_info*) g_slice_alloc (sizeof (header_field_info )));
8442 | hfinfo->name = name;
8443 | hfinfo->abbrev = filter_name;
8444 | hfinfo->type = field_type;
8445 | hfinfo->display = BASE_NONE;
8446 | if (field_type == FT_BYTES) {
8447 | hfinfo->display |= (BASE_NO_DISPLAY_VALUE0x00002000|BASE_PROTOCOL_INFO0x00004000);
8448 | }
8449 | hfinfo->strings = protocol;
8450 | hfinfo->bitmask = 0;
8451 | hfinfo->ref_type = HF_REF_TYPE_NONE;
8452 | hfinfo->blurb = NULL((void*)0);
8453 | hfinfo->parent = -1; /* This field differentiates protos and fields */
8454 |
8455 | protocol->proto_id = proto_register_field_init(hfinfo, hfinfo->parent);
8456 | return protocol->proto_id;
8457 | }
8458 |
8459 | bool_Bool
8460 | proto_deregister_protocol(const char *short_name)
8461 | {
8462 | protocol_t *protocol;
8463 | header_field_info *hfinfo;
8464 | int proto_id;
8465 | unsigned i;
8466 |
8467 | proto_id = proto_get_id_by_short_name(short_name);
8468 | protocol = find_protocol_by_id(proto_id);
8469 | if (protocol == NULL((void*)0))
8470 | return false0;
8471 |
8472 | g_hash_table_remove(proto_names, protocol->name);
8473 | g_hash_table_remove(proto_short_names, (void *)short_name);
8474 | g_hash_table_remove(proto_filter_names, (void *)protocol->filter_name);
8475 |
8476 | if (protocol->fields) {
8477 | for (i = 0; i < protocol->fields->len; i++) {
8478 | hfinfo = (header_field_info *)g_ptr_array_index(protocol->fields, i)((protocol->fields)->pdata)[i];
8479 | hfinfo_remove_from_gpa_name_map(hfinfo);
8480 | expert_deregister_expertinfo(hfinfo->abbrev);
8481 | g_ptr_array_add(deregistered_fields, gpa_hfinfo.hfi[hfinfo->id]);
8482 | }
8483 | g_ptr_array_free(protocol->fields, true1);
8484 | protocol->fields = NULL((void*)0);
8485 | }
8486 |
8487 | g_list_free(protocol->heur_list);
8488 |
8489 | /* Remove this protocol from the list of known protocols */
8490 | protocols = g_list_remove(protocols, protocol);
8491 |
8492 | g_ptr_array_add(deregistered_fields, gpa_hfinfo.hfi[proto_id]);
8493 | wmem_map_remove(gpa_name_map, protocol->filter_name);
8494 |
8495 | g_free(last_field_name);
8496 | last_field_name = NULL((void*)0);
8497 |
8498 | return true1;
8499 | }
8500 |
8501 | void
8502 | proto_register_alias(const int proto_id, const char *alias_name)
8503 | {
8504 | protocol_t *protocol;
8505 |
8506 | protocol = find_protocol_by_id(proto_id);
8507 | if (alias_name && protocol) {
8508 | g_hash_table_insert(gpa_protocol_aliases, (void *) alias_name, (void *)protocol->filter_name);
8509 | }
8510 | }
8511 |
8512 | /*
8513 | * Routines to use to iterate over the protocols.
8514 | * The argument passed to the iterator routines is an opaque cookie to
8515 | * their callers; it's the GList pointer for the current element in
8516 | * the list.
8517 | * The ID of the protocol is returned, or -1 if there is no protocol.
8518 | */
8519 | int
8520 | proto_get_first_protocol(void **cookie)
8521 | {
8522 | protocol_t *protocol;
8523 |
8524 | if (protocols == NULL((void*)0))
8525 | return -1;
8526 | *cookie = protocols;
8527 | protocol = (protocol_t *)protocols->data;
8528 | return protocol->proto_id;
8529 | }
8530 |
8531 | int
8532 | proto_get_data_protocol(void *cookie)
8533 | {
8534 | GList *list_item = (GList *)cookie;
8535 |
8536 | protocol_t *protocol = (protocol_t *)list_item->data;
8537 | return protocol->proto_id;
8538 | }
8539 |
8540 | int
8541 | proto_get_next_protocol(void **cookie)
8542 | {
8543 | GList *list_item = (GList *)*cookie;
8544 | protocol_t *protocol;
8545 |
8546 | list_item = g_list_next(list_item)((list_item) ? (((GList *)(list_item))->next) : ((void*)0) );
8547 | if (list_item == NULL((void*)0))
8548 | return -1;
8549 | *cookie = list_item;
8550 | protocol = (protocol_t *)list_item->data;
8551 | return protocol->proto_id;
8552 | }
8553 |
8554 | header_field_info *
8555 | proto_get_first_protocol_field(const int proto_id, void **cookie)
8556 | {
8557 | protocol_t *protocol = find_protocol_by_id(proto_id);
8558 |
8559 | if ((protocol == NULL((void*)0)) || (protocol->fields == NULL((void*)0)) || (protocol->fields->len == 0))
8560 | return NULL((void*)0);
8561 |
8562 | *cookie = GUINT_TO_POINTER(0)((gpointer) (gulong) (0));
8563 | return (header_field_info *)g_ptr_array_index(protocol->fields, 0)((protocol->fields)->pdata)[0];
8564 | }
8565 |
8566 | header_field_info *
8567 | proto_get_next_protocol_field(const int proto_id, void **cookie)
8568 | {
8569 | protocol_t *protocol = find_protocol_by_id(proto_id);
8570 | unsigned i = GPOINTER_TO_UINT(*cookie)((guint) (gulong) (*cookie));
8571 |
8572 | i++;
8573 |
8574 | if ((protocol->fields == NULL((void*)0)) || (i >= protocol->fields->len))
8575 | return NULL((void*)0);
8576 |
8577 | *cookie = GUINT_TO_POINTER(i)((gpointer) (gulong) (i));
8578 | return (header_field_info *)g_ptr_array_index(protocol->fields, i)((protocol->fields)->pdata)[i];
8579 | }
8580 |
8581 | protocol_t *
8582 | find_protocol_by_id(const int proto_id)
8583 | {
8584 | header_field_info *hfinfo;
8585 |
8586 | if (proto_id <= 0)
8587 | return NULL((void*)0);
8588 |
8589 | PROTO_REGISTRAR_GET_NTH(proto_id, hfinfo)if((proto_id == 0 || (unsigned)proto_id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 8589, __func__, "Unregistered hf! index=%d" , proto_id); ((void) ((proto_id > 0 && (unsigned)proto_id < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 8589, "proto_id > 0 && (unsigned)proto_id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[proto_id] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 8589, "gpa_hfinfo.hfi[proto_id] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[proto_id];;
8590 | if (hfinfo->type != FT_PROTOCOL) {
8591 | DISSECTOR_ASSERT(hfinfo->display & BASE_PROTOCOL_INFO)((void) ((hfinfo->display & 0x00004000) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 8591, "hfinfo->display & 0x00004000" ))));
8592 | }
8593 | return (protocol_t *)hfinfo->strings;
8594 | }
8595 |
8596 | int
8597 | proto_get_id(const protocol_t *protocol)
8598 | {
8599 | return protocol->proto_id;
8600 | }
8601 |
8602 | bool_Bool
8603 | proto_name_already_registered(const char *name)
8604 | {
8605 | DISSECTOR_ASSERT_HINT(name, "No name present")((void) ((name) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 8605, "name", "No name present"))));
8606 |
8607 | if (g_hash_table_lookup(proto_names, name) != NULL((void*)0))
8608 | return true1;
8609 | return false0;
8610 | }
8611 |
8612 | int
8613 | proto_get_id_by_filter_name(const char *filter_name)
8614 | {
8615 | const protocol_t *protocol = NULL((void*)0);
8616 |
8617 | DISSECTOR_ASSERT_HINT(filter_name, "No filter name present")((void) ((filter_name) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 8617, "filter_name", "No filter name present"))));
8618 |
8619 | protocol = (const protocol_t *)g_hash_table_lookup(proto_filter_names, filter_name);
8620 |
8621 | if (protocol == NULL((void*)0))
8622 | return -1;
8623 | return protocol->proto_id;
8624 | }
8625 |
8626 | int
8627 | proto_get_id_by_short_name(const char *short_name)
8628 | {
8629 | const protocol_t *protocol = NULL((void*)0);
8630 |
8631 | DISSECTOR_ASSERT_HINT(short_name, "No short name present")((void) ((short_name) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 8631, "short_name", "No short name present"))));
8632 |
8633 | protocol = (const protocol_t *)g_hash_table_lookup(proto_short_names, short_name);
8634 |
8635 | if (protocol == NULL((void*)0))
8636 | return -1;
8637 | return protocol->proto_id;
8638 | }
8639 |
8640 | const char *
8641 | proto_get_protocol_name(const int proto_id)
8642 | {
8643 | protocol_t *protocol;
8644 |
8645 | protocol = find_protocol_by_id(proto_id);
8646 |
8647 | if (protocol == NULL((void*)0))
8648 | return NULL((void*)0);
8649 | return protocol->name;
8650 | }
8651 |
8652 | const char *
8653 | proto_get_protocol_short_name(const protocol_t *protocol)
8654 | {
8655 | if (protocol == NULL((void*)0))
8656 | return "(none)";
8657 | return protocol->short_name;
8658 | }
8659 |
8660 | const char *
8661 | proto_get_protocol_long_name(const protocol_t *protocol)
8662 | {
8663 | if (protocol == NULL((void*)0))
8664 | return "(none)";
8665 | return protocol->name;
8666 | }
8667 |
8668 | const char *
8669 | proto_get_protocol_filter_name(const int proto_id)
8670 | {
8671 | protocol_t *protocol;
8672 |
8673 | protocol = find_protocol_by_id(proto_id);
8674 | if (protocol == NULL((void*)0))
8675 | return "(none)";
8676 | return protocol->filter_name;
8677 | }
8678 |
8679 | void proto_add_heuristic_dissector(protocol_t *protocol, const char *short_name)
8680 | {
8681 | heur_dtbl_entry_t* heuristic_dissector;
8682 |
8683 | if (protocol == NULL((void*)0))
8684 | return;
8685 |
8686 | heuristic_dissector = find_heur_dissector_by_unique_short_name(short_name);
8687 | if (heuristic_dissector != NULL((void*)0))
8688 | {
8689 | protocol->heur_list = g_list_prepend (protocol->heur_list, heuristic_dissector);
8690 | }
8691 | }
8692 |
8693 | void proto_heuristic_dissector_foreach(const protocol_t *protocol, GFunc func, void *user_data)
8694 | {
8695 | if (protocol == NULL((void*)0))
8696 | return;
8697 |
8698 | g_list_foreach(protocol->heur_list, func, user_data);
8699 | }
8700 |
8701 | void
8702 | proto_get_frame_protocols(const wmem_list_t *layers, bool_Bool *is_ip,
8703 | bool_Bool *is_tcp, bool_Bool *is_udp,
8704 | bool_Bool *is_sctp, bool_Bool *is_tls,
8705 | bool_Bool *is_rtp,
8706 | bool_Bool *is_lte_rlc)
8707 | {
8708 | wmem_list_frame_t *protos = wmem_list_head(layers);
8709 | int proto_id;
8710 | const char *proto_name;
8711 |
8712 | /* Walk the list of a available protocols in the packet and
8713 | attempt to find "major" ones. */
8714 | /* It might make more sense to assemble and return a bitfield. */
8715 | while (protos != NULL((void*)0))
8716 | {
8717 | proto_id = GPOINTER_TO_INT(wmem_list_frame_data(protos))((gint) (glong) (wmem_list_frame_data(protos)));
8718 | proto_name = proto_get_protocol_filter_name(proto_id);
8719 |
8720 | if (is_ip && ((!strcmp(proto_name, "ip")) ||
8721 | (!strcmp(proto_name, "ipv6")))) {
8722 | *is_ip = true1;
8723 | } else if (is_tcp && !strcmp(proto_name, "tcp")) {
8724 | *is_tcp = true1;
8725 | } else if (is_udp && !strcmp(proto_name, "udp")) {
8726 | *is_udp = true1;
8727 | } else if (is_sctp && !strcmp(proto_name, "sctp")) {
8728 | *is_sctp = true1;
8729 | } else if (is_tls && !strcmp(proto_name, "tls")) {
8730 | *is_tls = true1;
8731 | } else if (is_rtp && !strcmp(proto_name, "rtp")) {
8732 | *is_rtp = true1;
8733 | } else if (is_lte_rlc && (!strcmp(proto_name, "rlc-lte") || !strcmp(proto_name, "rlc-nr"))) {
8734 | *is_lte_rlc = true1;
8735 | }
8736 |
8737 | protos = wmem_list_frame_next(protos);
8738 | }
8739 | }
8740 |
8741 | bool_Bool
8742 | proto_is_frame_protocol(const wmem_list_t *layers, const char* proto_name)
8743 | {
8744 | wmem_list_frame_t *protos = wmem_list_head(layers);
8745 | int proto_id;
8746 | const char *name;
8747 |
8748 | /* Walk the list of a available protocols in the packet and
8749 | attempt to find the specified protocol. */
8750 | while (protos != NULL((void*)0))
8751 | {
8752 | proto_id = GPOINTER_TO_INT(wmem_list_frame_data(protos))((gint) (glong) (wmem_list_frame_data(protos)));
8753 | name = proto_get_protocol_filter_name(proto_id);
8754 |
8755 | if (!strcmp(name, proto_name))
8756 | {
8757 | return true1;
8758 | }
8759 |
8760 | protos = wmem_list_frame_next(protos);
8761 | }
8762 |
8763 | return false0;
8764 | }
8765 |
8766 | char *
8767 | proto_list_layers(const packet_info *pinfo)
8768 | {
8769 | wmem_strbuf_t *buf;
8770 | wmem_list_frame_t *layers = wmem_list_head(pinfo->layers);
8771 |
8772 | buf = wmem_strbuf_new_sized(pinfo->pool, 128);
8773 |
8774 | /* Walk the list of layers in the packet and
8775 | return a string of all entries. */
8776 | while (layers != NULL((void*)0))
8777 | {
8778 | wmem_strbuf_append(buf, proto_get_protocol_filter_name(GPOINTER_TO_UINT(wmem_list_frame_data(layers))((guint) (gulong) (wmem_list_frame_data(layers)))));
8779 |
8780 | layers = wmem_list_frame_next(layers);
8781 | if (layers != NULL((void*)0)) {
8782 | wmem_strbuf_append_c(buf, ':');
8783 | }
8784 | }
8785 |
8786 | return wmem_strbuf_finalize(buf);
8787 | }
8788 |
8789 | uint8_t
8790 | proto_get_layer_num(const packet_info *pinfo, const int proto_id)
8791 | {
8792 | int *proto_layer_num_ptr;
8793 |
8794 | proto_layer_num_ptr = wmem_map_lookup(pinfo->proto_layers, GINT_TO_POINTER(proto_id)((gpointer) (glong) (proto_id)));
8795 | if (proto_layer_num_ptr == NULL((void*)0)) {
8796 | return 0;
8797 | }
8798 |
8799 | return (uint8_t)*proto_layer_num_ptr;
8800 | }
8801 |
8802 | bool_Bool
8803 | proto_is_pino(const protocol_t *protocol)
8804 | {
8805 | return (protocol->parent_proto_id != -1);
8806 | }
8807 |
8808 | bool_Bool
8809 | // NOLINTNEXTLINE(misc-no-recursion)
8810 | proto_is_protocol_enabled(const protocol_t *protocol)
8811 | {
8812 | if (protocol == NULL((void*)0))
8813 | return false0;
8814 |
8815 | //parent protocol determines enable/disable for helper dissectors
8816 | if (proto_is_pino(protocol))
8817 | return proto_is_protocol_enabled(find_protocol_by_id(protocol->parent_proto_id));
8818 |
8819 | return protocol->is_enabled;
8820 | }
8821 |
8822 | bool_Bool
8823 | // NOLINTNEXTLINE(misc-no-recursion)
8824 | proto_is_protocol_enabled_by_default(const protocol_t *protocol)
8825 | {
8826 | //parent protocol determines enable/disable for helper dissectors
8827 | if (proto_is_pino(protocol))
8828 | return proto_is_protocol_enabled_by_default(find_protocol_by_id(protocol->parent_proto_id));
8829 |
8830 | return protocol->enabled_by_default;
8831 | }
8832 |
8833 | bool_Bool
8834 | // NOLINTNEXTLINE(misc-no-recursion)
8835 | proto_can_toggle_protocol(const int proto_id)
8836 | {
8837 | protocol_t *protocol;
8838 |
8839 | protocol = find_protocol_by_id(proto_id);
8840 | //parent protocol determines toggling for helper dissectors
8841 | if (proto_is_pino(protocol))
8842 | return proto_can_toggle_protocol(protocol->parent_proto_id);
8843 |
8844 | return protocol->can_toggle;
8845 | }
8846 |
8847 | void
8848 | proto_disable_by_default(const int proto_id)
8849 | {
8850 | protocol_t *protocol;
8851 |
8852 | protocol = find_protocol_by_id(proto_id);
8853 | DISSECTOR_ASSERT(protocol->can_toggle)((void) ((protocol->can_toggle) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 8853, "protocol->can_toggle" ))));
8854 | DISSECTOR_ASSERT(proto_is_pino(protocol) == false)((void) ((proto_is_pino(protocol) == 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 8854, "proto_is_pino(protocol) == 0" ))));
8855 | protocol->is_enabled = false0;
8856 | protocol->enabled_by_default = false0;
8857 | }
8858 |
8859 | void
8860 | proto_set_decoding(const int proto_id, const bool_Bool enabled)
8861 | {
8862 | protocol_t *protocol;
8863 |
8864 | protocol = find_protocol_by_id(proto_id);
8865 | DISSECTOR_ASSERT(protocol->can_toggle)((void) ((protocol->can_toggle) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 8865, "protocol->can_toggle" ))));
8866 | DISSECTOR_ASSERT(proto_is_pino(protocol) == false)((void) ((proto_is_pino(protocol) == 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 8866, "proto_is_pino(protocol) == 0" ))));
8867 | protocol->is_enabled = enabled;
8868 | }
8869 |
8870 | void
8871 | proto_disable_all(void)
8872 | {
8873 | /* This doesn't explicitly disable heuristic protocols,
8874 | * but the heuristic doesn't get called if the parent
8875 | * protocol isn't enabled.
8876 | */
8877 | protocol_t *protocol;
8878 | GList *list_item = protocols;
8879 |
8880 | if (protocols == NULL((void*)0))
8881 | return;
8882 |
8883 | while (list_item) {
8884 | protocol = (protocol_t *)list_item->data;
8885 | if (protocol->can_toggle) {
8886 | protocol->is_enabled = false0;
8887 | }
8888 | list_item = g_list_next(list_item)((list_item) ? (((GList *)(list_item))->next) : ((void*)0) );
8889 | }
8890 | }
8891 |
8892 | static void
8893 | heur_reenable_cb(void *data, void *user_data _U___attribute__((unused)))
8894 | {
8895 | heur_dtbl_entry_t *heur = (heur_dtbl_entry_t*)data;
8896 |
8897 | heur->enabled = heur->enabled_by_default;
8898 | }
8899 |
8900 | void
8901 | proto_reenable_all(void)
8902 | {
8903 | protocol_t *protocol;
8904 | GList *list_item = protocols;
8905 |
8906 | if (protocols == NULL((void*)0))
8907 | return;
8908 |
8909 | while (list_item) {
8910 | protocol = (protocol_t *)list_item->data;
8911 | if (protocol->can_toggle)
8912 | protocol->is_enabled = protocol->enabled_by_default;
8913 | proto_heuristic_dissector_foreach(protocol, heur_reenable_cb, NULL((void*)0));
8914 | list_item = g_list_next(list_item)((list_item) ? (((GList *)(list_item))->next) : ((void*)0) );
8915 | }
8916 | }
8917 |
8918 | void
8919 | proto_set_cant_toggle(const int proto_id)
8920 | {
8921 | protocol_t *protocol;
8922 |
8923 | protocol = find_protocol_by_id(proto_id);
8924 | protocol->can_toggle = false0;
8925 | }
8926 |
8927 | static int
8928 | proto_register_field_common(protocol_t *proto, header_field_info *hfi, const int parent)
8929 | {
8930 | g_ptr_array_add(proto->fields, hfi);
8931 |
8932 | return proto_register_field_init(hfi, parent);
8933 | }
8934 |
8935 | /* for use with static arrays only, since we don't allocate our own copies
8936 | of the header_field_info struct contained within the hf_register_info struct */
8937 | void
8938 | proto_register_field_array(const int parent, hf_register_info *hf, const int num_records)
8939 | {
8940 | hf_register_info *ptr = hf;
8941 | protocol_t *proto;
8942 | int i;
8943 |
8944 | proto = find_protocol_by_id(parent);
8945 |
8946 | /* if (proto == NULL) - error or return? */
8947 |
8948 | if (proto->fields == NULL((void*)0)) {
8949 | /* Ironically, the NEW_PROTO_TREE_API was removed shortly before
8950 | * GLib introduced g_ptr_array_new_from_array, which might have
8951 | * given a reason to actually use it. (#17774)
8952 | */
8953 | proto->fields = g_ptr_array_sized_new(num_records);
8954 | }
8955 |
8956 | for (i = 0; i < num_records; i++, ptr++) {
8957 | /*
8958 | * Make sure we haven't registered this yet.
8959 | * Most fields have variables associated with them that
8960 | * are initialized to 0; some are initialized to -1 (which
8961 | * was the standard before 4.4).
8962 | *
8963 | * XXX - Since this is called almost 300000 times at startup,
8964 | * it might be nice to compare to only 0 and require
8965 | * dissectors to pass in zero for unregistered fields.
8966 | */
8967 | if (*ptr->p_id != -1 && *ptr->p_id != 0) {
8968 | REPORT_DISSECTOR_BUG(proto_report_dissector_bug("Duplicate field detected in call to proto_register_field_array: %s is already registered" , ptr->hfinfo.abbrev)
8969 | "Duplicate field detected in call to proto_register_field_array: %s is already registered",proto_report_dissector_bug("Duplicate field detected in call to proto_register_field_array: %s is already registered" , ptr->hfinfo.abbrev)
8970 | ptr->hfinfo.abbrev)proto_report_dissector_bug("Duplicate field detected in call to proto_register_field_array: %s is already registered" , ptr->hfinfo.abbrev);
8971 | return;
8972 | }
8973 |
8974 | *ptr->p_id = proto_register_field_common(proto, &ptr->hfinfo, parent);
8975 | }
8976 | }
8977 |
8978 | /* deregister already registered fields */
8979 | void
8980 | proto_deregister_field (const int parent, int hf_id)
8981 | {
8982 | header_field_info *hfi;
8983 | protocol_t *proto;
8984 | unsigned i;
8985 |
8986 | g_free(last_field_name);
8987 | last_field_name = NULL((void*)0);
8988 |
8989 | if (hf_id == -1 || hf_id == 0)
8990 | return;
8991 |
8992 | proto = find_protocol_by_id (parent);
8993 | if (!proto || proto->fields == NULL((void*)0)) {
8994 | return;
8995 | }
8996 |
8997 | for (i = 0; i < proto->fields->len; i++) {
8998 | hfi = (header_field_info *)g_ptr_array_index(proto->fields, i)((proto->fields)->pdata)[i];
8999 | if (hfi->id == hf_id) {
9000 | /* Found the hf_id in this protocol */
9001 | wmem_map_remove(gpa_name_map, hfi->abbrev);
9002 | g_ptr_array_remove_index_fast(proto->fields, i);
9003 | g_ptr_array_add(deregistered_fields, gpa_hfinfo.hfi[hf_id]);
9004 | return;
9005 | }
9006 | }
9007 | }
9008 |
9009 | /* Deregister all registered fields starting with a prefix. Use for dynamic registered fields only! */
9010 | void
9011 | proto_deregister_all_fields_with_prefix(const int parent, const char *prefix)
9012 | {
9013 | header_field_info *hfinfo;
9014 | protocol_t *proto;
9015 |
9016 | g_free(last_field_name);
9017 | last_field_name = NULL((void*)0);
9018 |
9019 | proto = find_protocol_by_id(parent);
9020 | if (proto && proto->fields && proto->fields->len > 0) {
9021 | unsigned i = proto->fields->len;
9022 | do {
9023 | i--;
9024 |
9025 | hfinfo = (header_field_info *)g_ptr_array_index(proto->fields, i)((proto->fields)->pdata)[i];
9026 | if (g_str_has_prefix(hfinfo->abbrev, prefix)(__builtin_constant_p (prefix)? __extension__ ({ const char * const __str = (hfinfo->abbrev); const char * const __prefix = (prefix); gboolean __result = (0); if (__str == ((void*)0) || __prefix == ((void*)0)) __result = (g_str_has_prefix) (__str , __prefix); else { const size_t __str_len = strlen (((__str) + !(__str))); const size_t __prefix_len = strlen (((__prefix ) + !(__prefix))); if (__str_len >= __prefix_len) __result = memcmp (((__str) + !(__str)), ((__prefix) + !(__prefix)), __prefix_len ) == 0; } __result; }) : (g_str_has_prefix) (hfinfo->abbrev , prefix) )) {
9027 | hfinfo_remove_from_gpa_name_map(hfinfo);
9028 | expert_deregister_expertinfo(hfinfo->abbrev);
9029 | g_ptr_array_add(deregistered_fields, gpa_hfinfo.hfi[hfinfo->id]);
9030 | g_ptr_array_remove_index_fast(proto->fields, i);
9031 | }
9032 | } while (i > 0);
9033 | }
9034 | }
9035 |
9036 | void
9037 | proto_add_deregistered_data (void *data)
9038 | {
9039 | g_ptr_array_add(deregistered_data, data);
9040 | }
9041 |
9042 | void
9043 | proto_add_deregistered_slice (size_t block_size, void *mem_block)
9044 | {
9045 | struct g_slice_data *slice_data = g_slice_new(struct g_slice_data)((struct g_slice_data*) g_slice_alloc (sizeof (struct g_slice_data )));
9046 |
9047 | slice_data->block_size = block_size;
9048 | slice_data->mem_block = mem_block;
9049 |
9050 | g_ptr_array_add(deregistered_slice, slice_data);
9051 | }
9052 |
9053 | void proto_free_field_strings (ftenum_t field_type, unsigned int field_display, const void *field_strings)
9054 | {
9055 | if (field_strings == NULL((void*)0)) {
9056 | return;
9057 | }
9058 |
9059 | switch (field_type) {
9060 | case FT_FRAMENUM:
9061 | /* This is just an integer represented as a pointer */
9062 | break;
9063 | case FT_PROTOCOL: {
9064 | protocol_t *protocol = (protocol_t *)field_strings;
9065 | g_free((char *)protocol->short_name);
9066 | break;
9067 | }
9068 | case FT_BOOLEAN: {
9069 | true_false_string *tf = (true_false_string *)field_strings;
9070 | g_free((char *)tf->true_string);
9071 | g_free((char *)tf->false_string);
9072 | break;
9073 | }
9074 | case FT_UINT40:
9075 | case FT_INT40:
9076 | case FT_UINT48:
9077 | case FT_INT48:
9078 | case FT_UINT56:
9079 | case FT_INT56:
9080 | case FT_UINT64:
9081 | case FT_INT64: {
9082 | if (field_display & BASE_UNIT_STRING0x00001000) {
9083 | unit_name_string *unit = (unit_name_string *)field_strings;
9084 | g_free((char *)unit->singular);
9085 | g_free((char *)unit->plural);
9086 | } else if (field_display & BASE_RANGE_STRING0x00000100) {
9087 | range_string *rs = (range_string *)field_strings;
9088 | while (rs->strptr) {
9089 | g_free((char *)rs->strptr);
9090 | rs++;
9091 | }
9092 | } else if (field_display & BASE_EXT_STRING0x00000200) {
9093 | val64_string_ext *vse = (val64_string_ext *)field_strings;
9094 | val64_string *vs = (val64_string *)vse->_vs_p;
9095 | while (vs->strptr) {
9096 | g_free((char *)vs->strptr);
9097 | vs++;
9098 | }
9099 | val64_string_ext_free(vse);
9100 | field_strings = NULL((void*)0);
9101 | } else if (field_display == BASE_CUSTOM) {
9102 | /* this will be a pointer to a function, don't free that */
9103 | field_strings = NULL((void*)0);
9104 | } else {
9105 | val64_string *vs64 = (val64_string *)field_strings;
9106 | while (vs64->strptr) {
9107 | g_free((char *)vs64->strptr);
9108 | vs64++;
9109 | }
9110 | }
9111 | break;
9112 | }
9113 | case FT_CHAR:
9114 | case FT_UINT8:
9115 | case FT_INT8:
9116 | case FT_UINT16:
9117 | case FT_INT16:
9118 | case FT_UINT24:
9119 | case FT_INT24:
9120 | case FT_UINT32:
9121 | case FT_INT32:
9122 | case FT_FLOAT:
9123 | case FT_DOUBLE: {
9124 | if (field_display & BASE_UNIT_STRING0x00001000) {
9125 | unit_name_string *unit = (unit_name_string *)field_strings;
9126 | g_free((char *)unit->singular);
9127 | g_free((char *)unit->plural);
9128 | } else if (field_display & BASE_RANGE_STRING0x00000100) {
9129 | range_string *rs = (range_string *)field_strings;
9130 | while (rs->strptr) {
9131 | g_free((char *)rs->strptr);
9132 | rs++;
9133 | }
9134 | } else if (field_display & BASE_EXT_STRING0x00000200) {
9135 | value_string_ext *vse = (value_string_ext *)field_strings;
9136 | value_string *vs = (value_string *)vse->_vs_p;
9137 | while (vs->strptr) {
9138 | g_free((char *)vs->strptr);
9139 | vs++;
9140 | }
9141 | value_string_ext_free(vse);
9142 | field_strings = NULL((void*)0);
9143 | } else if (field_display == BASE_CUSTOM) {
9144 | /* this will be a pointer to a function, don't free that */
9145 | field_strings = NULL((void*)0);
9146 | } else {
9147 | value_string *vs = (value_string *)field_strings;
9148 | while (vs->strptr) {
9149 | g_free((char *)vs->strptr);
9150 | vs++;
9151 | }
9152 | }
9153 | break;
9154 | default:
9155 | break;
9156 | }
9157 | }
9158 |
9159 | if (field_type != FT_FRAMENUM) {
9160 | g_free((void *)field_strings);
9161 | }
9162 | }
9163 |
9164 | static void
9165 | free_deregistered_field (void *data, void *user_data _U___attribute__((unused)))
9166 | {
9167 | header_field_info *hfi = (header_field_info *) data;
9168 | int hf_id = hfi->id;
9169 |
9170 | g_free((char *)hfi->name);
9171 | g_free((char *)hfi->abbrev);
9172 | g_free((char *)hfi->blurb);
9173 |
9174 | proto_free_field_strings(hfi->type, hfi->display, hfi->strings);
9175 |
9176 | if (hfi->parent == -1)
9177 | g_slice_free(header_field_info, hfi)do { if (1) g_slice_free1 (sizeof (header_field_info), (hfi)) ; else (void) ((header_field_info*) 0 == (hfi)); } while (0);
9178 |
9179 | gpa_hfinfo.hfi[hf_id] = NULL((void*)0); /* Invalidate this hf_id / proto_id */
9180 | }
9181 |
9182 | static void
9183 | free_deregistered_data (void *data, void *user_data _U___attribute__((unused)))
9184 | {
9185 | g_free (data);
9186 | }
9187 |
9188 | static void
9189 | free_deregistered_slice (void *data, void *user_data _U___attribute__((unused)))
9190 | {
9191 | struct g_slice_data *slice_data = (struct g_slice_data *)data;
9192 |
9193 | g_slice_free1(slice_data->block_size, slice_data->mem_block);
9194 | g_slice_free(struct g_slice_data, slice_data)do { if (1) g_slice_free1 (sizeof (struct g_slice_data), (slice_data )); else (void) ((struct g_slice_data*) 0 == (slice_data)); } while (0);
9195 | }
9196 |
9197 | /* free deregistered fields and data */
9198 | void
9199 | proto_free_deregistered_fields (void)
9200 | {
9201 | expert_free_deregistered_expertinfos();
9202 |
9203 | g_ptr_array_foreach(deregistered_fields, free_deregistered_field, NULL((void*)0));
9204 | g_ptr_array_free(deregistered_fields, true1);
9205 | deregistered_fields = g_ptr_array_new();
9206 |
9207 | g_ptr_array_foreach(deregistered_data, free_deregistered_data, NULL((void*)0));
9208 | g_ptr_array_free(deregistered_data, true1);
9209 | deregistered_data = g_ptr_array_new();
9210 |
9211 | g_ptr_array_foreach(deregistered_slice, free_deregistered_slice, NULL((void*)0));
9212 | g_ptr_array_free(deregistered_slice, true1);
9213 | deregistered_slice = g_ptr_array_new();
9214 | }
9215 |
9216 | static const value_string hf_display[] = {
9217 | { BASE_NONE, "BASE_NONE" },
9218 | { BASE_DEC, "BASE_DEC" },
9219 | { BASE_HEX, "BASE_HEX" },
9220 | { BASE_OCT, "BASE_OCT" },
9221 | { BASE_DEC_HEX, "BASE_DEC_HEX" },
9222 | { BASE_HEX_DEC, "BASE_HEX_DEC" },
9223 | { BASE_CUSTOM, "BASE_CUSTOM" },
9224 | { BASE_NONE|BASE_RANGE_STRING0x00000100, "BASE_NONE|BASE_RANGE_STRING" },
9225 | { BASE_DEC|BASE_RANGE_STRING0x00000100, "BASE_DEC|BASE_RANGE_STRING" },
9226 | { BASE_HEX|BASE_RANGE_STRING0x00000100, "BASE_HEX|BASE_RANGE_STRING" },
9227 | { BASE_OCT|BASE_RANGE_STRING0x00000100, "BASE_OCT|BASE_RANGE_STRING" },
9228 | { BASE_DEC_HEX|BASE_RANGE_STRING0x00000100, "BASE_DEC_HEX|BASE_RANGE_STRING" },
9229 | { BASE_HEX_DEC|BASE_RANGE_STRING0x00000100, "BASE_HEX_DEC|BASE_RANGE_STRING" },
9230 | { BASE_CUSTOM|BASE_RANGE_STRING0x00000100, "BASE_CUSTOM|BASE_RANGE_STRING" },
9231 | { BASE_NONE|BASE_VAL64_STRING0x00000400, "BASE_NONE|BASE_VAL64_STRING" },
9232 | { BASE_DEC|BASE_VAL64_STRING0x00000400, "BASE_DEC|BASE_VAL64_STRING" },
9233 | { BASE_HEX|BASE_VAL64_STRING0x00000400, "BASE_HEX|BASE_VAL64_STRING" },
9234 | { BASE_OCT|BASE_VAL64_STRING0x00000400, "BASE_OCT|BASE_VAL64_STRING" },
9235 | { BASE_DEC_HEX|BASE_VAL64_STRING0x00000400, "BASE_DEC_HEX|BASE_VAL64_STRING" },
9236 | { BASE_HEX_DEC|BASE_VAL64_STRING0x00000400, "BASE_HEX_DEC|BASE_VAL64_STRING" },
9237 | { BASE_CUSTOM|BASE_VAL64_STRING0x00000400, "BASE_CUSTOM|BASE_VAL64_STRING" },
9238 | { ABSOLUTE_TIME_LOCAL, "ABSOLUTE_TIME_LOCAL" },
9239 | { ABSOLUTE_TIME_UTC, "ABSOLUTE_TIME_UTC" },
9240 | { ABSOLUTE_TIME_DOY_UTC, "ABSOLUTE_TIME_DOY_UTC" },
9241 | { BASE_PT_UDP, "BASE_PT_UDP" },
9242 | { BASE_PT_TCP, "BASE_PT_TCP" },
9243 | { BASE_PT_DCCP, "BASE_PT_DCCP" },
9244 | { BASE_PT_SCTP, "BASE_PT_SCTP" },
9245 | { BASE_OUI, "BASE_OUI" },
9246 | { 0, NULL((void*)0) } };
9247 |
9248 | const char* proto_field_display_to_string(int field_display)
9249 | {
9250 | return val_to_str_const(field_display, hf_display, "Unknown");
9251 | }
9252 |
9253 | static inline port_type
9254 | display_to_port_type(field_display_e e)
9255 | {
9256 | switch (e) {
9257 | case BASE_PT_UDP:
9258 | return PT_UDP;
9259 | case BASE_PT_TCP:
9260 | return PT_TCP;
9261 | case BASE_PT_DCCP:
9262 | return PT_DCCP;
9263 | case BASE_PT_SCTP:
9264 | return PT_SCTP;
9265 | default:
9266 | break;
9267 | }
9268 | return PT_NONE;
9269 | }
9270 |
9271 | /* temporary function containing assert part for easier profiling */
9272 | static void
9273 | tmp_fld_check_assert(header_field_info *hfinfo)
9274 | {
9275 | char* tmp_str;
9276 |
9277 | /* The field must have a name (with length > 0) */
9278 | if (!hfinfo->name || !hfinfo->name[0]) {
9279 | if (hfinfo->abbrev)
9280 | /* Try to identify the field */
9281 | REPORT_DISSECTOR_BUG("Field (abbrev='%s') does not have a name",proto_report_dissector_bug("Field (abbrev='%s') does not have a name" , hfinfo->abbrev)
9282 | hfinfo->abbrev)proto_report_dissector_bug("Field (abbrev='%s') does not have a name" , hfinfo->abbrev);
9283 | else
9284 | /* Hum, no luck */
9285 | REPORT_DISSECTOR_BUG("Field does not have a name (nor an abbreviation)")proto_report_dissector_bug("Field does not have a name (nor an abbreviation)" );
9286 | }
9287 |
9288 | /* fields with an empty string for an abbreviation aren't filterable */
9289 | if (!hfinfo->abbrev || !hfinfo->abbrev[0])
9290 | REPORT_DISSECTOR_BUG("Field '%s' does not have an abbreviation", hfinfo->name)proto_report_dissector_bug("Field '%s' does not have an abbreviation" , hfinfo->name);
9291 |
9292 | /* TODO: This check is a significant percentage of startup time (~10%),
9293 | although not nearly as slow as what's enabled by ENABLE_CHECK_FILTER.
9294 | It might be nice to have a way to disable this check when, e.g.,
9295 | running TShark many times with the same configuration. */
9296 | /* Check that the filter name (abbreviation) is legal;
9297 | * it must contain only alphanumerics, '-', "_", and ".". */
9298 | unsigned char c;
9299 | c = module_check_valid_name(hfinfo->abbrev, false0);
9300 | if (c) {
9301 | if (c == '.') {
9302 | REPORT_DISSECTOR_BUG("Invalid leading, duplicated or trailing '.' found in filter name '%s'", hfinfo->abbrev)proto_report_dissector_bug("Invalid leading, duplicated or trailing '.' found in filter name '%s'" , hfinfo->abbrev);
9303 | } else if (g_ascii_isprint(c)((g_ascii_table[(guchar) (c)] & G_ASCII_PRINT) != 0)) {
9304 | REPORT_DISSECTOR_BUG("Invalid character '%c' in filter name '%s'", c, hfinfo->abbrev)proto_report_dissector_bug("Invalid character '%c' in filter name '%s'" , c, hfinfo->abbrev);
9305 | } else {
9306 | REPORT_DISSECTOR_BUG("Invalid byte \\%03o in filter name '%s'", c, hfinfo->abbrev)proto_report_dissector_bug("Invalid byte \\%03o in filter name '%s'" , c, hfinfo->abbrev);
9307 | }
9308 | }
9309 |
9310 | /* These types of fields are allowed to have value_strings,
9311 | * true_false_strings or a protocol_t struct
9312 | */
9313 | if (hfinfo->strings != NULL((void*)0) && FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF) != BASE_CUSTOM) {
9314 | switch (hfinfo->type) {
9315 |
9316 | /*
9317 | * These types are allowed to support display value_strings,
9318 | * value64_strings, the extended versions of the previous
9319 | * two, range strings, or unit strings.
9320 | */
9321 | case FT_CHAR:
9322 | case FT_UINT8:
9323 | case FT_UINT16:
9324 | case FT_UINT24:
9325 | case FT_UINT32:
9326 | case FT_UINT40:
9327 | case FT_UINT48:
9328 | case FT_UINT56:
9329 | case FT_UINT64:
9330 | case FT_INT8:
9331 | case FT_INT16:
9332 | case FT_INT24:
9333 | case FT_INT32:
9334 | case FT_INT40:
9335 | case FT_INT48:
9336 | case FT_INT56:
9337 | case FT_INT64:
9338 | case FT_BOOLEAN:
9339 | case FT_PROTOCOL:
9340 | break;
9341 |
9342 | /*
9343 | * This is allowed to have a value of type
9344 | * enum ft_framenum_type to indicate what relationship
9345 | * the frame in question has to the frame in which
9346 | * the field is put.
9347 | */
9348 | case FT_FRAMENUM:
9349 | break;
9350 |
9351 | /*
9352 | * These types are allowed to support only unit strings.
9353 | */
9354 | case FT_FLOAT:
9355 | case FT_DOUBLE:
9356 | case FT_IEEE_11073_SFLOAT:
9357 | case FT_IEEE_11073_FLOAT:
9358 | if (!(hfinfo->display & BASE_UNIT_STRING0x00001000)) {
9359 | REPORT_DISSECTOR_BUG("Field '%s' (%s) has a non-unit-strings 'strings' value but is of type %s"proto_report_dissector_bug("Field '%s' (%s) has a non-unit-strings 'strings' value but is of type %s" " (which is only allowed to have unit strings)", hfinfo-> name, hfinfo->abbrev, ftype_name(hfinfo->type))
9360 | " (which is only allowed to have unit strings)",proto_report_dissector_bug("Field '%s' (%s) has a non-unit-strings 'strings' value but is of type %s" " (which is only allowed to have unit strings)", hfinfo-> name, hfinfo->abbrev, ftype_name(hfinfo->type))
9361 | hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) has a non-unit-strings 'strings' value but is of type %s" " (which is only allowed to have unit strings)", hfinfo-> name, hfinfo->abbrev, ftype_name(hfinfo->type));
9362 | }
9363 | break;
9364 |
9365 | /*
9366 | * These types are allowed to support display
9367 | * time_value_strings.
9368 | */
9369 | case FT_ABSOLUTE_TIME:
9370 | if (hfinfo->display & BASE_RANGE_STRING0x00000100 ||
9371 | hfinfo->display & BASE_EXT_STRING0x00000200 ||
9372 | hfinfo->display & BASE_VAL64_STRING0x00000400 ||
9373 | hfinfo->display & BASE_UNIT_STRING0x00001000) {
9374 | REPORT_DISSECTOR_BUG("Field '%s' (%s) has a non-time-value-strings 'strings' value but is of type %s"proto_report_dissector_bug("Field '%s' (%s) has a non-time-value-strings 'strings' value but is of type %s" " (which is only allowed to have time-value strings)", hfinfo ->name, hfinfo->abbrev, ftype_name(hfinfo->type))
9375 | " (which is only allowed to have time-value strings)",proto_report_dissector_bug("Field '%s' (%s) has a non-time-value-strings 'strings' value but is of type %s" " (which is only allowed to have time-value strings)", hfinfo ->name, hfinfo->abbrev, ftype_name(hfinfo->type))
9376 | hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) has a non-time-value-strings 'strings' value but is of type %s" " (which is only allowed to have time-value strings)", hfinfo ->name, hfinfo->abbrev, ftype_name(hfinfo->type));
9377 | }
9378 | break;
9379 |
9380 | /*
9381 | * This type is only allowed to support a string if it's
9382 | * a protocol (for pinos).
9383 | */
9384 | case FT_BYTES:
9385 | if (!(hfinfo->display & BASE_PROTOCOL_INFO0x00004000)) {
9386 | REPORT_DISSECTOR_BUG("Field '%s' (%s) has a non-protocol-info 'strings' value but is of type %s"proto_report_dissector_bug("Field '%s' (%s) has a non-protocol-info 'strings' value but is of type %s" " (which is only allowed to have protocol-info strings)", hfinfo ->name, hfinfo->abbrev, ftype_name(hfinfo->type))
9387 | " (which is only allowed to have protocol-info strings)",proto_report_dissector_bug("Field '%s' (%s) has a non-protocol-info 'strings' value but is of type %s" " (which is only allowed to have protocol-info strings)", hfinfo ->name, hfinfo->abbrev, ftype_name(hfinfo->type))
9388 | hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) has a non-protocol-info 'strings' value but is of type %s" " (which is only allowed to have protocol-info strings)", hfinfo ->name, hfinfo->abbrev, ftype_name(hfinfo->type));
9389 | }
9390 | break;
9391 |
9392 | default:
9393 | REPORT_DISSECTOR_BUG("Field '%s' (%s) has a 'strings' value but is of type %s"proto_report_dissector_bug("Field '%s' (%s) has a 'strings' value but is of type %s" " (which is not allowed to have strings)", hfinfo->name, hfinfo ->abbrev, ftype_name(hfinfo->type))
9394 | " (which is not allowed to have strings)",proto_report_dissector_bug("Field '%s' (%s) has a 'strings' value but is of type %s" " (which is not allowed to have strings)", hfinfo->name, hfinfo ->abbrev, ftype_name(hfinfo->type))
9395 | hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) has a 'strings' value but is of type %s" " (which is not allowed to have strings)", hfinfo->name, hfinfo ->abbrev, ftype_name(hfinfo->type));
9396 | }
9397 | }
9398 |
9399 | /* TODO: This check may slow down startup, and output quite a few warnings.
9400 | It would be good to be able to enable this (and possibly other checks?)
9401 | in non-release builds. */
9402 | #ifdef ENABLE_CHECK_FILTER
9403 | /* Check for duplicate value_string values.
9404 | There are lots that have the same value *and* string, so for now only
9405 | report those that have same value but different string. */
9406 | if ((hfinfo->strings != NULL((void*)0)) &&
9407 | !(hfinfo->display & BASE_RANGE_STRING0x00000100) &&
9408 | !(hfinfo->display & BASE_UNIT_STRING0x00001000) &&
9409 | !((hfinfo->display & FIELD_DISPLAY_E_MASK0xFF) == BASE_CUSTOM) &&
9410 | (
9411 | (hfinfo->type == FT_CHAR) ||
9412 | (hfinfo->type == FT_UINT8) ||
9413 | (hfinfo->type == FT_UINT16) ||
9414 | (hfinfo->type == FT_UINT24) ||
9415 | (hfinfo->type == FT_UINT32) ||
9416 | (hfinfo->type == FT_INT8) ||
9417 | (hfinfo->type == FT_INT16) ||
9418 | (hfinfo->type == FT_INT24) ||
9419 | (hfinfo->type == FT_INT32) )) {
9420 |
9421 | if (hfinfo->display & BASE_EXT_STRING0x00000200) {
9422 | if (hfinfo->display & BASE_VAL64_STRING0x00000400) {
9423 | const val64_string *start_values = VAL64_STRING_EXT_VS_P((const val64_string_ext*)hfinfo->strings)((const val64_string_ext*)hfinfo->strings)->_vs_p;
9424 | CHECK_HF_VALUE(val64_string, PRIu64"l" "u", start_values);
9425 | } else {
9426 | const value_string *start_values = VALUE_STRING_EXT_VS_P((const value_string_ext*)hfinfo->strings)((const value_string_ext*)hfinfo->strings)->_vs_p;
9427 | CHECK_HF_VALUE(value_string, "u", start_values);
9428 | }
9429 | } else {
9430 | const value_string *start_values = (const value_string*)hfinfo->strings;
9431 | CHECK_HF_VALUE(value_string, "u", start_values);
9432 | }
9433 | }
9434 |
9435 | if (hfinfo->type == FT_BOOLEAN) {
9436 | const true_false_string *tfs = (const true_false_string*)hfinfo->strings;
9437 | if (tfs) {
9438 | if (strcmp(tfs->false_string, tfs->true_string) == 0) {
9439 | ws_error("Field '%s' (%s) has identical true and false strings (\"%s\", \"%s\")",ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 9441 , __func__, "Field '%s' (%s) has identical true and false strings (\"%s\", \"%s\")" , hfinfo->name, hfinfo->abbrev, tfs->false_string, tfs ->true_string)
9440 | hfinfo->name, hfinfo->abbrev,ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 9441 , __func__, "Field '%s' (%s) has identical true and false strings (\"%s\", \"%s\")" , hfinfo->name, hfinfo->abbrev, tfs->false_string, tfs ->true_string)
9441 | tfs->false_string, tfs->true_string)ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 9441 , __func__, "Field '%s' (%s) has identical true and false strings (\"%s\", \"%s\")" , hfinfo->name, hfinfo->abbrev, tfs->false_string, tfs ->true_string);
9442 | }
9443 | }
9444 | }
9445 |
9446 | if (hfinfo->display & BASE_RANGE_STRING0x00000100) {
9447 | const range_string *rs = (const range_string*)(hfinfo->strings);
9448 | if (rs) {
9449 | const range_string *this_it = rs;
9450 |
9451 | do {
9452 | if (this_it->value_max < this_it->value_min) {
9453 | ws_warning("value_range_string error: %s (%s) entry for \"%s\" - max(%"PRIu64" 0x%"PRIx64") is less than min(%"PRIu64" 0x%"PRIx64")",do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 9457, __func__, "value_range_string error: %s (%s) entry for \"%s\" - max(%" "l" "u"" 0x%""l" "x"") is less than min(%""l" "u"" 0x%""l" "x" ")", hfinfo->name, hfinfo->abbrev, this_it->strptr, this_it ->value_max, this_it->value_max, this_it->value_min, this_it->value_min); } } while (0)
9454 | hfinfo->name, hfinfo->abbrev,do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 9457, __func__, "value_range_string error: %s (%s) entry for \"%s\" - max(%" "l" "u"" 0x%""l" "x"") is less than min(%""l" "u"" 0x%""l" "x" ")", hfinfo->name, hfinfo->abbrev, this_it->strptr, this_it ->value_max, this_it->value_max, this_it->value_min, this_it->value_min); } } while (0)
9455 | this_it->strptr,do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 9457, __func__, "value_range_string error: %s (%s) entry for \"%s\" - max(%" "l" "u"" 0x%""l" "x"") is less than min(%""l" "u"" 0x%""l" "x" ")", hfinfo->name, hfinfo->abbrev, this_it->strptr, this_it ->value_max, this_it->value_max, this_it->value_min, this_it->value_min); } } while (0)
9456 | this_it->value_max, this_it->value_max,do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 9457, __func__, "value_range_string error: %s (%s) entry for \"%s\" - max(%" "l" "u"" 0x%""l" "x"") is less than min(%""l" "u"" 0x%""l" "x" ")", hfinfo->name, hfinfo->abbrev, this_it->strptr, this_it ->value_max, this_it->value_max, this_it->value_min, this_it->value_min); } } while (0)
9457 | this_it->value_min, this_it->value_min)do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 9457, __func__, "value_range_string error: %s (%s) entry for \"%s\" - max(%" "l" "u"" 0x%""l" "x"") is less than min(%""l" "u"" 0x%""l" "x" ")", hfinfo->name, hfinfo->abbrev, this_it->strptr, this_it ->value_max, this_it->value_max, this_it->value_min, this_it->value_min); } } while (0);
9458 | ++this_it;
9459 | continue;
9460 | }
9461 |
9462 | for (const range_string *prev_it=rs; prev_it < this_it; ++prev_it) {
9463 | /* Not OK if this one is completely hidden by an earlier one! */
9464 | if ((prev_it->value_min <= this_it->value_min) && (prev_it->value_max >= this_it->value_max)) {
9465 | ws_warning("value_range_string error: %s (%s) hidden by earlier entry "do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 9471, __func__, "value_range_string error: %s (%s) hidden by earlier entry " "(prev=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%" "l" "x"") (this=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%""l" "x"")", hfinfo->name, hfinfo->abbrev, prev_it ->strptr, prev_it->value_min, prev_it->value_min, prev_it ->value_max, prev_it->value_max, this_it->strptr, this_it ->value_min, this_it->value_min, this_it->value_max, this_it->value_max); } } while (0)
9466 | "(prev=\"%s\": %"PRIu64" 0x%"PRIx64" -> %"PRIu64" 0x%"PRIx64") (this=\"%s\": %"PRIu64" 0x%"PRIx64" -> %"PRIu64" 0x%"PRIx64")",do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 9471, __func__, "value_range_string error: %s (%s) hidden by earlier entry " "(prev=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%" "l" "x"") (this=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%""l" "x"")", hfinfo->name, hfinfo->abbrev, prev_it ->strptr, prev_it->value_min, prev_it->value_min, prev_it ->value_max, prev_it->value_max, this_it->strptr, this_it ->value_min, this_it->value_min, this_it->value_max, this_it->value_max); } } while (0)
9467 | hfinfo->name, hfinfo->abbrev,do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 9471, __func__, "value_range_string error: %s (%s) hidden by earlier entry " "(prev=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%" "l" "x"") (this=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%""l" "x"")", hfinfo->name, hfinfo->abbrev, prev_it ->strptr, prev_it->value_min, prev_it->value_min, prev_it ->value_max, prev_it->value_max, this_it->strptr, this_it ->value_min, this_it->value_min, this_it->value_max, this_it->value_max); } } while (0)
9468 | prev_it->strptr, prev_it->value_min, prev_it->value_min,do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 9471, __func__, "value_range_string error: %s (%s) hidden by earlier entry " "(prev=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%" "l" "x"") (this=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%""l" "x"")", hfinfo->name, hfinfo->abbrev, prev_it ->strptr, prev_it->value_min, prev_it->value_min, prev_it ->value_max, prev_it->value_max, this_it->strptr, this_it ->value_min, this_it->value_min, this_it->value_max, this_it->value_max); } } while (0)
9469 | prev_it->value_max, prev_it->value_max,do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 9471, __func__, "value_range_string error: %s (%s) hidden by earlier entry " "(prev=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%" "l" "x"") (this=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%""l" "x"")", hfinfo->name, hfinfo->abbrev, prev_it ->strptr, prev_it->value_min, prev_it->value_min, prev_it ->value_max, prev_it->value_max, this_it->strptr, this_it ->value_min, this_it->value_min, this_it->value_max, this_it->value_max); } } while (0)
9470 | this_it->strptr, this_it->value_min, this_it->value_min,do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 9471, __func__, "value_range_string error: %s (%s) hidden by earlier entry " "(prev=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%" "l" "x"") (this=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%""l" "x"")", hfinfo->name, hfinfo->abbrev, prev_it ->strptr, prev_it->value_min, prev_it->value_min, prev_it ->value_max, prev_it->value_max, this_it->strptr, this_it ->value_min, this_it->value_min, this_it->value_max, this_it->value_max); } } while (0)
9471 | this_it->value_max, this_it->value_max)do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 9471, __func__, "value_range_string error: %s (%s) hidden by earlier entry " "(prev=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%" "l" "x"") (this=\"%s\": %""l" "u"" 0x%""l" "x"" -> %""l" "u"" 0x%""l" "x"")", hfinfo->name, hfinfo->abbrev, prev_it ->strptr, prev_it->value_min, prev_it->value_min, prev_it ->value_max, prev_it->value_max, this_it->strptr, this_it ->value_min, this_it->value_min, this_it->value_max, this_it->value_max); } } while (0);
9472 | }
9473 | }
9474 | ++this_it;
9475 | } while (this_it->strptr);
9476 | }
9477 | }
9478 | #endif
9479 |
9480 | switch (hfinfo->type) {
9481 |
9482 | case FT_CHAR:
9483 | /* Require the char type to have BASE_HEX, BASE_OCT,
9484 | * BASE_CUSTOM, or BASE_NONE as its base.
9485 | *
9486 | * If the display value is BASE_NONE and there is a
9487 | * strings conversion then the dissector writer is
9488 | * telling us that the field's numerical value is
9489 | * meaningless; we'll avoid showing the value to the
9490 | * user.
9491 | */
9492 | switch (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF)) {
9493 | case BASE_HEX:
9494 | case BASE_OCT:
9495 | case BASE_CUSTOM: /* hfinfo_numeric_value_format() treats this as decimal */
9496 | break;
9497 | case BASE_NONE:
9498 | if (hfinfo->strings == NULL((void*)0))
9499 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an integral value (%s)"proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as BASE_NONE but" " without a strings conversion" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9500 | " but is being displayed as BASE_NONE but"proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as BASE_NONE but" " without a strings conversion" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9501 | " without a strings conversion",proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as BASE_NONE but" " without a strings conversion" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9502 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as BASE_NONE but" " without a strings conversion" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9503 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as BASE_NONE but" " without a strings conversion" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9504 | break;
9505 | default:
9506 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Unknown: 0x%x)");
9507 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is a character value (%s)"proto_report_dissector_bug("Field '%s' (%s) is a character value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9508 | " but is being displayed as %s",proto_report_dissector_bug("Field '%s' (%s) is a character value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9509 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is a character value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9510 | ftype_name(hfinfo->type), tmp_str)proto_report_dissector_bug("Field '%s' (%s) is a character value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str);
9511 | //wmem_free(NULL, tmp_str);
9512 | }
9513 | if (hfinfo->display & BASE_UNIT_STRING0x00001000) {
9514 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is a character value (%s) but has a unit string",proto_report_dissector_bug("Field '%s' (%s) is a character value (%s) but has a unit string" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9515 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is a character value (%s) but has a unit string" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9516 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is a character value (%s) but has a unit string" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9517 | }
9518 | break;
9519 | case FT_INT8:
9520 | case FT_INT16:
9521 | case FT_INT24:
9522 | case FT_INT32:
9523 | case FT_INT40:
9524 | case FT_INT48:
9525 | case FT_INT56:
9526 | case FT_INT64:
9527 | /* Hexadecimal and octal are, in printf() and everywhere
9528 | * else, unsigned so don't allow dissectors to register a
9529 | * signed field to be displayed unsigned. (Else how would
9530 | * we display negative values?)
9531 | */
9532 | switch (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF)) {
9533 | case BASE_HEX:
9534 | case BASE_OCT:
9535 | case BASE_DEC_HEX:
9536 | case BASE_HEX_DEC:
9537 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Bit count: %d)");
9538 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is signed (%s) but is being displayed unsigned (%s)",proto_report_dissector_bug("Field '%s' (%s) is signed (%s) but is being displayed unsigned (%s)" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9539 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is signed (%s) but is being displayed unsigned (%s)" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9540 | ftype_name(hfinfo->type), tmp_str)proto_report_dissector_bug("Field '%s' (%s) is signed (%s) but is being displayed unsigned (%s)" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str);
9541 | //wmem_free(NULL, tmp_str);
9542 | }
9543 | /* FALL THROUGH */
9544 | case FT_UINT8:
9545 | case FT_UINT16:
9546 | case FT_UINT24:
9547 | case FT_UINT32:
9548 | case FT_UINT40:
9549 | case FT_UINT48:
9550 | case FT_UINT56:
9551 | case FT_UINT64:
9552 | if (IS_BASE_PORT(hfinfo->display)(((hfinfo->display)==BASE_PT_UDP||(hfinfo->display)==BASE_PT_TCP ||(hfinfo->display)==BASE_PT_DCCP||(hfinfo->display)==BASE_PT_SCTP ))) {
9553 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Unknown: 0x%x)");
9554 | if (hfinfo->type != FT_UINT16) {
9555 | REPORT_DISSECTOR_BUG("Field '%s' (%s) has 'display' value %s but it can only be used with FT_UINT16, not %s",proto_report_dissector_bug("Field '%s' (%s) has 'display' value %s but it can only be used with FT_UINT16, not %s" , hfinfo->name, hfinfo->abbrev, tmp_str, ftype_name(hfinfo ->type))
9556 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) has 'display' value %s but it can only be used with FT_UINT16, not %s" , hfinfo->name, hfinfo->abbrev, tmp_str, ftype_name(hfinfo ->type))
9557 | tmp_str, ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) has 'display' value %s but it can only be used with FT_UINT16, not %s" , hfinfo->name, hfinfo->abbrev, tmp_str, ftype_name(hfinfo ->type));
9558 | }
9559 | if (hfinfo->strings != NULL((void*)0)) {
9560 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s (%s) but has a strings value",proto_report_dissector_bug("Field '%s' (%s) is an %s (%s) but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9561 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s (%s) but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9562 | ftype_name(hfinfo->type), tmp_str)proto_report_dissector_bug("Field '%s' (%s) is an %s (%s) but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str);
9563 | }
9564 | if (hfinfo->bitmask != 0) {
9565 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s (%s) but has a bitmask",proto_report_dissector_bug("Field '%s' (%s) is an %s (%s) but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9566 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s (%s) but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9567 | ftype_name(hfinfo->type), tmp_str)proto_report_dissector_bug("Field '%s' (%s) is an %s (%s) but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str);
9568 | }
9569 | wmem_free(NULL((void*)0), tmp_str);
9570 | break;
9571 | }
9572 |
9573 | if (hfinfo->display == BASE_OUI) {
9574 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Unknown: 0x%x)");
9575 | if (hfinfo->type != FT_UINT24) {
9576 | REPORT_DISSECTOR_BUG("Field '%s' (%s) has 'display' value %s but it can only be used with FT_UINT24, not %s",proto_report_dissector_bug("Field '%s' (%s) has 'display' value %s but it can only be used with FT_UINT24, not %s" , hfinfo->name, hfinfo->abbrev, tmp_str, ftype_name(hfinfo ->type))
9577 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) has 'display' value %s but it can only be used with FT_UINT24, not %s" , hfinfo->name, hfinfo->abbrev, tmp_str, ftype_name(hfinfo ->type))
9578 | tmp_str, ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) has 'display' value %s but it can only be used with FT_UINT24, not %s" , hfinfo->name, hfinfo->abbrev, tmp_str, ftype_name(hfinfo ->type));
9579 | }
9580 | if (hfinfo->strings != NULL((void*)0)) {
9581 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s (%s) but has a strings value",proto_report_dissector_bug("Field '%s' (%s) is an %s (%s) but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9582 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s (%s) but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9583 | ftype_name(hfinfo->type), tmp_str)proto_report_dissector_bug("Field '%s' (%s) is an %s (%s) but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str);
9584 | }
9585 | if (hfinfo->bitmask != 0) {
9586 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s (%s) but has a bitmask",proto_report_dissector_bug("Field '%s' (%s) is an %s (%s) but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9587 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s (%s) but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9588 | ftype_name(hfinfo->type), tmp_str)proto_report_dissector_bug("Field '%s' (%s) is an %s (%s) but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str);
9589 | }
9590 | wmem_free(NULL((void*)0), tmp_str);
9591 | break;
9592 | }
9593 |
9594 | /* Require integral types (other than frame number,
9595 | * which is always displayed in decimal) to have a
9596 | * number base.
9597 | *
9598 | * If the display value is BASE_NONE and there is a
9599 | * strings conversion then the dissector writer is
9600 | * telling us that the field's numerical value is
9601 | * meaningless; we'll avoid showing the value to the
9602 | * user.
9603 | */
9604 | switch (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF)) {
9605 | case BASE_DEC:
9606 | case BASE_HEX:
9607 | case BASE_OCT:
9608 | case BASE_DEC_HEX:
9609 | case BASE_HEX_DEC:
9610 | case BASE_CUSTOM: /* hfinfo_numeric_value_format() treats this as decimal */
9611 | break;
9612 | case BASE_NONE:
9613 | if (hfinfo->strings == NULL((void*)0)) {
9614 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an integral value (%s)"proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as BASE_NONE but" " without a strings conversion" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9615 | " but is being displayed as BASE_NONE but"proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as BASE_NONE but" " without a strings conversion" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9616 | " without a strings conversion",proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as BASE_NONE but" " without a strings conversion" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9617 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as BASE_NONE but" " without a strings conversion" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9618 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as BASE_NONE but" " without a strings conversion" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9619 | }
9620 | if (hfinfo->display & BASE_SPECIAL_VALS0x00008000) {
9621 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an integral value (%s)"proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " that is being displayed as BASE_NONE but" " with BASE_SPECIAL_VALS" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9622 | " that is being displayed as BASE_NONE but"proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " that is being displayed as BASE_NONE but" " with BASE_SPECIAL_VALS" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9623 | " with BASE_SPECIAL_VALS",proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " that is being displayed as BASE_NONE but" " with BASE_SPECIAL_VALS" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9624 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " that is being displayed as BASE_NONE but" " with BASE_SPECIAL_VALS" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9625 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " that is being displayed as BASE_NONE but" " with BASE_SPECIAL_VALS" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9626 | }
9627 | break;
9628 |
9629 | default:
9630 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Unknown: 0x%x)");
9631 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an integral value (%s)"proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9632 | " but is being displayed as %s",proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9633 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9634 | ftype_name(hfinfo->type), tmp_str)proto_report_dissector_bug("Field '%s' (%s) is an integral value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str);
9635 | //wmem_free(NULL, tmp_str);
9636 | }
9637 | break;
9638 | case FT_BYTES:
9639 | case FT_UINT_BYTES:
9640 | /* Require bytes to have a "display type" that could
9641 | * add a character between displayed bytes.
9642 | */
9643 | switch (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF)) {
9644 | case BASE_NONE:
9645 | case SEP_DOT:
9646 | case SEP_DASH:
9647 | case SEP_COLON:
9648 | case SEP_SPACE:
9649 | break;
9650 | default:
9651 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Bit count: %d)");
9652 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an byte array but is being displayed as %s instead of BASE_NONE, SEP_DOT, SEP_DASH, SEP_COLON, or SEP_SPACE",proto_report_dissector_bug("Field '%s' (%s) is an byte array but is being displayed as %s instead of BASE_NONE, SEP_DOT, SEP_DASH, SEP_COLON, or SEP_SPACE" , hfinfo->name, hfinfo->abbrev, tmp_str)
9653 | hfinfo->name, hfinfo->abbrev, tmp_str)proto_report_dissector_bug("Field '%s' (%s) is an byte array but is being displayed as %s instead of BASE_NONE, SEP_DOT, SEP_DASH, SEP_COLON, or SEP_SPACE" , hfinfo->name, hfinfo->abbrev, tmp_str);
9654 | //wmem_free(NULL, tmp_str);
9655 | }
9656 | if (hfinfo->bitmask != 0)
9657 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but has a bitmask",proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9658 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9659 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9660 | //allowed to support string if its a protocol (for pinos)
9661 | if ((hfinfo->strings != NULL((void*)0)) && (!(hfinfo->display & BASE_PROTOCOL_INFO0x00004000)))
9662 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but has a strings value",proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9663 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9664 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9665 | break;
9666 |
9667 | case FT_PROTOCOL:
9668 | case FT_FRAMENUM:
9669 | if (hfinfo->display != BASE_NONE) {
9670 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Bit count: %d)");
9671 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE",proto_report_dissector_bug("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9672 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9673 | ftype_name(hfinfo->type), tmp_str)proto_report_dissector_bug("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str);
9674 | //wmem_free(NULL, tmp_str);
9675 | }
9676 | if (hfinfo->bitmask != 0)
9677 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but has a bitmask",proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9678 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9679 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9680 | break;
9681 |
9682 | case FT_BOOLEAN:
9683 | break;
9684 |
9685 | case FT_ABSOLUTE_TIME:
9686 | if (!FIELD_DISPLAY_IS_ABSOLUTE_TIME(hfinfo->display)(((hfinfo->display) & 0xFF) >= ABSOLUTE_TIME_LOCAL && ((hfinfo->display) & 0xFF) <= ABSOLUTE_TIME_UNIX)) {
9687 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Bit count: %d)");
9688 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is a %s but is being displayed as %s instead of as a time",proto_report_dissector_bug("Field '%s' (%s) is a %s but is being displayed as %s instead of as a time" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9689 | hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type), tmp_str)proto_report_dissector_bug("Field '%s' (%s) is a %s but is being displayed as %s instead of as a time" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str);
9690 | //wmem_free(NULL, tmp_str);
9691 | }
9692 | if (hfinfo->bitmask != 0)
9693 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but has a bitmask",proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9694 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9695 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9696 | break;
9697 |
9698 | case FT_STRING:
9699 | case FT_STRINGZ:
9700 | case FT_UINT_STRING:
9701 | case FT_STRINGZPAD:
9702 | case FT_STRINGZTRUNC:
9703 | switch (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF)) {
9704 | case BASE_NONE:
9705 | case BASE_STR_WSP:
9706 | break;
9707 |
9708 | default:
9709 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Unknown: 0x%x)");
9710 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an string value (%s)"proto_report_dissector_bug("Field '%s' (%s) is an string value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9711 | " but is being displayed as %s",proto_report_dissector_bug("Field '%s' (%s) is an string value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9712 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an string value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9713 | ftype_name(hfinfo->type), tmp_str)proto_report_dissector_bug("Field '%s' (%s) is an string value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str);
9714 | //wmem_free(NULL, tmp_str);
9715 | }
9716 |
9717 | if (hfinfo->bitmask != 0)
9718 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but has a bitmask",proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9719 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9720 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9721 | if (hfinfo->strings != NULL((void*)0))
9722 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but has a strings value",proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9723 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9724 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9725 | break;
9726 |
9727 | case FT_IPv4:
9728 | switch (hfinfo->display) {
9729 | case BASE_NONE:
9730 | case BASE_NETMASK:
9731 | break;
9732 |
9733 | default:
9734 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Unknown: 0x%x)");
9735 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an IPv4 value (%s)"proto_report_dissector_bug("Field '%s' (%s) is an IPv4 value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9736 | " but is being displayed as %s",proto_report_dissector_bug("Field '%s' (%s) is an IPv4 value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9737 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an IPv4 value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9738 | ftype_name(hfinfo->type), tmp_str)proto_report_dissector_bug("Field '%s' (%s) is an IPv4 value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str);
9739 | //wmem_free(NULL, tmp_str);
9740 | break;
9741 | }
9742 | break;
9743 | case FT_FLOAT:
9744 | case FT_DOUBLE:
9745 | switch (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF)) {
9746 | case BASE_NONE:
9747 | case BASE_DEC:
9748 | case BASE_HEX:
9749 | case BASE_EXP:
9750 | case BASE_CUSTOM:
9751 | break;
9752 | default:
9753 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Unknown: 0x%x)");
9754 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is a float value (%s)"proto_report_dissector_bug("Field '%s' (%s) is a float value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9755 | " but is being displayed as %s",proto_report_dissector_bug("Field '%s' (%s) is a float value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9756 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is a float value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str)
9757 | ftype_name(hfinfo->type), tmp_str)proto_report_dissector_bug("Field '%s' (%s) is a float value (%s)" " but is being displayed as %s", hfinfo->name, hfinfo-> abbrev, ftype_name(hfinfo->type), tmp_str);
9758 | //wmem_free(NULL, tmp_str);
9759 | }
9760 | if (hfinfo->bitmask != 0)
9761 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but has a bitmask",proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9762 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9763 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9764 | if (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF) != BASE_CUSTOM && (hfinfo->strings != NULL((void*)0)) && !(hfinfo->display & BASE_UNIT_STRING0x00001000))
9765 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but has a strings value",proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9766 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9767 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9768 | break;
9769 | case FT_IEEE_11073_SFLOAT:
9770 | case FT_IEEE_11073_FLOAT:
9771 | if (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF) != BASE_NONE) {
9772 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Bit count: %d)");
9773 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE",proto_report_dissector_bug("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9774 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9775 | ftype_name(hfinfo->type),proto_report_dissector_bug("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9776 | tmp_str)proto_report_dissector_bug("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str);
9777 | //wmem_free(NULL, tmp_str);
9778 | }
9779 | if (hfinfo->bitmask != 0)
9780 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but has a bitmask",proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9781 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9782 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9783 | if ((hfinfo->strings != NULL((void*)0)) && !(hfinfo->display & BASE_UNIT_STRING0x00001000))
9784 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but has a strings value",proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9785 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9786 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9787 | break;
9788 | default:
9789 | if (hfinfo->display != BASE_NONE) {
9790 | tmp_str = val_to_str(NULL((void*)0), hfinfo->display, hf_display, "(Bit count: %d)");
9791 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE",proto_report_dissector_bug("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9792 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9793 | ftype_name(hfinfo->type),proto_report_dissector_bug("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str)
9794 | tmp_str)proto_report_dissector_bug("Field '%s' (%s) is an %s but is being displayed as %s instead of BASE_NONE" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ), tmp_str);
9795 | //wmem_free(NULL, tmp_str);
9796 | }
9797 | if (hfinfo->bitmask != 0)
9798 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but has a bitmask",proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9799 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9800 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an %s but has a bitmask" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9801 | if (hfinfo->strings != NULL((void*)0))
9802 | REPORT_DISSECTOR_BUG("Field '%s' (%s) is an %s but has a strings value",proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9803 | hfinfo->name, hfinfo->abbrev,proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ))
9804 | ftype_name(hfinfo->type))proto_report_dissector_bug("Field '%s' (%s) is an %s but has a strings value" , hfinfo->name, hfinfo->abbrev, ftype_name(hfinfo->type ));
9805 | break;
9806 | }
9807 | }
9808 |
9809 | static void
9810 | register_type_length_mismatch(void)
9811 | {
9812 | static ei_register_info ei[] = {
9813 | { &ei_type_length_mismatch_error, { "_ws.type_length.mismatch", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "Trying to fetch X with length Y", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9814 | { &ei_type_length_mismatch_warn, { "_ws.type_length.mismatch_warn", PI_MALFORMED0x07000000, PI_WARN0x00600000, "Trying to fetch X with length Y", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9815 | };
9816 |
9817 | expert_module_t* expert_type_length_mismatch;
9818 |
9819 | proto_type_length_mismatch = proto_register_protocol("Type Length Mismatch", "Type length mismatch", "_ws.type_length");
9820 |
9821 | expert_type_length_mismatch = expert_register_protocol(proto_type_length_mismatch);
9822 | expert_register_field_array(expert_type_length_mismatch, ei, array_length(ei)(sizeof (ei) / sizeof (ei)[0]));
9823 |
9824 | /* "Type Length Mismatch" isn't really a protocol, it's an error indication;
9825 | disabling them makes no sense. */
9826 | proto_set_cant_toggle(proto_type_length_mismatch);
9827 | }
9828 |
9829 | static void
9830 | register_byte_array_string_decodinws_error(void)
9831 | {
9832 | static ei_register_info ei[] = {
9833 | { &ei_byte_array_string_decoding_failed_error,
9834 | { "_ws.byte_array_string.decoding_error.failed", PI_MALFORMED0x07000000, PI_ERROR0x00800000,
9835 | "Failed to decode byte array from string", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}
9836 | }
9837 | },
9838 | };
9839 |
9840 | expert_module_t* expert_byte_array_string_decoding_error;
9841 |
9842 | proto_byte_array_string_decoding_error =
9843 | proto_register_protocol("Byte Array-String Decoding Error",
9844 | "Byte Array-string decoding error",
9845 | "_ws.byte_array_string.decoding_error");
9846 |
9847 | expert_byte_array_string_decoding_error =
9848 | expert_register_protocol(proto_byte_array_string_decoding_error);
9849 | expert_register_field_array(expert_byte_array_string_decoding_error, ei, array_length(ei)(sizeof (ei) / sizeof (ei)[0]));
9850 |
9851 | /* "Byte Array-String Decoding Error" isn't really a protocol, it's an error indication;
9852 | disabling them makes no sense. */
9853 | proto_set_cant_toggle(proto_byte_array_string_decoding_error);
9854 | }
9855 |
9856 | static void
9857 | register_date_time_string_decodinws_error(void)
9858 | {
9859 | static ei_register_info ei[] = {
9860 | { &ei_date_time_string_decoding_failed_error,
9861 | { "_ws.date_time_string.decoding_error.failed", PI_MALFORMED0x07000000, PI_ERROR0x00800000,
9862 | "Failed to decode date and time from string", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}}
9863 | }
9864 | },
9865 | };
9866 |
9867 | expert_module_t* expert_date_time_string_decoding_error;
9868 |
9869 | proto_date_time_string_decoding_error =
9870 | proto_register_protocol("Date and Time-String Decoding Error",
9871 | "Date and Time-string decoding error",
9872 | "_ws.date_time_string.decoding_error");
9873 |
9874 | expert_date_time_string_decoding_error =
9875 | expert_register_protocol(proto_date_time_string_decoding_error);
9876 | expert_register_field_array(expert_date_time_string_decoding_error, ei, array_length(ei)(sizeof (ei) / sizeof (ei)[0]));
9877 |
9878 | /* "Date and Time-String Decoding Error" isn't really a protocol, it's an error indication;
9879 | disabling them makes no sense. */
9880 | proto_set_cant_toggle(proto_date_time_string_decoding_error);
9881 | }
9882 |
9883 | static void
9884 | register_string_errors(void)
9885 | {
9886 | static ei_register_info ei[] = {
9887 | { &ei_string_trailing_characters,
9888 | { "_ws.string.trailing_stray_characters", PI_UNDECODED0x05000000, PI_WARN0x00600000, "Trailing stray characters", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }
9889 | },
9890 | };
9891 |
9892 | expert_module_t* expert_string_errors;
9893 |
9894 | proto_string_errors = proto_register_protocol("String Errors", "String errors", "_ws.string");
9895 |
9896 | expert_string_errors = expert_register_protocol(proto_string_errors);
9897 | expert_register_field_array(expert_string_errors, ei, array_length(ei)(sizeof (ei) / sizeof (ei)[0]));
9898 |
9899 | /* "String Errors" isn't really a protocol, it's an error indication;
9900 | disabling them makes no sense. */
9901 | proto_set_cant_toggle(proto_string_errors);
9902 | }
9903 |
9904 | static int
9905 | proto_register_field_init(header_field_info *hfinfo, const int parent)
9906 | {
9907 |
9908 | tmp_fld_check_assert(hfinfo);
9909 |
9910 | hfinfo->parent = parent;
9911 | hfinfo->same_name_next = NULL((void*)0);
9912 | hfinfo->same_name_prev_id = -1;
9913 |
9914 | /* if we always add and never delete, then id == len - 1 is correct */
9915 | if (gpa_hfinfo.len >= gpa_hfinfo.allocated_len) {
9916 | if (!gpa_hfinfo.hfi) {
9917 | gpa_hfinfo.allocated_len = PROTO_PRE_ALLOC_HF_FIELDS_MEM(300000+5000);
9918 | gpa_hfinfo.hfi = (header_field_info **)g_malloc(sizeof(header_field_info *)*PROTO_PRE_ALLOC_HF_FIELDS_MEM(300000+5000));
9919 | /* The entry with index 0 is not used. */
9920 | gpa_hfinfo.hfi[0] = NULL((void*)0);
9921 | gpa_hfinfo.len = 1;
9922 | } else {
9923 | gpa_hfinfo.allocated_len += 1000;
9924 | gpa_hfinfo.hfi = (header_field_info **)g_realloc(gpa_hfinfo.hfi,
9925 | sizeof(header_field_info *)*gpa_hfinfo.allocated_len);
9926 | /*ws_warning("gpa_hfinfo.allocated_len %u", gpa_hfinfo.allocated_len);*/
9927 | }
9928 | }
9929 | gpa_hfinfo.hfi[gpa_hfinfo.len] = hfinfo;
9930 | gpa_hfinfo.len++;
9931 | hfinfo->id = gpa_hfinfo.len - 1;
9932 |
9933 | /* if we have real names, enter this field in the name tree */
9934 | /* Already checked in tmp_fld_check_assert */
9935 | /*if ((hfinfo->name[0] != 0) && (hfinfo->abbrev[0] != 0 )) */
9936 | {
9937 |
9938 | header_field_info *same_name_next_hfinfo;
9939 |
9940 | /* We allow multiple hfinfo's to be registered under the same
9941 | * abbreviation. This was done for X.25, as, depending
9942 | * on whether it's modulo-8 or modulo-128 operation,
9943 | * some bitfield fields may be in different bits of
9944 | * a byte, and we want to be able to refer to that field
9945 | * with one name regardless of whether the packets
9946 | * are modulo-8 or modulo-128 packets. */
9947 |
9948 | /* wmem_map_insert - if key is already present the previous
9949 | * hfinfo with the same key/name is returned, otherwise NULL */
9950 | same_name_hfinfo = wmem_map_insert(gpa_name_map, (void *) (hfinfo->abbrev), hfinfo);
9951 | if (same_name_hfinfo) {
9952 | /* There's already a field with this name.
9953 | * Put the current field *before* that field
9954 | * in the list of fields with this name, Thus,
9955 | * we end up with an effectively
9956 | * doubly-linked-list of same-named hfinfo's,
9957 | * with the head of the list (stored in the
9958 | * hash) being the last seen hfinfo.
9959 | */
9960 | same_name_next_hfinfo =
9961 | same_name_hfinfo->same_name_next;
9962 |
9963 | hfinfo->same_name_next = same_name_next_hfinfo;
9964 | if (same_name_next_hfinfo)
9965 | same_name_next_hfinfo->same_name_prev_id = hfinfo->id;
9966 |
9967 | same_name_hfinfo->same_name_next = hfinfo;
9968 | hfinfo->same_name_prev_id = same_name_hfinfo->id;
9969 | #ifdef ENABLE_CHECK_FILTER
9970 | while (same_name_hfinfo) {
9971 | if (!ftype_similar_types(hfinfo->type, same_name_hfinfo->type))
9972 | ws_error("'%s' exists multiple times with incompatible types: %s and %s", hfinfo->abbrev, ftype_name(hfinfo->type), ftype_name(same_name_hfinfo->type))ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 9972 , __func__, "'%s' exists multiple times with incompatible types: %s and %s" , hfinfo->abbrev, ftype_name(hfinfo->type), ftype_name( same_name_hfinfo->type));
9973 | same_name_hfinfo = same_name_hfinfo->same_name_next;
9974 | }
9975 | #endif
9976 | }
9977 | }
9978 |
9979 | return hfinfo->id;
9980 | }
9981 |
9982 | void
9983 | proto_register_subtree_array(int * const *indices, const int num_indices)
9984 | {
9985 | int i;
9986 | int *const *ptr = indices;
9987 |
9988 | /*
9989 | * If we've already allocated the array of tree types, expand
9990 | * it; this lets plugins such as mate add tree types after
9991 | * the initial startup. (If we haven't already allocated it,
9992 | * we don't allocate it; on the first pass, we just assign
9993 | * ett values and keep track of how many we've assigned, and
9994 | * when we're finished registering all dissectors we allocate
9995 | * the array, so that we do only one allocation rather than
9996 | * wasting CPU time and memory by growing the array for each
9997 | * dissector that registers ett values.)
9998 | */
9999 | if (tree_is_expanded != NULL((void*)0)) {
10000 | tree_is_expanded = (uint32_t *)g_realloc(tree_is_expanded, (1+((num_tree_types + num_indices)/32)) * sizeof(uint32_t));
10001 |
10002 | /* set new items to 0 */
10003 | /* XXX, slow!!! optimize when needed (align 'i' to 32, and set rest of uint32_t to 0) */
10004 | for (i = num_tree_types; i < num_tree_types + num_indices; i++)
10005 | tree_is_expanded[i >> 5] &= ~(1U << (i & 31));
10006 | }
10007 |
10008 | /*
10009 | * Assign "num_indices" subtree numbers starting at "num_tree_types",
10010 | * returning the indices through the pointers in the array whose
10011 | * first element is pointed to by "indices", and update
10012 | * "num_tree_types" appropriately.
10013 | */
10014 | for (i = 0; i < num_indices; i++, ptr++, num_tree_types++) {
10015 | if (**ptr != -1 && **ptr != 0) {
10016 | REPORT_DISSECTOR_BUG("register_subtree_array: subtree item type (ett_...) not -1 or 0 !"proto_report_dissector_bug("register_subtree_array: subtree item type (ett_...) not -1 or 0 !" " This is a development error:" " Either the subtree item type has already been assigned or" " was not initialized to -1 or 0.")
10017 | " This is a development error:"proto_report_dissector_bug("register_subtree_array: subtree item type (ett_...) not -1 or 0 !" " This is a development error:" " Either the subtree item type has already been assigned or" " was not initialized to -1 or 0.")
10018 | " Either the subtree item type has already been assigned or"proto_report_dissector_bug("register_subtree_array: subtree item type (ett_...) not -1 or 0 !" " This is a development error:" " Either the subtree item type has already been assigned or" " was not initialized to -1 or 0.")
10019 | " was not initialized to -1 or 0.")proto_report_dissector_bug("register_subtree_array: subtree item type (ett_...) not -1 or 0 !" " This is a development error:" " Either the subtree item type has already been assigned or" " was not initialized to -1 or 0.");
10020 | }
10021 | **ptr = num_tree_types;
10022 | }
10023 | }
10024 |
10025 | static void
10026 | mark_truncated(char *label_str, size_t name_pos, const size_t size, size_t *value_pos)
10027 | {
10028 | static const char trunc_str[] = " [" UTF8_HORIZONTAL_ELLIPSIS"\u2026" "] ";
10029 | const size_t trunc_len = sizeof(trunc_str)-2; /* Default do not include the trailing space. */
10030 | char *last_char;
10031 |
10032 | /* ..... field_name: dataaaaaaaaaaaaa
10033 | * |
10034 | * ^^^^^ name_pos
10035 | *
10036 | * ..... field_name […]: dataaaaaaaaaaaaa
10037 | *
10038 | * name_pos==0 means that we have only data or only a field_name
10039 | */
10040 |
10041 | ws_abort_if_fail(size > trunc_len)do { if ((1) && !(size > trunc_len)) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 10041, __func__, "assertion failed: %s" , "size > trunc_len"); } while (0);
10042 |
10043 | if (name_pos >= size - trunc_len) {
10044 | /* No room for trunc_str after the field_name, put it first. */
10045 | name_pos = 0;
10046 | }
10047 |
10048 | memmove(label_str + name_pos + trunc_len, label_str + name_pos, size - name_pos - trunc_len);
10049 | if (name_pos == 0) {
10050 | /* Copy the trunc_str after the first byte, so that we don't have a leading space in the label. */
10051 | memcpy(label_str, trunc_str + 1, trunc_len);
10052 | } else {
10053 | memcpy(label_str + name_pos, trunc_str, trunc_len);
10054 | }
10055 | /* in general, label_str is UTF-8
10056 | we can truncate it only at the beginning of a new character
10057 | we go backwards from the byte right after our buffer and
10058 | find the next starting byte of a UTF-8 character, this is
10059 | where we cut
10060 | there's no need to use g_utf8_find_prev_char(), the search
10061 | will always succeed since we copied trunc_str into the
10062 | buffer */
10063 | /* g_utf8_prev_char does not deference the memory address
10064 | * passed in (until after decrementing it, so it is perfectly
10065 | * legal to pass in a pointer one past the last element.
10066 | */
10067 | last_char = g_utf8_prev_char(label_str + size);
10068 | *last_char = '\0';
10069 | /* This is unnecessary (above always terminates), but try to
10070 | * convince Coverity to avoid dozens of false positives. */
10071 | label_str[size - 1] = '\0';
10072 |
10073 | if (value_pos && *value_pos > 0) {
10074 | if (name_pos == 0) {
10075 | *value_pos += trunc_len;
10076 | } else {
10077 | /* Move one back to include trunc_str in the value. */
10078 | *value_pos -= 1;
10079 | }
10080 | }
10081 |
10082 | /* Check if value_pos is past label_str. */
10083 | if (value_pos && *value_pos >= size) {
10084 | *value_pos = size - 1;
10085 | }
10086 | }
10087 |
10088 | static void
10089 | label_mark_truncated(char *label_str, size_t name_pos, size_t *value_pos)
10090 | {
10091 | mark_truncated(label_str, name_pos, ITEM_LABEL_LENGTH240, value_pos);
10092 | }
10093 |
10094 | static size_t
10095 | label_fill(char *label_str, size_t pos, const header_field_info *hfinfo, const char *text, size_t *value_pos)
10096 | {
10097 | size_t name_pos;
10098 |
10099 | /* "%s: %s", hfinfo->name, text */
10100 | name_pos = pos = label_concat(label_str, pos, (const uint8_t*)hfinfo->name)ws_label_strcpy(label_str, 240, pos, (const uint8_t*)hfinfo-> name, 0);
10101 | if (!(hfinfo->display & BASE_NO_DISPLAY_VALUE0x00002000)) {
10102 | pos = label_concat(label_str, pos, (const uint8_t*)": ")ws_label_strcpy(label_str, 240, pos, (const uint8_t*)": ", 0);
10103 | if (value_pos) {
10104 | *value_pos = pos;
10105 | }
10106 | pos = ws_label_strcpy(label_str, ITEM_LABEL_LENGTH240, pos, (const uint8_t*)(text ? text : "(null)"), label_strcat_flags(hfinfo));
10107 | }
10108 |
10109 | if (pos >= ITEM_LABEL_LENGTH240) {
10110 | /* Uh oh, we don't have enough room. Tell the user that the field is truncated. */
10111 | label_mark_truncated(label_str, name_pos, value_pos);
10112 | }
10113 |
10114 | return pos;
10115 | }
10116 |
10117 | static size_t
10118 | label_fill_descr(char *label_str, size_t pos, const header_field_info *hfinfo, const char *text, const char *descr, size_t *value_pos)
10119 | {
10120 | size_t name_pos;
10121 |
10122 | /* "%s: %s (%s)", hfinfo->name, text, descr */
10123 | name_pos = pos = label_concat(label_str, pos, (const uint8_t*)hfinfo->name)ws_label_strcpy(label_str, 240, pos, (const uint8_t*)hfinfo-> name, 0);
10124 | if (!(hfinfo->display & BASE_NO_DISPLAY_VALUE0x00002000)) {
10125 | pos = label_concat(label_str, pos, (const uint8_t*)": ")ws_label_strcpy(label_str, 240, pos, (const uint8_t*)": ", 0);
10126 | if (value_pos) {
10127 | *value_pos = pos;
10128 | }
10129 | if (hfinfo->display & BASE_UNIT_STRING0x00001000) {
10130 | pos = label_concat(label_str, pos, (const uint8_t*)(descr ? descr : "(null)"))ws_label_strcpy(label_str, 240, pos, (const uint8_t*)(descr ? descr : "(null)"), 0);
10131 | pos = label_concat(label_str, pos, (const uint8_t*)(text ? text : "(null)"))ws_label_strcpy(label_str, 240, pos, (const uint8_t*)(text ? text : "(null)"), 0);
10132 | } else {
10133 | pos = label_concat(label_str, pos, (const uint8_t*)(text ? text : "(null)"))ws_label_strcpy(label_str, 240, pos, (const uint8_t*)(text ? text : "(null)"), 0);
10134 | pos = label_concat(label_str, pos, (const uint8_t*)" (")ws_label_strcpy(label_str, 240, pos, (const uint8_t*)" (", 0);
10135 | pos = label_concat(label_str, pos, (const uint8_t*)(descr ? descr : "(null)"))ws_label_strcpy(label_str, 240, pos, (const uint8_t*)(descr ? descr : "(null)"), 0);
10136 | pos = label_concat(label_str, pos, (const uint8_t*)")")ws_label_strcpy(label_str, 240, pos, (const uint8_t*)")", 0);
10137 | }
10138 | }
10139 |
10140 | if (pos >= ITEM_LABEL_LENGTH240) {
10141 | /* Uh oh, we don't have enough room. Tell the user that the field is truncated. */
10142 | label_mark_truncated(label_str, name_pos, value_pos);
10143 | }
10144 |
10145 | return pos;
10146 | }
10147 |
10148 | void
10149 | proto_item_fill_label(const field_info *fi, char *label_str, size_t *value_pos)
10150 | {
10151 | const header_field_info *hfinfo;
10152 | const char *str;
10153 | const uint8_t *bytes;
10154 | uint32_t integer;
10155 | const ipv4_addr_and_mask *ipv4;
10156 | const ipv6_addr_and_prefix *ipv6;
10157 | const e_guid_t *guid;
10158 | char *name;
10159 | address addr;
10160 | char *addr_str;
10161 | char *tmp;
10162 |
10163 | if (!label_str) {
10164 | ws_warning("NULL label_str passed to proto_item_fill_label.")do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 10164, __func__, "NULL label_str passed to proto_item_fill_label." ); } } while (0);
10165 | return;
10166 | }
10167 |
10168 | label_str[0]= '\0';
10169 |
10170 | if (!fi) {
10171 | return;
10172 | }
10173 |
10174 | hfinfo = fi->hfinfo;
10175 |
10176 | switch (hfinfo->type) {
10177 | case FT_NONE:
10178 | case FT_PROTOCOL:
10179 | (void) g_strlcpy(label_str, hfinfo->name, ITEM_LABEL_LENGTH240);
10180 | if (value_pos) {
10181 | *value_pos = strlen(hfinfo->name);
10182 | }
10183 | break;
10184 |
10185 | case FT_BOOLEAN:
10186 | fill_label_boolean(fi, label_str, value_pos);
10187 | break;
10188 |
10189 | case FT_BYTES:
10190 | case FT_UINT_BYTES:
10191 | tmp = format_bytes_hfinfo(NULL((void*)0), hfinfo,
10192 | fvalue_get_bytes_data(fi->value),
10193 | (unsigned)fvalue_length2(fi->value));
10194 | label_fill(label_str, 0, hfinfo, tmp, value_pos);
10195 | wmem_free(NULL((void*)0), tmp);
10196 | break;
10197 |
10198 | case FT_CHAR:
10199 | if (hfinfo->bitmask) {
10200 | fill_label_bitfield_char(fi, label_str, value_pos);
10201 | } else {
10202 | fill_label_char(fi, label_str, value_pos);
10203 | }
10204 | break;
10205 |
10206 | /* Four types of integers to take care of:
10207 | * Bitfield, with val_string
10208 | * Bitfield, w/o val_string
10209 | * Non-bitfield, with val_string
10210 | * Non-bitfield, w/o val_string
10211 | */
10212 | case FT_UINT8:
10213 | case FT_UINT16:
10214 | case FT_UINT24:
10215 | case FT_UINT32:
10216 | if (hfinfo->bitmask) {
10217 | fill_label_bitfield(fi, label_str, value_pos, false0);
10218 | } else {
10219 | fill_label_number(fi, label_str, value_pos, false0);
10220 | }
10221 | break;
10222 |
10223 | case FT_FRAMENUM:
10224 | fill_label_number(fi, label_str, value_pos, false0);
10225 | break;
10226 |
10227 | case FT_UINT40:
10228 | case FT_UINT48:
10229 | case FT_UINT56:
10230 | case FT_UINT64:
10231 | if (hfinfo->bitmask) {
10232 | fill_label_bitfield64(fi, label_str, value_pos, false0);
10233 | } else {
10234 | fill_label_number64(fi, label_str, value_pos, false0);
10235 | }
10236 | break;
10237 |
10238 | case FT_INT8:
10239 | case FT_INT16:
10240 | case FT_INT24:
10241 | case FT_INT32:
10242 | if (hfinfo->bitmask) {
10243 | fill_label_bitfield(fi, label_str, value_pos, true1);
10244 | } else {
10245 | fill_label_number(fi, label_str, value_pos, true1);
10246 | }
10247 | break;
10248 |
10249 | case FT_INT40:
10250 | case FT_INT48:
10251 | case FT_INT56:
10252 | case FT_INT64:
10253 | if (hfinfo->bitmask) {
10254 | fill_label_bitfield64(fi, label_str, value_pos, true1);
10255 | } else {
10256 | fill_label_number64(fi, label_str, value_pos, true1);
10257 | }
10258 | break;
10259 |
10260 | case FT_FLOAT:
10261 | case FT_DOUBLE:
10262 | fill_label_float(fi, label_str, value_pos);
10263 | break;
10264 |
10265 | case FT_ABSOLUTE_TIME:
10266 | {
10267 | const nstime_t *value = fvalue_get_time(fi->value);
10268 | int flags = ABS_TIME_TO_STR_SHOW_ZONE(1U << 0);
10269 | if (prefs.display_abs_time_ascii < ABS_TIME_ASCII_TREE) {
10270 | flags |= ABS_TIME_TO_STR_ISO8601(1U << 3);
10271 | }
10272 | if (hfinfo->strings) {
10273 | /*
10274 | * Table of time valus to be displayed
10275 | * specially.
10276 | */
10277 | const char *time_string = try_time_val_to_str(value, (const time_value_string *)hfinfo->strings);
10278 | if (time_string != NULL((void*)0)) {
10279 | label_fill(label_str, 0, hfinfo, time_string, value_pos);
10280 | break;
10281 | }
10282 | }
10283 | tmp = abs_time_to_str_ex(NULL((void*)0), value, hfinfo->display, flags);
10284 | label_fill(label_str, 0, hfinfo, tmp, value_pos);
10285 | wmem_free(NULL((void*)0), tmp);
10286 | break;
10287 | }
10288 | case FT_RELATIVE_TIME:
10289 | tmp = rel_time_to_str(NULL((void*)0), fvalue_get_time(fi->value));
10290 | label_fill(label_str, 0, hfinfo, tmp, value_pos);
10291 | wmem_free(NULL((void*)0), tmp);
10292 | break;
10293 |
10294 | case FT_IPXNET:
10295 | integer = fvalue_get_uinteger(fi->value);
10296 | tmp = get_ipxnet_name(NULL((void*)0), integer);
10297 | addr_str = wmem_strdup_printf(NULL((void*)0), "0x%08X", integer);
10298 | label_fill_descr(label_str, 0, hfinfo, tmp, addr_str, value_pos);
10299 | wmem_free(NULL((void*)0), tmp);
10300 | wmem_free(NULL((void*)0), addr_str);
10301 | break;
10302 |
10303 | case FT_VINES:
10304 | addr.type = AT_VINES;
10305 | addr.len = VINES_ADDR_LEN6;
10306 | addr.data = fvalue_get_bytes_data(fi->value);
10307 |
10308 | addr_str = (char*)address_to_str(NULL((void*)0), &addr);
10309 | label_fill(label_str, 0, hfinfo, addr_str, value_pos);
10310 | wmem_free(NULL((void*)0), addr_str);
10311 | break;
10312 |
10313 | case FT_ETHER:
10314 | bytes = fvalue_get_bytes_data(fi->value);
10315 |
10316 | addr.type = AT_ETHER;
10317 | addr.len = 6;
10318 | addr.data = bytes;
10319 |
10320 | addr_str = (char*)address_with_resolution_to_str(NULL((void*)0), &addr);
10321 | label_fill(label_str, 0, hfinfo, addr_str, value_pos);
10322 | wmem_free(NULL((void*)0), addr_str);
10323 | break;
10324 |
10325 | case FT_IPv4:
10326 | ipv4 = fvalue_get_ipv4(fi->value);
10327 | set_address_ipv4(&addr, ipv4);
10328 |
10329 | if (hfinfo->display == BASE_NETMASK) {
10330 | addr_str = (char*)address_to_str(NULL((void*)0), &addr);
10331 | } else {
10332 | addr_str = (char*)address_with_resolution_to_str(NULL((void*)0), &addr);
10333 | }
10334 | label_fill(label_str, 0, hfinfo, addr_str, value_pos);
10335 | wmem_free(NULL((void*)0), addr_str);
10336 | free_address(&addr);
10337 | break;
10338 |
10339 | case FT_IPv6:
10340 | ipv6 = fvalue_get_ipv6(fi->value);
10341 | set_address_ipv6(&addr, ipv6);
10342 |
10343 | addr_str = (char*)address_with_resolution_to_str(NULL((void*)0), &addr);
10344 | label_fill(label_str, 0, hfinfo, addr_str, value_pos);
10345 | wmem_free(NULL((void*)0), addr_str);
10346 | free_address(&addr);
10347 | break;
10348 |
10349 | case FT_FCWWN:
10350 | bytes = fvalue_get_bytes_data(fi->value);
10351 | addr.type = AT_FCWWN;
10352 | addr.len = FCWWN_ADDR_LEN8;
10353 | addr.data = bytes;
10354 |
10355 | addr_str = (char*)address_with_resolution_to_str(NULL((void*)0), &addr);
10356 | label_fill(label_str, 0, hfinfo, addr_str, value_pos);
10357 | wmem_free(NULL((void*)0), addr_str);
10358 | break;
10359 |
10360 | case FT_GUID:
10361 | guid = fvalue_get_guid(fi->value);
10362 | tmp = guid_to_str(NULL((void*)0), guid);
10363 | label_fill(label_str, 0, hfinfo, tmp, value_pos);
10364 | wmem_free(NULL((void*)0), tmp);
10365 | break;
10366 |
10367 | case FT_OID:
10368 | bytes = fvalue_get_bytes_data(fi->value);
10369 | name = oid_resolved_from_encoded(NULL((void*)0), bytes, (int)fvalue_length2(fi->value));
10370 | tmp = oid_encoded2string(NULL((void*)0), bytes, (unsigned)fvalue_length2(fi->value));
10371 | if (name) {
10372 | label_fill_descr(label_str, 0, hfinfo, tmp, name, value_pos);
10373 | wmem_free(NULL((void*)0), name);
10374 | } else {
10375 | label_fill(label_str, 0, hfinfo, tmp, value_pos);
10376 | }
10377 | wmem_free(NULL((void*)0), tmp);
10378 | break;
10379 |
10380 | case FT_REL_OID:
10381 | bytes = fvalue_get_bytes_data(fi->value);
10382 | name = rel_oid_resolved_from_encoded(NULL((void*)0), bytes, (int)fvalue_length2(fi->value));
10383 | tmp = rel_oid_encoded2string(NULL((void*)0), bytes, (unsigned)fvalue_length2(fi->value));
10384 | if (name) {
10385 | label_fill_descr(label_str, 0, hfinfo, tmp, name, value_pos);
10386 | wmem_free(NULL((void*)0), name);
10387 | } else {
10388 | label_fill(label_str, 0, hfinfo, tmp, value_pos);
10389 | }
10390 | wmem_free(NULL((void*)0), tmp);
10391 | break;
10392 |
10393 | case FT_SYSTEM_ID:
10394 | bytes = fvalue_get_bytes_data(fi->value);
10395 | tmp = print_system_id(NULL((void*)0), bytes, (int)fvalue_length2(fi->value));
10396 | label_fill(label_str, 0, hfinfo, tmp, value_pos);
10397 | wmem_free(NULL((void*)0), tmp);
10398 | break;
10399 |
10400 | case FT_EUI64:
10401 | bytes = fvalue_get_bytes_data(fi->value);
10402 | addr.type = AT_EUI64;
10403 | addr.len = EUI64_ADDR_LEN8;
10404 | addr.data = bytes;
10405 |
10406 | addr_str = (char*)address_with_resolution_to_str(NULL((void*)0), &addr);
10407 | label_fill(label_str, 0, hfinfo, addr_str, value_pos);
10408 | wmem_free(NULL((void*)0), addr_str);
10409 | break;
10410 | case FT_STRING:
10411 | case FT_STRINGZ:
10412 | case FT_UINT_STRING:
10413 | case FT_STRINGZPAD:
10414 | case FT_STRINGZTRUNC:
10415 | case FT_AX25:
10416 | str = fvalue_get_string(fi->value);
10417 | label_fill(label_str, 0, hfinfo, str, value_pos);
10418 | break;
10419 |
10420 | case FT_IEEE_11073_SFLOAT:
10421 | case FT_IEEE_11073_FLOAT:
10422 | fill_label_ieee_11073_float(fi, label_str, value_pos);
10423 | break;
10424 |
10425 | default:
10426 | REPORT_DISSECTOR_BUG("field %s has type %d (%s) not handled in proto_item_fill_label()",proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_item_fill_label()" , hfinfo->abbrev, hfinfo->type, ftype_name(hfinfo->type ))
10427 | hfinfo->abbrev,proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_item_fill_label()" , hfinfo->abbrev, hfinfo->type, ftype_name(hfinfo->type ))
10428 | hfinfo->type,proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_item_fill_label()" , hfinfo->abbrev, hfinfo->type, ftype_name(hfinfo->type ))
10429 | ftype_name(hfinfo->type))proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_item_fill_label()" , hfinfo->abbrev, hfinfo->type, ftype_name(hfinfo->type ));
10430 | break;
10431 | }
10432 | }
10433 |
10434 | static void
10435 | fill_label_boolean(const field_info *fi, char *label_str, size_t *value_pos)
10436 | {
10437 | char *p;
10438 | int bitfield_byte_length = 0, bitwidth;
10439 | uint64_t unshifted_value;
10440 | uint64_t value;
10441 |
10442 | const header_field_info *hfinfo = fi->hfinfo;
10443 |
10444 | value = fvalue_get_uinteger64(fi->value);
10445 | if (hfinfo->bitmask) {
10446 | /* Figure out the bit width */
10447 | bitwidth = hfinfo_container_bitwidth(hfinfo);
10448 |
10449 | /* Un-shift bits */
10450 | unshifted_value = value;
10451 | unshifted_value <<= hfinfo_bitshift(hfinfo);
10452 |
10453 | /* Create the bitfield first */
10454 | p = decode_bitfield_value(label_str, unshifted_value, hfinfo->bitmask, bitwidth);
10455 | bitfield_byte_length = (int) (p - label_str);
10456 | }
10457 |
10458 | /* Fill in the textual info */
10459 | label_fill(label_str, bitfield_byte_length, hfinfo, tfs_get_string(!!value, hfinfo->strings), value_pos);
10460 | }
10461 |
10462 | static const char *
10463 | hf_try_val_to_str(uint32_t value, const header_field_info *hfinfo)
10464 | {
10465 | if (hfinfo->display & BASE_RANGE_STRING0x00000100)
10466 | return try_rval_to_str(value, (const range_string *) hfinfo->strings);
10467 |
10468 | if (hfinfo->display & BASE_EXT_STRING0x00000200) {
10469 | if (hfinfo->display & BASE_VAL64_STRING0x00000400)
10470 | return try_val64_to_str_ext(value, (val64_string_ext *) hfinfo->strings);
10471 | else
10472 | return try_val_to_str_ext(value, (value_string_ext *) hfinfo->strings);
10473 | }
10474 |
10475 | if (hfinfo->display & BASE_VAL64_STRING0x00000400)
10476 | return try_val64_to_str(value, (const val64_string *) hfinfo->strings);
10477 |
10478 | if (hfinfo->display & BASE_UNIT_STRING0x00001000)
10479 | return unit_name_string_get_value(value, (const struct unit_name_string*) hfinfo->strings);
10480 |
10481 | return try_val_to_str(value, (const value_string *) hfinfo->strings);
10482 | }
10483 |
10484 | static const char *
10485 | hf_try_val64_to_str(uint64_t value, const header_field_info *hfinfo)
10486 | {
10487 | if (hfinfo->display & BASE_VAL64_STRING0x00000400) {
10488 | if (hfinfo->display & BASE_EXT_STRING0x00000200)
10489 | return try_val64_to_str_ext(value, (val64_string_ext *) hfinfo->strings);
10490 | else
10491 | return try_val64_to_str(value, (const val64_string *) hfinfo->strings);
10492 | }
10493 |
10494 | if (hfinfo->display & BASE_RANGE_STRING0x00000100)
10495 | return try_rval64_to_str(value, (const range_string *) hfinfo->strings);
10496 |
10497 | if (hfinfo->display & BASE_UNIT_STRING0x00001000)
10498 | return unit_name_string_get_value64(value, (const struct unit_name_string*) hfinfo->strings);
10499 |
10500 | /* If this is reached somebody registered a 64-bit field with a 32-bit
10501 | * value-string, which isn't right. */
10502 | REPORT_DISSECTOR_BUG("field %s is a 64-bit field with a 32-bit value_string",proto_report_dissector_bug("field %s is a 64-bit field with a 32-bit value_string" , hfinfo->abbrev)
10503 | hfinfo->abbrev)proto_report_dissector_bug("field %s is a 64-bit field with a 32-bit value_string" , hfinfo->abbrev);
10504 |
10505 | /* This is necessary to squelch MSVC errors; is there
10506 | any way to tell it that DISSECTOR_ASSERT_NOT_REACHED()
10507 | never returns? */
10508 | return NULL((void*)0);
10509 | }
10510 |
10511 | static const char *
10512 | hf_try_double_val_to_str(double value, const header_field_info *hfinfo)
10513 | {
10514 | if (hfinfo->display & BASE_UNIT_STRING0x00001000)
10515 | return unit_name_string_get_double(value, (const struct unit_name_string*)hfinfo->strings);
10516 |
10517 | REPORT_DISSECTOR_BUG("field %s (FT_DOUBLE) has no base_unit_string", hfinfo->abbrev)proto_report_dissector_bug("field %s (FT_DOUBLE) has no base_unit_string" , hfinfo->abbrev);
10518 |
10519 | /* This is necessary to squelch MSVC errors; is there
10520 | any way to tell it that DISSECTOR_ASSERT_NOT_REACHED()
10521 | never returns? */
10522 | return NULL((void*)0);
10523 | }
10524 |
10525 | static const char *
10526 | hf_try_val_to_str_const(uint32_t value, const header_field_info *hfinfo, const char *unknown_str)
10527 | {
10528 | const char *str = hf_try_val_to_str(value, hfinfo);
10529 |
10530 | return (str) ? str : unknown_str;
10531 | }
10532 |
10533 | static const char *
10534 | hf_try_val64_to_str_const(uint64_t value, const header_field_info *hfinfo, const char *unknown_str)
10535 | {
10536 | const char *str = hf_try_val64_to_str(value, hfinfo);
10537 |
10538 | return (str) ? str : unknown_str;
10539 | }
10540 |
10541 | /* Fills data for bitfield chars with val_strings */
10542 | static void
10543 | fill_label_bitfield_char(const field_info *fi, char *label_str, size_t *value_pos)
10544 | {
10545 | char *p;
10546 | int bitfield_byte_length, bitwidth;
10547 | uint32_t unshifted_value;
10548 | uint32_t value;
10549 |
10550 | char buf[32];
10551 | const char *out;
10552 |
10553 | const header_field_info *hfinfo = fi->hfinfo;
10554 |
10555 | /* Figure out the bit width */
10556 | bitwidth = hfinfo_container_bitwidth(hfinfo);
10557 |
10558 | /* Un-shift bits */
10559 | value = fvalue_get_uinteger(fi->value);
10560 |
10561 | unshifted_value = value;
10562 | if (hfinfo->bitmask) {
10563 | unshifted_value <<= hfinfo_bitshift(hfinfo);
10564 | }
10565 |
10566 | /* Create the bitfield first */
10567 | p = decode_bitfield_value(label_str, unshifted_value, hfinfo->bitmask, bitwidth);
10568 | bitfield_byte_length = (int) (p - label_str);
10569 |
10570 | /* Fill in the textual info using stored (shifted) value */
10571 | if (hfinfo->display == BASE_CUSTOM) {
10572 | char tmp[ITEM_LABEL_LENGTH240];
10573 | const custom_fmt_func_t fmtfunc = (const custom_fmt_func_t)hfinfo->strings;
10574 |
10575 | DISSECTOR_ASSERT(fmtfunc)((void) ((fmtfunc) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 10575, "fmtfunc"))));
10576 | fmtfunc(tmp, value);
10577 | label_fill(label_str, bitfield_byte_length, hfinfo, tmp, value_pos);
10578 | }
10579 | else if (hfinfo->strings) {
10580 | const char *val_str = hf_try_val_to_str_const(value, hfinfo, "Unknown");
10581 |
10582 | out = hfinfo_char_vals_format(hfinfo, buf, value);
10583 | if (out == NULL((void*)0)) /* BASE_NONE so don't put integer in descr */
10584 | label_fill(label_str, bitfield_byte_length, hfinfo, val_str, value_pos);
10585 | else
10586 | label_fill_descr(label_str, bitfield_byte_length, hfinfo, val_str, out, value_pos);
10587 | }
10588 | else {
10589 | out = hfinfo_char_value_format(hfinfo, buf, value);
10590 |
10591 | label_fill(label_str, bitfield_byte_length, hfinfo, out, value_pos);
10592 | }
10593 | }
10594 |
10595 | /* Fills data for bitfield ints with val_strings */
10596 | static void
10597 | fill_label_bitfield(const field_info *fi, char *label_str, size_t *value_pos, bool_Bool is_signed)
10598 | {
10599 | char *p;
10600 | int bitfield_byte_length, bitwidth;
10601 | uint32_t value, unshifted_value;
10602 | char buf[NUMBER_LABEL_LENGTH80];
10603 | const char *out;
10604 |
10605 | const header_field_info *hfinfo = fi->hfinfo;
10606 |
10607 | /* Figure out the bit width */
10608 | if (fi->flags & FI_VARINT0x00040000)
10609 | bitwidth = fi->length*8;
10610 | else
10611 | bitwidth = hfinfo_container_bitwidth(hfinfo);
10612 |
10613 | /* Un-shift bits */
10614 | if (is_signed)
10615 | value = fvalue_get_sinteger(fi->value);
10616 | else
10617 | value = fvalue_get_uinteger(fi->value);
10618 |
10619 | unshifted_value = value;
10620 | if (hfinfo->bitmask) {
10621 | unshifted_value <<= hfinfo_bitshift(hfinfo);
10622 | }
10623 |
10624 | /* Create the bitfield first */
10625 | if (fi->flags & FI_VARINT0x00040000)
10626 | p = decode_bitfield_varint_value(label_str, unshifted_value, hfinfo->bitmask, bitwidth);
10627 | else
10628 | p = decode_bitfield_value(label_str, unshifted_value, hfinfo->bitmask, bitwidth);
10629 | bitfield_byte_length = (int) (p - label_str);
10630 |
10631 | /* Fill in the textual info using stored (shifted) value */
10632 | if (hfinfo->display == BASE_CUSTOM) {
10633 | char tmp[ITEM_LABEL_LENGTH240];
10634 | const custom_fmt_func_t fmtfunc = (const custom_fmt_func_t)hfinfo->strings;
10635 |
10636 | DISSECTOR_ASSERT(fmtfunc)((void) ((fmtfunc) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 10636, "fmtfunc"))));
10637 | fmtfunc(tmp, value);
10638 | label_fill(label_str, bitfield_byte_length, hfinfo, tmp, value_pos);
10639 | }
10640 | else if (hfinfo->strings) {
10641 | const char *val_str = hf_try_val_to_str(value, hfinfo);
10642 |
10643 | out = hfinfo_number_vals_format(hfinfo, buf, value);
10644 | if (hfinfo->display & BASE_SPECIAL_VALS0x00008000) {
10645 | /*
10646 | * Unique values only display value_string string
10647 | * if there is a match. Otherwise it's just a number
10648 | */
10649 | if (val_str) {
10650 | label_fill_descr(label_str, bitfield_byte_length, hfinfo, val_str, out, value_pos);
10651 | } else {
10652 | label_fill(label_str, bitfield_byte_length, hfinfo, out, value_pos);
10653 | }
10654 | } else {
10655 | if (val_str == NULL((void*)0))
10656 | val_str = "Unknown";
10657 |
10658 | if (out == NULL((void*)0)) /* BASE_NONE so don't put integer in descr */
10659 | label_fill(label_str, bitfield_byte_length, hfinfo, val_str, value_pos);
10660 | else
10661 | label_fill_descr(label_str, bitfield_byte_length, hfinfo, val_str, out, value_pos);
10662 | }
10663 | }
10664 | else {
10665 | out = hfinfo_number_value_format(hfinfo, buf, value);
10666 |
10667 | label_fill(label_str, bitfield_byte_length, hfinfo, out, value_pos);
10668 | }
10669 | }
10670 |
10671 | static void
10672 | fill_label_bitfield64(const field_info *fi, char *label_str, size_t *value_pos, bool_Bool is_signed)
10673 | {
10674 | char *p;
10675 | int bitfield_byte_length, bitwidth;
10676 | uint64_t value, unshifted_value;
10677 | char buf[NUMBER_LABEL_LENGTH80];
10678 | const char *out;
10679 |
10680 | const header_field_info *hfinfo = fi->hfinfo;
10681 |
10682 | /* Figure out the bit width */
10683 | if (fi->flags & FI_VARINT0x00040000)
10684 | bitwidth = fi->length*8;
10685 | else
10686 | bitwidth = hfinfo_container_bitwidth(hfinfo);
10687 |
10688 | /* Un-shift bits */
10689 | if (is_signed)
10690 | value = fvalue_get_sinteger64(fi->value);
10691 | else
10692 | value = fvalue_get_uinteger64(fi->value);
10693 |
10694 | unshifted_value = value;
10695 | if (hfinfo->bitmask) {
10696 | unshifted_value <<= hfinfo_bitshift(hfinfo);
10697 | }
10698 |
10699 | /* Create the bitfield first */
10700 | if (fi->flags & FI_VARINT0x00040000)
10701 | p = decode_bitfield_varint_value(label_str, unshifted_value, hfinfo->bitmask, bitwidth);
10702 | else
10703 | p = decode_bitfield_value(label_str, unshifted_value, hfinfo->bitmask, bitwidth);
10704 | bitfield_byte_length = (int) (p - label_str);
10705 |
10706 | /* Fill in the textual info using stored (shifted) value */
10707 | if (hfinfo->display == BASE_CUSTOM) {
10708 | char tmp[ITEM_LABEL_LENGTH240];
10709 | const custom_fmt_func_64_t fmtfunc64 = (const custom_fmt_func_64_t)hfinfo->strings;
10710 |
10711 | DISSECTOR_ASSERT(fmtfunc64)((void) ((fmtfunc64) ? (void)0 : (proto_report_dissector_bug( "%s:%u: failed assertion \"%s\"", "epan/proto.c", 10711, "fmtfunc64" ))));
10712 | fmtfunc64(tmp, value);
10713 | label_fill(label_str, bitfield_byte_length, hfinfo, tmp, value_pos);
10714 | }
10715 | else if (hfinfo->strings) {
10716 | const char *val_str = hf_try_val64_to_str(value, hfinfo);
10717 |
10718 | out = hfinfo_number_vals_format64(hfinfo, buf, value);
10719 | if (hfinfo->display & BASE_SPECIAL_VALS0x00008000) {
10720 | /*
10721 | * Unique values only display value_string string
10722 | * if there is a match. Otherwise it's just a number
10723 | */
10724 | if (val_str) {
10725 | label_fill_descr(label_str, bitfield_byte_length, hfinfo, val_str, out, value_pos);
10726 | } else {
10727 | label_fill(label_str, bitfield_byte_length, hfinfo, out, value_pos);
10728 | }
10729 | } else {
10730 | if (val_str == NULL((void*)0))
10731 | val_str = "Unknown";
10732 |
10733 | if (out == NULL((void*)0)) /* BASE_NONE so don't put integer in descr */
10734 | label_fill(label_str, bitfield_byte_length, hfinfo, val_str, value_pos);
10735 | else
10736 | label_fill_descr(label_str, bitfield_byte_length, hfinfo, val_str, out, value_pos);
10737 | }
10738 | }
10739 | else {
10740 | out = hfinfo_number_value_format64(hfinfo, buf, value);
10741 |
10742 | label_fill(label_str, bitfield_byte_length, hfinfo, out, value_pos);
10743 | }
10744 | }
10745 |
10746 | static void
10747 | fill_label_char(const field_info *fi, char *label_str, size_t *value_pos)
10748 | {
10749 | const header_field_info *hfinfo = fi->hfinfo;
10750 | uint32_t value;
10751 |
10752 | char buf[32];
10753 | const char *out;
10754 |
10755 | value = fvalue_get_uinteger(fi->value);
10756 |
10757 | /* Fill in the textual info */
10758 | if (hfinfo->display == BASE_CUSTOM) {
10759 | char tmp[ITEM_LABEL_LENGTH240];
10760 | const custom_fmt_func_t fmtfunc = (const custom_fmt_func_t)hfinfo->strings;
10761 |
10762 | DISSECTOR_ASSERT(fmtfunc)((void) ((fmtfunc) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 10762, "fmtfunc"))));
10763 | fmtfunc(tmp, value);
10764 | label_fill(label_str, 0, hfinfo, tmp, value_pos);
10765 | }
10766 | else if (hfinfo->strings) {
10767 | const char *val_str = hf_try_val_to_str_const(value, hfinfo, "Unknown");
10768 |
10769 | out = hfinfo_char_vals_format(hfinfo, buf, value);
10770 | label_fill_descr(label_str, 0, hfinfo, val_str, out, value_pos);
10771 | }
10772 | else {
10773 | out = hfinfo_char_value_format(hfinfo, buf, value);
10774 |
10775 | label_fill(label_str, 0, hfinfo, out, value_pos);
10776 | }
10777 | }
10778 |
10779 | static void
10780 | fill_label_number(const field_info *fi, char *label_str, size_t *value_pos, bool_Bool is_signed)
10781 | {
10782 | const header_field_info *hfinfo = fi->hfinfo;
10783 | uint32_t value;
10784 |
10785 | char buf[NUMBER_LABEL_LENGTH80];
10786 | const char *out;
10787 |
10788 | if (is_signed)
10789 | value = fvalue_get_sinteger(fi->value);
10790 | else
10791 | value = fvalue_get_uinteger(fi->value);
10792 |
10793 | /* Fill in the textual info */
10794 | if (hfinfo->display == BASE_CUSTOM) {
10795 | char tmp[ITEM_LABEL_LENGTH240];
10796 | const custom_fmt_func_t fmtfunc = (const custom_fmt_func_t)hfinfo->strings;
10797 |
10798 | DISSECTOR_ASSERT(fmtfunc)((void) ((fmtfunc) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 10798, "fmtfunc"))));
10799 | fmtfunc(tmp, value);
10800 | label_fill(label_str, 0, hfinfo, tmp, value_pos);
10801 | }
10802 | else if (hfinfo->strings && hfinfo->type != FT_FRAMENUM) {
10803 | /*
10804 | * It makes no sense to have a value-string table for a
10805 | * frame-number field - they're just integers giving
10806 | * the ordinal frame number.
10807 | */
10808 | const char *val_str = hf_try_val_to_str(value, hfinfo);
10809 |
10810 | out = hfinfo_number_vals_format(hfinfo, buf, value);
10811 | if (hfinfo->display & BASE_SPECIAL_VALS0x00008000) {
10812 | /*
10813 | * Unique values only display value_string string
10814 | * if there is a match. Otherwise it's just a number
10815 | */
10816 | if (val_str) {
10817 | label_fill_descr(label_str, 0, hfinfo, val_str, out, value_pos);
10818 | } else {
10819 | label_fill(label_str, 0, hfinfo, out, value_pos);
10820 | }
10821 | } else {
10822 | if (val_str == NULL((void*)0))
10823 | val_str = "Unknown";
10824 |
10825 | if (out == NULL((void*)0)) /* BASE_NONE so don't put integer in descr */
10826 | label_fill(label_str, 0, hfinfo, val_str, value_pos);
10827 | else
10828 | label_fill_descr(label_str, 0, hfinfo, val_str, out, value_pos);
10829 | }
10830 | }
10831 | else if (IS_BASE_PORT(hfinfo->display)(((hfinfo->display)==BASE_PT_UDP||(hfinfo->display)==BASE_PT_TCP ||(hfinfo->display)==BASE_PT_DCCP||(hfinfo->display)==BASE_PT_SCTP ))) {
10832 | char tmp[ITEM_LABEL_LENGTH240];
10833 |
10834 | port_with_resolution_to_str_buf(tmp, sizeof(tmp),
10835 | display_to_port_type((field_display_e)hfinfo->display), value);
10836 | label_fill(label_str, 0, hfinfo, tmp, value_pos);
10837 | }
10838 | else {
10839 | out = hfinfo_number_value_format(hfinfo, buf, value);
10840 |
10841 | label_fill(label_str, 0, hfinfo, out, value_pos);
10842 | }
10843 | }
10844 |
10845 | static void
10846 | fill_label_number64(const field_info *fi, char *label_str, size_t *value_pos, bool_Bool is_signed)
10847 | {
10848 | const header_field_info *hfinfo = fi->hfinfo;
10849 | uint64_t value;
10850 |
10851 | char buf[NUMBER_LABEL_LENGTH80];
10852 | const char *out;
10853 |
10854 | if (is_signed)
10855 | value = fvalue_get_sinteger64(fi->value);
10856 | else
10857 | value = fvalue_get_uinteger64(fi->value);
10858 |
10859 | /* Fill in the textual info */
10860 | if (hfinfo->display == BASE_CUSTOM) {
10861 | char tmp[ITEM_LABEL_LENGTH240];
10862 | const custom_fmt_func_64_t fmtfunc64 = (const custom_fmt_func_64_t)hfinfo->strings;
10863 |
10864 | DISSECTOR_ASSERT(fmtfunc64)((void) ((fmtfunc64) ? (void)0 : (proto_report_dissector_bug( "%s:%u: failed assertion \"%s\"", "epan/proto.c", 10864, "fmtfunc64" ))));
10865 | fmtfunc64(tmp, value);
10866 | label_fill(label_str, 0, hfinfo, tmp, value_pos);
10867 | }
10868 | else if (hfinfo->strings) {
10869 | const char *val_str = hf_try_val64_to_str(value, hfinfo);
10870 |
10871 | out = hfinfo_number_vals_format64(hfinfo, buf, value);
10872 | if (hfinfo->display & BASE_SPECIAL_VALS0x00008000) {
10873 | /*
10874 | * Unique values only display value_string string
10875 | * if there is a match. Otherwise it's just a number
10876 | */
10877 | if (val_str) {
10878 | label_fill_descr(label_str, 0, hfinfo, val_str, out, value_pos);
10879 | } else {
10880 | label_fill(label_str, 0, hfinfo, out, value_pos);
10881 | }
10882 | } else {
10883 | if (val_str == NULL((void*)0))
10884 | val_str = "Unknown";
10885 |
10886 | if (out == NULL((void*)0)) /* BASE_NONE so don't put integer in descr */
10887 | label_fill(label_str, 0, hfinfo, val_str, value_pos);
10888 | else
10889 | label_fill_descr(label_str, 0, hfinfo, val_str, out, value_pos);
10890 | }
10891 | }
10892 | else {
10893 | out = hfinfo_number_value_format64(hfinfo, buf, value);
10894 |
10895 | label_fill(label_str, 0, hfinfo, out, value_pos);
10896 | }
10897 | }
10898 |
10899 | static size_t
10900 | fill_display_label_float(const field_info *fi, char *label_str, const int label_str_size)
10901 | {
10902 | int display;
10903 | int n;
10904 | double value;
10905 |
10906 | if (label_str_size < 12) {
10907 | /* Not enough room to write an entire floating point value. */
10908 | return 0;
10909 | }
10910 |
10911 | display = FIELD_DISPLAY(fi->hfinfo->display)((fi->hfinfo->display) & 0xFF);
10912 | value = fvalue_get_floating(fi->value);
10913 |
10914 | if (display == BASE_CUSTOM) {
10915 | const custom_fmt_func_double_t fmtfunc = (const custom_fmt_func_double_t)fi->hfinfo->strings;
10916 | DISSECTOR_ASSERT(fmtfunc)((void) ((fmtfunc) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 10916, "fmtfunc"))));
10917 | fmtfunc(label_str, value);
10918 | return strlen(label_str);
10919 | }
10920 |
10921 | switch (display) {
10922 | case BASE_NONE:
10923 | if (fi->hfinfo->type == FT_FLOAT) {
10924 | n = snprintf(label_str, label_str_size, "%.*g", FLT_DIG6, value);
10925 | } else {
10926 | n = (int)strlen(dtoa_g_fmt(label_str, value));
10927 | }
10928 | break;
10929 | case BASE_DEC:
10930 | n = snprintf(label_str, label_str_size, "%f", value);
10931 | break;
10932 | case BASE_HEX:
10933 | n = snprintf(label_str, label_str_size, "%a", value);
10934 | break;
10935 | case BASE_EXP:
10936 | n = snprintf(label_str, label_str_size, "%e", value);
10937 | break;
10938 | default:
10939 | ws_assert_not_reached()ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 10939 , __func__, "assertion \"not reached\" failed");
10940 | }
10941 | if (n < 0) {
10942 | return 0; /* error */
10943 | }
10944 | if ((fi->hfinfo->strings) && (fi->hfinfo->display & BASE_UNIT_STRING0x00001000)) {
10945 | const char *hf_str_val;
10946 | hf_str_val = hf_try_double_val_to_str(value, fi->hfinfo);
10947 | n += proto_strlcpy(label_str + n, hf_str_val, label_str_size - n);
10948 | }
10949 | if (n > label_str_size) {
10950 | ws_warning("label length too small")do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 10950, __func__, "label length too small"); } } while (0);
10951 | return strlen(label_str);
10952 | }
10953 |
10954 | return n;
10955 | }
10956 |
10957 | void
10958 | fill_label_float(const field_info *fi, char *label_str, size_t *value_pos)
10959 | {
10960 | char tmp[ITEM_LABEL_LENGTH240];
10961 |
10962 | fill_display_label_float(fi, tmp, ITEM_LABEL_LENGTH240);
10963 | label_fill(label_str, 0, fi->hfinfo, tmp, value_pos);
10964 | }
10965 |
10966 | static size_t
10967 | fill_display_label_ieee_11073_float(const field_info *fi, char *label_str, const int label_str_size)
10968 | {
10969 | int display;
10970 | size_t pos = 0;
10971 | double value;
10972 | char* tmp_str;
10973 |
10974 | if (label_str_size < 12) {
10975 | /* Not enough room to write an entire floating point value. */
10976 | return 0;
10977 | }
10978 |
10979 | display = FIELD_DISPLAY(fi->hfinfo->display)((fi->hfinfo->display) & 0xFF);
10980 | tmp_str = fvalue_to_string_repr(NULL((void*)0), fi->value, FTREPR_DISPLAY, display);
10981 | pos = label_concat(label_str, pos, (const uint8_t*)tmp_str)ws_label_strcpy(label_str, 240, pos, (const uint8_t*)tmp_str, 0);
10982 | wmem_free(NULL((void*)0), tmp_str);
10983 |
10984 | if ((fi->hfinfo->strings) && (fi->hfinfo->display & BASE_UNIT_STRING0x00001000)) {
10985 | const char *hf_str_val;
10986 | fvalue_to_double(fi->value, &value);
10987 | hf_str_val = unit_name_string_get_double(value, (const struct unit_name_string*)fi->hfinfo->strings);
10988 | pos = label_concat(label_str, pos, (const uint8_t*)hf_str_val)ws_label_strcpy(label_str, 240, pos, (const uint8_t*)hf_str_val , 0);
10989 | }
10990 | if ((int)pos > label_str_size) {
10991 | ws_warning("label length too small")do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 10991, __func__, "label length too small"); } } while (0);
10992 | return strlen(label_str);
10993 | }
10994 |
10995 | return pos;
10996 | }
10997 |
10998 | void
10999 | fill_label_ieee_11073_float(const field_info *fi, char *label_str, size_t *value_pos)
11000 | {
11001 | char tmp[ITEM_LABEL_LENGTH240];
11002 |
11003 | fill_display_label_ieee_11073_float(fi, tmp, ITEM_LABEL_LENGTH240);
11004 | label_fill(label_str, 0, fi->hfinfo, tmp, value_pos);
11005 | }
11006 |
11007 | int
11008 | hfinfo_bitshift(const header_field_info *hfinfo)
11009 | {
11010 | return ws_ctz(hfinfo->bitmask);
11011 | }
11012 |
11013 |
11014 | static int
11015 | hfinfo_bitoffset(const header_field_info *hfinfo)
11016 | {
11017 | if (!hfinfo->bitmask) {
11018 | return 0;
11019 | }
11020 |
11021 | /* ilog2 = first set bit, counting 0 as the last bit; we want 0
11022 | * as the first bit */
11023 | return hfinfo_container_bitwidth(hfinfo) - 1 - ws_ilog2(hfinfo->bitmask);
11024 | }
11025 |
11026 | static int
11027 | hfinfo_mask_bitwidth(const header_field_info *hfinfo)
11028 | {
11029 | if (!hfinfo->bitmask) {
11030 | return 0;
11031 | }
11032 |
11033 | /* ilog2 = first set bit, ctz = last set bit */
11034 | return ws_ilog2(hfinfo->bitmask) - ws_ctz(hfinfo->bitmask) + 1;
11035 | }
11036 |
11037 | static int
11038 | hfinfo_type_bitwidth(enum ftenum type)
11039 | {
11040 | int bitwidth = 0;
11041 |
11042 | switch (type) {
11043 | case FT_CHAR:
11044 | case FT_UINT8:
11045 | case FT_INT8:
11046 | bitwidth = 8;
11047 | break;
11048 | case FT_UINT16:
11049 | case FT_INT16:
11050 | bitwidth = 16;
11051 | break;
11052 | case FT_UINT24:
11053 | case FT_INT24:
11054 | bitwidth = 24;
11055 | break;
11056 | case FT_UINT32:
11057 | case FT_INT32:
11058 | bitwidth = 32;
11059 | break;
11060 | case FT_UINT40:
11061 | case FT_INT40:
11062 | bitwidth = 40;
11063 | break;
11064 | case FT_UINT48:
11065 | case FT_INT48:
11066 | bitwidth = 48;
11067 | break;
11068 | case FT_UINT56:
11069 | case FT_INT56:
11070 | bitwidth = 56;
11071 | break;
11072 | case FT_UINT64:
11073 | case FT_INT64:
11074 | bitwidth = 64;
11075 | break;
11076 | default:
11077 | DISSECTOR_ASSERT_NOT_REACHED()(proto_report_dissector_bug("%s:%u: failed assertion \"DISSECTOR_ASSERT_NOT_REACHED\"" , "epan/proto.c", 11077));
11078 | ;
11079 | }
11080 | return bitwidth;
11081 | }
11082 |
11083 |
11084 | static int
11085 | hfinfo_container_bitwidth(const header_field_info *hfinfo)
11086 | {
11087 | if (!hfinfo->bitmask) {
11088 | return 0;
11089 | }
11090 |
11091 | if (hfinfo->type == FT_BOOLEAN) {
11092 | return hfinfo->display; /* hacky? :) */
11093 | }
11094 |
11095 | return hfinfo_type_bitwidth(hfinfo->type);
11096 | }
11097 |
11098 | static int
11099 | hfinfo_hex_digits(const header_field_info *hfinfo)
11100 | {
11101 | int bitwidth;
11102 |
11103 | /* If we have a bitmask, hfinfo->type is the width of the container, so not
11104 | * appropriate to determine the number of hex digits for the field.
11105 | * So instead, we compute it from the bitmask.
11106 | */
11107 | if (hfinfo->bitmask != 0) {
11108 | bitwidth = hfinfo_mask_bitwidth(hfinfo);
11109 | } else {
11110 | bitwidth = hfinfo_type_bitwidth(hfinfo->type);
11111 | }
11112 |
11113 | /* Divide by 4, rounding up, to get number of hex digits. */
11114 | return (bitwidth + 3) / 4;
11115 | }
11116 |
11117 | const char *
11118 | hfinfo_char_value_format_display(int display, char buf[7], uint32_t value)
11119 | {
11120 | char *ptr = &buf[6];
11121 | static const char hex_digits[16] =
11122 | { '0', '1', '2', '3', '4', '5', '6', '7',
11123 | '8', '9', 'a', 'b', 'c', 'd', 'e', 'f' };
11124 |
11125 | *ptr = '\0';
11126 | *(--ptr) = '\'';
11127 | /* Properly format value */
11128 | if (g_ascii_isprint(value)((g_ascii_table[(guchar) (value)] & G_ASCII_PRINT) != 0)) {
11129 | /*
11130 | * Printable, so just show the character, and, if it needs
11131 | * to be escaped, escape it.
11132 | */
11133 | *(--ptr) = value;
11134 | if (value == '\\' || value == '\'')
11135 | *(--ptr) = '\\';
11136 | } else {
11137 | /*
11138 | * Non-printable; show it as an escape sequence.
11139 | */
11140 | switch (value) {
11141 |
11142 | case '\0':
11143 | /*
11144 | * Show a NUL with only one digit.
11145 | */
11146 | *(--ptr) = '0';
11147 | break;
11148 |
11149 | case '\a':
11150 | case '\b':
11151 | case '\f':
11152 | case '\n':
11153 | case '\r':
11154 | case '\t':
11155 | case '\v':
11156 | *(--ptr) = value - '\a' + 'a';
11157 | break;
11158 |
11159 | default:
11160 | switch (FIELD_DISPLAY(display)((display) & 0xFF)) {
11161 |
11162 | case BASE_OCT:
11163 | *(--ptr) = (value & 0x7) + '0';
11164 | value >>= 3;
11165 | *(--ptr) = (value & 0x7) + '0';
11166 | value >>= 3;
11167 | *(--ptr) = (value & 0x7) + '0';
11168 | break;
11169 |
11170 | case BASE_HEX:
11171 | *(--ptr) = hex_digits[value & 0x0F];
11172 | value >>= 4;
11173 | *(--ptr) = hex_digits[value & 0x0F];
11174 | *(--ptr) = 'x';
11175 | break;
11176 |
11177 | default:
11178 | REPORT_DISSECTOR_BUG("Invalid base: %d", FIELD_DISPLAY(display))proto_report_dissector_bug("Invalid base: %d", ((display) & 0xFF));
11179 | }
11180 | }
11181 | *(--ptr) = '\\';
11182 | }
11183 | *(--ptr) = '\'';
11184 | return ptr;
11185 | }
11186 |
11187 | static const char *
11188 | hfinfo_number_value_format_display(const header_field_info *hfinfo, int display, char buf[NUMBER_LABEL_LENGTH80], uint32_t value)
11189 | {
11190 | char *ptr = &buf[NUMBER_LABEL_LENGTH80-1];
11191 | bool_Bool isint = FT_IS_INT(hfinfo->type)(((hfinfo->type) == FT_INT8 || (hfinfo->type) == FT_INT16 || (hfinfo->type) == FT_INT24 || (hfinfo->type) == FT_INT32 ) || ((hfinfo->type) == FT_INT40 || (hfinfo->type) == FT_INT48 || (hfinfo->type) == FT_INT56 || (hfinfo->type) == FT_INT64 ));
11192 |
11193 | *ptr = '\0';
11194 | /* Properly format value */
11195 | switch (FIELD_DISPLAY(display)((display) & 0xFF)) {
11196 | case BASE_DEC:
11197 | return isint ? int_to_str_back(ptr, (int32_t) value) : uint_to_str_back(ptr, value);
11198 |
11199 | case BASE_DEC_HEX:
11200 | *(--ptr) = ')';
11201 | ptr = hex_to_str_back_len(ptr, value, hfinfo_hex_digits(hfinfo));
11202 | *(--ptr) = '(';
11203 | *(--ptr) = ' ';
11204 | ptr = isint ? int_to_str_back(ptr, (int32_t) value) : uint_to_str_back(ptr, value);
11205 | return ptr;
11206 |
11207 | case BASE_OCT:
11208 | return oct_to_str_back(ptr, value);
11209 |
11210 | case BASE_HEX:
11211 | return hex_to_str_back_len(ptr, value, hfinfo_hex_digits(hfinfo));
11212 |
11213 | case BASE_HEX_DEC:
11214 | *(--ptr) = ')';
11215 | ptr = isint ? int_to_str_back(ptr, (int32_t) value) : uint_to_str_back(ptr, value);
11216 | *(--ptr) = '(';
11217 | *(--ptr) = ' ';
11218 | ptr = hex_to_str_back_len(ptr, value, hfinfo_hex_digits(hfinfo));
11219 | return ptr;
11220 |
11221 | case BASE_PT_UDP:
11222 | case BASE_PT_TCP:
11223 | case BASE_PT_DCCP:
11224 | case BASE_PT_SCTP:
11225 | port_with_resolution_to_str_buf(buf, NUMBER_LABEL_LENGTH80,
11226 | display_to_port_type((field_display_e)display), value);
11227 | return buf;
11228 | case BASE_OUI:
11229 | {
11230 | uint8_t p_oui[3];
11231 | const char *manuf_name;
11232 |
11233 | p_oui[0] = value >> 16 & 0xFF;
11234 | p_oui[1] = value >> 8 & 0xFF;
11235 | p_oui[2] = value & 0xFF;
11236 |
11237 | /* Attempt an OUI lookup. */
11238 | manuf_name = uint_get_manuf_name_if_known(value);
11239 | if (manuf_name == NULL((void*)0)) {
11240 | /* Could not find an OUI. */
11241 | snprintf(buf, NUMBER_LABEL_LENGTH80, "%02x:%02x:%02x", p_oui[0], p_oui[1], p_oui[2]);
11242 | }
11243 | else {
11244 | /* Found an address string. */
11245 | snprintf(buf, NUMBER_LABEL_LENGTH80, "%02x:%02x:%02x (%s)", p_oui[0], p_oui[1], p_oui[2], manuf_name);
11246 | }
11247 | return buf;
11248 | }
11249 |
11250 | default:
11251 | REPORT_DISSECTOR_BUG("Invalid base: %d", FIELD_DISPLAY(display))proto_report_dissector_bug("Invalid base: %d", ((display) & 0xFF));
11252 | }
11253 | return ptr;
11254 | }
11255 |
11256 | static const char *
11257 | hfinfo_number_value_format_display64(const header_field_info *hfinfo, int display, char buf[NUMBER_LABEL_LENGTH80], uint64_t value)
11258 | {
11259 | char *ptr = &buf[NUMBER_LABEL_LENGTH80-1];
11260 | bool_Bool isint = FT_IS_INT(hfinfo->type)(((hfinfo->type) == FT_INT8 || (hfinfo->type) == FT_INT16 || (hfinfo->type) == FT_INT24 || (hfinfo->type) == FT_INT32 ) || ((hfinfo->type) == FT_INT40 || (hfinfo->type) == FT_INT48 || (hfinfo->type) == FT_INT56 || (hfinfo->type) == FT_INT64 ));
11261 |
11262 | *ptr = '\0';
11263 | /* Properly format value */
11264 | switch (FIELD_DISPLAY(display)((display) & 0xFF)) {
11265 | case BASE_DEC:
11266 | return isint ? int64_to_str_back(ptr, (int64_t) value) : uint64_to_str_back(ptr, value);
11267 |
11268 | case BASE_DEC_HEX:
11269 | *(--ptr) = ')';
11270 | ptr = hex64_to_str_back_len(ptr, value, hfinfo_hex_digits(hfinfo));
11271 | *(--ptr) = '(';
11272 | *(--ptr) = ' ';
11273 | ptr = isint ? int64_to_str_back(ptr, (int64_t) value) : uint64_to_str_back(ptr, value);
11274 | return ptr;
11275 |
11276 | case BASE_OCT:
11277 | return oct64_to_str_back(ptr, value);
11278 |
11279 | case BASE_HEX:
11280 | return hex64_to_str_back_len(ptr, value, hfinfo_hex_digits(hfinfo));
11281 |
11282 | case BASE_HEX_DEC:
11283 | *(--ptr) = ')';
11284 | ptr = isint ? int64_to_str_back(ptr, (int64_t) value) : uint64_to_str_back(ptr, value);
11285 | *(--ptr) = '(';
11286 | *(--ptr) = ' ';
11287 | ptr = hex64_to_str_back_len(ptr, value, hfinfo_hex_digits(hfinfo));
11288 | return ptr;
11289 |
11290 | default:
11291 | REPORT_DISSECTOR_BUG("Invalid base: %d", FIELD_DISPLAY(display))proto_report_dissector_bug("Invalid base: %d", ((display) & 0xFF));
11292 | }
11293 |
11294 | return ptr;
11295 | }
11296 |
11297 | static const char *
11298 | hfinfo_number_value_format(const header_field_info *hfinfo, char buf[NUMBER_LABEL_LENGTH80], uint32_t value)
11299 | {
11300 | int display = hfinfo->display;
11301 |
11302 | if (hfinfo->type == FT_FRAMENUM) {
11303 | /*
11304 | * Frame numbers are always displayed in decimal.
11305 | */
11306 | display = BASE_DEC;
11307 | }
11308 |
11309 | return hfinfo_number_value_format_display(hfinfo, display, buf, value);
11310 | }
11311 |
11312 | static const char *
11313 | hfinfo_number_value_format64(const header_field_info *hfinfo, char buf[NUMBER_LABEL_LENGTH80], uint64_t value)
11314 | {
11315 | int display = hfinfo->display;
11316 |
11317 | if (hfinfo->type == FT_FRAMENUM) {
11318 | /*
11319 | * Frame numbers are always displayed in decimal.
11320 | */
11321 | display = BASE_DEC;
11322 | }
11323 |
11324 | return hfinfo_number_value_format_display64(hfinfo, display, buf, value);
11325 | }
11326 |
11327 | static const char *
11328 | hfinfo_char_value_format(const header_field_info *hfinfo, char buf[32], uint32_t value)
11329 | {
11330 | /* Get the underlying BASE_ value */
11331 | int display = FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF);
11332 |
11333 | return hfinfo_char_value_format_display(display, buf, value);
11334 | }
11335 |
11336 | static const char *
11337 | hfinfo_numeric_value_format(const header_field_info *hfinfo, char buf[NUMBER_LABEL_LENGTH80], uint32_t value)
11338 | {
11339 | /* Get the underlying BASE_ value */
11340 | int display = FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF);
11341 |
11342 | if (hfinfo->type == FT_FRAMENUM) {
11343 | /*
11344 | * Frame numbers are always displayed in decimal.
11345 | */
11346 | display = BASE_DEC;
11347 | }
11348 |
11349 | if (IS_BASE_PORT(display)(((display)==BASE_PT_UDP||(display)==BASE_PT_TCP||(display)== BASE_PT_DCCP||(display)==BASE_PT_SCTP))) {
11350 | display = BASE_DEC;
11351 | } else if (display == BASE_OUI) {
11352 | display = BASE_HEX;
11353 | }
11354 |
11355 | switch (display) {
11356 | case BASE_NONE:
11357 | /* case BASE_DEC: */
11358 | case BASE_DEC_HEX:
11359 | case BASE_OCT: /* XXX, why we're changing BASE_OCT to BASE_DEC? */
11360 | case BASE_CUSTOM:
11361 | display = BASE_DEC;
11362 | break;
11363 |
11364 | /* case BASE_HEX: */
11365 | case BASE_HEX_DEC:
11366 | display = BASE_HEX;
11367 | break;
11368 | }
11369 |
11370 | return hfinfo_number_value_format_display(hfinfo, display, buf, value);
11371 | }
11372 |
11373 | static const char *
11374 | hfinfo_numeric_value_format64(const header_field_info *hfinfo, char buf[NUMBER_LABEL_LENGTH80], uint64_t value)
11375 | {
11376 | /* Get the underlying BASE_ value */
11377 | int display = FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF);
11378 |
11379 | if (hfinfo->type == FT_FRAMENUM) {
11380 | /*
11381 | * Frame numbers are always displayed in decimal.
11382 | */
11383 | display = BASE_DEC;
11384 | }
11385 |
11386 | switch (display) {
11387 | case BASE_NONE:
11388 | /* case BASE_DEC: */
11389 | case BASE_DEC_HEX:
11390 | case BASE_OCT: /* XXX, why we're changing BASE_OCT to BASE_DEC? */
11391 | case BASE_CUSTOM:
11392 | display = BASE_DEC;
11393 | break;
11394 |
11395 | /* case BASE_HEX: */
11396 | case BASE_HEX_DEC:
11397 | display = BASE_HEX;
11398 | break;
11399 | }
11400 |
11401 | return hfinfo_number_value_format_display64(hfinfo, display, buf, value);
11402 | }
11403 |
11404 | static const char *
11405 | hfinfo_char_vals_format(const header_field_info *hfinfo, char buf[32], uint32_t value)
11406 | {
11407 | /* Get the underlying BASE_ value */
11408 | int display = FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF);
11409 |
11410 | return hfinfo_char_value_format_display(display, buf, value);
11411 | }
11412 |
11413 | static const char *
11414 | hfinfo_number_vals_format(const header_field_info *hfinfo, char buf[NUMBER_LABEL_LENGTH80], uint32_t value)
11415 | {
11416 | /* Get the underlying BASE_ value */
11417 | int display = FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF);
11418 |
11419 | if (display == BASE_NONE)
11420 | return NULL((void*)0);
11421 |
11422 | if (display == BASE_DEC_HEX)
11423 | display = BASE_DEC;
11424 | if (display == BASE_HEX_DEC)
11425 | display = BASE_HEX;
11426 |
11427 | return hfinfo_number_value_format_display(hfinfo, display, buf, value);
11428 | }
11429 |
11430 | static const char *
11431 | hfinfo_number_vals_format64(const header_field_info *hfinfo, char buf[NUMBER_LABEL_LENGTH80], uint64_t value)
11432 | {
11433 | /* Get the underlying BASE_ value */
11434 | int display = FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF);
11435 |
11436 | if (display == BASE_NONE)
11437 | return NULL((void*)0);
11438 |
11439 | if (display == BASE_DEC_HEX)
11440 | display = BASE_DEC;
11441 | if (display == BASE_HEX_DEC)
11442 | display = BASE_HEX;
11443 |
11444 | return hfinfo_number_value_format_display64(hfinfo, display, buf, value);
11445 | }
11446 |
11447 | const char *
11448 | proto_registrar_get_name(const int n)
11449 | {
11450 | header_field_info *hfinfo;
11451 |
11452 | PROTO_REGISTRAR_GET_NTH(n, hfinfo)if((n == 0 || (unsigned)n > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 11452 , __func__, "Unregistered hf! index=%d", n); ((void) ((n > 0 && (unsigned)n < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 11452 , "n > 0 && (unsigned)n < gpa_hfinfo.len", "Unregistered hf!" )))) ; ((void) ((gpa_hfinfo.hfi[n] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 11452, "gpa_hfinfo.hfi[n] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[n];;
11453 | return hfinfo->name;
11454 | }
11455 |
11456 | const char *
11457 | proto_registrar_get_abbrev(const int n)
11458 | {
11459 | header_field_info *hfinfo;
11460 |
11461 | PROTO_REGISTRAR_GET_NTH(n, hfinfo)if((n == 0 || (unsigned)n > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 11461 , __func__, "Unregistered hf! index=%d", n); ((void) ((n > 0 && (unsigned)n < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 11461 , "n > 0 && (unsigned)n < gpa_hfinfo.len", "Unregistered hf!" )))) ; ((void) ((gpa_hfinfo.hfi[n] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 11461, "gpa_hfinfo.hfi[n] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[n];;
11462 | return hfinfo->abbrev;
11463 | }
11464 |
11465 | enum ftenum
11466 | proto_registrar_get_ftype(const int n)
11467 | {
11468 | header_field_info *hfinfo;
11469 |
11470 | PROTO_REGISTRAR_GET_NTH(n, hfinfo)if((n == 0 || (unsigned)n > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 11470 , __func__, "Unregistered hf! index=%d", n); ((void) ((n > 0 && (unsigned)n < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 11470 , "n > 0 && (unsigned)n < gpa_hfinfo.len", "Unregistered hf!" )))) ; ((void) ((gpa_hfinfo.hfi[n] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 11470, "gpa_hfinfo.hfi[n] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[n];;
11471 | return hfinfo->type;
11472 | }
11473 |
11474 | int
11475 | proto_registrar_get_parent(const int n)
11476 | {
11477 | header_field_info *hfinfo;
11478 |
11479 | PROTO_REGISTRAR_GET_NTH(n, hfinfo)if((n == 0 || (unsigned)n > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 11479 , __func__, "Unregistered hf! index=%d", n); ((void) ((n > 0 && (unsigned)n < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 11479 , "n > 0 && (unsigned)n < gpa_hfinfo.len", "Unregistered hf!" )))) ; ((void) ((gpa_hfinfo.hfi[n] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 11479, "gpa_hfinfo.hfi[n] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[n];;
11480 | return hfinfo->parent;
11481 | }
11482 |
11483 | bool_Bool
11484 | proto_registrar_is_protocol(const int n)
11485 | {
11486 | header_field_info *hfinfo;
11487 |
11488 | PROTO_REGISTRAR_GET_NTH(n, hfinfo)if((n == 0 || (unsigned)n > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 11488 , __func__, "Unregistered hf! index=%d", n); ((void) ((n > 0 && (unsigned)n < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 11488 , "n > 0 && (unsigned)n < gpa_hfinfo.len", "Unregistered hf!" )))) ; ((void) ((gpa_hfinfo.hfi[n] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 11488, "gpa_hfinfo.hfi[n] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[n];;
11489 | return (((hfinfo->id != hf_text_only) && (hfinfo->parent == -1)) ? true1 : false0);
11490 | }
11491 |
11492 | /* Returns length of field in packet (not necessarily the length
11493 | * in our internal representation, as in the case of IPv4).
11494 | * 0 means undeterminable at time of registration
11495 | * -1 means the field is not registered. */
11496 | int
11497 | proto_registrar_get_length(const int n)
11498 | {
11499 | header_field_info *hfinfo;
11500 |
11501 | PROTO_REGISTRAR_GET_NTH(n, hfinfo)if((n == 0 || (unsigned)n > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 11501 , __func__, "Unregistered hf! index=%d", n); ((void) ((n > 0 && (unsigned)n < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 11501 , "n > 0 && (unsigned)n < gpa_hfinfo.len", "Unregistered hf!" )))) ; ((void) ((gpa_hfinfo.hfi[n] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 11501, "gpa_hfinfo.hfi[n] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[n];;
11502 | return ftype_wire_size(hfinfo->type);
11503 | }
11504 |
11505 | size_t
11506 | proto_registrar_get_count(struct proto_registrar_stats *stats)
11507 | {
11508 | header_field_info *hfinfo;
11509 |
11510 | // Index zero is not used. We have to skip it.
11511 | size_t total_count = gpa_hfinfo.len - 1;
11512 | if (stats == NULL((void*)0)) {
11513 | return total_count;
11514 | }
11515 | for (uint32_t id = 1; id < gpa_hfinfo.len; id++) {
11516 | if (gpa_hfinfo.hfi[id] == NULL((void*)0)) {
11517 | stats->deregistered_count++;
11518 | continue; /* This is a deregistered protocol or header field */
11519 | }
11520 |
11521 | PROTO_REGISTRAR_GET_NTH(id, hfinfo)if((id == 0 || (unsigned)id > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 11521 , __func__, "Unregistered hf! index=%d", id); ((void) ((id > 0 && (unsigned)id < gpa_hfinfo.len) ? (void)0 : ( proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 11521, "id > 0 && (unsigned)id < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[id] != (( void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 11521, "gpa_hfinfo.hfi[id] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[id];;
11522 |
11523 | if (proto_registrar_is_protocol(id))
11524 | stats->protocol_count++;
11525 |
11526 | if (hfinfo->same_name_prev_id != -1)
11527 | stats->same_name_count++;
11528 | }
11529 |
11530 | return total_count;
11531 | }
11532 |
11533 | /* Looks for a protocol or a field in a proto_tree. Returns true if
11534 | * it exists anywhere, or false if it exists nowhere. */
11535 | bool_Bool
11536 | proto_check_for_protocol_or_field(const proto_tree* tree, const int id)
11537 | {
11538 | GPtrArray *ptrs = proto_get_finfo_ptr_array(tree, id);
11539 |
11540 | if (g_ptr_array_len(ptrs)((ptrs) ? (ptrs)->len : 0) > 0) {
11541 | return true1;
11542 | }
11543 | else {
11544 | return false0;
11545 | }
11546 | }
11547 |
11548 | /* Return GPtrArray* of field_info pointers for all hfindex that appear in tree.
11549 | * This only works if the hfindex was "primed" before the dissection
11550 | * took place, as we just pass back the already-created GPtrArray*.
11551 | * The caller should *not* free the GPtrArray*; proto_tree_free_node()
11552 | * handles that. */
11553 | GPtrArray *
11554 | proto_get_finfo_ptr_array(const proto_tree *tree, const int id)
11555 | {
11556 | if (!tree)
11557 | return NULL((void*)0);
11558 |
11559 | if (PTREE_DATA(tree)((tree)->tree_data)->interesting_hfids != NULL((void*)0))
11560 | return (GPtrArray *)g_hash_table_lookup(PTREE_DATA(tree)((tree)->tree_data)->interesting_hfids,
11561 | GINT_TO_POINTER(id)((gpointer) (glong) (id)));
11562 | else
11563 | return NULL((void*)0);
11564 | }
11565 |
11566 | bool_Bool
11567 | proto_tracking_interesting_fields(const proto_tree *tree)
11568 | {
11569 | GHashTable *interesting_hfids;
11570 |
11571 | if (!tree)
11572 | return false0;
11573 |
11574 | interesting_hfids = PTREE_DATA(tree)((tree)->tree_data)->interesting_hfids;
11575 |
11576 | return (interesting_hfids != NULL((void*)0)) && g_hash_table_size(interesting_hfids);
11577 | }
11578 |
11579 | /* Helper struct for proto_find_info() and proto_all_finfos() */
11580 | typedef struct {
11581 | GPtrArray *array;
11582 | int id;
11583 | } ffdata_t;
11584 |
11585 | /* Helper function for proto_find_info() */
11586 | static bool_Bool
11587 | find_finfo(proto_node *node, void * data)
11588 | {
11589 | field_info *fi = PNODE_FINFO(node)((node)->finfo);
11590 | if (fi && fi->hfinfo) {
11591 | if (fi->hfinfo->id == ((ffdata_t*)data)->id) {
11592 | g_ptr_array_add(((ffdata_t*)data)->array, fi);
11593 | }
11594 | }
11595 |
11596 | /* Don't stop traversing. */
11597 | return false0;
11598 | }
11599 |
11600 | /* Helper function for proto_find_first_info() */
11601 | static bool_Bool
11602 | find_first_finfo(proto_node *node, void *data)
11603 | {
11604 | field_info *fi = PNODE_FINFO(node)((node)->finfo);
11605 | if (fi && fi->hfinfo) {
11606 | if (fi->hfinfo->id == ((ffdata_t*)data)->id) {
11607 | g_ptr_array_add(((ffdata_t*)data)->array, fi);
11608 |
11609 | /* Stop traversing. */
11610 | return true1;
11611 | }
11612 | }
11613 |
11614 | /* Continue traversing. */
11615 | return false0;
11616 | }
11617 |
11618 | /* Return GPtrArray* of field_info pointers for all hfindex that appear in a tree.
11619 | * This works on any proto_tree, primed or unprimed, but actually searches
11620 | * the tree, so it is slower than using proto_get_finfo_ptr_array on a primed tree.
11621 | * The caller does need to free the returned GPtrArray with
11622 | * g_ptr_array_free(<array>, true).
11623 | */
11624 | GPtrArray *
11625 | proto_find_finfo(proto_tree *tree, const int id)
11626 | {
11627 | ffdata_t ffdata;
11628 |
11629 | ffdata.array = g_ptr_array_new();
11630 | ffdata.id = id;
11631 |
11632 | proto_tree_traverse_pre_order(tree, find_finfo, &ffdata);
11633 |
11634 | return ffdata.array;
11635 | }
11636 |
11637 | /* Return GPtrArray* of first field_info pointers for the searched hfindex that appear in a tree.
11638 | * This works on any proto_tree, primed or unprimed, but actually searches
11639 | * the tree, so it is slower than using proto_get_finfo_ptr_array on a primed tree.
11640 | * The caller does need to free the returned GPtrArray with
11641 | * g_ptr_array_free(<array>, true).
11642 | */
11643 | GPtrArray *
11644 | proto_find_first_finfo(proto_tree *tree, const int id)
11645 | {
11646 | ffdata_t ffdata;
11647 |
11648 | ffdata.array = g_ptr_array_new();
11649 | ffdata.id = id;
11650 |
11651 | proto_tree_traverse_pre_order(tree, find_first_finfo, &ffdata);
11652 |
11653 | return ffdata.array;
11654 | }
11655 |
11656 | /* Helper function for proto_all_finfos() */
11657 | static bool_Bool
11658 | every_finfo(proto_node *node, void * data)
11659 | {
11660 | field_info *fi = PNODE_FINFO(node)((node)->finfo);
11661 | if (fi && fi->hfinfo) {
11662 | g_ptr_array_add(((ffdata_t*)data)->array, fi);
11663 | }
11664 |
11665 | /* Don't stop traversing. */
11666 | return false0;
11667 | }
11668 |
11669 | /* Return GPtrArray* of field_info pointers containing all hfindexes that appear in a tree.
11670 | * The caller does need to free the returned GPtrArray with
11671 | * g_ptr_array_free(<array>, true).
11672 | */
11673 | GPtrArray *
11674 | proto_all_finfos(proto_tree *tree)
11675 | {
11676 | ffdata_t ffdata;
11677 |
11678 | /* Pre allocate enough space to hold all fields in most cases */
11679 | ffdata.array = g_ptr_array_sized_new(512);
11680 | ffdata.id = 0;
11681 |
11682 | proto_tree_traverse_pre_order(tree, every_finfo, &ffdata);
11683 |
11684 | return ffdata.array;
11685 | }
11686 |
11687 |
11688 | typedef struct {
11689 | unsigned offset;
11690 | field_info *finfo;
11691 | tvbuff_t *tvb;
11692 | } offset_search_t;
11693 |
11694 | static bool_Bool
11695 | check_for_offset(proto_node *node, void * data)
11696 | {
11697 | field_info *fi = PNODE_FINFO(node)((node)->finfo);
11698 | offset_search_t *offsearch = (offset_search_t *)data;
11699 |
11700 | /* !fi == the top most container node which holds nothing */
11701 | if (fi && !proto_item_is_hidden(node) && !proto_item_is_generated(node) && fi->ds_tvb && offsearch->tvb == fi->ds_tvb) {
11702 | if (offsearch->offset >= (unsigned) fi->start &&
11703 | offsearch->offset < (unsigned) (fi->start + fi->length)) {
11704 |
11705 | offsearch->finfo = fi;
11706 | return false0; /* keep traversing */
11707 | }
11708 | }
11709 | return false0; /* keep traversing */
11710 | }
11711 |
11712 | /* Search a proto_tree backwards (from leaves to root) looking for the field
11713 | * whose start/length occupies 'offset' */
11714 | /* XXX - I couldn't find an easy way to search backwards, so I search
11715 | * forwards, w/o stopping. Therefore, the last finfo I find will the be
11716 | * the one I want to return to the user. This algorithm is inefficient
11717 | * and could be re-done, but I'd have to handle all the children and
11718 | * siblings of each node myself. When I have more time I'll do that.
11719 | * (yeah right) */
11720 | field_info *
11721 | proto_find_field_from_offset(proto_tree *tree, unsigned offset, tvbuff_t *tvb)
11722 | {
11723 | offset_search_t offsearch;
11724 |
11725 | offsearch.offset = offset;
11726 | offsearch.finfo = NULL((void*)0);
11727 | offsearch.tvb = tvb;
11728 |
11729 | proto_tree_traverse_pre_order(tree, check_for_offset, &offsearch);
11730 |
11731 | return offsearch.finfo;
11732 | }
11733 |
11734 | typedef struct {
11735 | unsigned length;
11736 | char *buf;
11737 | } decoded_data_t;
11738 |
11739 | static bool_Bool
11740 | check_for_undecoded(proto_node *node, void * data)
11741 | {
11742 | field_info *fi = PNODE_FINFO(node)((node)->finfo);
11743 | decoded_data_t* decoded = (decoded_data_t*)data;
11744 | unsigned i;
11745 | unsigned byte;
11746 | unsigned bit;
11747 |
11748 | if (fi && fi->hfinfo->type != FT_PROTOCOL) {
11749 | for (i = fi->start; i < fi->start + fi->length && i < decoded->length; i++) {
11750 | byte = i / 8;
11751 | bit = i % 8;
11752 | decoded->buf[byte] |= (1 << bit);
11753 | }
11754 | }
11755 |
11756 | return false0;
11757 | }
11758 |
11759 | char*
11760 | proto_find_undecoded_data(proto_tree *tree, unsigned length)
11761 | {
11762 | decoded_data_t decoded;
11763 | decoded.length = length;
11764 | decoded.buf = (char*)wmem_alloc0(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool), length / 8 + 1);
11765 |
11766 | proto_tree_traverse_pre_order(tree, check_for_undecoded, &decoded);
11767 | return decoded.buf;
11768 | }
11769 |
11770 | /* Dumps the protocols in the registration database to stdout. An independent
11771 | * program can take this output and format it into nice tables or HTML or
11772 | * whatever.
11773 | *
11774 | * There is one record per line. The fields are tab-delimited.
11775 | *
11776 | * Field 1 = protocol name
11777 | * Field 2 = protocol short name
11778 | * Field 3 = protocol filter name
11779 | * Field 4 = protocol enabled
11780 | * Field 5 = protocol enabled by default
11781 | * Field 6 = protocol can toggle
11782 | */
11783 | void
11784 | proto_registrar_dump_protocols(void)
11785 | {
11786 | protocol_t *protocol;
11787 | int i;
11788 | void *cookie = NULL((void*)0);
11789 |
11790 |
11791 | i = proto_get_first_protocol(&cookie);
11792 | while (i != -1) {
11793 | protocol = find_protocol_by_id(i);
11794 | printf("%s\t%s\t%s\t%c\t%c\t%c\n",
11795 | protocol->name,
11796 | protocol->short_name,
11797 | protocol->filter_name,
11798 | (proto_is_protocol_enabled_by_default(protocol) ? 'T' : 'F'),
11799 | (proto_is_protocol_enabled(protocol) ? 'T' : 'F'),
11800 | (proto_can_toggle_protocol(protocol->proto_id) ? 'T' : 'F'));
11801 | i = proto_get_next_protocol(&cookie);
11802 | }
11803 | }
11804 |
11805 | /* Dumps the value_strings, extended value string headers, range_strings
11806 | * or true/false strings for fields that have them.
11807 | * There is one record per line. Fields are tab-delimited.
11808 | * There are four types of records: Value String, Extended Value String Header,
11809 | * Range String and True/False String. The first field, 'V', 'E', 'R' or 'T', indicates
11810 | * the type of record.
11811 | *
11812 | * Note that a record will be generated only if the value_string,... is referenced
11813 | * in a registered hfinfo entry.
11814 | *
11815 | *
11816 | * Value Strings
11817 | * -------------
11818 | * Field 1 = 'V'
11819 | * Field 2 = Field abbreviation to which this value string corresponds
11820 | * Field 3 = Integer value
11821 | * Field 4 = String
11822 | *
11823 | * Extended Value String Headers
11824 | * -----------------------------
11825 | * Field 1 = 'E'
11826 | * Field 2 = Field abbreviation to which this extended value string header corresponds
11827 | * Field 3 = Extended Value String "Name"
11828 | * Field 4 = Number of entries in the associated value_string array
11829 | * Field 5 = Access Type: "Linear Search", "Binary Search", "Direct (indexed) Access"
11830 | *
11831 | * Range Strings
11832 | * -------------
11833 | * Field 1 = 'R'
11834 | * Field 2 = Field abbreviation to which this range string corresponds
11835 | * Field 3 = Integer value: lower bound
11836 | * Field 4 = Integer value: upper bound
11837 | * Field 5 = String
11838 | *
11839 | * True/False Strings
11840 | * ------------------
11841 | * Field 1 = 'T'
11842 | * Field 2 = Field abbreviation to which this true/false string corresponds
11843 | * Field 3 = True String
11844 | * Field 4 = False String
11845 | */
11846 | void
11847 | proto_registrar_dump_values(void)
11848 | {
11849 | header_field_info *hfinfo;
11850 | int i, len, vi;
11851 | const value_string *vals;
11852 | const val64_string *vals64;
11853 | const range_string *range;
11854 | const true_false_string *tfs;
11855 | const unit_name_string *units;
11856 |
11857 | len = gpa_hfinfo.len;
11858 | for (i = 1; i < len ; i++) {
11859 | if (gpa_hfinfo.hfi[i] == NULL((void*)0))
11860 | continue; /* This is a deregistered protocol or field */
11861 |
11862 | PROTO_REGISTRAR_GET_NTH(i, hfinfo)if((i == 0 || (unsigned)i > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 11862 , __func__, "Unregistered hf! index=%d", i); ((void) ((i > 0 && (unsigned)i < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 11862 , "i > 0 && (unsigned)i < gpa_hfinfo.len", "Unregistered hf!" )))) ; ((void) ((gpa_hfinfo.hfi[i] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 11862, "gpa_hfinfo.hfi[i] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[i];;
11863 |
11864 | if (hfinfo->id == hf_text_only) {
11865 | continue;
11866 | }
11867 |
11868 | /* ignore protocols */
11869 | if (proto_registrar_is_protocol(i)) {
11870 | continue;
11871 | }
11872 | /* process header fields */
11873 | #if 0 /* XXX: We apparently allow fields with the same name but with differing "strings" content */
11874 | /*
11875 | * If this field isn't at the head of the list of
11876 | * fields with this name, skip this field - all
11877 | * fields with the same name are really just versions
11878 | * of the same field stored in different bits, and
11879 | * should have the same type/radix/value list, and
11880 | * just differ in their bit masks. (If a field isn't
11881 | * a bitfield, but can be, say, 1 or 2 bytes long,
11882 | * it can just be made FT_UINT16, meaning the
11883 | * *maximum* length is 2 bytes, and be used
11884 | * for all lengths.)
11885 | */
11886 | if (hfinfo->same_name_prev_id != -1)
11887 | continue;
11888 | #endif
11889 | vals = NULL((void*)0);
11890 | vals64 = NULL((void*)0);
11891 | range = NULL((void*)0);
11892 | tfs = NULL((void*)0);
11893 | units = NULL((void*)0);
11894 |
11895 | if (hfinfo->strings != NULL((void*)0)) {
11896 | if (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF) != BASE_CUSTOM &&
11897 | (hfinfo->type == FT_CHAR ||
11898 | hfinfo->type == FT_UINT8 ||
11899 | hfinfo->type == FT_UINT16 ||
11900 | hfinfo->type == FT_UINT24 ||
11901 | hfinfo->type == FT_UINT32 ||
11902 | hfinfo->type == FT_UINT40 ||
11903 | hfinfo->type == FT_UINT48 ||
11904 | hfinfo->type == FT_UINT56 ||
11905 | hfinfo->type == FT_UINT64 ||
11906 | hfinfo->type == FT_INT8 ||
11907 | hfinfo->type == FT_INT16 ||
11908 | hfinfo->type == FT_INT24 ||
11909 | hfinfo->type == FT_INT32 ||
11910 | hfinfo->type == FT_INT40 ||
11911 | hfinfo->type == FT_INT48 ||
11912 | hfinfo->type == FT_INT56 ||
11913 | hfinfo->type == FT_INT64 ||
11914 | hfinfo->type == FT_FLOAT ||
11915 | hfinfo->type == FT_DOUBLE)) {
11916 |
11917 | if (hfinfo->display & BASE_RANGE_STRING0x00000100) {
11918 | range = (const range_string *)hfinfo->strings;
11919 | } else if (hfinfo->display & BASE_EXT_STRING0x00000200) {
11920 | if (hfinfo->display & BASE_VAL64_STRING0x00000400) {
11921 | vals64 = VAL64_STRING_EXT_VS_P((const val64_string_ext *)hfinfo->strings)((const val64_string_ext *)hfinfo->strings)->_vs_p;
11922 | } else {
11923 | vals = VALUE_STRING_EXT_VS_P((const value_string_ext *)hfinfo->strings)((const value_string_ext *)hfinfo->strings)->_vs_p;
11924 | }
11925 | } else if (hfinfo->display & BASE_VAL64_STRING0x00000400) {
11926 | vals64 = (const val64_string *)hfinfo->strings;
11927 | } else if (hfinfo->display & BASE_UNIT_STRING0x00001000) {
11928 | units = (const unit_name_string *)hfinfo->strings;
11929 | } else {
11930 | vals = (const value_string *)hfinfo->strings;
11931 | }
11932 | }
11933 | else if (hfinfo->type == FT_BOOLEAN) {
11934 | tfs = (const struct true_false_string *)hfinfo->strings;
11935 | }
11936 | }
11937 |
11938 | /* Print value strings? */
11939 | if (vals) {
11940 | if (hfinfo->display & BASE_EXT_STRING0x00000200) {
11941 | if (hfinfo->display & BASE_VAL64_STRING0x00000400) {
11942 | val64_string_ext *vse_p = (val64_string_ext *)hfinfo->strings;
11943 | if (!val64_string_ext_validate(vse_p)) {
11944 | ws_warning("Invalid val64_string_ext ptr for: %s", hfinfo->abbrev)do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 11944, __func__, "Invalid val64_string_ext ptr for: %s", hfinfo ->abbrev); } } while (0);
11945 | continue;
11946 | }
11947 | try_val64_to_str_ext(0, vse_p); /* "prime" the extended val64_string */
11948 | printf("E\t%s\t%u\t%s\t%s\n",
11949 | hfinfo->abbrev,
11950 | VAL64_STRING_EXT_VS_NUM_ENTRIES(vse_p)(vse_p)->_vs_num_entries,
11951 | VAL64_STRING_EXT_VS_NAME(vse_p)(vse_p)->_vs_name,
11952 | val64_string_ext_match_type_str(vse_p));
11953 | } else {
11954 | value_string_ext *vse_p = (value_string_ext *)hfinfo->strings;
11955 | if (!value_string_ext_validate(vse_p)) {
11956 | ws_warning("Invalid value_string_ext ptr for: %s", hfinfo->abbrev)do { if (1) { ws_log_full("Epan", LOG_LEVEL_WARNING, "epan/proto.c" , 11956, __func__, "Invalid value_string_ext ptr for: %s", hfinfo ->abbrev); } } while (0);
11957 | continue;
11958 | }
11959 | try_val_to_str_ext(0, vse_p); /* "prime" the extended value_string */
11960 | printf("E\t%s\t%u\t%s\t%s\n",
11961 | hfinfo->abbrev,
11962 | VALUE_STRING_EXT_VS_NUM_ENTRIES(vse_p)(vse_p)->_vs_num_entries,
11963 | VALUE_STRING_EXT_VS_NAME(vse_p)(vse_p)->_vs_name,
11964 | value_string_ext_match_type_str(vse_p));
11965 | }
11966 | }
11967 | vi = 0;
11968 | while (vals[vi].strptr) {
11969 | /* Print in the proper base */
11970 | if (hfinfo->type == FT_CHAR) {
11971 | if (g_ascii_isprint(vals[vi].value)((g_ascii_table[(guchar) (vals[vi].value)] & G_ASCII_PRINT ) != 0)) {
11972 | printf("V\t%s\t'%c'\t%s\n",
11973 | hfinfo->abbrev,
11974 | vals[vi].value,
11975 | vals[vi].strptr);
11976 | } else {
11977 | if (hfinfo->display == BASE_HEX) {
11978 | printf("V\t%s\t'\\x%02x'\t%s\n",
11979 | hfinfo->abbrev,
11980 | vals[vi].value,
11981 | vals[vi].strptr);
11982 | }
11983 | else {
11984 | printf("V\t%s\t'\\%03o'\t%s\n",
11985 | hfinfo->abbrev,
11986 | vals[vi].value,
11987 | vals[vi].strptr);
11988 | }
11989 | }
11990 | } else {
11991 | if (hfinfo->display == BASE_HEX) {
11992 | printf("V\t%s\t0x%x\t%s\n",
11993 | hfinfo->abbrev,
11994 | vals[vi].value,
11995 | vals[vi].strptr);
11996 | }
11997 | else {
11998 | printf("V\t%s\t%u\t%s\n",
11999 | hfinfo->abbrev,
12000 | vals[vi].value,
12001 | vals[vi].strptr);
12002 | }
12003 | }
12004 | vi++;
12005 | }
12006 | }
12007 | else if (vals64) {
12008 | vi = 0;
12009 | while (vals64[vi].strptr) {
12010 | printf("V64\t%s\t%" PRIu64"l" "u" "\t%s\n",
12011 | hfinfo->abbrev,
12012 | vals64[vi].value,
12013 | vals64[vi].strptr);
12014 | vi++;
12015 | }
12016 | }
12017 |
12018 | /* print range strings? */
12019 | else if (range) {
12020 | vi = 0;
12021 | while (range[vi].strptr) {
12022 | /* Print in the proper base */
12023 | if (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF) == BASE_HEX) {
12024 | printf("R\t%s\t0x%"PRIx64"l" "x""\t0x%"PRIx64"l" "x""\t%s\n",
12025 | hfinfo->abbrev,
12026 | range[vi].value_min,
12027 | range[vi].value_max,
12028 | range[vi].strptr);
12029 | }
12030 | else {
12031 | printf("R\t%s\t%"PRIu64"l" "u""\t%"PRIu64"l" "u""\t%s\n",
12032 | hfinfo->abbrev,
12033 | range[vi].value_min,
12034 | range[vi].value_max,
12035 | range[vi].strptr);
12036 | }
12037 | vi++;
12038 | }
12039 | }
12040 |
12041 | /* Print true/false strings? */
12042 | else if (tfs) {
12043 | printf("T\t%s\t%s\t%s\n", hfinfo->abbrev,
12044 | tfs->true_string, tfs->false_string);
12045 | }
12046 | /* Print unit strings? */
12047 | else if (units) {
12048 | printf("U\t%s\t%s\t%s\n", hfinfo->abbrev,
12049 | units->singular, units->plural ? units->plural : "(no plural)");
12050 | }
12051 | }
12052 | }
12053 |
12054 | /* Prints the number of registered fields.
12055 | * Useful for determining an appropriate value for
12056 | * PROTO_PRE_ALLOC_HF_FIELDS_MEM.
12057 | *
12058 | * Returns false if PROTO_PRE_ALLOC_HF_FIELDS_MEM is larger than or equal to
12059 | * the number of fields, true otherwise.
12060 | */
12061 | bool_Bool
12062 | proto_registrar_dump_fieldcount(void)
12063 | {
12064 | struct proto_registrar_stats stats = {0, 0, 0};
12065 | size_t total_count = proto_registrar_get_count(&stats);
12066 |
12067 | printf("There are %zu header fields registered, of which:\n"
12068 | "\t%zu are deregistered\n"
12069 | "\t%zu are protocols\n"
12070 | "\t%zu have the same name as another field\n\n",
12071 | total_count, stats.deregistered_count, stats.protocol_count,
12072 | stats.same_name_count);
12073 |
12074 | printf("%d fields were pre-allocated.\n%s", PROTO_PRE_ALLOC_HF_FIELDS_MEM(300000+5000),
12075 | (gpa_hfinfo.allocated_len > PROTO_PRE_ALLOC_HF_FIELDS_MEM(300000+5000)) ?
12076 | "* * Please increase PROTO_PRE_ALLOC_HF_FIELDS_MEM (in epan/proto.c)! * *\n\n" :
12077 | "\n");
12078 |
12079 | printf("The header field table consumes %u KiB of memory.\n",
12080 | (unsigned int)(gpa_hfinfo.allocated_len * sizeof(header_field_info *) / 1024));
12081 | printf("The fields themselves consume %u KiB of memory.\n",
12082 | (unsigned int)(gpa_hfinfo.len * sizeof(header_field_info) / 1024));
12083 |
12084 | return (gpa_hfinfo.allocated_len > PROTO_PRE_ALLOC_HF_FIELDS_MEM(300000+5000));
12085 | }
12086 |
12087 | static void
12088 | elastic_add_base_mapping(json_dumper *dumper)
12089 | {
12090 | json_dumper_set_member_name(dumper, "index_patterns");
12091 | json_dumper_begin_array(dumper);
12092 | // The index names from write_json_index() in print.c
12093 | json_dumper_value_string(dumper, "packets-*");
12094 | json_dumper_end_array(dumper);
12095 |
12096 | json_dumper_set_member_name(dumper, "settings");
12097 | json_dumper_begin_object(dumper);
12098 | json_dumper_set_member_name(dumper, "index.mapping.total_fields.limit");
12099 | json_dumper_value_anyf(dumper, "%d", 1000000);
12100 | json_dumper_end_object(dumper);
12101 | }
12102 |
12103 | static char*
12104 | ws_type_to_elastic(unsigned type)
12105 | {
12106 | switch(type) {
12107 | case FT_INT8:
12108 | return "byte";
12109 | case FT_UINT8:
12110 | case FT_INT16:
12111 | return "short";
12112 | case FT_UINT16:
12113 | case FT_INT32:
12114 | case FT_UINT24:
12115 | case FT_INT24:
12116 | return "integer";
12117 | case FT_FRAMENUM:
12118 | case FT_UINT32:
12119 | case FT_UINT40:
12120 | case FT_UINT48:
12121 | case FT_UINT56:
12122 | case FT_INT40:
12123 | case FT_INT48:
12124 | case FT_INT56:
12125 | case FT_INT64:
12126 | return "long";
12127 | case FT_UINT64:
12128 | return "unsigned long"; // ElasticSearch since 7.0, OpenSearch 2.8
12129 | case FT_FLOAT:
12130 | return "float";
12131 | case FT_DOUBLE:
12132 | case FT_RELATIVE_TIME: // "scaled_float" with "scaling_factor" 1e9 superior?
12133 | return "double";
12134 | case FT_IPv6:
12135 | case FT_IPv4:
12136 | return "ip";
12137 | case FT_ABSOLUTE_TIME:
12138 | return "date_nanos"; // This is a 64 bit integer of nanoseconds, so it does have a Y2262 problem
12139 | case FT_BOOLEAN:
12140 | return "boolean";
12141 | default:
12142 | return NULL((void*)0);
12143 | }
12144 | }
12145 |
12146 | static char*
12147 | dot_to_underscore(char* str)
12148 | {
12149 | unsigned i;
12150 | for (i = 0; i < strlen(str); i++) {
12151 | if (str[i] == '.')
12152 | str[i] = '_';
12153 | }
12154 | return str;
12155 | }
12156 |
12157 | /* Dumps a mapping file for ElasticSearch
12158 | * This is the v1 (legacy) _template API.
12159 | * At some point it may need to be updated with the composable templates
12160 | * introduced in Elasticsearch 7.8 (_index_template)
12161 | */
12162 | void
12163 | proto_registrar_dump_elastic(const char* filter)
12164 | {
12165 | header_field_info *hfinfo;
12166 | header_field_info *parent_hfinfo;
12167 | unsigned i;
12168 | bool_Bool open_object = true1;
12169 | const char* prev_proto = NULL((void*)0);
12170 | char* str;
12171 | char** protos = NULL((void*)0);
12172 | char* proto;
12173 | bool_Bool found;
12174 | unsigned j;
12175 | char* type;
12176 | char* prev_item = NULL((void*)0);
12177 |
12178 | /* We have filtering protocols. Extract them. */
12179 | if (filter) {
12180 | protos = g_strsplit(filter, ",", -1);
12181 | }
12182 |
12183 | /*
12184 | * To help tracking down the json tree, objects have been appended with a comment:
12185 | * n.label -> where n is the indentation level and label the name of the object
12186 | */
12187 |
12188 | json_dumper dumper = {
12189 | .output_file = stdoutstdout,
12190 | .flags = JSON_DUMPER_FLAGS_PRETTY_PRINT(1 << 0),
12191 | };
12192 | json_dumper_begin_object(&dumper); // 1.root
12193 | elastic_add_base_mapping(&dumper);
12194 |
12195 | json_dumper_set_member_name(&dumper, "mappings");
12196 | json_dumper_begin_object(&dumper); // 2.mappings
12197 |
12198 | json_dumper_set_member_name(&dumper, "properties");
12199 | json_dumper_begin_object(&dumper); // 3.properties
12200 | json_dumper_set_member_name(&dumper, "timestamp");
12201 | json_dumper_begin_object(&dumper); // 4.timestamp
12202 | json_dumper_set_member_name(&dumper, "type");
12203 | json_dumper_value_string(&dumper, "date");
12204 | json_dumper_end_object(&dumper); // 4.timestamp
12205 |
12206 | json_dumper_set_member_name(&dumper, "layers");
12207 | json_dumper_begin_object(&dumper); // 4.layers
12208 | json_dumper_set_member_name(&dumper, "properties");
12209 | json_dumper_begin_object(&dumper); // 5.properties
12210 |
12211 | for (i = 1; i < gpa_hfinfo.len; i++) {
12212 | if (gpa_hfinfo.hfi[i] == NULL((void*)0))
12213 | continue; /* This is a deregistered protocol or header field */
12214 |
12215 | PROTO_REGISTRAR_GET_NTH(i, hfinfo)if((i == 0 || (unsigned)i > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 12215 , __func__, "Unregistered hf! index=%d", i); ((void) ((i > 0 && (unsigned)i < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 12215 , "i > 0 && (unsigned)i < gpa_hfinfo.len", "Unregistered hf!" )))) ; ((void) ((gpa_hfinfo.hfi[i] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 12215, "gpa_hfinfo.hfi[i] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[i];;
12216 |
12217 | /*
12218 | * Skip the pseudo-field for "proto_tree_add_text()" since
12219 | * we don't want it in the list of filterable protocols.
12220 | */
12221 | if (hfinfo->id == hf_text_only)
12222 | continue;
12223 |
12224 | if (!proto_registrar_is_protocol(i)) {
12225 | PROTO_REGISTRAR_GET_NTH(hfinfo->parent, parent_hfinfo)if((hfinfo->parent == 0 || (unsigned)hfinfo->parent > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 12225 , __func__, "Unregistered hf! index=%d", hfinfo->parent); ( (void) ((hfinfo->parent > 0 && (unsigned)hfinfo ->parent < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 12225 , "hfinfo->parent > 0 && (unsigned)hfinfo->parent < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> parent] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 12225 , "gpa_hfinfo.hfi[hfinfo->parent] != ((void*)0)", "Unregistered hf!" )))) ; parent_hfinfo = gpa_hfinfo.hfi[hfinfo->parent];;
12226 |
12227 | /*
12228 | * Skip the field if filter protocols have been set and this one's
12229 | * parent is not listed.
12230 | */
12231 | if (protos) {
12232 | found = false0;
12233 | j = 0;
12234 | proto = protos[0];
12235 | while(proto) {
12236 | if (!g_strcmp0(proto, parent_hfinfo->abbrev)) {
12237 | found = true1;
12238 | break;
12239 | }
12240 | j++;
12241 | proto = protos[j];
12242 | }
12243 | if (!found)
12244 | continue;
12245 | }
12246 |
12247 | if (prev_proto && g_strcmp0(parent_hfinfo->abbrev, prev_proto)) {
12248 | json_dumper_end_object(&dumper); // 7.properties
12249 | json_dumper_end_object(&dumper); // 8.parent_hfinfo->abbrev
12250 | open_object = true1;
12251 | }
12252 |
12253 | prev_proto = parent_hfinfo->abbrev;
12254 |
12255 | if (open_object) {
12256 | json_dumper_set_member_name(&dumper, parent_hfinfo->abbrev);
12257 | json_dumper_begin_object(&dumper); // 6.parent_hfinfo->abbrev
12258 | json_dumper_set_member_name(&dumper, "properties");
12259 | json_dumper_begin_object(&dumper); // 7.properties
12260 | open_object = false0;
12261 | }
12262 | /* Skip the fields that would map into string. This is the default in elasticsearch. */
12263 | type = ws_type_to_elastic(hfinfo->type);
12264 | /* when type is NULL, we have the default mapping: string */
12265 | if (type) {
12266 | str = ws_strdup_printf("%s_%s", prev_proto, hfinfo->abbrev)wmem_strdup_printf(((void*)0), "%s_%s", prev_proto, hfinfo-> abbrev);
12267 | dot_to_underscore(str);
12268 | if (g_strcmp0(prev_item, str)) {
12269 | json_dumper_set_member_name(&dumper, str);
12270 | json_dumper_begin_object(&dumper); // 8.hfinfo->abbrev
12271 | json_dumper_set_member_name(&dumper, "type");
12272 | json_dumper_value_string(&dumper, type);
12273 | json_dumper_end_object(&dumper); // 8.hfinfo->abbrev
12274 | }
12275 | g_free(prev_item);
12276 | prev_item = str;
12277 | }
12278 | }
12279 | }
12280 | g_free(prev_item);
12281 |
12282 | if (prev_proto) {
12283 | json_dumper_end_object(&dumper); // 7.properties
12284 | json_dumper_end_object(&dumper); // 6.parent_hfinfo->abbrev
12285 | }
12286 |
12287 | json_dumper_end_object(&dumper); // 5.properties
12288 | json_dumper_end_object(&dumper); // 4.layers
12289 | json_dumper_end_object(&dumper); // 3.properties
12290 | json_dumper_end_object(&dumper); // 2.mappings
12291 | json_dumper_end_object(&dumper); // 1.root
12292 | bool_Bool ret = json_dumper_finish(&dumper);
12293 | DISSECTOR_ASSERT(ret)((void) ((ret) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 12293, "ret"))));
12294 |
12295 | g_strfreev(protos);
12296 | }
12297 |
12298 | /* Dumps the contents of the registration database to stdout. An independent
12299 | * program can take this output and format it into nice tables or HTML or
12300 | * whatever.
12301 | *
12302 | * There is one record per line. Each record is either a protocol or a header
12303 | * field, differentiated by the first field. The fields are tab-delimited.
12304 | *
12305 | * Protocols
12306 | * ---------
12307 | * Field 1 = 'P'
12308 | * Field 2 = descriptive protocol name
12309 | * Field 3 = protocol abbreviation
12310 | *
12311 | * Header Fields
12312 | * -------------
12313 | * Field 1 = 'F'
12314 | * Field 2 = descriptive field name
12315 | * Field 3 = field abbreviation
12316 | * Field 4 = type ( textual representation of the ftenum type )
12317 | * Field 5 = parent protocol abbreviation
12318 | * Field 6 = base for display (for integer types); "parent bitfield width" for FT_BOOLEAN
12319 | * Field 7 = bitmask: format: hex: 0x....
12320 | * Field 8 = blurb describing field
12321 | */
12322 | void
12323 | proto_registrar_dump_fields(void)
12324 | {
12325 | header_field_info *hfinfo, *parent_hfinfo;
12326 | int i, len;
12327 | const char *enum_name;
12328 | const char *base_name;
12329 | const char *blurb;
12330 | char width[5];
12331 |
12332 | len = gpa_hfinfo.len;
12333 | for (i = 1; i < len ; i++) {
12334 | if (gpa_hfinfo.hfi[i] == NULL((void*)0))
12335 | continue; /* This is a deregistered protocol or header field */
12336 |
12337 | PROTO_REGISTRAR_GET_NTH(i, hfinfo)if((i == 0 || (unsigned)i > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 12337 , __func__, "Unregistered hf! index=%d", i); ((void) ((i > 0 && (unsigned)i < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 12337 , "i > 0 && (unsigned)i < gpa_hfinfo.len", "Unregistered hf!" )))) ; ((void) ((gpa_hfinfo.hfi[i] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 12337, "gpa_hfinfo.hfi[i] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[i];;
12338 |
12339 | /*
12340 | * Skip the pseudo-field for "proto_tree_add_text()" since
12341 | * we don't want it in the list of filterable fields.
12342 | */
12343 | if (hfinfo->id == hf_text_only)
12344 | continue;
12345 |
12346 | /* format for protocols */
12347 | if (proto_registrar_is_protocol(i)) {
12348 | printf("P\t%s\t%s\n", hfinfo->name, hfinfo->abbrev);
12349 | }
12350 | /* format for header fields */
12351 | else {
12352 | /*
12353 | * If this field isn't at the head of the list of
12354 | * fields with this name, skip this field - all
12355 | * fields with the same name are really just versions
12356 | * of the same field stored in different bits, and
12357 | * should have the same type/radix/value list, and
12358 | * just differ in their bit masks. (If a field isn't
12359 | * a bitfield, but can be, say, 1 or 2 bytes long,
12360 | * it can just be made FT_UINT16, meaning the
12361 | * *maximum* length is 2 bytes, and be used
12362 | * for all lengths.)
12363 | */
12364 | if (hfinfo->same_name_prev_id != -1)
12365 | continue;
12366 |
12367 | PROTO_REGISTRAR_GET_NTH(hfinfo->parent, parent_hfinfo)if((hfinfo->parent == 0 || (unsigned)hfinfo->parent > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 12367 , __func__, "Unregistered hf! index=%d", hfinfo->parent); ( (void) ((hfinfo->parent > 0 && (unsigned)hfinfo ->parent < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 12367 , "hfinfo->parent > 0 && (unsigned)hfinfo->parent < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfinfo-> parent] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 12367 , "gpa_hfinfo.hfi[hfinfo->parent] != ((void*)0)", "Unregistered hf!" )))) ; parent_hfinfo = gpa_hfinfo.hfi[hfinfo->parent];;
12368 |
12369 | enum_name = ftype_name(hfinfo->type);
12370 | base_name = "";
12371 |
12372 | if (hfinfo->type == FT_CHAR ||
12373 | hfinfo->type == FT_UINT8 ||
12374 | hfinfo->type == FT_UINT16 ||
12375 | hfinfo->type == FT_UINT24 ||
12376 | hfinfo->type == FT_UINT32 ||
12377 | hfinfo->type == FT_UINT40 ||
12378 | hfinfo->type == FT_UINT48 ||
12379 | hfinfo->type == FT_UINT56 ||
12380 | hfinfo->type == FT_UINT64 ||
12381 | hfinfo->type == FT_INT8 ||
12382 | hfinfo->type == FT_INT16 ||
12383 | hfinfo->type == FT_INT24 ||
12384 | hfinfo->type == FT_INT32 ||
12385 | hfinfo->type == FT_INT40 ||
12386 | hfinfo->type == FT_INT48 ||
12387 | hfinfo->type == FT_INT56 ||
12388 | hfinfo->type == FT_INT64) {
12389 |
12390 | switch (FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF)) {
12391 | case BASE_NONE:
12392 | case BASE_DEC:
12393 | case BASE_HEX:
12394 | case BASE_OCT:
12395 | case BASE_DEC_HEX:
12396 | case BASE_HEX_DEC:
12397 | case BASE_CUSTOM:
12398 | case BASE_PT_UDP:
12399 | case BASE_PT_TCP:
12400 | case BASE_PT_DCCP:
12401 | case BASE_PT_SCTP:
12402 | case BASE_OUI:
12403 | base_name = val_to_str_const(FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF), hf_display, "????");
12404 | break;
12405 | default:
12406 | base_name = "????";
12407 | break;
12408 | }
12409 | } else if (hfinfo->type == FT_BOOLEAN) {
12410 | /* For FT_BOOLEAN: 'display' can be "parent bitfield width" */
12411 | snprintf(width, sizeof(width), "%d", hfinfo->display);
12412 | base_name = width;
12413 | }
12414 |
12415 | blurb = hfinfo->blurb;
12416 | if (blurb == NULL((void*)0))
12417 | blurb = "";
12418 | else if (strlen(blurb) == 0)
12419 | blurb = "\"\"";
12420 |
12421 | printf("F\t%s\t%s\t%s\t%s\t%s\t0x%" PRIx64"l" "x" "\t%s\n",
12422 | hfinfo->name, hfinfo->abbrev, enum_name,
12423 | parent_hfinfo->abbrev, base_name,
12424 | hfinfo->bitmask, blurb);
12425 | }
12426 | }
12427 | }
12428 |
12429 | /* Dumps all abbreviated field and protocol completions of the given string to
12430 | * stdout. An independent program may use this for command-line tab completion
12431 | * of fields.
12432 | */
12433 | bool_Bool
12434 | proto_registrar_dump_field_completions(const char *prefix)
12435 | {
12436 | header_field_info *hfinfo;
12437 | int i, len;
12438 | size_t prefix_len;
12439 | bool_Bool matched = false0;
12440 |
12441 | prefix_len = strlen(prefix);
12442 | len = gpa_hfinfo.len;
12443 | for (i = 1; i < len ; i++) {
12444 | if (gpa_hfinfo.hfi[i] == NULL((void*)0))
12445 | continue; /* This is a deregistered protocol or header field */
12446 |
12447 | PROTO_REGISTRAR_GET_NTH(i, hfinfo)if((i == 0 || (unsigned)i > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 12447 , __func__, "Unregistered hf! index=%d", i); ((void) ((i > 0 && (unsigned)i < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 12447 , "i > 0 && (unsigned)i < gpa_hfinfo.len", "Unregistered hf!" )))) ; ((void) ((gpa_hfinfo.hfi[i] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 12447, "gpa_hfinfo.hfi[i] != ((void*)0)", "Unregistered hf!" )))) ; hfinfo = gpa_hfinfo.hfi[i];;
12448 |
12449 | /*
12450 | * Skip the pseudo-field for "proto_tree_add_text()" since
12451 | * we don't want it in the list of filterable fields.
12452 | */
12453 | if (hfinfo->id == hf_text_only)
12454 | continue;
12455 |
12456 | /* format for protocols */
12457 | if (proto_registrar_is_protocol(i)) {
12458 | if(0 == strncmp(hfinfo->abbrev, prefix, prefix_len)) {
12459 | matched = true1;
12460 | printf("%s\t%s\n", hfinfo->abbrev, hfinfo->name);
12461 | }
12462 | }
12463 | /* format for header fields */
12464 | else {
12465 | /*
12466 | * If this field isn't at the head of the list of
12467 | * fields with this name, skip this field - all
12468 | * fields with the same name are really just versions
12469 | * of the same field stored in different bits, and
12470 | * should have the same type/radix/value list, and
12471 | * just differ in their bit masks. (If a field isn't
12472 | * a bitfield, but can be, say, 1 or 2 bytes long,
12473 | * it can just be made FT_UINT16, meaning the
12474 | * *maximum* length is 2 bytes, and be used
12475 | * for all lengths.)
12476 | */
12477 | if (hfinfo->same_name_prev_id != -1)
12478 | continue;
12479 |
12480 | if(0 == strncmp(hfinfo->abbrev, prefix, prefix_len)) {
12481 | matched = true1;
12482 | printf("%s\t%s\n", hfinfo->abbrev, hfinfo->name);
12483 | }
12484 | }
12485 | }
12486 | return matched;
12487 | }
12488 |
12489 | /* Dumps field types and descriptive names to stdout. An independent
12490 | * program can take this output and format it into nice tables or HTML or
12491 | * whatever.
12492 | *
12493 | * There is one record per line. The fields are tab-delimited.
12494 | *
12495 | * Field 1 = field type name, e.g. FT_UINT8
12496 | * Field 2 = descriptive name, e.g. "Unsigned, 1 byte"
12497 | */
12498 | void
12499 | proto_registrar_dump_ftypes(void)
12500 | {
12501 | int fte;
12502 |
12503 | for (fte = 0; fte < FT_NUM_TYPES; fte++) {
12504 | printf("%s\t%s\n", ftype_name((ftenum_t)fte), ftype_pretty_name((ftenum_t)fte));
12505 | }
12506 | }
12507 |
12508 | /* This function indicates whether it's possible to construct a
12509 | * "match selected" display filter string for the specified field,
12510 | * returns an indication of whether it's possible, and, if it's
12511 | * possible and "filter" is non-null, constructs the filter and
12512 | * sets "*filter" to point to it.
12513 | * You do not need to [g_]free() this string since it will be automatically
12514 | * freed once the next packet is dissected.
12515 | */
12516 | static bool_Bool
12517 | construct_match_selected_string(const field_info *finfo, epan_dissect_t *edt,
12518 | char **filter)
12519 | {
12520 | const header_field_info *hfinfo;
12521 | int start, length, length_remaining;
12522 |
12523 | if (!finfo)
12524 | return false0;
12525 |
12526 | hfinfo = finfo->hfinfo;
12527 | DISSECTOR_ASSERT(hfinfo)((void) ((hfinfo) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 12527, "hfinfo"))));
12528 |
12529 | /* If we have BASE_NONE and strings (a non-NULL FIELDCONVERT),
12530 | * then "the numeric value ... is not used when preparing
12531 | * filters for the field in question." If it's any other
12532 | * base, we'll generate the filter normally (which will
12533 | * be numeric, even though the human-readable string does
12534 | * work for filtering.)
12535 | *
12536 | * XXX - It might be nice to use fvalue_to_string_repr() in
12537 | * "proto_item_fill_label()" as well, although, there, you'd
12538 | * have to deal with the base *and* with resolved values for
12539 | * addresses.
12540 | *
12541 | * Perhaps in addition to taking the repr type (DISPLAY
12542 | * or DFILTER) and the display (base), fvalue_to_string_repr()
12543 | * should have the the "strings" values in the header_field_info
12544 | * structure for the field as a parameter, so it can have
12545 | * if the field is Boolean or an enumerated integer type,
12546 | * the tables used to generate human-readable values.
12547 | */
12548 | if (hfinfo->strings && FIELD_DISPLAY(hfinfo->display)((hfinfo->display) & 0xFF) == BASE_NONE) {
12549 | const char *str = NULL((void*)0);
12550 |
12551 | switch (hfinfo->type) {
12552 |
12553 | case FT_INT8:
12554 | case FT_INT16:
12555 | case FT_INT24:
12556 | case FT_INT32:
12557 | str = hf_try_val_to_str(fvalue_get_sinteger(finfo->value), hfinfo);
12558 | break;
12559 |
12560 | case FT_CHAR:
12561 | case FT_UINT8:
12562 | case FT_UINT16:
12563 | case FT_UINT24:
12564 | case FT_UINT32:
12565 | str = hf_try_val_to_str(fvalue_get_uinteger(finfo->value), hfinfo);
12566 | break;
12567 |
12568 | default:
12569 | break;
12570 | }
12571 |
12572 | if (str != NULL((void*)0) && filter != NULL((void*)0)) {
12573 | *filter = wmem_strdup_printf(NULL((void*)0), "%s == \"%s\"", hfinfo->abbrev, str);
12574 | return true1;
12575 | }
12576 | }
12577 |
12578 | switch (hfinfo->type) {
12579 |
12580 | case FT_PROTOCOL:
12581 | if (filter != NULL((void*)0))
12582 | *filter = wmem_strdup(NULL((void*)0), finfo->hfinfo->abbrev);
12583 | break;
12584 |
12585 | case FT_NONE:
12586 | /*
12587 | * If the length is 0, just match the name of the
12588 | * field.
12589 | *
12590 | * (Also check for negative values, just in case,
12591 | * as we'll cast it to an unsigned value later.)
12592 | */
12593 | length = finfo->length;
12594 | if (length == 0) {
12595 | if (filter != NULL((void*)0))
12596 | *filter = wmem_strdup(NULL((void*)0), finfo->hfinfo->abbrev);
12597 | break;
12598 | }
12599 | if (length < 0)
12600 | return false0;
12601 |
12602 | /*
12603 | * This doesn't have a value, so we'd match
12604 | * on the raw bytes at this address.
12605 | *
12606 | * Should we be allowed to access to the raw bytes?
12607 | * If "edt" is NULL, the answer is "no".
12608 | */
12609 | if (edt == NULL((void*)0))
12610 | return false0;
12611 |
12612 | /*
12613 | * Is this field part of the raw frame tvbuff?
12614 | * If not, we can't use "frame[N:M]" to match
12615 | * it.
12616 | *
12617 | * XXX - should this be frame-relative, or
12618 | * protocol-relative?
12619 | *
12620 | * XXX - does this fallback for non-registered
12621 | * fields even make sense?
12622 | */
12623 | if (finfo->ds_tvb != edt->tvb)
12624 | return false0; /* you lose */
12625 |
12626 | /*
12627 | * Don't go past the end of that tvbuff.
12628 | */
12629 | length_remaining = tvb_captured_length_remaining(finfo->ds_tvb, finfo->start);
12630 | if (length > length_remaining)
12631 | length = length_remaining;
12632 | if (length <= 0)
12633 | return false0;
12634 |
12635 | if (filter != NULL((void*)0)) {
12636 | start = finfo->start;
12637 | char *str = bytes_to_dfilter_repr(NULL((void*)0), tvb_get_ptr(finfo->ds_tvb, start, length), length);
12638 | *filter = wmem_strdup_printf(NULL((void*)0), "frame[%d:%d] == %s", finfo->start, length, str);
12639 | wmem_free(NULL((void*)0), str);
12640 | }
12641 | break;
12642 |
12643 | /* By default, use the fvalue's "to_string_repr" method. */
12644 | default:
12645 | if (filter != NULL((void*)0)) {
12646 | char *str = fvalue_to_string_repr(NULL((void*)0), finfo->value, FTREPR_DFILTER, finfo->hfinfo->display);
12647 | *filter = wmem_strdup_printf(NULL((void*)0), "%s == %s", hfinfo->abbrev, str);
12648 | wmem_free(NULL((void*)0), str);
12649 | }
12650 | break;
12651 | }
12652 |
12653 | return true1;
12654 | }
12655 |
12656 | /*
12657 | * Returns true if we can do a "match selected" on the field, false
12658 | * otherwise.
12659 | */
12660 | bool_Bool
12661 | proto_can_match_selected(const field_info *finfo, epan_dissect_t *edt)
12662 | {
12663 | return construct_match_selected_string(finfo, edt, NULL((void*)0));
12664 | }
12665 |
12666 | /* This function attempts to construct a "match selected" display filter
12667 | * string for the specified field; if it can do so, it returns a pointer
12668 | * to the string, otherwise it returns NULL.
12669 | *
12670 | * The string is wmem allocated and must be freed with "wmem_free(NULL, ...)".
12671 | */
12672 | char *
12673 | proto_construct_match_selected_string(const field_info *finfo, epan_dissect_t *edt)
12674 | {
12675 | char *filter = NULL((void*)0);
12676 |
12677 | if (!construct_match_selected_string(finfo, edt, &filter))
12678 | {
12679 | wmem_free(NULL((void*)0), filter);
12680 | return NULL((void*)0);
12681 | }
12682 | return filter;
12683 | }
12684 |
12685 | /* This function is common code for all proto_tree_add_bitmask... functions.
12686 | */
12687 |
12688 | static bool_Bool
12689 | proto_item_add_bitmask_tree(proto_item *item, tvbuff_t *tvb, const int offset,
12690 | const int len, const int ett, int * const *fields,
12691 | const int flags, bool_Bool first,
12692 | bool_Bool use_parent_tree,
12693 | proto_tree* tree, uint64_t value)
12694 | {
12695 | uint64_t available_bits = UINT64_MAX(18446744073709551615UL);
12696 | uint64_t bitmask = 0;
12697 | uint64_t tmpval;
12698 | header_field_info *hf;
12699 | uint32_t integer32;
12700 | int bit_offset;
12701 | int no_of_bits;
12702 |
12703 | if (!*fields)
12704 | REPORT_DISSECTOR_BUG("Illegal call of proto_item_add_bitmask_tree without fields")proto_report_dissector_bug("Illegal call of proto_item_add_bitmask_tree without fields" );
12705 |
12706 | if (len < 0 || len > 8)
12707 | REPORT_DISSECTOR_BUG("Invalid len: %d", len)proto_report_dissector_bug("Invalid len: %d", len);
12708 | /**
12709 | * packet-frame.c uses len=0 since the value is taken from the packet
12710 | * metadata, not the packet bytes. In that case, assume that all bits
12711 | * in the provided value are valid.
12712 | */
12713 | if (len > 0) {
12714 | available_bits >>= (8 - (unsigned)len)*8;
12715 | }
12716 |
12717 | if (use_parent_tree == false0)
12718 | tree = proto_item_add_subtree(item, ett);
12719 |
12720 | while (*fields) {
12721 | uint64_t present_bits;
12722 | PROTO_REGISTRAR_GET_NTH(**fields,hf)if((**fields == 0 || (unsigned)**fields > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 12722, __func__, "Unregistered hf! index=%d" , **fields); ((void) ((**fields > 0 && (unsigned)* *fields < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 12722 , "**fields > 0 && (unsigned)**fields < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[**fields] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 12722, "gpa_hfinfo.hfi[**fields] != ((void*)0)" , "Unregistered hf!")))) ; hf = gpa_hfinfo.hfi[**fields];;
12723 | DISSECTOR_ASSERT_HINT(hf->bitmask != 0, hf->abbrev)((void) ((hf->bitmask != 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 12723 , "hf->bitmask != 0", hf->abbrev))));
12724 |
12725 | bitmask |= hf->bitmask;
12726 |
12727 | /* Skip fields that aren't fully present */
12728 | present_bits = available_bits & hf->bitmask;
12729 | if (present_bits != hf->bitmask) {
12730 | fields++;
12731 | continue;
12732 | }
12733 |
12734 | switch (hf->type) {
12735 | case FT_CHAR:
12736 | case FT_UINT8:
12737 | case FT_UINT16:
12738 | case FT_UINT24:
12739 | case FT_UINT32:
12740 | proto_tree_add_uint(tree, **fields, tvb, offset, len, (uint32_t)value);
12741 | break;
12742 |
12743 | case FT_INT8:
12744 | case FT_INT16:
12745 | case FT_INT24:
12746 | case FT_INT32:
12747 | proto_tree_add_int(tree, **fields, tvb, offset, len, (int32_t)value);
12748 | break;
12749 |
12750 | case FT_UINT40:
12751 | case FT_UINT48:
12752 | case FT_UINT56:
12753 | case FT_UINT64:
12754 | proto_tree_add_uint64(tree, **fields, tvb, offset, len, value);
12755 | break;
12756 |
12757 | case FT_INT40:
12758 | case FT_INT48:
12759 | case FT_INT56:
12760 | case FT_INT64:
12761 | proto_tree_add_int64(tree, **fields, tvb, offset, len, (int64_t)value);
12762 | break;
12763 |
12764 | case FT_BOOLEAN:
12765 | proto_tree_add_boolean(tree, **fields, tvb, offset, len, value);
12766 | break;
12767 |
12768 | default:
12769 | REPORT_DISSECTOR_BUG("field %s has type %d (%s) not handled in proto_item_add_bitmask_tree()",proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_item_add_bitmask_tree()" , hf->abbrev, hf->type, ftype_name(hf->type))
12770 | hf->abbrev,proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_item_add_bitmask_tree()" , hf->abbrev, hf->type, ftype_name(hf->type))
12771 | hf->type,proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_item_add_bitmask_tree()" , hf->abbrev, hf->type, ftype_name(hf->type))
12772 | ftype_name(hf->type))proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_item_add_bitmask_tree()" , hf->abbrev, hf->type, ftype_name(hf->type));
12773 | break;
12774 | }
12775 | if (flags & BMT_NO_APPEND0x01) {
12776 | fields++;
12777 | continue;
12778 | }
12779 | tmpval = (value & hf->bitmask) >> hfinfo_bitshift(hf);
12780 |
12781 | /* XXX: README.developer and the comments have always defined
12782 | * BMT_NO_INT as "only boolean flags are added to the title /
12783 | * don't add non-boolean (integral) fields", but the
12784 | * implementation has always added BASE_CUSTOM and fields with
12785 | * value_strings, though not fields with unit_strings.
12786 | * Possibly this is because some dissectors use a FT_UINT8
12787 | * with a value_string for fields that should be a FT_BOOLEAN.
12788 | */
12789 | switch (hf->type) {
12790 | case FT_CHAR:
12791 | if (hf->display == BASE_CUSTOM) {
12792 | char lbl[ITEM_LABEL_LENGTH240];
12793 | const custom_fmt_func_t fmtfunc = (const custom_fmt_func_t)hf->strings;
12794 |
12795 | DISSECTOR_ASSERT(fmtfunc)((void) ((fmtfunc) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 12795, "fmtfunc"))));
12796 | fmtfunc(lbl, (uint32_t) tmpval);
12797 | proto_item_append_text(item, "%s%s: %s", first ? "" : ", ",
12798 | hf->name, lbl);
12799 | first = false0;
12800 | }
12801 | else if (hf->strings) {
12802 | proto_item_append_text(item, "%s%s: %s", first ? "" : ", ",
12803 | hf->name, hf_try_val_to_str_const((uint32_t) tmpval, hf, "Unknown"));
12804 | first = false0;
12805 | }
12806 | else if (!(flags & BMT_NO_INT0x02)) {
12807 | char buf[32];
12808 | const char *out;
12809 |
12810 | if (!first) {
12811 | proto_item_append_text(item, ", ");
12812 | }
12813 |
12814 | out = hfinfo_char_value_format(hf, buf, (uint32_t) tmpval);
12815 | proto_item_append_text(item, "%s: %s", hf->name, out);
12816 | first = false0;
12817 | }
12818 |
12819 | break;
12820 |
12821 | case FT_UINT8:
12822 | case FT_UINT16:
12823 | case FT_UINT24:
12824 | case FT_UINT32:
12825 | if (hf->display == BASE_CUSTOM) {
12826 | char lbl[ITEM_LABEL_LENGTH240];
12827 | const custom_fmt_func_t fmtfunc = (const custom_fmt_func_t)hf->strings;
12828 |
12829 | DISSECTOR_ASSERT(fmtfunc)((void) ((fmtfunc) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 12829, "fmtfunc"))));
12830 | fmtfunc(lbl, (uint32_t) tmpval);
12831 | proto_item_append_text(item, "%s%s: %s", first ? "" : ", ",
12832 | hf->name, lbl);
12833 | first = false0;
12834 | }
12835 | else if ((hf->strings) &&(!(hf->display & (BASE_UNIT_STRING0x00001000|BASE_SPECIAL_VALS0x00008000)))) {
12836 | proto_item_append_text(item, "%s%s: %s", first ? "" : ", ",
12837 | hf->name, hf_try_val_to_str_const((uint32_t) tmpval, hf, "Unknown"));
12838 | first = false0;
12839 | }
12840 | else if (!(flags & BMT_NO_INT0x02)) {
12841 | char buf[NUMBER_LABEL_LENGTH80];
12842 | const char *out = NULL((void*)0);
12843 |
12844 | if (!first) {
12845 | proto_item_append_text(item, ", ");
12846 | }
12847 |
12848 | if (hf->strings && hf->display & BASE_SPECIAL_VALS0x00008000) {
12849 | out = hf_try_val_to_str((uint32_t) tmpval, hf);
12850 | }
12851 | if (out == NULL((void*)0)) {
12852 | out = hfinfo_number_value_format(hf, buf, (uint32_t) tmpval);
12853 | }
12854 | proto_item_append_text(item, "%s: %s", hf->name, out);
12855 | if (hf->strings && hf->display & BASE_UNIT_STRING0x00001000) {
12856 | proto_item_append_text(item, "%s", unit_name_string_get_value((uint32_t) tmpval, (const unit_name_string*)hf->strings));
12857 | }
12858 | first = false0;
12859 | }
12860 |
12861 | break;
12862 |
12863 | case FT_INT8:
12864 | case FT_INT16:
12865 | case FT_INT24:
12866 | case FT_INT32:
12867 | integer32 = (uint32_t) tmpval;
12868 | if (hf->bitmask) {
12869 | no_of_bits = ws_count_ones(hf->bitmask);
12870 | integer32 = ws_sign_ext32(integer32, no_of_bits);
12871 | }
12872 | if (hf->display == BASE_CUSTOM) {
12873 | char lbl[ITEM_LABEL_LENGTH240];
12874 | const custom_fmt_func_t fmtfunc = (const custom_fmt_func_t)hf->strings;
12875 |
12876 | DISSECTOR_ASSERT(fmtfunc)((void) ((fmtfunc) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 12876, "fmtfunc"))));
12877 | fmtfunc(lbl, (int32_t) integer32);
12878 | proto_item_append_text(item, "%s%s: %s", first ? "" : ", ",
12879 | hf->name, lbl);
12880 | first = false0;
12881 | }
12882 | else if ((hf->strings) &&(!(hf->display & (BASE_UNIT_STRING0x00001000|BASE_SPECIAL_VALS0x00008000)))) {
12883 | proto_item_append_text(item, "%s%s: %s", first ? "" : ", ",
12884 | hf->name, hf_try_val_to_str_const((int32_t) integer32, hf, "Unknown"));
12885 | first = false0;
12886 | }
12887 | else if (!(flags & BMT_NO_INT0x02)) {
12888 | char buf[NUMBER_LABEL_LENGTH80];
12889 | const char *out = NULL((void*)0);
12890 |
12891 | if (!first) {
12892 | proto_item_append_text(item, ", ");
12893 | }
12894 |
12895 | if (hf->strings && hf->display & BASE_SPECIAL_VALS0x00008000) {
12896 | out = hf_try_val_to_str((int32_t) integer32, hf);
12897 | }
12898 | if (out == NULL((void*)0)) {
12899 | out = hfinfo_number_value_format(hf, buf, (int32_t) integer32);
12900 | }
12901 | proto_item_append_text(item, "%s: %s", hf->name, out);
12902 | if (hf->strings && hf->display & BASE_UNIT_STRING0x00001000) {
12903 | proto_item_append_text(item, "%s", unit_name_string_get_value((uint32_t) tmpval, (const unit_name_string*)hf->strings));
12904 | }
12905 | first = false0;
12906 | }
12907 |
12908 | break;
12909 |
12910 | case FT_UINT40:
12911 | case FT_UINT48:
12912 | case FT_UINT56:
12913 | case FT_UINT64:
12914 | if (hf->display == BASE_CUSTOM) {
12915 | char lbl[ITEM_LABEL_LENGTH240];
12916 | const custom_fmt_func_64_t fmtfunc = (const custom_fmt_func_64_t)hf->strings;
12917 |
12918 | DISSECTOR_ASSERT(fmtfunc)((void) ((fmtfunc) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 12918, "fmtfunc"))));
12919 | fmtfunc(lbl, tmpval);
12920 | proto_item_append_text(item, "%s%s: %s", first ? "" : ", ",
12921 | hf->name, lbl);
12922 | first = false0;
12923 | }
12924 | else if ((hf->strings) &&(!(hf->display & (BASE_UNIT_STRING0x00001000|BASE_SPECIAL_VALS0x00008000)))) {
12925 | proto_item_append_text(item, "%s%s: %s", first ? "" : ", ",
12926 | hf->name, hf_try_val64_to_str_const(tmpval, hf, "Unknown"));
12927 | first = false0;
12928 | }
12929 | else if (!(flags & BMT_NO_INT0x02)) {
12930 | char buf[NUMBER_LABEL_LENGTH80];
12931 | const char *out = NULL((void*)0);
12932 |
12933 | if (!first) {
12934 | proto_item_append_text(item, ", ");
12935 | }
12936 |
12937 | if (hf->strings && hf->display & BASE_SPECIAL_VALS0x00008000) {
12938 | out = hf_try_val64_to_str(tmpval, hf);
12939 | }
12940 | if (out == NULL((void*)0)) {
12941 | out = hfinfo_number_value_format64(hf, buf, tmpval);
12942 | }
12943 | proto_item_append_text(item, "%s: %s", hf->name, out);
12944 | if (hf->strings && hf->display & BASE_UNIT_STRING0x00001000) {
12945 | proto_item_append_text(item, "%s", unit_name_string_get_value64(tmpval, (const unit_name_string*)hf->strings));
12946 | }
12947 | first = false0;
12948 | }
12949 |
12950 | break;
12951 |
12952 | case FT_INT40:
12953 | case FT_INT48:
12954 | case FT_INT56:
12955 | case FT_INT64:
12956 | if (hf->bitmask) {
12957 | no_of_bits = ws_count_ones(hf->bitmask);
12958 | tmpval = ws_sign_ext64(tmpval, no_of_bits);
12959 | }
12960 | if (hf->display == BASE_CUSTOM) {
12961 | char lbl[ITEM_LABEL_LENGTH240];
12962 | const custom_fmt_func_64_t fmtfunc = (const custom_fmt_func_64_t)hf->strings;
12963 |
12964 | DISSECTOR_ASSERT(fmtfunc)((void) ((fmtfunc) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\"" , "epan/proto.c", 12964, "fmtfunc"))));
12965 | fmtfunc(lbl, (int64_t) tmpval);
12966 | proto_item_append_text(item, "%s%s: %s", first ? "" : ", ",
12967 | hf->name, lbl);
12968 | first = false0;
12969 | }
12970 | else if ((hf->strings) &&(!(hf->display & (BASE_UNIT_STRING0x00001000|BASE_SPECIAL_VALS0x00008000)))) {
12971 | proto_item_append_text(item, "%s%s: %s", first ? "" : ", ",
12972 | hf->name, hf_try_val64_to_str_const((int64_t) tmpval, hf, "Unknown"));
12973 | first = false0;
12974 | }
12975 | else if (!(flags & BMT_NO_INT0x02)) {
12976 | char buf[NUMBER_LABEL_LENGTH80];
12977 | const char *out = NULL((void*)0);
12978 |
12979 | if (!first) {
12980 | proto_item_append_text(item, ", ");
12981 | }
12982 |
12983 | if (hf->strings && hf->display & BASE_SPECIAL_VALS0x00008000) {
12984 | out = hf_try_val64_to_str((int64_t) tmpval, hf);
12985 | }
12986 | if (out == NULL((void*)0)) {
12987 | out = hfinfo_number_value_format64(hf, buf, (int64_t) tmpval);
12988 | }
12989 | proto_item_append_text(item, "%s: %s", hf->name, out);
12990 | if (hf->strings && hf->display & BASE_UNIT_STRING0x00001000) {
12991 | proto_item_append_text(item, "%s", unit_name_string_get_value64(tmpval, (const unit_name_string*)hf->strings));
12992 | }
12993 | first = false0;
12994 | }
12995 |
12996 | break;
12997 |
12998 | case FT_BOOLEAN:
12999 | if (hf->strings && !(flags & BMT_NO_TFS0x08)) {
13000 | /* If we have true/false strings, emit full - otherwise messages
13001 | might look weird */
13002 | const struct true_false_string *tfs =
13003 | (const struct true_false_string *)hf->strings;
13004 |
13005 | if (tmpval) {
13006 | proto_item_append_text(item, "%s%s: %s", first ? "" : ", ",
13007 | hf->name, tfs->true_string);
13008 | first = false0;
13009 | } else if (!(flags & BMT_NO_FALSE0x04)) {
13010 | proto_item_append_text(item, "%s%s: %s", first ? "" : ", ",
13011 | hf->name, tfs->false_string);
13012 | first = false0;
13013 | }
13014 | } else if (hf->bitmask & value) {
13015 | /* If the flag is set, show the name */
13016 | proto_item_append_text(item, "%s%s", first ? "" : ", ", hf->name);
13017 | first = false0;
13018 | }
13019 | break;
13020 | default:
13021 | REPORT_DISSECTOR_BUG("field %s has type %d (%s) not handled in proto_item_add_bitmask_tree()",proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_item_add_bitmask_tree()" , hf->abbrev, hf->type, ftype_name(hf->type))
13022 | hf->abbrev,proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_item_add_bitmask_tree()" , hf->abbrev, hf->type, ftype_name(hf->type))
13023 | hf->type,proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_item_add_bitmask_tree()" , hf->abbrev, hf->type, ftype_name(hf->type))
13024 | ftype_name(hf->type))proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_item_add_bitmask_tree()" , hf->abbrev, hf->type, ftype_name(hf->type));
13025 | break;
13026 | }
13027 |
13028 | fields++;
13029 | }
13030 |
13031 | /* XXX: We don't pass the hfi into this function. Perhaps we should,
13032 | * but then again most dissectors don't set the bitmask field for
13033 | * the higher level bitmask hfi, so calculate the bitmask from the
13034 | * fields present. */
13035 | if (item) {
13036 | bit_offset = len*8 - 1 - ws_ilog2(bitmask);
13037 | no_of_bits = ws_ilog2(bitmask) - ws_ctz(bitmask) + 1;
13038 | FI_SET_FLAG(PNODE_FINFO(item), FI_BITS_OFFSET(bit_offset))do { if (((item)->finfo)) (((item)->finfo))->flags = (((item)->finfo))->flags | ((((bit_offset) & 63) << 5)); } while(0);
13039 | FI_SET_FLAG(PNODE_FINFO(item), FI_BITS_SIZE(no_of_bits))do { if (((item)->finfo)) (((item)->finfo))->flags = (((item)->finfo))->flags | ((((no_of_bits) & 63) << 12)); } while(0);
13040 | }
13041 | return first;
13042 | }
13043 |
13044 | /* This function will dissect a sequence of bytes that describe a
13045 | * bitmask and supply the value of that sequence through a pointer.
13046 | * hf_hdr is a 8/16/24/32/40/48/56/64 bit integer that describes the bitmask
13047 | * to be dissected.
13048 | * This field will form an expansion under which the individual fields of the
13049 | * bitmask is dissected and displayed.
13050 | * This field must be of the type FT_[U]INT{8|16|24|32|40|48|56|64}.
13051 | *
13052 | * fields is an array of pointers to int that lists all the fields of the
13053 | * bitmask. These fields can be either of the type FT_BOOLEAN for flags
13054 | * or another integer of the same type/size as hf_hdr with a mask specified.
13055 | * This array is terminated by a NULL entry.
13056 | *
13057 | * FT_BOOLEAN bits that are set to 1 will have the name added to the expansion.
13058 | * FT_integer fields that have a value_string attached will have the
13059 | * matched string displayed on the expansion line.
13060 | */
13061 | proto_item *
13062 | proto_tree_add_bitmask_ret_uint64(proto_tree *parent_tree, tvbuff_t *tvb,
13063 | const unsigned offset, const int hf_hdr,
13064 | const int ett, int * const *fields,
13065 | const unsigned encoding, uint64_t *retval)
13066 | {
13067 | return proto_tree_add_bitmask_with_flags_ret_uint64(parent_tree, tvb, offset, hf_hdr, ett, fields, encoding, BMT_NO_INT0x02|BMT_NO_TFS0x08, retval);
13068 | }
13069 |
13070 | /* This function will dissect a sequence of bytes that describe a
13071 | * bitmask.
13072 | * hf_hdr is a 8/16/24/32/40/48/56/64 bit integer that describes the bitmask
13073 | * to be dissected.
13074 | * This field will form an expansion under which the individual fields of the
13075 | * bitmask is dissected and displayed.
13076 | * This field must be of the type FT_[U]INT{8|16|24|32|40|48|56|64}.
13077 | *
13078 | * fields is an array of pointers to int that lists all the fields of the
13079 | * bitmask. These fields can be either of the type FT_BOOLEAN for flags
13080 | * or another integer of the same type/size as hf_hdr with a mask specified.
13081 | * This array is terminated by a NULL entry.
13082 | *
13083 | * FT_BOOLEAN bits that are set to 1 will have the name added to the expansion.
13084 | * FT_integer fields that have a value_string attached will have the
13085 | * matched string displayed on the expansion line.
13086 | */
13087 | proto_item *
13088 | proto_tree_add_bitmask(proto_tree *parent_tree, tvbuff_t *tvb,
13089 | const unsigned offset, const int hf_hdr,
13090 | const int ett, int * const *fields,
13091 | const unsigned encoding)
13092 | {
13093 | return proto_tree_add_bitmask_with_flags(parent_tree, tvb, offset, hf_hdr, ett, fields, encoding, BMT_NO_INT0x02|BMT_NO_TFS0x08);
13094 | }
13095 |
13096 | /* The same as proto_tree_add_bitmask_ret_uint64(), but uses user-supplied flags to determine
13097 | * what data is appended to the header.
13098 | */
13099 | proto_item *
13100 | proto_tree_add_bitmask_with_flags_ret_uint64(proto_tree *parent_tree, tvbuff_t *tvb, const unsigned offset,
13101 | const int hf_hdr, const int ett, int * const *fields, const unsigned encoding, const int flags,
13102 | uint64_t *retval)
13103 | {
13104 | proto_item *item = NULL((void*)0);
13105 | header_field_info *hf;
13106 | int len;
13107 | uint64_t value;
13108 |
13109 | PROTO_REGISTRAR_GET_NTH(hf_hdr,hf)if((hf_hdr == 0 || (unsigned)hf_hdr > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 13109, __func__, "Unregistered hf! index=%d" , hf_hdr); ((void) ((hf_hdr > 0 && (unsigned)hf_hdr < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 13109 , "hf_hdr > 0 && (unsigned)hf_hdr < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hf_hdr] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13109, "gpa_hfinfo.hfi[hf_hdr] != ((void*)0)" , "Unregistered hf!")))) ; hf = gpa_hfinfo.hfi[hf_hdr];;
13110 | DISSECTOR_ASSERT_FIELD_TYPE_IS_INTEGRAL(hf)((void) (((((((hf)->type) == FT_INT8 || ((hf)->type) == FT_INT16 || ((hf)->type) == FT_INT24 || ((hf)->type) == FT_INT32) || (((hf)->type) == FT_INT40 || ((hf)->type) == FT_INT48 || ((hf)->type) == FT_INT56 || ((hf)->type ) == FT_INT64)) || ((((hf)->type) == FT_CHAR || ((hf)-> type) == FT_UINT8 || ((hf)->type) == FT_UINT16 || ((hf)-> type) == FT_UINT24 || ((hf)->type) == FT_UINT32 || ((hf)-> type) == FT_FRAMENUM) || (((hf)->type) == FT_UINT40 || ((hf )->type) == FT_UINT48 || ((hf)->type) == FT_UINT56 || ( (hf)->type) == FT_UINT64)))) ? (void)0 : proto_report_dissector_bug ("%s:%u: field %s is not of type FT_CHAR or an FT_{U}INTn type" , "epan/proto.c", 13110, (hf)->abbrev)));
13111 | len = ftype_wire_size(hf->type);
13112 | value = get_uint64_value(parent_tree, tvb, offset, len, encoding);
13113 |
13114 | if (parent_tree) {
13115 | item = proto_tree_add_item(parent_tree, hf_hdr, tvb, offset, len, encoding);
13116 | proto_item_add_bitmask_tree(item, tvb, offset, len, ett, fields,
13117 | flags, false0, false0, NULL((void*)0), value);
13118 | }
13119 |
13120 | *retval = value;
13121 | if (hf->bitmask) {
13122 | /* Mask out irrelevant portions */
13123 | *retval &= hf->bitmask;
13124 | /* Shift bits */
13125 | *retval >>= hfinfo_bitshift(hf);
13126 | }
13127 |
13128 | return item;
13129 | }
13130 |
13131 | /* The same as proto_tree_add_bitmask_ret_uint64(), but uses user-supplied flags to determine
13132 | * what data is appended to the header.
13133 | */
13134 | proto_item *
13135 | proto_tree_add_bitmask_with_flags(proto_tree *parent_tree, tvbuff_t *tvb, const unsigned offset,
13136 | const int hf_hdr, const int ett, int * const *fields, const unsigned encoding, const int flags)
13137 | {
13138 | proto_item *item = NULL((void*)0);
13139 | header_field_info *hf;
13140 | int len;
13141 | uint64_t value;
13142 |
13143 | PROTO_REGISTRAR_GET_NTH(hf_hdr,hf)if((hf_hdr == 0 || (unsigned)hf_hdr > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 13143, __func__, "Unregistered hf! index=%d" , hf_hdr); ((void) ((hf_hdr > 0 && (unsigned)hf_hdr < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 13143 , "hf_hdr > 0 && (unsigned)hf_hdr < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hf_hdr] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13143, "gpa_hfinfo.hfi[hf_hdr] != ((void*)0)" , "Unregistered hf!")))) ; hf = gpa_hfinfo.hfi[hf_hdr];;
13144 | DISSECTOR_ASSERT_FIELD_TYPE_IS_INTEGRAL(hf)((void) (((((((hf)->type) == FT_INT8 || ((hf)->type) == FT_INT16 || ((hf)->type) == FT_INT24 || ((hf)->type) == FT_INT32) || (((hf)->type) == FT_INT40 || ((hf)->type) == FT_INT48 || ((hf)->type) == FT_INT56 || ((hf)->type ) == FT_INT64)) || ((((hf)->type) == FT_CHAR || ((hf)-> type) == FT_UINT8 || ((hf)->type) == FT_UINT16 || ((hf)-> type) == FT_UINT24 || ((hf)->type) == FT_UINT32 || ((hf)-> type) == FT_FRAMENUM) || (((hf)->type) == FT_UINT40 || ((hf )->type) == FT_UINT48 || ((hf)->type) == FT_UINT56 || ( (hf)->type) == FT_UINT64)))) ? (void)0 : proto_report_dissector_bug ("%s:%u: field %s is not of type FT_CHAR or an FT_{U}INTn type" , "epan/proto.c", 13144, (hf)->abbrev)));
13145 |
13146 | if (parent_tree) {
13147 | len = ftype_wire_size(hf->type);
13148 | item = proto_tree_add_item(parent_tree, hf_hdr, tvb, offset, len, encoding);
13149 | value = get_uint64_value(parent_tree, tvb, offset, len, encoding);
13150 | proto_item_add_bitmask_tree(item, tvb, offset, len, ett, fields,
13151 | flags, false0, false0, NULL((void*)0), value);
13152 | }
13153 |
13154 | return item;
13155 | }
13156 |
13157 | /* Similar to proto_tree_add_bitmask(), but with a passed in value (presumably because it
13158 | can't be retrieved directly from tvb) */
13159 | proto_item *
13160 | proto_tree_add_bitmask_value(proto_tree *parent_tree, tvbuff_t *tvb, const unsigned offset,
13161 | const int hf_hdr, const int ett, int * const *fields, const uint64_t value)
13162 | {
13163 | return proto_tree_add_bitmask_value_with_flags(parent_tree, tvb, offset,
13164 | hf_hdr, ett, fields, value, BMT_NO_INT0x02|BMT_NO_TFS0x08);
13165 | }
13166 |
13167 | /* Similar to proto_tree_add_bitmask_value(), but with control of flag values */
13168 | WS_DLL_PUBLIC__attribute__ ((visibility ("default"))) extern proto_item *
13169 | proto_tree_add_bitmask_value_with_flags(proto_tree *parent_tree, tvbuff_t *tvb, const unsigned offset,
13170 | const int hf_hdr, const int ett, int * const *fields, const uint64_t value, const int flags)
13171 | {
13172 | proto_item *item = NULL((void*)0);
13173 | header_field_info *hf;
13174 | int len;
13175 |
13176 | PROTO_REGISTRAR_GET_NTH(hf_hdr,hf)if((hf_hdr == 0 || (unsigned)hf_hdr > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 13176, __func__, "Unregistered hf! index=%d" , hf_hdr); ((void) ((hf_hdr > 0 && (unsigned)hf_hdr < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 13176 , "hf_hdr > 0 && (unsigned)hf_hdr < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hf_hdr] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13176, "gpa_hfinfo.hfi[hf_hdr] != ((void*)0)" , "Unregistered hf!")))) ; hf = gpa_hfinfo.hfi[hf_hdr];;
13177 | DISSECTOR_ASSERT_FIELD_TYPE_IS_INTEGRAL(hf)((void) (((((((hf)->type) == FT_INT8 || ((hf)->type) == FT_INT16 || ((hf)->type) == FT_INT24 || ((hf)->type) == FT_INT32) || (((hf)->type) == FT_INT40 || ((hf)->type) == FT_INT48 || ((hf)->type) == FT_INT56 || ((hf)->type ) == FT_INT64)) || ((((hf)->type) == FT_CHAR || ((hf)-> type) == FT_UINT8 || ((hf)->type) == FT_UINT16 || ((hf)-> type) == FT_UINT24 || ((hf)->type) == FT_UINT32 || ((hf)-> type) == FT_FRAMENUM) || (((hf)->type) == FT_UINT40 || ((hf )->type) == FT_UINT48 || ((hf)->type) == FT_UINT56 || ( (hf)->type) == FT_UINT64)))) ? (void)0 : proto_report_dissector_bug ("%s:%u: field %s is not of type FT_CHAR or an FT_{U}INTn type" , "epan/proto.c", 13177, (hf)->abbrev)));
13178 | /* the proto_tree_add_uint/_uint64() calls below
13179 | will fail if tvb==NULL and len!=0 */
13180 | len = tvb ? ftype_wire_size(hf->type) : 0;
13181 |
13182 | if (parent_tree) {
13183 | if (len <= 4)
13184 | item = proto_tree_add_uint(parent_tree, hf_hdr, tvb, offset, len, (uint32_t)value);
13185 | else
13186 | item = proto_tree_add_uint64(parent_tree, hf_hdr, tvb, offset, len, value);
13187 |
13188 | proto_item_add_bitmask_tree(item, tvb, offset, len, ett, fields,
13189 | flags, false0, false0, NULL((void*)0), value);
13190 | }
13191 |
13192 | return item;
13193 | }
13194 |
13195 | /* Similar to proto_tree_add_bitmask(), but with no "header" item to group all of the fields */
13196 | void
13197 | proto_tree_add_bitmask_list(proto_tree *tree, tvbuff_t *tvb, const unsigned offset,
13198 | const int len, int * const *fields, const unsigned encoding)
13199 | {
13200 | uint64_t value;
13201 |
13202 | if (tree) {
13203 | value = get_uint64_value(tree, tvb, offset, len, encoding);
13204 | proto_item_add_bitmask_tree(NULL((void*)0), tvb, offset, len, -1, fields,
13205 | BMT_NO_APPEND0x01, false0, true1, tree, value);
13206 | }
13207 | }
13208 |
13209 | WS_DLL_PUBLIC__attribute__ ((visibility ("default"))) extern void
13210 | proto_tree_add_bitmask_list_ret_uint64(proto_tree *tree, tvbuff_t *tvb, const unsigned offset,
13211 | const int len, int * const *fields, const unsigned encoding, uint64_t *retval)
13212 | {
13213 | uint64_t value;
13214 |
13215 | value = get_uint64_value(tree, tvb, offset, len, encoding);
13216 | if (tree) {
13217 | proto_item_add_bitmask_tree(NULL((void*)0), tvb, offset, len, -1, fields,
13218 | BMT_NO_APPEND0x01, false0, true1, tree, value);
13219 | }
13220 | if (retval) {
13221 | *retval = value;
13222 | }
13223 | }
13224 |
13225 | WS_DLL_PUBLIC__attribute__ ((visibility ("default"))) extern void
13226 | proto_tree_add_bitmask_list_value(proto_tree *tree, tvbuff_t *tvb, const unsigned offset,
13227 | const int len, int * const *fields, const uint64_t value)
13228 | {
13229 | if (tree) {
13230 | proto_item_add_bitmask_tree(NULL((void*)0), tvb, offset, len, -1, fields,
13231 | BMT_NO_APPEND0x01, false0, true1, tree, value);
13232 | }
13233 | }
13234 |
13235 |
13236 | /* The same as proto_tree_add_bitmask(), but using a caller-supplied length.
13237 | * This is intended to support bitmask fields whose lengths can vary, perhaps
13238 | * as the underlying standard evolves over time.
13239 | * With this API there is the possibility of being called to display more or
13240 | * less data than the dissector was coded to support.
13241 | * In such cases, it is assumed that bitmasks are extended on the MSb end.
13242 | * Thus when presented with "too much" or "too little" data, MSbits will be
13243 | * ignored or MSfields sacrificed.
13244 | *
13245 | * Only fields for which all defined bits are available are displayed.
13246 | */
13247 | proto_item *
13248 | proto_tree_add_bitmask_len(proto_tree *parent_tree, tvbuff_t *tvb,
13249 | const unsigned offset, const unsigned len, const int hf_hdr,
13250 | const int ett, int * const *fields, struct expert_field* exp,
13251 | const unsigned encoding)
13252 | {
13253 | proto_item *item = NULL((void*)0);
13254 | header_field_info *hf;
13255 | unsigned decodable_len;
13256 | unsigned decodable_offset;
13257 | uint32_t decodable_value;
13258 | uint64_t value;
13259 |
13260 | PROTO_REGISTRAR_GET_NTH(hf_hdr, hf)if((hf_hdr == 0 || (unsigned)hf_hdr > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 13260, __func__, "Unregistered hf! index=%d" , hf_hdr); ((void) ((hf_hdr > 0 && (unsigned)hf_hdr < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 13260 , "hf_hdr > 0 && (unsigned)hf_hdr < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hf_hdr] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13260, "gpa_hfinfo.hfi[hf_hdr] != ((void*)0)" , "Unregistered hf!")))) ; hf = gpa_hfinfo.hfi[hf_hdr];;
13261 | DISSECTOR_ASSERT_FIELD_TYPE_IS_INTEGRAL(hf)((void) (((((((hf)->type) == FT_INT8 || ((hf)->type) == FT_INT16 || ((hf)->type) == FT_INT24 || ((hf)->type) == FT_INT32) || (((hf)->type) == FT_INT40 || ((hf)->type) == FT_INT48 || ((hf)->type) == FT_INT56 || ((hf)->type ) == FT_INT64)) || ((((hf)->type) == FT_CHAR || ((hf)-> type) == FT_UINT8 || ((hf)->type) == FT_UINT16 || ((hf)-> type) == FT_UINT24 || ((hf)->type) == FT_UINT32 || ((hf)-> type) == FT_FRAMENUM) || (((hf)->type) == FT_UINT40 || ((hf )->type) == FT_UINT48 || ((hf)->type) == FT_UINT56 || ( (hf)->type) == FT_UINT64)))) ? (void)0 : proto_report_dissector_bug ("%s:%u: field %s is not of type FT_CHAR or an FT_{U}INTn type" , "epan/proto.c", 13261, (hf)->abbrev)));
13262 |
13263 | decodable_offset = offset;
13264 | decodable_len = MIN(len, (unsigned) ftype_wire_size(hf->type))(((len) < ((unsigned) ftype_wire_size(hf->type))) ? (len ) : ((unsigned) ftype_wire_size(hf->type)));
13265 |
13266 | /* If we are ftype_wire_size-limited,
13267 | * make sure we decode as many LSBs as possible.
13268 | */
13269 | if (encoding == ENC_BIG_ENDIAN0x00000000) {
13270 | decodable_offset += (len - decodable_len);
13271 | }
13272 |
13273 | if (parent_tree) {
13274 | decodable_value = get_uint_value(parent_tree, tvb, decodable_offset,
13275 | decodable_len, encoding);
13276 |
13277 | /* The root item covers all the bytes even if we can't decode them all */
13278 | item = proto_tree_add_uint(parent_tree, hf_hdr, tvb, offset, len,
13279 | decodable_value);
13280 | }
13281 |
13282 | if (decodable_len < len) {
13283 | /* Dissector likely requires updating for new protocol revision */
13284 | expert_add_info_format(NULL((void*)0), item, exp,
13285 | "Only least-significant %d of %d bytes decoded",
13286 | decodable_len, len);
13287 | }
13288 |
13289 | if (item) {
13290 | value = get_uint64_value(parent_tree, tvb, decodable_offset, decodable_len, encoding);
13291 | proto_item_add_bitmask_tree(item, tvb, decodable_offset, decodable_len,
13292 | ett, fields, BMT_NO_INT0x02|BMT_NO_TFS0x08, false0, false0, NULL((void*)0), value);
13293 | }
13294 |
13295 | return item;
13296 | }
13297 |
13298 | /* The same as proto_tree_add_bitmask(), but using an arbitrary text as a top-level item */
13299 | proto_item *
13300 | proto_tree_add_bitmask_text(proto_tree *parent_tree, tvbuff_t *tvb,
13301 | const unsigned offset, const unsigned len,
13302 | const char *name, const char *fallback,
13303 | const int ett, int * const *fields,
13304 | const unsigned encoding, const int flags)
13305 | {
13306 | proto_item *item = NULL((void*)0);
13307 | uint64_t value;
13308 |
13309 | if (parent_tree) {
13310 | item = proto_tree_add_text_internal(parent_tree, tvb, offset, len, "%s", name ? name : "");
13311 | value = get_uint64_value(parent_tree, tvb, offset, len, encoding);
13312 | if (proto_item_add_bitmask_tree(item, tvb, offset, len, ett, fields,
13313 | flags, true1, false0, NULL((void*)0), value) && fallback) {
13314 | /* Still at first item - append 'fallback' text if any */
13315 | proto_item_append_text(item, "%s", fallback);
13316 | }
13317 | }
13318 |
13319 | return item;
13320 | }
13321 |
13322 | proto_item *
13323 | proto_tree_add_bits_item(proto_tree *tree, const int hfindex, tvbuff_t *tvb,
13324 | const unsigned bit_offset, const int no_of_bits,
13325 | const unsigned encoding)
13326 | {
13327 | header_field_info *hfinfo;
13328 | int octet_length;
13329 | int octet_offset;
13330 |
13331 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 13331, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 13331 , "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13331, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
13332 |
13333 | if (no_of_bits < 0) {
13334 | THROW(ReportedBoundsError)except_throw(1, (3), ((void*)0));
13335 | }
13336 | octet_length = (no_of_bits + 7) >> 3;
13337 | octet_offset = bit_offset >> 3;
13338 | test_length(hfinfo, tvb, octet_offset, octet_length, encoding);
13339 |
13340 | /* Yes, we try to fake this item again in proto_tree_add_bits_ret_val()
13341 | * but only after doing a bunch more work (which we can, in the common
13342 | * case, shortcut here).
13343 | */
13344 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
13345 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13345 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13345, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13345, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13345, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
13346 |
13347 | return proto_tree_add_bits_ret_val(tree, hfindex, tvb, bit_offset, no_of_bits, NULL((void*)0), encoding);
13348 | }
13349 |
13350 | /*
13351 | * This function will dissect a sequence of bits that does not need to be byte aligned; the bits
13352 | * set will be shown in the tree as ..10 10.. and the integer value returned if return_value is set.
13353 | * Offset should be given in bits from the start of the tvb.
13354 | */
13355 |
13356 | static proto_item *
13357 | _proto_tree_add_bits_ret_val(proto_tree *tree, const int hfindex, tvbuff_t *tvb,
13358 | const unsigned bit_offset, const int no_of_bits,
13359 | uint64_t *return_value, const unsigned encoding)
13360 | {
13361 | int offset;
13362 | unsigned length;
13363 | uint8_t tot_no_bits;
13364 | char *bf_str;
13365 | char lbl_str[ITEM_LABEL_LENGTH240];
13366 | uint64_t value = 0;
13367 | uint8_t *bytes = NULL((void*)0);
13368 | size_t bytes_length = 0;
13369 |
13370 | proto_item *pi;
13371 | header_field_info *hf_field;
13372 |
13373 | /* We can't fake it just yet. We have to fill in the 'return_value' parameter */
13374 | PROTO_REGISTRAR_GET_NTH(hfindex, hf_field)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 13374, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 13374 , "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13374, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hf_field = gpa_hfinfo.hfi[hfindex] ;;
13375 |
13376 | if (hf_field->bitmask != 0) {
13377 | REPORT_DISSECTOR_BUG("Incompatible use of proto_tree_add_bits_ret_val"proto_report_dissector_bug("Incompatible use of proto_tree_add_bits_ret_val" " with field '%s' (%s) with bitmask != 0", hf_field->abbrev , hf_field->name)
13378 | " with field '%s' (%s) with bitmask != 0",proto_report_dissector_bug("Incompatible use of proto_tree_add_bits_ret_val" " with field '%s' (%s) with bitmask != 0", hf_field->abbrev , hf_field->name)
13379 | hf_field->abbrev, hf_field->name)proto_report_dissector_bug("Incompatible use of proto_tree_add_bits_ret_val" " with field '%s' (%s) with bitmask != 0", hf_field->abbrev , hf_field->name);
13380 | }
13381 |
13382 | if (no_of_bits < 0) {
13383 | THROW(ReportedBoundsError)except_throw(1, (3), ((void*)0));
13384 | } else if (no_of_bits == 0) {
13385 | REPORT_DISSECTOR_BUG("field %s passed to proto_tree_add_bits_ret_val() has a bit width of 0",proto_report_dissector_bug("field %s passed to proto_tree_add_bits_ret_val() has a bit width of 0" , hf_field->abbrev)
13386 | hf_field->abbrev)proto_report_dissector_bug("field %s passed to proto_tree_add_bits_ret_val() has a bit width of 0" , hf_field->abbrev);
13387 | }
13388 |
13389 | /* Byte align offset */
13390 | offset = bit_offset>>3;
13391 |
13392 | /*
13393 | * Calculate the number of octets used to hold the bits
13394 | */
13395 | tot_no_bits = ((bit_offset&0x7) + no_of_bits);
13396 | length = (tot_no_bits + 7) >> 3;
13397 |
13398 | if (no_of_bits < 65) {
13399 | value = tvb_get_bits64(tvb, bit_offset, no_of_bits, encoding);
13400 | } else if (hf_field->type != FT_BYTES) {
13401 | REPORT_DISSECTOR_BUG("field %s passed to proto_tree_add_bits_ret_val() has a bit width of %u > 64",proto_report_dissector_bug("field %s passed to proto_tree_add_bits_ret_val() has a bit width of %u > 64" , hf_field->abbrev, no_of_bits)
13402 | hf_field->abbrev, no_of_bits)proto_report_dissector_bug("field %s passed to proto_tree_add_bits_ret_val() has a bit width of %u > 64" , hf_field->abbrev, no_of_bits);
13403 | return NULL((void*)0);
13404 | }
13405 |
13406 | /* Sign extend for signed types */
13407 | switch (hf_field->type) {
13408 | case FT_INT8:
13409 | case FT_INT16:
13410 | case FT_INT24:
13411 | case FT_INT32:
13412 | case FT_INT40:
13413 | case FT_INT48:
13414 | case FT_INT56:
13415 | case FT_INT64:
13416 | value = ws_sign_ext64(value, no_of_bits);
13417 | break;
13418 |
13419 | default:
13420 | break;
13421 | }
13422 |
13423 | if (return_value) {
13424 | *return_value = value;
13425 | }
13426 |
13427 | /* Coast clear. Try and fake it */
13428 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
13429 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hf_field)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13429 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13429, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13429, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hf_field = gpa_hfinfo.hfi[hfindex] ;; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13429, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items); ((tree)-> tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items))); } if (!(( (tree)->tree_data)->visible)) { if (proto_item_is_hidden ((tree))) { if ((hf_field->ref_type != HF_REF_TYPE_DIRECT) && (hf_field->ref_type != HF_REF_TYPE_PRINT) && (hf_field->type != FT_PROTOCOL || ((tree)->tree_data)-> fake_protocols)) { ((void)0); return proto_tree_add_fake_node (tree, hf_field); } } };
13430 |
13431 | bf_str = decode_bits_in_field(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool), bit_offset, no_of_bits, value, encoding);
13432 |
13433 | switch (hf_field->type) {
13434 | case FT_BOOLEAN:
13435 | /* Boolean field */
13436 | return proto_tree_add_boolean_format(tree, hfindex, tvb, offset, length, value,
13437 | "%s = %s: %s",
13438 | bf_str, hf_field->name, tfs_get_string(!!value, hf_field->strings));
13439 | break;
13440 |
13441 | case FT_CHAR:
13442 | pi = proto_tree_add_uint(tree, hfindex, tvb, offset, length, (uint32_t)value);
13443 | fill_label_char(PITEM_FINFO(pi)((pi)->finfo), lbl_str, NULL((void*)0));
13444 | break;
13445 |
13446 | case FT_UINT8:
13447 | case FT_UINT16:
13448 | case FT_UINT24:
13449 | case FT_UINT32:
13450 | pi = proto_tree_add_uint(tree, hfindex, tvb, offset, length, (uint32_t)value);
13451 | fill_label_number(PITEM_FINFO(pi)((pi)->finfo), lbl_str, NULL((void*)0), false0);
13452 | break;
13453 |
13454 | case FT_INT8:
13455 | case FT_INT16:
13456 | case FT_INT24:
13457 | case FT_INT32:
13458 | pi = proto_tree_add_int(tree, hfindex, tvb, offset, length, (int32_t)value);
13459 | fill_label_number(PITEM_FINFO(pi)((pi)->finfo), lbl_str, NULL((void*)0), true1);
13460 | break;
13461 |
13462 | case FT_UINT40:
13463 | case FT_UINT48:
13464 | case FT_UINT56:
13465 | case FT_UINT64:
13466 | pi = proto_tree_add_uint64(tree, hfindex, tvb, offset, length, value);
13467 | fill_label_number64(PITEM_FINFO(pi)((pi)->finfo), lbl_str, NULL((void*)0), false0);
13468 | break;
13469 |
13470 | case FT_INT40:
13471 | case FT_INT48:
13472 | case FT_INT56:
13473 | case FT_INT64:
13474 | pi = proto_tree_add_int64(tree, hfindex, tvb, offset, length, (int64_t)value);
13475 | fill_label_number64(PITEM_FINFO(pi)((pi)->finfo), lbl_str, NULL((void*)0), true1);
13476 | break;
13477 |
13478 | case FT_BYTES:
13479 | bytes = tvb_get_bits_array(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool), tvb, bit_offset, no_of_bits, &bytes_length, encoding);
13480 | pi = proto_tree_add_bytes_with_length(tree, hfindex, tvb, offset, length, bytes, (int) bytes_length);
13481 | proto_item_fill_label(PITEM_FINFO(pi)((pi)->finfo), lbl_str, NULL((void*)0));
13482 | proto_item_set_text(pi, "%s", lbl_str);
13483 | return pi;
13484 |
13485 | /* TODO: should handle FT_UINT_BYTES ? */
13486 |
13487 | default:
13488 | REPORT_DISSECTOR_BUG("field %s has type %d (%s) not handled in proto_tree_add_bits_ret_val()",proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_tree_add_bits_ret_val()" , hf_field->abbrev, hf_field->type, ftype_name(hf_field ->type))
13489 | hf_field->abbrev,proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_tree_add_bits_ret_val()" , hf_field->abbrev, hf_field->type, ftype_name(hf_field ->type))
13490 | hf_field->type,proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_tree_add_bits_ret_val()" , hf_field->abbrev, hf_field->type, ftype_name(hf_field ->type))
13491 | ftype_name(hf_field->type))proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_tree_add_bits_ret_val()" , hf_field->abbrev, hf_field->type, ftype_name(hf_field ->type));
13492 | return NULL((void*)0);
13493 | }
13494 |
13495 | proto_item_set_text(pi, "%s = %s", bf_str, lbl_str);
13496 | return pi;
13497 | }
13498 |
13499 | proto_item *
13500 | proto_tree_add_split_bits_item_ret_val(proto_tree *tree, const int hfindex, tvbuff_t *tvb,
13501 | const unsigned bit_offset, const crumb_spec_t *crumb_spec,
13502 | uint64_t *return_value)
13503 | {
13504 | proto_item *pi;
13505 | int no_of_bits;
13506 | int octet_offset;
13507 | unsigned mask_initial_bit_offset;
13508 | unsigned mask_greatest_bit_offset;
13509 | unsigned octet_length;
13510 | uint8_t i;
13511 | char bf_str[256];
13512 | char lbl_str[ITEM_LABEL_LENGTH240];
13513 | uint64_t value;
13514 | uint64_t composite_bitmask;
13515 | uint64_t composite_bitmap;
13516 |
13517 | header_field_info *hf_field;
13518 |
13519 | /* We can't fake it just yet. We have to fill in the 'return_value' parameter */
13520 | PROTO_REGISTRAR_GET_NTH(hfindex, hf_field)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 13520, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 13520 , "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13520, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hf_field = gpa_hfinfo.hfi[hfindex] ;;
1 | Assuming 'hfindex' is not equal to 0 | →
2 | ← | Assuming 'hfindex' is <= field 'len' | →
3 | ← | Assuming 'hfindex' is > 0 | →
4 | ← | Assuming 'hfindex' is < field 'len' | →
5 | ← | '?' condition is true | →
6 | ← | Assuming the condition is true | →
7 | ← | '?' condition is true | →
13521 |
13522 | if (hf_field->bitmask != 0) {
8 | ← | Assuming field 'bitmask' is equal to 0 | →
9 | ← | Taking false branch | →
13523 | REPORT_DISSECTOR_BUG("Incompatible use of proto_tree_add_split_bits_item_ret_val"proto_report_dissector_bug("Incompatible use of proto_tree_add_split_bits_item_ret_val" " with field '%s' (%s) with bitmask != 0", hf_field->abbrev , hf_field->name)
13524 | " with field '%s' (%s) with bitmask != 0",proto_report_dissector_bug("Incompatible use of proto_tree_add_split_bits_item_ret_val" " with field '%s' (%s) with bitmask != 0", hf_field->abbrev , hf_field->name)
13525 | hf_field->abbrev, hf_field->name)proto_report_dissector_bug("Incompatible use of proto_tree_add_split_bits_item_ret_val" " with field '%s' (%s) with bitmask != 0", hf_field->abbrev , hf_field->name);
13526 | }
13527 |
13528 | mask_initial_bit_offset = bit_offset % 8;
13529 |
13530 | no_of_bits = 0;
13531 | value = 0;
13532 | i = 0;
13533 | mask_greatest_bit_offset = 0;
13534 | composite_bitmask = 0;
13535 | composite_bitmap = 0;
13536 |
13537 | while (crumb_spec[i].crumb_bit_length != 0) {
10 | ← | Assuming field 'crumb_bit_length' is not equal to 0 | →
11 | ← | Loop condition is true. Entering loop body | →
13538 | uint64_t crumb_mask, crumb_value;
13539 | uint8_t crumb_end_bit_offset;
13540 |
13541 | crumb_value = tvb_get_bits64(tvb,
13542 | bit_offset + crumb_spec[i].crumb_bit_offset,
13543 | crumb_spec[i].crumb_bit_length,
13544 | ENC_BIG_ENDIAN0x00000000);
13545 | value += crumb_value;
13546 | no_of_bits += crumb_spec[i].crumb_bit_length;
13547 | DISSECTOR_ASSERT_HINT(no_of_bits <= 64, "a value larger than 64 bits cannot be represented")((void) ((no_of_bits <= 64) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 13547 , "no_of_bits <= 64", "a value larger than 64 bits cannot be represented" ))));
12 | ← | Assuming 'no_of_bits' is <= 64 | →
13 | ← | '?' condition is true | →
13548 |
13549 | /* The bitmask is 64 bit, left-aligned, starting at the first bit of the
13550 | octet containing the initial offset.
13551 | If the mask is beyond 32 bits, then give up on bit map display.
13552 | This could be improved in future, probably showing a table
13553 | of 32 or 64 bits per row */
13554 | if (mask_greatest_bit_offset
13.1 | 'mask_greatest_bit_offset' is < 32
< 32) {
14 | ← | Taking true branch | →
13555 | crumb_end_bit_offset = mask_initial_bit_offset
13556 | + crumb_spec[i].crumb_bit_offset
13557 | + crumb_spec[i].crumb_bit_length;
13558 | crumb_mask = (UINT64_C(1)1UL << crumb_spec[i].crumb_bit_length) - 1;
15 | ← | Assuming right operand of bit shift is less than 64 | →
16 | ← | Value assigned to 'crumb_mask' | →
13559 |
13560 | if (crumb_end_bit_offset > mask_greatest_bit_offset) {
17 | ← | Assuming 'crumb_end_bit_offset' is <= 'mask_greatest_bit_offset' | →
18 | ← | Taking false branch | →
13561 | mask_greatest_bit_offset = crumb_end_bit_offset;
13562 | }
13563 | /* Currently the bitmap of the crumbs are only shown if
13564 | * smaller than 32 bits. Do not bother calculating the
13565 | * mask if it is larger than that. */
13566 | if (crumb_end_bit_offset
18.1 | 'crumb_end_bit_offset' is <= 32
<= 32) {
19 | ← | Taking true branch | →
13567 | composite_bitmask |= (crumb_mask << (64 - crumb_end_bit_offset));
20 | ← | The result of left shift is undefined because the right operand '64' is not smaller than 64, the capacity of 'uint64_t'
13568 | composite_bitmap |= (crumb_value << (64 - crumb_end_bit_offset));
13569 | }
13570 | }
13571 | /* Shift left for the next segment */
13572 | value <<= crumb_spec[++i].crumb_bit_length;
13573 | }
13574 |
13575 | /* Sign extend for signed types */
13576 | switch (hf_field->type) {
13577 | case FT_INT8:
13578 | case FT_INT16:
13579 | case FT_INT24:
13580 | case FT_INT32:
13581 | case FT_INT40:
13582 | case FT_INT48:
13583 | case FT_INT56:
13584 | case FT_INT64:
13585 | value = ws_sign_ext64(value, no_of_bits);
13586 | break;
13587 | default:
13588 | break;
13589 | }
13590 |
13591 | if (return_value) {
13592 | *return_value = value;
13593 | }
13594 |
13595 | /* Coast clear. Try and fake it */
13596 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
13597 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hf_field)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13597 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13597, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13597, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hf_field = gpa_hfinfo.hfi[hfindex] ;; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13597, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items); ((tree)-> tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items))); } if (!(( (tree)->tree_data)->visible)) { if (proto_item_is_hidden ((tree))) { if ((hf_field->ref_type != HF_REF_TYPE_DIRECT) && (hf_field->ref_type != HF_REF_TYPE_PRINT) && (hf_field->type != FT_PROTOCOL || ((tree)->tree_data)-> fake_protocols)) { ((void)0); return proto_tree_add_fake_node (tree, hf_field); } } };
13598 |
13599 | /* initialise the format string */
13600 | bf_str[0] = '\0';
13601 |
13602 | octet_offset = bit_offset >> 3;
13603 |
13604 | /* Round up mask length to nearest octet */
13605 | octet_length = ((mask_greatest_bit_offset + 7) >> 3);
13606 | mask_greatest_bit_offset = octet_length << 3;
13607 |
13608 | /* As noted above, we currently only produce a bitmap if the crumbs span less than 4 octets of the tvb.
13609 | It would be a useful enhancement to eliminate this restriction. */
13610 | if (mask_greatest_bit_offset > 0 && mask_greatest_bit_offset <= 32) {
13611 | other_decode_bitfield_value(bf_str,
13612 | (uint32_t)(composite_bitmap >> (64 - mask_greatest_bit_offset)),
13613 | (uint32_t)(composite_bitmask >> (64 - mask_greatest_bit_offset)),
13614 | mask_greatest_bit_offset);
13615 | } else {
13616 | /* If the bitmask is too large, try to describe its contents. */
13617 | snprintf(bf_str, sizeof(bf_str), "%d bits", no_of_bits);
13618 | }
13619 |
13620 | switch (hf_field->type) {
13621 | case FT_BOOLEAN: /* it is a bit odd to have a boolean encoded as split-bits, but possible, I suppose? */
13622 | /* Boolean field */
13623 | return proto_tree_add_boolean_format(tree, hfindex,
13624 | tvb, octet_offset, octet_length, value,
13625 | "%s = %s: %s",
13626 | bf_str, hf_field->name, tfs_get_string(!!value, hf_field->strings));
13627 | break;
13628 |
13629 | case FT_CHAR:
13630 | pi = proto_tree_add_uint(tree, hfindex, tvb, octet_offset, octet_length, (uint32_t)value);
13631 | fill_label_char(PITEM_FINFO(pi)((pi)->finfo), lbl_str, NULL((void*)0));
13632 | break;
13633 |
13634 | case FT_UINT8:
13635 | case FT_UINT16:
13636 | case FT_UINT24:
13637 | case FT_UINT32:
13638 | pi = proto_tree_add_uint(tree, hfindex, tvb, octet_offset, octet_length, (uint32_t)value);
13639 | fill_label_number(PITEM_FINFO(pi)((pi)->finfo), lbl_str, NULL((void*)0), false0);
13640 | break;
13641 |
13642 | case FT_INT8:
13643 | case FT_INT16:
13644 | case FT_INT24:
13645 | case FT_INT32:
13646 | pi = proto_tree_add_int(tree, hfindex, tvb, octet_offset, octet_length, (int32_t)value);
13647 | fill_label_number(PITEM_FINFO(pi)((pi)->finfo), lbl_str, NULL((void*)0), true1);
13648 | break;
13649 |
13650 | case FT_UINT40:
13651 | case FT_UINT48:
13652 | case FT_UINT56:
13653 | case FT_UINT64:
13654 | pi = proto_tree_add_uint64(tree, hfindex, tvb, octet_offset, octet_length, value);
13655 | fill_label_number64(PITEM_FINFO(pi)((pi)->finfo), lbl_str, NULL((void*)0), false0);
13656 | break;
13657 |
13658 | case FT_INT40:
13659 | case FT_INT48:
13660 | case FT_INT56:
13661 | case FT_INT64:
13662 | pi = proto_tree_add_int64(tree, hfindex, tvb, octet_offset, octet_length, (int64_t)value);
13663 | fill_label_number64(PITEM_FINFO(pi)((pi)->finfo), lbl_str, NULL((void*)0), true1);
13664 | break;
13665 |
13666 | default:
13667 | REPORT_DISSECTOR_BUG("field %s has type %d (%s) not handled in proto_tree_add_split_bits_item_ret_val()",proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_tree_add_split_bits_item_ret_val()" , hf_field->abbrev, hf_field->type, ftype_name(hf_field ->type))
13668 | hf_field->abbrev,proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_tree_add_split_bits_item_ret_val()" , hf_field->abbrev, hf_field->type, ftype_name(hf_field ->type))
13669 | hf_field->type,proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_tree_add_split_bits_item_ret_val()" , hf_field->abbrev, hf_field->type, ftype_name(hf_field ->type))
13670 | ftype_name(hf_field->type))proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_tree_add_split_bits_item_ret_val()" , hf_field->abbrev, hf_field->type, ftype_name(hf_field ->type));
13671 | return NULL((void*)0);
13672 | }
13673 | proto_item_set_text(pi, "%s = %s", bf_str, lbl_str);
13674 | return pi;
13675 | }
13676 |
13677 | void
13678 | proto_tree_add_split_bits_crumb(proto_tree *tree, const int hfindex, tvbuff_t *tvb, const unsigned bit_offset,
13679 | const crumb_spec_t *crumb_spec, uint16_t crumb_index)
13680 | {
13681 | header_field_info *hfinfo;
13682 | int start = bit_offset >> 3;
13683 | int length = ((bit_offset + crumb_spec[crumb_index].crumb_bit_length - 1) >> 3) - (bit_offset >> 3) + 1;
13684 |
13685 | /* We have to duplicate this length check from proto_tree_add_text_internal in order to check for a null tree
13686 | * so that we can use the tree's memory scope in calculating the string */
13687 | if (length == -1) {
13688 | tvb_captured_length(tvb) ? tvb_ensure_captured_length_remaining(tvb, start) : 0;
13689 | } else {
13690 | tvb_ensure_bytes_exist(tvb, start, length);
13691 | }
13692 | if (!tree) return;
13693 |
13694 | PROTO_REGISTRAR_GET_NTH(hfindex, hfinfo)if((hfindex == 0 || (unsigned)hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 13694, __func__, "Unregistered hf! index=%d" , hfindex); ((void) ((hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 13694 , "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13694, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];;
13695 | proto_tree_add_text_internal(tree, tvb, start, length,
13696 | "%s crumb %d of %s (decoded above)",
13697 | decode_bits_in_field(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool), bit_offset, crumb_spec[crumb_index].crumb_bit_length,
13698 | tvb_get_bits32(tvb,
13699 | bit_offset,
13700 | crumb_spec[crumb_index].crumb_bit_length,
13701 | ENC_BIG_ENDIAN0x00000000),
13702 | ENC_BIG_ENDIAN0x00000000),
13703 | crumb_index,
13704 | hfinfo->name);
13705 | }
13706 |
13707 | proto_item *
13708 | proto_tree_add_bits_ret_val(proto_tree *tree, const int hfindex, tvbuff_t *tvb,
13709 | const unsigned bit_offset, const int no_of_bits,
13710 | uint64_t *return_value, const unsigned encoding)
13711 | {
13712 | proto_item *item;
13713 |
13714 | if ((item = _proto_tree_add_bits_ret_val(tree, hfindex, tvb,
13715 | bit_offset, no_of_bits,
13716 | return_value, encoding))) {
13717 | FI_SET_FLAG(PNODE_FINFO(item), FI_BITS_OFFSET(bit_offset&0x7))do { if (((item)->finfo)) (((item)->finfo))->flags = (((item)->finfo))->flags | ((((bit_offset&0x7) & 63) << 5)); } while(0);
13718 | FI_SET_FLAG(PNODE_FINFO(item), FI_BITS_SIZE(no_of_bits))do { if (((item)->finfo)) (((item)->finfo))->flags = (((item)->finfo))->flags | ((((no_of_bits) & 63) << 12)); } while(0);
13719 | }
13720 | return item;
13721 | }
13722 |
13723 | static proto_item *
13724 | _proto_tree_add_bits_format_value(proto_tree *tree, const int hfindex,
13725 | tvbuff_t *tvb, const unsigned bit_offset,
13726 | const int no_of_bits, void *value_ptr,
13727 | const unsigned encoding, char *value_str)
13728 | {
13729 | int offset;
13730 | unsigned length;
13731 | uint8_t tot_no_bits;
13732 | char *str;
13733 | uint64_t value = 0;
13734 | header_field_info *hf_field;
13735 |
13736 | /* We do not have to return a value, try to fake it as soon as possible */
13737 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
13738 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hf_field)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13738 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13738, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13738, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hf_field = gpa_hfinfo.hfi[hfindex] ;; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13738, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items); ((tree)-> tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items))); } if (!(( (tree)->tree_data)->visible)) { if (proto_item_is_hidden ((tree))) { if ((hf_field->ref_type != HF_REF_TYPE_DIRECT) && (hf_field->ref_type != HF_REF_TYPE_PRINT) && (hf_field->type != FT_PROTOCOL || ((tree)->tree_data)-> fake_protocols)) { ((void)0); return proto_tree_add_fake_node (tree, hf_field); } } };
13739 |
13740 | if (hf_field->bitmask != 0) {
13741 | REPORT_DISSECTOR_BUG("Incompatible use of proto_tree_add_bits_format_value"proto_report_dissector_bug("Incompatible use of proto_tree_add_bits_format_value" " with field '%s' (%s) with bitmask != 0", hf_field->abbrev , hf_field->name)
13742 | " with field '%s' (%s) with bitmask != 0",proto_report_dissector_bug("Incompatible use of proto_tree_add_bits_format_value" " with field '%s' (%s) with bitmask != 0", hf_field->abbrev , hf_field->name)
13743 | hf_field->abbrev, hf_field->name)proto_report_dissector_bug("Incompatible use of proto_tree_add_bits_format_value" " with field '%s' (%s) with bitmask != 0", hf_field->abbrev , hf_field->name);
13744 | }
13745 |
13746 | if (no_of_bits < 0) {
13747 | THROW(ReportedBoundsError)except_throw(1, (3), ((void*)0));
13748 | } else if (no_of_bits == 0) {
13749 | REPORT_DISSECTOR_BUG("field %s passed to proto_tree_add_bits_format_value() has a bit width of 0",proto_report_dissector_bug("field %s passed to proto_tree_add_bits_format_value() has a bit width of 0" , hf_field->abbrev)
13750 | hf_field->abbrev)proto_report_dissector_bug("field %s passed to proto_tree_add_bits_format_value() has a bit width of 0" , hf_field->abbrev);
13751 | }
13752 |
13753 | /* Byte align offset */
13754 | offset = bit_offset>>3;
13755 |
13756 | /*
13757 | * Calculate the number of octets used to hold the bits
13758 | */
13759 | tot_no_bits = ((bit_offset&0x7) + no_of_bits);
13760 | length = tot_no_bits>>3;
13761 | /* If we are using part of the next octet, increase length by 1 */
13762 | if (tot_no_bits & 0x07)
13763 | length++;
13764 |
13765 | if (no_of_bits < 65) {
13766 | value = tvb_get_bits64(tvb, bit_offset, no_of_bits, encoding);
13767 | } else {
13768 | REPORT_DISSECTOR_BUG("field %s passed to proto_tree_add_bits_format_value() has a bit width of %u > 65",proto_report_dissector_bug("field %s passed to proto_tree_add_bits_format_value() has a bit width of %u > 65" , hf_field->abbrev, no_of_bits)
13769 | hf_field->abbrev, no_of_bits)proto_report_dissector_bug("field %s passed to proto_tree_add_bits_format_value() has a bit width of %u > 65" , hf_field->abbrev, no_of_bits);
13770 | return NULL((void*)0);
13771 | }
13772 |
13773 | str = decode_bits_in_field(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool), bit_offset, no_of_bits, value, encoding);
13774 |
13775 | (void) g_strlcat(str, " = ", 256+64);
13776 | (void) g_strlcat(str, hf_field->name, 256+64);
13777 |
13778 | /*
13779 | * This function does not receive an actual value but a dimensionless pointer to that value.
13780 | * For this reason, the type of the header field is examined in order to determine
13781 | * what kind of value we should read from this address.
13782 | * The caller of this function must make sure that for the specific header field type the address of
13783 | * a compatible value is provided.
13784 | */
13785 | switch (hf_field->type) {
13786 | case FT_BOOLEAN:
13787 | return proto_tree_add_boolean_format(tree, hfindex, tvb, offset, length, *(uint64_t *)value_ptr,
13788 | "%s: %s", str, value_str);
13789 | break;
13790 |
13791 | case FT_CHAR:
13792 | case FT_UINT8:
13793 | case FT_UINT16:
13794 | case FT_UINT24:
13795 | case FT_UINT32:
13796 | return proto_tree_add_uint_format(tree, hfindex, tvb, offset, length, *(uint32_t *)value_ptr,
13797 | "%s: %s", str, value_str);
13798 | break;
13799 |
13800 | case FT_UINT40:
13801 | case FT_UINT48:
13802 | case FT_UINT56:
13803 | case FT_UINT64:
13804 | return proto_tree_add_uint64_format(tree, hfindex, tvb, offset, length, *(uint64_t *)value_ptr,
13805 | "%s: %s", str, value_str);
13806 | break;
13807 |
13808 | case FT_INT8:
13809 | case FT_INT16:
13810 | case FT_INT24:
13811 | case FT_INT32:
13812 | return proto_tree_add_int_format(tree, hfindex, tvb, offset, length, *(int32_t *)value_ptr,
13813 | "%s: %s", str, value_str);
13814 | break;
13815 |
13816 | case FT_INT40:
13817 | case FT_INT48:
13818 | case FT_INT56:
13819 | case FT_INT64:
13820 | return proto_tree_add_int64_format(tree, hfindex, tvb, offset, length, *(int64_t *)value_ptr,
13821 | "%s: %s", str, value_str);
13822 | break;
13823 |
13824 | case FT_FLOAT:
13825 | return proto_tree_add_float_format(tree, hfindex, tvb, offset, length, *(float *)value_ptr,
13826 | "%s: %s", str, value_str);
13827 | break;
13828 |
13829 | default:
13830 | REPORT_DISSECTOR_BUG("field %s has type %d (%s) not handled in proto_tree_add_bits_format_value()",proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_tree_add_bits_format_value()" , hf_field->abbrev, hf_field->type, ftype_name(hf_field ->type))
13831 | hf_field->abbrev,proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_tree_add_bits_format_value()" , hf_field->abbrev, hf_field->type, ftype_name(hf_field ->type))
13832 | hf_field->type,proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_tree_add_bits_format_value()" , hf_field->abbrev, hf_field->type, ftype_name(hf_field ->type))
13833 | ftype_name(hf_field->type))proto_report_dissector_bug("field %s has type %d (%s) not handled in proto_tree_add_bits_format_value()" , hf_field->abbrev, hf_field->type, ftype_name(hf_field ->type));
13834 | return NULL((void*)0);
13835 | }
13836 | }
13837 |
13838 | static proto_item *
13839 | proto_tree_add_bits_format_value(proto_tree *tree, const int hfindex,
13840 | tvbuff_t *tvb, const unsigned bit_offset,
13841 | const int no_of_bits, void *value_ptr,
13842 | const unsigned encoding, char *value_str)
13843 | {
13844 | proto_item *item;
13845 |
13846 | if ((item = _proto_tree_add_bits_format_value(tree, hfindex,
13847 | tvb, bit_offset, no_of_bits,
13848 | value_ptr, encoding, value_str))) {
13849 | FI_SET_FLAG(PNODE_FINFO(item), FI_BITS_OFFSET(bit_offset&0x7))do { if (((item)->finfo)) (((item)->finfo))->flags = (((item)->finfo))->flags | ((((bit_offset&0x7) & 63) << 5)); } while(0);
13850 | FI_SET_FLAG(PNODE_FINFO(item), FI_BITS_SIZE(no_of_bits))do { if (((item)->finfo)) (((item)->finfo))->flags = (((item)->finfo))->flags | ((((no_of_bits) & 63) << 12)); } while(0);
13851 | }
13852 | return item;
13853 | }
13854 |
13855 | #define CREATE_VALUE_STRING(tree,dst,format,ap)__builtin_va_start(ap, format); dst = wmem_strdup_vprintf(((tree )->tree_data->pinfo->pool), format, ap); __builtin_va_end (ap); \
13856 | va_start(ap, format)__builtin_va_start(ap, format); \
13857 | dst = wmem_strdup_vprintf(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool), format, ap); \
13858 | va_end(ap)__builtin_va_end(ap);
13859 |
13860 | proto_item *
13861 | proto_tree_add_uint_bits_format_value(proto_tree *tree, const int hfindex,
13862 | tvbuff_t *tvb, const unsigned bit_offset,
13863 | const int no_of_bits, uint32_t value,
13864 | const unsigned encoding,
13865 | const char *format, ...)
13866 | {
13867 | va_list ap;
13868 | char *dst;
13869 | header_field_info *hf_field;
13870 |
13871 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
13872 |
13873 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hf_field)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13873 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13873, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13873, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hf_field = gpa_hfinfo.hfi[hfindex] ;; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13873, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items); ((tree)-> tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items))); } if (!(( (tree)->tree_data)->visible)) { if (proto_item_is_hidden ((tree))) { if ((hf_field->ref_type != HF_REF_TYPE_DIRECT) && (hf_field->ref_type != HF_REF_TYPE_PRINT) && (hf_field->type != FT_PROTOCOL || ((tree)->tree_data)-> fake_protocols)) { ((void)0); return proto_tree_add_fake_node (tree, hf_field); } } };
13874 |
13875 | switch (hf_field->type) {
13876 | case FT_UINT8:
13877 | case FT_UINT16:
13878 | case FT_UINT24:
13879 | case FT_UINT32:
13880 | break;
13881 |
13882 | default:
13883 | REPORT_DISSECTOR_BUG("field %s is not of type FT_UINT8, FT_UINT16, FT_UINT24, or FT_UINT32",proto_report_dissector_bug("field %s is not of type FT_UINT8, FT_UINT16, FT_UINT24, or FT_UINT32" , hf_field->abbrev)
13884 | hf_field->abbrev)proto_report_dissector_bug("field %s is not of type FT_UINT8, FT_UINT16, FT_UINT24, or FT_UINT32" , hf_field->abbrev);
13885 | return NULL((void*)0);
13886 | }
13887 |
13888 | CREATE_VALUE_STRING(tree, dst, format, ap)__builtin_va_start(ap, format); dst = wmem_strdup_vprintf(((tree )->tree_data->pinfo->pool), format, ap); __builtin_va_end (ap);;
13889 |
13890 | return proto_tree_add_bits_format_value(tree, hfindex, tvb, bit_offset, no_of_bits, &value, encoding, dst);
13891 | }
13892 |
13893 | proto_item *
13894 | proto_tree_add_uint64_bits_format_value(proto_tree *tree, const int hfindex,
13895 | tvbuff_t *tvb, const unsigned bit_offset,
13896 | const int no_of_bits, uint64_t value,
13897 | const unsigned encoding,
13898 | const char *format, ...)
13899 | {
13900 | va_list ap;
13901 | char *dst;
13902 | header_field_info *hf_field;
13903 |
13904 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
13905 |
13906 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hf_field)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13906 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13906, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13906, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hf_field = gpa_hfinfo.hfi[hfindex] ;; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13906, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items); ((tree)-> tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items))); } if (!(( (tree)->tree_data)->visible)) { if (proto_item_is_hidden ((tree))) { if ((hf_field->ref_type != HF_REF_TYPE_DIRECT) && (hf_field->ref_type != HF_REF_TYPE_PRINT) && (hf_field->type != FT_PROTOCOL || ((tree)->tree_data)-> fake_protocols)) { ((void)0); return proto_tree_add_fake_node (tree, hf_field); } } };
13907 |
13908 | switch (hf_field->type) {
13909 | case FT_UINT40:
13910 | case FT_UINT48:
13911 | case FT_UINT56:
13912 | case FT_UINT64:
13913 | break;
13914 |
13915 | default:
13916 | REPORT_DISSECTOR_BUG("field %s is not of type FT_UINT40, FT_UINT48, FT_UINT56, or FT_UINT64",proto_report_dissector_bug("field %s is not of type FT_UINT40, FT_UINT48, FT_UINT56, or FT_UINT64" , hf_field->abbrev)
13917 | hf_field->abbrev)proto_report_dissector_bug("field %s is not of type FT_UINT40, FT_UINT48, FT_UINT56, or FT_UINT64" , hf_field->abbrev);
13918 | return NULL((void*)0);
13919 | }
13920 |
13921 | CREATE_VALUE_STRING(tree, dst, format, ap)__builtin_va_start(ap, format); dst = wmem_strdup_vprintf(((tree )->tree_data->pinfo->pool), format, ap); __builtin_va_end (ap);;
13922 |
13923 | return proto_tree_add_bits_format_value(tree, hfindex, tvb, bit_offset, no_of_bits, &value, encoding, dst);
13924 | }
13925 |
13926 | proto_item *
13927 | proto_tree_add_float_bits_format_value(proto_tree *tree, const int hfindex,
13928 | tvbuff_t *tvb, const unsigned bit_offset,
13929 | const int no_of_bits, float value,
13930 | const unsigned encoding,
13931 | const char *format, ...)
13932 | {
13933 | va_list ap;
13934 | char *dst;
13935 | header_field_info *hf_field;
13936 |
13937 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
13938 |
13939 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hf_field)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13939 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13939, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13939, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hf_field = gpa_hfinfo.hfi[hfindex] ;; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13939, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items); ((tree)-> tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items))); } if (!(( (tree)->tree_data)->visible)) { if (proto_item_is_hidden ((tree))) { if ((hf_field->ref_type != HF_REF_TYPE_DIRECT) && (hf_field->ref_type != HF_REF_TYPE_PRINT) && (hf_field->type != FT_PROTOCOL || ((tree)->tree_data)-> fake_protocols)) { ((void)0); return proto_tree_add_fake_node (tree, hf_field); } } };
13940 |
13941 | DISSECTOR_ASSERT_FIELD_TYPE(hf_field, FT_FLOAT)((void) (((hf_field)->type == FT_FLOAT) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_FLOAT", "epan/proto.c", 13941, ((hf_field))->abbrev))));
13942 |
13943 | CREATE_VALUE_STRING(tree, dst, format, ap)__builtin_va_start(ap, format); dst = wmem_strdup_vprintf(((tree )->tree_data->pinfo->pool), format, ap); __builtin_va_end (ap);;
13944 |
13945 | return proto_tree_add_bits_format_value(tree, hfindex, tvb, bit_offset, no_of_bits, &value, encoding, dst);
13946 | }
13947 |
13948 | proto_item *
13949 | proto_tree_add_int_bits_format_value(proto_tree *tree, const int hfindex,
13950 | tvbuff_t *tvb, const unsigned bit_offset,
13951 | const int no_of_bits, int32_t value,
13952 | const unsigned encoding,
13953 | const char *format, ...)
13954 | {
13955 | va_list ap;
13956 | char *dst;
13957 | header_field_info *hf_field;
13958 |
13959 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
13960 |
13961 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hf_field)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13961 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13961, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13961, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hf_field = gpa_hfinfo.hfi[hfindex] ;; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13961, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items); ((tree)-> tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items))); } if (!(( (tree)->tree_data)->visible)) { if (proto_item_is_hidden ((tree))) { if ((hf_field->ref_type != HF_REF_TYPE_DIRECT) && (hf_field->ref_type != HF_REF_TYPE_PRINT) && (hf_field->type != FT_PROTOCOL || ((tree)->tree_data)-> fake_protocols)) { ((void)0); return proto_tree_add_fake_node (tree, hf_field); } } };
13962 |
13963 | switch (hf_field->type) {
13964 | case FT_INT8:
13965 | case FT_INT16:
13966 | case FT_INT24:
13967 | case FT_INT32:
13968 | break;
13969 |
13970 | default:
13971 | REPORT_DISSECTOR_BUG("field %s is not of type FT_INT8, FT_INT16, FT_INT24, or FT_INT32",proto_report_dissector_bug("field %s is not of type FT_INT8, FT_INT16, FT_INT24, or FT_INT32" , hf_field->abbrev)
13972 | hf_field->abbrev)proto_report_dissector_bug("field %s is not of type FT_INT8, FT_INT16, FT_INT24, or FT_INT32" , hf_field->abbrev);
13973 | return NULL((void*)0);
13974 | }
13975 |
13976 | CREATE_VALUE_STRING(tree, dst, format, ap)__builtin_va_start(ap, format); dst = wmem_strdup_vprintf(((tree )->tree_data->pinfo->pool), format, ap); __builtin_va_end (ap);;
13977 |
13978 | return proto_tree_add_bits_format_value(tree, hfindex, tvb, bit_offset, no_of_bits, &value, encoding, dst);
13979 | }
13980 |
13981 | proto_item *
13982 | proto_tree_add_int64_bits_format_value(proto_tree *tree, const int hfindex,
13983 | tvbuff_t *tvb, const unsigned bit_offset,
13984 | const int no_of_bits, int64_t value,
13985 | const unsigned encoding,
13986 | const char *format, ...)
13987 | {
13988 | va_list ap;
13989 | char *dst;
13990 | header_field_info *hf_field;
13991 |
13992 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
13993 |
13994 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hf_field)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13994 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13994, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 13994, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hf_field = gpa_hfinfo.hfi[hfindex] ;; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 13994, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items); ((tree)-> tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items))); } if (!(( (tree)->tree_data)->visible)) { if (proto_item_is_hidden ((tree))) { if ((hf_field->ref_type != HF_REF_TYPE_DIRECT) && (hf_field->ref_type != HF_REF_TYPE_PRINT) && (hf_field->type != FT_PROTOCOL || ((tree)->tree_data)-> fake_protocols)) { ((void)0); return proto_tree_add_fake_node (tree, hf_field); } } };
13995 |
13996 | switch (hf_field->type) {
13997 | case FT_INT40:
13998 | case FT_INT48:
13999 | case FT_INT56:
14000 | case FT_INT64:
14001 | break;
14002 |
14003 | default:
14004 | REPORT_DISSECTOR_BUG("field %s is not of type FT_INT40, FT_INT48, FT_INT56, or FT_INT64",proto_report_dissector_bug("field %s is not of type FT_INT40, FT_INT48, FT_INT56, or FT_INT64" , hf_field->abbrev)
14005 | hf_field->abbrev)proto_report_dissector_bug("field %s is not of type FT_INT40, FT_INT48, FT_INT56, or FT_INT64" , hf_field->abbrev);
14006 | return NULL((void*)0);
14007 | }
14008 |
14009 | CREATE_VALUE_STRING(tree, dst, format, ap)__builtin_va_start(ap, format); dst = wmem_strdup_vprintf(((tree )->tree_data->pinfo->pool), format, ap); __builtin_va_end (ap);;
14010 |
14011 | return proto_tree_add_bits_format_value(tree, hfindex, tvb, bit_offset, no_of_bits, &value, encoding, dst);
14012 | }
14013 |
14014 | proto_item *
14015 | proto_tree_add_boolean_bits_format_value(proto_tree *tree, const int hfindex,
14016 | tvbuff_t *tvb, const unsigned bit_offset,
14017 | const int no_of_bits, uint64_t value,
14018 | const unsigned encoding,
14019 | const char *format, ...)
14020 | {
14021 | va_list ap;
14022 | char *dst;
14023 | header_field_info *hf_field;
14024 |
14025 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
14026 |
14027 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hf_field)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 14027 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 14027, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 14027, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hf_field = gpa_hfinfo.hfi[hfindex] ;; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 14027, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items); ((tree)-> tree_data)->count = 0; except_throw(1, (6), (wmem_strdup_printf (((tree)->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hf_field->abbrev, prefs.gui_max_tree_items))); } if (!(( (tree)->tree_data)->visible)) { if (proto_item_is_hidden ((tree))) { if ((hf_field->ref_type != HF_REF_TYPE_DIRECT) && (hf_field->ref_type != HF_REF_TYPE_PRINT) && (hf_field->type != FT_PROTOCOL || ((tree)->tree_data)-> fake_protocols)) { ((void)0); return proto_tree_add_fake_node (tree, hf_field); } } };
14028 |
14029 | DISSECTOR_ASSERT_FIELD_TYPE(hf_field, FT_BOOLEAN)((void) (((hf_field)->type == FT_BOOLEAN) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_BOOLEAN", "epan/proto.c" , 14029, ((hf_field))->abbrev))));
14030 |
14031 | CREATE_VALUE_STRING(tree, dst, format, ap)__builtin_va_start(ap, format); dst = wmem_strdup_vprintf(((tree )->tree_data->pinfo->pool), format, ap); __builtin_va_end (ap);;
14032 |
14033 | return proto_tree_add_bits_format_value(tree, hfindex, tvb, bit_offset, no_of_bits, &value, encoding, dst);
14034 | }
14035 |
14036 | proto_item *
14037 | proto_tree_add_ts_23_038_7bits_packed_item(proto_tree *tree, const int hfindex, tvbuff_t *tvb,
14038 | const unsigned bit_offset, const int no_of_chars)
14039 | {
14040 | proto_item *pi;
14041 | header_field_info *hfinfo;
14042 | int byte_length;
14043 | int byte_offset;
14044 | char *string;
14045 |
14046 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
14047 |
14048 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 14048 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 14048, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 14048, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 14048, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
14049 |
14050 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_STRING)((void) (((hfinfo)->type == FT_STRING) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_STRING", "epan/proto.c" , 14050, ((hfinfo))->abbrev))));
14051 |
14052 | byte_length = (((no_of_chars + 1) * 7) + (bit_offset & 0x07)) >> 3;
14053 | byte_offset = bit_offset >> 3;
14054 |
14055 | string = tvb_get_ts_23_038_7bits_string_packed(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool), tvb, bit_offset, no_of_chars);
14056 |
14057 | pi = proto_tree_add_pi(tree, hfinfo, tvb, byte_offset, &byte_length);
14058 | DISSECTOR_ASSERT(byte_length >= 0)((void) ((byte_length >= 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 14058, "byte_length >= 0" ))));
14059 | proto_tree_set_string(PNODE_FINFO(pi)((pi)->finfo), string);
14060 |
14061 | return pi;
14062 | }
14063 |
14064 | proto_item *
14065 | proto_tree_add_ascii_7bits_item(proto_tree *tree, const int hfindex, tvbuff_t *tvb,
14066 | const unsigned bit_offset, const int no_of_chars)
14067 | {
14068 | proto_item *pi;
14069 | header_field_info *hfinfo;
14070 | int byte_length;
14071 | int byte_offset;
14072 | char *string;
14073 |
14074 | CHECK_FOR_NULL_TREE(tree)if (!tree) { ((void)0); return ((void*)0); };
14075 |
14076 | TRY_TO_FAKE_THIS_ITEM(tree, hfindex, hfinfo)((tree)->tree_data)->count++; if((hfindex == 0 || (unsigned )hfindex > gpa_hfinfo.len) && wireshark_abort_on_dissector_bug ) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 14076 , __func__, "Unregistered hf! index=%d", hfindex); ((void) (( hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len ) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 14076, "hfindex > 0 && (unsigned)hfindex < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hfindex] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 14076, "gpa_hfinfo.hfi[hfindex] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hfindex];; if (((tree)->tree_data)->count > prefs.gui_max_tree_items ) { ((void)0); if (wireshark_abort_on_too_many_items) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 14076, __func__, "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items); ((tree)->tree_data )->count = 0; except_throw(1, (6), (wmem_strdup_printf(((tree )->tree_data->pinfo->pool), "Adding %s would put more than %d items in the tree -- possible infinite loop (max number of items can be increased in advanced preferences)" , hfinfo->abbrev, prefs.gui_max_tree_items))); } if (!(((tree )->tree_data)->visible)) { if (proto_item_is_hidden((tree ))) { if ((hfinfo->ref_type != HF_REF_TYPE_DIRECT) && (hfinfo->ref_type != HF_REF_TYPE_PRINT) && (hfinfo ->type != FT_PROTOCOL || ((tree)->tree_data)->fake_protocols )) { ((void)0); return proto_tree_add_fake_node(tree, hfinfo) ; } } };
14077 |
14078 | DISSECTOR_ASSERT_FIELD_TYPE(hfinfo, FT_STRING)((void) (((hfinfo)->type == FT_STRING) ? (void)0 : (proto_report_dissector_bug ("%s:%u: field %s is not of type ""FT_STRING", "epan/proto.c" , 14078, ((hfinfo))->abbrev))));
14079 |
14080 | byte_length = (((no_of_chars + 1) * 7) + (bit_offset & 0x07)) >> 3;
14081 | byte_offset = bit_offset >> 3;
14082 |
14083 | string = tvb_get_ascii_7bits_string(PNODE_POOL(tree)((tree)->tree_data->pinfo->pool), tvb, bit_offset, no_of_chars);
14084 |
14085 | pi = proto_tree_add_pi(tree, hfinfo, tvb, byte_offset, &byte_length);
14086 | DISSECTOR_ASSERT(byte_length >= 0)((void) ((byte_length >= 0) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\"", "epan/proto.c", 14086, "byte_length >= 0" ))));
14087 | proto_tree_set_string(PNODE_FINFO(pi)((pi)->finfo), string);
14088 |
14089 | return pi;
14090 | }
14091 |
14092 | const value_string proto_checksum_vals[] = {
14093 | { PROTO_CHECKSUM_E_BAD, "Bad" },
14094 | { PROTO_CHECKSUM_E_GOOD, "Good" },
14095 | { PROTO_CHECKSUM_E_UNVERIFIED, "Unverified" },
14096 | { PROTO_CHECKSUM_E_NOT_PRESENT, "Not present" },
14097 | { PROTO_CHECKSUM_E_ILLEGAL, "Illegal" },
14098 |
14099 | { 0, NULL((void*)0) }
14100 | };
14101 |
14102 | proto_item *
14103 | proto_tree_add_checksum(proto_tree *tree, tvbuff_t *tvb, const unsigned offset,
14104 | const int hf_checksum, const int hf_checksum_status, struct expert_field* bad_checksum_expert,
14105 | packet_info *pinfo, uint32_t computed_checksum, const unsigned encoding, const unsigned flags)
14106 | {
14107 | header_field_info *hfinfo;
14108 | uint32_t checksum;
14109 | uint32_t len;
14110 | proto_item* ti = NULL((void*)0);
14111 | proto_item* ti2;
14112 | bool_Bool incorrect_checksum = true1;
14113 |
14114 | PROTO_REGISTRAR_GET_NTH(hf_checksum, hfinfo)if((hf_checksum == 0 || (unsigned)hf_checksum > gpa_hfinfo .len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 14114, __func__, "Unregistered hf! index=%d" , hf_checksum); ((void) ((hf_checksum > 0 && (unsigned )hf_checksum < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 14114 , "hf_checksum > 0 && (unsigned)hf_checksum < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hf_checksum ] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 14114, "gpa_hfinfo.hfi[hf_checksum] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hf_checksum ];;
14115 |
14116 | switch (hfinfo->type) {
14117 | case FT_UINT8:
14118 | len = 1;
14119 | break;
14120 | case FT_UINT16:
14121 | len = 2;
14122 | break;
14123 | case FT_UINT24:
14124 | len = 3;
14125 | break;
14126 | case FT_UINT32:
14127 | len = 4;
14128 | break;
14129 | default:
14130 | REPORT_DISSECTOR_BUG("field %s is not of type FT_UINT8, FT_UINT16, FT_UINT24, or FT_UINT32",proto_report_dissector_bug("field %s is not of type FT_UINT8, FT_UINT16, FT_UINT24, or FT_UINT32" , hfinfo->abbrev)
14131 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_UINT8, FT_UINT16, FT_UINT24, or FT_UINT32" , hfinfo->abbrev);
14132 | }
14133 |
14134 | if (flags & PROTO_CHECKSUM_NOT_PRESENT0x10) {
14135 | ti = proto_tree_add_uint_format_value(tree, hf_checksum, tvb, offset, len, 0, "[missing]");
14136 | proto_item_set_generated(ti);
14137 | if (hf_checksum_status != -1) {
14138 | ti2 = proto_tree_add_uint(tree, hf_checksum_status, tvb, offset, len, PROTO_CHECKSUM_E_NOT_PRESENT);
14139 | proto_item_set_generated(ti2);
14140 | }
14141 | return ti;
14142 | }
14143 |
14144 | if (flags & PROTO_CHECKSUM_GENERATED0x02) {
14145 | ti = proto_tree_add_uint(tree, hf_checksum, tvb, offset, len, computed_checksum);
14146 | proto_item_set_generated(ti);
14147 | } else {
14148 | ti = proto_tree_add_item_ret_uint(tree, hf_checksum, tvb, offset, len, encoding, &checksum);
14149 | if (flags & PROTO_CHECKSUM_VERIFY0x01) {
14150 | if (flags & (PROTO_CHECKSUM_IN_CKSUM0x04|PROTO_CHECKSUM_ZERO0x08)) {
14151 | if (computed_checksum == 0) {
14152 | proto_item_append_text(ti, " [correct]");
14153 | if (hf_checksum_status != -1) {
14154 | ti2 = proto_tree_add_uint(tree, hf_checksum_status, tvb, offset, 0, PROTO_CHECKSUM_E_GOOD);
14155 | proto_item_set_generated(ti2);
14156 | }
14157 | incorrect_checksum = false0;
14158 | } else if (flags & PROTO_CHECKSUM_IN_CKSUM0x04) {
14159 | computed_checksum = in_cksum_shouldbe(checksum, computed_checksum);
14160 | /* XXX - This can't distinguish between "shouldbe"
14161 | * 0x0000 and 0xFFFF unless we know whether there
14162 | * were any nonzero bits (other than the checksum).
14163 | * Protocols should not use this path if they might
14164 | * have an all zero packet.
14165 | * Some implementations put the wrong zero; maybe
14166 | * we should have a special expert info for that?
14167 | */
14168 | }
14169 | } else {
14170 | if (checksum == computed_checksum) {
14171 | proto_item_append_text(ti, " [correct]");
14172 | if (hf_checksum_status != -1) {
14173 | ti2 = proto_tree_add_uint(tree, hf_checksum_status, tvb, offset, 0, PROTO_CHECKSUM_E_GOOD);
14174 | proto_item_set_generated(ti2);
14175 | }
14176 | incorrect_checksum = false0;
14177 | }
14178 | }
14179 |
14180 | if (incorrect_checksum) {
14181 | if (hf_checksum_status != -1) {
14182 | ti2 = proto_tree_add_uint(tree, hf_checksum_status, tvb, offset, 0, PROTO_CHECKSUM_E_BAD);
14183 | proto_item_set_generated(ti2);
14184 | }
14185 | if (flags & PROTO_CHECKSUM_ZERO0x08) {
14186 | proto_item_append_text(ti, " [incorrect]");
14187 | if (bad_checksum_expert != NULL((void*)0))
14188 | expert_add_info_format(pinfo, ti, bad_checksum_expert, "%s", expert_get_summary(bad_checksum_expert));
14189 | } else {
14190 | proto_item_append_text(ti, " incorrect, should be 0x%0*x", len*2, computed_checksum);
14191 | if (bad_checksum_expert != NULL((void*)0))
14192 | expert_add_info_format(pinfo, ti, bad_checksum_expert, "%s [should be 0x%0*x]", expert_get_summary(bad_checksum_expert), len * 2, computed_checksum);
14193 | }
14194 | }
14195 | } else {
14196 | if (hf_checksum_status != -1) {
14197 | proto_item_append_text(ti, " [unverified]");
14198 | ti2 = proto_tree_add_uint(tree, hf_checksum_status, tvb, offset, 0, PROTO_CHECKSUM_E_UNVERIFIED);
14199 | proto_item_set_generated(ti2);
14200 | }
14201 | }
14202 | }
14203 |
14204 | return ti;
14205 | }
14206 |
14207 | proto_item *
14208 | proto_tree_add_checksum_bytes(proto_tree *tree, tvbuff_t *tvb, const unsigned offset,
14209 | const int hf_checksum, const int hf_checksum_status, struct expert_field* bad_checksum_expert,
14210 | packet_info *pinfo, const uint8_t *computed_checksum, size_t checksum_len, const unsigned flags)
14211 | {
14212 | header_field_info *hfinfo;
14213 | uint8_t *checksum = NULL((void*)0);
14214 | proto_item* ti = NULL((void*)0);
14215 | proto_item* ti2;
14216 | bool_Bool incorrect_checksum = true1;
14217 |
14218 | PROTO_REGISTRAR_GET_NTH(hf_checksum, hfinfo)if((hf_checksum == 0 || (unsigned)hf_checksum > gpa_hfinfo .len) && wireshark_abort_on_dissector_bug) ws_log_fatal_full ("Epan", LOG_LEVEL_ERROR, "epan/proto.c", 14218, __func__, "Unregistered hf! index=%d" , hf_checksum); ((void) ((hf_checksum > 0 && (unsigned )hf_checksum < gpa_hfinfo.len) ? (void)0 : (proto_report_dissector_bug ("%s:%u: failed assertion \"%s\" (%s)", "epan/proto.c", 14218 , "hf_checksum > 0 && (unsigned)hf_checksum < gpa_hfinfo.len" , "Unregistered hf!")))) ; ((void) ((gpa_hfinfo.hfi[hf_checksum ] != ((void*)0)) ? (void)0 : (proto_report_dissector_bug("%s:%u: failed assertion \"%s\" (%s)" , "epan/proto.c", 14218, "gpa_hfinfo.hfi[hf_checksum] != ((void*)0)" , "Unregistered hf!")))) ; hfinfo = gpa_hfinfo.hfi[hf_checksum ];;
14219 |
14220 | if (hfinfo->type != FT_BYTES) {
14221 | REPORT_DISSECTOR_BUG("field %s is not of type FT_BYTES",proto_report_dissector_bug("field %s is not of type FT_BYTES" , hfinfo->abbrev)
14222 | hfinfo->abbrev)proto_report_dissector_bug("field %s is not of type FT_BYTES" , hfinfo->abbrev);
14223 | }
14224 |
14225 | if (flags & PROTO_CHECKSUM_NOT_PRESENT0x10) {
14226 | ti = proto_tree_add_bytes_format_value(tree, hf_checksum, tvb, offset, (int)checksum_len, 0, "[missing]");
14227 | proto_item_set_generated(ti);
14228 | if (hf_checksum_status != -1) {
14229 | ti2 = proto_tree_add_uint(tree, hf_checksum_status, tvb, offset, (int)checksum_len, PROTO_CHECKSUM_E_NOT_PRESENT);
14230 | proto_item_set_generated(ti2);
14231 | }
14232 | return ti;
14233 | }
14234 |
14235 | if (flags & PROTO_CHECKSUM_GENERATED0x02) {
14236 | ti = proto_tree_add_bytes(tree, hf_checksum, tvb, offset, (int)checksum_len, computed_checksum);
14237 | proto_item_set_generated(ti);
14238 | } else {
14239 | checksum = (uint8_t*)wmem_alloc0_array(pinfo->pool, uint8_t, checksum_len)((uint8_t*)wmem_alloc0((pinfo->pool), (((((checksum_len)) <= 0) || ((size_t)sizeof(uint8_t) > (9223372036854775807L / ( size_t)((checksum_len))))) ? 0 : (sizeof(uint8_t) * ((checksum_len ))))));
14240 | tvb_memcpy(tvb, checksum, offset, checksum_len);
14241 | ti = proto_tree_add_bytes(tree, hf_checksum, tvb, offset, (int)checksum_len, checksum);
14242 | if (flags & PROTO_CHECKSUM_VERIFY0x01) {
14243 | if (flags & (PROTO_CHECKSUM_IN_CKSUM0x04|PROTO_CHECKSUM_ZERO0x08)) {
14244 | if (computed_checksum == 0) {
14245 | proto_item_append_text(ti, " [correct]");
14246 | if (hf_checksum_status != -1) {
14247 | ti2 = proto_tree_add_uint(tree, hf_checksum_status, tvb, offset, 0, PROTO_CHECKSUM_E_GOOD);
14248 | proto_item_set_generated(ti2);
14249 | }
14250 | incorrect_checksum = false0;
14251 | }
14252 | } else {
14253 | if (memcmp(computed_checksum, checksum, checksum_len) == 0) {
14254 | proto_item_append_text(ti, " [correct]");
14255 | if (hf_checksum_status != -1) {
14256 | ti2 = proto_tree_add_uint(tree, hf_checksum_status, tvb, offset, 0, PROTO_CHECKSUM_E_GOOD);
14257 | proto_item_set_generated(ti2);
14258 | }
14259 | incorrect_checksum = false0;
14260 | }
14261 | }
14262 |
14263 | if (incorrect_checksum) {
14264 | if (hf_checksum_status != -1) {
14265 | ti2 = proto_tree_add_uint(tree, hf_checksum_status, tvb, offset, 0, PROTO_CHECKSUM_E_BAD);
14266 | proto_item_set_generated(ti2);
14267 | }
14268 | if (flags & PROTO_CHECKSUM_ZERO0x08) {
14269 | proto_item_append_text(ti, " [incorrect]");
14270 | if (bad_checksum_expert != NULL((void*)0))
14271 | expert_add_info_format(pinfo, ti, bad_checksum_expert, "%s", expert_get_summary(bad_checksum_expert));
14272 | } else {
14273 | size_t computed_checksum_str_len = (2 * checksum_len * sizeof(char)) + 1;
14274 | char *computed_checksum_str = (char*)wmem_alloc0_array(pinfo->pool, char, computed_checksum_str_len)((char*)wmem_alloc0((pinfo->pool), (((((computed_checksum_str_len )) <= 0) || ((size_t)sizeof(char) > (9223372036854775807L / (size_t)((computed_checksum_str_len))))) ? 0 : (sizeof(char ) * ((computed_checksum_str_len))))));
14275 | for (size_t counter = 0; counter < checksum_len; ++counter) {
14276 | snprintf(
14277 | /* On ecah iteration inserts two characters */
14278 | (char*)&computed_checksum_str[counter << 1],
14279 | computed_checksum_str_len - (counter << 1),
14280 | "%02x",
14281 | computed_checksum[counter]);
14282 | }
14283 | proto_item_append_text(ti, " incorrect, should be 0x%s", computed_checksum_str);
14284 | if (bad_checksum_expert != NULL((void*)0))
14285 | expert_add_info_format(pinfo, ti, bad_checksum_expert, "%s [should be 0x%s]", expert_get_summary(bad_checksum_expert), computed_checksum_str);
14286 | }
14287 | }
14288 | } else {
14289 | if (hf_checksum_status != -1) {
14290 | proto_item_append_text(ti, " [unverified]");
14291 | ti2 = proto_tree_add_uint(tree, hf_checksum_status, tvb, offset, 0, PROTO_CHECKSUM_E_UNVERIFIED);
14292 | proto_item_set_generated(ti2);
14293 | }
14294 | }
14295 | }
14296 |
14297 | return ti;
14298 | }
14299 |
14300 | unsigned char
14301 | proto_check_field_name(const char *field_name)
14302 | {
14303 | return module_check_valid_name(field_name, false0);
14304 | }
14305 |
14306 | unsigned char
14307 | proto_check_field_name_lower(const char *field_name)
14308 | {
14309 | return module_check_valid_name(field_name, true1);
14310 | }
14311 |
14312 | bool_Bool
14313 | tree_expanded(int tree_type)
14314 | {
14315 | if (tree_type <= 0) {
14316 | return false0;
14317 | }
14318 | ws_assert(tree_type >= 0 && tree_type < num_tree_types)do { if ((1) && !(tree_type >= 0 && tree_type < num_tree_types)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 14318, __func__, "assertion failed: %s", "tree_type >= 0 && tree_type < num_tree_types" ); } while (0);
14319 | return tree_is_expanded[tree_type >> 5] & (1U << (tree_type & 31));
14320 | }
14321 |
14322 | void
14323 | tree_expanded_set(int tree_type, bool_Bool value)
14324 | {
14325 | ws_assert(tree_type >= 0 && tree_type < num_tree_types)do { if ((1) && !(tree_type >= 0 && tree_type < num_tree_types)) ws_log_fatal_full("Epan", LOG_LEVEL_ERROR , "epan/proto.c", 14325, __func__, "assertion failed: %s", "tree_type >= 0 && tree_type < num_tree_types" ); } while (0);
14326 |
14327 | if (value)
14328 | tree_is_expanded[tree_type >> 5] |= (1U << (tree_type & 31));
14329 | else
14330 | tree_is_expanded[tree_type >> 5] &= ~(1U << (tree_type & 31));
14331 | }
14332 |
14333 | /*
14334 | * Editor modelines - https://www.wireshark.org/tools/modelines.html
14335 | *
14336 | * Local variables:
14337 | * c-basic-offset: 8
14338 | * tab-width: 8
14339 | * indent-tabs-mode: t
14340 | * End:
14341 | *
14342 | * vi: set shiftwidth=8 tabstop=8 noexpandtab:
14343 | * :indentSize=8:tabSize=8:noTabs=false:
14344 | */