### Bug Summary

File: | builds/wireshark/wireshark/epan/addr_resolv.c
Warning: | line 774, column 9 Value of 'errno' was not checked and may be overwritten by function 'fgets'

### Annotated Source Code

Press '?' to see keyboard shortcuts

Show analyzer invocation
clang -cc1 -cc1 -triple x86_64-pc-linux-gnu -analyze -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name addr_resolv.c -analyzer-checker=core -analyzer-checker=apiModeling -analyzer-checker=unix -analyzer-checker=deadcode -analyzer-checker=security.insecureAPI.UncheckedReturn -analyzer-checker=security.insecureAPI.getpw -analyzer-checker=security.insecureAPI.gets -analyzer-checker=security.insecureAPI.mktemp -analyzer-checker=security.insecureAPI.mkstemp -analyzer-checker=security.insecureAPI.vfork -analyzer-checker=nullability.NullPassedToNonnull -analyzer-checker=nullability.NullReturnedFromNonnull -analyzer-output plist -w -setup-static-analyzer -mrelocation-model pic -pic-level 2 -fhalf-no-semantic-interposition -fno-delete-null-pointer-checks -mframe-pointer=all -relaxed-aliasing -fmath-errno -ffp-contract=on -fno-rounding-math -ffloat16-excess-precision=fast -fbfloat16-excess-precision=fast -mconstructor-aliases -funwind-tables=2 -target-cpu x86-64 -tune-cpu generic -debugger-tuning=gdb -fdebug-compilation-dir=/builds/wireshark/wireshark/build -fcoverage-compilation-dir=/builds/wireshark/wireshark/build -resource-dir /usr/lib/llvm-21/lib/clang/21 -isystem /usr/include/glib-2.0 -isystem /usr/lib/x86_64-linux-gnu/glib-2.0/include -isystem /builds/wireshark/wireshark/epan -isystem /builds/wireshark/wireshark/build/epan -isystem /usr/include/mit-krb5 -isystem /usr/include/libxml2 -isystem /usr/include/lua5.4 -D G_DISABLE_DEPRECATED -D G_DISABLE_SINGLE_INCLUDES -D WS_BUILD_DLL -D WS_DEBUG -D WS_DEBUG_UTF_8 -D epan_EXPORTS -I /builds/wireshark/wireshark/build -I /builds/wireshark/wireshark -I /builds/wireshark/wireshark/include -I /builds/wireshark/wireshark/wiretap -D _GLIBCXX_ASSERTIONS -internal-isystem /usr/lib/llvm-21/lib/clang/21/include -internal-isystem /usr/local/include -internal-isystem /usr/lib/gcc/x86_64-linux-gnu/14/../../../../x86_64-linux-gnu/include -internal-externc-isystem /usr/include/x86_64-linux-gnu -internal-externc-isystem /include -internal-externc-isystem /usr/include -fmacro-prefix-map=/builds/wireshark/wireshark/= -fmacro-prefix-map=/builds/wireshark/wireshark/build/= -fmacro-prefix-map=../= -Wno-format-nonliteral -std=gnu11 -ferror-limit 19 -fvisibility=hidden -fwrapv -fwrapv-pointer -fstrict-flex-arrays=3 -stack-protector 2 -fstack-clash-protection -fcf-protection=full -fgnuc-version=4.2.1 -fskip-odr-check-in-gmf -fexceptions -fcolor-diagnostics -analyzer-output=html -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -o /builds/wireshark/wireshark/sbout/2026-03-02-100418-3623-1 -x c /builds/wireshark/wireshark/epan/addr_resolv.c

Keyboard shortcuts:

- Use 'j/k' keys for keyboard navigation
- Use 'Shift+S' to show/hide relevant lines
- Use '?' to toggle this window

Close
Show only relevant lines Show control flow arrows

1 | /* addr_resolv.c
2 | * Routines for network object lookup
3 | *
4 | * Laurent Deniel <laurent.deniel@free.fr>
5 | *
6 | * Add option to resolv VLAN ID to describing name
7 | * Uli Heilmeier, March 2016
8 | *
9 | * Wireshark - Network traffic analyzer
10 | * By Gerald Combs <gerald@wireshark.org>
11 | * Copyright 1998 Gerald Combs
12 | *
13 | * SPDX-License-Identifier: GPL-2.0-or-later
14 | */
15 |
16 | #include "config.h"
17 |
18 | #include <stdio.h>
19 | #include <stdlib.h>
20 | #include <string.h>
21 | #include <errno(*__errno_location ()).h>
22 |
23 | #include <wsutil/strtoi.h>
24 | #include <wsutil/ws_assert.h>
25 |
26 | #include "iana-info.h"
27 | #include "manuf.h"
28 |
29 | /*
30 | * Win32 doesn't have SIGALRM (and it's the OS where name lookup calls
31 | * are most likely to take a long time, given the way address-to-name
32 | * lookups are done over NBNS).
33 | *
34 | * macOS does have SIGALRM, but if you longjmp() out of a name resolution
35 | * call in a signal handler, you might crash, because the state of the
36 | * resolution code that sends messages to lookupd might be inconsistent
37 | * if you jump out of it in middle of a call.
38 | *
39 | * There's no guarantee that longjmp()ing out of name resolution calls
40 | * will work on *any* platform; OpenBSD got rid of the alarm/longjmp
41 | * code in tcpdump, to avoid those sorts of problems, and that was
42 | * picked up by tcpdump.org tcpdump.
43 | *
44 | * So, for now, we do not use alarm() and SIGALRM to time out host name
45 | * lookups. If we get a lot of complaints about lookups taking a long time,
46 | * we can reconsider that decision. (Note that tcpdump originally added
47 | * such a timeout mechanism that for the benefit of systems using NIS to
48 | * look up host names; that might now be fixed in NIS implementations, for
49 | * those sites still using NIS rather than DNS for that.... tcpdump no
50 | * longer does that, for the same reasons that we don't.)
51 | *
52 | * If we're using an asynchronous DNS resolver, that shouldn't be an issue.
53 | * If we're using a synchronous name lookup mechanism (which we'd do mainly
54 | * to support resolving addresses and host names using more mechanisms than
55 | * just DNS, such as NIS, NBNS, or Mr. Hosts File), we could do that in
56 | * a separate thread, making it, in effect, asynchronous.
57 | */
58 |
59 | #ifdef HAVE_NETINET_IN_H1
60 | # include <netinet/in.h>
61 | #endif
62 |
63 | #ifdef HAVE_NETDB_H1
64 | #include <netdb.h>
65 | #endif
66 |
67 | #ifdef HAVE_SYS_SOCKET_H1
68 | #include <sys/socket.h> /* needed to define AF_ values on UNIX */
69 | #endif
70 |
71 | #ifdef _WIN32
72 | #include <winsock2.h> /* needed to define AF_ values on Windows */
73 | #include <ws2tcpip.h>
74 | #endif
75 |
76 | #ifdef _WIN32
77 | # define socklen_t unsigned int
78 | #endif
79 | #include <ares.h>
80 | #include <ares_version.h>
81 |
82 | #include <glib.h>
83 |
84 | #include <epan/packet.h>
85 | #include "addr_resolv.h"
86 | #include "wsutil/filesystem.h"
87 |
88 | #include <wsutil/report_message.h>
89 | #include <wsutil/file_util.h>
90 | #include <wsutil/pint.h>
91 | #include <wsutil/inet_cidr.h>
92 |
93 | #include <epan/strutil.h>
94 | #include <epan/to_str.h>
95 | #include <epan/maxmind_db.h>
96 | #include <epan/prefs.h>
97 | #include <epan/uat.h>
98 |
99 | #define ENAME_HOSTS"hosts" "hosts"
100 | #define ENAME_SUBNETS"subnets" "subnets"
101 | #define ENAME_ETHERS"ethers" "ethers"
102 | #define ENAME_IPXNETS"ipxnets" "ipxnets"
103 | #define ENAME_MANUF"manuf" "manuf"
104 | #define ENAME_WKA"wka" "wka"
105 | #define ENAME_SERVICES"services" "services"
106 | #define ENAME_VLANS"vlans" "vlans"
107 | #define ENAME_SS7PCS"ss7pcs" "ss7pcs"
108 | #define ENAME_ENTERPRISES"enterprises" "enterprises"
109 | #define ENAME_TACS"tacs" "tacs"
110 |
111 | #define HASHETHSIZE2048 2048
112 | #define HASHHOSTSIZE2048 2048
113 | #define HASHIPXNETSIZE256 256
114 | #define SUBNETLENGTHSIZE32 32 /*1-32 inc.*/
115 |
116 | /* hash table used for IPv4 lookup */
117 |
118 | #define HASH_IPV4_ADDRESS(addr)((((((guint32) ( (((guint32) (addr) & (guint32) 0x000000ffU ) << 24) | (((guint32) (addr) & (guint32) 0x0000ff00U ) << 8) | (((guint32) (addr) & (guint32) 0x00ff0000U ) >> 8) | (((guint32) (addr) & (guint32) 0xff000000U ) >> 24)))))) & (2048 - 1)) (g_htonl(addr)(((((guint32) ( (((guint32) (addr) & (guint32) 0x000000ffU ) << 24) | (((guint32) (addr) & (guint32) 0x0000ff00U ) << 8) | (((guint32) (addr) & (guint32) 0x00ff0000U ) >> 8) | (((guint32) (addr) & (guint32) 0xff000000U ) >> 24)))))) & (HASHHOSTSIZE2048 - 1))
119 |
120 |
121 | typedef struct sub_net_hashipv4 {
122 | unsigned addr;
123 | /* XXX: No longer needed?*/
124 | uint8_t flags; /* B0 dummy_entry, B1 resolve, B2 If the address is used in the trace */
125 | struct sub_net_hashipv4 *next;
126 | char name[MAXNAMELEN64];
127 | } sub_net_hashipv4_t;
128 |
129 | /* Array of entries of subnets of different lengths */
130 | typedef struct {
131 | size_t mask_length; /*1-32*/
132 | uint32_t mask; /* e.g. 255.255.255.*/
133 | sub_net_hashipv4_t** subnet_addresses; /* Hash table of subnet addresses */
134 | } subnet_length_entry_t;
135 |
136 |
137 | /* hash table used for IPX network lookup */
138 |
139 | /* XXX - check goodness of hash function */
140 |
141 | #define HASH_IPX_NET(net)((net) & (256 - 1)) ((net) & (HASHIPXNETSIZE256 - 1))
142 |
143 | typedef struct hashipxnet {
144 | unsigned addr;
145 | struct hashipxnet *next;
146 | char name[MAXNAMELEN64];
147 | } hashipxnet_t;
148 |
149 | typedef struct hashvlan {
150 | unsigned id;
151 | /* struct hashvlan *next; */
152 | char name[MAXVLANNAMELEN128];
153 | } hashvlan_t;
154 |
155 | typedef struct ss7pc {
156 | uint32_t id; /* 1st byte NI, 3 following bytes: Point Code */
157 | char pc_addr[MAXNAMELEN64];
158 | char name[MAXNAMELEN64];
159 | } hashss7pc_t;
160 |
161 | /* hash tables used for ethernet and manufacturer lookup */
162 | struct hashether {
163 | uint8_t flags; /* (See above) */
164 | uint8_t addr[6];
165 | char hexaddr[6*3];
166 | char resolved_name[MAXNAMELEN64];
167 | };
168 |
169 | struct hasheui64 {
170 | uint8_t flags; /* (See above) */
171 | uint8_t addr[EUI64_ADDR_LEN8];
172 | char hexaddr[EUI64_ADDR_LEN8*3];
173 | char resolved_name[MAXNAMELEN64];
174 | };
175 |
176 | struct hashwka {
177 | uint8_t flags; /* (See above) */
178 | char* name;
179 | };
180 |
181 | struct hashmanuf {
182 | uint8_t flags; /* (See above) */
183 | uint8_t addr[3];
184 | char hexaddr[3*3];
185 | char resolved_name[MAXNAMELEN64];
186 | char resolved_longname[MAXNAMELEN64];
187 | };
188 |
189 | /* internal type used when reading ethers file (or wka, manuf) */
190 | typedef struct _ether
191 | {
192 | uint8_t addr[8];
193 | char name[MAXNAMELEN64];
194 | char longname[MAXNAMELEN64];
195 | } ether_t;
196 |
197 | /* internal ipxnet type */
198 | typedef struct _ipxnet
199 | {
200 | unsigned addr;
201 | char name[MAXNAMELEN64];
202 | } ipxnet_t;
203 |
204 | /* internal vlan type */
205 | typedef struct _vlan
206 | {
207 | unsigned id;
208 | char name[MAXVLANNAMELEN128];
209 | } vlan_t;
210 |
211 | static wmem_allocator_t *addr_resolv_scope;
212 |
213 | // Maps unsigned -> hashipxnet_t*
214 | static wmem_map_t *ipxnet_hash_table;
215 | static wmem_map_t *ipv4_hash_table;
216 | static wmem_map_t *ipv6_hash_table;
217 | // Maps unsigned -> hashvlan_t*
218 | static wmem_map_t *vlan_hash_table;
219 | static wmem_map_t *ss7pc_hash_table;
220 | static wmem_map_t *tac_hash_table;
221 |
222 | // Maps IP address -> manually set hostname.
223 | static wmem_map_t *manually_resolved_ipv4_list;
224 | static wmem_map_t *manually_resolved_ipv6_list;
225 |
226 | static addrinfo_lists_t addrinfo_lists;
227 |
228 | struct cb_serv_data {
229 | char *service;
230 | port_type proto;
231 | };
232 |
233 | // Maps unsigned -> hashmanuf_t*
234 | // XXX: Note that hashmanuf_t* only accommodates 24-bit OUIs.
235 | // We might want to store vendor names from MA-M and MA-S to
236 | // present in the Resolved Addresses dialog.
237 | static wmem_map_t *manuf_hashtable;
238 | // Maps address -> hashwka_t*
239 | static wmem_map_t *wka_hashtable;
240 | // Maps address -> hashether_t*
241 | static wmem_map_t *eth_hashtable;
242 | // Maps address -> hasheui64_t*
243 | static wmem_map_t *eui64_hashtable;
244 | // Maps unsigned -> serv_port_t*
245 | static wmem_map_t *serv_port_hashtable;
246 | static wmem_map_t *serv_port_custom_hashtable;
247 |
248 | // Maps enterprise-id -> enterprise-desc (only used for user additions)
249 | static GHashTable *enterprises_hashtable;
250 |
251 | static subnet_length_entry_t subnet_length_entries[SUBNETLENGTHSIZE32]; /* Ordered array of entries */
252 | static bool_Bool have_subnet_entry;
253 |
254 | static bool_Bool new_resolved_objects;
255 |
256 | static GPtrArray* extra_hosts_files;
257 |
258 | static hashether_t *add_eth_name(const uint8_t *addr, const char *name, bool_Bool static_entry);
259 | static hasheui64_t *add_eui64_name(const uint8_t *addr, const char *name, bool_Bool static_entry);
260 | static void add_serv_port_cb(const uint32_t port, void *ptr);
261 |
262 | /* http://eternallyconfuzzled.com/tuts/algorithms/jsw_tut_hashing.aspx#existing
263 | * One-at-a-Time hash
264 | */
265 | unsigned
266 | ipv6_oat_hash(const void *key)
267 | {
268 | int len = 16;
269 | const unsigned char *p = (const unsigned char *)key;
270 | unsigned h = 0;
271 | int i;
272 |
273 | for ( i = 0; i < len; i++ ) {
274 | h += p[i];
275 | h += ( h << 10 );
276 | h ^= ( h >> 6 );
277 | }
278 |
279 | h += ( h << 3 );
280 | h ^= ( h >> 11 );
281 | h += ( h << 15 );
282 |
283 | return h;
284 | }
285 |
286 | unsigned
287 | ws_ipv6_hash(const void* key)
288 | {
289 | #ifdef HAVE_XXHASH1
290 | return wmem_strong_hash(key, 16);
291 | #else
292 | return ipv6_oat_hash(key);
293 | #endif
294 | }
295 |
296 | gboolean
297 | ipv6_equal(const void *v1, const void *v2)
298 | {
299 |
300 | if (memcmp(v1, v2, sizeof (ws_in6_addr)) == 0) {
301 | return true1;
302 | }
303 |
304 | return false0;
305 | }
306 |
307 | /*
308 | * Flag controlling what names to resolve.
309 | */
310 | e_addr_resolve gbl_resolv_flags = {
311 | true1, /* mac_name */
312 | false0, /* network_name */
313 | false0, /* transport_name */
314 | true1, /* dns_pkt_addr_resolution */
315 | false0, /* handshake_sni_addr_resolution */
316 | true1, /* use_external_net_name_resolver */
317 | false0, /* vlan_name */
318 | false0, /* ss7 point code names */
319 | true1, /* maxmind_geoip */
320 | false0, /* tac_name */
321 | };
322 |
323 | /* XXX - ares_init_options(3) says:
324 | * "The recommended concurrent query limit is about 32k queries"
325 | */
326 | static unsigned name_resolve_concurrency = 500;
327 | static bool_Bool resolve_synchronously;
328 |
329 | /*
330 | * Global variables (can be changed in GUI sections)
331 | * XXX - they could be changed in GUI code, but there's currently no
332 | * GUI code to change them.
333 | */
334 |
335 | char *g_ethers_path; /* global ethers file */
336 | char *g_pethers_path; /* personal ethers file */
337 | char *g_wka_path; /* global well-known-addresses file */
338 | char *g_manuf_path; /* global manuf file */
339 | char *g_pmanuf_path; /* personal manuf file */
340 | char *g_ipxnets_path; /* global ipxnets file */
341 | char *g_pipxnets_path; /* personal ipxnets file */
342 | char *g_services_path; /* global services file */
343 | char *g_pservices_path; /* personal services file */
344 | char *g_pvlan_path; /* personal vlans file */
345 | char *g_ss7pcs_path; /* personal ss7pcs file */
346 | char *g_enterprises_path; /* global enterprises file */
347 | char *g_penterprises_path; /* personal enterprises file */
348 | /* first resolving call */
349 |
350 | /*
351 | * Submitted asynchronous queries trigger a callback (c_ares_ghba_cb()).
352 | * Queries are added to c_ares_queue_head. During processing, queries are
353 | * popped off the front of c_ares_queue_head and submitted using
354 | * ares_gethostbyaddr().
355 | * The callback processes the response, then frees the request.
356 | */
357 | typedef struct _async_dns_queue_msg
358 | {
359 | union {
360 | uint32_t ip4;
361 | ws_in6_addr ip6;
362 | } addr;
363 | int family;
364 | } async_dns_queue_msg_t;
365 |
366 | typedef struct _async_hostent {
367 | int addr_size;
368 | int copied;
369 | void *addrp;
370 | } async_hostent_t;
371 |
372 | static void
373 | c_ares_ghba_cb(void *arg, int status, int timeouts _U___attribute__((unused)), struct hostent *he);
374 |
375 | /*
376 | * Submitted synchronous queries trigger a callback (c_ares_ghba_sync_cb()).
377 | * The callback processes the response, sets completed to true if
378 | * completed is non-NULL, then frees the request.
379 | */
380 | typedef struct _sync_dns_data
381 | {
382 | union {
383 | uint32_t ip4;
384 | ws_in6_addr ip6;
385 | } addr;
386 | int family;
387 | bool_Bool *completed;
388 | } sync_dns_data_t;
389 |
390 | static ares_channel ghba_chan; /* ares_gethostbyaddr -- Usually non-interactive, no timeout */
391 | static ares_channel ghbn_chan; /* ares_gethostbyname -- Usually interactive, timeout */
392 |
393 | static bool_Bool async_dns_initialized;
394 | static unsigned async_dns_in_flight;
395 | static wmem_list_t *async_dns_queue_head;
396 | static GMutex async_dns_queue_mtx;
397 |
398 | //UAT for providing a list of DNS servers to C-ARES for name resolution
399 | bool_Bool use_custom_dns_server_list;
400 | struct dns_server_data {
401 | char *ipaddr;
402 | uint32_t udp_port;
403 | uint32_t tcp_port;
404 | };
405 |
406 | UAT_CSTRING_CB_DEF(dnsserverlist_uats, ipaddr, struct dns_server_data)static void dnsserverlist_uats_ipaddr_set_cb(void* rec, const char* buf, unsigned len, const void* u1 __attribute__((unused )), const void* u2 __attribute__((unused))) { char* new_buf = g_strndup(buf,len); g_free((((struct dns_server_data*)rec)-> ipaddr)); (((struct dns_server_data*)rec)->ipaddr) = new_buf ; } static void dnsserverlist_uats_ipaddr_tostr_cb(void* rec, char** out_ptr, unsigned* out_len, const void* u1 __attribute__ ((unused)), const void* u2 __attribute__((unused))) { if (((struct dns_server_data*)rec)->ipaddr ) { *out_ptr = g_strdup_inline ((((struct dns_server_data*)rec)->ipaddr)); *out_len = (unsigned )strlen((((struct dns_server_data*)rec)->ipaddr)); } else { *out_ptr = g_strdup_inline (""); *out_len = 0; } }
407 | UAT_DEC_CB_DEF(dnsserverlist_uats, tcp_port, struct dns_server_data)static void dnsserverlist_uats_tcp_port_set_cb(void* rec, const char* buf, unsigned len, const void* u1 __attribute__((unused )), const void* u2 __attribute__((unused))) { char* tmp_str = g_strndup(buf,len); ws_strtou32(tmp_str, ((void*)0), &(( struct dns_server_data*)rec)->tcp_port); g_free(tmp_str); } static void dnsserverlist_uats_tcp_port_tostr_cb(void* rec, char ** out_ptr, unsigned* out_len, const void* u1 __attribute__(( unused)), const void* u2 __attribute__((unused))) { *out_ptr = wmem_strdup_printf(((void*)0), "%u",((struct dns_server_data *)rec)->tcp_port); *out_len = (unsigned)strlen(*out_ptr); }
408 | UAT_DEC_CB_DEF(dnsserverlist_uats, udp_port, struct dns_server_data)static void dnsserverlist_uats_udp_port_set_cb(void* rec, const char* buf, unsigned len, const void* u1 __attribute__((unused )), const void* u2 __attribute__((unused))) { char* tmp_str = g_strndup(buf,len); ws_strtou32(tmp_str, ((void*)0), &(( struct dns_server_data*)rec)->udp_port); g_free(tmp_str); } static void dnsserverlist_uats_udp_port_tostr_cb(void* rec, char ** out_ptr, unsigned* out_len, const void* u1 __attribute__(( unused)), const void* u2 __attribute__((unused))) { *out_ptr = wmem_strdup_printf(((void*)0), "%u",((struct dns_server_data *)rec)->udp_port); *out_len = (unsigned)strlen(*out_ptr); }
409 |
410 | static uat_t *dnsserver_uat;
411 | static struct dns_server_data *dnsserverlist_uats;
412 | static unsigned ndnsservers;
413 |
414 | static void
415 | dns_server_free_cb(void *data)
416 | {
417 | struct dns_server_data *h = (struct dns_server_data*)data;
418 |
419 | g_free(h->ipaddr);
420 | }
421 |
422 | static void*
423 | dns_server_copy_cb(void *dst_, const void *src_, size_t len _U___attribute__((unused)))
424 | {
425 | const struct dns_server_data *src = (const struct dns_server_data *)src_;
426 | struct dns_server_data *dst = (struct dns_server_data *)dst_;
427 |
428 | dst->ipaddr = g_strdup(src->ipaddr)g_strdup_inline (src->ipaddr);
429 | dst->udp_port = src->udp_port;
430 | dst->tcp_port = src->tcp_port;
431 |
432 | return dst;
433 | }
434 |
435 | static bool_Bool
436 | dnsserver_uat_fld_ip_chk_cb(void* r _U___attribute__((unused)), const char* ipaddr, unsigned len _U___attribute__((unused)), const void* u1 _U___attribute__((unused)), const void* u2 _U___attribute__((unused)), char** err)
437 | {
438 | //Check for a valid IPv4 or IPv6 address.
439 | if (ipaddr && g_hostname_is_ip_address(ipaddr)) {
440 | *err = NULL((void*)0);
441 | return true1;
442 | }
443 |
444 | *err = ws_strdup_printf("No valid IP address given.")wmem_strdup_printf(((void*)0), "No valid IP address given.");
445 | return false0;
446 | }
447 |
448 | static bool_Bool
449 | dnsserver_uat_fld_port_chk_cb(void* r _U___attribute__((unused)), const char* p, unsigned len _U___attribute__((unused)), const void* u1 _U___attribute__((unused)), const void* u2 _U___attribute__((unused)), char** err)
450 | {
451 | if (!p || strlen(p) == 0u) {
452 | // This should be removed in favor of Decode As. Make it optional.
453 | *err = NULL((void*)0);
454 | return true1;
455 | }
456 |
457 | if (strcmp(p, "53") != 0){
458 | uint16_t port;
459 | if (!ws_strtou16(p, NULL((void*)0), &port)) {
460 | *err = g_strdup("Invalid port given.")g_strdup_inline ("Invalid port given.");
461 | return false0;
462 | }
463 | }
464 |
465 | *err = NULL((void*)0);
466 | return true1;
467 | }
468 |
469 | static void
470 | c_ares_ghba_sync_cb(void *arg, int status, int timeouts _U___attribute__((unused)), struct hostent *he) {
471 | sync_dns_data_t *sdd = (sync_dns_data_t *)arg;
472 | char **p;
473 |
474 | if (status == ARES_SUCCESS) {
475 | for (p = he->h_addr_list; *p != NULL((void*)0); p++) {
476 | switch(sdd->family) {
477 | case AF_INET2:
478 | add_ipv4_name(sdd->addr.ip4, he->h_name, false0);
479 | break;
480 | case AF_INET610:
481 | add_ipv6_name(&sdd->addr.ip6, he->h_name, false0);
482 | break;
483 | default:
484 | /* Throw an exception? */
485 | break;
486 | }
487 | }
488 |
489 | }
490 |
491 | /*
492 | * Let our caller know that this is complete.
493 | */
494 | *sdd->completed = true1;
495 |
496 | /*
497 | * Free the structure for this call.
498 | */
499 | g_free(sdd);
500 | }
501 |
502 | static void
503 | wait_for_sync_resolv(bool_Bool *completed) {
504 | int nfds;
505 | fd_set rfds, wfds;
506 | struct timeval tv;
507 |
508 | while (!*completed) {
509 | /*
510 | * Not yet resolved; wait for something to show up on the
511 | * address-to-name C-ARES channel.
512 | *
513 | * To quote the source code for ares_timeout() as of C-ARES
514 | * 1.12.0, "WARNING: Beware that this is linear in the number
515 | * of outstanding requests! You are probably far better off
516 | * just calling ares_process() once per second, rather than
517 | * calling ares_timeout() to figure out when to next call
518 | * ares_process().", although we should have only one request
519 | * outstanding.
520 | * As of C-ARES 1.20.0, the ares_timeout() function is now O(1),
521 | * but we don't require that minimum version.
522 | * https://github.com/c-ares/c-ares/commit/cf99c025cfb3e21295b59923876a31a68ea2cb4b
523 | *
524 | * And, yes, we have to reset it each time, as select(), in
525 | * some OSes modifies the timeout to reflect the time remaining
526 | * (e.g., Linux) and select() in other OSes doesn't (most if not
527 | * all other UN*Xes, Windows?), so we can't rely on *either*
528 | * behavior.
529 | */
530 | tv.tv_sec = 1;
531 | tv.tv_usec = 0;
532 |
533 | FD_ZERO(&rfds)do { unsigned int __i; fd_set *__arr = (&rfds); for (__i = 0; __i < sizeof (fd_set) / sizeof (__fd_mask); ++__i) ((__arr )->__fds_bits)[__i] = 0; } while (0);
534 | FD_ZERO(&wfds)do { unsigned int __i; fd_set *__arr = (&wfds); for (__i = 0; __i < sizeof (fd_set) / sizeof (__fd_mask); ++__i) ((__arr )->__fds_bits)[__i] = 0; } while (0);
535 | nfds = ares_fds(ghba_chan, &rfds, &wfds);
536 | if (nfds > 0) {
537 | if (select(nfds, &rfds, &wfds, NULL((void*)0), &tv) == -1) { /* call to select() failed */
538 | /* If it's interrupted by a signal, no need to put out a message */
539 | if (errno(*__errno_location ()) != EINTR4)
540 | fprintf(stderrstderr, "Warning: call to select() failed, error is %s\n", g_strerror(errno(*__errno_location ())));
541 | return;
542 | }
543 | ares_process(ghba_chan, &rfds, &wfds);
544 | }
545 | }
546 | }
547 |
548 | static void
549 | process_async_dns_queue(void)
550 | {
551 | wmem_list_frame_t* head;
552 | async_dns_queue_msg_t *caqm;
553 |
554 | if (async_dns_queue_head == NULL((void*)0))
555 | return;
556 |
557 | if (!g_mutex_trylock(&async_dns_queue_mtx))
558 | return;
559 |
560 | head = wmem_list_head(async_dns_queue_head);
561 |
562 | while (head != NULL((void*)0) && async_dns_in_flight <= name_resolve_concurrency) {
563 | caqm = (async_dns_queue_msg_t *)wmem_list_frame_data(head);
564 | wmem_list_remove_frame(async_dns_queue_head, head);
565 | if (caqm->family == AF_INET2) {
566 | ares_gethostbyaddr(ghba_chan, &caqm->addr.ip4, sizeof(uint32_t), AF_INET2,
567 | c_ares_ghba_cb, caqm);
568 | async_dns_in_flight++;
569 | } else if (caqm->family == AF_INET610) {
570 | ares_gethostbyaddr(ghba_chan, &caqm->addr.ip6, sizeof(ws_in6_addr),
571 | AF_INET610, c_ares_ghba_cb, caqm);
572 | async_dns_in_flight++;
573 | }
574 |
575 | head = wmem_list_head(async_dns_queue_head);
576 | }
577 |
578 | g_mutex_unlock(&async_dns_queue_mtx);
579 | }
580 |
581 | static void
582 | wait_for_async_queue(void)
583 | {
584 | struct timeval tv = { 0, 0 };
585 | int nfds;
586 | fd_set rfds, wfds;
587 |
588 | new_resolved_objects = false0;
589 |
590 | if (!async_dns_initialized) {
591 | maxmind_db_lookup_process();
592 | return;
593 | }
594 |
595 | while (1) {
596 | /* We're switching to synchronous lookups, so process anything in
597 | * the asynchronous queue. There might be more in the queue than
598 | * name_resolve_concurrency allows, so check each cycle.
599 | */
600 | process_async_dns_queue();
601 |
602 | FD_ZERO(&rfds)do { unsigned int __i; fd_set *__arr = (&rfds); for (__i = 0; __i < sizeof (fd_set) / sizeof (__fd_mask); ++__i) ((__arr )->__fds_bits)[__i] = 0; } while (0);
603 | FD_ZERO(&wfds)do { unsigned int __i; fd_set *__arr = (&wfds); for (__i = 0; __i < sizeof (fd_set) / sizeof (__fd_mask); ++__i) ((__arr )->__fds_bits)[__i] = 0; } while (0);
604 | nfds = ares_fds(ghba_chan, &rfds, &wfds);
605 | if (nfds == 0) {
606 | /* No more requests waiting for reply; we're done here. */
607 | break;
608 | }
609 |
610 | /* See comment in wait_for_sync_resolv() about ares_timeout() being
611 | * O(N) in the number of outstanding requests until c-ares 1.20, and
612 | * why we might as well just set a 1 second to select().
613 | */
614 | tv.tv_sec = 1;
615 | tv.tv_usec = 0;
616 |
617 | if (select(nfds, &rfds, &wfds, NULL((void*)0), &tv) == -1) { /* call to select() failed */
618 | /* If it's interrupted by a signal, no need to put out a message */
619 | if (errno(*__errno_location ()) != EINTR4)
620 | fprintf(stderrstderr, "Warning: call to select() failed, error is %s\n", g_strerror(errno(*__errno_location ())));
621 | return;
622 | }
623 | ares_process(ghba_chan, &rfds, &wfds);
624 | }
625 |
626 | maxmind_db_lookup_process();
627 | return;
628 | }
629 |
630 | static void
631 | sync_lookup_ip4(const uint32_t addr)
632 | {
633 | bool_Bool completed = false0;
634 | sync_dns_data_t *sdd;
635 |
636 | if (!async_dns_initialized) {
637 | /*
638 | * c-ares not initialized. Bail out.
639 | */
640 | return;
641 | }
642 |
643 | /*
644 | * Start the request.
645 | */
646 | sdd = g_new(sync_dns_data_t, 1)((sync_dns_data_t *) g_malloc_n ((1), sizeof (sync_dns_data_t )));
647 | sdd->family = AF_INET2;
648 | sdd->addr.ip4 = addr;
649 | sdd->completed = &completed;
650 | ares_gethostbyaddr(ghba_chan, &addr, sizeof(uint32_t), AF_INET2,
651 | c_ares_ghba_sync_cb, sdd);
652 |
653 | /*
654 | * Now wait for it to finish.
655 | */
656 | wait_for_sync_resolv(&completed);
657 | }
658 |
659 | static void
660 | sync_lookup_ip6(const ws_in6_addr *addrp)
661 | {
662 | bool_Bool completed = false0;
663 | sync_dns_data_t *sdd;
664 |
665 | if (!async_dns_initialized) {
666 | /*
667 | * c-ares not initialized. Bail out.
668 | */
669 | return;
670 | }
671 |
672 | /*
673 | * Start the request.
674 | */
675 | sdd = g_new(sync_dns_data_t, 1)((sync_dns_data_t *) g_malloc_n ((1), sizeof (sync_dns_data_t )));
676 | sdd->family = AF_INET610;
677 | memcpy(&sdd->addr.ip6, addrp, sizeof(sdd->addr.ip6));
678 | sdd->completed = &completed;
679 | ares_gethostbyaddr(ghba_chan, addrp, sizeof(ws_in6_addr), AF_INET610,
680 | c_ares_ghba_sync_cb, sdd);
681 |
682 | /*
683 | * Now wait for it to finish.
684 | */
685 | wait_for_sync_resolv(&completed);
686 | }
687 |
688 | void
689 | set_resolution_synchrony(bool_Bool synchronous)
690 | {
691 | resolve_synchronously = synchronous;
692 | maxmind_db_set_synchrony(synchronous);
693 |
694 | if (synchronous) {
695 | wait_for_async_queue();
696 | }
697 | }
698 |
699 | static void
700 | c_ares_set_dns_servers(void)
701 | {
702 | if ((!async_dns_initialized) || (!use_custom_dns_server_list))
703 | return;
704 |
705 | if (ndnsservers == 0) {
706 | //clear the list of servers. This may effectively disable name resolution
707 | ares_set_servers_ports(ghba_chan, NULL((void*)0));
708 | ares_set_servers_ports(ghbn_chan, NULL((void*)0));
709 | } else {
710 | struct ares_addr_port_node* servers = wmem_alloc_array(NULL, struct ares_addr_port_node, ndnsservers)((struct ares_addr_port_node*)wmem_alloc((((void*)0)), (((((ndnsservers )) <= 0) || ((size_t)sizeof(struct ares_addr_port_node) > (9223372036854775807L / (size_t)((ndnsservers))))) ? 0 : (sizeof (struct ares_addr_port_node) * ((ndnsservers))))));
711 | ws_in4_addr ipv4addr;
712 | ws_in6_addr ipv6addr;
713 | bool_Bool invalid_IP_found = false0;
714 | struct ares_addr_port_node* server;
715 | unsigned i;
716 | for (i = 0, server = servers; i < ndnsservers-1; i++, server++) {
717 | if (ws_inet_pton6(dnsserverlist_uats[i].ipaddr, &ipv6addr)) {
718 | server->family = AF_INET610;
719 | memcpy(&server->addr.addr6, &ipv6addr, 16);
720 | } else if (ws_inet_pton4(dnsserverlist_uats[i].ipaddr, &ipv4addr)) {
721 | server->family = AF_INET2;
722 | memcpy(&server->addr.addr4, &ipv4addr, 4);
723 | } else {
724 | //This shouldn't happen, but just in case...
725 | invalid_IP_found = true1;
726 | server->family = 0;
727 | memset(&server->addr.addr4, 0, 4);
728 | break;
729 | }
730 |
731 | server->udp_port = (int)dnsserverlist_uats[i].udp_port;
732 | server->tcp_port = (int)dnsserverlist_uats[i].tcp_port;
733 |
734 | server->next = (server+1);
735 | }
736 | if (!invalid_IP_found) {
737 | if (ws_inet_pton6(dnsserverlist_uats[i].ipaddr, &ipv6addr)) {
738 | server->family = AF_INET610;
739 | memcpy(&server->addr.addr6, &ipv6addr, 16);
740 | }
741 | else if (ws_inet_pton4(dnsserverlist_uats[i].ipaddr, &ipv4addr)) {
742 | server->family = AF_INET2;
743 | memcpy(&server->addr.addr4, &ipv4addr, 4);
744 | } else {
745 | //This shouldn't happen, but just in case...
746 | server->family = 0;
747 | memset(&server->addr.addr4, 0, 4);
748 | }
749 | }
750 | server->udp_port = (int)dnsserverlist_uats[i].udp_port;
751 | server->tcp_port = (int)dnsserverlist_uats[i].tcp_port;
752 |
753 | server->next = NULL((void*)0);
754 |
755 | ares_set_servers_ports(ghba_chan, servers);
756 | ares_set_servers_ports(ghbn_chan, servers);
757 | wmem_free(NULL((void*)0), servers);
758 | }
759 | }
760 |
761 | typedef struct {
762 | uint32_t mask;
763 | size_t mask_length;
764 | const char* name; /* Shallow copy */
765 | } subnet_entry_t;
766 |
767 | /* Maximum supported line length of hosts, services, manuf, etc. */
768 | #define MAX_LINELEN1024 1024
769 |
770 | /** Read a line without trailing (CR)LF. Returns -1 on failure. */
771 | static int
772 | fgetline(char *buf, int size, FILE *fp)
773 | {
774 | if (fgets(buf, size, fp)) {
15 | ← | Value of 'errno' was not checked and may be overwritten by function 'fgets'
775 | int len = (int)strcspn(buf, "\r\n");
776 | buf[len] = '\0';
777 | return len;
778 | }
779 | return -1;
780 |
781 | } /* fgetline */
782 |
783 |
784 | /*
785 | * Local function definitions
786 | */
787 | static subnet_entry_t subnet_lookup(const uint32_t addr);
788 | static void subnet_entry_set(uint32_t subnet_addr, const uint8_t mask_length, const char* name);
789 |
790 | static unsigned serv_port_custom_hash(const void *k)
791 | {
792 | const serv_port_key_t *key = (const serv_port_key_t*)k;
793 | return key->port + (key->type << 16);
794 | }
795 |
796 | static gboolean serv_port_custom_equal(const void *k1, const void *k2)
797 | {
798 | const serv_port_key_t *key1 = (const serv_port_key_t*)k1;
799 | const serv_port_key_t *key2 = (const serv_port_key_t*)k2;
800 |
801 | return (key1->port == key2->port) && (key1->type == key2->type);
802 | }
803 |
804 | static void
805 | add_custom_service_name(port_type proto, const unsigned port, const char *service_name)
806 | {
807 | char *name;
808 | serv_port_key_t *key, *orig_key;
809 |
810 | key = wmem_new(addr_resolv_scope, serv_port_key_t)((serv_port_key_t*)wmem_alloc((addr_resolv_scope), sizeof(serv_port_key_t )));
811 | key->port = (uint16_t)port;
812 | key->type = proto;
813 |
814 | if (wmem_map_lookup_extended(serv_port_custom_hashtable, key, (const void**)&orig_key, (void**)&name)) {
815 | wmem_free(addr_resolv_scope, orig_key);
816 | wmem_free(addr_resolv_scope, name);
817 | }
818 |
819 | name = wmem_strdup(addr_resolv_scope, service_name);
820 | wmem_map_insert(serv_port_custom_hashtable, key, name);
821 |
822 | // A new custom entry is not a new resolved object.
823 | // new_resolved_objects = true;
824 | }
825 |
826 | static void
827 | add_service_name(port_type proto, const unsigned port, const char *service_name)
828 | {
829 | serv_port_key_t *key = wmem_new(addr_resolv_scope, serv_port_key_t)((serv_port_key_t*)wmem_alloc((addr_resolv_scope), sizeof(serv_port_key_t )));
830 | key->port = (uint16_t)port;
831 | key->type = proto;
832 |
833 | wmem_map_insert(serv_port_hashtable, key, (void*)service_name);
834 |
835 | new_resolved_objects = true1;
836 | }
837 |
838 | static void
839 | parse_service_line (char *line)
840 | {
841 | char *cp;
842 | char *service;
843 | char *port;
844 | port_type proto;
845 | struct cb_serv_data cb_data;
846 | range_t *port_rng = NULL((void*)0);
847 |
848 | if ((cp = strchr(line, '#')))
849 | *cp = '\0';
850 |
851 | if ((cp = strtok(line, " \t")) == NULL((void*)0))
852 | return;
853 |
854 | service = cp;
855 |
856 | if ((cp = strtok(NULL((void*)0), " \t")) == NULL((void*)0))
857 | return;
858 |
859 | port = cp;
860 |
861 | if (strtok(cp, "/") == NULL((void*)0))
862 | return;
863 |
864 | if (range_convert_str(NULL((void*)0), &port_rng, port, UINT16_MAX(65535)) != CVT_NO_ERROR) {
865 | wmem_free (NULL((void*)0), port_rng);
866 | return;
867 | }
868 |
869 | while ((cp = strtok(NULL((void*)0), "/")) != NULL((void*)0)) {
870 | if (strcmp(cp, "tcp") == 0) {
871 | proto = PT_TCP;
872 | }
873 | else if (strcmp(cp, "udp") == 0) {
874 | proto = PT_UDP;
875 | }
876 | else if (strcmp(cp, "sctp") == 0) {
877 | proto = PT_SCTP;
878 | }
879 | else if (strcmp(cp, "dccp") == 0) {
880 | proto = PT_DCCP;
881 | }
882 | else {
883 | break;
884 | }
885 | cb_data.service = service;
886 | cb_data.proto = proto;
887 | range_foreach(port_rng, add_serv_port_cb, &cb_data);
888 | }
889 |
890 | wmem_free (NULL((void*)0), port_rng);
891 | } /* parse_service_line */
892 |
893 |
894 | static void
895 | add_serv_port_cb(const uint32_t port, void *ptr)
896 | {
897 | struct cb_serv_data *cb_data = (struct cb_serv_data *)ptr;
898 |
899 | if ( port ) {
900 | add_custom_service_name(cb_data->proto, port, cb_data->service);
901 | }
902 | }
903 |
904 |
905 | static bool_Bool
906 | parse_services_file(const char * path)
907 | {
908 | FILE *serv_p;
909 | char buf[MAX_LINELEN1024];
910 |
911 | /* services hash table initialization */
912 | serv_p = ws_fopenfopen(path, "r");
913 |
914 | if (serv_p == NULL((void*)0))
915 | return false0;
916 |
917 | while (fgetline(buf, sizeof(buf), serv_p) >= 0) {
918 | parse_service_line(buf);
919 | }
920 |
921 | fclose(serv_p);
922 | return true1;
923 | }
924 |
925 | /* -----------------
926 | * unsigned integer to ascii
927 | */
928 | static char *
929 | wmem_utoa(wmem_allocator_t *allocator, unsigned port)
930 | {
931 | char *bp = (char *)wmem_alloc(allocator, MAXNAMELEN64);
932 |
933 | /* XXX, uint32_to_str() ? */
934 | uint32_to_str_buf(port, bp, MAXNAMELEN64);
935 | return bp;
936 | }
937 |
938 | static const char *
939 | _serv_name_lookup(port_type proto, unsigned port)
940 | {
941 | const char* name = NULL((void*)0);
942 | ws_services_proto_t p;
943 | ws_services_entry_t const *serv;
944 |
945 | const serv_port_key_t custom_key = { (uint16_t)port, proto };
946 | /* Look in the cache. Use an extended lookup so we can distinguish a port
947 | * we already tried but had no name from one we haven't tried. */
948 | if (!wmem_map_lookup_extended(serv_port_hashtable, &custom_key, NULL((void*)0), (void **)&name)) {
949 | /* Try the user custom table */
950 | name = wmem_map_lookup(serv_port_custom_hashtable, &custom_key);
951 |
952 | if (name == NULL((void*)0)) {
953 | /* now look in the global tables */
954 | bool_Bool valid_proto = true1;
955 | switch(proto) {
956 | case PT_TCP: p = ws_tcp; break;
957 | case PT_UDP: p = ws_udp; break;
958 | case PT_SCTP: p = ws_sctp; break;
959 | case PT_DCCP: p = ws_dccp; break;
960 | default: valid_proto = false0;
961 | }
962 | if (valid_proto) {
963 | serv = global_services_lookup(port, p);
964 | if (serv) {
965 | name = serv->name;
966 | }
967 | }
968 | }
969 |
970 | /* Cache result (even if NULL, so we can know we have no result.) */
971 | add_service_name(proto, port, name);
972 | }
973 |
974 | return name;
975 | }
976 |
977 | const char *
978 | try_serv_name_lookup(port_type proto, unsigned port)
979 | {
980 | return (proto == PT_NONE) ? NULL((void*)0) : _serv_name_lookup(proto, port);
981 | }
982 |
983 | const char *
984 | serv_name_lookup(port_type proto, unsigned port)
985 | {
986 | const char *name;
987 |
988 | /* first look for the name */
989 | name = _serv_name_lookup(proto, port);
990 | if (name != NULL((void*)0))
991 | return name;
992 |
993 | /* No resolved name. Do we have a cached numeric string? */
994 | const serv_port_key_t key = { (uint16_t)port, PT_NONE };
995 | name = (const char*)wmem_map_lookup(serv_port_hashtable, &key);
996 | /* No name; create the numeric string. */
997 | if (name == NULL((void*)0)) {
998 | name = wmem_strdup_printf(addr_resolv_scope, "%u", port);
999 | add_service_name(PT_NONE, port, name);
1000 | }
1001 |
1002 | return name;
1003 | }
1004 |
1005 | static void
1006 | initialize_services(const char* app_env_var_prefix)
1007 | {
1008 | ws_assert(serv_port_hashtable == NULL)do { if ((1) && !(serv_port_hashtable == ((void*)0))) ws_log_fatal_full("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 1008, __func__, "assertion failed: %s", "serv_port_hashtable == ((void*)0)" ); } while (0);
1009 | serv_port_hashtable = wmem_map_new(addr_resolv_scope, serv_port_custom_hash, serv_port_custom_equal);
1010 | ws_assert(serv_port_custom_hashtable == NULL)do { if ((1) && !(serv_port_custom_hashtable == ((void *)0))) ws_log_fatal_full("", LOG_LEVEL_ERROR, "epan/addr_resolv.c" , 1010, __func__, "assertion failed: %s", "serv_port_custom_hashtable == ((void*)0)" ); } while (0);
1011 | serv_port_custom_hashtable = wmem_map_new(addr_resolv_scope, serv_port_custom_hash, serv_port_custom_equal);
1012 |
1013 | /* Compute the pathname of the global services file. */
1014 | if (g_services_path == NULL((void*)0)) {
1015 | g_services_path = get_datafile_path(ENAME_SERVICES"services", app_env_var_prefix);
1016 | }
1017 | parse_services_file(g_services_path);
1018 |
1019 | /* Compute the pathname of the personal services file */
1020 | if (g_pservices_path == NULL((void*)0)) {
1021 | /* Check profile directory before personal configuration */
1022 | g_pservices_path = get_persconffile_path(ENAME_SERVICES"services", true1, app_env_var_prefix);
1023 | if (!parse_services_file(g_pservices_path)) {
1024 | g_free(g_pservices_path);
1025 | g_pservices_path = get_persconffile_path(ENAME_SERVICES"services", false0, app_env_var_prefix);
1026 | parse_services_file(g_pservices_path);
1027 | }
1028 | }
1029 | }
1030 |
1031 | static void
1032 | service_name_lookup_cleanup(void)
1033 | {
1034 | serv_port_hashtable = NULL((void*)0);
1035 | serv_port_custom_hashtable = NULL((void*)0);
1036 | g_free(g_services_path);
1037 | g_services_path = NULL((void*)0);
1038 | g_free(g_pservices_path);
1039 | g_pservices_path = NULL((void*)0);
1040 | }
1041 |
1042 | static void
1043 | parse_enterprises_line (char *line)
1044 | {
1045 | char *tok, *dec_str, *org_str;
1046 | uint32_t dec;
1047 | bool_Bool had_comment = false0;
1048 |
1049 | /* Stop the line at any comment found */
1050 | if ((tok = strchr(line, '#'))) {
1051 | *tok = '\0';
1052 | had_comment = true1;
1053 | }
1054 | /* Get enterprise number */
1055 | dec_str = strtok(line, " \t");
1056 | if (!dec_str)
1057 | return;
1058 | /* Get enterprise name */
1059 | org_str = strtok(NULL((void*)0), ""); /* everything else */
1060 | if (org_str && had_comment) {
1061 | /* Only need to strip after (between name and where comment was) */
1062 | org_str = g_strchomp(org_str);
1063 | }
1064 | if (!org_str)
1065 | return;
1066 |
1067 | /* Add entry using number as key */
1068 | if (!ws_strtou32(dec_str, NULL((void*)0), &dec))
1069 | return;
1070 | g_hash_table_insert(enterprises_hashtable, GUINT_TO_POINTER(dec)((gpointer) (gulong) (dec)), g_strdup(org_str)g_strdup_inline (org_str));
1071 | }
1072 |
1073 |
1074 | static bool_Bool
1075 | parse_enterprises_file(const char * path)
1076 | {
1077 | FILE *fp;
1078 | char buf[MAX_LINELEN1024];
1079 |
1080 | fp = ws_fopenfopen(path, "r");
1081 | if (fp == NULL((void*)0))
1082 | return false0;
1083 |
1084 | while (fgetline(buf, sizeof(buf), fp) >= 0) {
1085 | parse_enterprises_line(buf);
1086 | }
1087 |
1088 | fclose(fp);
1089 | return true1;
1090 | }
1091 |
1092 | static void
1093 | initialize_enterprises(const char* app_env_var_prefix)
1094 | {
1095 | ws_assert(enterprises_hashtable == NULL)do { if ((1) && !(enterprises_hashtable == ((void*)0) )) ws_log_fatal_full("", LOG_LEVEL_ERROR, "epan/addr_resolv.c" , 1095, __func__, "assertion failed: %s", "enterprises_hashtable == ((void*)0)" ); } while (0);
1096 | enterprises_hashtable = g_hash_table_new_full(NULL((void*)0), NULL((void*)0), NULL((void*)0), g_free);
1097 |
1098 | if (g_enterprises_path == NULL((void*)0)) {
1099 | g_enterprises_path = get_datafile_path(ENAME_ENTERPRISES"enterprises", app_env_var_prefix);
1100 | }
1101 | parse_enterprises_file(g_enterprises_path);
1102 |
1103 | /* Populate entries from profile or personal */
1104 | if (g_penterprises_path == NULL((void*)0)) {
1105 | /* Check profile directory before personal configuration */
1106 | g_penterprises_path = get_persconffile_path(ENAME_ENTERPRISES"enterprises", true1, app_env_var_prefix);
1107 | if (!file_exists(g_penterprises_path)) {
1108 | g_free(g_penterprises_path);
1109 | g_penterprises_path = get_persconffile_path(ENAME_ENTERPRISES"enterprises", false0, app_env_var_prefix);
1110 | }
1111 | }
1112 | /* Parse personal file (if present) */
1113 | parse_enterprises_file(g_penterprises_path);
1114 | }
1115 |
1116 | const char *
1117 | try_enterprises_lookup(uint32_t value)
1118 | {
1119 | /* Trying extra entries first. N.B. This does allow entries to be overwritten and found.. */
1120 | const char *name = (const char *)g_hash_table_lookup(enterprises_hashtable, GUINT_TO_POINTER(value)((gpointer) (gulong) (value)));
1121 | if (name)
1122 | return name;
1123 |
1124 | return val_to_str_ext_const(value, &enterprise_val_ext, "Unknown");
1125 | }
1126 |
1127 | const char *
1128 | enterprises_lookup(uint32_t value, const char *unknown_str)
1129 | {
1130 | const char *s;
1131 |
1132 | s = try_enterprises_lookup(value);
1133 | if (s != NULL((void*)0))
1134 | return s;
1135 | if (unknown_str != NULL((void*)0))
1136 | return unknown_str;
1137 | return "<Unknown>";
1138 | }
1139 |
1140 | void
1141 | enterprises_base_custom(char *buf, uint32_t value)
1142 | {
1143 | const char *s;
1144 |
1145 | if ((s = try_enterprises_lookup(value)) == NULL((void*)0))
1146 | s = ITEM_LABEL_UNKNOWN_STR"Unknown";
1147 | snprintf(buf, ITEM_LABEL_LENGTH240, "%s (%u)", s, value);
1148 | }
1149 |
1150 | static void
1151 | enterprises_cleanup(void)
1152 | {
1153 | ws_assert(enterprises_hashtable)do { if ((1) && !(enterprises_hashtable)) ws_log_fatal_full ("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 1153, __func__, "assertion failed: %s" , "enterprises_hashtable"); } while (0);
1154 | g_hash_table_destroy(enterprises_hashtable);
1155 | enterprises_hashtable = NULL((void*)0);
1156 | g_free(g_enterprises_path);
1157 | g_enterprises_path = NULL((void*)0);
1158 | g_free(g_penterprises_path);
1159 | g_penterprises_path = NULL((void*)0);
1160 | }
1161 |
1162 | /* Fill in an IP4 structure with info from subnets file or just with the
1163 | * string form of the address.
1164 | */
1165 | bool_Bool
1166 | fill_dummy_ip4(const unsigned addr, hashipv4_t* volatile tp)
1167 | {
1168 | subnet_entry_t subnet_entry;
1169 |
1170 | /* return value : true if addr matches any subnet */
1171 | bool_Bool cidr_covered = false0;
1172 |
1173 | /* Overwrite if we get async DNS reply */
1174 |
1175 | /* Do we have a subnet for this address? */
1176 | subnet_entry = subnet_lookup(addr);
1177 | if (0 != subnet_entry.mask) {
1178 | /* Print name, then '.' then IP address after subnet mask */
1179 | uint32_t host_addr;
1180 | char buffer[WS_INET_ADDRSTRLEN16];
1181 | char* paddr;
1182 | size_t i;
1183 |
1184 | host_addr = addr & (~subnet_entry.mask);
1185 | ip_addr_to_str_buf(&host_addr, buffer, WS_INET_ADDRSTRLEN16);
1186 | paddr = buffer;
1187 |
1188 | /* Skip to first octet that is not totally masked
1189 | * If length of mask is 32, we chomp the whole address.
1190 | * If the address string starts '.' (should not happen?),
1191 | * we skip that '.'.
1192 | */
1193 | i = subnet_entry.mask_length / 8;
1194 | while(*(paddr) != '\0' && i > 0) {
1195 | if (*(++paddr) == '.') {
1196 | --i;
1197 | }
1198 | }
1199 |
1200 | /* There are more efficient ways to do this, but this is safe if we
1201 | * trust snprintf and MAXDNSNAMELEN
1202 | */
1203 | snprintf(tp->name, MAXDNSNAMELEN256, "%s%s", subnet_entry.name, paddr);
1204 |
1205 | /* Evaluate the subnet in CIDR notation
1206 | * Reuse buffers built above
1207 | */
1208 | uint32_t subnet_addr;
1209 | subnet_addr = addr & subnet_entry.mask;
1210 |
1211 | char buffer_subnet[WS_INET_ADDRSTRLEN16];
1212 | ip_addr_to_str_buf(&subnet_addr, buffer_subnet, WS_INET_ADDRSTRLEN16);
1213 |
1214 | char buffer_cidr[WS_INET_CIDRADDRSTRLEN19];
1215 | snprintf(buffer_cidr, WS_INET_CIDRADDRSTRLEN19, "%s%s%u", buffer_subnet, "/", (unsigned)subnet_entry.mask_length);
1216 |
1217 | snprintf(tp->cidr_addr, WS_INET_CIDRADDRSTRLEN19, "%s%s%u", buffer_subnet, "/", (unsigned)subnet_entry.mask_length);
1218 | cidr_covered = true1;
1219 | } else {
1220 | /* XXX: This means we end up printing "1.2.3.4 (1.2.3.4)" in many cases */
1221 | ip_addr_to_str_buf(&addr, tp->name, MAXDNSNAMELEN256);
1222 |
1223 | /* IP does not belong to any known subnet, just indicate this IP without "/.32" */
1224 | ip_addr_to_str_buf(&addr, tp->cidr_addr, MAXDNSNAMELEN256);
1225 | }
1226 | return cidr_covered;
1227 | }
1228 |
1229 |
1230 | /* Fill in an IP6 structure with the string form of the address.
1231 | */
1232 | static void
1233 | fill_dummy_ip6(hashipv6_t* volatile tp)
1234 | {
1235 | /* Overwrite if we get async DNS reply */
1236 | (void) g_strlcpy(tp->name, tp->ip6, MAXDNSNAMELEN256);
1237 | }
1238 |
1239 | static void
1240 | c_ares_ghba_cb(void *arg, int status, int timeouts _U___attribute__((unused)), struct hostent *he) {
1241 | async_dns_queue_msg_t *caqm = (async_dns_queue_msg_t *)arg;
1242 | char **p;
1243 |
1244 | if (!caqm) return;
1245 | /* XXX, what to do if async_dns_in_flight == 0? */
1246 | async_dns_in_flight--;
1247 |
1248 | if (status == ARES_SUCCESS) {
1249 | for (p = he->h_addr_list; *p != NULL((void*)0); p++) {
1250 | switch(caqm->family) {
1251 | case AF_INET2:
1252 | add_ipv4_name(caqm->addr.ip4, he->h_name, false0);
1253 | break;
1254 | case AF_INET610:
1255 | add_ipv6_name(&caqm->addr.ip6, he->h_name, false0);
1256 | break;
1257 | default:
1258 | /* Throw an exception? */
1259 | break;
1260 | }
1261 | }
1262 | }
1263 | wmem_free(addr_resolv_scope, caqm);
1264 | }
1265 |
1266 | /* --------------- */
1267 | hashipv4_t *
1268 | new_ipv4(const unsigned addr)
1269 | {
1270 | hashipv4_t *tp = wmem_new(addr_resolv_scope, hashipv4_t)((hashipv4_t*)wmem_alloc((addr_resolv_scope), sizeof(hashipv4_t )));
1271 | tp->addr = addr;
1272 | tp->flags = 0;
1273 | tp->name[0] = '\0';
1274 | ip_addr_to_str_buf(&addr, tp->ip, sizeof(tp->ip));
1275 | return tp;
1276 | }
1277 |
1278 | static hashipv4_t *
1279 | host_lookup(const unsigned addr)
1280 | {
1281 | hashipv4_t * volatile tp;
1282 |
1283 | tp = (hashipv4_t *)wmem_map_lookup(ipv4_hash_table, GUINT_TO_POINTER(addr)((gpointer) (gulong) (addr)));
1284 | if (tp == NULL((void*)0)) {
1285 | /*
1286 | * We don't already have an entry for this host name; create one,
1287 | * and then try to resolve it.
1288 | */
1289 | tp = new_ipv4(addr);
1290 | fill_dummy_ip4(addr, tp);
1291 | wmem_map_insert(ipv4_hash_table, GUINT_TO_POINTER(addr)((gpointer) (gulong) (addr)), tp);
1292 | } else if (tp->flags & TRIED_OR_RESOLVED_MASK((1U<<0) | (1U<<1))) {
1293 | return tp;
1294 | }
1295 |
1296 | /*
1297 | * This hasn't been resolved yet, and we haven't tried to
1298 | * resolve it already.
1299 | */
1300 |
1301 | if (!gbl_resolv_flags.network_name)
1302 | return tp;
1303 |
1304 | if (gbl_resolv_flags.use_external_net_name_resolver) {
1305 | tp->flags |= TRIED_RESOLVE_ADDRESS(1U<<0);
1306 |
1307 | if (async_dns_initialized) {
1308 | /* c-ares is initialized, so we can use it */
1309 | if (resolve_synchronously || name_resolve_concurrency == 0) {
1310 | /*
1311 | * Either all names are to be resolved synchronously or
1312 | * the concurrency level is 0; do the resolution
1313 | * synchronously.
1314 | */
1315 | sync_lookup_ip4(addr);
1316 | } else {
1317 | /*
1318 | * Names are to be resolved asynchronously, and we
1319 | * allow at least one asynchronous request in flight;
1320 | * post an asynchronous request.
1321 | */
1322 | async_dns_queue_msg_t *caqm;
1323 |
1324 | caqm = wmem_new(addr_resolv_scope, async_dns_queue_msg_t)((async_dns_queue_msg_t*)wmem_alloc((addr_resolv_scope), sizeof (async_dns_queue_msg_t)));
1325 | caqm->family = AF_INET2;
1326 | caqm->addr.ip4 = addr;
1327 | wmem_list_append(async_dns_queue_head, (void *) caqm);
1328 | }
1329 | }
1330 | }
1331 |
1332 | return tp;
1333 |
1334 | } /* host_lookup */
1335 |
1336 | /* --------------- */
1337 | static hashipv6_t *
1338 | new_ipv6(const ws_in6_addr *addr)
1339 | {
1340 | hashipv6_t *tp = wmem_new(addr_resolv_scope, hashipv6_t)((hashipv6_t*)wmem_alloc((addr_resolv_scope), sizeof(hashipv6_t )));
1341 | memcpy(tp->addr, addr->bytes, sizeof tp->addr);
1342 | tp->flags = 0;
1343 | tp->name[0] = '\0';
1344 | ip6_to_str_buf(addr, tp->ip6, sizeof(tp->ip6));
1345 | return tp;
1346 | }
1347 |
1348 | /* ------------------------------------ */
1349 | static hashipv6_t *
1350 | host_lookup6(const ws_in6_addr *addr)
1351 | {
1352 | hashipv6_t * volatile tp;
1353 |
1354 | tp = (hashipv6_t *)wmem_map_lookup(ipv6_hash_table, addr);
1355 | if (tp == NULL((void*)0)) {
1356 | /*
1357 | * We don't already have an entry for this host name; create one,
1358 | * and then try to resolve it.
1359 | */
1360 | ws_in6_addr *addr_key;
1361 |
1362 | addr_key = wmem_new(addr_resolv_scope, ws_in6_addr)((ws_in6_addr*)wmem_alloc((addr_resolv_scope), sizeof(ws_in6_addr )));
1363 | tp = new_ipv6(addr);
1364 | memcpy(addr_key, addr, 16);
1365 | fill_dummy_ip6(tp);
1366 | wmem_map_insert(ipv6_hash_table, addr_key, tp);
1367 | } else if (tp->flags & TRIED_OR_RESOLVED_MASK((1U<<0) | (1U<<1))) {
1368 | return tp;
1369 | }
1370 |
1371 | /*
1372 | * This hasn't been resolved yet, and we haven't tried to
1373 | * resolve it already.
1374 | */
1375 |
1376 | if (!gbl_resolv_flags.network_name)
1377 | return tp;
1378 |
1379 | if (gbl_resolv_flags.use_external_net_name_resolver) {
1380 | tp->flags |= TRIED_RESOLVE_ADDRESS(1U<<0);
1381 |
1382 | if (async_dns_initialized) {
1383 | /* c-ares is initialized, so we can use it */
1384 | if (resolve_synchronously || name_resolve_concurrency == 0) {
1385 | /*
1386 | * Either all names are to be resolved synchronously or
1387 | * the concurrency level is 0; do the resolution
1388 | * synchronously.
1389 | */
1390 | sync_lookup_ip6(addr);
1391 | } else {
1392 | /*
1393 | * Names are to be resolved asynchronously, and we
1394 | * allow at least one asynchronous request in flight;
1395 | * post an asynchronous request.
1396 | */
1397 | async_dns_queue_msg_t *caqm;
1398 |
1399 | caqm = wmem_new(addr_resolv_scope, async_dns_queue_msg_t)((async_dns_queue_msg_t*)wmem_alloc((addr_resolv_scope), sizeof (async_dns_queue_msg_t)));
1400 | caqm->family = AF_INET610;
1401 | memcpy(&caqm->addr.ip6, addr, sizeof(caqm->addr.ip6));
1402 | wmem_list_append(async_dns_queue_head, (void *) caqm);
1403 | }
1404 | }
1405 | }
1406 |
1407 | return tp;
1408 |
1409 | } /* host_lookup6 */
1410 |
1411 | /*
1412 | * Ethernet / manufacturer resolution
1413 | *
1414 | * The following functions implement ethernet address resolution and
1415 | * ethers files parsing (see ethers(4)).
1416 | *
1417 | * The manuf file has the same format as ethers(4) except that names are
1418 | * truncated to MAXMANUFLEN-1 (8) characters and that an address contains
1419 | * only 3 bytes (instead of 6).
1420 | *
1421 | * Notes:
1422 | *
1423 | * I decide to not use the existing functions (see ethers(3) on some
1424 | * operating systems) for the following reasons:
1425 | * - performance gains (use of hash tables and some other enhancements),
1426 | * - use of two ethers files (system-wide and per user),
1427 | * - avoid the use of NIS maps,
1428 | * - lack of these functions on some systems.
1429 | *
1430 | * So the following functions do _not_ behave as the standard ones.
1431 | *
1432 | * -- Laurent.
1433 | */
1434 |
1435 | /*
1436 | * Converts Ethernet addresses of the form aa:bb:cc or aa:bb:cc:dd:ee:ff/28.
1437 | * '-' is also supported as a separator. The
1438 | * octets must be exactly two hexadecimal characters and the mask must be either
1439 | * 28 or 36. Pre-condition: cp MUST be at least 21 bytes.
1440 | */
1441 | static bool_Bool
1442 | parse_ether_address_fast(const unsigned char *cp, ether_t *eth, unsigned int *mask,
1443 | const bool_Bool accept_mask)
1444 | {
1445 | /* XXX copied from strutil.c */
1446 | /* a map from ASCII hex chars to their value */
1447 | static const int8_t str_to_nibble[256] = {
1448 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1449 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1450 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1451 | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9,-1,-1,-1,-1,-1,-1,
1452 | -1,10,11,12,13,14,15,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1453 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1454 | -1,10,11,12,13,14,15,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1455 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1456 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1457 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1458 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1459 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1460 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1461 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1462 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,
1463 | -1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1,-1
1464 | };
1465 | const uint8_t *str_to_nibble_usg = (const uint8_t *)str_to_nibble;
1466 |
1467 | unsigned char sep = cp[2];
1468 | if ((sep != ':' && sep != '-') || cp[5] != sep) {
1469 | /* Unexpected separators. */
1470 | return false0;
1471 | }
1472 |
1473 | /* N.B. store octet values in an int to detect invalid (-1) entries */
1474 | int num0 = (str_to_nibble_usg[cp[0]] << 4) | (int8_t)str_to_nibble_usg[cp[1]];
1475 | int num1 = (str_to_nibble_usg[cp[3]] << 4) | (int8_t)str_to_nibble_usg[cp[4]];
1476 | int num2 = (str_to_nibble_usg[cp[6]] << 4) | (int8_t)str_to_nibble_usg[cp[7]];
1477 |
1478 | if ((num0 | num1 | num2) & 0x100) {
1479 | /* Not hexadecimal numbers. */
1480 | return false0;
1481 | }
1482 |
1483 | eth->addr[0] = (uint8_t)num0;
1484 | eth->addr[1] = (uint8_t)num1;
1485 | eth->addr[2] = (uint8_t)num2;
1486 |
1487 | if (cp[8] == '\0' && accept_mask) {
1488 | /* Indicate that this is a manufacturer ID (0 is not allowed as a mask). */
1489 | *mask = 0;
1490 | return true1;
1491 | } else if (cp[8] != sep || !accept_mask) {
1492 | /* Format not handled by this fast path. */
1493 | return false0;
1494 | }
1495 |
1496 | /* N.B. store octet values in an int to detect invalid (-1) entries */
1497 | int num3 = (str_to_nibble_usg[cp[9]] << 4) | (int8_t)str_to_nibble_usg[cp[10]];
1498 | int num4 = (str_to_nibble_usg[cp[12]] << 4) | (int8_t)str_to_nibble_usg[cp[13]];
1499 | int num5 = (str_to_nibble_usg[cp[15]] << 4) | (int8_t)str_to_nibble_usg[cp[16]];
1500 |
1501 | if (((num3 | num4 | num5) & 0x100) || cp[11] != sep || cp[14] != sep) {
1502 | /* Not hexadecimal numbers or invalid separators. */
1503 | return false0;
1504 | }
1505 |
1506 | eth->addr[3] = (uint8_t)num3;
1507 | eth->addr[4] = (uint8_t)num4;
1508 | eth->addr[5] = (uint8_t)num5;
1509 | if (cp[17] == '\0') {
1510 | /* We got 6 bytes, so this is a MAC address (48 is not allowed as a mask). */
1511 | *mask = 48;
1512 | return true1;
1513 | } else if (cp[17] != '/' || cp[20] != '\0') {
1514 | /* Format not handled by this fast path. */
1515 | return false0;
1516 | }
1517 |
1518 | int m1 = cp[18];
1519 | int m2 = cp[19];
1520 | if (m1 == '3' && m2 == '6') { /* Mask /36 */
1521 | eth->addr[4] &= 0xf0;
1522 | eth->addr[5] = 0;
1523 | *mask = 36;
1524 | return true1;
1525 | }
1526 | if (m1 == '2' && m2 == '8') { /* Mask /28 */
1527 | eth->addr[3] &= 0xf0;
1528 | eth->addr[4] = 0;
1529 | eth->addr[5] = 0;
1530 | *mask = 28;
1531 | return true1;
1532 | }
1533 | /* Unsupported mask */
1534 | return false0;
1535 | }
1536 |
1537 | /*
1538 | * If "accept_mask" is false, cp must point to an address that consists
1539 | * of exactly 6 (EUI-48) or 8 (EUI-64) bytes.
1540 | * If "accept_mask" is true, parse an up-to-6-byte sequence with an optional
1541 | * mask.
1542 | */
1543 | static bool_Bool
1544 | parse_ether_address(const char *cp, ether_t *eth, unsigned int *mask,
1545 | const bool_Bool accept_mask)
1546 | {
1547 | int i;
1548 | unsigned long num;
1549 | char *p;
1550 | char sep = '\0';
1551 |
1552 | for (i = 0; i < EUI64_ADDR_LEN8; i++) {
1553 | /* Get a hex number, 1 or 2 digits, no sign characters allowed. */
1554 | if (!g_ascii_isxdigit(*cp)((g_ascii_table[(guchar) (*cp)] & G_ASCII_XDIGIT) != 0))
1555 | return false0;
1556 | num = strtoul(cp, &p, 16);
1557 | if (p == cp)
1558 | return false0; /* failed */
1559 | if (num > 0xFF)
1560 | return false0; /* not a valid octet */
1561 | eth->addr[i] = (uint8_t) num;
1562 | cp = p; /* skip past the number */
1563 |
1564 | /* OK, what character terminated the octet? */
1565 | if (*cp == '/') {
1566 | /* "/" - this has a mask. */
1567 | if (!accept_mask) {
1568 | /* Entries with masks are not allowed in this file. */
1569 | return false0;
1570 | }
1571 | cp++; /* skip past the '/' to get to the mask */
1572 | if (!g_ascii_isdigit(*cp)((g_ascii_table[(guchar) (*cp)] & G_ASCII_DIGIT) != 0))
1573 | return false0; /* no sign allowed */
1574 | num = strtoul(cp, &p, 10);
1575 | if (p == cp)
1576 | return false0; /* failed */
1577 | cp = p; /* skip past the number */
1578 | if (*cp != '\0' && !g_ascii_isspace(*cp)((g_ascii_table[(guchar) (*cp)] & G_ASCII_SPACE) != 0))
1579 | return false0; /* bogus terminator */
1580 | if (num == 0 || num >= 48)
1581 | return false0; /* bogus mask */
1582 | /* Mask out the bits not covered by the mask */
1583 | *mask = (int)num;
1584 | for (i = 0; num >= 8; i++, num -= 8)
1585 | ; /* skip octets entirely covered by the mask */
1586 | /* Mask out the first masked octet */
1587 | eth->addr[i] &= (0xFF << (8 - num));
1588 | i++;
1589 | /* Mask out completely-masked-out octets */
1590 | for (; i < 6; i++)
1591 | eth->addr[i] = 0;
1592 | return true1;
1593 | }
1594 | if (*cp == '\0') {
1595 | /* We're at the end of the address, and there's no mask. */
1596 | if (i == 2) {
1597 | /* We got 3 bytes, so this is a manufacturer ID. */
1598 | if (!accept_mask) {
1599 | /* Manufacturer IDs are not allowed in this file */
1600 | return false0;
1601 | }
1602 | /* Indicate that this is a manufacturer ID (0 is not allowed
1603 | as a mask). */
1604 | *mask = 0;
1605 | return true1;
1606 | }
1607 |
1608 | if (i == 5) {
1609 | /* We got 6 bytes, so this is a MAC address (48 is not allowed as a mask). */
1610 | if (mask) {
1611 | *mask = 48;
1612 | }
1613 | return true1;
1614 | }
1615 |
1616 | if (i == 7) {
1617 | /* We got 8 bytes, so this is a EUI-64 address (64 is not allowed as a mask). */
1618 | if (mask) {
1619 | *mask = 64;
1620 | }
1621 | return true1;
1622 | }
1623 |
1624 | /* We didn't get 3 or 6 or 8 bytes, and there's no mask; this is
1625 | illegal. */
1626 | return false0;
1627 | } else {
1628 | if (sep == '\0') {
1629 | /* We don't know the separator used in this number; it can either
1630 | be ':', '-', or '.'. */
1631 | if (*cp != ':' && *cp != '-' && *cp != '.')
1632 | return false0;
1633 | sep = *cp; /* subsequent separators must be the same */
1634 | } else {
1635 | /* It has to be the same as the first separator */
1636 | if (*cp != sep)
1637 | return false0;
1638 | }
1639 | }
1640 | cp++;
1641 | }
1642 |
1643 | return true1;
1644 | }
1645 |
1646 | static int
1647 | parse_ether_line(char *line, ether_t *eth, unsigned int *mask,
1648 | const bool_Bool accept_mask)
1649 | {
1650 | /*
1651 | * See the ethers(4) or ethers(5) man page for ethers file format
1652 | * (not available on all systems).
1653 | * We allow both ethernet address separators (':' and '-'),
1654 | * as well as Wireshark's '.' separator.
1655 | */
1656 |
1657 | char *cp;
1658 |
1659 | line = g_strstrip(line)g_strchomp (g_strchug (line));
1660 | if (line[0] == '\0' || line[0] == '#')
1661 | return -1;
1662 |
1663 | if ((cp = strchr(line, '#'))) {
1664 | *cp = '\0';
1665 | g_strchomp(line);
1666 | }
1667 |
1668 | if ((cp = strtok(line, " \t")) == NULL((void*)0))
1669 | return -1;
1670 |
1671 | /* First try to match the common format for the large ethers file. */
1672 | if (!parse_ether_address_fast((const uint8_t*)cp, eth, mask, accept_mask)) {
1673 | /* Fallback for the well-known addresses (wka) file. */
1674 | if (!parse_ether_address(cp, eth, mask, accept_mask))
1675 | return -1;
1676 | }
1677 |
1678 | if ((cp = strtok(NULL((void*)0), " \t")) == NULL((void*)0))
1679 | return -1;
1680 |
1681 | (void) g_strlcpy(eth->name, cp, MAXNAMELEN64);
1682 |
1683 | if ((cp = strtok(NULL((void*)0), "\t")) != NULL((void*)0))
1684 | {
1685 | (void) g_strlcpy(eth->longname, cp, MAXNAMELEN64);
1686 | } else {
1687 | /* Make the long name the short name */
1688 | (void) g_strlcpy(eth->longname, eth->name, MAXNAMELEN64);
1689 | }
1690 |
1691 | return 0;
1692 |
1693 | } /* parse_ether_line */
1694 |
1695 | static FILE *eth_p;
1696 |
1697 | static void
1698 | set_ethent(char *path)
1699 | {
1700 | if (eth_p)
1701 | rewind(eth_p);
1702 | else
1703 | eth_p = ws_fopenfopen(path, "r");
1704 | }
1705 |
1706 | static void
1707 | end_ethent(void)
1708 | {
1709 | if (eth_p) {
1710 | fclose(eth_p);
1711 | eth_p = NULL((void*)0);
1712 | }
1713 | }
1714 |
1715 | static ether_t *
1716 | get_ethent(unsigned int *mask, const bool_Bool accept_mask)
1717 | {
1718 |
1719 | static ether_t eth;
1720 | char buf[MAX_LINELEN1024];
1721 |
1722 | if (eth_p == NULL((void*)0))
1723 | return NULL((void*)0);
1724 |
1725 | while (fgetline(buf, sizeof(buf), eth_p) >= 0) {
1726 | if (parse_ether_line(buf, &eth, mask, accept_mask) == 0) {
1727 | return &eth;
1728 | }
1729 | }
1730 |
1731 | return NULL((void*)0);
1732 |
1733 | } /* get_ethent */
1734 |
1735 | static hashmanuf_t *
1736 | manuf_hash_new_entry(const uint8_t *addr, const char* name, const char* longname)
1737 | {
1738 | unsigned manuf_key;
1739 | hashmanuf_t *manuf_value;
1740 | char *endp;
1741 |
1742 | /* manuf needs only the 3 most significant octets of the ethernet address */
1743 | manuf_key = (addr[0] << 16) + (addr[1] << 8) + addr[2];
1744 | manuf_value = wmem_new(addr_resolv_scope, hashmanuf_t)((hashmanuf_t*)wmem_alloc((addr_resolv_scope), sizeof(hashmanuf_t )));
1745 |
1746 | memcpy(manuf_value->addr, addr, 3);
1747 | if (name != NULL((void*)0)) {
1748 | (void) g_strlcpy(manuf_value->resolved_name, name, MAXNAMELEN64);
1749 | manuf_value->flags = NAME_RESOLVED(1U<<1);
1750 | if (longname != NULL((void*)0)) {
1751 | (void) g_strlcpy(manuf_value->resolved_longname, longname, MAXNAMELEN64);
1752 | }
1753 | else {
1754 | (void) g_strlcpy(manuf_value->resolved_longname, name, MAXNAMELEN64);
1755 | }
1756 | }
1757 | else {
1758 | manuf_value->flags = 0;
1759 | manuf_value->resolved_name[0] = '\0';
1760 | manuf_value->resolved_longname[0] = '\0';
1761 | }
1762 | /* Values returned by bytes_to_hexstr_punct() are *not* null-terminated */
1763 | endp = bytes_to_hexstr_punct(manuf_value->hexaddr, addr, sizeof(manuf_value->addr), ':');
1764 | *endp = '\0';
1765 |
1766 | wmem_map_insert(manuf_hashtable, GUINT_TO_POINTER(manuf_key)((gpointer) (gulong) (manuf_key)), manuf_value);
1767 | return manuf_value;
1768 | }
1769 |
1770 | static hashwka_t*
1771 | wka_hash_new_entry(const uint8_t *addr, char* name)
1772 | {
1773 | uint8_t *wka_key;
1774 | hashwka_t *wka_value;
1775 |
1776 | wka_key = (uint8_t *)wmem_alloc(addr_resolv_scope, 6);
1777 | memcpy(wka_key, addr, 6);
1778 |
1779 | wka_value = (hashwka_t*)wmem_new(addr_resolv_scope, hashwka_t)((hashwka_t*)wmem_alloc((addr_resolv_scope), sizeof(hashwka_t )));
1780 | wka_value->flags = NAME_RESOLVED(1U<<1);
1781 | wka_value->name = wmem_strdup(addr_resolv_scope, name);
1782 |
1783 | wmem_map_insert(wka_hashtable, wka_key, wka_value);
1784 | return wka_value;
1785 | }
1786 |
1787 | static void
1788 | add_manuf_name(const uint8_t *addr, unsigned int mask, char *name, char *longname)
1789 | {
1790 | switch (mask)
1791 | {
1792 | case 0:
1793 | {
1794 | /* This is a manufacturer ID; add it to the manufacturer ID hash table */
1795 | hashmanuf_t *entry = manuf_hash_new_entry(addr, name, longname);
1796 | entry->flags |= STATIC_HOSTNAME(1U<<3);
1797 | break;
1798 | }
1799 | case 48:
1800 | {
1801 | /* This is a well-known MAC address; add it to the Ethernet hash table */
1802 | add_eth_name(addr, name, true1);
1803 | break;
1804 | }
1805 | default:
1806 | {
1807 | /* This is a range of well-known addresses; add it to the well-known-address table */
1808 | hashwka_t *entry = wka_hash_new_entry(addr, name);
1809 | entry->flags |= STATIC_HOSTNAME(1U<<3);
1810 | break;
1811 | }
1812 | }
1813 | } /* add_manuf_name */
1814 |
1815 | /* XXX: manuf_name_lookup returns a hashmanuf_t*, which cannot hold a 28 or
1816 | * 36 bit MA-M or MA-S. So it returns those as unresolved. For EUI-48 and
1817 | * EUI-64, MA-M and MA-S should be checked for separately in the global
1818 | * tables.
1819 | *
1820 | * XXX - size_t is used only in a ws_return_val_if() that checks
1821 | * whether the argument has at least 3 bytes; that's done only if
1822 | * assertions are enabled, so it's used only if assertions are
1823 | * enabled. This means that, if assertions aren't enabled, a
1824 | * warning that the argument is unused will be issued by at least
1825 | * some compilers, so we mark it as unused. Should we do that
1826 | * check unconditionally, and just emit a warning if assertions
1827 | * are enabled?
1828 | */
1829 | static hashmanuf_t *
1830 | manuf_name_lookup(const uint8_t *addr, size_t size _U___attribute__((unused)))
1831 | {
1832 | uint32_t manuf_key;
1833 | uint8_t oct;
1834 | hashmanuf_t *manuf_value;
1835 |
1836 | ws_return_val_if(size < 3, NULL)do { if (1 && (size < 3)) { ws_log_full("InvalidArg" , LOG_LEVEL_WARNING, "epan/addr_resolv.c", 1836, __func__, "invalid argument: %s" , "size < 3"); return (((void*)0)); } } while (0);
1837 |
1838 | /* manuf needs only the 3 most significant octets of the ethernet address */
1839 | manuf_key = addr[0];
1840 | manuf_key = manuf_key<<8;
1841 | oct = addr[1];
1842 | manuf_key = manuf_key | oct;
1843 | manuf_key = manuf_key<<8;
1844 | oct = addr[2];
1845 | manuf_key = manuf_key | oct;
1846 |
1847 |
1848 | /* first try to find a "perfect match" */
1849 | manuf_value = (hashmanuf_t*)wmem_map_lookup(manuf_hashtable, GUINT_TO_POINTER(manuf_key)((gpointer) (gulong) (manuf_key)));
1850 | if (manuf_value != NULL((void*)0)) {
1851 | manuf_value->flags |= TRIED_RESOLVE_ADDRESS(1U<<0);
1852 | return manuf_value;
1853 | }
1854 |
1855 | /* Mask out the broadcast/multicast flag but not the locally
1856 | * administered flag as locally administered means: not assigned
1857 | * by the IEEE but the local administrator instead.
1858 | * 0x01 multicast / broadcast bit
1859 | * 0x02 locally administered bit */
1860 | if ((manuf_key & 0x00010000) != 0) {
1861 | manuf_key &= 0x00FEFFFF;
1862 | manuf_value = (hashmanuf_t*)wmem_map_lookup(manuf_hashtable, GUINT_TO_POINTER(manuf_key)((gpointer) (gulong) (manuf_key)));
1863 | if (manuf_value != NULL((void*)0)) {
1864 | manuf_value->flags |= TRIED_RESOLVE_ADDRESS(1U<<0);
1865 | return manuf_value;
1866 | }
1867 | }
1868 |
1869 | /* Try the global manuf tables. */
1870 | const char *short_name, *long_name;
1871 | /* We can't insert a 28 or 36 bit entry into the used hash table. */
1872 | short_name = ws_manuf_lookup_oui24(addr, &long_name);
1873 | if (short_name != NULL((void*)0)) {
1874 | /* Found it */
1875 | manuf_value = manuf_hash_new_entry(addr, short_name, long_name);
1876 | } else {
1877 | /* Add the address as a hex string */
1878 | manuf_value = manuf_hash_new_entry(addr, NULL((void*)0), NULL((void*)0));
1879 | }
1880 |
1881 | manuf_value->flags |= TRIED_RESOLVE_ADDRESS(1U<<0);
1882 | return manuf_value;
1883 |
1884 | } /* manuf_name_lookup */
1885 |
1886 | static char *
1887 | wka_name_lookup(const uint8_t *addr, const unsigned int mask)
1888 | {
1889 | uint8_t masked_addr[6];
1890 | unsigned num;
1891 | int i;
1892 | hashwka_t *value;
1893 |
1894 | if (wka_hashtable == NULL((void*)0)) {
1895 | return NULL((void*)0);
1896 | }
1897 | /* Get the part of the address covered by the mask. */
1898 | for (i = 0, num = mask; num >= 8; i++, num -= 8)
1899 | masked_addr[i] = addr[i]; /* copy octets entirely covered by the mask */
1900 | /* Mask out the first masked octet */
1901 | masked_addr[i] = addr[i] & (0xFF << (8 - num));
1902 | i++;
1903 | /* Zero out completely-masked-out octets */
1904 | for (; i < 6; i++)
1905 | masked_addr[i] = 0;
1906 |
1907 | value = (hashwka_t*)wmem_map_lookup(wka_hashtable, masked_addr);
1908 |
1909 | if (value) {
1910 | value->flags |= TRIED_RESOLVE_ADDRESS(1U<<0);
1911 | return value->name;
1912 | }
1913 |
1914 | return NULL((void*)0);
1915 |
1916 | } /* wka_name_lookup */
1917 |
1918 | unsigned get_hash_ether_status(hashether_t* ether)
1919 | {
1920 | return ether->flags;
1921 | }
1922 |
1923 | bool_Bool get_hash_ether_used(hashether_t* ether)
1924 | {
1925 | return ((ether->flags & TRIED_OR_RESOLVED_MASK((1U<<0) | (1U<<1))) == TRIED_OR_RESOLVED_MASK((1U<<0) | (1U<<1)));
1926 | }
1927 |
1928 | char* get_hash_ether_hexaddr(hashether_t* ether)
1929 | {
1930 | return ether->hexaddr;
1931 | }
1932 |
1933 | char* get_hash_ether_resolved_name(hashether_t* ether)
1934 | {
1935 | return ether->resolved_name;
1936 | }
1937 |
1938 | bool_Bool get_hash_wka_used(hashwka_t* wka)
1939 | {
1940 | return ((wka->flags & TRIED_OR_RESOLVED_MASK((1U<<0) | (1U<<1))) == TRIED_OR_RESOLVED_MASK((1U<<0) | (1U<<1)));
1941 | }
1942 |
1943 | char* get_hash_wka_resolved_name(hashwka_t* wka)
1944 | {
1945 | return wka->name;
1946 | }
1947 |
1948 | static unsigned
1949 | eth_addr_hash(const void *key)
1950 | {
1951 | return wmem_strong_hash((const uint8_t *)key, 6);
1952 | }
1953 |
1954 | static gboolean
1955 | eth_addr_cmp(const void *a, const void *b)
1956 | {
1957 | return (memcmp(a, b, 6) == 0);
1958 | }
1959 |
1960 | static unsigned
1961 | eui64_addr_hash(const void *key)
1962 | {
1963 | return wmem_strong_hash((const uint8_t *)key, EUI64_ADDR_LEN8);
1964 | }
1965 |
1966 | static gboolean
1967 | eui64_addr_cmp(const void *a, const void *b)
1968 | {
1969 | return (memcmp(a, b, EUI64_ADDR_LEN8) == 0);
1970 | }
1971 |
1972 | static void
1973 | initialize_ethers(const char* app_env_var_prefix)
1974 | {
1975 | ether_t *eth;
1976 | unsigned mask = 0;
1977 |
1978 | /* hash table initialization */
1979 | ws_assert(wka_hashtable == NULL)do { if ((1) && !(wka_hashtable == ((void*)0))) ws_log_fatal_full ("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 1979, __func__, "assertion failed: %s" , "wka_hashtable == ((void*)0)"); } while (0);
1980 | wka_hashtable = wmem_map_new(addr_resolv_scope, eth_addr_hash, eth_addr_cmp);
1981 | ws_assert(manuf_hashtable == NULL)do { if ((1) && !(manuf_hashtable == ((void*)0))) ws_log_fatal_full ("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 1981, __func__, "assertion failed: %s" , "manuf_hashtable == ((void*)0)"); } while (0);
1982 | manuf_hashtable = wmem_map_new(addr_resolv_scope, g_direct_hash, g_direct_equal);
1983 | ws_assert(eth_hashtable == NULL)do { if ((1) && !(eth_hashtable == ((void*)0))) ws_log_fatal_full ("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 1983, __func__, "assertion failed: %s" , "eth_hashtable == ((void*)0)"); } while (0);
1984 | eth_hashtable = wmem_map_new(addr_resolv_scope, eth_addr_hash, eth_addr_cmp);
1985 | ws_assert(eui64_hashtable == NULL)do { if ((1) && !(eui64_hashtable == ((void*)0))) ws_log_fatal_full ("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 1985, __func__, "assertion failed: %s" , "eui64_hashtable == ((void*)0)"); } while (0);
1986 | eui64_hashtable = wmem_map_new(addr_resolv_scope, eui64_addr_hash, eui64_addr_cmp);
1987 |
1988 | /* Compute the pathname of the ethers file. */
1989 | if (g_ethers_path == NULL((void*)0)) {
1990 | g_ethers_path = g_build_filename(get_systemfile_dir(app_env_var_prefix), ENAME_ETHERS"ethers", NULL((void*)0));
1991 | }
1992 |
1993 | /* Compute the pathname of the personal ethers file. */
1994 | if (g_pethers_path == NULL((void*)0)) {
1995 | /* Check profile directory before personal configuration */
1996 | g_pethers_path = get_persconffile_path(ENAME_ETHERS"ethers", true1, app_env_var_prefix);
1997 | if (!file_exists(g_pethers_path)) {
1998 | g_free(g_pethers_path);
1999 | g_pethers_path = get_persconffile_path(ENAME_ETHERS"ethers", false0, app_env_var_prefix);
2000 | }
2001 | }
2002 |
2003 | /* Compute the pathname of the global manuf file */
2004 | if (g_manuf_path == NULL((void*)0))
2005 | g_manuf_path = get_datafile_path(ENAME_MANUF"manuf", app_env_var_prefix);
2006 | /* Read it and initialize the hash table */
2007 | if (file_exists(g_manuf_path)) {
2008 | set_ethent(g_manuf_path);
2009 | while ((eth = get_ethent(&mask, true1))) {
2010 | add_manuf_name(eth->addr, mask, eth->name, eth->longname);
2011 | }
2012 | end_ethent();
2013 | }
2014 |
2015 | /* Compute the pathname of the personal manuf file */
2016 | if (g_pmanuf_path == NULL((void*)0)) {
2017 | /* Check profile directory before personal configuration */
2018 | g_pmanuf_path = get_persconffile_path(ENAME_MANUF"manuf", true1, app_env_var_prefix);
2019 | if (!file_exists(g_pmanuf_path)) {
2020 | g_free(g_pmanuf_path);
2021 | g_pmanuf_path = get_persconffile_path(ENAME_MANUF"manuf", false0, app_env_var_prefix);
2022 | }
2023 | }
2024 | /* Read it and initialize the hash table */
2025 | if (file_exists(g_pmanuf_path)) {
2026 | set_ethent(g_pmanuf_path);
2027 | while ((eth = get_ethent(&mask, true1))) {
2028 | add_manuf_name(eth->addr, mask, eth->name, eth->longname);
2029 | }
2030 | end_ethent();
2031 | }
2032 |
2033 | /* Compute the pathname of the wka file */
2034 | if (g_wka_path == NULL((void*)0))
2035 | g_wka_path = get_datafile_path(ENAME_WKA"wka", app_env_var_prefix);
2036 |
2037 | /* Read it and initialize the hash table */
2038 | set_ethent(g_wka_path);
2039 | while ((eth = get_ethent(&mask, true1))) {
2040 | add_manuf_name(eth->addr, mask, eth->name, eth->longname);
2041 | }
2042 | end_ethent();
2043 |
2044 | /* Look at the ethers files last. These are set as static names,
2045 | * so they override earlier entries, and the ones we read last
2046 | * take precedence. Order of precedence is personal ethers file,
2047 | * global ethers file, wka file, personal manuf file, global manuf
2048 | * file, and then non-static sources like ARP Eth -> IP hostname
2049 | * discovery (if enabled), NRB entries (if wiretap adds support for
2050 | * EUI-48 in NRBs), etc.
2051 | * XXX: What _is_ the proper order of precedence, and should it
2052 | * be configurable? (cf. #18075) */
2053 | set_ethent(g_ethers_path);
2054 | while ((eth = get_ethent(&mask, false0))) {
2055 | if (mask == 48) {
2056 | add_eth_name(eth->addr, eth->name, true1);
2057 | } else if (mask == 64) {
2058 | add_eui64_name(eth->addr, eth->name, true1);
2059 | }
2060 | }
2061 | end_ethent();
2062 |
2063 | if (file_exists(g_pethers_path)) {
2064 | set_ethent(g_pethers_path);
2065 | while ((eth = get_ethent(&mask, false0))) {
2066 | if (mask == 48) {
2067 | add_eth_name(eth->addr, eth->name, true1);
2068 | } else if (mask == 64) {
2069 | add_eui64_name(eth->addr, eth->name, true1);
2070 | }
2071 | }
2072 | end_ethent();
2073 | }
2074 |
2075 | } /* initialize_ethers */
2076 |
2077 | static void
2078 | ethers_cleanup(void)
2079 | {
2080 | wka_hashtable = NULL((void*)0);
2081 | manuf_hashtable = NULL((void*)0);
2082 | eth_hashtable = NULL((void*)0);
2083 | eui64_hashtable = NULL((void*)0);
2084 | g_free(g_ethers_path);
2085 | g_ethers_path = NULL((void*)0);
2086 | g_free(g_pethers_path);
2087 | g_pethers_path = NULL((void*)0);
2088 | g_free(g_manuf_path);
2089 | g_manuf_path = NULL((void*)0);
2090 | g_free(g_pmanuf_path);
2091 | g_pmanuf_path = NULL((void*)0);
2092 | g_free(g_wka_path);
2093 | g_wka_path = NULL((void*)0);
2094 | }
2095 |
2096 | static void
2097 | eth_resolved_name_fill(hashether_t *tp, const char *name, unsigned mask, const uint8_t *addr)
2098 | {
2099 | switch (mask) {
2100 | case 24:
2101 | snprintf(tp->resolved_name, MAXNAMELEN64, "%s_%02x:%02x:%02x",
2102 | name, addr[3], addr[4], addr[5]);
2103 | break;
2104 | case 28:
2105 | snprintf(tp->resolved_name, MAXNAMELEN64, "%s_%01x:%02x:%02x",
2106 | name, addr[3] & 0x0F, addr[4], addr[5]);
2107 | break;
2108 | case 36:
2109 | snprintf(tp->resolved_name, MAXNAMELEN64, "%s_%01x:%02x",
2110 | name, addr[4] & 0x0F, addr[5]);
2111 | break;
2112 | default: // Future-proof generic algorithm
2113 | {
2114 | unsigned bytes = mask / 8;
2115 | unsigned bitmask = mask % 8;
2116 |
2117 | int pos = snprintf(tp->resolved_name, MAXNAMELEN64, "%s", name);
2118 | if (pos >= MAXNAMELEN64) return;
2119 |
2120 | if (bytes < 6) {
2121 | pos += snprintf(tp->resolved_name + pos, MAXNAMELEN64 - pos,
2122 | bitmask >= 4 ? "_%01x" : "_%02x",
2123 | addr[bytes] & (0xFF >> bitmask));
2124 | bytes++;
2125 | }
2126 |
2127 | while (bytes < 6) {
2128 | if (pos >= MAXNAMELEN64) return;
2129 | pos += snprintf(tp->resolved_name + pos, MAXNAMELEN64 - pos, ":%02x",
2130 | addr[bytes]);
2131 | bytes++;
2132 | }
2133 | }
2134 | }
2135 | }
2136 |
2137 | /* Resolve ethernet address */
2138 | static hashether_t *
2139 | eth_addr_resolve(hashether_t *tp) {
2140 | hashmanuf_t *manuf_value;
2141 | const uint8_t *addr = tp->addr;
2142 | size_t addr_size = sizeof(tp->addr);
2143 |
2144 | if (!(tp->flags & NAME_RESOLVED(1U<<1))) {
2145 | unsigned mask;
2146 | char *name;
2147 | address ether_addr;
2148 |
2149 | /* Unknown name. Try looking for it in the well-known-address
2150 | tables for well-known address ranges smaller than 2^24. */
2151 | mask = 7;
2152 | do {
2153 | /* Only the topmost 5 bytes participate fully */
2154 | if ((name = wka_name_lookup(addr, mask+40)) != NULL((void*)0)) {
2155 | snprintf(tp->resolved_name, MAXNAMELEN64, "%s_%02x",
2156 | name, addr[5] & (0xFF >> mask));
2157 | tp->flags |= NAME_RESOLVED(1U<<1) | NAME_RESOLVED_PREFIX(1U<<4);
2158 | return tp;
2159 | }
2160 | } while (mask--);
2161 |
2162 | mask = 7;
2163 | do {
2164 | /* Only the topmost 4 bytes participate fully */
2165 | if ((name = wka_name_lookup(addr, mask+32)) != NULL((void*)0)) {
2166 | snprintf(tp->resolved_name, MAXNAMELEN64, "%s_%02x:%02x",
2167 | name, addr[4] & (0xFF >> mask), addr[5]);
2168 | tp->flags |= NAME_RESOLVED(1U<<1) | NAME_RESOLVED_PREFIX(1U<<4);
2169 | return tp;
2170 | }
2171 | } while (mask--);
2172 |
2173 | mask = 7;
2174 | do {
2175 | /* Only the topmost 3 bytes participate fully */
2176 | if ((name = wka_name_lookup(addr, mask+24)) != NULL((void*)0)) {
2177 | snprintf(tp->resolved_name, MAXNAMELEN64, "%s_%02x:%02x:%02x",
2178 | name, addr[3] & (0xFF >> mask), addr[4], addr[5]);
2179 | tp->flags |= NAME_RESOLVED(1U<<1) | NAME_RESOLVED_PREFIX(1U<<4);
2180 | return tp;
2181 | }
2182 | } while (mask--);
2183 |
2184 | /* Now try looking in the manufacturer table. */
2185 | manuf_value = manuf_name_lookup(addr, addr_size);
2186 | if ((manuf_value != NULL((void*)0)) && ((manuf_value->flags & NAME_RESOLVED(1U<<1)) == NAME_RESOLVED(1U<<1))) {
2187 | snprintf(tp->resolved_name, MAXNAMELEN64, "%.*s_%02x:%02x:%02x",
2188 | MAXNAMELEN64 - 10, manuf_value->resolved_name, addr[3], addr[4], addr[5]);
2189 | tp->flags |= NAME_RESOLVED(1U<<1) | NAME_RESOLVED_PREFIX(1U<<4);
2190 | return tp;
2191 | }
2192 |
2193 | /* Now try looking for it in the well-known-address
2194 | tables for well-known address ranges larger than 2^24. */
2195 | mask = 7;
2196 | do {
2197 | /* Only the topmost 2 bytes participate fully */
2198 | if ((name = wka_name_lookup(addr, mask+16)) != NULL((void*)0)) {
2199 | snprintf(tp->resolved_name, MAXNAMELEN64, "%s_%02x:%02x:%02x:%02x",
2200 | name, addr[2] & (0xFF >> mask), addr[3], addr[4],
2201 | addr[5]);
2202 | tp->flags |= NAME_RESOLVED(1U<<1) | NAME_RESOLVED_PREFIX(1U<<4);
2203 | return tp;
2204 | }
2205 | } while (mask--);
2206 |
2207 | mask = 7;
2208 | do {
2209 | /* Only the topmost byte participates fully */
2210 | if ((name = wka_name_lookup(addr, mask+8)) != NULL((void*)0)) {
2211 | snprintf(tp->resolved_name, MAXNAMELEN64, "%s_%02x:%02x:%02x:%02x:%02x",
2212 | name, addr[1] & (0xFF >> mask), addr[2], addr[3],
2213 | addr[4], addr[5]);
2214 | tp->flags |= NAME_RESOLVED(1U<<1) | NAME_RESOLVED_PREFIX(1U<<4);
2215 | return tp;
2216 | }
2217 | } while (mask--);
2218 |
2219 | mask = 7;
2220 | do {
2221 | /* Not even the topmost byte participates fully */
2222 | if ((name = wka_name_lookup(addr, mask)) != NULL((void*)0)) {
2223 | snprintf(tp->resolved_name, MAXNAMELEN64, "%s_%02x:%02x:%02x:%02x:%02x:%02x",
2224 | name, addr[0] & (0xFF >> mask), addr[1], addr[2],
2225 | addr[3], addr[4], addr[5]);
2226 | tp->flags |= NAME_RESOLVED(1U<<1) | NAME_RESOLVED_PREFIX(1U<<4);
2227 | return tp;
2228 | }
2229 | } while (--mask); /* Work down to the last bit */
2230 |
2231 | /* Now try looking in the global manuf data for a MA-M or MA-S
2232 | * match. We do this last so that the other files override this
2233 | * result.
2234 | */
2235 | const char *short_name, *long_name;
2236 | short_name = ws_manuf_lookup(addr, &long_name, &mask);
2237 | if (short_name != NULL((void*)0)) {
2238 | if (mask == 24) {
2239 | /* This shouldn't happen as it should be handled above,
2240 | * but it doesn't hurt.
2241 | */
2242 | manuf_hash_new_entry(addr, short_name, long_name);
2243 | }
2244 | eth_resolved_name_fill(tp, short_name, mask, addr);
2245 | tp->flags |= NAME_RESOLVED(1U<<1) | NAME_RESOLVED_PREFIX(1U<<4);
2246 | return tp;
2247 | }
2248 | /* No match whatsoever. */
2249 | set_address(&ether_addr, AT_ETHER, 6, addr);
2250 | address_to_str_buf(&ether_addr, tp->resolved_name, MAXNAMELEN64);
2251 | return tp;
2252 | }
2253 | return tp;
2254 | } /* eth_addr_resolve */
2255 |
2256 | static hashether_t *
2257 | eth_hash_new_entry(const uint8_t *addr, const bool_Bool resolve)
2258 | {
2259 | hashether_t *tp;
2260 | char *endp;
2261 |
2262 | tp = wmem_new(addr_resolv_scope, hashether_t)((hashether_t*)wmem_alloc((addr_resolv_scope), sizeof(hashether_t )));
2263 | memcpy(tp->addr, addr, sizeof(tp->addr));
2264 | tp->flags = 0;
2265 | /* Values returned by bytes_to_hexstr_punct() are *not* null-terminated */
2266 | endp = bytes_to_hexstr_punct(tp->hexaddr, addr, sizeof(tp->addr), ':');
2267 | *endp = '\0';
2268 | tp->resolved_name[0] = '\0';
2269 |
2270 | if (resolve)
2271 | eth_addr_resolve(tp);
2272 |
2273 | wmem_map_insert(eth_hashtable, tp->addr, tp);
2274 |
2275 | return tp;
2276 | } /* eth_hash_new_entry */
2277 |
2278 | static hashether_t *
2279 | add_eth_name(const uint8_t *addr, const char *name, bool_Bool static_entry)
2280 | {
2281 | hashether_t *tp;
2282 |
2283 | tp = (hashether_t *)wmem_map_lookup(eth_hashtable, addr);
2284 |
2285 | if (tp == NULL((void*)0)) {
2286 | tp = eth_hash_new_entry(addr, false0);
2287 | }
2288 |
2289 | if (strcmp(tp->resolved_name, name) != 0 && (static_entry || !(tp->flags & STATIC_HOSTNAME(1U<<3)))) {
2290 | (void) g_strlcpy(tp->resolved_name, name, MAXNAMELEN64);
2291 | tp->flags |= NAME_RESOLVED(1U<<1);
2292 | if (static_entry) {
2293 | tp->flags |= STATIC_HOSTNAME(1U<<3);
2294 | }
2295 | new_resolved_objects = true1;
2296 | }
2297 |
2298 | return tp;
2299 | } /* add_eth_name */
2300 |
2301 | static hashether_t *
2302 | eth_name_lookup(const uint8_t *addr, const bool_Bool resolve)
2303 | {
2304 | hashether_t *tp;
2305 |
2306 | tp = (hashether_t *)wmem_map_lookup(eth_hashtable, addr);
2307 |
2308 | if (tp == NULL((void*)0)) {
2309 | tp = eth_hash_new_entry(addr, resolve);
2310 | } else {
2311 | if (resolve && !(tp->flags & TRIED_OR_RESOLVED_MASK((1U<<0) | (1U<<1)))) {
2312 | eth_addr_resolve(tp); /* Found but needs to be resolved */
2313 | }
2314 | }
2315 | if (resolve) {
2316 | tp->flags |= TRIED_RESOLVE_ADDRESS(1U<<0);
2317 | }
2318 |
2319 | return tp;
2320 |
2321 | } /* eth_name_lookup */
2322 |
2323 | static void
2324 | eui64_resolved_name_fill(hasheui64_t *tp, const char *name, unsigned mask, const uint8_t *addr)
2325 | {
2326 | switch (mask) {
2327 | case 24:
2328 | snprintf(tp->resolved_name, MAXNAMELEN64, "%s_%02x:%02x:%02x:%02x:%02x",
2329 | name, addr[3], addr[4], addr[5], addr[6], addr[7]);
2330 | break;
2331 | case 28:
2332 | snprintf(tp->resolved_name, MAXNAMELEN64, "%s_%01x:%02x:%02x:%02x:%02x",
2333 | name, addr[3] & 0x0F, addr[4], addr[5], addr[6], addr[7]);
2334 | break;
2335 | case 36:
2336 | snprintf(tp->resolved_name, MAXNAMELEN64, "%s_%01x:%02x:%02x:%02x",
2337 | name, addr[4] & 0x0F, addr[5], addr[6], addr[7]);
2338 | break;
2339 | default: // Future-proof generic algorithm
2340 | {
2341 | unsigned bytes = mask / 8;
2342 | unsigned bitmask = mask % 8;
2343 |
2344 | int pos = snprintf(tp->resolved_name, MAXNAMELEN64, "%s", name);
2345 | if (pos >= MAXNAMELEN64) return;
2346 |
2347 | if (bytes < EUI64_ADDR_LEN8) {
2348 | pos += snprintf(tp->resolved_name + pos, MAXNAMELEN64 - pos,
2349 | bitmask >= 4 ? "_%01x" : "_%02x",
2350 | addr[bytes] & (0xFF >> bitmask));
2351 | bytes++;
2352 | }
2353 |
2354 | while (bytes < EUI64_ADDR_LEN8) {
2355 | if (pos >= MAXNAMELEN64) return;
2356 | pos += snprintf(tp->resolved_name + pos, MAXNAMELEN64 - pos, ":%02x",
2357 | addr[bytes]);
2358 | bytes++;
2359 | }
2360 | }
2361 | }
2362 | }
2363 |
2364 | /* Resolve EUI-64 address */
2365 | static hasheui64_t *
2366 | eui64_addr_resolve(hasheui64_t *tp)
2367 | {
2368 | hashmanuf_t *manuf_value;
2369 | const uint8_t *addr = tp->addr;
2370 | size_t addr_size = sizeof(tp->addr);
2371 |
2372 | if (!(tp->flags & NAME_RESOLVED(1U<<1))) {
2373 | unsigned mask;
2374 | address eui64_addr;
2375 | /* manuf_name_lookup returns a hashmanuf_t* that covers an entire /24,
2376 | * so we can't properly use it for MA-M and MA-S. We do want to check
2377 | * it first so it also covers the user-defined tables.
2378 | */
2379 | manuf_value = manuf_name_lookup(addr, addr_size);
2380 | if ((manuf_value != NULL((void*)0)) && ((manuf_value->flags & NAME_RESOLVED(1U<<1)) == NAME_RESOLVED(1U<<1))) {
2381 | snprintf(tp->resolved_name, MAXNAMELEN64, "%.*s_%02x:%02x:%02x:%02x:%02x",
2382 | MAXNAMELEN64 - 16, manuf_value->resolved_name, addr[3], addr[4], addr[5], addr[6], addr[7]);
2383 | tp->flags |= NAME_RESOLVED(1U<<1) | NAME_RESOLVED_PREFIX(1U<<4);
2384 | return tp;
2385 | }
2386 |
2387 | /* Now try looking in the global manuf data for a MA-M or MA-S
2388 | * match. We do this last so that the other files override this
2389 | * result.
2390 | */
2391 | const char *short_name, *long_name;
2392 | short_name = ws_manuf_lookup(addr, &long_name, &mask);
2393 | if (short_name != NULL((void*)0)) {
2394 | if (mask == 24) {
2395 | /* This shouldn't happen as it should be handled above,
2396 | * but it doesn't hurt.
2397 | */
2398 | manuf_hash_new_entry(addr, short_name, long_name);
2399 | }
2400 | eui64_resolved_name_fill(tp, short_name, mask, addr);
2401 | tp->flags |= NAME_RESOLVED(1U<<1) | NAME_RESOLVED_PREFIX(1U<<4);
2402 | return tp;
2403 | }
2404 | /* No match whatsoever. */
2405 | set_address(&eui64_addr, AT_EUI64, 8, addr);
2406 | address_to_str_buf(&eui64_addr, tp->resolved_name, MAXNAMELEN64);
2407 | return tp;
2408 | }
2409 |
2410 | return tp;
2411 | } /* eui64_addr_resolve */
2412 |
2413 | static hasheui64_t *
2414 | eui64_hash_new_entry(const uint8_t *addr, const bool_Bool resolve)
2415 | {
2416 | hasheui64_t *tp;
2417 | char *endp;
2418 |
2419 | tp = wmem_new(addr_resolv_scope, hasheui64_t)((hasheui64_t*)wmem_alloc((addr_resolv_scope), sizeof(hasheui64_t )));
2420 | memcpy(tp->addr, addr, sizeof(tp->addr));
2421 | tp->flags = 0;
2422 | /* Values returned by bytes_to_hexstr_punct() are *not* null-terminated */
2423 | endp = bytes_to_hexstr_punct(tp->hexaddr, addr, sizeof(tp->addr), ':');
2424 | *endp = '\0';
2425 | tp->resolved_name[0] = '\0';
2426 |
2427 | if (resolve)
2428 | eui64_addr_resolve(tp);
2429 |
2430 | wmem_map_insert(eui64_hashtable, tp->addr, tp);
2431 |
2432 | return tp;
2433 | } /* eui64_hash_new_entry */
2434 |
2435 | static hasheui64_t *
2436 | add_eui64_name(const uint8_t *addr, const char *name, bool_Bool static_entry)
2437 | {
2438 | hasheui64_t *tp;
2439 |
2440 | tp = (hasheui64_t *)wmem_map_lookup(eui64_hashtable, addr);
2441 |
2442 | if (tp == NULL((void*)0)) {
2443 | tp = eui64_hash_new_entry(addr, false0);
2444 | }
2445 |
2446 | if (strcmp(tp->resolved_name, name) != 0 && (static_entry || !(tp->flags & STATIC_HOSTNAME(1U<<3)))) {
2447 | (void) g_strlcpy(tp->resolved_name, name, MAXNAMELEN64);
2448 | tp->flags |= NAME_RESOLVED(1U<<1);
2449 | if (static_entry) {
2450 | tp->flags |= STATIC_HOSTNAME(1U<<3);
2451 | }
2452 | new_resolved_objects = true1;
2453 | }
2454 |
2455 | return tp;
2456 | } /* add_eui64_name */
2457 |
2458 | static hasheui64_t *
2459 | eui64_name_lookup(const uint8_t *addr, const bool_Bool resolve)
2460 | {
2461 | hasheui64_t *tp;
2462 |
2463 | tp = (hasheui64_t *)wmem_map_lookup(eui64_hashtable, addr);
2464 |
2465 | if (tp == NULL((void*)0)) {
2466 | tp = eui64_hash_new_entry(addr, resolve);
2467 | } else {
2468 | if (resolve && !(tp->flags & TRIED_OR_RESOLVED_MASK((1U<<0) | (1U<<1)))) {
2469 | eui64_addr_resolve(tp); /* Found but needs to be resolved */
2470 | }
2471 | }
2472 | if (resolve) {
2473 | tp->flags |= TRIED_RESOLVE_ADDRESS(1U<<0);
2474 | }
2475 |
2476 | return tp;
2477 |
2478 | } /* eui64_name_lookup */
2479 |
2480 | /* IPXNETS */
2481 | static int
2482 | parse_ipxnets_line(char *line, ipxnet_t *ipxnet)
2483 | {
2484 | /*
2485 | * We allow three address separators (':', '-', and '.'),
2486 | * as well as no separators
2487 | */
2488 |
2489 | char *cp;
2490 | uint32_t a, a0, a1, a2, a3;
2491 | bool_Bool found_single_number = false0;
2492 |
2493 | if ((cp = strchr(line, '#')))
2494 | *cp = '\0';
2495 |
2496 | if ((cp = strtok(line, " \t\n")) == NULL((void*)0))
2497 | return -1;
2498 |
2499 | /* Either fill a0,a1,a2,a3 and found_single_number is false,
2500 | * fill a and found_single_number is true,
2501 | * or return -1
2502 | */
2503 | if (sscanf(cp, "%x:%x:%x:%x", &a0, &a1, &a2, &a3) != 4) {
2504 | if (sscanf(cp, "%x-%x-%x-%x", &a0, &a1, &a2, &a3) != 4) {
2505 | if (sscanf(cp, "%x.%x.%x.%x", &a0, &a1, &a2, &a3) != 4) {
2506 | if (sscanf(cp, "%x", &a) == 1) {
2507 | found_single_number = true1;
2508 | }
2509 | else {
2510 | return -1;
2511 | }
2512 | }
2513 | }
2514 | }
2515 |
2516 | if ((cp = strtok(NULL((void*)0), " \t\n")) == NULL((void*)0))
2517 | return -1;
2518 |
2519 | if (found_single_number) {
2520 | ipxnet->addr = a;
2521 | }
2522 | else {
2523 | ipxnet->addr = (a0 << 24) | (a1 << 16) | (a2 << 8) | a3;
2524 | }
2525 |
2526 | (void) g_strlcpy(ipxnet->name, cp, MAXNAMELEN64);
2527 |
2528 | return 0;
2529 |
2530 | } /* parse_ipxnets_line */
2531 |
2532 | static FILE *ipxnet_p;
2533 |
2534 | static void
2535 | set_ipxnetent(char *path)
2536 | {
2537 | if (ipxnet_p)
8 | ← | Assuming 'ipxnet_p' is non-null | →
9 | ← | Taking true branch | →
2538 | rewind(ipxnet_p);
10 | ← | After calling 'rewind' reading 'errno' is required to find out if the call has failed | →
2539 | else
2540 | ipxnet_p = ws_fopenfopen(path, "r");
2541 | }
2542 |
2543 | static void
2544 | end_ipxnetent(void)
2545 | {
2546 | if (ipxnet_p) {
2547 | fclose(ipxnet_p);
2548 | ipxnet_p = NULL((void*)0);
2549 | }
2550 | }
2551 |
2552 | static ipxnet_t *
2553 | get_ipxnetent(void)
2554 | {
2555 |
2556 | static ipxnet_t ipxnet;
2557 | char buf[MAX_LINELEN1024];
2558 |
2559 | if (ipxnet_p
12.1 | 'ipxnet_p' is not equal to NULL
== NULL((void*)0))
13 | ← | Taking false branch | →
2560 | return NULL((void*)0);
2561 |
2562 | while (fgetline(buf, sizeof(buf), ipxnet_p) >= 0) {
14 | ← | Calling 'fgetline' | →
2563 | if (parse_ipxnets_line(buf, &ipxnet) == 0) {
2564 | return &ipxnet;
2565 | }
2566 | }
2567 |
2568 | return NULL((void*)0);
2569 |
2570 | } /* get_ipxnetent */
2571 |
2572 | static ipxnet_t *
2573 | get_ipxnetbyaddr(uint32_t addr)
2574 | {
2575 | ipxnet_t *ipxnet;
2576 |
2577 | set_ipxnetent(g_ipxnets_path);
7 | ← | Calling 'set_ipxnetent' | →
11 | ← | Returning from 'set_ipxnetent' | →
2578 |
2579 | while (((ipxnet = get_ipxnetent()) != NULL((void*)0)) && (addr != ipxnet->addr) ) ;
12 | ← | Calling 'get_ipxnetent' | →
2580 |
2581 | if (ipxnet == NULL((void*)0)) {
2582 | end_ipxnetent();
2583 |
2584 | set_ipxnetent(g_pipxnets_path);
2585 |
2586 | while (((ipxnet = get_ipxnetent()) != NULL((void*)0)) && (addr != ipxnet->addr) )
2587 | ;
2588 |
2589 | end_ipxnetent();
2590 | }
2591 |
2592 | return ipxnet;
2593 |
2594 | } /* get_ipxnetbyaddr */
2595 |
2596 | static void
2597 | initialize_ipxnets(const char* app_env_var_prefix)
2598 | {
2599 | /* Compute the pathname of the ipxnets file.
2600 | *
2601 | * XXX - is there a notion of an "ipxnets file" in any flavor of
2602 | * UNIX, or with any add-on Netware package for UNIX? If not,
2603 | * should the UNIX version of the ipxnets file be in the datafile
2604 | * directory as well?
2605 | */
2606 | if (g_ipxnets_path == NULL((void*)0)) {
2607 | g_ipxnets_path = wmem_strdup_printf(addr_resolv_scope, "%s" G_DIR_SEPARATOR_S"/" "%s",
2608 | get_systemfile_dir(app_env_var_prefix), ENAME_IPXNETS"ipxnets");
2609 | }
2610 |
2611 | /* Set g_pipxnets_path here, but don't actually do anything
2612 | * with it. It's used in get_ipxnetbyaddr().
2613 | */
2614 | if (g_pipxnets_path == NULL((void*)0)) {
2615 | /* Check profile directory before personal configuration */
2616 | g_pipxnets_path = get_persconffile_path(ENAME_IPXNETS"ipxnets", true1, app_env_var_prefix);
2617 | if (!file_exists(g_pipxnets_path)) {
2618 | g_free(g_pipxnets_path);
2619 | g_pipxnets_path = get_persconffile_path(ENAME_IPXNETS"ipxnets", false0, app_env_var_prefix);
2620 | }
2621 | }
2622 |
2623 | } /* initialize_ipxnets */
2624 |
2625 | static void
2626 | ipx_name_lookup_cleanup(void)
2627 | {
2628 | g_ipxnets_path = NULL((void*)0);
2629 | g_free(g_pipxnets_path);
2630 | g_pipxnets_path = NULL((void*)0);
2631 | }
2632 |
2633 | static char *
2634 | ipxnet_name_lookup(wmem_allocator_t *allocator, const unsigned addr)
2635 | {
2636 | hashipxnet_t *tp;
2637 | ipxnet_t *ipxnet;
2638 |
2639 | tp = (hashipxnet_t *)wmem_map_lookup(ipxnet_hash_table, GUINT_TO_POINTER(addr)((gpointer) (gulong) (addr)));
2640 | if (tp == NULL((void*)0)) {
4 | ← | Assuming 'tp' is equal to NULL | →
5 | ← | Taking true branch | →
2641 | tp = wmem_new(addr_resolv_scope, hashipxnet_t)((hashipxnet_t*)wmem_alloc((addr_resolv_scope), sizeof(hashipxnet_t )));
2642 | wmem_map_insert(ipxnet_hash_table, GUINT_TO_POINTER(addr)((gpointer) (gulong) (addr)), tp);
2643 | } else {
2644 | return wmem_strdup(allocator, tp->name);
2645 | }
2646 |
2647 | /* fill in a new entry */
2648 |
2649 | tp->addr = addr;
2650 |
2651 | if ( (ipxnet = get_ipxnetbyaddr(addr)) == NULL((void*)0)) {
6 | ← | Calling 'get_ipxnetbyaddr' | →
2652 | /* unknown name */
2653 | snprintf(tp->name, MAXNAMELEN64, "%X", addr);
2654 |
2655 | } else {
2656 | (void) g_strlcpy(tp->name, ipxnet->name, MAXNAMELEN64);
2657 | }
2658 |
2659 | return wmem_strdup(allocator, tp->name);
2660 |
2661 | } /* ipxnet_name_lookup */
2662 |
2663 | /* VLANS */
2664 | static int
2665 | parse_vlan_line(char *line, vlan_t *vlan)
2666 | {
2667 | char *cp;
2668 | uint16_t id;
2669 |
2670 | if ((cp = strchr(line, '#')))
2671 | *cp = '\0';
2672 |
2673 | if ((cp = strtok(line, " \t\n")) == NULL((void*)0))
2674 | return -1;
2675 |
2676 | if (sscanf(cp, "%" SCNu16"hu", &id) == 1) {
2677 | vlan->id = id;
2678 | }
2679 | else {
2680 | return -1;
2681 | }
2682 |
2683 | if ((cp = strtok(NULL((void*)0), "\t\n")) == NULL((void*)0))
2684 | return -1;
2685 |
2686 | (void) g_strlcpy(vlan->name, cp, MAXVLANNAMELEN128);
2687 |
2688 | return 0;
2689 |
2690 | } /* parse_vlan_line */
2691 |
2692 | static FILE *vlan_p;
2693 |
2694 | static void
2695 | set_vlanent(char *path)
2696 | {
2697 | if (vlan_p)
2698 | rewind(vlan_p);
2699 | else
2700 | vlan_p = ws_fopenfopen(path, "r");
2701 | }
2702 |
2703 | static void
2704 | end_vlanent(void)
2705 | {
2706 | if (vlan_p) {
2707 | fclose(vlan_p);
2708 | vlan_p = NULL((void*)0);
2709 | }
2710 | }
2711 |
2712 | static vlan_t *
2713 | get_vlanent(void)
2714 | {
2715 |
2716 | static vlan_t vlan;
2717 | char buf[MAX_LINELEN1024];
2718 |
2719 | if (vlan_p == NULL((void*)0))
2720 | return NULL((void*)0);
2721 |
2722 | while (fgetline(buf, sizeof(buf), vlan_p) >= 0) {
2723 | if (parse_vlan_line(buf, &vlan) == 0) {
2724 | return &vlan;
2725 | }
2726 | }
2727 |
2728 | return NULL((void*)0);
2729 |
2730 | } /* get_vlanent */
2731 |
2732 | static vlan_t *
2733 | get_vlannamebyid(uint16_t id)
2734 | {
2735 | vlan_t *vlan;
2736 |
2737 | set_vlanent(g_pvlan_path);
2738 |
2739 | while (((vlan = get_vlanent()) != NULL((void*)0)) && (id != vlan->id) ) ;
2740 |
2741 | if (vlan == NULL((void*)0)) {
2742 | end_vlanent();
2743 |
2744 | }
2745 |
2746 | return vlan;
2747 |
2748 | } /* get_vlannamebyid */
2749 |
2750 | static void
2751 | initialize_vlans(const char* app_env_var_prefix)
2752 | {
2753 | ws_assert(vlan_hash_table == NULL)do { if ((1) && !(vlan_hash_table == ((void*)0))) ws_log_fatal_full ("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 2753, __func__, "assertion failed: %s" , "vlan_hash_table == ((void*)0)"); } while (0);
2754 | vlan_hash_table = wmem_map_new(addr_resolv_scope, g_direct_hash, g_direct_equal);
2755 |
2756 | /* Set g_pvlan_path here, but don't actually do anything
2757 | * with it. It's used in get_vlannamebyid()
2758 | */
2759 | if (g_pvlan_path == NULL((void*)0)) {
2760 | /* Check profile directory before personal configuration */
2761 | g_pvlan_path = get_persconffile_path(ENAME_VLANS"vlans", true1, app_env_var_prefix);
2762 | if (!file_exists(g_pvlan_path)) {
2763 | g_free(g_pvlan_path);
2764 | g_pvlan_path = get_persconffile_path(ENAME_VLANS"vlans", false0, app_env_var_prefix);
2765 | }
2766 | }
2767 | } /* initialize_vlans */
2768 |
2769 | static void
2770 | vlan_name_lookup_cleanup(void)
2771 | {
2772 | end_vlanent();
2773 | vlan_hash_table = NULL((void*)0);
2774 | g_free(g_pvlan_path);
2775 | g_pvlan_path = NULL((void*)0);
2776 | }
2777 |
2778 | static const char *
2779 | vlan_name_lookup(const unsigned id)
2780 | {
2781 | hashvlan_t *tp;
2782 | vlan_t *vlan;
2783 |
2784 | tp = (hashvlan_t *)wmem_map_lookup(vlan_hash_table, GUINT_TO_POINTER(id)((gpointer) (gulong) (id)));
2785 | if (tp == NULL((void*)0)) {
2786 | tp = wmem_new(addr_resolv_scope, hashvlan_t)((hashvlan_t*)wmem_alloc((addr_resolv_scope), sizeof(hashvlan_t )));
2787 | wmem_map_insert(vlan_hash_table, GUINT_TO_POINTER(id)((gpointer) (gulong) (id)), tp);
2788 | } else {
2789 | return tp->name;
2790 | }
2791 |
2792 | /* fill in a new entry */
2793 |
2794 | tp->id = id;
2795 |
2796 | if ( (vlan = get_vlannamebyid(id)) == NULL((void*)0)) {
2797 | /* unknown name */
2798 | snprintf(tp->name, MAXVLANNAMELEN128, "<%u>", id);
2799 |
2800 | } else {
2801 | (void) g_strlcpy(tp->name, vlan->name, MAXVLANNAMELEN128);
2802 | }
2803 |
2804 | return tp->name;
2805 |
2806 | } /* vlan_name_lookup */
2807 | /* VLAN END */
2808 |
2809 | static bool_Bool
2810 | read_hosts_file (const char *hostspath, bool_Bool store_entries)
2811 | {
2812 | FILE *hf;
2813 | char line[MAX_LINELEN1024];
2814 | char *cp;
2815 | union {
2816 | uint32_t ip4_addr;
2817 | ws_in6_addr ip6_addr;
2818 | } host_addr;
2819 | bool_Bool is_ipv6, entry_found = false0;
2820 |
2821 | /*
2822 | * See the hosts(4) or hosts(5) man page for hosts file format
2823 | * (not available on all systems).
2824 | */
2825 | if ((hf = ws_fopenfopen(hostspath, "r")) == NULL((void*)0))
2826 | return false0;
2827 |
2828 | while (fgetline(line, sizeof(line), hf) >= 0) {
2829 | if ((cp = strchr(line, '#')))
2830 | *cp = '\0';
2831 |
2832 | if ((cp = strtok(line, " \t")) == NULL((void*)0))
2833 | continue; /* no tokens in the line */
2834 |
2835 | if (ws_inet_pton6(cp, &host_addr.ip6_addr)) {
2836 | /* Valid IPv6 */
2837 | is_ipv6 = true1;
2838 | } else if (ws_inet_pton4(cp, &host_addr.ip4_addr)) {
2839 | /* Valid IPv4 */
2840 | is_ipv6 = false0;
2841 | } else {
2842 | continue;
2843 | }
2844 |
2845 | if ((cp = strtok(NULL((void*)0), " \t")) == NULL((void*)0))
2846 | continue; /* no host name */
2847 |
2848 | entry_found = true1;
2849 | if (store_entries) {
2850 | if (is_ipv6) {
2851 | add_ipv6_name(&host_addr.ip6_addr, cp, true1);
2852 | } else {
2853 | add_ipv4_name(host_addr.ip4_addr, cp, true1);
2854 | }
2855 | }
2856 | }
2857 |
2858 | fclose(hf);
2859 | return entry_found ? true1 : false0;
2860 | } /* read_hosts_file */
2861 |
2862 | bool_Bool
2863 | add_hosts_file (const char *hosts_file)
2864 | {
2865 | bool_Bool found = false0;
2866 | unsigned i;
2867 |
2868 | if (!hosts_file)
2869 | return false0;
2870 |
2871 | if (!extra_hosts_files)
2872 | extra_hosts_files = g_ptr_array_new();
2873 |
2874 | for (i = 0; i < extra_hosts_files->len; i++) {
2875 | if (strcmp(hosts_file, (const char *) g_ptr_array_index(extra_hosts_files, i)((extra_hosts_files)->pdata)[i]) == 0)
2876 | found = true1;
2877 | }
2878 |
2879 | if (!found) {
2880 | g_ptr_array_add(extra_hosts_files, wmem_strdup(wmem_epan_scope(), hosts_file));
2881 | return read_hosts_file (hosts_file, false0);
2882 | }
2883 | return true1;
2884 | }
2885 |
2886 | bool_Bool
2887 | add_ip_name_from_string (const char *addr, const char *name)
2888 | {
2889 | union {
2890 | uint32_t ip4_addr;
2891 | ws_in6_addr ip6_addr;
2892 | } host_addr;
2893 | bool_Bool is_ipv6;
2894 | resolved_name_t *resolved_entry;
2895 |
2896 | if (ws_inet_pton6(addr, &host_addr.ip6_addr)) {
2897 | is_ipv6 = true1;
2898 | } else if (ws_inet_pton4(addr, &host_addr.ip4_addr)) {
2899 | is_ipv6 = false0;
2900 | } else {
2901 | return false0;
2902 | }
2903 |
2904 | if (is_ipv6) {
2905 | resolved_entry = (resolved_name_t*)wmem_map_lookup(manually_resolved_ipv6_list, &host_addr.ip6_addr);
2906 | if (resolved_entry)
2907 | {
2908 | // If we found a previous matching key (IP address), then just update the value (custom hostname);
2909 | (void) g_strlcpy(resolved_entry->name, name, MAXDNSNAMELEN256);
2910 | }
2911 | else
2912 | {
2913 | // Add a new mapping entry, if this IP address isn't already in the list.
2914 | ws_in6_addr* addr_key = wmem_new(wmem_epan_scope(), ws_in6_addr)((ws_in6_addr*)wmem_alloc((wmem_epan_scope()), sizeof(ws_in6_addr )));
2915 | memcpy(addr_key, &host_addr.ip6_addr, sizeof(ws_in6_addr));
2916 |
2917 | resolved_entry = wmem_new(wmem_epan_scope(), resolved_name_t)((resolved_name_t*)wmem_alloc((wmem_epan_scope()), sizeof(resolved_name_t )));
2918 | (void) g_strlcpy(resolved_entry->name, name, MAXDNSNAMELEN256);
2919 |
2920 | wmem_map_insert(manually_resolved_ipv6_list, addr_key, resolved_entry);
2921 | }
2922 | } else {
2923 | resolved_entry = (resolved_name_t*)wmem_map_lookup(manually_resolved_ipv4_list, GUINT_TO_POINTER(host_addr.ip4_addr)((gpointer) (gulong) (host_addr.ip4_addr)));
2924 | if (resolved_entry)
2925 | {
2926 | // If we found a previous matching key (IP address), then just update the value (custom hostname);
2927 | (void) g_strlcpy(resolved_entry->name, name, MAXDNSNAMELEN256);
2928 | }
2929 | else
2930 | {
2931 | // Add a new mapping entry, if this IP address isn't already in the list.
2932 | resolved_entry = wmem_new(wmem_epan_scope(), resolved_name_t)((resolved_name_t*)wmem_alloc((wmem_epan_scope()), sizeof(resolved_name_t )));
2933 | (void) g_strlcpy(resolved_entry->name, name, MAXDNSNAMELEN256);
2934 |
2935 | wmem_map_insert(manually_resolved_ipv4_list, GUINT_TO_POINTER(host_addr.ip4_addr)((gpointer) (gulong) (host_addr.ip4_addr)), resolved_entry);
2936 | }
2937 | }
2938 |
2939 | return true1;
2940 | } /* add_ip_name_from_string */
2941 |
2942 | extern resolved_name_t* get_edited_resolved_name(const char* addr)
2943 | {
2944 | uint32_t ip4_addr;
2945 | ws_in6_addr ip6_addr;
2946 | resolved_name_t* resolved_entry = NULL((void*)0);
2947 |
2948 | if (ws_inet_pton6(addr, &ip6_addr)) {
2949 | resolved_entry = (resolved_name_t*)wmem_map_lookup(manually_resolved_ipv6_list, &ip6_addr);
2950 | }
2951 | else if (ws_inet_pton4(addr, &ip4_addr)) {
2952 | resolved_entry = (resolved_name_t*)wmem_map_lookup(manually_resolved_ipv4_list, GUINT_TO_POINTER(ip4_addr)((gpointer) (gulong) (ip4_addr)));
2953 | }
2954 |
2955 | return resolved_entry;
2956 | }
2957 |
2958 | /*
2959 | * Add the resolved addresses that are in use to the list used to create the pcapng NRB
2960 | */
2961 | static void
2962 | ipv4_hash_table_resolved_to_list(void *key _U___attribute__((unused)), void *value, void *user_data)
2963 | {
2964 | addrinfo_lists_t *lists = (addrinfo_lists_t *)user_data;
2965 | hashipv4_t *ipv4_hash_table_entry = (hashipv4_t *)value;
2966 |
2967 | if ((ipv4_hash_table_entry->flags & USED_AND_RESOLVED_MASK((1U<<1) | (1U<<2))) == USED_AND_RESOLVED_MASK((1U<<1) | (1U<<2))) {
2968 | lists->ipv4_addr_list = g_list_prepend(lists->ipv4_addr_list, ipv4_hash_table_entry);
2969 | }
2970 | }
2971 |
2972 | /*
2973 | * Add the resolved addresses that are in use to the list used to create the pcapng NRB
2974 | */
2975 | static void
2976 | ipv6_hash_table_resolved_to_list(void *key _U___attribute__((unused)), void *value, void *user_data)
2977 | {
2978 | addrinfo_lists_t *lists = (addrinfo_lists_t *)user_data;
2979 | hashipv6_t *ipv6_hash_table_entry = (hashipv6_t *)value;
2980 |
2981 | if ((ipv6_hash_table_entry->flags & USED_AND_RESOLVED_MASK((1U<<1) | (1U<<2))) == USED_AND_RESOLVED_MASK((1U<<1) | (1U<<2))) {
2982 | lists->ipv6_addr_list = g_list_prepend(lists->ipv6_addr_list, ipv6_hash_table_entry);
2983 | }
2984 | }
2985 |
2986 | addrinfo_lists_t *
2987 | get_addrinfo_list(void)
2988 | {
2989 | if (ipv4_hash_table) {
2990 | wmem_map_foreach(ipv4_hash_table, ipv4_hash_table_resolved_to_list, &addrinfo_lists);
2991 | }
2992 |
2993 | if (ipv6_hash_table) {
2994 | wmem_map_foreach(ipv6_hash_table, ipv6_hash_table_resolved_to_list, &addrinfo_lists);
2995 | }
2996 |
2997 | return &addrinfo_lists;
2998 | }
2999 |
3000 | /* Read in a list of subnet definition - name pairs.
3001 | * <line> = <comment> | <entry> | <whitespace>
3002 | * <comment> = <whitespace>#<any>
3003 | * <entry> = <subnet_definition> <whitespace> <subnet_name> [<comment>|<whitespace><any>]
3004 | * <subnet_definition> = <ipv4_address> / <subnet_mask_length>
3005 | * <ipv4_address> is a full address; it will be masked to get the subnet-ID.
3006 | * <subnet_mask_length> is a decimal 1-31
3007 | * <subnet_name> is a string containing no whitespace.
3008 | * <whitespace> = (space | tab)+
3009 | * Any malformed entries are ignored.
3010 | * Any trailing data after the subnet_name is ignored.
3011 | *
3012 | * XXX Support IPv6
3013 | */
3014 | static bool_Bool
3015 | read_subnets_file (const char *subnetspath)
3016 | {
3017 | FILE *hf;
3018 | char line[MAX_LINELEN1024];
3019 | char *cp, *cp2;
3020 | uint32_t host_addr; /* IPv4 ONLY */
3021 | uint8_t mask_length;
3022 |
3023 | if ((hf = ws_fopenfopen(subnetspath, "r")) == NULL((void*)0))
3024 | return false0;
3025 |
3026 | while (fgetline(line, sizeof(line), hf) >= 0) {
3027 | if ((cp = strchr(line, '#')))
3028 | *cp = '\0';
3029 |
3030 | if ((cp = strtok(line, " \t")) == NULL((void*)0))
3031 | continue; /* no tokens in the line */
3032 |
3033 |
3034 | /* Expected format is <IP4 address>/<subnet length> */
3035 | cp2 = strchr(cp, '/');
3036 | if (NULL((void*)0) == cp2) {
3037 | /* No length */
3038 | continue;
3039 | }
3040 | *cp2 = '\0'; /* Cut token */
3041 | ++cp2 ;
3042 |
3043 | /* Check if this is a valid IPv4 address */
3044 | if (!str_to_ip(cp, &host_addr)) {
3045 | continue; /* no */
3046 | }
3047 |
3048 | if (!ws_strtou8(cp2, NULL((void*)0), &mask_length) || mask_length == 0 || mask_length > 32) {
3049 | continue; /* invalid mask length */
3050 | }
3051 |
3052 | if ((cp = strtok(NULL((void*)0), " \t")) == NULL((void*)0))
3053 | continue; /* no subnet name */
3054 |
3055 | subnet_entry_set(host_addr, mask_length, cp);
3056 | }
3057 |
3058 | fclose(hf);
3059 | return true1;
3060 | } /* read_subnets_file */
3061 |
3062 | static subnet_entry_t
3063 | subnet_lookup(const uint32_t addr)
3064 | {
3065 | subnet_entry_t subnet_entry;
3066 | uint32_t i;
3067 |
3068 | /* Search mask lengths linearly, longest first */
3069 |
3070 | i = SUBNETLENGTHSIZE32;
3071 | while(have_subnet_entry && i > 0) {
3072 | uint32_t masked_addr;
3073 | subnet_length_entry_t* length_entry;
3074 |
3075 | /* Note that we run from 31 (length 32) to 0 (length 1) */
3076 | --i;
3077 | ws_assert(i < SUBNETLENGTHSIZE)do { if ((1) && !(i < 32)) ws_log_fatal_full("", LOG_LEVEL_ERROR , "epan/addr_resolv.c", 3077, __func__, "assertion failed: %s" , "i < 32"); } while (0);
3078 |
3079 |
3080 | length_entry = &subnet_length_entries[i];
3081 |
3082 | if (NULL((void*)0) != length_entry->subnet_addresses) {
3083 | sub_net_hashipv4_t * tp;
3084 | uint32_t hash_idx;
3085 |
3086 | masked_addr = addr & length_entry->mask;
3087 | hash_idx = HASH_IPV4_ADDRESS(masked_addr)((((((guint32) ( (((guint32) (masked_addr) & (guint32) 0x000000ffU ) << 24) | (((guint32) (masked_addr) & (guint32) 0x0000ff00U ) << 8) | (((guint32) (masked_addr) & (guint32) 0x00ff0000U ) >> 8) | (((guint32) (masked_addr) & (guint32) 0xff000000U ) >> 24)))))) & (2048 - 1));
3088 |
3089 | tp = length_entry->subnet_addresses[hash_idx];
3090 | while(tp != NULL((void*)0) && tp->addr != masked_addr) {
3091 | tp = tp->next;
3092 | }
3093 |
3094 | if (NULL((void*)0) != tp) {
3095 | subnet_entry.mask = length_entry->mask;
3096 | subnet_entry.mask_length = i + 1; /* Length is offset + 1 */
3097 | subnet_entry.name = tp->name;
3098 | return subnet_entry;
3099 | }
3100 | }
3101 | }
3102 |
3103 | subnet_entry.mask = 0;
3104 | subnet_entry.mask_length = 0;
3105 | subnet_entry.name = NULL((void*)0);
3106 |
3107 | return subnet_entry;
3108 | }
3109 |
3110 | /* Add a subnet-definition - name pair to the set.
3111 | * The definition is taken by masking the address passed in with the mask of the
3112 | * given length.
3113 | */
3114 | static void
3115 | subnet_entry_set(uint32_t subnet_addr, const uint8_t mask_length, const char* name)
3116 | {
3117 | subnet_length_entry_t* entry;
3118 | sub_net_hashipv4_t * tp;
3119 | size_t hash_idx;
3120 |
3121 | ws_assert(mask_length > 0 && mask_length <= 32)do { if ((1) && !(mask_length > 0 && mask_length <= 32)) ws_log_fatal_full("", LOG_LEVEL_ERROR, "epan/addr_resolv.c" , 3121, __func__, "assertion failed: %s", "mask_length > 0 && mask_length <= 32" ); } while (0);
3122 |
3123 | entry = &subnet_length_entries[mask_length - 1];
3124 |
3125 | subnet_addr &= entry->mask;
3126 |
3127 | hash_idx = HASH_IPV4_ADDRESS(subnet_addr)((((((guint32) ( (((guint32) (subnet_addr) & (guint32) 0x000000ffU ) << 24) | (((guint32) (subnet_addr) & (guint32) 0x0000ff00U ) << 8) | (((guint32) (subnet_addr) & (guint32) 0x00ff0000U ) >> 8) | (((guint32) (subnet_addr) & (guint32) 0xff000000U ) >> 24)))))) & (2048 - 1));
3128 |
3129 | if (NULL((void*)0) == entry->subnet_addresses) {
3130 | entry->subnet_addresses = (sub_net_hashipv4_t**)wmem_alloc0(addr_resolv_scope, sizeof(sub_net_hashipv4_t*) * HASHHOSTSIZE2048);
3131 | }
3132 |
3133 | if (NULL((void*)0) != (tp = entry->subnet_addresses[hash_idx])) {
3134 | sub_net_hashipv4_t * new_tp;
3135 |
3136 | while (tp->next) {
3137 | if (tp->addr == subnet_addr) {
3138 | return; /* XXX provide warning that an address was repeated? */
3139 | } else {
3140 | tp = tp->next;
3141 | }
3142 | }
3143 |
3144 | new_tp = wmem_new(addr_resolv_scope, sub_net_hashipv4_t)((sub_net_hashipv4_t*)wmem_alloc((addr_resolv_scope), sizeof( sub_net_hashipv4_t)));
3145 | tp->next = new_tp;
3146 | tp = new_tp;
3147 | } else {
3148 | tp = entry->subnet_addresses[hash_idx] = wmem_new(addr_resolv_scope, sub_net_hashipv4_t)((sub_net_hashipv4_t*)wmem_alloc((addr_resolv_scope), sizeof( sub_net_hashipv4_t)));
3149 | }
3150 |
3151 | tp->next = NULL((void*)0);
3152 | tp->addr = subnet_addr;
3153 | (void) g_strlcpy(tp->name, name, MAXNAMELEN64); /* This is longer than subnet names can actually be */
3154 | have_subnet_entry = true1;
3155 | }
3156 |
3157 | static void
3158 | subnet_name_lookup_init(const char* app_env_var_prefix)
3159 | {
3160 | char* subnetspath;
3161 | uint32_t i;
3162 |
3163 | for(i = 0; i < SUBNETLENGTHSIZE32; ++i) {
3164 | uint32_t length = i + 1;
3165 |
3166 | subnet_length_entries[i].subnet_addresses = NULL((void*)0);
3167 | subnet_length_entries[i].mask_length = length;
3168 | subnet_length_entries[i].mask = g_htonl(ws_ipv4_get_subnet_mask(length))(((((guint32) ( (((guint32) (ws_ipv4_get_subnet_mask(length)) & (guint32) 0x000000ffU) << 24) | (((guint32) (ws_ipv4_get_subnet_mask (length)) & (guint32) 0x0000ff00U) << 8) | (((guint32 ) (ws_ipv4_get_subnet_mask(length)) & (guint32) 0x00ff0000U ) >> 8) | (((guint32) (ws_ipv4_get_subnet_mask(length)) & (guint32) 0xff000000U) >> 24))))));
3169 | }
3170 |
3171 | /* Check profile directory before personal configuration */
3172 | subnetspath = get_persconffile_path(ENAME_SUBNETS"subnets", true1, app_env_var_prefix);
3173 | if (!read_subnets_file(subnetspath)) {
3174 | if (errno(*__errno_location ()) != ENOENT2) {
3175 | report_open_failure(subnetspath, errno(*__errno_location ()), false0);
3176 | }
3177 |
3178 | g_free(subnetspath);
3179 | subnetspath = get_persconffile_path(ENAME_SUBNETS"subnets", false0, app_env_var_prefix);
3180 | if (!read_subnets_file(subnetspath) && errno(*__errno_location ()) != ENOENT2) {
3181 | report_open_failure(subnetspath, errno(*__errno_location ()), false0);
3182 | }
3183 | }
3184 | g_free(subnetspath);
3185 |
3186 | /*
3187 | * Load the global subnets file, if we have one.
3188 | */
3189 | subnetspath = get_datafile_path(ENAME_SUBNETS"subnets", app_env_var_prefix);
3190 | if (!read_subnets_file(subnetspath) && errno(*__errno_location ()) != ENOENT2) {
3191 | report_open_failure(subnetspath, errno(*__errno_location ()), false0);
3192 | }
3193 | g_free(subnetspath);
3194 | }
3195 |
3196 | /* SS7 PC Name Resolution Portion */
3197 | static hashss7pc_t *
3198 | new_ss7pc(const uint8_t ni, const uint32_t pc)
3199 | {
3200 | hashss7pc_t *tp = wmem_new(addr_resolv_scope, hashss7pc_t)((hashss7pc_t*)wmem_alloc((addr_resolv_scope), sizeof(hashss7pc_t )));
3201 | tp->id = (ni<<24) + (pc&0xffffff);
3202 | tp->pc_addr[0] = '\0';
3203 | tp->name[0] = '\0';
3204 |
3205 | return tp;
3206 | }
3207 |
3208 | static hashss7pc_t *
3209 | host_lookup_ss7pc(const uint8_t ni, const uint32_t pc)
3210 | {
3211 | hashss7pc_t * volatile tp;
3212 | uint32_t id;
3213 |
3214 | id = (ni<<24) + (pc&0xffffff);
3215 |
3216 | tp = (hashss7pc_t *)wmem_map_lookup(ss7pc_hash_table, GUINT_TO_POINTER(id)((gpointer) (gulong) (id)));
3217 | if (tp == NULL((void*)0)) {
3218 | tp = new_ss7pc(ni, pc);
3219 | wmem_map_insert(ss7pc_hash_table, GUINT_TO_POINTER(id)((gpointer) (gulong) (id)), tp);
3220 | }
3221 |
3222 | return tp;
3223 | }
3224 |
3225 | void fill_unresolved_ss7pc(const char * pc_addr, const uint8_t ni, const uint32_t pc)
3226 | {
3227 | hashss7pc_t *tp = host_lookup_ss7pc(ni, pc);
3228 |
3229 | (void) g_strlcpy(tp->pc_addr, pc_addr, MAXNAMELEN64);
3230 | }
3231 |
3232 | const char *
3233 | get_hostname_ss7pc(const uint8_t ni, const uint32_t pc)
3234 | {
3235 | hashss7pc_t *tp = host_lookup_ss7pc(ni, pc);
3236 |
3237 | /* never resolved yet*/
3238 | if (tp->pc_addr[0] == '\0')
3239 | return tp->pc_addr;
3240 |
3241 | /* Don't have name in file */
3242 | if (tp->name[0] == '\0')
3243 | return tp->pc_addr;
3244 |
3245 | if (!gbl_resolv_flags.ss7pc_name)
3246 | return tp->pc_addr;
3247 |
3248 | return tp->name;
3249 | }
3250 |
3251 | static void
3252 | add_ss7pc_name(const uint8_t ni, uint32_t pc, const char *name)
3253 | {
3254 | hashss7pc_t *tp;
3255 | uint32_t id;
3256 |
3257 | if (!name || name[0] == '\0')
3258 | return;
3259 |
3260 | id = (ni<<24) + (pc&0xffffff);
3261 | tp = (hashss7pc_t *)wmem_map_lookup(ss7pc_hash_table, GUINT_TO_POINTER(id)((gpointer) (gulong) (id)));
3262 | if (!tp) {
3263 | tp = new_ss7pc(ni, pc);
3264 | wmem_map_insert(ss7pc_hash_table, GUINT_TO_POINTER(id)((gpointer) (gulong) (id)), tp);
3265 | }
3266 |
3267 | if (g_ascii_strcasecmp(tp->name, name)) {
3268 | (void) g_strlcpy(tp->name, name, MAXNAMELEN64);
3269 | }
3270 | }
3271 |
3272 | static bool_Bool
3273 | read_ss7pcs_file(const char *ss7pcspath)
3274 | {
3275 | FILE *hf;
3276 | char line[MAX_LINELEN1024];
3277 | char *cp;
3278 | uint8_t ni;
3279 | uint32_t pc;
3280 | bool_Bool entry_found = false0;
3281 |
3282 | /*
3283 | * File format is Network Indicator (decimal)<dash>Point Code (Decimal)<tab/space>Hostname
3284 | */
3285 | if ((hf = ws_fopenfopen(ss7pcspath, "r")) == NULL((void*)0))
3286 | return false0;
3287 |
3288 | while (fgetline(line, sizeof(line), hf) >= 0) {
3289 | if ((cp = strchr(line, '#')))
3290 | *cp = '\0';
3291 |
3292 | if ((cp = strtok(line, "-")) == NULL((void*)0))
3293 | continue; /*no ni-pc separator*/
3294 | if (!ws_strtou8(cp, NULL((void*)0), &ni))
3295 | continue;
3296 | if (ni > 3)
3297 | continue;
3298 |
3299 | if ((cp = strtok(NULL((void*)0), " \t")) == NULL((void*)0))
3300 | continue; /* no tokens for pc and name */
3301 | if (!ws_strtou32(cp, NULL((void*)0), &pc))
3302 | continue;
3303 | if (pc >> 24 > 0)
3304 | continue;
3305 |
3306 | if ((cp = strtok(NULL((void*)0), " \t")) == NULL((void*)0))
3307 | continue; /* no host name */
3308 |
3309 | entry_found = true1;
3310 | add_ss7pc_name(ni, pc, cp);
3311 | }
3312 |
3313 | fclose(hf);
3314 | return entry_found ? true1 : false0;
3315 | }
3316 |
3317 | static void
3318 | ss7pc_name_lookup_init(const char* app_env_var_prefix)
3319 | {
3320 | char *ss7pcspath;
3321 |
3322 | ws_assert(ss7pc_hash_table == NULL)do { if ((1) && !(ss7pc_hash_table == ((void*)0))) ws_log_fatal_full ("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 3322, __func__, "assertion failed: %s" , "ss7pc_hash_table == ((void*)0)"); } while (0);
3323 |
3324 | ss7pc_hash_table = wmem_map_new(addr_resolv_scope, g_direct_hash, g_direct_equal);
3325 |
3326 | /*
3327 | * Load the user's ss7pcs file
3328 | */
3329 | ss7pcspath = get_persconffile_path(ENAME_SS7PCS"ss7pcs", true1, app_env_var_prefix);
3330 | if (!read_ss7pcs_file(ss7pcspath) && errno(*__errno_location ()) != ENOENT2) {
3331 | report_open_failure(ss7pcspath, errno(*__errno_location ()), false0);
3332 | }
3333 | g_free(ss7pcspath);
3334 | }
3335 |
3336 | /* SS7PC Name Resolution End*/
3337 |
3338 | /* TACS */
3339 | static bool_Bool
3340 | read_tacs_file(const char *tacspath)
3341 | {
3342 | FILE *hf;
3343 | char line[MAX_LINELEN1024];
3344 | char *cp;
3345 | uint16_t id;
3346 | wmem_strbuf_t *tac_name = NULL((void*)0);
3347 |
3348 | /*
3349 | * File format is TAC(decimal)<tab/space>TACName (no spaces)
3350 | */
3351 | if ((hf = ws_fopenfopen(tacspath, "r")) == NULL((void*)0))
3352 | return false0;
3353 |
3354 | while (fgetline(line, sizeof(line), hf) >= 0) {
3355 | if ((cp = strchr(line, '#')))
3356 | *cp = '\0';
3357 |
3358 | if ((cp = strtok(line, " \t")) == NULL((void*)0))
3359 | continue;
3360 |
3361 | if (sscanf(cp, "%" SCNu16"hu", &id) != 1) {
3362 | continue;
3363 | }
3364 |
3365 | if ((cp = strtok(NULL((void*)0), " \t\n")) == NULL((void*)0))
3366 | continue; /* no TAC name */
3367 |
3368 | if (!wmem_map_lookup(tac_hash_table, GUINT_TO_POINTER(id)((gpointer) (gulong) (id)))) {
3369 | tac_name = wmem_strbuf_new(addr_resolv_scope, cp);
3370 | wmem_map_insert(tac_hash_table, GUINT_TO_POINTER(id)((gpointer) (gulong) (id)), (void *)wmem_strbuf_get_str(tac_name));
3371 | }
3372 | }
3373 |
3374 | fclose(hf);
3375 | return true1;
3376 | }
3377 |
3378 | static void
3379 | initialize_tacs(const char* app_env_var_prefix)
3380 | {
3381 | char *tacspath;
3382 | ws_assert(tac_hash_table == NULL)do { if ((1) && !(tac_hash_table == ((void*)0))) ws_log_fatal_full ("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 3382, __func__, "assertion failed: %s" , "tac_hash_table == ((void*)0)"); } while (0);
3383 | tac_hash_table = wmem_map_new(addr_resolv_scope, g_direct_hash, g_direct_equal);
3384 |
3385 | tacspath = get_persconffile_path(ENAME_TACS"tacs", true1, app_env_var_prefix);
3386 | if (!read_tacs_file(tacspath) && errno(*__errno_location ()) != ENOENT2) {
3387 | report_open_failure(tacspath, errno(*__errno_location ()), false0);
3388 | }
3389 | g_free(tacspath);
3390 | }
3391 |
3392 | static void
3393 | tac_name_lookup_cleanup(void)
3394 | {
3395 | tac_hash_table = NULL((void*)0);
3396 | }
3397 |
3398 | const char *
3399 | tac_name_lookup(const unsigned id)
3400 | {
3401 | return (const char *)wmem_map_lookup(tac_hash_table, GUINT_TO_POINTER(id)((gpointer) (gulong) (id)));
3402 | }
3403 | /* TAC END */
3404 |
3405 | /*
3406 | * External Functions
3407 | */
3408 |
3409 | void
3410 | addr_resolve_pref_init(module_t *nameres)
3411 | {
3412 | prefs_register_bool_preference(nameres, "mac_name",
3413 | "Resolve MAC addresses",
3414 | "Resolve Ethernet MAC addresses to host names from the preferences"
3415 | " or system's Ethers file, or to a manufacturer based name.",
3416 | &gbl_resolv_flags.mac_name);
3417 |
3418 | prefs_register_bool_preference(nameres, "transport_name",
3419 | "Resolve transport names",
3420 | "Resolve TCP/UDP ports into service names",
3421 | &gbl_resolv_flags.transport_name);
3422 |
3423 | prefs_register_bool_preference(nameres, "network_name",
3424 | "Resolve network (IP) addresses",
3425 | "Resolve IPv4, IPv6, and IPX addresses into host names."
3426 | " The next set of check boxes determines how name resolution should be performed."
3427 | " If no other options are checked name resolution is made from Wireshark's host file"
3428 | " and capture file name resolution blocks.",
3429 | &gbl_resolv_flags.network_name);
3430 |
3431 | prefs_register_bool_preference(nameres, "dns_pkt_addr_resolution",
3432 | "Use captured DNS packet data for name resolution",
3433 | "Use address/name pairs found in captured DNS packets for name resolution.",
3434 | &gbl_resolv_flags.dns_pkt_addr_resolution);
3435 |
3436 | prefs_register_bool_preference(nameres, "handshake_sni_addr_resolution",
3437 | "Use SNI information from captured handshake packets",
3438 | "Use the Server Name Indication found in TLS handshakes for name resolution.",
3439 | &gbl_resolv_flags.handshake_sni_addr_resolution);
3440 |
3441 | prefs_register_bool_preference(nameres, "use_external_name_resolver",
3442 | "Use your system's DNS settings for name resolution",
3443 | "Use your system's configured name resolver"
3444 | " (usually DNS) to resolve network names."
3445 | " Only applies when network name resolution"
3446 | " is enabled.",
3447 | &gbl_resolv_flags.use_external_net_name_resolver);
3448 |
3449 | prefs_register_bool_preference(nameres, "use_custom_dns_servers",
3450 | "Use a custom list of DNS servers for name resolution",
3451 | "Use a DNS Servers list to resolve network names if true. If false, default information is used",
3452 | &use_custom_dns_server_list);
3453 |
3454 | static uat_field_t dns_server_uats_flds[] = {
3455 | UAT_FLD_CSTRING_OTHER(dnsserverlist_uats, ipaddr, "IP address", dnsserver_uat_fld_ip_chk_cb, "IPv4 or IPv6 address"){"ipaddr", "IP address", PT_TXTMOD_STRING,{ dnsserver_uat_fld_ip_chk_cb ,dnsserverlist_uats_ipaddr_set_cb,dnsserverlist_uats_ipaddr_tostr_cb },{0,0,0},0,"IPv4 or IPv6 address",((void*)0)},
3456 | UAT_FLD_CSTRING_OTHER(dnsserverlist_uats, tcp_port, "TCP Port", dnsserver_uat_fld_port_chk_cb, "Port Number (TCP)"){"tcp_port", "TCP Port", PT_TXTMOD_STRING,{ dnsserver_uat_fld_port_chk_cb ,dnsserverlist_uats_tcp_port_set_cb,dnsserverlist_uats_tcp_port_tostr_cb },{0,0,0},0,"Port Number (TCP)",((void*)0)},
3457 | UAT_FLD_CSTRING_OTHER(dnsserverlist_uats, udp_port, "UDP Port", dnsserver_uat_fld_port_chk_cb, "Port Number (UDP)"){"udp_port", "UDP Port", PT_TXTMOD_STRING,{ dnsserver_uat_fld_port_chk_cb ,dnsserverlist_uats_udp_port_set_cb,dnsserverlist_uats_udp_port_tostr_cb },{0,0,0},0,"Port Number (UDP)",((void*)0)},
3458 | UAT_END_FIELDS{((void*)0),((void*)0),PT_TXTMOD_NONE,{0,0,0},{0,0,0},0,0,((void *)0)}
3459 | };
3460 |
3461 | dnsserver_uat = uat_new("DNS Servers",
3462 | sizeof(struct dns_server_data),
3463 | "addr_resolve_dns_servers", /* filename */
3464 | true1, /* from_profile */
3465 | &dnsserverlist_uats, /* data_ptr */
3466 | &ndnsservers, /* numitems_ptr */
3467 | UAT_AFFECTS_DISSECTION0x00000001,
3468 | NULL((void*)0),
3469 | dns_server_copy_cb,
3470 | NULL((void*)0),
3471 | dns_server_free_cb,
3472 | c_ares_set_dns_servers,
3473 | NULL((void*)0),
3474 | dns_server_uats_flds);
3475 | static const char *dnsserver_uat_defaults[] = { NULL((void*)0), "53", "53" };
3476 | uat_set_default_values(dnsserver_uat, dnsserver_uat_defaults);
3477 | prefs_register_uat_preference(nameres, "dns_servers",
3478 | "DNS Servers",
3479 | "A table of IPv4 and IPv6 addresses of DNS servers to be used to resolve IP names and addresses",
3480 | dnsserver_uat);
3481 |
3482 | prefs_register_obsolete_preference(nameres, "concurrent_dns");
3483 |
3484 | prefs_register_uint_preference(nameres, "name_resolve_concurrency",
3485 | "Maximum concurrent requests",
3486 | "The maximum number of DNS requests that may"
3487 | " be active at any time. A large value (many"
3488 | " thousands) might overload the network or make"
3489 | " your DNS server behave badly.",
3490 | 10,
3491 | &name_resolve_concurrency);
3492 |
3493 | prefs_register_obsolete_preference(nameres, "hosts_file_handling");
3494 |
3495 | prefs_register_bool_preference(nameres, "vlan_name",
3496 | "Resolve VLAN IDs",
3497 | "Resolve VLAN IDs to network names from the preferences \"vlans\" file."
3498 | " Format of the file is: \"ID<Tab>Name\"."
3499 | " One line per VLAN, e.g.: 1 Management",
3500 | &gbl_resolv_flags.vlan_name);
3501 |
3502 | prefs_register_bool_preference(nameres, "ss7_pc_name",
3503 | "Resolve SS7 PCs",
3504 | "Resolve SS7 Point Codes to node names from the profiles \"ss7pcs\" file."
3505 | " Format of the file is: \"Network_Indicator<Dash>PC_Decimal<Tab>Name\"."
3506 | " One line per Point Code, e.g.: 2-1234 MyPointCode1",
3507 | &gbl_resolv_flags.ss7pc_name);
3508 |
3509 | prefs_register_bool_preference(nameres, "tac_name",
3510 | "Resolve TAC",
3511 | "Resolve TAC to area names from the preferences \"tac\" file."
3512 | " Format of the file is: \"TAC(decimail)<Tab/space>Name\"."
3513 | " One line per TAC, e.g.: 30123 City1",
3514 | &gbl_resolv_flags.tac_name);
3515 |
3516 | }
3517 |
3518 | void addr_resolve_pref_apply(void)
3519 | {
3520 | c_ares_set_dns_servers();
3521 | maxmind_db_pref_apply();
3522 | }
3523 |
3524 | void
3525 | disable_name_resolution(void) {
3526 | gbl_resolv_flags.mac_name = false0;
3527 | gbl_resolv_flags.network_name = false0;
3528 | gbl_resolv_flags.transport_name = false0;
3529 | gbl_resolv_flags.dns_pkt_addr_resolution = false0;
3530 | gbl_resolv_flags.handshake_sni_addr_resolution = false0;
3531 | gbl_resolv_flags.use_external_net_name_resolver = false0;
3532 | gbl_resolv_flags.vlan_name = false0;
3533 | gbl_resolv_flags.ss7pc_name = false0;
3534 | gbl_resolv_flags.maxmind_geoip = false0;
3535 | gbl_resolv_flags.tac_name = false0;
3536 | }
3537 |
3538 | bool_Bool
3539 | host_name_lookup_process(void) {
3540 | struct timeval tv = { 0, 0 };
3541 | int nfds;
3542 | fd_set rfds, wfds;
3543 | bool_Bool nro = new_resolved_objects;
3544 |
3545 | new_resolved_objects = false0;
3546 | nro |= maxmind_db_lookup_process();
3547 |
3548 | if (!async_dns_initialized)
3549 | /* c-ares not initialized. Bail out and cancel timers. */
3550 | return nro;
3551 |
3552 | process_async_dns_queue();
3553 |
3554 | FD_ZERO(&rfds)do { unsigned int __i; fd_set *__arr = (&rfds); for (__i = 0; __i < sizeof (fd_set) / sizeof (__fd_mask); ++__i) ((__arr )->__fds_bits)[__i] = 0; } while (0);
3555 | FD_ZERO(&wfds)do { unsigned int __i; fd_set *__arr = (&wfds); for (__i = 0; __i < sizeof (fd_set) / sizeof (__fd_mask); ++__i) ((__arr )->__fds_bits)[__i] = 0; } while (0);
3556 | nfds = ares_fds(ghba_chan, &rfds, &wfds);
3557 | if (nfds > 0) {
3558 | if (select(nfds, &rfds, &wfds, NULL((void*)0), &tv) == -1) { /* call to select() failed */
3559 | /* If it's interrupted by a signal, no need to put out a message */
3560 | if (errno(*__errno_location ()) != EINTR4)
3561 | fprintf(stderrstderr, "Warning: call to select() failed, error is %s\n", g_strerror(errno(*__errno_location ())));
3562 | return nro;
3563 | }
3564 | ares_process(ghba_chan, &rfds, &wfds);
3565 | }
3566 |
3567 | /* Any new entries? */
3568 | return nro;
3569 | }
3570 |
3571 | static void
3572 | _host_name_lookup_cleanup(void) {
3573 | async_dns_queue_head = NULL((void*)0);
3574 |
3575 | if (async_dns_initialized) {
3576 | ares_destroy(ghba_chan);
3577 | ares_destroy(ghbn_chan);
3578 | }
3579 | #ifdef CARES_HAVE_ARES_LIBRARY_INIT1
3580 | ares_library_cleanup();
3581 | #endif
3582 | async_dns_initialized = false0;
3583 | }
3584 |
3585 | const char *
3586 | get_hostname(const unsigned addr)
3587 | {
3588 | /* XXX why do we call this if we're not resolving? To create hash entries?
3589 | * Why? So that we can return a const char*?
3590 | *
3591 | * Note the returned string is in addr_resolv_scope, which has a similar
3592 | * life to the global file scope (slightly larger, in that the resolved
3593 | * addresses need to be available during dissector registration, e.g.
3594 | * for RADIUS and enterprises), so if not copied it is possible to use
3595 | * it after freeing.
3596 | *
3597 | * Should this be deprecated in favor of get_hostname_wmem so that
3598 | * host name lookups don't increase persistent memory usage even when
3599 | * hostname lookups are disabled? (An alternative would be to return
3600 | * NULL when lookups are disabled, but callers don't expect that.)
3601 | */
3602 | hashipv4_t *tp = host_lookup(addr);
3603 |
3604 | if (!gbl_resolv_flags.network_name)
3605 | return tp->ip;
3606 |
3607 | tp->flags |= RESOLVED_ADDRESS_USED(1U<<2);
3608 |
3609 | return tp->name;
3610 | }
3611 |
3612 | char *
3613 | get_hostname_wmem(wmem_allocator_t *allocator, const unsigned addr)
3614 | {
3615 | if (!gbl_resolv_flags.network_name)
3616 | return ip_addr_to_str(allocator, &addr);
3617 |
3618 | hashipv4_t *tp = host_lookup(addr);
3619 |
3620 | tp->flags |= RESOLVED_ADDRESS_USED(1U<<2);
3621 |
3622 | return wmem_strdup(allocator, tp->name);
3623 | }
3624 | /* -------------------------- */
3625 |
3626 | const char *
3627 | get_hostname6(const ws_in6_addr *addr)
3628 | {
3629 | /* XXX why do we call this if we're not resolving? To create hash entries?
3630 | * Why? The same comments as get_hostname above apply.
3631 | */
3632 | hashipv6_t *tp = host_lookup6(addr);
3633 |
3634 | if (!gbl_resolv_flags.network_name)
3635 | return tp->ip6;
3636 |
3637 | tp->flags |= RESOLVED_ADDRESS_USED(1U<<2);
3638 |
3639 | return tp->name;
3640 | }
3641 |
3642 | char *
3643 | get_hostname6_wmem(wmem_allocator_t *allocator, const ws_in6_addr *addr)
3644 | {
3645 | if (!gbl_resolv_flags.network_name)
3646 | return ip6_to_str(allocator, addr);
3647 |
3648 | hashipv6_t *tp = host_lookup6(addr);
3649 |
3650 | tp->flags |= RESOLVED_ADDRESS_USED(1U<<2);
3651 |
3652 | return wmem_strdup(allocator, tp->name);
3653 | }
3654 | /* -------------------------- */
3655 | void
3656 | add_ipv4_name(const unsigned addr, const char *name, bool_Bool static_entry)
3657 | {
3658 | hashipv4_t *tp;
3659 |
3660 | /*
3661 | * Don't add zero-length names; apparently, some resolvers will return
3662 | * them if they get them from DNS.
3663 | */
3664 | if (!name || name[0] == '\0')
3665 | return;
3666 |
3667 | tp = (hashipv4_t *)wmem_map_lookup(ipv4_hash_table, GUINT_TO_POINTER(addr)((gpointer) (gulong) (addr)));
3668 | if (!tp) {
3669 | tp = new_ipv4(addr);
3670 | wmem_map_insert(ipv4_hash_table, GUINT_TO_POINTER(addr)((gpointer) (gulong) (addr)), tp);
3671 | }
3672 |
3673 | if (g_ascii_strcasecmp(tp->name, name) && (static_entry || !(tp->flags & STATIC_HOSTNAME(1U<<3)))) {
3674 | (void) g_strlcpy(tp->name, name, MAXDNSNAMELEN256);
3675 | new_resolved_objects = true1;
3676 | if (static_entry)
3677 | tp->flags |= STATIC_HOSTNAME(1U<<3);
3678 | }
3679 | tp->flags |= TRIED_RESOLVE_ADDRESS(1U<<0)|NAME_RESOLVED(1U<<1);
3680 | } /* add_ipv4_name */
3681 |
3682 | /* -------------------------- */
3683 | void
3684 | add_ipv6_name(const ws_in6_addr *addrp, const char *name, const bool_Bool static_entry)
3685 | {
3686 | hashipv6_t *tp;
3687 |
3688 | /*
3689 | * Don't add zero-length names; apparently, some resolvers will return
3690 | * them if they get them from DNS.
3691 | */
3692 | if (!name || name[0] == '\0')
3693 | return;
3694 |
3695 | tp = (hashipv6_t *)wmem_map_lookup(ipv6_hash_table, addrp);
3696 | if (!tp) {
3697 | ws_in6_addr *addr_key;
3698 |
3699 | addr_key = wmem_new(addr_resolv_scope, ws_in6_addr)((ws_in6_addr*)wmem_alloc((addr_resolv_scope), sizeof(ws_in6_addr )));
3700 | tp = new_ipv6(addrp);
3701 | memcpy(addr_key, addrp, 16);
3702 | wmem_map_insert(ipv6_hash_table, addr_key, tp);
3703 | }
3704 |
3705 | if (g_ascii_strcasecmp(tp->name, name) && (static_entry || !(tp->flags & STATIC_HOSTNAME(1U<<3)))) {
3706 | (void) g_strlcpy(tp->name, name, MAXDNSNAMELEN256);
3707 | new_resolved_objects = true1;
3708 | if (static_entry)
3709 | tp->flags |= STATIC_HOSTNAME(1U<<3);
3710 | }
3711 | tp->flags |= TRIED_RESOLVE_ADDRESS(1U<<0)|NAME_RESOLVED(1U<<1);
3712 | } /* add_ipv6_name */
3713 |
3714 | static void
3715 | add_manually_resolved_ipv4(void *key, void *value, void *user_data _U___attribute__((unused)))
3716 | {
3717 | resolved_name_t *resolved_ipv4_entry = (resolved_name_t*)value;
3718 | add_ipv4_name(GPOINTER_TO_UINT(key)((guint) (gulong) (key)), resolved_ipv4_entry->name, true1);
3719 | }
3720 |
3721 | static void
3722 | add_manually_resolved_ipv6(void *key, void *value, void *user_data _U___attribute__((unused)))
3723 | {
3724 | resolved_name_t *resolved_ipv6_entry = (resolved_name_t*)value;
3725 | add_ipv6_name((ws_in6_addr*)key, resolved_ipv6_entry->name, true1);
3726 | }
3727 |
3728 | static void
3729 | add_manually_resolved(void)
3730 | {
3731 | if (manually_resolved_ipv4_list) {
3732 | wmem_map_foreach(manually_resolved_ipv4_list, add_manually_resolved_ipv4, NULL((void*)0));
3733 | }
3734 |
3735 | if (manually_resolved_ipv6_list) {
3736 | wmem_map_foreach(manually_resolved_ipv6_list, add_manually_resolved_ipv6, NULL((void*)0));
3737 | }
3738 | }
3739 |
3740 | static void
3741 | host_name_lookup_init(const char* app_env_var_prefix)
3742 | {
3743 | char *hostspath;
3744 | unsigned i;
3745 |
3746 | ws_assert(ipxnet_hash_table == NULL)do { if ((1) && !(ipxnet_hash_table == ((void*)0))) ws_log_fatal_full ("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 3746, __func__, "assertion failed: %s" , "ipxnet_hash_table == ((void*)0)"); } while (0);
3747 | ipxnet_hash_table = wmem_map_new(addr_resolv_scope, g_direct_hash, g_direct_equal);
3748 |
3749 | ws_assert(ipv4_hash_table == NULL)do { if ((1) && !(ipv4_hash_table == ((void*)0))) ws_log_fatal_full ("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 3749, __func__, "assertion failed: %s" , "ipv4_hash_table == ((void*)0)"); } while (0);
3750 | ipv4_hash_table = wmem_map_new(addr_resolv_scope, g_direct_hash, g_direct_equal);
3751 |
3752 | ws_assert(ipv6_hash_table == NULL)do { if ((1) && !(ipv6_hash_table == ((void*)0))) ws_log_fatal_full ("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 3752, __func__, "assertion failed: %s" , "ipv6_hash_table == ((void*)0)"); } while (0);
3753 | ipv6_hash_table = wmem_map_new(addr_resolv_scope, ipv6_oat_hash, ipv6_equal);
3754 |
3755 | ws_assert(async_dns_queue_head == NULL)do { if ((1) && !(async_dns_queue_head == ((void*)0)) ) ws_log_fatal_full("", LOG_LEVEL_ERROR, "epan/addr_resolv.c" , 3755, __func__, "assertion failed: %s", "async_dns_queue_head == ((void*)0)" ); } while (0);
3756 | async_dns_queue_head = wmem_list_new(addr_resolv_scope);
3757 |
3758 | /*
3759 | * The manually resolved lists are the only address resolution maps
3760 | * that are not reset by addr_resolv_cleanup(), because they are
3761 | * the only ones that do not have entries from personal configuration
3762 | * files that can change when changing configurations. All their
3763 | * entries must also be in epan scope.
3764 | */
3765 | if (manually_resolved_ipv4_list == NULL((void*)0))
3766 | manually_resolved_ipv4_list = wmem_map_new(wmem_epan_scope(), g_direct_hash, g_direct_equal);
3767 |
3768 | if (manually_resolved_ipv6_list == NULL((void*)0))
3769 | manually_resolved_ipv6_list = wmem_map_new(wmem_epan_scope(), ws_ipv6_hash, ipv6_equal);
3770 |
3771 | /*
3772 | * Load the global hosts file, if we have one.
3773 | */
3774 | hostspath = get_datafile_path(ENAME_HOSTS"hosts", app_env_var_prefix);
3775 | if (!read_hosts_file(hostspath, true1) && errno(*__errno_location ()) != ENOENT2) {
3776 | report_open_failure(hostspath, errno(*__errno_location ()), false0);
3777 | }
3778 | g_free(hostspath);
3779 | /*
3780 | * Load the user's hosts file no matter what, if they have one.
3781 | */
3782 | hostspath = get_persconffile_path(ENAME_HOSTS"hosts", true1, app_env_var_prefix);
3783 | if (!read_hosts_file(hostspath, true1) && errno(*__errno_location ()) != ENOENT2) {
3784 | report_open_failure(hostspath, errno(*__errno_location ()), false0);
3785 | }
3786 | g_free(hostspath);
3787 | #ifdef CARES_HAVE_ARES_LIBRARY_INIT1
3788 | if (ares_library_init(ARES_LIB_INIT_ALL((1 << 0))) == ARES_SUCCESS) {
3789 | #endif
3790 | /* XXX - Check which options we should set */
3791 | if (ares_init_options(&ghba_chan, NULL((void*)0), 0) == ARES_SUCCESS && ares_init_options(&ghbn_chan, NULL((void*)0), 0) == ARES_SUCCESS) {
3792 | async_dns_initialized = true1;
3793 | c_ares_set_dns_servers();
3794 | }
3795 | #ifdef CARES_HAVE_ARES_LIBRARY_INIT1
3796 | }
3797 | #endif
3798 |
3799 | if (extra_hosts_files) {
3800 | for (i = 0; i < extra_hosts_files->len; i++) {
3801 | read_hosts_file((const char *) g_ptr_array_index(extra_hosts_files, i)((extra_hosts_files)->pdata)[i], true1);
3802 | }
3803 | }
3804 |
3805 | subnet_name_lookup_init(app_env_var_prefix);
3806 |
3807 | add_manually_resolved();
3808 |
3809 | ss7pc_name_lookup_init(app_env_var_prefix);
3810 | }
3811 |
3812 | static void
3813 | host_name_lookup_cleanup(void)
3814 | {
3815 | uint32_t i, j;
3816 | sub_net_hashipv4_t *entry, *next_entry;
3817 |
3818 | _host_name_lookup_cleanup();
3819 |
3820 | ipxnet_hash_table = NULL((void*)0);
3821 | ipv4_hash_table = NULL((void*)0);
3822 | ipv6_hash_table = NULL((void*)0);
3823 | ss7pc_hash_table = NULL((void*)0);
3824 |
3825 | for(i = 0; i < SUBNETLENGTHSIZE32; ++i) {
3826 | if (subnet_length_entries[i].subnet_addresses != NULL((void*)0)) {
3827 | for (j = 0; j < HASHHOSTSIZE2048; j++) {
3828 | for (entry = subnet_length_entries[i].subnet_addresses[j];
3829 | entry != NULL((void*)0); entry = next_entry) {
3830 | next_entry = entry->next;
3831 | wmem_free(addr_resolv_scope, entry);
3832 | }
3833 | }
3834 | wmem_free(addr_resolv_scope, subnet_length_entries[i].subnet_addresses);
3835 | subnet_length_entries[i].subnet_addresses = NULL((void*)0);
3836 | }
3837 | }
3838 |
3839 | have_subnet_entry = false0;
3840 | new_resolved_objects = false0;
3841 | }
3842 |
3843 |
3844 | void host_name_lookup_reset(const char* app_env_var_prefix)
3845 | {
3846 | addr_resolv_cleanup();
3847 | addr_resolv_init(app_env_var_prefix);
3848 | }
3849 |
3850 | char *
3851 | udp_port_to_display(wmem_allocator_t *allocator, unsigned port)
3852 | {
3853 |
3854 | if (!gbl_resolv_flags.transport_name) {
3855 | return wmem_utoa(allocator, port);
3856 | }
3857 |
3858 | return wmem_strdup(allocator, serv_name_lookup(PT_UDP, port));
3859 |
3860 | } /* udp_port_to_display */
3861 |
3862 | char *
3863 | dccp_port_to_display(wmem_allocator_t *allocator, unsigned port)
3864 | {
3865 |
3866 | if (!gbl_resolv_flags.transport_name) {
3867 | return wmem_utoa(allocator, port);
3868 | }
3869 |
3870 | return wmem_strdup(allocator, serv_name_lookup(PT_DCCP, port));
3871 |
3872 | } /* dccp_port_to_display */
3873 |
3874 | char *
3875 | tcp_port_to_display(wmem_allocator_t *allocator, unsigned port)
3876 | {
3877 |
3878 | if (!gbl_resolv_flags.transport_name) {
3879 | return wmem_utoa(allocator, port);
3880 | }
3881 |
3882 | return wmem_strdup(allocator, serv_name_lookup(PT_TCP, port));
3883 |
3884 | } /* tcp_port_to_display */
3885 |
3886 | char *
3887 | sctp_port_to_display(wmem_allocator_t *allocator, unsigned port)
3888 | {
3889 |
3890 | if (!gbl_resolv_flags.transport_name) {
3891 | return wmem_utoa(allocator, port);
3892 | }
3893 |
3894 | return wmem_strdup(allocator, serv_name_lookup(PT_SCTP, port));
3895 |
3896 | } /* sctp_port_to_display */
3897 |
3898 | char *
3899 | port_with_resolution_to_str(wmem_allocator_t *scope, port_type proto, unsigned port)
3900 | {
3901 | const char *port_str;
3902 |
3903 | if (!gbl_resolv_flags.transport_name || (proto == PT_NONE)) {
3904 | /* No name resolution support, just return port string */
3905 | return wmem_strdup_printf(scope, "%u", port);
3906 | }
3907 | port_str = serv_name_lookup(proto, port);
3908 | ws_assert(port_str)do { if ((1) && !(port_str)) ws_log_fatal_full("", LOG_LEVEL_ERROR , "epan/addr_resolv.c", 3908, __func__, "assertion failed: %s" , "port_str"); } while (0);
3909 | return wmem_strdup_printf(scope, "%s (%u)", port_str, port);
3910 | }
3911 |
3912 | int
3913 | port_with_resolution_to_str_buf(char *buf, unsigned long buf_size, port_type proto, unsigned port)
3914 | {
3915 | const char *port_str;
3916 |
3917 | if (!gbl_resolv_flags.transport_name || (proto == PT_NONE)) {
3918 | /* No name resolution support, just return port string */
3919 | return snprintf(buf, buf_size, "%u", port);
3920 | }
3921 | port_str = serv_name_lookup(proto, port);
3922 | ws_assert(port_str)do { if ((1) && !(port_str)) ws_log_fatal_full("", LOG_LEVEL_ERROR , "epan/addr_resolv.c", 3922, __func__, "assertion failed: %s" , "port_str"); } while (0);
3923 | return snprintf(buf, buf_size, "%s (%u)", port_str, port);
3924 | }
3925 |
3926 | const char *
3927 | get_ether_name(const uint8_t *addr)
3928 | {
3929 | hashether_t *tp;
3930 | bool_Bool resolve = gbl_resolv_flags.mac_name;
3931 |
3932 | tp = eth_name_lookup(addr, resolve);
3933 |
3934 | return resolve ? tp->resolved_name : tp->hexaddr;
3935 |
3936 | } /* get_ether_name */
3937 |
3938 | const char *
3939 | tvb_get_ether_name(tvbuff_t *tvb, unsigned offset)
3940 | {
3941 | return get_ether_name(tvb_get_ptr(tvb, offset, 6));
3942 | }
3943 |
3944 | /* Look for a (non-dummy) ether name in the hash, and return it if found.
3945 | * If it's not found, simply return NULL.
3946 | */
3947 | const char *
3948 | get_ether_name_if_known(const uint8_t *addr)
3949 | {
3950 | hashether_t *tp;
3951 |
3952 | /* Initialize ether structs if we're the first
3953 | * ether-related function called */
3954 | if (!gbl_resolv_flags.mac_name)
3955 | return NULL((void*)0);
3956 |
3957 | /* eth_name_lookup will create a (resolved) hash entry
3958 | * if it doesn't exist, so it never returns NULL */
3959 | tp = eth_name_lookup(addr, true1);
3960 |
3961 | if ((tp->flags & (NAME_RESOLVED(1U<<1) | NAME_RESOLVED_PREFIX(1U<<4))) == NAME_RESOLVED(1U<<1)) {
3962 | /* Name is from an exact match, not a prefix/OUI */
3963 | return tp->resolved_name;
3964 | }
3965 | else {
3966 | /* Name was created */
3967 | return NULL((void*)0);
3968 | }
3969 | }
3970 |
3971 | void
3972 | add_ether_byip(const unsigned ip, const uint8_t *eth)
3973 | {
3974 | hashipv4_t *tp;
3975 |
3976 | /* first check that IP address can be resolved */
3977 | if (!gbl_resolv_flags.network_name)
3978 | return;
3979 |
3980 | tp = host_lookup(ip);
3981 |
3982 | /*
3983 | * Was this IP address resolved to a host name?
3984 | */
3985 | if (tp->flags & NAME_RESOLVED(1U<<1)) {
3986 | /*
3987 | * Yes, so add an entry in the ethers hashtable resolving
3988 | * the MAC address to that name.
3989 | */
3990 | add_eth_name(eth, tp->name, false0);
3991 | }
3992 |
3993 | } /* add_ether_byip */
3994 |
3995 | char *
3996 | get_ipxnet_name(wmem_allocator_t *allocator, const uint32_t addr)
3997 | {
3998 |
3999 | if (!gbl_resolv_flags.network_name) {
1 | Assuming field 'network_name' is true | →
2 | ← | Taking false branch | →
4000 | return ipxnet_to_str_punct(allocator, addr, '\0');
4001 | }
4002 |
4003 | return ipxnet_name_lookup(allocator, addr);
3 | ← | Calling 'ipxnet_name_lookup' | →
4004 |
4005 | } /* get_ipxnet_name */
4006 |
4007 | char *
4008 | get_vlan_name(wmem_allocator_t *allocator, const uint16_t id)
4009 | {
4010 |
4011 | if (!gbl_resolv_flags.vlan_name) {
4012 | return NULL((void*)0);
4013 | }
4014 |
4015 | return wmem_strdup(allocator, vlan_name_lookup(id));
4016 |
4017 | } /* get_vlan_name */
4018 |
4019 | const char *
4020 | get_manuf_name(const uint8_t *addr, size_t size)
4021 | {
4022 | hashmanuf_t *manuf_value;
4023 |
4024 | ws_return_val_if(size < 3, NULL)do { if (1 && (size < 3)) { ws_log_full("InvalidArg" , LOG_LEVEL_WARNING, "epan/addr_resolv.c", 4024, __func__, "invalid argument: %s" , "size < 3"); return (((void*)0)); } } while (0);
4025 |
4026 | manuf_value = manuf_name_lookup(addr, size);
4027 | if (gbl_resolv_flags.mac_name && ((manuf_value->flags & NAME_RESOLVED(1U<<1)) == NAME_RESOLVED(1U<<1)))
4028 | return manuf_value->resolved_name;
4029 |
4030 | return manuf_value->hexaddr;
4031 |
4032 | } /* get_manuf_name */
4033 |
4034 | const char *
4035 | tvb_get_manuf_name(tvbuff_t *tvb, unsigned offset)
4036 | {
4037 | uint8_t buf[3] = { 0 };
4038 | tvb_memcpy(tvb, buf, offset, 3);
4039 | return get_manuf_name(buf, sizeof(buf));
4040 | }
4041 |
4042 | const char *
4043 | get_manuf_name_if_known(const uint8_t *addr, size_t size)
4044 | {
4045 | hashmanuf_t *manuf_value;
4046 |
4047 | ws_return_val_if(size < 3, NULL)do { if (1 && (size < 3)) { ws_log_full("InvalidArg" , LOG_LEVEL_WARNING, "epan/addr_resolv.c", 4047, __func__, "invalid argument: %s" , "size < 3"); return (((void*)0)); } } while (0);
4048 |
4049 | manuf_value = manuf_name_lookup(addr, size);
4050 | if (manuf_value != NULL((void*)0) && ((manuf_value->flags & NAME_RESOLVED(1U<<1)) == NAME_RESOLVED(1U<<1))) {
4051 | return manuf_value->resolved_longname;
4052 | }
4053 |
4054 | if (size >= 6) {
4055 | /* Try the global manuf tables. */
4056 | const char *short_name, *long_name;
4057 | short_name = ws_manuf_lookup_str(addr, &long_name);
4058 | if (short_name != NULL((void*)0)) {
4059 | /* Found it */
4060 | return long_name;
4061 | }
4062 | }
4063 |
4064 | return NULL((void*)0);
4065 |
4066 | } /* get_manuf_name_if_known */
4067 |
4068 | const char *
4069 | uint_get_manuf_name_if_known(const uint32_t manuf_key)
4070 | {
4071 | uint8_t addr[6] = { 0 };
4072 | addr[0] = (manuf_key >> 16) & 0xFF;
4073 | addr[1] = (manuf_key >> 8) & 0xFF;
4074 | addr[2] = manuf_key & 0xFF;
4075 |
4076 | return get_manuf_name_if_known(addr, sizeof(addr));
4077 | }
4078 |
4079 | const char *
4080 | tvb_get_manuf_name_if_known(tvbuff_t *tvb, unsigned offset)
4081 | {
4082 | uint8_t buf[3] = { 0 };
4083 | tvb_memcpy(tvb, buf, offset, 3);
4084 | return get_manuf_name_if_known(buf, sizeof(buf));
4085 | }
4086 |
4087 | bool_Bool get_hash_manuf_used(hashmanuf_t* manuf)
4088 | {
4089 | return ((manuf->flags & TRIED_OR_RESOLVED_MASK((1U<<0) | (1U<<1))) == TRIED_OR_RESOLVED_MASK((1U<<0) | (1U<<1)));
4090 | }
4091 |
4092 | char* get_hash_manuf_resolved_name(hashmanuf_t* manuf)
4093 | {
4094 | return manuf->resolved_longname;
4095 | }
4096 |
4097 | const char *
4098 | get_eui64_name(const uint8_t *addr)
4099 | {
4100 | hasheui64_t *tp;
4101 | bool_Bool resolve = gbl_resolv_flags.mac_name;
4102 |
4103 | tp = eui64_name_lookup(addr, resolve);
4104 |
4105 | return resolve ? tp->resolved_name : tp->hexaddr;
4106 |
4107 | } /* get_eui64_name */
4108 |
4109 | char *
4110 | eui64_to_display(wmem_allocator_t *allocator, const uint64_t addr_eui64)
4111 | {
4112 | uint8_t addr[EUI64_ADDR_LEN8];
4113 |
4114 | phtonu64(addr, addr_eui64);
4115 |
4116 | const char *result = get_eui64_name(addr);
4117 |
4118 | return wmem_strdup(allocator, result);
4119 | } /* eui64_to_display */
4120 |
4121 | #define GHI_TIMEOUT(250 * 1000) (250 * 1000)
4122 | static void
4123 | c_ares_ghi_cb(void *arg, int status, int timeouts _U___attribute__((unused)), struct hostent *hp) {
4124 | /*
4125 | * XXX - If we wanted to be really fancy we could cache results here and
4126 | * look them up in get_host_ipaddr* below.
4127 | *
4128 | * XXX - This only gets the first host address if there's more than one.
4129 | */
4130 | async_hostent_t *ahp = (async_hostent_t *)arg;
4131 | if (status == ARES_SUCCESS && hp && ahp && hp->h_length == ahp->addr_size) {
4132 | memcpy(ahp->addrp, hp->h_addrh_addr_list[0], hp->h_length);
4133 | ahp->copied = hp->h_length;
4134 | }
4135 | }
4136 |
4137 | /* Translate a string, assumed either to be a dotted-quad IPv4 address or
4138 | * a host name, to a numeric IPv4 address. Return true if we succeed and
4139 | * set "*addrp" to that numeric IPv4 address; return false if we fail. */
4140 | bool_Bool
4141 | get_host_ipaddr(const char *host, uint32_t *addrp)
4142 | {
4143 | struct timeval tv = { 0, GHI_TIMEOUT(250 * 1000) }, *tvp;
4144 | int nfds;
4145 | fd_set rfds, wfds;
4146 | async_hostent_t ahe;
4147 |
4148 | /*
4149 | * XXX - are there places where this is used to translate something
4150 | * that's *only* supposed to be an IPv4 address, and where it
4151 | * *shouldn't* translate host names?
4152 | */
4153 | if (!ws_inet_pton4(host, addrp)) {
4154 |
4155 | /* It's not a valid dotted-quad IP address; is it a valid
4156 | * host name?
4157 | */
4158 |
4159 | /* If we're not allowed to do name resolution, don't do name
4160 | * resolution...
4161 | * XXX - What if we're allowed to do name resolution, and the name
4162 | * is in a DNS packet we've dissected or in a Name Resolution Block,
4163 | * or a user-entered manual name resolution?
4164 | */
4165 | if (!gbl_resolv_flags.network_name ||
4166 | !gbl_resolv_flags.use_external_net_name_resolver) {
4167 | return false0;
4168 | }
4169 |
4170 | if (!async_dns_initialized || name_resolve_concurrency < 1) {
4171 | return false0;
4172 | }
4173 | ahe.addr_size = (int) sizeof (struct in_addr);
4174 | ahe.copied = 0;
4175 | ahe.addrp = addrp;
4176 | ares_gethostbyname(ghbn_chan, host, AF_INET2, c_ares_ghi_cb, &ahe);
4177 | FD_ZERO(&rfds)do { unsigned int __i; fd_set *__arr = (&rfds); for (__i = 0; __i < sizeof (fd_set) / sizeof (__fd_mask); ++__i) ((__arr )->__fds_bits)[__i] = 0; } while (0);
4178 | FD_ZERO(&wfds)do { unsigned int __i; fd_set *__arr = (&wfds); for (__i = 0; __i < sizeof (fd_set) / sizeof (__fd_mask); ++__i) ((__arr )->__fds_bits)[__i] = 0; } while (0);
4179 | nfds = ares_fds(ghbn_chan, &rfds, &wfds);
4180 | if (nfds > 0) {
4181 | tvp = ares_timeout(ghbn_chan, &tv, &tv);
4182 | if (select(nfds, &rfds, &wfds, NULL((void*)0), tvp) == -1) { /* call to select() failed */
4183 | /* If it's interrupted by a signal, no need to put out a message */
4184 | if (errno(*__errno_location ()) != EINTR4)
4185 | fprintf(stderrstderr, "Warning: call to select() failed, error is %s\n", g_strerror(errno(*__errno_location ())));
4186 | return false0;
4187 | }
4188 | ares_process(ghbn_chan, &rfds, &wfds);
4189 | }
4190 | ares_cancel(ghbn_chan);
4191 | if (ahe.addr_size == ahe.copied) {
4192 | return true1;
4193 | }
4194 | return false0;
4195 | }
4196 |
4197 | return true1;
4198 | }
4199 |
4200 | /*
4201 | * Translate IPv6 numeric address or FQDN hostname into binary IPv6 address.
4202 | * Return true if we succeed and set "*addrp" to that numeric IPv6 address;
4203 | * return false if we fail.
4204 | */
4205 | bool_Bool
4206 | get_host_ipaddr6(const char *host, ws_in6_addr *addrp)
4207 | {
4208 | struct timeval tv = { 0, GHI_TIMEOUT(250 * 1000) }, *tvp;
4209 | int nfds;
4210 | fd_set rfds, wfds;
4211 | async_hostent_t ahe;
4212 |
4213 | if (str_to_ip6(host, addrp))
4214 | return true1;
4215 |
4216 | /* It's not a valid dotted-quad IP address; is it a valid
4217 | * host name?
4218 | *
4219 | * XXX - are there places where this is used to translate something
4220 | * that's *only* supposed to be an IPv6 address, and where it
4221 | * *shouldn't* translate host names?
4222 | */
4223 |
4224 | /* If we're not allowed to do name resolution, don't do name
4225 | * resolution...
4226 | * XXX - What if we're allowed to do name resolution, and the name
4227 | * is in a DNS packet we've dissected or in a Name Resolution Block,
4228 | * or a user-entered manual name resolution?
4229 | */
4230 | if (!gbl_resolv_flags.network_name ||
4231 | !gbl_resolv_flags.use_external_net_name_resolver) {
4232 | return false0;
4233 | }
4234 |
4235 | /* try FQDN */
4236 | if (!async_dns_initialized || name_resolve_concurrency < 1) {
4237 | return false0;
4238 | }
4239 | ahe.addr_size = (int) sizeof (ws_in6_addr);
4240 | ahe.copied = 0;
4241 | ahe.addrp = addrp;
4242 | ares_gethostbyname(ghbn_chan, host, AF_INET610, c_ares_ghi_cb, &ahe);
4243 | FD_ZERO(&rfds)do { unsigned int __i; fd_set *__arr = (&rfds); for (__i = 0; __i < sizeof (fd_set) / sizeof (__fd_mask); ++__i) ((__arr )->__fds_bits)[__i] = 0; } while (0);
4244 | FD_ZERO(&wfds)do { unsigned int __i; fd_set *__arr = (&wfds); for (__i = 0; __i < sizeof (fd_set) / sizeof (__fd_mask); ++__i) ((__arr )->__fds_bits)[__i] = 0; } while (0);
4245 | nfds = ares_fds(ghbn_chan, &rfds, &wfds);
4246 | if (nfds > 0) {
4247 | tvp = ares_timeout(ghbn_chan, &tv, &tv);
4248 | if (select(nfds, &rfds, &wfds, NULL((void*)0), tvp) == -1) { /* call to select() failed */
4249 | /* If it's interrupted by a signal, no need to put out a message */
4250 | if (errno(*__errno_location ()) != EINTR4)
4251 | fprintf(stderrstderr, "Warning: call to select() failed, error is %s\n", g_strerror(errno(*__errno_location ())));
4252 | return false0;
4253 | }
4254 | ares_process(ghbn_chan, &rfds, &wfds);
4255 | }
4256 | ares_cancel(ghbn_chan);
4257 | if (ahe.addr_size == ahe.copied) {
4258 | return true1;
4259 | }
4260 |
4261 | return false0;
4262 | }
4263 |
4264 | wmem_map_t *
4265 | get_manuf_hashtable(void)
4266 | {
4267 | return manuf_hashtable;
4268 | }
4269 |
4270 | wmem_map_t *
4271 | get_wka_hashtable(void)
4272 | {
4273 | return wka_hashtable;
4274 | }
4275 |
4276 | wmem_map_t *
4277 | get_eth_hashtable(void)
4278 | {
4279 | return eth_hashtable;
4280 | }
4281 |
4282 | wmem_map_t *
4283 | get_serv_port_hashtable(void)
4284 | {
4285 | return serv_port_hashtable;
4286 | }
4287 |
4288 | wmem_map_t *
4289 | get_ipxnet_hash_table(void)
4290 | {
4291 | return ipxnet_hash_table;
4292 | }
4293 |
4294 | wmem_map_t *
4295 | get_vlan_hash_table(void)
4296 | {
4297 | return vlan_hash_table;
4298 | }
4299 |
4300 | wmem_map_t *
4301 | get_ipv4_hash_table(void)
4302 | {
4303 | return ipv4_hash_table;
4304 | }
4305 |
4306 | wmem_map_t *
4307 | get_ipv6_hash_table(void)
4308 | {
4309 | return ipv6_hash_table;
4310 | }
4311 | /* Initialize all the address resolution subsystems in this file */
4312 | void
4313 | addr_resolv_init(const char* app_env_var_prefix)
4314 | {
4315 | ws_assert(addr_resolv_scope == NULL)do { if ((1) && !(addr_resolv_scope == ((void*)0))) ws_log_fatal_full ("", LOG_LEVEL_ERROR, "epan/addr_resolv.c", 4315, __func__, "assertion failed: %s" , "addr_resolv_scope == ((void*)0)"); } while (0);
4316 | addr_resolv_scope = wmem_allocator_new(WMEM_ALLOCATOR_BLOCK);
4317 | initialize_services(app_env_var_prefix);
4318 | initialize_ethers(app_env_var_prefix);
4319 | initialize_ipxnets(app_env_var_prefix);
4320 | initialize_vlans(app_env_var_prefix);
4321 | initialize_enterprises(app_env_var_prefix);
4322 | host_name_lookup_init(app_env_var_prefix);
4323 | initialize_tacs(app_env_var_prefix);
4324 | }
4325 |
4326 | /* Clean up all the address resolution subsystems in this file */
4327 | void
4328 | addr_resolv_cleanup(void)
4329 | {
4330 | vlan_name_lookup_cleanup();
4331 | service_name_lookup_cleanup();
4332 | ethers_cleanup();
4333 | ipx_name_lookup_cleanup();
4334 | enterprises_cleanup();
4335 | host_name_lookup_cleanup();
4336 | tac_name_lookup_cleanup();
4337 |
4338 | wmem_destroy_allocator(addr_resolv_scope);
4339 | addr_resolv_scope = NULL((void*)0);
4340 | }
4341 |
4342 | bool_Bool
4343 | str_to_ip(const char *str, void *dst)
4344 | {
4345 | return ws_inet_pton4(str, (uint32_t *)dst);
4346 | }
4347 |
4348 | bool_Bool
4349 | str_to_ip6(const char *str, void *dst)
4350 | {
4351 | return ws_inet_pton6(str, (ws_in6_addr *)dst);
4352 | }
4353 |
4354 | /*
4355 | * convert a 0-terminated string that contains an ethernet address into
4356 | * the corresponding sequence of 6 bytes
4357 | * eth_bytes is a buffer >= 6 bytes that was allocated by the caller
4358 | */
4359 | bool_Bool
4360 | str_to_eth(const char *str, uint8_t (*eth_bytes)[6])
4361 | {
4362 | ether_t eth;
4363 | unsigned mask;
4364 |
4365 | if (!parse_ether_address(str, &eth, &mask, false0))
4366 | return false0;
4367 |
4368 | if (mask == 48) {
4369 | memcpy(eth_bytes, eth.addr, 6);
4370 | }
4371 | return true1;
4372 | }
4373 |
4374 | /*
4375 | * Editor modelines - https://www.wireshark.org/tools/modelines.html
4376 | *
4377 | * Local variables:
4378 | * c-basic-offset: 4
4379 | * tab-width: 8
4380 | * indent-tabs-mode: nil
4381 | * End:
4382 | *
4383 | * vi: set shiftwidth=4 tabstop=8 expandtab:
4384 | * :indentSize=4:tabSize=8:noTabs=true:
4385 | */